/**
  @page note Note for MDK-ARM
  
  @verbatim
  ******************** (C) COPYRIGHT 2010 STMicroelectronics *******************
  * @file    note.txt
  * @author  MCD Application Team
  * @version V3.4.0
  * @date    10/15/2010
  * @brief   This file contains the needed steps to use the default startup file
  *          provided by RealView Microcontroller Development Kit(MDK-ARM).
  ******************************************************************************
  * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME.
  * AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
  * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE
  * CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING
  * INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
  ******************************************************************************


With MDK-ARM toolchain, a simple putchar function executes a SWI and activates 
a low level putchar function. 
You have to redirect the low level to your own implementation of these functions.

To guarantee that no functions using the semihosting SWI are included in your 
application, either:

1. Ensure that the MicroLib option is checked since the microlib does not support
semihosting
or 
2. Use
- IMPORT __use_no_semihosting_swi from assembly language
- #pragma import(__use_no_semihosting_swi) from C.
 
 @endverbatim
 
@note
 - Low-density Value line devices are STM32F100xx microcontrollers where the 
   Flash memory density ranges between 16 and 32 Kbytes.
 - Low-density devices are STM32F101xx, STM32F102xx and STM32F103xx 
   microcontrollers where the Flash memory density ranges between 16 and 32 Kbytes.
 - Medium-density Value line devices are STM32F100xx microcontrollers where
   the Flash memory density ranges between 32 and 128 Kbytes.  
 - Medium-density devices are STM32F101xx, STM32F102xx and STM32F103xx 
   microcontrollers where the Flash memory density ranges between 32 and 128 Kbytes.
 - High-density Value line devices are STM32F100xx microcontrollers where the 
   Flash memory density ranges between 256 and 512 Kbytes.
 - High-density devices are STM32F101xx and STM32F103xx microcontrollers where
   the Flash memory density ranges between 256 and 512 Kbytes.
 - XL-density devices are STM32F101xx and STM32F103xx microcontrollers where
   the Flash memory density ranges between 512 and 1024 Kbytes.
 - Connectivity line devices are STM32F105xx and STM32F107xx microcontrollers. 

 * <h3><center>&copy; COPYRIGHT 2010 STMicroelectronics</center></h3>
 */
