# Static Call Graph for image .\Release\Neigungsmessung.axf

#<CALLGRAPH># ARM Linker, RVCT4.0 [Build 728]: Last Updated: Sun Apr 17 20:00:59 2011

### Maximum Stack Usage = 260 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ atan2 ⇒ atan ⇒ __kernel_poly ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - Reset_Handler
  - NMI_Handler
  - HardFault_Handler
  - MemManage_Handler
  - BusFault_Handler
  - UsageFault_Handler
  - SVC_Handler
  - DebugMon_Handler
  - PendSV_Handler
  - SysTick_Handler
  - WWDG_IRQHandler
  - PVD_IRQHandler
  - TAMPER_IRQHandler
  - RTC_IRQHandler
  - FLASH_IRQHandler
  - RCC_IRQHandler
  - EXTI0_IRQHandler
  - EXTI1_IRQHandler
  - EXTI2_IRQHandler
  - EXTI3_IRQHandler
  - EXTI4_IRQHandler
  - DMA1_Channel1_IRQHandler
  - DMA1_Channel2_IRQHandler
  - DMA1_Channel3_IRQHandler
  - DMA1_Channel4_IRQHandler
  - DMA1_Channel5_IRQHandler
  - DMA1_Channel6_IRQHandler
  - DMA1_Channel7_IRQHandler
  - ADC1_2_IRQHandler
  - USB_HP_CAN1_TX_IRQHandler
  - USB_LP_CAN1_RX0_IRQHandler
  - CAN1_RX1_IRQHandler
  - CAN1_SCE_IRQHandler
  - EXTI9_5_IRQHandler
  - TIM1_BRK_IRQHandler
  - TIM1_UP_IRQHandler
  - TIM1_TRG_COM_IRQHandler
  - TIM1_CC_IRQHandler
  - TIM2_IRQHandler
  - TIM3_IRQHandler
  - TIM4_IRQHandler
  - I2C1_EV_IRQHandler
  - I2C1_ER_IRQHandler
  - I2C2_EV_IRQHandler
  - I2C2_ER_IRQHandler
  - SPI1_IRQHandler
  - SPI2_IRQHandler
  - USART1_IRQHandler
  - USART2_IRQHandler
  - USART3_IRQHandler
  - EXTI15_10_IRQHandler
  - RTCAlarm_IRQHandler
  - USBWakeUp_IRQHandler
  - TIM8_BRK_IRQHandler
  - TIM8_UP_IRQHandler
  - TIM8_TRG_COM_IRQHandler
  - TIM8_CC_IRQHandler
  - ADC3_IRQHandler
  - FSMC_IRQHandler
  - SDIO_IRQHandler
  - TIM5_IRQHandler
  - SPI3_IRQHandler
  - UART4_IRQHandler
  - UART5_IRQHandler
  - TIM6_IRQHandler
  - TIM7_IRQHandler
  - DMA2_Channel1_IRQHandler
  - DMA2_Channel2_IRQHandler
  - DMA2_Channel3_IRQHandler
  - DMA2_Channel4_5_IRQHandler
  - main
  - SystemInit
  - __main

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry7.o(.ARM.Collect$$$$00000007))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __aeabi_dadd (Thumb, 338 bytes, Stack size 72 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 124
  - Call Chain = __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_round
  - >> _double_epilogue
  [Called By]
  - >> __aeabi_dsub
  - >> __aeabi_drsub
  - >> __kernel_poly
  - >> atan
  - >> atan2

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 124
  - Call Chain = __aeabi_dsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> atan
  - >> atan2

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 124
  - Call Chain = __aeabi_drsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> atan
  - >> atan2

  __aeabi_dmul (Thumb, 240 bytes, Stack size 64 bytes, dmul.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> __kernel_poly
  - >> atan

  __aeabi_ui2d (Thumb, 26 bytes, Stack size 16 bytes, dfltui.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> main

  __aeabi_llsl (Thumb, 32 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_dadd
  - >> _double_epilogue

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 34 bytes, Stack size 0 bytes, llsshr.o(.text))
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  __I$use$fp (Thumb, 0 bytes, Stack size 20 bytes, iusefp.o(.text), UNUSED)

  _double_round (Thumb, 50 bytes, Stack size 20 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = _double_round
  [Called By]
  - >> __aeabi_dadd
  - >> _double_epilogue
  - >> __aeabi_ddiv

  _double_epilogue (Thumb, 184 bytes, Stack size 32 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> _double_round
  [Called By]
  - >> __aeabi_ui2d
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  __aeabi_ddiv (Thumb, 280 bytes, Stack size 56 bytes, ddiv.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> _double_round
  [Called By]
  - >> atan
  - >> atan2

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 30 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> _double_epilogue

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __ARM_scalbn (Thumb, 64 bytes, Stack size 16 bytes, dscalb.o(.text), UNUSED)

  scalbn (Thumb, 0 bytes, Stack size 16 bytes, dscalb.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = scalbn
  [Called By]
  - >> atan

  ADC_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_Cmd))
  [Called By]

  - >> ADC_Configuration

  ADC_Configuration (Thumb, 106 bytes, Stack size 32 bytes, neigungsmessung.o(i.ADC_Configuration))
  [Stack]

  - Max Depth = 44
  - Call Chain = ADC_Configuration ⇒ ADC_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_ADCCLKConfig
  - >> ADC_StartCalibration
  - >> ADC_ResetCalibration
  - >> ADC_Init
  - >> ADC_GetResetCalibrationStatus
  - >> ADC_GetCalibrationStatus
  - >> ADC_DeInit
  - >> ADC_Cmd
  [Called By]
  - >> main

  ADC_DeInit (Thumb, 56 bytes, Stack size 8 bytes, stm32f10x_adc.o(i.ADC_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC_DeInit
  [Calls]
  - >> RCC_APB2PeriphResetCmd
  [Called By]
  - >> ADC_Configuration

  ADC_GetCalibrationStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_GetCalibrationStatus))
  [Called By]

  - >> ADC_Configuration

  ADC_GetConversionValue (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_GetConversionValue))
  [Called By]

  - >> ADC_Read

  ADC_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_GetFlagStatus))
  [Called By]

  - >> ADC_Read

  ADC_GetResetCalibrationStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_GetResetCalibrationStatus))
  [Called By]

  - >> ADC_Configuration

  ADC_Init (Thumb, 62 bytes, Stack size 12 bytes, stm32f10x_adc.o(i.ADC_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = ADC_Init
  [Called By]
  - >> ADC_Configuration

  ADC_Read (Thumb, 46 bytes, Stack size 8 bytes, neigungsmessung.o(i.ADC_Read))
  [Stack]

  - Max Depth = 24
  - Call Chain = ADC_Read ⇒ ADC_RegularChannelConfig
  [Calls]
  - >> ADC_SoftwareStartConvCmd
  - >> ADC_RegularChannelConfig
  - >> ADC_GetFlagStatus
  - >> ADC_GetConversionValue
  [Called By]
  - >> main

  ADC_RegularChannelConfig (Thumb, 116 bytes, Stack size 16 bytes, stm32f10x_adc.o(i.ADC_RegularChannelConfig))
  [Stack]

  - Max Depth = 16
  - Call Chain = ADC_RegularChannelConfig
  [Called By]
  - >> ADC_Read

  ADC_ResetCalibration (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_ResetCalibration))
  [Called By]

  - >> ADC_Configuration

  ADC_SoftwareStartConvCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_SoftwareStartConvCmd))
  [Called By]

  - >> ADC_Read

  ADC_StartCalibration (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_StartCalibration))
  [Called By]

  - >> ADC_Configuration

  BKP_DeInit (Thumb, 18 bytes, Stack size 8 bytes, stm32f10x_bkp.o(i.BKP_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = BKP_DeInit
  [Calls]
  - >> RCC_BackupResetCmd
  - >> FLASH_SetLatency
  [Called By]
  - >> RTCSetup

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_PrefetchBufferCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_PrefetchBufferCmd))
  [Called By]

  - >> RCC_Configuration

  FLASH_SetLatency (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_SetLatency))
  [Called By]

  - >> BKP_DeInit
  - >> RCC_Configuration

  GPIO_Init (Thumb, 158 bytes, Stack size 20 bytes, stm32f10x_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> USART_Configuration
  - >> LCD_init

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_StructInit))
  [Called By]

  - >> USART_Configuration
  - >> LCD_init

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_WriteBit))
  [Called By]

  - >> LCD_init
  - >> LCD_enable
  - >> LCD_data
  - >> LCD_command

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  LCD_clear (Thumb, 18 bytes, Stack size 8 bytes, neigungsmessung.o(i.LCD_clear))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_clear ⇒ LCD_command ⇒ LCD_enable
  [Calls]
  - >> delay_ms
  - >> LCD_command
  [Called By]
  - >> LCD_init

  LCD_command (Thumb, 56 bytes, Stack size 16 bytes, neigungsmessung.o(i.LCD_command))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_command ⇒ LCD_enable
  [Calls]
  - >> GPIO_WriteBit
  - >> delay_us
  - >> LCD_enable
  [Called By]
  - >> LCD_init
  - >> LCD_clear

  LCD_data (Thumb, 56 bytes, Stack size 16 bytes, neigungsmessung.o(i.LCD_data))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_data ⇒ LCD_enable
  [Calls]
  - >> GPIO_WriteBit
  - >> delay_us
  - >> LCD_enable
  [Called By]
  - >> LCD_string

  LCD_enable (Thumb, 34 bytes, Stack size 8 bytes, neigungsmessung.o(i.LCD_enable))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_enable
  [Calls]
  - >> GPIO_WriteBit
  - >> delay_us
  [Called By]
  - >> LCD_init
  - >> LCD_data
  - >> LCD_command

  LCD_init (Thumb, 144 bytes, Stack size 16 bytes, neigungsmessung.o(i.LCD_init))
  [Stack]

  - Max Depth = 48
  - Call Chain = LCD_init ⇒ LCD_clear ⇒ LCD_command ⇒ LCD_enable
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_WriteBit
  - >> GPIO_StructInit
  - >> GPIO_Init
  - >> delay_ms
  - >> LCD_enable
  - >> LCD_command
  - >> LCD_clear
  [Called By]
  - >> main

  LCD_string (Thumb, 22 bytes, Stack size 8 bytes, neigungsmessung.o(i.LCD_string))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_string ⇒ LCD_data ⇒ LCD_enable
  [Calls]
  - >> LCD_data
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  NVIC_Configuration (Thumb, 10 bytes, Stack size 0 bytes, neigungsmessung.o(i.NVIC_Configuration))
  [Called By]

  - >> main

  NVIC_SetVectorTable (Thumb, 12 bytes, Stack size 0 bytes, misc.o(i.NVIC_SetVectorTable), UNUSED)

  PWR_BackupAccessCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_pwr.o(i.PWR_BackupAccessCmd))
  [Called By]

  - >> RTCSetup

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_ADCCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_ADCCLKConfig))
  [Called By]

  - >> ADC_Configuration

  RCC_APB1PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> USART_Configuration
  - >> RTCSetup

  RCC_APB1PeriphResetCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphResetCmd))
  [Called By]

  - >> USART_DeInit

  RCC_APB2PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> USART_Configuration
  - >> LCD_init
  - >> ADC_Configuration

  RCC_APB2PeriphResetCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphResetCmd))
  [Called By]

  - >> USART_DeInit
  - >> ADC_DeInit

  RCC_BackupResetCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_BackupResetCmd))
  [Called By]

  - >> BKP_DeInit

  RCC_Configuration (Thumb, 98 bytes, Stack size 8 bytes, neigungsmessung.o(i.RCC_Configuration))
  [Stack]

  - Max Depth = 20
  - Call Chain = RCC_Configuration ⇒ RCC_WaitForHSEStartUp
  [Calls]
  - >> RCC_WaitForHSEStartUp
  - >> RCC_SYSCLKConfig
  - >> RCC_PLLConfig
  - >> RCC_PLLCmd
  - >> RCC_PCLK2Config
  - >> RCC_PCLK1Config
  - >> RCC_HSEConfig
  - >> RCC_HCLKConfig
  - >> RCC_GetSYSCLKSource
  - >> RCC_GetFlagStatus
  - >> RCC_DeInit
  - >> FLASH_SetLatency
  - >> FLASH_PrefetchBufferCmd
  [Called By]
  - >> main

  RCC_DeInit (Thumb, 50 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_DeInit))
  [Called By]

  - >> RCC_Configuration

  RCC_GetClocksFreq (Thumb, 132 bytes, Stack size 8 bytes, stm32f10x_rcc.o(i.RCC_GetClocksFreq))
  [Stack]

  - Max Depth = 8
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  RCC_GetFlagStatus (Thumb, 42 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_GetFlagStatus))
  [Called By]

  - >> RCC_WaitForHSEStartUp
  - >> RTCSetup
  - >> RCC_Configuration

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_GetSYSCLKSource))
  [Called By]

  - >> RCC_Configuration

  RCC_HCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_HCLKConfig))
  [Called By]

  - >> RCC_Configuration

  RCC_HSEConfig (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_HSEConfig))
  [Called By]

  - >> RCC_Configuration

  RCC_LSEConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_LSEConfig))
  [Called By]

  - >> RTCSetup

  RCC_PCLK1Config (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PCLK1Config))
  [Called By]

  - >> RCC_Configuration

  RCC_PCLK2Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PCLK2Config))
  [Called By]

  - >> RCC_Configuration

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PLLCmd))
  [Called By]

  - >> RCC_Configuration

  RCC_PLLConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PLLConfig))
  [Called By]

  - >> RCC_Configuration

  RCC_RTCCLKCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_RTCCLKCmd))
  [Called By]

  - >> RTCSetup

  RCC_RTCCLKConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_RTCCLKConfig))
  [Called By]

  - >> RTCSetup

  RCC_SYSCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_SYSCLKConfig))
  [Called By]

  - >> RCC_Configuration

  RCC_WaitForHSEStartUp (Thumb, 38 bytes, Stack size 12 bytes, stm32f10x_rcc.o(i.RCC_WaitForHSEStartUp))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_WaitForHSEStartUp
  [Calls]
  - >> RCC_GetFlagStatus
  [Called By]
  - >> RCC_Configuration

  RTCSetup (Thumb, 88 bytes, Stack size 8 bytes, neigungsmessung.o(i.RTCSetup))
  [Stack]

  - Max Depth = 16
  - Call Chain = RTCSetup ⇒ BKP_DeInit
  [Calls]
  - >> RTC_WaitForSynchro
  - >> RTC_WaitForLastTask
  - >> RTC_SetPrescaler
  - >> RTC_ITConfig
  - >> RCC_RTCCLKConfig
  - >> RCC_RTCCLKCmd
  - >> RCC_LSEConfig
  - >> RCC_GetFlagStatus
  - >> RCC_APB1PeriphClockCmd
  - >> PWR_BackupAccessCmd
  - >> BKP_DeInit
  [Called By]
  - >> main

  RTC_EnterConfigMode (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_rtc.o(i.RTC_EnterConfigMode))
  [Called By]

  - >> RTC_SetPrescaler

  RTC_ExitConfigMode (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_rtc.o(i.RTC_ExitConfigMode))
  [Called By]

  - >> RTC_SetPrescaler

  RTC_ITConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_rtc.o(i.RTC_ITConfig))
  [Called By]

  - >> RTCSetup

  RTC_SetPrescaler (Thumb, 26 bytes, Stack size 4 bytes, stm32f10x_rtc.o(i.RTC_SetPrescaler))
  [Stack]

  - Max Depth = 4
  - Call Chain = RTC_SetPrescaler
  [Calls]
  - >> RTC_ExitConfigMode
  - >> RTC_EnterConfigMode
  [Called By]
  - >> RTCSetup

  RTC_WaitForLastTask (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rtc.o(i.RTC_WaitForLastTask))
  [Called By]

  - >> RTCSetup

  RTC_WaitForSynchro (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rtc.o(i.RTC_WaitForSynchro))
  [Called By]

  - >> RTCSetup

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SysTick_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SysTick_fkt (Thumb, 10 bytes, Stack size 0 bytes, neigungsmessung.o(i.SysTick_fkt), UNUSED)

  SystemInit (Thumb, 64 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SystemInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = SystemInit
  [Calls]
  - >> SetSysClockTo72
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(.text)

  USART_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_Cmd))
  [Called By]

  - >> USART_Configuration

  USART_Configuration (Thumb, 148 bytes, Stack size 32 bytes, neigungsmessung.o(i.USART_Configuration))
  [Stack]

  - Max Depth = 72
  - Call Chain = USART_Configuration ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_StructInit
  - >> USART_Init
  - >> USART_DeInit
  - >> USART_Cmd
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> GPIO_StructInit
  - >> GPIO_Init
  [Called By]
  - >> main

  USART_DeInit (Thumb, 96 bytes, Stack size 8 bytes, stm32f10x_usart.o(i.USART_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART_DeInit
  [Calls]
  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB1PeriphResetCmd
  [Called By]
  - >> USART_Configuration

  USART_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_GetFlagStatus))
  [Called By]

  - >> USART_Send

  USART_Init (Thumb, 176 bytes, Stack size 32 bytes, stm32f10x_usart.o(i.USART_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> USART_Configuration

  USART_Send (Thumb, 34 bytes, Stack size 16 bytes, neigungsmessung.o(i.USART_Send))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_Send
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Called By]
  - >> main

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_SendData))
  [Called By]

  - >> USART_Send

  USART_StructInit (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_StructInit))
  [Called By]

  - >> USART_Configuration

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  __kernel_poly (Thumb, 170 bytes, Stack size 24 bytes, poly.o(i.__kernel_poly))
  [Stack]

  - Max Depth = 148
  - Call Chain = __kernel_poly ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dmul
  - >> __aeabi_dadd
  [Called By]
  - >> atan

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  __set_errno (Thumb, 6 bytes, Stack size 0 bytes, errno.o(i.__set_errno))
  [Called By]

  - >> atan2

  atan (Thumb, 524 bytes, Stack size 40 bytes, atan.o(i.atan))
  [Stack]

  - Max Depth = 188
  - Call Chain = atan ⇒ __kernel_poly ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dsub
  - >> __aeabi_drsub
  - >> __aeabi_dmul
  - >> __aeabi_dadd
  - >> __kernel_poly
  - >> scalbn
  - >> __aeabi_ddiv
  [Called By]
  - >> atan2

  atan2 (Thumb, 376 bytes, Stack size 32 bytes, atan2.o(i.atan2))
  [Stack]

  - Max Depth = 220
  - Call Chain = atan2 ⇒ atan ⇒ __kernel_poly ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dsub
  - >> __aeabi_drsub
  - >> __aeabi_dadd
  - >> __set_errno
  - >> atan
  - >> __aeabi_ddiv
  [Called By]
  - >> main

  delay_ms (Thumb, 20 bytes, Stack size 0 bytes, neigungsmessung.o(i.delay_ms))
  [Called By]

  - >> LCD_init
  - >> LCD_clear

  delay_us (Thumb, 14 bytes, Stack size 0 bytes, neigungsmessung.o(i.delay_us))
  [Called By]

  - >> LCD_enable
  - >> LCD_data
  - >> LCD_command

  main (Thumb, 164 bytes, Stack size 40 bytes, neigungsmessung.o(i.main))
  [Stack]

  - Max Depth = 260
  - Call Chain = main ⇒ atan2 ⇒ atan ⇒ __kernel_poly ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_ui2d
  - >> USART_Send
  - >> USART_Configuration
  - >> RTCSetup
  - >> RCC_Configuration
  - >> NVIC_Configuration
  - >> LCD_string
  - >> LCD_init
  - >> ADC_Read
  - >> ADC_Configuration
  - >> atan2
  [Address Reference Count : 1]
  - entry7.o(.ARM.Collect$$$$00000007)

  ### Local Symbols

  SetSysClockTo72 (Thumb, 136 bytes, Stack size 0 bytes, system_stm32f10x.o(i.SetSysClockTo72))
  [Called By]

  - >> SystemInit

  ### Undefined Global Symbols