Embedded Webserver Modul |  | Internet: http://www.easyToWeb.net
easyToWeb-AVR with ATmega128(L) | E-Mail: info@easyToWeb.net

The easyToWeb-AVR Embedded Webserver - a powerful solution with ATmega128(L)TM and 10Mbit-Ethernetcontroller CS8900A
easyToWeb-AVR Features ATmega128(L) Microcontroller 10 Mbit Ethernetcontroller 32..64 kByte SRAM 2..16 Mbit Dataflash 4 LED's for AVR Status-Informations 2 LED's for CS8900 Status-Informations onboard Power 5V. easyToWeb-AVR Connections Ethernet-RJ45 Twisted Pair, Two RS232-Interfaces, Two UART-Interfaces, On-Board programming with external adapter, eTW-Interface supports all ATmega128-signals + serial interfaces. |  | easyToWeb-AVR software and protocols Software - adapted for AVR - based on the free available C-sources - easyToWeb-Server from the extra booklet "Embedded Internet" to Design & Elektronik, Project with the CodeVisionAVR C-Compiler, supported protocolls (TCP/IP, UDP, ARP, BooTP, ICMP and HTTP-Server), The software is described globally in the extra booklet "Embedded Internet" to Design & Elektronik, The adapted C-sources are freely available. easyToWeb-AVR technical data Boardsize 73 x 85 mm2, 5V DC about 145 mA (16Mhz), 3.3V DC about 85 mA (7.3728Mhz), eTW-Interface: 88 in all.