 ;ASCII table, character definition - for graphics LCD display (yampp7)
 ;Allow codes from 0 to 127 - 7 bit coding for lower memory usage.
 .byte 0x00,0x00,0x00,0x00,0x00,0x00	;00 - blank char
 .byte 0x3E,0x0A,0x34,0x00,0x3E,0x0C	;01 - random sign L		OK
 .byte 0x18,0x3E,0x00,0x3E,0x22,0x1C	;02 - random sign R		OK
 .byte 0x00,0x3E,0x20,0x20,0x00,0x3E	;03 - loudness sign L		OK
 .byte 0x22,0x1C,0x00,0x24,0x2A,0x12	;04 - loudness sign R		OK
 .byte 0x7F,0x41,0x55,0x41,0x55,0x41	;05 - keylock sign L		OK
 .byte 0x41,0x5D,0x51,0x5D,0x41,0x7f	;06 - key unlocked sign R	OK
 .byte 0x00,0x38,0x38,0x44,0x82,0xFE	;07 - min volume sign		OK
 .byte 0x00,0x1C,0x3E,0x62,0x62,0x32	;08 - low battery sign L	OK
 .byte 0x3A,0x2E,0x26,0x23,0x23,0x3E	;09 - low battery sign R	OK
 .byte 0x00,0x00,0x00,0x00,0x00,0x00	;0a - don't use
 .byte 0x00,0x1C,0x3E,0x36,0x22,0x36	;0b - good battery sign L	OK
 .byte 0x3E,0x3E,0x36,0x36,0x36,0x3E	;0c - good battery sign R	OK
 .byte 0x00,0x00,0x00,0x00,0x00,0x00	;0d - don't use
 .byte 0x41,0x5D,0x51,0x51,0x41,0x7f	;0e - key locked sign R		OK
 .byte 0x41,0x5D,0x4b,0x5d,0x41,0x7F	;0f - autolock on sign R	OK
 .byte 0x00,0x3E,0x0A,0x04,0x78,0x40	;10 - repeat sign 1 L		OK
 .byte 0x00,0x3E,0x0A,0x04,0x78,0x40	;11 - repeat sign 2 L		OK
 .byte 0x00,0x38,0x44,0x5F,0x4E,0x44	;12 - repeat sign 3 L		OK
 .byte 0x00,0x38,0x44,0x44,0x5F,0x4E	;13 - repeat sign 4 L		OK
 .byte 0x00,0X3C,0x3C,0x3C,0x3C,0x00	;14 - repeat sign 1 R		OK
 .byte 0x00,0x3E,0x0A,0x04,0x78,0x40	;15 - repeat sign 2 R		OK
 .byte 0x00,0x3E,0x0A,0x04,0x78,0x40	;16 - repeat sign 3 R		OK
 .byte 0x44,0x40,0x38,0x00,0x04,0x7E	;17 - repeat sign 4 R		OK
 .byte 0x00,0x7F,0x3E,0x1C,0x08,0x00	;18 - sign ">" for menus	OK
 .byte 0x08,0x08,0x2A,0x1C,0x08,0x00	;19 - balance right arrow	OK
 .byte 0x08,0x1C,0x2A,0x08,0x08,0x00	;1a - balancr left arrow	OK
 .byte 0x08,0x08,0x2A,0x08,0x08,0x00	;1b -
 .byte 0x00,0x3C,0x20,0x00,0x00,0x00	;1c -
 .byte 0x08,0x14,0x00,0x14,0x08,0x00	;1d -
 .byte 0x08,0x0C,0x0E,0x0C,0x08,0x00	;1e -
 .byte 0x08,0x18,0x38,0x18,0x08,0x00	;1f -
 .byte 0x00,0x00,0x00,0x00,0x00,0x00
 .byte 0x00,0x00,0x5F,0x00,0x00,0x00
 .byte 0x00,0x07,0x00,0x07,0x00,0x00
 .byte 0x14,0x7F,0x14,0x7F,0x14,0x00
 .byte 0x24,0x2A,0x7F,0x2A,0x12,0x00
 .byte 0x23,0x13,0x08,0x64,0x62,0x00
 .byte 0x36,0x49,0x55,0x22,0x50,0x00
 .byte 0x00,0x05,0x03,0x00,0x00,0x00
 .byte 0x00,0x1C,0x22,0x41,0x00,0x00
 .byte 0x00,0x41,0x22,0x1C,0x00,0x00
 .byte 0x14,0x08,0x3E,0x08,0x14,0x00
 .byte 0x08,0x08,0x3E,0x08,0x08,0x00
 .byte 0x00,0x50,0x30,0x00,0x00,0x00
 .byte 0x08,0x08,0x08,0x08,0x08,0x00
 .byte 0x00,0x60,0x60,0x00,0x00,0x00
 .byte 0x20,0x10,0x08,0x04,0x02,0x00
 .byte 0x3E,0x51,0x49,0x45,0x3E,0x00
 .byte 0x00,0x42,0x7F,0x40,0x00,0x00
 .byte 0x42,0x61,0x51,0x49,0x46,0x00
 .byte 0x21,0x41,0x45,0x4B,0x31,0x00
 .byte 0x18,0x14,0x12,0x7F,0x10,0x00
 .byte 0x27,0x45,0x45,0x45,0x39,0x00
 .byte 0x3C,0x4A,0x49,0x49,0x30,0x00
 .byte 0x01,0x71,0x09,0x05,0x03,0x00
 .byte 0x36,0x49,0x49,0x49,0x36,0x00
 .byte 0x06,0x49,0x49,0x29,0x1E,0x00
 .byte 0x00,0x36,0x36,0x00,0x00,0x00
 .byte 0x00,0x56,0x36,0x00,0x00,0x00
 .byte 0x08,0x14,0x22,0x41,0x00,0x00
 .byte 0x14,0x14,0x14,0x14,0x14,0x00
 .byte 0x00,0x41,0x22,0x14,0x08,0x00
 .byte 0x02,0x01,0x51,0x09,0x06,0x00
 .byte 0x32,0x49,0x79,0x41,0x3E,0x00
 .byte 0x7E,0x11,0x11,0x11,0x7E,0x00
 .byte 0x7F,0x49,0x49,0x49,0x36,0x00
 .byte 0x3E,0x41,0x41,0x41,0x22,0x00
 .byte 0x7F,0x41,0x41,0x22,0x1C,0x00
 .byte 0x7F,0x49,0x49,0x49,0x41,0x00
 .byte 0x7F,0x09,0x09,0x09,0x01,0x00
 .byte 0x3E,0x41,0x49,0x49,0x7A,0x00
 .byte 0x7F,0x08,0x08,0x08,0x7F,0x00
 .byte 0x00,0x41,0x7F,0x41,0x00,0x00
 .byte 0x20,0x40,0x41,0x3F,0x01,0x00
 .byte 0x7F,0x08,0x14,0x22,0x41,0x00
 .byte 0x7F,0x40,0x40,0x40,0x40,0x00
 .byte 0x7F,0x02,0x0C,0x02,0x7F,0x00
 .byte 0x7F,0x04,0x08,0x10,0x7F,0x00
 .byte 0x3E,0x41,0x41,0x41,0x3E,0x00
 .byte 0x7F,0x09,0x09,0x09,0x06,0x00
 .byte 0x3E,0x41,0x51,0x21,0x5E,0x00
 .byte 0x7F,0x09,0x19,0x29,0x46,0x00
 .byte 0x46,0x49,0x49,0x49,0x31,0x00
 .byte 0x01,0x01,0x7F,0x01,0x01,0x00
 .byte 0x3F,0x40,0x40,0x40,0x3F,0x00
 .byte 0x1F,0x20,0x40,0x20,0x1F,0x00
 .byte 0x3F,0x40,0x38,0x40,0x3F,0x00
 .byte 0x63,0x14,0x08,0x14,0x63,0x00
 .byte 0x07,0x08,0x70,0x08,0x07,0x00
 .byte 0x61,0x51,0x49,0x45,0x43,0x00
 .byte 0x00,0x7F,0x41,0x41,0x00,0x00
 .byte 0x02,0x04,0x08,0x10,0x20,0x00
 .byte 0x00,0x41,0x41,0x7F,0x00,0x00
 .byte 0x04,0x02,0x01,0x02,0x04,0x00
 .byte 0x40,0x40,0x40,0x40,0x40,0x00
 .byte 0x00,0x01,0x02,0x04,0x00,0x00
 .byte 0x20,0x54,0x54,0x54,0x78,0x00
 .byte 0x7F,0x48,0x44,0x44,0x38,0x00
 .byte 0x38,0x44,0x44,0x44,0x20,0x00
 .byte 0x38,0x44,0x44,0x48,0x7F,0x00
 .byte 0x38,0x54,0x54,0x54,0x18,0x00
 .byte 0x08,0x7E,0x09,0x01,0x02,0x00
 .byte 0x0C,0x52,0x52,0x52,0x3E,0x00
 .byte 0x7F,0x08,0x04,0x04,0x78,0x00
 .byte 0x00,0x44,0x7D,0x40,0x00,0x00
 .byte 0x20,0x40,0x44,0x3D,0x00,0x00
 .byte 0x7F,0x10,0x28,0x44,0x00,0x00
 .byte 0x00,0x41,0x7F,0x40,0x00,0x00
 .byte 0x7C,0x04,0x18,0x04,0x78,0x00
 .byte 0x7C,0x08,0x04,0x04,0x78,0x00
 .byte 0x38,0x44,0x44,0x44,0x38,0x00
 .byte 0x7C,0x14,0x14,0x14,0x08,0x00
 .byte 0x08,0x14,0x14,0x18,0x7C,0x00
 .byte 0x7C,0x08,0x04,0x04,0x08,0x00
 .byte 0x48,0x54,0x54,0x54,0x20,0x00
 .byte 0x04,0x3F,0x44,0x40,0x20,0x00
 .byte 0x3C,0x40,0x40,0x20,0x7C,0x00
 .byte 0x1C,0x20,0x40,0x20,0x1C,0x00
 .byte 0x3C,0x40,0x30,0x40,0x3C,0x00
 .byte 0x44,0x28,0x10,0x28,0x44,0x00
 .byte 0x0C,0x50,0x50,0x50,0x3C,0x00
 .byte 0x44,0x64,0x54,0x4C,0x44,0x00
 .byte 0x00,0x08,0x36,0x41,0x00,0x00
 .byte 0x00,0x00,0x7F,0x00,0x00,0x00
 .byte 0x00,0x41,0x36,0x08,0x00,0x00
 .byte 0x10,0x08,0x08,0x10,0x08,0x00
 .byte 0x78,0x46,0x41,0x46,0x78,0x00
