<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="35.738" y1="0" x2="35.738" y2="10.912" width="0" layer="20"/>
<wire x1="35.738" y1="10.912" x2="0" y2="10.912" width="0" layer="20"/>
<wire x1="0" y1="10.912" x2="0" y2="0" width="0" layer="20"/>
<wire x1="35.992" y1="-0.01" x2="0" y2="-0.01" width="0" layer="20"/>
</plain>
<libraries>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="PB3XX301V050A">
<description>&lt;b&gt;RGB LED&lt;/b&gt; with integrated controller chip&lt;p&gt;
Source: &lt;a href="http://www.kirronlightcomponents.com/produkte/dyco-led1/"&gt; Data sheedt &lt;/a&gt; DycoLED.pdf&lt;br&gt;
http://www.ubleds.com.tw</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="led" package="PB3XX301V050A" value="PB3XX301V050A"/>
<element name="LED2" library="led" package="PB3XX301V050A" value="PB3XX301V050A"/>
<element name="LED3" library="led" package="PB3XX301V050A" value="PB3XX301V050A"/>
<element name="C1" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="C2" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
<element name="C3" library="SparkFun-Passives" package="0402-CAP" value="0.1uF"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="LED1" pad="4"/>
<contactref element="LED2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="5"/>
<contactref element="LED2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="LED2" pad="4"/>
<contactref element="LED3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="LED2" pad="5"/>
<contactref element="LED3" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="LED1" pad="6"/>
<contactref element="LED2" pad="6"/>
<contactref element="LED3" pad="6"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="LED1" pad="3"/>
<contactref element="LED2" pad="3"/>
<contactref element="LED3" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
</signals>
</board>
</drawing>
</eagle>
