<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<library>
<packages>
<package name="STM32F407_LQFP176">
<description>LQFP176 Package für STM32F4xx by E. Guenes 2012</description>
</package>
</packages>
<symbols>
<symbol name="STM32F407_LQFP176">
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PI8"/>
<pin name="PC13"/>
<pin name="PC14/OSC32_IN"/>
<pin name="PC15/OSC32_OUT"/>
<pin name="PI9"/>
<pin name="PI10"/>
<pin name="PI11"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="VSS_1" direction="pwr"/>
<pin name="VDD_1" direction="pwr"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF10"/>
<pin name="PH0/OSC_IN"/>
<pin name="PH1/OSC_OUT"/>
<pin name="NRST"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="PA0/WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PA3"/>
<pin name="VSS_4" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2/BOOT_1"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="VSS_5" direction="pwr"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PE7"/>
<pin name="PE8"/>
<pin name="PE9"/>
<pin name="VSS_6" direction="pwr"/>
<pin name="VDD_5" direction="pwr"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="VCAP_1" direction="pwr"/>
<pin name="VDD_6" direction="pwr"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PH8"/>
<pin name="PH9"/>
<pin name="PH10"/>
<pin name="PH11"/>
<pin name="PH12"/>
<pin name="VSS_7" direction="pwr"/>
<pin name="VDD_7" direction="pwr"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="VSS_8" direction="pwr"/>
<pin name="VDD_8" direction="pwr"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="VSS_9" direction="pwr"/>
<pin name="VDD_9" direction="pwr"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="VCAP_2" direction="pwr"/>
<pin name="VSS_10" direction="pwr"/>
<pin name="VDD_10" direction="pwr"/>
<pin name="PH13"/>
<pin name="PH14"/>
<pin name="PH15"/>
<pin name="PI0"/>
<pin name="PI1"/>
<pin name="PI2"/>
<pin name="PI3"/>
<pin name="VSS_11" direction="pwr"/>
<pin name="VDD_11" direction="pwr"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="VSS_12" direction="pwr"/>
<pin name="VDD_12" direction="pwr"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG11"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="VSS_13" direction="pwr"/>
<pin name="VDD_13" direction="pwr"/>
<pin name="PG15"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="BOOT_0"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PDR_ON"/>
<pin name="VDD_14" direction="pwr"/>
<pin name="PI4"/>
<pin name="PI5"/>
<pin name="PI6"/>
<pin name="PI7"/>
</symbol>
<symbol name="STM32F4_A">
<pin name="PI2"/>
<pin name="PI3"/>
<pin name="VSS11" direction="pwr"/>
<pin name="VDD11" direction="pwr"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="VSS12" direction="pwr"/>
<pin name="VDD12" direction="pwr"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG11"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="VSS13" direction="pwr"/>
<pin name="VDD13" direction="pwr"/>
<pin name="PG15"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="BOOT_0"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PDR_ON"/>
<pin name="VDD14" direction="pwr"/>
<pin name="PI4"/>
<pin name="PI5"/>
<pin name="PI6"/>
<pin name="PI7"/>
</symbol>
<symbol name="STM32F4_B">
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PI8"/>
<pin name="PC13"/>
<pin name="PC14/OSC32_IN"/>
<pin name="PC15/OSC32_OUT"/>
<pin name="PI9"/>
<pin name="PI10"/>
<pin name="PI11"/>
<pin name="VSS1" direction="pwr"/>
<pin name="VDD1" direction="pwr"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="VSS2" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF10"/>
<pin name="PH0/OSC_IN"/>
<pin name="PH1/OSC_OUT"/>
<pin name="NRST"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="VDDA1" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VDDA2" direction="pwr"/>
<pin name="PA0/WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PH2"/>
<pin name="PH3"/>
</symbol>
<symbol name="STM32F4_C">
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PA3"/>
<pin name="VSS3" direction="pwr"/>
<pin name="VDD3" direction="pwr"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2/BOOT_1"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="VSS4" direction="pwr"/>
<pin name="VDD4" direction="pwr"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PE7"/>
<pin name="PE8"/>
<pin name="PE9"/>
<pin name="VSS5" direction="pwr"/>
<pin name="VDD5" direction="pwr"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="VCAP_1" direction="pwr"/>
<pin name="VDD6" direction="pwr"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PH8"/>
<pin name="PH9"/>
<pin name="PH10"/>
<pin name="PH11"/>
</symbol>
<symbol name="STM32F4_D">
<pin name="PH12"/>
<pin name="VSS7" direction="pwr"/>
<pin name="VDD7" direction="pwr"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="VSS8" direction="pwr"/>
<pin name="VDD8" direction="pwr"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="VSS9" direction="pwr"/>
<pin name="VDD9" direction="pwr"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="VCAP_2" direction="pwr"/>
<pin name="VSS10" direction="pwr"/>
<pin name="VDD10" direction="pwr"/>
<pin name="PH13"/>
<pin name="PH14"/>
<pin name="PH15"/>
<pin name="PI0"/>
<pin name="PI1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="STM32F407_LQFP176" prefix="IC_">
<description>STM32F4xx in LQFP176 Package, 176 Pin
Microcontroller (MCU) ARM Cortex M4  Version 1.0 by E.Guenes</description>
<gates>
<gate name="G$1" symbol="STM32F4_A"/>
<gate name="G$2" symbol="STM32F4_B"/>
<gate name="G$3" symbol="STM32F4_C"/>
<gate name="G$4" symbol="STM32F4_D"/>
</gates>
<devices>
<device name="" package="STM32F407_LQFP176">
<connects>
<connect gate="G$1" pin="BOOT_0" pad="166"/>
<connect gate="G$1" pin="PA14" pad="137"/>
<connect gate="G$1" pin="PA15" pad="138"/>
<connect gate="G$1" pin="PB3" pad="161"/>
<connect gate="G$1" pin="PB4" pad="162"/>
<connect gate="G$1" pin="PB5" pad="163"/>
<connect gate="G$1" pin="PB6" pad="164"/>
<connect gate="G$1" pin="PB7" pad="165"/>
<connect gate="G$1" pin="PB8" pad="167"/>
<connect gate="G$1" pin="PB9" pad="168"/>
<connect gate="G$1" pin="PC10" pad="139"/>
<connect gate="G$1" pin="PC11" pad="140"/>
<connect gate="G$1" pin="PC12" pad="141"/>
<connect gate="G$1" pin="PD0" pad="142"/>
<connect gate="G$1" pin="PD1" pad="143"/>
<connect gate="G$1" pin="PD2" pad="144"/>
<connect gate="G$1" pin="PD3" pad="145"/>
<connect gate="G$1" pin="PD4" pad="146"/>
<connect gate="G$1" pin="PD5" pad="147"/>
<connect gate="G$1" pin="PD6" pad="150"/>
<connect gate="G$1" pin="PD7" pad="151"/>
<connect gate="G$1" pin="PDR_ON" pad="171"/>
<connect gate="G$1" pin="PE0" pad="169"/>
<connect gate="G$1" pin="PE1" pad="170"/>
<connect gate="G$1" pin="PG10" pad="153"/>
<connect gate="G$1" pin="PG11" pad="154"/>
<connect gate="G$1" pin="PG12" pad="155"/>
<connect gate="G$1" pin="PG13" pad="156"/>
<connect gate="G$1" pin="PG14" pad="157"/>
<connect gate="G$1" pin="PG15" pad="160"/>
<connect gate="G$1" pin="PG9" pad="152"/>
<connect gate="G$1" pin="PI2" pad="133"/>
<connect gate="G$1" pin="PI3" pad="134"/>
<connect gate="G$1" pin="PI4" pad="173"/>
<connect gate="G$1" pin="PI5" pad="174"/>
<connect gate="G$1" pin="PI6" pad="175"/>
<connect gate="G$1" pin="PI7" pad="176"/>
<connect gate="G$1" pin="VDD11" pad="136"/>
<connect gate="G$1" pin="VDD12" pad="149"/>
<connect gate="G$1" pin="VDD13" pad="159"/>
<connect gate="G$1" pin="VDD14" pad="172"/>
<connect gate="G$1" pin="VSS11" pad="135"/>
<connect gate="G$1" pin="VSS12" pad="148"/>
<connect gate="G$1" pin="VSS13" pad="158"/>
<connect gate="G$2" pin="NRST" pad="31"/>
<connect gate="G$2" pin="PA0/WKUP" pad="40"/>
<connect gate="G$2" pin="PA1" pad="41"/>
<connect gate="G$2" pin="PA2" pad="42"/>
<connect gate="G$2" pin="PC0" pad="32"/>
<connect gate="G$2" pin="PC1" pad="33"/>
<connect gate="G$2" pin="PC13" pad="8"/>
<connect gate="G$2" pin="PC14/OSC32_IN" pad="9"/>
<connect gate="G$2" pin="PC15/OSC32_OUT" pad="10"/>
<connect gate="G$2" pin="PC2" pad="34"/>
<connect gate="G$2" pin="PC3" pad="35"/>
<connect gate="G$2" pin="PE2" pad="1"/>
<connect gate="G$2" pin="PE3" pad="2"/>
<connect gate="G$2" pin="PE4" pad="3"/>
<connect gate="G$2" pin="PE5" pad="4"/>
<connect gate="G$2" pin="PE6" pad="5"/>
<connect gate="G$2" pin="PF0" pad="16"/>
<connect gate="G$2" pin="PF1" pad="17"/>
<connect gate="G$2" pin="PF10" pad="28"/>
<connect gate="G$2" pin="PF2" pad="18"/>
<connect gate="G$2" pin="PF3" pad="19"/>
<connect gate="G$2" pin="PF4" pad="20"/>
<connect gate="G$2" pin="PF5" pad="21"/>
<connect gate="G$2" pin="PF6" pad="24"/>
<connect gate="G$2" pin="PF7" pad="25"/>
<connect gate="G$2" pin="PF8" pad="26"/>
<connect gate="G$2" pin="PF9" pad="27"/>
<connect gate="G$2" pin="PH0/OSC_IN" pad="29"/>
<connect gate="G$2" pin="PH1/OSC_OUT" pad="30"/>
<connect gate="G$2" pin="PH2" pad="43"/>
<connect gate="G$2" pin="PH3" pad="44"/>
<connect gate="G$2" pin="PI10" pad="12"/>
<connect gate="G$2" pin="PI11" pad="13"/>
<connect gate="G$2" pin="PI8" pad="7"/>
<connect gate="G$2" pin="PI9" pad="11"/>
<connect gate="G$2" pin="VBAT" pad="6"/>
<connect gate="G$2" pin="VDD1" pad="15"/>
<connect gate="G$2" pin="VDD2" pad="23"/>
<connect gate="G$2" pin="VDDA1" pad="36"/>
<connect gate="G$2" pin="VDDA2" pad="39"/>
<connect gate="G$2" pin="VREF+" pad="38"/>
<connect gate="G$2" pin="VSS1" pad="14"/>
<connect gate="G$2" pin="VSS2" pad="22"/>
<connect gate="G$2" pin="VSSA" pad="37"/>
<connect gate="G$3" pin="PA3" pad="47"/>
<connect gate="G$3" pin="PA4" pad="50"/>
<connect gate="G$3" pin="PA5" pad="51"/>
<connect gate="G$3" pin="PA6" pad="52"/>
<connect gate="G$3" pin="PA7" pad="53"/>
<connect gate="G$3" pin="PB0" pad="56"/>
<connect gate="G$3" pin="PB1" pad="57"/>
<connect gate="G$3" pin="PB10" pad="79"/>
<connect gate="G$3" pin="PB11" pad="80"/>
<connect gate="G$3" pin="PB2/BOOT_1" pad="58"/>
<connect gate="G$3" pin="PC4" pad="54"/>
<connect gate="G$3" pin="PC5" pad="55"/>
<connect gate="G$3" pin="PE10" pad="73"/>
<connect gate="G$3" pin="PE11" pad="74"/>
<connect gate="G$3" pin="PE12" pad="75"/>
<connect gate="G$3" pin="PE13" pad="76"/>
<connect gate="G$3" pin="PE14" pad="77"/>
<connect gate="G$3" pin="PE15" pad="78"/>
<connect gate="G$3" pin="PE7" pad="68"/>
<connect gate="G$3" pin="PE8" pad="69"/>
<connect gate="G$3" pin="PE9" pad="70"/>
<connect gate="G$3" pin="PF11" pad="59"/>
<connect gate="G$3" pin="PF12" pad="60"/>
<connect gate="G$3" pin="PF13" pad="63"/>
<connect gate="G$3" pin="PF14" pad="64"/>
<connect gate="G$3" pin="PF15" pad="65"/>
<connect gate="G$3" pin="PG0" pad="66"/>
<connect gate="G$3" pin="PG1" pad="67"/>
<connect gate="G$3" pin="PH10" pad="87"/>
<connect gate="G$3" pin="PH11" pad="88"/>
<connect gate="G$3" pin="PH4" pad="45"/>
<connect gate="G$3" pin="PH5" pad="46"/>
<connect gate="G$3" pin="PH6" pad="83"/>
<connect gate="G$3" pin="PH7" pad="84"/>
<connect gate="G$3" pin="PH8" pad="85"/>
<connect gate="G$3" pin="PH9" pad="86"/>
<connect gate="G$3" pin="VCAP_1" pad="81"/>
<connect gate="G$3" pin="VDD3" pad="49"/>
<connect gate="G$3" pin="VDD4" pad="62"/>
<connect gate="G$3" pin="VDD5" pad="72"/>
<connect gate="G$3" pin="VDD6" pad="82"/>
<connect gate="G$3" pin="VSS3" pad="48"/>
<connect gate="G$3" pin="VSS4" pad="61"/>
<connect gate="G$3" pin="VSS5" pad="71"/>
<connect gate="G$4" pin="PA10" pad="121"/>
<connect gate="G$4" pin="PA11" pad="122"/>
<connect gate="G$4" pin="PA12" pad="123"/>
<connect gate="G$4" pin="PA13" pad="124"/>
<connect gate="G$4" pin="PA8" pad="119"/>
<connect gate="G$4" pin="PA9" pad="120"/>
<connect gate="G$4" pin="PB12" pad="92"/>
<connect gate="G$4" pin="PB13" pad="93"/>
<connect gate="G$4" pin="PB14" pad="94"/>
<connect gate="G$4" pin="PB15" pad="95"/>
<connect gate="G$4" pin="PC6" pad="115"/>
<connect gate="G$4" pin="PC7" pad="116"/>
<connect gate="G$4" pin="PC8" pad="117"/>
<connect gate="G$4" pin="PC9" pad="118"/>
<connect gate="G$4" pin="PD10" pad="98"/>
<connect gate="G$4" pin="PD11" pad="99"/>
<connect gate="G$4" pin="PD12" pad="100"/>
<connect gate="G$4" pin="PD13" pad="101"/>
<connect gate="G$4" pin="PD14" pad="104"/>
<connect gate="G$4" pin="PD15" pad="105"/>
<connect gate="G$4" pin="PD8" pad="96"/>
<connect gate="G$4" pin="PD9" pad="97"/>
<connect gate="G$4" pin="PG2" pad="106"/>
<connect gate="G$4" pin="PG3" pad="107"/>
<connect gate="G$4" pin="PG4" pad="108"/>
<connect gate="G$4" pin="PG5" pad="109"/>
<connect gate="G$4" pin="PG6" pad="110"/>
<connect gate="G$4" pin="PG7" pad="111"/>
<connect gate="G$4" pin="PG8" pad="112"/>
<connect gate="G$4" pin="PH12" pad="89"/>
<connect gate="G$4" pin="PH13" pad="128"/>
<connect gate="G$4" pin="PH14" pad="129"/>
<connect gate="G$4" pin="PH15" pad="130"/>
<connect gate="G$4" pin="PI0" pad="131"/>
<connect gate="G$4" pin="PI1" pad="132"/>
<connect gate="G$4" pin="VCAP_2" pad="125"/>
<connect gate="G$4" pin="VDD10" pad="127"/>
<connect gate="G$4" pin="VDD7" pad="91"/>
<connect gate="G$4" pin="VDD8" pad="103"/>
<connect gate="G$4" pin="VDD9" pad="114"/>
<connect gate="G$4" pin="VSS10" pad="126"/>
<connect gate="G$4" pin="VSS7" pad="90"/>
<connect gate="G$4" pin="VSS8" pad="102"/>
<connect gate="G$4" pin="VSS9" pad="113"/>
</connects>
<technologies>
<technology name="LQFP">
<attribute name="MCU" value="1"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
