<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50" y2="0" width="0" layer="20"/>
<wire x1="50" y1="0" x2="50" y2="18" width="0" layer="20"/>
<wire x1="50" y1="18" x2="0" y2="18" width="0" layer="20"/>
<wire x1="0" y1="18" x2="0" y2="0" width="0" layer="20"/>
<text>FireFly 1.0</text>
<text>BAT+</text>
<text>SOLAR+</text>
<text>SOLAR-</text>
<text>BAT-</text>
</plain>
<libraries>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="max1724">
<packages>
<package name="THIN-SOT23-5">
</package>
</packages>
</library>
<library name="R_C_0805">
<packages>
<package name="SMD1210">
</package>
<package name="0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="SOT23-BEC">
<description>TO-236 ITT Intermetall</description>
</package>
</packages>
</library>
<library name="generisch">
<packages>
<package name="SOT23">
</package>
<package name="TP-3-MM">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC2" library="avr-7" package="SOIC8" value="TINY25/45/85-20SU">
<attribute name="NAME"/>
</element>
<element name="IC1" library="max1724" package="THIN-SOT23-5" value="MAX1724">
<attribute name="NAME"/>
</element>
<element name="L1" library="R_C_0805" package="SMD1210" value="10u / LQH3C 10µ">
<attribute name="NAME"/>
</element>
<element name="C1" library="R_C_0805" package="0805" value="4.7u">
<attribute name="NAME"/>
</element>
<element name="C2" library="R_C_0805" package="0805" value="4.7u">
<attribute name="NAME"/>
</element>
<element name="T1" library="transistor" package="SOT23" value="BC847">
<attribute name="NAME"/>
</element>
<element name="T2" library="generisch" package="SOT23" value="BSS138">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="SOT23" value="BAV70">
<attribute name="NAME"/>
</element>
<element name="T3" library="transistor" package="SOT23-BEC" value="BCW61">
<attribute name="NAME"/>
</element>
<element name="R1" library="R_C_0805" package="0805" value="100">
<attribute name="NAME"/>
</element>
<element name="R2" library="R_C_0805" package="0805" value="100">
<attribute name="NAME"/>
</element>
<element name="R3" library="R_C_0805" package="0805" value="100">
<attribute name="NAME"/>
</element>
<element name="R4" library="R_C_0805" package="0805" value="100">
<attribute name="NAME"/>
</element>
<element name="R5" library="R_C_0805" package="0805" value="330k">
<attribute name="NAME"/>
</element>
<element name="TP1" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
<element name="TP2" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
<element name="TP3" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
<element name="TP4" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
<element name="TP5" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
<element name="TP6" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
<element name="TP7" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
<element name="TP8" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
<element name="TP9" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
<element name="TP10" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
<element name="TP11" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
<element name="TP12" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
<element name="TP13" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
<element name="TP14" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
<element name="TP15" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
<element name="TP16" library="generisch" package="TP-3-MM" value="TP-3-MM"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="4"/>
<contactref element="IC2" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="GND">
<contactref element="IC2" pad="4"/>
<contactref element="T3" pad="C"/>
<contactref element="T1" pad="2"/>
<contactref element="T2" pad="2"/>
<contactref element="TP16" pad="P$1"/>
<contactref element="C2" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="5"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="IC2" pad="5"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="1"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="IC2" pad="7"/>
<contactref element="R5" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R1" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R2" pad="2"/>
<contactref element="TP4" pad="P$1"/>
<contactref element="TP5" pad="P$1"/>
<contactref element="TP6" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="R1" pad="2"/>
<contactref element="TP2" pad="P$1"/>
<contactref element="TP3" pad="P$1"/>
<contactref element="TP1" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="2"/>
<contactref element="TP8" pad="P$1"/>
<contactref element="TP7" pad="P$1"/>
<contactref element="TP9" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="R4" pad="2"/>
<contactref element="TP11" pad="P$1"/>
<contactref element="TP10" pad="P$1"/>
<contactref element="TP12" pad="P$1"/>
</signal>
<signal name="N$14">
<contactref element="T3" pad="E"/>
<contactref element="T1" pad="1"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="T1" pad="3"/>
<contactref element="T2" pad="1"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="T2" pad="3"/>
<contactref element="T3" pad="B"/>
<contactref element="TP13" pad="P$1"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="TP15" pad="P$1"/>
<contactref element="TP14" pad="P$1"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC2" pad="2"/>
<contactref element="D1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
