<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<text>+</text>
<wire x1="0" y1="24" x2="36.8" y2="24" width="0.1" layer="20" style="shortdash"/>
<wire x1="36.8" y1="24" x2="36.8" y2="0" width="0.1" layer="20" style="shortdash"/>
<wire x1="36.8" y1="0" x2="0" y2="0" width="0.1" layer="20" style="shortdash"/>
<wire x1="0" y1="0" x2="0" y2="24" width="0.1" layer="20" style="shortdash"/>
</plain>
<libraries>
<library name="rfm70">
<packages>
<package name="RFM70">
</package>
</packages>
</library>
<library name="atmega8-1">
<description>&lt;b&gt;Atmel ATmega8, ATmega48, ATmega88, ATmega168: 8-bit AVR microcontrollers&lt;/b&gt;
&lt;p&gt;&lt;ul&gt;
&lt;li&gt;ATmega8, ATmega8L:&lt;br&gt;
28-pin PDIP, 32-lead TQFP and 32-pad QFN/MLF
&lt;li&gt;ATmega48, ATmega48V, ATmega88, ATmega88V, ATmega168, ATmega168V:&lt;br&gt;
 28-pin PDIP, 32-lead TQFP and 32-pad QFN/MLF (no 28-pad QFN/MLF!)
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>Spark Fun Electronics' preferred foot prints. &lt;b&gt;Not to be used for commercial purposes.&lt;/b&gt; We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.</description>
<packages>
<package name="0603">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="maxim">
<description>&lt;b&gt;Maxim Components&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="RFM">
<packages>
<package name="SC70-5L">
<description>&lt;b&gt;SC-70 Package&lt;/b&gt;</description>
</package>
<package name="SC70-3L">
<description>&lt;b&gt;SC-70 Package&lt;/b&gt;</description>
</package>
<package name="6-PADS">
</package>
</packages>
</library>
<library name="murata-filter">
<description>&lt;b&gt;Murata Filters&lt;/b&gt;&lt;p&gt;
Distributor RS Components&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CSTCR6M">
<description>Source: http://search.murata.co.jp/Ceramy/CatalogshowpageAction.do?sDirnm=A07X&amp;sFilnm=81G07006&amp;sType=2&amp;sLang=en&amp;sNHinnm=CSTCR6M00G53Z-R0&amp;sCapt=Standard_Land_Pattern_Dimensions</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP13SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SOD-323F">
</package>
<package name="SOD-123">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="rfm70" package="RFM70" value="RFM70"/>
<element name="IC1" library="atmega8-1" package="TQFP32-08" value="ATMEGA48/88/168-AU"/>
<element name="C3" library="SparkFun" package="0603" value="1 µF"/>
<element name="C4" library="SparkFun" package="0603" value="1 µF"/>
<element name="R2" library="SparkFun" package="0603" value="47 kΩ"/>
<element name="IC4" library="maxim" package="SOT23-5L" value="MAX1555">
<attribute name="OC_NEWARK" value="59J2761"/>
<attribute name="MPN" value="MAX1555EZK+T"/>
<attribute name="MF" value="MAXIM"/>
<attribute name="OC_FARNELL" value="1628222"/>
</element>
<element name="C5" library="SparkFun" package="0603" value="1 µF"/>
<element name="IND_1" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254"/>
<element name="IND_MID" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254"/>
<element name="C6" library="SparkFun" package="0603" value="100 nF"/>
<element name="C7" library="SparkFun" package="0603" value="1 µF"/>
<element name="C8" library="SparkFun" package="0603" value="100 nF"/>
<element name="C10" library="SparkFun" package="0603" value="4,7 nF"/>
<element name="Q1" library="murata-filter" package="CSTCR6M" value="CSTCR6M00G53Z">
<attribute name="OC_NEWARK" value="25M8759"/>
<attribute name="MPN" value="CSTCR6M00G53-R0"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1170434"/>
</element>
<element name="U$2" library="RFM" package="SC70-5L" value="TC1016SC70"/>
<element name="U$3" library="RFM" package="SC70-3L" value="MAX_VDECT"/>
<element name="IND_2" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254"/>
<element name="C1" library="SparkFun" package="0603" value="1 µF"/>
<element name="AKKU_VDD" library="testpad" package="TP13SQ" value="VDD">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="AKKU_GND" library="testpad" package="TP13SQ" value="GND">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="C2" library="SparkFun" package="0805" value="6,8 µF"/>
<element name="D1" library="adafruit" package="SOD-323F" value=""/>
<element name="D2" library="adafruit" package="SOD-323F" value=""/>
<element name="D5" library="adafruit" package="SOD-123" value=""/>
<element name="D6" library="adafruit" package="SOD-123" value=""/>
<element name="R3" library="SparkFun" package="0603" value="47 kΩ"/>
<element name="R4" library="SparkFun" package="0603" value="47 kΩ"/>
<element name="R1" library="SparkFun" package="0603" value="47 kΩ"/>
<element name="R5" library="SparkFun" package="0603" value="47 kΩ"/>
<element name="C9" library="SparkFun" package="0603" value="100 nF"/>
<element name="U$4" library="RFM" package="6-PADS" value="6-PADS"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="GND"/>
<contactref element="C3" pad="2"/>
<contactref element="U$1" pad="GND"/>
<contactref element="C4" pad="2"/>
<contactref element="IC4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="C7" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$3" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="C8" pad="2"/>
<contactref element="IC1" pad="21"/>
<contactref element="AKKU_GND" pad="TP"/>
<contactref element="R4" pad="2"/>
<contactref element="IC4" pad="4"/>
<contactref element="IND_MID" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="U$4" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="IC4" pad="5"/>
<contactref element="C4" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="U$2" pad="5"/>
<contactref element="U$3" pad="3"/>
<contactref element="AKKU_VDD" pad="TP"/>
<contactref element="R1" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="18"/>
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="VDD"/>
<contactref element="C8" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="C6" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="6"/>
<contactref element="C3" pad="1"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$4" pad="3"/>
</signal>
<signal name="V+">
<contactref element="R3" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="IC4" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="D6" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="D5" pad="C"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="CE"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="CSN"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="SCK"/>
<contactref element="IC1" pad="17"/>
<contactref element="U$4" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="MOSI"/>
<contactref element="IC1" pad="15"/>
<contactref element="U$4" pad="5"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="MISO"/>
<contactref element="IC1" pad="16"/>
<contactref element="U$4" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="IC1" pad="29"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="N$24">
</signal>
<signal name="N$27">
<contactref element="U$3" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="3"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="1"/>
<contactref element="U$1" pad="IRQ"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="32"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="IC4" pad="3"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="N$14">
<contactref element="IND_2" pad="1"/>
<contactref element="D6" pad="A"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="IND_1" pad="1"/>
<contactref element="D5" pad="A"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="IC1" pad="24"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
