<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="-21" y1="-21" x2="21" y2="-21" width="0" layer="20"/>
<wire x1="21" y1="-21" x2="21" y2="21" width="0" layer="20"/>
<wire x1="21" y1="21" x2="-21" y2="21" width="0" layer="20"/>
<wire x1="-21" y1="21" x2="-21" y2="-21" width="0" layer="20"/>
</plain>
<libraries>
<library name="taster">
<packages>
<package name="MULTIMEC_COMB">
<description>Combined - could be used for through hole and smd</description>
</package>
</packages>
</library>
<library name="pinhead">
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<packages>
<package name="3,2">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.2 mm with drill center</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="UP" library="taster" package="MULTIMEC_COMB" value="MULTIMECTH_COMB">
<attribute name="NAME"/>
</element>
<element name="DOWN" library="taster" package="MULTIMEC_COMB" value="MULTIMECTH_COMB">
<attribute name="NAME"/>
</element>
<element name="ON" library="taster" package="MULTIMEC_COMB" value="MULTIMECTH_COMB">
<attribute name="NAME"/>
</element>
<element name="OFF" library="taster" package="MULTIMEC_COMB" value="MULTIMECTH_COMB">
<attribute name="NAME"/>
</element>
<element name="ENTER" library="taster" package="MULTIMEC_COMB" value="MULTIMECTH_COMB">
<attribute name="NAME"/>
</element>
<element name="JP1" library="pinhead" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
<element name="H2" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
<element name="H3" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
<element name="H4" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="UP" pad="4"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="DOWN" pad="4"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="ON" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="5"/>
<contactref element="OFF" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="6"/>
<contactref element="ENTER" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="UP" pad="2"/>
<contactref element="ENTER" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="DOWN" pad="1"/>
<contactref element="OFF" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="JP1" pad="1"/>
<contactref element="ON" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="DOWN" pad="2"/>
<contactref element="ON" pad="1"/>
<contactref element="ENTER" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
