<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4.4">
<drawing>
<library>
<packages>
<package name="TEST">
</package>
<package name="SOIC16N">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;</description>
</package>
<package name="VERGLEICH">
</package>
</packages>
<symbols>
<symbol name="SI4836-10">
<pin name="LOUT" direction="out"/>
<pin name="TUNE1" direction="pas"/>
<pin name="TUNE2" direction="pas"/>
<pin name="BAND" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="FMI" direction="in"/>
<pin name="RFGND" direction="pwr"/>
<pin name="AMI" direction="in"/>
<pin name="!RST!" direction="in"/>
<pin name="ST/LNA_EN"/>
<pin name="STATION"/>
<pin name="XTALO" direction="out"/>
<pin name="XTALI" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="ROUT" direction="out"/>
</symbol>
<symbol name="TEST">
<pin name="LOUT"/>
<pin name="TUNE1"/>
<pin name="TUNE2"/>
<pin name="BAND"/>
<pin name="NC"/>
<pin name="FMI"/>
<pin name="RFGND"/>
<pin name="AMI"/>
<pin name="RST"/>
<pin name="ST/LNA_EN"/>
<pin name="STATION"/>
<pin name="XTAL0"/>
<pin name="XTAL1"/>
<pin name="VDD"/>
<pin name="GND"/>
<pin name="ROUT"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TEST" prefix="IC">
<gates>
<gate name="G$1" symbol="SI4836-10"/>
</gates>
<devices>
<device name="" package="TEST">
<connects>
<connect gate="G$1" pin="!RST!" pad="9"/>
<connect gate="G$1" pin="AMI" pad="8"/>
<connect gate="G$1" pin="BAND" pad="4"/>
<connect gate="G$1" pin="FMI" pad="6"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="LOUT" pad="1"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="RFGND" pad="7"/>
<connect gate="G$1" pin="ROUT" pad="16"/>
<connect gate="G$1" pin="ST/LNA_EN" pad="10"/>
<connect gate="G$1" pin="STATION" pad="11"/>
<connect gate="G$1" pin="TUNE1" pad="2"/>
<connect gate="G$1" pin="TUNE2" pad="3"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="XTALI" pad="13"/>
<connect gate="G$1" pin="XTALO" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SI4836-10" prefix="IC">
<description>&lt;b&gt;AM/FM/SW RADIORECEIVER&lt;/B&gt;&lt;p&gt;

Worldwide FM band support (64–109 MHz)&lt;br&gt;
Worldwide AM band support (504–1750 kHz)&lt;br&gt;
SW band support (2.3–28.5 MHz)&lt;br&gt;
No manual alignment necessary&lt;br&gt;
Stereo audio output&lt;br&gt;
 Selectable support AM/FM/SW &lt;br&gt;
regional bands&lt;br&gt;
 Enhanced FM/SW band coverage&lt;br&gt;
Station and stereo LED indicators&lt;br&gt;
China TV channels audio carrier reception in FM band&lt;br&gt;
Automatic frequency control (AFC)&lt;br&gt;
Integrated LDO regulator&lt;br&gt;
2.0 to 3.6 V supply voltage &lt;br&gt;
Wide range of ferriteloop sticks and air loop antennas supported&lt;br&gt;
16-pin SOIC &lt;br&gt;
 RoHS-compliant&lt;br&gt;
Bass/Treble control&lt;br&gt;
EN55020 compliant&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="SI4836-10"/>
</gates>
<devices>
<device name="-GS" package="SOIC16N">
<connects>
<connect gate="G$1" pin="!RST!" pad="9"/>
<connect gate="G$1" pin="AMI" pad="8"/>
<connect gate="G$1" pin="BAND" pad="4"/>
<connect gate="G$1" pin="FMI" pad="6"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="LOUT" pad="1"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="RFGND" pad="7"/>
<connect gate="G$1" pin="ROUT" pad="16"/>
<connect gate="G$1" pin="ST/LNA_EN" pad="10"/>
<connect gate="G$1" pin="STATION" pad="11"/>
<connect gate="G$1" pin="TUNE1" pad="2"/>
<connect gate="G$1" pin="TUNE2" pad="3"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="XTALI" pad="13"/>
<connect gate="G$1" pin="XTALO" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
