| Kinetis SDK API Reference Manual 1.0.0-beta Freescale Semiconductor, Inc.

- Introduction
- Related Pages
- API Usage

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- c
- d
- g
- i
- k
- m
- o
- p
- s
- u

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Groups Pages
Here is a list of all documented functions, variables, defines, enums, and typedefs with links to the documentation:

### - k -

- kAdcChannel0 : fsl_adc_hal.h
- kAdcChannel10 : fsl_adc_hal.h
- kAdcChannel11 : fsl_adc_hal.h
- kAdcChannel12 : fsl_adc_hal.h
- kAdcChannel13 : fsl_adc_hal.h
- kAdcChannel14 : fsl_adc_hal.h
- kAdcChannel15 : fsl_adc_hal.h
- kAdcChannel16 : fsl_adc_hal.h
- kAdcChannel17 : fsl_adc_hal.h
- kAdcChannel18 : fsl_adc_hal.h
- kAdcChannel19 : fsl_adc_hal.h
- kAdcChannel2 : fsl_adc_hal.h
- kAdcChannel20 : fsl_adc_hal.h
- kAdcChannel21 : fsl_adc_hal.h
- kAdcChannel22 : fsl_adc_hal.h
- kAdcChannel23 : fsl_adc_hal.h
- kAdcChannel3 : fsl_adc_hal.h
- kAdcChannel4 : fsl_adc_hal.h
- kAdcChannel5 : fsl_adc_hal.h
- kAdcChannel6 : fsl_adc_hal.h
- kAdcChannel7 : fsl_adc_hal.h
- kAdcChannel8 : fsl_adc_hal.h
- kAdcChannel9 : fsl_adc_hal.h
- kAdcChannelBandgap : fsl_adc_hal.h
- kAdcChannelDisable : fsl_adc_hal.h
- kAdcChannell : fsl_adc_hal.h
- kAdcChannelMuxA : fsl_adc_hal.h
- kAdcChannelMuxB : fsl_adc_hal.h
- kAdcChannelReferenceVoltageHigh : fsl_adc_hal.h
- kAdcChannelReferenceVoltageLow : fsl_adc_hal.h
- kAdcChannelTemperature : fsl_adc_hal.h
- kAdcClockDivider1 : fsl_adc_hal.h
- kAdcClockDivider2 : fsl_adc_hal.h
- kAdcClockDivider4 : fsl_adc_hal.h
- kAdcClockDivider8 : fsl_adc_hal.h
- kAdcClockSourceAlternate : fsl_adc_hal.h
- kAdcClockSourceAsynchrounous : fsl_adc_hal.h
- kAdcClockSourceBusClk : fsl_adc_hal.h
- kAdcClockSourceBusClk2 : fsl_adc_hal.h
- kAdcHwAverageCount16 : fsl_adc_hal.h
- kAdcHwAverageCount32 : fsl_adc_hal.h
- kAdcHwAverageCount4 : fsl_adc_hal.h
- kAdcHwAverageCount8 : fsl_adc_hal.h
- kAdcLongSampleExtra12 : fsl_adc_hal.h
- kAdcLongSampleExtra2 : fsl_adc_hal.h
- kAdcLongSampleExtra20 : fsl_adc_hal.h
- kAdcLongSampleExtra6 : fsl_adc_hal.h
- kAdcSingleDiff10or11 : fsl_adc_hal.h
- kAdcSingleDiff12or13 : fsl_adc_hal.h
- kAdcSingleDiff16 : fsl_adc_hal.h
- kAdcSingleDiff8or9 : fsl_adc_hal.h
- kAdcVoltageValt : fsl_adc_hal.h
- kAdcVoltageVref : fsl_adc_hal.h
- kAllowHsrun : fsl_smc_hal.h
- kAllowLls : fsl_smc_hal.h
- kAllowVlls : fsl_smc_hal.h
- kAllowVlp : fsl_smc_hal.h
- kClockManagerNoSuchClockModule : fsl_clock_manager.h
- kClockManagerNoSuchClockName : fsl_clock_manager.h
- kClockManagerNoSuchClockSource : fsl_clock_manager.h
- kClockManagerNoSuchDivider : fsl_clock_manager.h
- kClockManagerSuccess : fsl_clock_manager.h
- kClockManagerUnknown : fsl_clock_manager.h
- kClockModuleNameSimMap : fsl_clock_manager_private.h
- kClockNameSimMap : fsl_clock_manager_private.h
- kClockSourceNameSimMap : fsl_clock_manager_private.h
- kClockSourceValueTable : fsl_sim_hal.h
- kDspiClockPhase_FirstEdge : fsl_dspi_hal.h
- kDspiClockPhase_SecondEdge : fsl_dspi_hal.h
- kDspiClockPolarity_ActiveHigh : fsl_dspi_hal.h
- kDspiClockPolarity_ActiveLow : fsl_dspi_hal.h
- kDspiCtar0 : fsl_dspi_hal.h
- kDspiCtar1 : fsl_dspi_hal.h
- kDspiEndOfQueue : fsl_dspi_hal.h
- kDspiLsbFirst : fsl_dspi_hal.h
- kDspiMaster : fsl_dspi_hal.h
- kDspiMsbFirst : fsl_dspi_hal.h
- kDspiPcs0 : fsl_dspi_hal.h
- kDspiPcs1 : fsl_dspi_hal.h
- kDspiPcs2 : fsl_dspi_hal.h
- kDspiPcs3 : fsl_dspi_hal.h
- kDspiPcs4 : fsl_dspi_hal.h
- kDspiPcs5 : fsl_dspi_hal.h
- kDspiPcs_ActiveHigh : fsl_dspi_hal.h
- kDspiPcs_ActiveLow : fsl_dspi_hal.h
- kDspiRxFifo : fsl_dspi_hal.h
- kDspiRxFifoCounter : fsl_dspi_hal.h
- kDspiRxFifoDrainRequest : fsl_dspi_hal.h
- kDspiRxFifoOverflow : fsl_dspi_hal.h
- kDspiRxFifoPointer : fsl_dspi_hal.h
- kDspiSckToSin_0Clock : fsl_dspi_hal.h
- kDspiSckToSin_1Clock : fsl_dspi_hal.h
- kDspiSckToSin_2Clock : fsl_dspi_hal.h
- kDspiSlave : fsl_dspi_hal.h
- kDspiTxAndRxStatus : fsl_dspi_hal.h
- kDspiTxComplete : fsl_dspi_hal.h
- kDspiTxFifo : fsl_dspi_hal.h
- kDspiTxFifoCounter : fsl_dspi_hal.h
- kDspiTxFifoFillRequest : fsl_dspi_hal.h
- kDspiTxFifoPointer : fsl_dspi_hal.h
- kDspiTxFifoUnderflow : fsl_dspi_hal.h
- kGpioDigitalInput : fsl_gpio_hal.h
- kGpioDigitalOutput : fsl_gpio_hal.h
- kOsc0 : fsl_osc_hal.h
- kOscCapacitor16p : fsl_osc_hal.h
- kOscCapacitor2p : fsl_osc_hal.h
- kOscCapacitor4p : fsl_osc_hal.h
- kOscCapacitor8p : fsl_osc_hal.h
- kOscCapacitorMask : fsl_osc_hal.h
- kPmcLvdvHighTrip : fsl_pmc_hal.h
- kPmcLvdvLowTrip : fsl_pmc_hal.h
- kPmcLvwvHighTrip : fsl_pmc_hal.h
- kPmcLvwvLowTrip : fsl_pmc_hal.h
- kPmcLvwvMid1Trip : fsl_pmc_hal.h
- kPmcLvwvMid2Trip : fsl_pmc_hal.h
- kSaiBclkSourceBusclk : fsl_sai_hal.h
- kSaiBclkSourceMclkDiv : fsl_sai_hal.h
- kSaiBclkSourceOtherSai0 : fsl_sai_hal.h
- kSaiBclkSourceOtherSai1 : fsl_sai_hal.h
- kSaiBusI2SLeft : fsl_sai_hal.h
- kSaiBusI2SRight : fsl_sai_hal.h
- kSaiBusI2SType : fsl_sai_hal.h
- kSaiDmaReqFIFORequest : fsl_sai_hal.h
- kSaiDmaReqFIFOWarning : fsl_sai_hal.h
- kSaiIntrequestFIFOError : fsl_sai_hal.h
- kSaiIntrequestFIFORequest : fsl_sai_hal.h
- kSaiIntrequestFIFOWarning : fsl_sai_hal.h
- kSaiIntrequestSyncError : fsl_sai_hal.h
- kSaiIntrequestWordStart : fsl_sai_hal.h
- kSaiIOModeDuplex : fsl_sai_hal.h
- kSaiIOModeReceive : fsl_sai_hal.h
- kSaiIOModeTransmit : fsl_sai_hal.h
- kSaiMaster : fsl_sai_hal.h
- kSaiMclkSourceAltclk : fsl_sai_hal.h
- kSaiMclkSourceExtal : fsl_sai_hal.h
- kSaiMclkSourcePllout : fsl_sai_hal.h
- kSaiMclkSourceSysclk : fsl_sai_hal.h
- kSaiModeAsync : fsl_sai_hal.h
- kSaiModeSync : fsl_sai_hal.h
- kSaiModeSyncWithOtherRx : fsl_sai_hal.h
- kSaiModeSyncWithOtherTx : fsl_sai_hal.h
- kSaiResetTypeFIFO : fsl_sai_hal.h
- kSaiResetTypeSoftware : fsl_sai_hal.h
- kSaiRunModeDebug : fsl_sai_hal.h
- kSaiRunModeStop : fsl_sai_hal.h
- kSaiSlave : fsl_sai_hal.h
- kSaiStateFlagFIFOError : fsl_sai_hal.h
- kSaiStateFlagSoftReset : fsl_sai_hal.h
- kSaiStateFlagSyncError : fsl_sai_hal.h
- kSaiStateFlagWordStart : fsl_sai_hal.h
- kSimClockGateModuleConfigTable : fsl_sim_hal.h
- kSimClockNameConfigTable : fsl_sim_hal.h
- kSmcHsrun : fsl_smc_hal.h
- kSmcLls : fsl_smc_hal.h
- kSmcLpoDisabled : fsl_smc_hal.h
- kSmcLpoEnabled : fsl_smc_hal.h
- kSmcLpwuiDisabled : fsl_smc_hal.h
- kSmcLpwuiEnabled : fsl_smc_hal.h
- kSmcManagerAlreadyInTheState : fsl_smc_manager.h
- kSmcManagerFailed : fsl_smc_manager.h
- kSmcManagerNoSuchModeName : fsl_smc_manager.h
- kSmcManagerSuccess : fsl_smc_manager.h
- kSmcOptionLpwui : fsl_smc_hal.h
- kSmcOptionPropo : fsl_smc_hal.h
- kSmcPorDisabled : fsl_smc_hal.h
- kSmcPorEnabled : fsl_smc_hal.h
- kSmcPstopStop : fsl_smc_hal.h
- kSmcPstopStop1 : fsl_smc_hal.h
- kSmcPstopStop2 : fsl_smc_hal.h
- kSmcReservedStop1 : fsl_smc_hal.h
- kSmcRun : fsl_smc_hal.h
- kSmcStop : fsl_smc_hal.h
- kSmcVlls : fsl_smc_hal.h
- kSmcVlpr : fsl_smc_hal.h
- kSmcVlps : fsl_smc_hal.h
- kSpiClockPhase_FirstEdge : fsl_spi_hal.h
- kSpiClockPhase_SecondEdge : fsl_spi_hal.h
- kSpiClockPolarity_ActiveHigh : fsl_spi_hal.h
- kSpiClockPolarity_ActiveLow : fsl_spi_hal.h
- kSpiLsbFirst : fsl_spi_hal.h
- kSpiMaster : fsl_spi_hal.h
- kSpiMsbFirst : fsl_spi_hal.h
- kSpiPinMode_Input : fsl_spi_hal.h
- kSpiPinMode_Normal : fsl_spi_hal.h
- kSpiPinMode_Output : fsl_spi_hal.h
- kSpiSlave : fsl_spi_hal.h
- kSpiSlaveSelect_AsGpio : fsl_spi_hal.h
- kSpiSlaveSelect_AutomaticOutput : fsl_spi_hal.h
- kSpiSlaveSelect_FaultInput : fsl_spi_hal.h
- kStatHsrun : fsl_smc_hal.h
- kStatLls : fsl_smc_hal.h
- kStatRun : fsl_smc_hal.h
- kStatStop : fsl_smc_hal.h
- kStatus_ADC_Failed : fsl_adc_hal.h
- kStatus_ADC_InvalidArgument : fsl_adc_hal.h
- kStatus_DSPI_Busy : fsl_dspi_hal.h
- kStatus_DSPI_InvalidBitCount : fsl_dspi_hal.h
- kStatus_DSPI_InvalidInstanceNumber : fsl_dspi_hal.h
- kStatus_DSPI_NoTransferInProgress : fsl_dspi_hal.h
- kStatus_DSPI_SlaveRxOverrun : fsl_dspi_hal.h
- kStatus_DSPI_SlaveTxUnderrun : fsl_dspi_hal.h
- kStatus_DSPI_Timeout : fsl_dspi_hal.h
- kStatus_SND_BufferAllocateFail : fsl_soundcard.h
- kStatus_SND_CodecFail : fsl_soundcard.h
- kStatus_SND_CtrlFail : fsl_soundcard.h
- kStatus_SND_DmaFail : fsl_soundcard.h
- kStatus_SND_Fail : fsl_soundcard.h
- kStatus_SND_Success : fsl_soundcard.h
- kStatus_SPI_Busy : fsl_spi_hal.h
- kStatus_SPI_NoTransferInProgress : fsl_spi_hal.h
- kStatus_SPI_SlaveRxOverrun : fsl_spi_hal.h
- kStatus_SPI_SlaveTxUnderrun : fsl_spi_hal.h
- kStatus_SPI_Timeout : fsl_spi_hal.h
- kStatus_UART_BaudRateCalculationError : fsl_uart_hal.h
- kStatus_UART_BaudRatePercentDiffExceeded : fsl_uart_hal.h
- kStatus_UART_BitCountNotSupported : fsl_uart_hal.h
- kStatus_UART_BothEdgeNotSupported : fsl_uart_hal.h
- kStatus_UART_ClearStatusFlagError : fsl_uart_hal.h
- kStatus_UART_InvalidBitSetting : fsl_uart_hal.h
- kStatus_UART_InvalidInstanceNumber : fsl_uart_hal.h
- kStatus_UART_MSBFirstNotSupported : fsl_uart_hal.h
- kStatus_UART_NoReceiveInProgress : fsl_uart_hal.h
- kStatus_UART_NoTransmitInProgress : fsl_uart_hal.h
- kStatus_UART_OverSamplingNotSupported : fsl_uart_hal.h
- kStatus_UART_ResyncNotSupported : fsl_uart_hal.h
- kStatus_UART_RxBusy : fsl_uart_hal.h
- kStatus_UART_RxNotDisabled : fsl_uart_hal.h
- kStatus_UART_RxStandbyModeError : fsl_uart_hal.h
- kStatus_UART_StopBitCountNotSupported : fsl_uart_hal.h
- kStatus_UART_Timeout : fsl_uart_hal.h
- kStatus_UART_TxBusy : fsl_uart_hal.h
- kStatus_UART_TxNotDisabled : fsl_uart_hal.h
- kStatus_UART_TxOrRxNotDisabled : fsl_uart_hal.h
- kStatVlls : fsl_smc_hal.h
- kStatVlpr : fsl_smc_hal.h
- kStatVlps : fsl_smc_hal.h
- kStatVlpw : fsl_smc_hal.h
- kUart10BitsPerChar : fsl_uart_hal.h
- kUart8BitsPerChar : fsl_uart_hal.h
- kUart9BitsPerChar : fsl_uart_hal.h
- kUartAddrMarkWake : fsl_uart_hal.h
- kUartBreakChar10BitMinimum : fsl_uart_hal.h
- kUartBreakChar13BitMinimum : fsl_uart_hal.h
- kUartFrameError : fsl_uart_hal.h
- kUartIdleLineAfterStartBit : fsl_uart_hal.h
- kUartIdleLineAfterStopBit : fsl_uart_hal.h
- kUartIdleLineDetect : fsl_uart_hal.h
- kUartIdleLineWake : fsl_uart_hal.h
- kUartIrOneFourthWidth : fsl_uart_hal.h
- kUartIrOneSixteenthWidth : fsl_uart_hal.h
- kUartIrOneThirtysecondsWidth : fsl_uart_hal.h
- kUartIrThreeSixteenthsWidth : fsl_uart_hal.h
- kUartLineBreakDetect : fsl_uart_hal.h
- kUartNoiseDetect : fsl_uart_hal.h
- kUartOneStopBit : fsl_uart_hal.h
- kUartOperates : fsl_uart_hal.h
- kUartParityDisabled : fsl_uart_hal.h
- kUartParityError : fsl_uart_hal.h
- kUartParityEven : fsl_uart_hal.h
- kUartParityOdd : fsl_uart_hal.h
- kUartReceiveActiveEdgeDetect : fsl_uart_hal.h
- kUartReceiveDataRegisterFull : fsl_uart_hal.h
- kUartReceiveOverrun : fsl_uart_hal.h
- kUartReceiverActive : fsl_uart_hal.h
- kUartSinglewireTxdirIn : fsl_uart_hal.h
- kUartSinglewireTxdirOut : fsl_uart_hal.h
- kUartStops : fsl_uart_hal.h
- kUartTransmissionComplete : fsl_uart_hal.h
- kUartTransmitDataRegisterEmpty : fsl_uart_hal.h
- kUartTwoStopBit : fsl_uart_hal.h