| Kinetis SDK API Reference Manual 1.0.0-beta Freescale Semiconductor, Inc.

- Introduction
- Related Pages
- API Usage

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- c
- d
- g
- i
- k
- m
- o
- p
- s
- u

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Groups Pages
Here is a list of all documented functions, variables, defines, enums, and typedefs with links to the documentation:

### - u -

- uart_bit_count_per_char_t : fsl_uart_hal.h
- uart_break_char_length_t : fsl_uart_hal.h
- uart_hal_clear_all_non_autoclear_status_flags() : fsl_uart_hal.h
- uart_hal_clear_status_flag() : fsl_uart_hal.h
- uart_hal_configure_bit_count_per_char() : fsl_uart_hal.h
- uart_hal_configure_dma() : fsl_uart_hal.h
- uart_hal_configure_idle_line_detect() : fsl_uart_hal.h
- uart_hal_configure_interrupts() : fsl_uart_hal.h
- uart_hal_configure_loopback_mode() : fsl_uart_hal.h
- uart_hal_configure_match_address_operation() : fsl_uart_hal.h
- uart_hal_configure_parity_mode() : fsl_uart_hal.h
- uart_hal_configure_receive_resync_disable_operation() : fsl_uart_hal.h
- uart_hal_configure_send_msb_first_operation() : fsl_uart_hal.h
- uart_hal_configure_singlewire_mode() : fsl_uart_hal.h
- uart_hal_configure_stop_bit_count() : fsl_uart_hal.h
- uart_hal_configure_tx_rx_inversion() : fsl_uart_hal.h
- uart_hal_configure_txdir_in_singlewire_mode() : fsl_uart_hal.h
- uart_hal_configure_wait_mode_operation() : fsl_uart_hal.h
- uart_hal_disable_break_detect_interrupt() : fsl_uart_hal.h
- uart_hal_disable_framing_error_interrupt() : fsl_uart_hal.h
- uart_hal_disable_idle_line_interrupt() : fsl_uart_hal.h
- uart_hal_disable_noise_error_interrupt() : fsl_uart_hal.h
- uart_hal_disable_parity_error_interrupt() : fsl_uart_hal.h
- uart_hal_disable_receiver() : fsl_uart_hal.h
- uart_hal_disable_rx_active_edge_interrupt() : fsl_uart_hal.h
- uart_hal_disable_rx_data_register_full_interrupt() : fsl_uart_hal.h
- uart_hal_disable_rx_overrun_interrupt() : fsl_uart_hal.h
- uart_hal_disable_transmission_complete_interrupt() : fsl_uart_hal.h
- uart_hal_disable_transmitter() : fsl_uart_hal.h
- uart_hal_disable_tx_data_register_empty_interrupt() : fsl_uart_hal.h
- uart_hal_enable_break_detect_interrupt() : fsl_uart_hal.h
- uart_hal_enable_framing_error_interrupt() : fsl_uart_hal.h
- uart_hal_enable_idle_line_interrupt() : fsl_uart_hal.h
- uart_hal_enable_noise_error_interrupt() : fsl_uart_hal.h
- uart_hal_enable_parity_error_interrupt() : fsl_uart_hal.h
- uart_hal_enable_receiver() : fsl_uart_hal.h
- uart_hal_enable_rx_active_edge_interrupt() : fsl_uart_hal.h
- uart_hal_enable_rx_data_register_full_interrupt() : fsl_uart_hal.h
- uart_hal_enable_rx_overrun_interrupt() : fsl_uart_hal.h
- uart_hal_enable_transmission_complete_interrupt() : fsl_uart_hal.h
- uart_hal_enable_transmitter() : fsl_uart_hal.h
- uart_hal_enable_tx_data_register_empty_interrupt() : fsl_uart_hal.h
- uart_hal_get_all_status_flag() : fsl_uart_hal.h
- uart_hal_get_receiver_wakeup_method() : fsl_uart_hal.h
- uart_hal_get_wait_mode_operation_config() : fsl_uart_hal.h
- uart_hal_getchar() : fsl_uart_hal.h
- uart_hal_getchar10() : fsl_uart_hal.h
- uart_hal_getchar9() : fsl_uart_hal.h
- uart_hal_init() : fsl_uart_hal.h
- uart_hal_is_break_detect_interrupt_enabled() : fsl_uart_hal.h
- uart_hal_is_frame_error_detected() : fsl_uart_hal.h
- uart_hal_is_framing_error_interrupt_enabled() : fsl_uart_hal.h
- uart_hal_is_idle_line_detected() : fsl_uart_hal.h
- uart_hal_is_idle_line_interrupt_enabled() : fsl_uart_hal.h
- uart_hal_is_line_break_detected() : fsl_uart_hal.h
- uart_hal_is_noise_detected() : fsl_uart_hal.h
- uart_hal_is_noise_error_interrupt_enabled() : fsl_uart_hal.h
- uart_hal_is_parity_error_detected() : fsl_uart_hal.h
- uart_hal_is_parity_error_interrupt_enabled() : fsl_uart_hal.h
- uart_hal_is_receive_active_edge_detected() : fsl_uart_hal.h
- uart_hal_is_receive_data_full_interrupt_enabled() : fsl_uart_hal.h
- uart_hal_is_receive_data_register_full() : fsl_uart_hal.h
- uart_hal_is_receive_overrun_detected() : fsl_uart_hal.h
- uart_hal_is_receiver_active() : fsl_uart_hal.h
- uart_hal_is_receiver_enabled() : fsl_uart_hal.h
- uart_hal_is_receiver_in_standby() : fsl_uart_hal.h
- uart_hal_is_rx_active_edge_interrupt_enabled() : fsl_uart_hal.h
- uart_hal_is_rx_overrun_interrupt_enabled() : fsl_uart_hal.h
- uart_hal_is_rxdma_enabled() : fsl_uart_hal.h
- uart_hal_is_transmission_complete() : fsl_uart_hal.h
- uart_hal_is_transmission_complete_interrupt_enabled() : fsl_uart_hal.h
- uart_hal_is_transmit_data_register_empty() : fsl_uart_hal.h
- uart_hal_is_transmitter_enabled() : fsl_uart_hal.h
- uart_hal_is_tx_data_register_empty_interrupt_enabled() : fsl_uart_hal.h
- uart_hal_is_txdma_enabled() : fsl_uart_hal.h
- uart_hal_put_receiver_in_normal_mode() : fsl_uart_hal.h
- uart_hal_put_receiver_in_standby_mode() : fsl_uart_hal.h
- uart_hal_putchar() : fsl_uart_hal.h
- uart_hal_putchar10() : fsl_uart_hal.h
- uart_hal_putchar9() : fsl_uart_hal.h
- uart_hal_queue_break_char_to_send() : fsl_uart_hal.h
- uart_hal_select_receiver_wakeup_method() : fsl_uart_hal.h
- uart_hal_set_baud_rate() : fsl_uart_hal.h
- uart_hal_set_baud_rate_divisor() : fsl_uart_hal.h
- uart_hal_set_break_char_detect_length() : fsl_uart_hal.h
- uart_hal_set_break_char_transmit_length() : fsl_uart_hal.h
- uart_idle_line_select_t : fsl_uart_hal.h
- uart_ir_tx_pulsewidth_t : fsl_uart_hal.h
- uart_operation_config_t : fsl_uart_hal.h
- uart_parity_mode_t : fsl_uart_hal.h
- uart_singlewire_txdir_t : fsl_uart_hal.h
- uart_status_flag_t : fsl_uart_hal.h
- uart_status_t : fsl_uart_hal.h
- uart_stop_bit_count_t : fsl_uart_hal.h
- uart_wakeup_method_t : fsl_uart_hal.h
- USEDMA : fsl_sai_driver.h