| Kinetis SDK API Reference Manual 1.0.0-beta Freescale Semiconductor, Inc.

- Introduction
- Related Pages
- API Usage

- Data Structures
- Data Fields

- All
- Variables

- a
- b
- c
- d
- e
- f
- g
- h
- i
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- y

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Groups Pages
Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - b -

- bandwidthControl : edma_tcd_control_t
- baudRate : lpuart_user_config_t , uart_user_config_t , uart_config_t , lpuart_config_t
- baudRate_kbps : i2c_device_t , i2c_config_t
- baudRateDivisor : dspi_baud_rate_divisors_t
- bclk_source : sai_user_config_t
- bit_rate : flexcan_bitrate_table_t
- bitCountPerChar : lpuart_user_config_t , lpuart_config_t , uart_user_config_t , uart_config_t
- bits : sai_data_format_t
- bitsPerFrame : dspi_master_state_t , dspi_slave_state_t , dspi_data_format_config_t
- bitsPerSec : dspi_device_t , dspi_master_config_t
- blockCount : sdhc_data_t
- blocks : audio_buffer_t
- blockSize : sdhc_data_t
- buff : audio_buffer_t
- buffer : enet_bd_struct_t , sound_card_t , sdhc_data_t
- buffer_error : audio_buffer_t
- bufferdescSize : enet_mac_context_t
- bus_type : sai_user_config_t
- busMode : sdhc_card_t
- busWidth : sdhc_user_config_t , sdhc_host_config_t , sdhc_host_t
- bytesTransferred : sdhc_data_t