| Kinetis SDK API Reference Manual 1.0.0-beta Freescale Semiconductor, Inc.

- Introduction
- Related Pages
- API Usage

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- c
- d
- g
- i
- k
- m
- o
- p
- s
- u

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Groups Pages
Here is a list of all documented functions, variables, defines, enums, and typedefs with links to the documentation:

### - g -

- gpio_clear_pin_interrupt_flag() : fsl_gpio_driver.h
- gpio_clear_pin_output() : fsl_gpio_driver.h
- GPIO_EXTRACT_PIN : fsl_gpio_driver.h
- GPIO_EXTRACT_PORT : fsl_gpio_driver.h
- gpio_get_pin_direction() : fsl_gpio_driver.h
- gpio_hal_clear_pin_output() : fsl_gpio_hal.h
- gpio_hal_get_pin_direction() : fsl_gpio_hal.h
- gpio_hal_get_port_direction() : fsl_gpio_hal.h
- gpio_hal_read_pin_input() : fsl_gpio_hal.h
- gpio_hal_read_pin_output() : fsl_gpio_hal.h
- gpio_hal_read_port_input() : fsl_gpio_hal.h
- gpio_hal_read_port_output() : fsl_gpio_hal.h
- gpio_hal_set_pin_direction() : fsl_gpio_hal.h
- gpio_hal_set_pin_output() : fsl_gpio_hal.h
- gpio_hal_set_port_direction() : fsl_gpio_hal.h
- gpio_hal_toggle_pin_output() : fsl_gpio_hal.h
- gpio_hal_write_pin_output() : fsl_gpio_hal.h
- gpio_hal_write_port_output() : fsl_gpio_hal.h
- gpio_init() : fsl_gpio_driver.h
- gpio_input_pin_init() : fsl_gpio_driver.h
- gpio_isr_callback_t : fsl_gpio_driver.h
- GPIO_MAKE_PIN : fsl_gpio_driver.h
- gpio_output_pin_init() : fsl_gpio_driver.h
- gpio_pin_direction_t : fsl_gpio_hal.h
- GPIO_PINS_OUT_OF_RANGE : fsl_gpio_driver.h
- GPIO_PORT_SHIFT : fsl_gpio_driver.h
- gpio_read_pin_input() : fsl_gpio_driver.h
- gpio_register_isr_callback_function() : fsl_gpio_driver.h
- gpio_set_pin_direction() : fsl_gpio_driver.h
- gpio_set_pin_output() : fsl_gpio_driver.h
- gpio_toggle_pin_output() : fsl_gpio_driver.h
- gpio_write_pin_output() : fsl_gpio_driver.h