| Kinetis SDK Demo Applications User Guide 1.0.0-beta Freescale Semiconductor, Inc.

- Main Page
- Related Pages
- Demos

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Lowe Power Demo Introduction
Low Power Demo

Introduction of the low power demo application. More...

### Low Power Demo Introduction

# Overview

This is a low power demo application which demonstate different low power modes supported in the Kinetis SoCs - those are WAIT, STOP, VLPR, VLPW, VLPS, LLS, VLLS. There is sequence to be followed to enter/exit each mode, and functionality availabile in different power modes are different. Application demonstrates multiple mode entry/exit cases as per the functionality availability.

# Supported Hardware

- FRDM-K64F120M (OpenSDA/TWR-SER as debug UART, SW1 and SW3 as wakeup sources)
- TWR-K64F120M (OpenSDA/TWR-SER as debug UART, SW2 and SW3 as wakeup sources)

# Default Debug Console

- UART instance: OpenSDA CDC/RS-232 serial cable connected to TWR-SER
- Baudrate: 19200bps

# Execution instruction

There are many demo cases listed out of reset in the serial console. Upon selection, further actions are either requested or execution o/p is printed on console. The user needs to follow them in order to get the desired output.