| Kinetis SDK Demo Applications User Guide 1.0.0-beta Freescale Semiconductor, Inc.

- Main Page
- Related Pages
- Demos

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
FlexCAN Demo Introduction
FlexCAN Demo

Introduction and the function/definition comments of this demo. More...

### FlexCAN Demo Introduction

# Overview

UART to FlexCAN project is a simple demonstration program based on KSDK peripheral drivers. It provides a way to demonstrate the performance of FlexCAN and UART peripheral drivers and use asynchronous send and receive functions to create a bridge between UART and FlexCAN. The features include:

1. UART send and receive support
2. Timeout supported by PIT0
3. FlexCAN transfer and receive configure support
4. FlexCAN send and receive support

# Supported platforms

So far this project has been supported on platforms listed as below:

     TWR-K64F120M

# Function Description

These are the five functions which are defined in main.c
The prototypes for these functions are:
void init_hardware(void);
int printf(const char *format,...);
int scanf(const char *format,...);
void PIT0_IRQHandler(void);
void main(void);

See the main.c file for more details.