<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<packages>
<package name="RASPBERRY_PI_BPLUS_TPLACE">
</package>
<package name="RASPBERRY_PI_BPLUS_DIM">
</package>
</packages>
<symbols>
<symbol name="RASPBERRY_PI_B+">
<pin name="5V0@1" direction="pwr"/>
<pin name="3V3@1" direction="pwr"/>
<pin name="GPIO02/SDA1"/>
<pin name="5V0@2" direction="pwr"/>
<pin name="GPIO03/SCL1"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GPIO04/GCKL"/>
<pin name="TXD0/GPIO14"/>
<pin name="GND@1" direction="pwr"/>
<pin name="RXD0/GPIO15"/>
<pin name="GPIO17/GEN0"/>
<pin name="GPIO18"/>
<pin name="GPIO27/GEN2"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GPIO22/GEN3"/>
<pin name="GEN4/GPIO23"/>
<pin name="3V3@2" direction="pwr"/>
<pin name="GEN5/GPIO24"/>
<pin name="GPIO10/MOSI"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GPIO09/MISO"/>
<pin name="GEN6/GPIO25"/>
<pin name="GPIO11/SCLK"/>
<pin name="!CE0!/GPIO08"/>
<pin name="GND@2" direction="pwr"/>
<pin name="!CE!/GPIO07"/>
<pin name="ID_SD"/>
<pin name="ID_SC"/>
<pin name="GPIO05"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GPIO06"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GPIO19"/>
<pin name="GPIO16"/>
<pin name="GPIO26"/>
<pin name="GPIO20"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GPIO21"/>
<pin name="TL"/>
<pin name="TR"/>
<pin name="BL"/>
<pin name="BR"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RASPBERRY_PI_B+" prefix="PCB">
<description>&lt;b&gt;Raspberry Pi B+&lt;/b&gt;&lt;br&gt;
Basedon issue: Thursday, July 10, 2014 - Rev 1.2&lt;p&gt;
LBR by Tim Rettmann 07-2014</description>
<gates>
<gate name="G$1" symbol="RASPBERRY_PI_B+"/>
</gates>
<devices>
<device name="_TPLACE" package="RASPBERRY_PI_BPLUS_TPLACE">
<connects>
<connect gate="G$1" pin="!CE!/GPIO07" pad="26"/>
<connect gate="G$1" pin="!CE0!/GPIO08" pad="24"/>
<connect gate="G$1" pin="3V3@1" pad="1"/>
<connect gate="G$1" pin="3V3@2" pad="17"/>
<connect gate="G$1" pin="5V0@1" pad="2"/>
<connect gate="G$1" pin="5V0@2" pad="4"/>
<connect gate="G$1" pin="BL" pad="PE_BL"/>
<connect gate="G$1" pin="BR" pad="PE_BR"/>
<connect gate="G$1" pin="GEN4/GPIO23" pad="16"/>
<connect gate="G$1" pin="GEN5/GPIO24" pad="18"/>
<connect gate="G$1" pin="GEN6/GPIO25" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="GND@4" pad="14"/>
<connect gate="G$1" pin="GND@5" pad="20"/>
<connect gate="G$1" pin="GND@6" pad="30"/>
<connect gate="G$1" pin="GND@7" pad="34"/>
<connect gate="G$1" pin="GND@8" pad="6"/>
<connect gate="G$1" pin="GPIO02/SDA1" pad="3"/>
<connect gate="G$1" pin="GPIO03/SCL1" pad="5"/>
<connect gate="G$1" pin="GPIO04/GCKL" pad="7"/>
<connect gate="G$1" pin="GPIO05" pad="29"/>
<connect gate="G$1" pin="GPIO06" pad="31"/>
<connect gate="G$1" pin="GPIO09/MISO" pad="21"/>
<connect gate="G$1" pin="GPIO10/MOSI" pad="19"/>
<connect gate="G$1" pin="GPIO11/SCLK" pad="23"/>
<connect gate="G$1" pin="GPIO12" pad="32"/>
<connect gate="G$1" pin="GPIO13" pad="33"/>
<connect gate="G$1" pin="GPIO16" pad="36"/>
<connect gate="G$1" pin="GPIO17/GEN0" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO19" pad="35"/>
<connect gate="G$1" pin="GPIO20" pad="38"/>
<connect gate="G$1" pin="GPIO21" pad="40"/>
<connect gate="G$1" pin="GPIO22/GEN3" pad="15"/>
<connect gate="G$1" pin="GPIO26" pad="37"/>
<connect gate="G$1" pin="GPIO27/GEN2" pad="13"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="RXD0/GPIO15" pad="10"/>
<connect gate="G$1" pin="TL" pad="PE_TL"/>
<connect gate="G$1" pin="TR" pad="PE_TR"/>
<connect gate="G$1" pin="TXD0/GPIO14" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_DIM" package="RASPBERRY_PI_BPLUS_DIM">
<connects>
<connect gate="G$1" pin="!CE!/GPIO07" pad="26"/>
<connect gate="G$1" pin="!CE0!/GPIO08" pad="24"/>
<connect gate="G$1" pin="3V3@1" pad="1"/>
<connect gate="G$1" pin="3V3@2" pad="17"/>
<connect gate="G$1" pin="5V0@1" pad="2"/>
<connect gate="G$1" pin="5V0@2" pad="4"/>
<connect gate="G$1" pin="BL" pad="PE_BL"/>
<connect gate="G$1" pin="BR" pad="PE_BR"/>
<connect gate="G$1" pin="GEN4/GPIO23" pad="16"/>
<connect gate="G$1" pin="GEN5/GPIO24" pad="18"/>
<connect gate="G$1" pin="GEN6/GPIO25" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="GND@4" pad="14"/>
<connect gate="G$1" pin="GND@5" pad="20"/>
<connect gate="G$1" pin="GND@6" pad="30"/>
<connect gate="G$1" pin="GND@7" pad="34"/>
<connect gate="G$1" pin="GND@8" pad="6"/>
<connect gate="G$1" pin="GPIO02/SDA1" pad="3"/>
<connect gate="G$1" pin="GPIO03/SCL1" pad="5"/>
<connect gate="G$1" pin="GPIO04/GCKL" pad="7"/>
<connect gate="G$1" pin="GPIO05" pad="29"/>
<connect gate="G$1" pin="GPIO06" pad="31"/>
<connect gate="G$1" pin="GPIO09/MISO" pad="21"/>
<connect gate="G$1" pin="GPIO10/MOSI" pad="19"/>
<connect gate="G$1" pin="GPIO11/SCLK" pad="23"/>
<connect gate="G$1" pin="GPIO12" pad="32"/>
<connect gate="G$1" pin="GPIO13" pad="33"/>
<connect gate="G$1" pin="GPIO16" pad="36"/>
<connect gate="G$1" pin="GPIO17/GEN0" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO19" pad="35"/>
<connect gate="G$1" pin="GPIO20" pad="38"/>
<connect gate="G$1" pin="GPIO21" pad="40"/>
<connect gate="G$1" pin="GPIO22/GEN3" pad="15"/>
<connect gate="G$1" pin="GPIO26" pad="37"/>
<connect gate="G$1" pin="GPIO27/GEN2" pad="13"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="RXD0/GPIO15" pad="10"/>
<connect gate="G$1" pin="TL" pad="PE_TL"/>
<connect gate="G$1" pin="TR" pad="PE_TR"/>
<connect gate="G$1" pin="TXD0/GPIO14" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
