(kicad_pcb (version 4) (host pcbnew "(2014-11-15 BZR 5288)-product")
  (general
    (links 53)
    (no_connects 0)
    (area 78.949999 73.949999 125.050001 126.050001)
    (thickness 1.6)
    (drawings 7)
    (tracks 369)
    (zones 0)
    (modules 16)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.76 2.4)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(IC1-Pad2)")
  (net 5 "Net-(IC1-Pad3)")
  (net 6 "Net-(IC1-Pad4)")
  (net 7 "Net-(IC1-Pad5)")
  (net 8 "Net-(IC1-Pad6)")
  (net 9 "Net-(IC1-Pad7)")
  (net 10 "Net-(IC1-Pad8)")
  (net 11 "Net-(IC1-Pad9)")
  (net 12 "Net-(IC1-Pad10)")
  (net 13 "Net-(IC1-Pad11)")
  (net 14 "Net-(IC1-Pad13)")
  (net 15 "Net-(IC1-Pad14)")
  (net 16 "Net-(IC1-Pad16)")
  (net 17 "Net-(IC1-Pad17)")
  (net 18 "Net-(IC1-Pad18)")
  (net 19 "Net-(IC1-Pad19)")
  (net 20 "Net-(IC1-Pad20)")
  (net 21 "Net-(IC1-Pad21)")
  (net 22 "Net-(IC1-Pad22)")
  (net 23 "Net-(IC1-Pad23)")
  (net 24 "Net-(IC1-Pad24)")
  (net 25 "Net-(IC1-Pad25)")
  (net 26 "Net-(IC1-Pad27)")
  (net 27 "Net-(IC1-Pad28)")
  (net 28 "Net-(P2-Pad10)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad16)")
    (add_net "Net-(IC1-Pad17)")
    (add_net "Net-(IC1-Pad18)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad21)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(P2-Pad10)")
  )
  (module vid28-05:vid28-05 (layer B.Cu) (tedit 547CF647)
    (at 100 100)
    (fp_text reference U1 (at 3.35 -3.85 90) (layer B.SilkS) hide)
    (fp_text value VID28-05 (at -17.9 -0.7 90) (layer B.SilkS) hide)
    (pad 5 thru_hole circle (at -19.32 -11.425) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 23 "Net-(IC1-Pad23)"))
    (pad 8 thru_hole circle (at -19.32 11.425) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 24 "Net-(IC1-Pad24)"))
    (pad 2 thru_hole circle (at 19.32 -11.425) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(IC1-Pad6)"))
    (pad 3 thru_hole circle (at 19.32 11.425) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 7 "Net-(IC1-Pad5)"))
    (pad 7 thru_hole circle (at -11.62 11.425) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 25 "Net-(IC1-Pad25)"))
    (pad 4 thru_hole circle (at 11.62 11.425) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 6 "Net-(IC1-Pad4)"))
    (pad 1 thru_hole circle (at 11.62 -11.425) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 6 thru_hole circle (at -11.62 -11.425) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 22 "Net-(IC1-Pad22)"))
    (pad "" np_thru_hole circle (at 0 -12) (size 3 3) (drill 3) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at -25 9) (size 3 3) (drill 3) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at 25 9) (size 3 3) (drill 3) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at -9.5 0) (size 7 7) (drill 7) (layers *.Cu *.Mask B.SilkS))
  )
  (module multiclock-cache:pinheader_10_50mil (layer B.Cu) (tedit 5480D7A7)
    (at 94 121)
    (fp_text reference P3 (at 0 1.905) (layer B.SilkS))
    (fp_text value CONN_02X05 (at 5.08 0.635) (layer B.SilkS) hide)
    (pad 2 thru_hole circle (at -2.54 0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 4 thru_hole circle (at -1.27 0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(IC1-Pad6)"))
    (pad 6 thru_hole circle (at 0 0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 25 "Net-(IC1-Pad25)"))
    (pad 8 thru_hole circle (at 1.27 0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 24 "Net-(IC1-Pad24)"))
    (pad 10 thru_hole circle (at 2.54 0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.54 -0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 7 "Net-(IC1-Pad5)"))
    (pad 3 thru_hole circle (at -1.27 -0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 6 "Net-(IC1-Pad4)"))
    (pad 5 thru_hole circle (at 0 -0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 22 "Net-(IC1-Pad22)"))
    (pad 7 thru_hole circle (at 1.27 -0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 23 "Net-(IC1-Pad23)"))
    (pad 9 thru_hole circle (at 2.54 -0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
  )
  (module multiclock-cache:pinheader_10_50mil (layer B.Cu) (tedit 5480D7B3)
    (at 94 79)
    (fp_text reference P2 (at 0 1.905) (layer B.SilkS))
    (fp_text value CONN_02X05 (at 5.08 0.635) (layer B.SilkS) hide)
    (pad 2 thru_hole circle (at -2.54 0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 21 "Net-(IC1-Pad21)"))
    (pad 4 thru_hole circle (at -1.27 0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 20 "Net-(IC1-Pad20)"))
    (pad 6 thru_hole circle (at 0 0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 13 "Net-(IC1-Pad11)"))
    (pad 8 thru_hole circle (at 1.27 0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 12 "Net-(IC1-Pad10)"))
    (pad 10 thru_hole circle (at 2.54 0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 28 "Net-(P2-Pad10)"))
    (pad 1 thru_hole circle (at -2.54 -0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 19 "Net-(IC1-Pad19)"))
    (pad 3 thru_hole circle (at -1.27 -0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 18 "Net-(IC1-Pad18)"))
    (pad 5 thru_hole circle (at 0 -0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 10 "Net-(IC1-Pad8)"))
    (pad 7 thru_hole circle (at 1.27 -0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 11 "Net-(IC1-Pad9)"))
    (pad 9 thru_hole circle (at 2.54 -0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 547CF669)
    (at 110.8 108.25)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 1.15 -1.85) (layer F.SilkS))
    (fp_text value 10µ (at 0 2.1) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 547CF68F)
    (at 95.15 91.75 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -0.1 -1.8 180) (layer F.SilkS))
    (fp_text value 10µ (at 0 2.1 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 547CF680)
    (at 95.55 109 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 3.85 -0.1 270) (layer F.SilkS))
    (fp_text value 1µ (at -0.05 2.15 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD/C_0805N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sparkfun:SPARKFUN-CONNECTORS_USB-MICROB (layer B.Cu) (tedit 5480EF10)
    (at 111.9 124.5 180)
    (descr "Micro USB Package")
    (fp_text reference CON1 (at -1.7 -0.55 180) (layer B.SilkS))
    (fp_text value USB-MICRO-B (at -5 -3.7 180) (layer B.SilkS) hide)
    (pad 3 smd rect (at 0 2.65 90) (size 1.4 0.35) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -0.65 2.65 90) (size 1.4 0.35) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.3 2.65 90) (size 1.4 0.35) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.65 2.65 90) (size 1.4 0.35) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -4 0 180) (size 1.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 4 0 180) (size 1.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.3 2.65 90) (size 1.4 0.35) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model walter/conn_pc/usb_B_micro_smd.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-28_7.5x17.9mm_Pitch1.27mm (layer F.Cu) (tedit 54130A77)
    (at 103 100 180)
    (descr "28-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC1 (at 1.15 -4.05 270) (layer F.SilkS))
    (fp_text value VID6606 (at -0.5 -2.1 270) (layer F.SilkS))
    (pad 1 smd rect (at -4.7 -8.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -4.7 -6.985 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -4.7 -5.715 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad3)"))
    (pad 4 smd rect (at -4.7 -4.445 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad4)"))
    (pad 5 smd rect (at -4.7 -3.175 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad5)"))
    (pad 6 smd rect (at -4.7 -1.905 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad6)"))
    (pad 7 smd rect (at -4.7 -0.635 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -4.7 0.635 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -4.7 1.905 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad9)"))
    (pad 10 smd rect (at -4.7 3.175 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at -4.7 4.445 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -4.7 5.715 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at -4.7 6.985 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at -4.7 8.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad14)"))
    (pad 15 smd rect (at 4.7 8.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 16 smd rect (at 4.7 6.985 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad16)"))
    (pad 17 smd rect (at 4.7 5.715 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad17)"))
    (pad 18 smd rect (at 4.7 4.445 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(IC1-Pad18)"))
    (pad 19 smd rect (at 4.7 3.175 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.7 1.905 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(IC1-Pad20)"))
    (pad 21 smd rect (at 4.7 0.635 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(IC1-Pad21)"))
    (pad 22 smd rect (at 4.7 -0.635 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.7 -1.905 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC1-Pad23)"))
    (pad 24 smd rect (at 4.7 -3.175 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(IC1-Pad24)"))
    (pad 25 smd rect (at 4.7 -4.445 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(IC1-Pad25)"))
    (pad 26 smd rect (at 4.7 -5.715 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 27 smd rect (at 4.7 -6.985 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad27)"))
    (pad 28 smd rect (at 4.7 -8.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(IC1-Pad28)"))
    (model Housings_SOIC/SOIC-28_7.5x17.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 547CF686)
    (at 93.5 109 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 3.85 0.1 270) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module multiclock-cache:pinheader_10_50mil (layer B.Cu) (tedit 5480D7AF)
    (at 110 79)
    (fp_text reference P1 (at 0 1.905) (layer B.SilkS))
    (fp_text value CONN_01X09 (at 5.08 0.635) (layer B.SilkS) hide)
    (pad 2 thru_hole circle (at -2.54 0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 15 "Net-(IC1-Pad14)"))
    (pad 4 thru_hole circle (at -1.27 0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 14 "Net-(IC1-Pad13)"))
    (pad 6 thru_hole circle (at 0 0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 5 "Net-(IC1-Pad3)"))
    (pad 8 thru_hole circle (at 1.27 0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 4 "Net-(IC1-Pad2)"))
    (pad 10 thru_hole circle (at 2.54 0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS))
    (pad 1 thru_hole circle (at -2.54 -0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 17 "Net-(IC1-Pad17)"))
    (pad 3 thru_hole circle (at -1.27 -0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 16 "Net-(IC1-Pad16)"))
    (pad 5 thru_hole circle (at 0 -0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 27 "Net-(IC1-Pad28)"))
    (pad 7 thru_hole circle (at 1.27 -0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 26 "Net-(IC1-Pad27)"))
    (pad 9 thru_hole circle (at 2.54 -0.635) (size 1.1 1.1) (drill 0.7) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5480EEF2)
    (at 95.25 82.05 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 0R (at 0.1 0.1 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(P2-Pad10)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02 (layer B.Cu) (tedit 5480DF0F)
    (at 103.5 119.5)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -2.286) (layer B.SilkS))
    (fp_text value CONN_01X02 (at 0.9 15.55) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 1.27 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Angled_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5480EF57)
    (at 121 78)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference MH (at 24.65 -7.25) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm_RevA_Date21Jun2010 (at 10.6 -10.45) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 3.50012) (layers))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5480EF8E)
    (at 83 78)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference MH (at -4.7 -7) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm_RevA_Date21Jun2010 (at -9.4 -10.5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 3.50012) (layers))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5480EFDB)
    (at 121 122)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference MH (at 13.75 7.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm_RevA_Date21Jun2010 (at 25.45 11.45) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 3.50012) (layers))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5480EFE2)
    (at 83 122)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference MH (at -13.95 4.4) (layer F.SilkS) hide)
    (fp_text value MountingHole_3-5mm_RevA_Date21Jun2010 (at -24.5 9.5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 3.50012) (layers))
  )
  (gr_line (start 125 107.5) (end 125 74) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125 110.5) (end 125 126) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 125 109) (end 123.5 109) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 125 109) (end 125 110.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79 74) (end 79 126) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125 74) (end 79 74) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79 126) (end 125 126) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 125 74) (xy 79 74) (xy 79 126) (xy 125 126)
      )
    )
  )
)
