<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="15" x2="0" y2="35" width="0" layer="20"/>
<wire x1="0" y1="35" x2="15" y2="49.5" width="0" layer="20"/>
<wire x1="15" y1="49.5" x2="20" y2="49.5" width="0" layer="20"/>
<wire x1="20" y1="49.5" x2="25" y2="46" width="0" layer="20" curve="90"/>
<wire x1="25" y1="46" x2="30" y2="49.5" width="0" layer="20" curve="90"/>
<wire x1="30" y1="49.5" x2="35" y2="49.5" width="0" layer="20"/>
<wire x1="35" y1="49.5" x2="50" y2="35" width="0" layer="20"/>
<wire x1="50" y1="35" x2="50" y2="15" width="0" layer="20"/>
<wire x1="50" y1="15" x2="35" y2="0.5" width="0" layer="20"/>
<wire x1="35" y1="0.5" x2="15" y2="0.5" width="0" layer="20"/>
<wire x1="15" y1="0.5" x2="0" y2="15" width="0" layer="20"/>
<hole x="14.451125" y="10.381625" drill="3.2"/>
<hole x="40.6575" y="39.791625" drill="3.2"/>
<text>PB6</text>
<text>PB7</text>
<text>PB8</text>
<text>PB0</text>
<text>PB1</text>
<text>PB2</text>
<text>PB3</text>
<text>PB4</text>
<text>PB5</text>
<text>rev20150612</text>
<text>3.3V</text>
<text>GND</text>
<text>RX</text>
<text>TX</text>
<text>HausbusCAN</text>
<text>PB14</text>
<text>PB15</text>
<text>PB13</text>
<text>PB12</text>
<text>PB11</text>
<text>PB10</text>
<text>PB9</text>
<text>PC14</text>
<text>PC15</text>
<text>SWDCLK</text>
<text>SWDIO</text>
<text>GND</text>
<text>+</text>
<text>GND</text>
<text>RX</text>
<text>TX</text>
<text>STM32F103C8T6</text>
<text>3.3V</text>
<text>5v</text>
<text>GND</text>
<text> CSTCE8M00G55</text>
<text>SCL2</text>
<text>SDA2</text>
<text>SCL1</text>
<text>SDA1</text>
</plain>
<libraries>
<library name="micro-stm_v3">
<description>&lt;b&gt;ARM 32-bit Cortex™ MCUs&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by jb@jenszuhause.de&lt;/author&gt;&lt;p&gt;
&lt;b&gt;You are using this libary by your own risk.&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Make sure to check everything well due to this libary before using it.&lt;/b&gt;</description>
<packages>
<package name="LQFP48">
<description>&lt;b&gt;LQFP48&lt;/b&gt;&lt;p&gt;
7 x 7 mm, 48-pin low-profile quad flat package</description>
</package>
</packages>
</library>
<library name="hausbus">
<packages>
<package name="0805">
</package>
<package name="0805CUTTABLE">
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; SOIC 150 mil</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ45-8">
</package>
<package name="1X09_LOCK">
</package>
<package name="1X02_LOCK">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="logic_pirate">
<description>Generated from &lt;b&gt;TinyLogic.sch&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="SPARKFUN02-20-08_RESONATOR-SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC2" library="micro-stm_v3" package="LQFP48" value="STM32F103C8T"/>
<element name="U$2" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="LED1" library="led" package="CHIP-LED0805" value="red">
<attribute name="NAME"/>
</element>
<element name="RLED" library="SparkFun-Resistors" package="0805" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LP2950" library="linear" package="TO92" value="LP2950Z">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="2.2uf"/>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="2ohm"/>
<element name="BOOT" library="pinhead" package="1X03" value="boot">
<attribute name="VALUE"/>
</element>
<element name="UART1" library="pinhead" package="1X04" value="UART1">
<attribute name="NAME"/>
</element>
<element name="UART2" library="pinhead" package="1X04" value="UART2">
<attribute name="NAME"/>
</element>
<element name="SWD" library="pinhead" package="1X02" value="SWD"/>
<element name="U$3" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$4" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$5" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$6" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$7" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$8" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$9" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$10" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$11" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$12" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$13" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$14" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$15" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="U$16" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="U$17" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="U$18" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="U$19" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="U$20" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="U$21" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="U$22" library="hausbus" package="0805" value="0805RESISTOR_NOPOP">
<attribute name="NAME"/>
</element>
<element name="U$23" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="U$24" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="U$25" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="U$26" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="JP1" library="SparkFun-Connectors" package="1X09_LOCK" value="M09LOCK"/>
<element name="JP2" library="SparkFun-Connectors" package="1X09_LOCK" value="M09LOCK"/>
<element name="JP3" library="SparkFun-Connectors" package="1X09_LOCK" value="M09LOCK"/>
<element name="JP4" library="SparkFun-Connectors" package="1X09_LOCK" value="M09LOCK"/>
<element name="U$27" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$28" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$29" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$30" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$31" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$32" library="hausbus" package="0805CUTTABLE" value="0805RESISTOR_CUTTABLE"/>
<element name="U$34" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="U$35" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="U$36" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="U$37" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="U$38" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="U$39" library="hausbus" package="0805" value="0805RESISTOR_NOPOP"/>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="hausbus" package="SO08" value="MAX3051">
<attribute name="VALUE"/>
</element>
<element name="RSLOPE" library="SparkFun-Resistors" package="0805" value="25k-200k"/>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$33" library="hausbus" package="SOT23" value="NUP2105L">
<attribute name="VALUE"/>
</element>
<element name="RCAN" library="hausbus" package="0805" value="0805RESISTOR_NOPOP">
<attribute name="NAME"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X02_LOCK" value="Supply">
<attribute name="VALUE"/>
</element>
<element name="U$40" library="logic_pirate" package="SPARKFUN02-20-08_RESONATOR-SMD" value="SPARKFUN02-20-08_RESONATORSMD"/>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="100n"/>
<element name="C7" library="SparkFun-Capacitors" package="EIA3216" value="10uF"/>
<element name="RBOOT" library="SparkFun-Resistors" package="0805" value="10k"/>
</elements>
<signals>
<signal name="GND">
<contactref element="LED1" pad="A"/>
<contactref element="JP2" pad="8"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP3" pad="8"/>
<contactref element="JP3" pad="5"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP2" pad="9"/>
<contactref element="JP2" pad="6"/>
<contactref element="JP3" pad="6"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP2" pad="5"/>
<contactref element="JP3" pad="7"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP3" pad="9"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP2" pad="7"/>
<contactref element="RSLOPE" pad="2"/>
<contactref element="U$33" pad="3"/>
<contactref element="C6" pad="1"/>
<contactref element="LP2950" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U$2" pad="8"/>
<contactref element="C5" pad="1"/>
<contactref element="IC2" pad="23"/>
<contactref element="BOOT" pad="3"/>
<contactref element="UART2" pad="4"/>
<contactref element="UART1" pad="4"/>
<contactref element="C4" pad="1"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="35"/>
<contactref element="C3" pad="1"/>
<contactref element="IC2" pad="47"/>
<contactref element="C8" pad="2"/>
<contactref element="U$1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="U$40" pad="2"/>
<contactref element="C7" pad="C"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="RX2">
<contactref element="IC2" pad="13"/>
<contactref element="UART2" pad="2"/>
</signal>
<signal name="TX2">
<contactref element="UART2" pad="3"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="SWCLK">
<contactref element="IC2" pad="37"/>
<contactref element="SWD" pad="1"/>
</signal>
<signal name="SWDIO">
<contactref element="IC2" pad="34"/>
<contactref element="SWD" pad="2"/>
</signal>
<signal name="PB0">
<contactref element="IC2" pad="18"/>
<contactref element="U$14" pad="1"/>
</signal>
<signal name="PB1">
<contactref element="U$13" pad="1"/>
<contactref element="IC2" pad="19"/>
</signal>
<signal name="PB2">
<contactref element="IC2" pad="20"/>
<contactref element="U$12" pad="1"/>
</signal>
<signal name="PB3">
<contactref element="U$11" pad="1"/>
<contactref element="IC2" pad="39"/>
</signal>
<signal name="PB4">
<contactref element="IC2" pad="40"/>
<contactref element="U$10" pad="1"/>
</signal>
<signal name="PB5">
<contactref element="U$9" pad="1"/>
<contactref element="IC2" pad="41"/>
</signal>
<signal name="PB11">
<contactref element="U$3" pad="1"/>
<contactref element="IC2" pad="22"/>
</signal>
<signal name="PB10">
<contactref element="IC2" pad="21"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="PB9">
<contactref element="U$5" pad="2"/>
<contactref element="JP4" pad="3"/>
<contactref element="U$16" pad="1"/>
</signal>
<signal name="PB8">
<contactref element="IC2" pad="45"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="PB7">
<contactref element="U$7" pad="1"/>
<contactref element="IC2" pad="43"/>
</signal>
<signal name="PB6">
<contactref element="IC2" pad="42"/>
<contactref element="U$8" pad="1"/>
</signal>
<signal name="PC14A">
<contactref element="IC2" pad="3"/>
<contactref element="U$32" pad="2"/>
</signal>
<signal name="PC15A">
<contactref element="U$31" pad="2"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="PB1X">
<contactref element="JP1" pad="8"/>
<contactref element="U$25" pad="1"/>
<contactref element="U$13" pad="2"/>
</signal>
<signal name="PB2X">
<contactref element="JP1" pad="7"/>
<contactref element="U$24" pad="1"/>
<contactref element="U$12" pad="2"/>
</signal>
<signal name="PB0X">
<contactref element="JP1" pad="9"/>
<contactref element="U$26" pad="1"/>
<contactref element="U$14" pad="2"/>
</signal>
<signal name="PB12">
<contactref element="IC2" pad="25"/>
<contactref element="U$27" pad="1"/>
</signal>
<signal name="P13">
<contactref element="IC2" pad="26"/>
<contactref element="U$28" pad="1"/>
</signal>
<signal name="PB14">
<contactref element="U$29" pad="1"/>
<contactref element="IC2" pad="27"/>
</signal>
<signal name="PC14">
<contactref element="U$32" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="U$17" pad="1"/>
</signal>
<signal name="PC15">
<contactref element="U$31" pad="1"/>
<contactref element="U$15" pad="1"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="PB15">
<contactref element="U$30" pad="1"/>
<contactref element="IC2" pad="28"/>
</signal>
<signal name="VCC">
<contactref element="LP2950" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="IC2" pad="24"/>
<contactref element="IC2" pad="48"/>
<contactref element="C3" pad="2"/>
<contactref element="IC2" pad="9"/>
<contactref element="BOOT" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="UART2" pad="1"/>
<contactref element="IC2" pad="36"/>
<contactref element="UART1" pad="1"/>
<contactref element="U$22" pad="2"/>
<contactref element="U$35" pad="2"/>
<contactref element="U$36" pad="2"/>
<contactref element="U$38" pad="2"/>
<contactref element="U$23" pad="2"/>
<contactref element="U$37" pad="2"/>
<contactref element="U$20" pad="2"/>
<contactref element="U$39" pad="2"/>
<contactref element="U$19" pad="2"/>
<contactref element="U$21" pad="2"/>
<contactref element="U$16" pad="2"/>
<contactref element="U$34" pad="2"/>
<contactref element="U$17" pad="2"/>
<contactref element="U$26" pad="2"/>
<contactref element="U$18" pad="2"/>
<contactref element="U$25" pad="2"/>
<contactref element="U$15" pad="2"/>
<contactref element="U$24" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="IC2" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="C"/>
<contactref element="RLED" pad="1"/>
</signal>
<signal name="PC13">
<contactref element="RLED" pad="2"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="PB13X">
<contactref element="U$28" pad="2"/>
<contactref element="JP4" pad="7"/>
<contactref element="U$36" pad="1"/>
</signal>
<signal name="PB14X">
<contactref element="U$29" pad="2"/>
<contactref element="JP4" pad="8"/>
<contactref element="U$35" pad="1"/>
</signal>
<signal name="PB12X">
<contactref element="U$27" pad="2"/>
<contactref element="JP4" pad="6"/>
<contactref element="U$37" pad="1"/>
</signal>
<signal name="PB11X">
<contactref element="U$3" pad="2"/>
<contactref element="JP4" pad="5"/>
<contactref element="U$38" pad="1"/>
</signal>
<signal name="PB15X">
<contactref element="U$30" pad="2"/>
<contactref element="JP4" pad="9"/>
<contactref element="U$34" pad="1"/>
</signal>
<signal name="PB10X">
<contactref element="U$4" pad="2"/>
<contactref element="U$39" pad="1"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="TX1">
<contactref element="IC2" pad="30"/>
<contactref element="UART1" pad="3"/>
</signal>
<signal name="RX1">
<contactref element="UART1" pad="2"/>
<contactref element="IC2" pad="31"/>
</signal>
<signal name="PB8X">
<contactref element="U$6" pad="2"/>
<contactref element="JP1" pad="6"/>
<contactref element="U$23" pad="1"/>
</signal>
<signal name="PB7X">
<contactref element="U$7" pad="2"/>
<contactref element="U$22" pad="1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="PB6X">
<contactref element="U$8" pad="2"/>
<contactref element="U$21" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="PB5X">
<contactref element="JP1" pad="3"/>
<contactref element="U$20" pad="1"/>
<contactref element="U$9" pad="2"/>
</signal>
<signal name="PB4X">
<contactref element="U$10" pad="2"/>
<contactref element="U$19" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="PB3X">
<contactref element="U$11" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="U$18" pad="1"/>
</signal>
<signal name="5V">
<contactref element="C2" pad="1"/>
<contactref element="LP2950" pad="3"/>
<contactref element="U$2" pad="7"/>
<contactref element="JP5" pad="2"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="CANH">
<contactref element="U$1" pad="7"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$33" pad="1"/>
<contactref element="RCAN" pad="2"/>
</signal>
<signal name="CANL">
<contactref element="U$1" pad="6"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$33" pad="2"/>
<contactref element="RCAN" pad="1"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="CANRXD">
<contactref element="IC2" pad="32"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="CANTXD">
<contactref element="U$1" pad="1"/>
<contactref element="IC2" pad="33"/>
</signal>
<signal name="RS">
<contactref element="IC2" pad="38"/>
<contactref element="U$1" pad="8"/>
<contactref element="RSLOPE" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC2" pad="46"/>
<contactref element="U$5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$40" pad="3"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="U$40" pad="1"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="SHDN">
<contactref element="IC2" pad="29"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="BOOT">
<contactref element="RBOOT" pad="2"/>
<contactref element="IC2" pad="44"/>
</signal>
<signal name="N$1">
<contactref element="BOOT" pad="2"/>
<contactref element="RBOOT" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
