<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<library>
<packages>
<package name="ARDUINO_MEGA">
<description>Footprint for representing an Arduino Mega board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
<package name="ARDUINO_DUE">
<description>Footprint for representing an Arduino Due board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
<package name="ARDUINO_LEONARDO">
<description>Footprint for representing an Arduino Leonardo board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
<package name="ARDUINO_UNO">
<description>Footprint for representing an Arduino Uno board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
<package name="ARDUINO_ETHERNET">
<description>Footprint for representing an Arduino Ethernet board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
<package name="ARDUINO_MICRO">
<description>Footprint for representing an Arduino Micro board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
<package name="ARDUINO_NANO">
<description>Footprint for representing an Arduino Nano board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
<package name="ARDUINO_MINI">
<description>Footprint for representing an Arduino Mini board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
<package name="ARDUINO_LILYPAD">
<description>Footprint for representing a Lilypad Arduino board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
</packages>
<symbols>
<symbol name="ARDUINO_UNO">
<description>Schematic symbol for representing an Arduino Uno board in an EAGLE schematic.
Created by Dave Young for Element14.  More EAGLE documentation at:
http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<pin name="28(SCL)"/>
<pin name="27(SDA)"/>
<pin name="AREF"/>
<pin name="GND"/>
<pin name="13"/>
<pin name="12"/>
<pin name="~11"/>
<pin name="~10"/>
<pin name="~9"/>
<pin name="8"/>
<pin name="7"/>
<pin name="~6"/>
<pin name="~5"/>
<pin name="4"/>
<pin name="~3"/>
<pin name="2"/>
<pin name="1(TX)"/>
<pin name="0(RX)"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VIN"/>
<pin name="GND."/>
<pin name="GND.."/>
<pin name="5V"/>
<pin name="3.3V"/>
<pin name="RESET"/>
<pin name="IOREF"/>
<pin name="(N/C)"/>
<pin name="&lt;PWR&gt;-V"/>
<pin name="&lt;PWR&gt;+V"/>
<pin name="&lt;USB&gt;GND"/>
<pin name="&lt;USB&gt;D-"/>
<pin name="&lt;USB&gt;D+"/>
<pin name="&lt;USB&gt;+V"/>
<pin name="+5V"/>
<pin name="MOSI"/>
<pin name="GND_"/>
<pin name="RESET."/>
<pin name="SCK"/>
<pin name="MISO"/>
</symbol>
<symbol name="ARDUINO_LEONARDO">
<description>Schematic symbol for representing an Arduino Leonardo board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<pin name="18(SCL)"/>
<pin name="19(SDA)"/>
<pin name="AREF"/>
<pin name="GND"/>
<pin name="13"/>
<pin name="12"/>
<pin name="~11"/>
<pin name="~10"/>
<pin name="~9"/>
<pin name="8"/>
<pin name="7"/>
<pin name="~6"/>
<pin name="~5"/>
<pin name="4"/>
<pin name="~3"/>
<pin name="2"/>
<pin name="1(TX)"/>
<pin name="0(RX)"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VIN"/>
<pin name="GND."/>
<pin name="GND.."/>
<pin name="5V"/>
<pin name="3.3V"/>
<pin name="RESET"/>
<pin name="IOREF"/>
<pin name="(N/C)"/>
<pin name="&lt;PWR&gt;-V"/>
<pin name="&lt;PWR&gt;+V"/>
<pin name="&lt;USB&gt;GND"/>
<pin name="&lt;USB&gt;D-"/>
<pin name="&lt;USB&gt;D+"/>
<pin name="&lt;USB&gt;+V"/>
<pin name="+5V"/>
<pin name="MOSI"/>
<pin name="GND_"/>
<pin name="RESET."/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="&lt;USB&gt;ID"/>
</symbol>
<symbol name="ARDUINO_DUE">
<description>Schematic symbol for representing an Arduino Due board in an EAGLE schematic. Created by Dave Young for Element14. 
More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle
&lt;note: No two pins can be named the same; in  this drawing +5V is the same as +5V. and +5V.. and +5V_ etc...&gt;</description>
<pin name="SCL1"/>
<pin name="SDA1"/>
<pin name="AREF"/>
<pin name="GND"/>
<pin name="13"/>
<pin name="12"/>
<pin name="11"/>
<pin name="10"/>
<pin name="9"/>
<pin name="8"/>
<pin name="7"/>
<pin name="6"/>
<pin name="5"/>
<pin name="4"/>
<pin name="3"/>
<pin name="2"/>
<pin name="1(TX)"/>
<pin name="0(RX)"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VIN"/>
<pin name="GND."/>
<pin name="GND.."/>
<pin name="5V"/>
<pin name="3.3V"/>
<pin name="RESET"/>
<pin name="IOREF"/>
<pin name="(N/C)"/>
<pin name="&lt;PWR&gt;-V"/>
<pin name="&lt;PWR&gt;+V"/>
<pin name="&lt;USB1&gt;GND"/>
<pin name="&lt;USB1&gt;D-"/>
<pin name="&lt;USB1&gt;D+"/>
<pin name="&lt;USB1&gt;+V"/>
<pin name="+5V"/>
<pin name="MOSI2"/>
<pin name="GND_"/>
<pin name="RESET2"/>
<pin name="SCK2"/>
<pin name="MISO2"/>
<pin name="&lt;USB2&gt;GND1"/>
<pin name="&lt;USB2&gt;D-1"/>
<pin name="&lt;USB2&gt;D+1"/>
<pin name="&lt;USB2&gt;+V1"/>
<pin name="14(TX3)"/>
<pin name="15(RX3)"/>
<pin name="16(TX2)"/>
<pin name="17(RX2)"/>
<pin name="18(TX1)"/>
<pin name="19(RX1)"/>
<pin name="20(SDA)"/>
<pin name="21(SCL)"/>
<pin name="CANTX"/>
<pin name="CANRX"/>
<pin name="DAC1"/>
<pin name="DAC0"/>
<pin name="A11"/>
<pin name="A10"/>
<pin name="A9"/>
<pin name="A8"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="+5V.."/>
<pin name="23"/>
<pin name="25"/>
<pin name="27"/>
<pin name="29"/>
<pin name="31"/>
<pin name="33"/>
<pin name="35"/>
<pin name="37"/>
<pin name="39"/>
<pin name="41"/>
<pin name="43"/>
<pin name="45"/>
<pin name="47"/>
<pin name="49"/>
<pin name="51"/>
<pin name="53"/>
<pin name="GND...."/>
<pin name="GND..."/>
<pin name="52"/>
<pin name="50"/>
<pin name="48"/>
<pin name="46"/>
<pin name="44"/>
<pin name="42"/>
<pin name="40"/>
<pin name="38"/>
<pin name="36"/>
<pin name="34"/>
<pin name="32"/>
<pin name="30"/>
<pin name="28"/>
<pin name="26"/>
<pin name="24"/>
<pin name="22"/>
<pin name="+5V."/>
<pin name="+5V_"/>
<pin name="MOSI"/>
<pin name="GND__"/>
<pin name="RESET."/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="RESET.."/>
<pin name="SWDIO"/>
<pin name="SWCLK"/>
<pin name="GND1"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TCK"/>
<pin name="TMS"/>
<pin name="RESET_"/>
<pin name="GND1..."/>
<pin name="N/C."/>
<pin name="GND1.."/>
<pin name="GND1."/>
<pin name="+3.3V"/>
<pin name="&lt;USB2&gt;ID"/>
<pin name="&lt;USB1&gt;ID"/>
</symbol>
<symbol name="ARDUINO_MEGA">
<description>Schematic symbol for representing an Arduino Mega board in an EAGLE schematic. Created by Dave Young for Element14. 
More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle
&lt;note: No two pins can be named the same; in  this drawing +5V is the same as +5V. and +5V.. and +5V_ etc...&gt;</description>
<pin name="SCL1"/>
<pin name="SDA1"/>
<pin name="AREF"/>
<pin name="GND"/>
<pin name="13"/>
<pin name="12"/>
<pin name="11"/>
<pin name="10"/>
<pin name="9"/>
<pin name="8"/>
<pin name="7"/>
<pin name="6"/>
<pin name="5"/>
<pin name="4"/>
<pin name="3"/>
<pin name="2"/>
<pin name="1(TX)"/>
<pin name="0(RX)"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VIN"/>
<pin name="GND."/>
<pin name="GND.."/>
<pin name="5V"/>
<pin name="3.3V"/>
<pin name="RESET"/>
<pin name="IOREF"/>
<pin name="(N/C)"/>
<pin name="&lt;PWR&gt;-V" direction="nc"/>
<pin name="&lt;PWR&gt;+V" direction="nc"/>
<pin name="&lt;USB&gt;GND" direction="nc"/>
<pin name="&lt;USB&gt;D-" direction="nc"/>
<pin name="&lt;USB&gt;D+" direction="nc"/>
<pin name="&lt;USB&gt;+V" direction="nc"/>
<pin name="14(TX3)"/>
<pin name="15(RX3)"/>
<pin name="16(TX2)"/>
<pin name="17(RX2)"/>
<pin name="18(TX1)"/>
<pin name="19(RX1)"/>
<pin name="20(SDA)"/>
<pin name="21(SCL)"/>
<pin name="A15"/>
<pin name="A14"/>
<pin name="A13"/>
<pin name="A12"/>
<pin name="A11"/>
<pin name="A10"/>
<pin name="A9"/>
<pin name="A8"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="+5V.."/>
<pin name="23"/>
<pin name="25"/>
<pin name="27"/>
<pin name="29"/>
<pin name="31"/>
<pin name="33"/>
<pin name="35"/>
<pin name="37"/>
<pin name="39"/>
<pin name="41"/>
<pin name="43"/>
<pin name="45"/>
<pin name="47"/>
<pin name="49"/>
<pin name="51"/>
<pin name="53"/>
<pin name="GND...."/>
<pin name="GND..."/>
<pin name="52"/>
<pin name="50"/>
<pin name="48"/>
<pin name="46"/>
<pin name="44"/>
<pin name="42"/>
<pin name="40"/>
<pin name="38"/>
<pin name="36"/>
<pin name="34"/>
<pin name="32"/>
<pin name="30"/>
<pin name="28"/>
<pin name="26"/>
<pin name="24"/>
<pin name="22"/>
<pin name="+5V."/>
<pin name="+5V_"/>
<pin name="MOSI"/>
<pin name="GND__"/>
<pin name="RESET."/>
<pin name="SCK"/>
<pin name="MISO"/>
</symbol>
<symbol name="ARDUINO_NANO">
<description>Schematic symbol for representing an Arduino Nano v3.0 board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<pin name="D12"/>
<pin name="D11"/>
<pin name="D10"/>
<pin name="D9"/>
<pin name="D8"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="GND"/>
<pin name="RST"/>
<pin name="RX0"/>
<pin name="TX1"/>
<pin name="5V"/>
<pin name="RST."/>
<pin name="GND."/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="REF"/>
<pin name="3V3"/>
<pin name="D13"/>
<pin name="&lt;USB&gt;GND"/>
<pin name="&lt;USB&gt;D-"/>
<pin name="&lt;USB&gt;D+"/>
<pin name="&lt;USB&gt;+V"/>
<pin name="5V."/>
<pin name="MOSI"/>
<pin name="GND_"/>
<pin name="RESET.."/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="VIN"/>
<pin name="&lt;USB&gt;ID"/>
</symbol>
<symbol name="ARDUINO_MICRO">
<description>Schematic symbol for representing an Arduino Micro R3 board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<pin name="D12"/>
<pin name="D11"/>
<pin name="D10"/>
<pin name="D9"/>
<pin name="D8"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="GND"/>
<pin name="RST"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="+5V"/>
<pin name="RST."/>
<pin name="GND."/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="NC."/>
<pin name="NC"/>
<pin name="REF"/>
<pin name="3V3"/>
<pin name="D13"/>
<pin name="&lt;USB&gt;GND"/>
<pin name="&lt;USB&gt;D-"/>
<pin name="&lt;USB&gt;D+"/>
<pin name="&lt;USB&gt;+V"/>
<pin name="5V"/>
<pin name="MOSI."/>
<pin name="GND_"/>
<pin name="RESET.."/>
<pin name="SCK."/>
<pin name="MISO."/>
<pin name="VIN"/>
<pin name="SS"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="&lt;USB&gt;ID"/>
</symbol>
<symbol name="ARDUINO_MINI">
<description>Schematic symbol for representing an Arduino Mini R5 board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<pin name="9V"/>
<pin name="GND.."/>
<pin name="GND"/>
<pin name="5V"/>
<pin name="13"/>
<pin name="12"/>
<pin name="11"/>
<pin name="10"/>
<pin name="R"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="9"/>
<pin name="A4"/>
<pin name="R."/>
<pin name="6"/>
<pin name="5"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="8"/>
<pin name="7"/>
<pin name="A5"/>
<pin name="IO7"/>
<pin name=".GND"/>
<pin name="TX."/>
<pin name="RX."/>
<pin name="5V."/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="2"/>
<pin name="..GND"/>
<pin name=".5V"/>
<pin name="3"/>
<pin name="4"/>
</symbol>
<symbol name="ARDUINO_ETHERNET">
<description>Schematic symbol for representing an Arduino Ethernet R3 board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="AREF"/>
<pin name="GND"/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="ETHCS"/>
<pin name="~9"/>
<pin name="8"/>
<pin name="7"/>
<pin name="~6"/>
<pin name="~5"/>
<pin name="SDCS"/>
<pin name="~3"/>
<pin name="2"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VIN"/>
<pin name="GND."/>
<pin name="GND.."/>
<pin name="5V"/>
<pin name="3.3V"/>
<pin name="RESET"/>
<pin name="IOREF"/>
<pin name="(N/C)"/>
<pin name="&lt;PWR&gt;-V"/>
<pin name="&lt;PWR&gt;+V"/>
<pin name="+5V."/>
<pin name="MOSI."/>
<pin name="GND_"/>
<pin name="RESET."/>
<pin name="SCK."/>
<pin name="MISO."/>
<pin name=".GND"/>
<pin name="N/C"/>
<pin name="5V."/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="RTS"/>
</symbol>
<symbol name="ARDUINO_LILYPAD">
<description>Schematic symbol for representing an LilyPad Arduino board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<pin name="8"/>
<pin name="12"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="13"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A5"/>
<pin name="0/RX"/>
<pin name="1/TX"/>
<pin name="2"/>
<pin name="3"/>
<pin name="6"/>
<pin name="5"/>
<pin name="+"/>
<pin name="-"/>
<pin name="4"/>
<pin name="7"/>
<pin name="A4"/>
<pin name="GND."/>
<pin name="GND.."/>
<pin name="VCC."/>
<pin name="RXI"/>
<pin name="TXO"/>
<pin name="DTR"/>
<pin name="MISO"/>
<pin name="VCC"/>
<pin name="SCK"/>
<pin name="MOSI"/>
<pin name="RST"/>
<pin name="GND"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ARDUINO_DUE_EXT" prefix="PCB">
<description>Device for representing an Arduino Due board in an EAGLE design without the PCB footprint.  Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_DUE"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="_EXTERNAL_" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_UNO_EXT" prefix="PCB">
<description>Device for representing an Arduino Uno board in an EAGLE design without the PCB footprint.  Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_UNO"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="_EXTERNAL_" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_NANO_EXT" prefix="PCB">
<description>Device for representing an Arduino Nano board in an EAGLE design without the PCB footprint.  Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_NANO"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_MINI_EXT" prefix="PCB">
<description>Device for representing an Arduino Mini board in an EAGLE design without the PCB footprint.  Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_MINI"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="_EXTERNAL_" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_MICRO_EXT" prefix="PCB">
<description>Device for representing an Arduino Micro board in an EAGLE design without the PCB footprint.  Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_MICRO"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="_EXTERNAL_" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_MEGA_EXT" prefix="PCB">
<description>Device for representing an Arduino Mega board in an EAGLE design without the PCB footprint.  Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_MEGA"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_LILYPAD_EXT" prefix="PCB">
<description>Device for representing a Lilypad Arduino board in an EAGLE design without the PCB footprint.  Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_LILYPAD"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="_EXTERNAL_" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_LEONARDO_EXT" prefix="PCB">
<description>Device for representing an Arduino Leonardo board in an EAGLE design without the PCB footprint.  Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_LEONARDO"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="_EXTERNAL_" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_ETHERNET_EXT" prefix="PCB">
<description>Device for representing an Arduino Ethernet board in an EAGLE design without the PCB footprint.  Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_ETHERNET"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="_EXTERNAL_" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_MEGA" prefix="PCB">
<description>Device for representing an Arduino Mega board with a footprint in an EAGLE design. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_MEGA"/>
</gates>
<devices>
<device name="" package="ARDUINO_MEGA">
<connects>
<connect gate="G$1" pin="(N/C)" pad="N/C"/>
<connect gate="G$1" pin="+5V." pad="5V."/>
<connect gate="G$1" pin="+5V.." pad="5V.."/>
<connect gate="G$1" pin="+5V_" pad="+5V_"/>
<connect gate="G$1" pin="0(RX)" pad="0"/>
<connect gate="G$1" pin="1(TX)" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14(TX3)" pad="14"/>
<connect gate="G$1" pin="15(RX3)" pad="15"/>
<connect gate="G$1" pin="16(TX2)" pad="16"/>
<connect gate="G$1" pin="17(RX2)" pad="17"/>
<connect gate="G$1" pin="18(TX1)" pad="18"/>
<connect gate="G$1" pin="19(RX1)" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20(SDA)" pad="20"/>
<connect gate="G$1" pin="21(SCL)" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="&lt;PWR&gt;+V" pad="&lt;PWR&gt;+V"/>
<connect gate="G$1" pin="&lt;PWR&gt;-V" pad="&lt;PWR&gt;-V"/>
<connect gate="G$1" pin="&lt;USB&gt;+V" pad="&lt;USB&gt;+V"/>
<connect gate="G$1" pin="&lt;USB&gt;D+" pad="&lt;USB&gt;D+"/>
<connect gate="G$1" pin="&lt;USB&gt;D-" pad="&lt;USB&gt;D-"/>
<connect gate="G$1" pin="&lt;USB&gt;GND" pad="&lt;USB&gt;GND"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A13" pad="A13"/>
<connect gate="G$1" pin="A14" pad="A14"/>
<connect gate="G$1" pin="A15" pad="A15"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND." pad="GND."/>
<connect gate="G$1" pin="GND.." pad="GND.."/>
<connect gate="G$1" pin="GND..." pad="GND..."/>
<connect gate="G$1" pin="GND...." pad="GND...."/>
<connect gate="G$1" pin="GND__" pad="GND__"/>
<connect gate="G$1" pin="IOREF" pad="I/OREF"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="RESET." pad="RESET."/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="SCL1" pad="SCL1"/>
<connect gate="G$1" pin="SDA1" pad="SDA1"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_DUE" prefix="PCB">
<description>Device for representing an Arduino Due board with a footprint in an EAGLE design. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_DUE"/>
</gates>
<devices>
<device name="" package="ARDUINO_DUE">
<connects>
<connect gate="G$1" pin="(N/C)" pad="N/C"/>
<connect gate="G$1" pin="+3.3V" pad="+3.3V"/>
<connect gate="G$1" pin="+5V" pad="+5V"/>
<connect gate="G$1" pin="+5V." pad="5V."/>
<connect gate="G$1" pin="+5V.." pad="5V.."/>
<connect gate="G$1" pin="+5V_" pad="+5V_"/>
<connect gate="G$1" pin="0(RX)" pad="0"/>
<connect gate="G$1" pin="1(TX)" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14(TX3)" pad="14"/>
<connect gate="G$1" pin="15(RX3)" pad="15"/>
<connect gate="G$1" pin="16(TX2)" pad="16"/>
<connect gate="G$1" pin="17(RX2)" pad="17"/>
<connect gate="G$1" pin="18(TX1)" pad="18"/>
<connect gate="G$1" pin="19(RX1)" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20(SDA)" pad="20"/>
<connect gate="G$1" pin="21(SCL)" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="&lt;PWR&gt;+V" pad="&lt;PWR&gt;+V"/>
<connect gate="G$1" pin="&lt;PWR&gt;-V" pad="&lt;PWR&gt;-V"/>
<connect gate="G$1" pin="&lt;USB1&gt;+V" pad="&lt;USB1&gt;+V"/>
<connect gate="G$1" pin="&lt;USB1&gt;D+" pad="&lt;USB1&gt;D+"/>
<connect gate="G$1" pin="&lt;USB1&gt;D-" pad="&lt;USB1&gt;D-"/>
<connect gate="G$1" pin="&lt;USB1&gt;GND" pad="&lt;USB1&gt;GND"/>
<connect gate="G$1" pin="&lt;USB1&gt;ID" pad="&lt;USB1&gt;ID"/>
<connect gate="G$1" pin="&lt;USB2&gt;+V1" pad="&lt;USB2&gt;+V1"/>
<connect gate="G$1" pin="&lt;USB2&gt;D+1" pad="&lt;USB2&gt;D+1"/>
<connect gate="G$1" pin="&lt;USB2&gt;D-1" pad="&lt;USB2&gt;D-1"/>
<connect gate="G$1" pin="&lt;USB2&gt;GND1" pad="&lt;USB2&gt;GND1"/>
<connect gate="G$1" pin="&lt;USB2&gt;ID" pad="&lt;USB2&gt;ID"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="CANRX" pad="A14"/>
<connect gate="G$1" pin="CANTX" pad="A15"/>
<connect gate="G$1" pin="DAC0" pad="A12"/>
<connect gate="G$1" pin="DAC1" pad="A13"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND." pad="GND."/>
<connect gate="G$1" pin="GND.." pad="GND.."/>
<connect gate="G$1" pin="GND..." pad="GND..."/>
<connect gate="G$1" pin="GND...." pad="GND...."/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND1." pad="GND1."/>
<connect gate="G$1" pin="GND1.." pad="GND1.."/>
<connect gate="G$1" pin="GND1..." pad="GND1..."/>
<connect gate="G$1" pin="GND_" pad="GND_"/>
<connect gate="G$1" pin="GND__" pad="GND__"/>
<connect gate="G$1" pin="IOREF" pad="I/OREF"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MISO2" pad="MISO2"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="MOSI2" pad="MOSI2"/>
<connect gate="G$1" pin="N/C." pad="N/C."/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="RESET." pad="RESET."/>
<connect gate="G$1" pin="RESET.." pad="RESET.."/>
<connect gate="G$1" pin="RESET2" pad="RESET2"/>
<connect gate="G$1" pin="RESET_" pad="RESET_"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="SCK2" pad="SCK2"/>
<connect gate="G$1" pin="SCL1" pad="SCL1"/>
<connect gate="G$1" pin="SDA1" pad="SDA1"/>
<connect gate="G$1" pin="SWCLK" pad="SWCLK"/>
<connect gate="G$1" pin="SWDIO" pad="SWDIO"/>
<connect gate="G$1" pin="TCK" pad="TCK"/>
<connect gate="G$1" pin="TDI" pad="TDI"/>
<connect gate="G$1" pin="TDO" pad="TDO"/>
<connect gate="G$1" pin="TMS" pad="TMS"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_LEONARDO" prefix="PCB">
<description>Device for representing an Arduino Leonardo board with a footprint in an EAGLE design. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_LEONARDO"/>
</gates>
<devices>
<device name="" package="ARDUINO_LEONARDO">
<connects>
<connect gate="G$1" pin="(N/C)" pad="N/C"/>
<connect gate="G$1" pin="+5V" pad="+5V"/>
<connect gate="G$1" pin="0(RX)" pad="0"/>
<connect gate="G$1" pin="1(TX)" pad="1"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="18(SCL)" pad="SCL"/>
<connect gate="G$1" pin="19(SDA)" pad="SDA"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="&lt;PWR&gt;+V" pad="&lt;PWR&gt;+V"/>
<connect gate="G$1" pin="&lt;PWR&gt;-V" pad="&lt;PWR&gt;-V"/>
<connect gate="G$1" pin="&lt;USB&gt;+V" pad="&lt;USB&gt;+V"/>
<connect gate="G$1" pin="&lt;USB&gt;D+" pad="&lt;USB&gt;D+"/>
<connect gate="G$1" pin="&lt;USB&gt;D-" pad="&lt;USB&gt;D-"/>
<connect gate="G$1" pin="&lt;USB&gt;GND" pad="&lt;USB&gt;GND"/>
<connect gate="G$1" pin="&lt;USB&gt;ID" pad="&lt;USB&gt;ID"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND." pad="GND."/>
<connect gate="G$1" pin="GND.." pad="GND.."/>
<connect gate="G$1" pin="GND_" pad="GND_"/>
<connect gate="G$1" pin="IOREF" pad="I/OREF"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="RESET." pad="RESET."/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
<connect gate="G$1" pin="~10" pad="10"/>
<connect gate="G$1" pin="~11" pad="11"/>
<connect gate="G$1" pin="~3" pad="3"/>
<connect gate="G$1" pin="~5" pad="5"/>
<connect gate="G$1" pin="~6" pad="6"/>
<connect gate="G$1" pin="~9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_UNO" prefix="PCB">
<description>Device for representing an Arduino Uno board with a footprint in an EAGLE design. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_UNO"/>
</gates>
<devices>
<device name="" package="ARDUINO_UNO">
<connects>
<connect gate="G$1" pin="(N/C)" pad="N/C"/>
<connect gate="G$1" pin="+5V" pad="+5V"/>
<connect gate="G$1" pin="0(RX)" pad="0"/>
<connect gate="G$1" pin="1(TX)" pad="1"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="27(SDA)" pad="SDA"/>
<connect gate="G$1" pin="28(SCL)" pad="SCL"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="&lt;PWR&gt;+V" pad="&lt;PWR&gt;+V"/>
<connect gate="G$1" pin="&lt;PWR&gt;-V" pad="&lt;PWR&gt;-V"/>
<connect gate="G$1" pin="&lt;USB&gt;+V" pad="&lt;USB&gt;+V"/>
<connect gate="G$1" pin="&lt;USB&gt;D+" pad="&lt;USB&gt;D+"/>
<connect gate="G$1" pin="&lt;USB&gt;D-" pad="&lt;USB&gt;D-"/>
<connect gate="G$1" pin="&lt;USB&gt;GND" pad="&lt;USB&gt;GND"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND." pad="GND."/>
<connect gate="G$1" pin="GND.." pad="GND.."/>
<connect gate="G$1" pin="GND_" pad="GND_"/>
<connect gate="G$1" pin="IOREF" pad="I/OREF"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="RESET." pad="RESET."/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
<connect gate="G$1" pin="~10" pad="10"/>
<connect gate="G$1" pin="~11" pad="11"/>
<connect gate="G$1" pin="~3" pad="3"/>
<connect gate="G$1" pin="~5" pad="5"/>
<connect gate="G$1" pin="~6" pad="6"/>
<connect gate="G$1" pin="~9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_ETHERNET" prefix="PCB">
<description>Device for representing an Arduino Ethernet board with a footprint in an EAGLE design. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_ETHERNET"/>
</gates>
<devices>
<device name="" package="ARDUINO_ETHERNET">
<connects>
<connect gate="G$1" pin="(N/C)" pad="(N/C)"/>
<connect gate="G$1" pin="+5V." pad="+5V."/>
<connect gate="G$1" pin=".GND" pad=".GND"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="5V." pad="5V."/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="&lt;PWR&gt;+V" pad="&lt;PWR&gt;+V"/>
<connect gate="G$1" pin="&lt;PWR&gt;-V" pad="&lt;PWR&gt;-V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="ETHCS" pad="ETHCS"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND." pad="GND."/>
<connect gate="G$1" pin="GND.." pad="GND.."/>
<connect gate="G$1" pin="GND_" pad="GND_"/>
<connect gate="G$1" pin="IOREF" pad="I/OREF"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MISO." pad="MISO."/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="MOSI." pad="MOSI."/>
<connect gate="G$1" pin="N/C" pad="N/C"/>
<connect gate="G$1" pin="PD0" pad="PD0"/>
<connect gate="G$1" pin="PD1" pad="PD1"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="RESET." pad="RESET."/>
<connect gate="G$1" pin="RTS" pad="RTS"/>
<connect gate="G$1" pin="RX" pad="0"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="SCK." pad="SCK."/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="SDCS" pad="4"/>
<connect gate="G$1" pin="TX" pad="1"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
<connect gate="G$1" pin="~3" pad="3"/>
<connect gate="G$1" pin="~5" pad="5"/>
<connect gate="G$1" pin="~6" pad="6"/>
<connect gate="G$1" pin="~9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_MICRO" prefix="PCB">
<description>Device for representing an Arduino Micro board with a footprint in an EAGLE design. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_MICRO"/>
</gates>
<devices>
<device name="" package="ARDUINO_MICRO">
<connects>
<connect gate="G$1" pin="+5V" pad="+5V"/>
<connect gate="G$1" pin="3V3" pad="3V3"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="&lt;USB&gt;+V" pad="&lt;USB&gt;+V"/>
<connect gate="G$1" pin="&lt;USB&gt;D+" pad="&lt;USB&gt;D+"/>
<connect gate="G$1" pin="&lt;USB&gt;D-" pad="&lt;USB&gt;D-"/>
<connect gate="G$1" pin="&lt;USB&gt;GND" pad="&lt;USB&gt;GND"/>
<connect gate="G$1" pin="&lt;USB&gt;ID" pad="&lt;USB&gt;ID"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND." pad="GND."/>
<connect gate="G$1" pin="GND_" pad="GND_"/>
<connect gate="G$1" pin="MISO" pad="MISO]"/>
<connect gate="G$1" pin="MISO." pad="MISO."/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="MOSI." pad="MOSI."/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="NC." pad="NC."/>
<connect gate="G$1" pin="REF" pad="REF"/>
<connect gate="G$1" pin="RESET.." pad="RESET.."/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RST." pad="RST."/>
<connect gate="G$1" pin="RX" pad="RX1"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="SCK." pad="SCK."/>
<connect gate="G$1" pin="SS" pad="SS"/>
<connect gate="G$1" pin="TX" pad="TX1"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_NANO" prefix="PCB">
<description>Device for representing an Arduino Nano board with a footprint in an EAGLE design. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_NANO"/>
</gates>
<devices>
<device name="" package="ARDUINO_NANO">
<connects>
<connect gate="G$1" pin="3V3" pad="3V3"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="5V." pad="5V."/>
<connect gate="G$1" pin="&lt;USB&gt;+V" pad="&lt;USB&gt;+V"/>
<connect gate="G$1" pin="&lt;USB&gt;D+" pad="&lt;USB&gt;D+"/>
<connect gate="G$1" pin="&lt;USB&gt;D-" pad="&lt;USB&gt;D-"/>
<connect gate="G$1" pin="&lt;USB&gt;GND" pad="&lt;USB&gt;GND"/>
<connect gate="G$1" pin="&lt;USB&gt;ID" pad="&lt;USB&gt;ID"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND." pad="GND."/>
<connect gate="G$1" pin="GND_" pad="GND_"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="REF" pad="REF"/>
<connect gate="G$1" pin="RESET.." pad="RESET.."/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RST." pad="RST."/>
<connect gate="G$1" pin="RX0" pad="RX1"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="TX1" pad="TX1"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_MINI" prefix="PCB">
<description>Device for representing an Arduino Mini board with a footprint in an EAGLE design. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_MINI"/>
</gates>
<devices>
<device name="" package="ARDUINO_MINI">
<connects>
<connect gate="G$1" pin="..GND" pad="..GND"/>
<connect gate="G$1" pin=".5V" pad=".5V"/>
<connect gate="G$1" pin=".GND" pad=".GND"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="5V." pad="5V."/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="9V" pad="9V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND.." pad="GND.."/>
<connect gate="G$1" pin="IO7" pad="IO7"/>
<connect gate="G$1" pin="R" pad="R"/>
<connect gate="G$1" pin="R." pad="R."/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="RX." pad="RX."/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="TX." pad="TX."/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_LILYPAD" prefix="PCB">
<description>Device for representing a Lilypad Arduino board with a footprint in an EAGLE design. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="G$1" symbol="ARDUINO_LILYPAD"/>
</gates>
<devices>
<device name="" package="ARDUINO_LILYPAD">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
<connect gate="G$1" pin="0/RX" pad="0/RX"/>
<connect gate="G$1" pin="1/TX" pad="1/TX"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="DTR" pad="DTR"/>
<connect gate="G$1" pin="GND" pad="GND_"/>
<connect gate="G$1" pin="GND." pad="GND."/>
<connect gate="G$1" pin="GND.." pad="GND.."/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RST" pad="RESET.."/>
<connect gate="G$1" pin="RXI" pad="RXI"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="TXO" pad="TXO"/>
<connect gate="G$1" pin="VCC" pad="5V."/>
<connect gate="G$1" pin="VCC." pad="VCC."/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
