<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<library>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
<symbols>
<symbol name="ATMEGA16M1">
<description>ATMEGA16M1, ATMEGA32M1, ATMEGA64M1</description>
<pin name="(ADC4/PSCOUT0B/SCK/PCINT7)PB7"/>
<pin name="(ADC7/PSCOUT1B/____PCINT6)PB6"/>
<pin name="(ADC6/INT2/ACMPN1/AMP2-/PCINT5)PB5"/>
<pin name="(AMP0+/PCINT4)PB4"/>
<pin name="(AMP0-/PCINT3)PB3"/>
<pin name="(ADC5/_INT1/ACMPN0/PCINT2)PB2"/>
<pin name="(MOSI/PSCOUT2B/PCINT1)PB1"/>
<pin name="(MISO/PSCOUT2A/PCINT0)PB0"/>
<pin name="(D2A/AMP2+/PCINT15)PC7"/>
<pin name="(ADC10/ACMP1/PCINT14)PC6"/>
<pin name="(ADC9/ACMP3/AMP1+/PCINT13)PC5"/>
<pin name="(ADC8/ACMPN3/AMP1-/PCINT12)PC4"/>
<pin name="(RXCAN/T1/ICP1B/PCINT11)PC3"/>
<pin name="(TXCAN/T0/PCINT10)PC2"/>
<pin name="(PSCIN1/OC1B/SS_A/PCINT9)PC1"/>
<pin name="(INT3/PSCOUT1A/PCINT8)PC0"/>
<pin name="VCC"/>
<pin name="AVCC"/>
<pin name="AREF"/>
<pin name="PE1(XTAL1/OC0B/PCINT25)"/>
<pin name="PE2(XTAL2/ADC0/PCINT26)"/>
<pin name="AGND" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PE0(OCD/RESET/PCINT24)" direction="in" function="dot"/>
<pin name="(PSCOUT0A/PCINT16)PD0"/>
<pin name="(PSCIN0/CLKO/PCINT17)PD1"/>
<pin name="(OC1A/PSCIN2/MISO_A/PCINT18)PD2"/>
<pin name="(OC0A/TXD/TXLIN/SS/MOSI_A/MOSI_A/PCINT19)PD3"/>
<pin name="(ICP1A/ADC1/RXD/RXLIN/SCK_A/PCINT20)PD4"/>
<pin name="(ADC2/ACMP2/PCINT21)PD5"/>
<pin name="(INT0/ADC3/ACMPN2/PCINT22)PD6"/>
<pin name="(ACMP0/PCINT23)PD7"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATMEGA16M1">
<description>ATMega16M1, ATMega32M1, ATMega64M1</description>
<gates>
<gate name="G$1" symbol="ATMEGA16M1"/>
</gates>
<devices>
<device name="" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="(ACMP0/PCINT23)PD7" pad="15"/>
<connect gate="G$1" pin="(ADC10/ACMP1/PCINT14)PC6" pad="22"/>
<connect gate="G$1" pin="(ADC2/ACMP2/PCINT21)PD5" pad="13"/>
<connect gate="G$1" pin="(ADC4/PSCOUT0B/SCK/PCINT7)PB7" pad="28"/>
<connect gate="G$1" pin="(ADC5/_INT1/ACMPN0/PCINT2)PB2" pad="16"/>
<connect gate="G$1" pin="(ADC6/INT2/ACMPN1/AMP2-/PCINT5)PB5" pad="26"/>
<connect gate="G$1" pin="(ADC7/PSCOUT1B/____PCINT6)PB6" pad="27"/>
<connect gate="G$1" pin="(ADC8/ACMPN3/AMP1-/PCINT12)PC4" pad="17"/>
<connect gate="G$1" pin="(ADC9/ACMP3/AMP1+/PCINT13)PC5" pad="18"/>
<connect gate="G$1" pin="(AMP0+/PCINT4)PB4" pad="24"/>
<connect gate="G$1" pin="(AMP0-/PCINT3)PB3" pad="23"/>
<connect gate="G$1" pin="(D2A/AMP2+/PCINT15)PC7" pad="25"/>
<connect gate="G$1" pin="(ICP1A/ADC1/RXD/RXLIN/SCK_A/PCINT20)PD4" pad="12"/>
<connect gate="G$1" pin="(INT0/ADC3/ACMPN2/PCINT22)PD6" pad="14"/>
<connect gate="G$1" pin="(INT3/PSCOUT1A/PCINT8)PC0" pad="30"/>
<connect gate="G$1" pin="(MISO/PSCOUT2A/PCINT0)PB0" pad="8"/>
<connect gate="G$1" pin="(MOSI/PSCOUT2B/PCINT1)PB1" pad="9"/>
<connect gate="G$1" pin="(OC0A/TXD/TXLIN/SS/MOSI_A/MOSI_A/PCINT19)PD3" pad="2"/>
<connect gate="G$1" pin="(OC1A/PSCIN2/MISO_A/PCINT18)PD2" pad="1"/>
<connect gate="G$1" pin="(PSCIN0/CLKO/PCINT17)PD1" pad="32"/>
<connect gate="G$1" pin="(PSCIN1/OC1B/SS_A/PCINT9)PC1" pad="3"/>
<connect gate="G$1" pin="(PSCOUT0A/PCINT16)PD0" pad="29"/>
<connect gate="G$1" pin="(RXCAN/T1/ICP1B/PCINT11)PC3" pad="7"/>
<connect gate="G$1" pin="(TXCAN/T0/PCINT10)PC2" pad="6"/>
<connect gate="G$1" pin="AGND" pad="20"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="19"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="PE0(OCD/RESET/PCINT24)" pad="31"/>
<connect gate="G$1" pin="PE1(XTAL1/OC0B/PCINT25)" pad="10"/>
<connect gate="G$1" pin="PE2(XTAL2/ADC0/PCINT26)" pad="11"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
