(kicad_pcb (version 4) (host pcbnew "(after 2015-mar-04 BZR unknown)-product")
  (general
    (links 25)
    (no_connects 0)
    (area 115.335 74.829999 170.415 149.960001)
    (thickness 1.6)
    (drawings 14)
    (tracks 61)
    (zones 0)
    (modules 21)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 2.54)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(Q1-Pad3)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C1-Pad2)")
  (net 4 "Net-(C6-Pad1)")
  (net 5 "Net-(C6-Pad2)")
  (net 6 "Net-(P3-Pad1)")
  (net 7 "Net-(P5-Pad1)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(Q1-Pad3)")
  )
  (module Connect:PINTST (layer F.Cu) (tedit 5643C2D8)
    (at 118.11 147.32)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -1.26746) (layer F.SilkS) hide)
    (fp_text value PINTST (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask F.SilkS))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 5643C2D8)
    (at 167.64 77.47)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -1.26746) (layer F.SilkS) hide)
    (fp_text value PINTST (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask F.SilkS))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 5643C2B9)
    (at 167.64 147.32)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -1.26746) (layer F.SilkS) hide)
    (fp_text value PINTST (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask F.SilkS))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_TO-92:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 54F24281)
    (at 140.97 105.41)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 0 -4) (layer F.SilkS))
    (fp_text value BC639 (at 0 3) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C1-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole oval (at 0 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad1)"))
    (model Housings_TO-92.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Housings_TO-92:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 54F24281)
    (at 148.5011 105.0036)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 0 -4) (layer F.SilkS))
    (fp_text value BC639 (at 0 3) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole oval (at 0 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C1-Pad2)"))
    (model Housings_TO-92.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5643AF1B)
    (at 143.51 96.52)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value C (at 0 2.1) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5643AF10)
    (at 143.51 90.17)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -2.1) (layer F.SilkS))
    (fp_text value C (at 0 2.1) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5643AF06)
    (at 143.51 83.82)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -2.1) (layer F.SilkS))
    (fp_text value C (at 0 2.1) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5643AF31)
    (at 147.32 93.98 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value C (at 0 2.1 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5643AF25)
    (at 147.32 87.63 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value C (at 0 2.1 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5643AEC4)
    (at 157.48 111.76 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value 100nF (at -6.35 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_NEOSID:Neosid_Inductor_MA-Bs75 (layer F.Cu) (tedit 0)
    (at 158.75 83.82 180)
    (descr "Neosid, Inductor, Bs75, Festinduktivitaet, Through hole, magneticaly shielded,")
    (tags "Neosid, Inductor, Bs75, Festinduktivitaet, Through hole, magneticaly shielded,")
    (fp_text reference L1 (at 0 -4.7498 180) (layer F.SilkS))
    (fp_text value INDUCTOR (at 0 5.00126 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.49936 0) (size 1.80086 1.80086) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.49936 0) (size 1.80086 1.80086) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C1-Pad2)"))
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 0)
    (at 161.29 96.52)
    (fp_text reference P1 (at 0 -3.81) (layer F.SilkS))
    (fp_text value CONN_1 (at -1.905 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 5643AEE3)
    (at 161.29 105.41)
    (fp_text reference P2 (at 0 -3.81) (layer F.SilkS))
    (fp_text value CONN_1 (at -1.905 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C6-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 0)
    (at 161.29 115.57)
    (fp_text reference P3 (at 0 -3.81) (layer F.SilkS))
    (fp_text value CONN_1 (at -1.905 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P3-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 0)
    (at 161.29 120.65)
    (fp_text reference P4 (at 0 -3.81) (layer F.SilkS))
    (fp_text value CONN_1 (at -1.905 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P3-Pad1)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 152.4 116.84 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 220k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 154.94 105.41 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 4k7 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(Q1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Triwood_RM-065 (layer F.Cu) (tedit 53FABC1B)
    (at 137.16 114.3 270)
    (descr "Potentiometer, Trimmer, RM-065")
    (tags "Potentiometer, Trimmer, RM-065")
    (fp_text reference RV1 (at 6.30936 -6.30936 270) (layer F.SilkS))
    (fp_text value POT (at 2.49936 2.58064 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.49936 -5.03936 270) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P5-Pad1)"))
    (pad 3 thru_hole circle (at 4.99872 0 270) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C1-Pad2)"))
    (model Potentiometers.3dshapes/Potentiometer_Triwood_RM-065.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 0)
    (at 146.05 116.84)
    (fp_text reference P5 (at 0 -3.81) (layer F.SilkS))
    (fp_text value CONN_1 (at -1.905 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P5-Pad1)"))
  )
  (module Connect:PINTST (layer F.Cu) (tedit 5643C2D8)
    (at 118.11 77.47)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -1.26746) (layer F.SilkS) hide)
    (fp_text value PINTST (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask F.SilkS))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Audion (at 134.62 107.95 90) (layer B.Cu))
  (gr_text Audion (at 132.08 107.95 90) (layer F.Cu))
  (gr_text +9V (at 165.1 96.52 90) (layer F.Cu))
  (gr_text GND (at 165.1 118.11 90) (layer F.Cu))
  (gr_text OUT (at 165.1 105.41 90) (layer F.Cu))
  (zone (net 6) (net_name "Net-(P3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 2.54))
    (min_thickness 1.52)
    (fill yes (arc_segments 16) (thermal_gap 2.54) (thermal_bridge_width 2.54))
    (polygon
      (pts
        (xy 168.91 149.86) (xy 115.57 149.86) (xy 115.57 74.93) (xy 168.91 74.93) (xy 168.91 149.86)
      )
    )
  )
  (zone (net 6) (net_name "Net-(P3-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 2.54))
    (min_thickness 1.52)
    (fill yes (arc_segments 16) (thermal_gap 2.54) (thermal_bridge_width 2.54))
    (polygon
      (pts
        (xy 168.91 149.86) (xy 163.83 149.86) (xy 160.02 149.86) (xy 115.57 149.86) (xy 115.57 74.93)
        (xy 162.56 74.93) (xy 163.83 74.93) (xy 168.91 74.93) (xy 168.91 149.86)
      )
    )
  )
)
