(kicad_pcb (version 4) (host pcbnew 4.0.0~rc1a-stable)
  (general
    (links 14)
    (no_connects 0)
    (area 120.146458 52.626 248.026543 88.471)
    (thickness 1.6)
    (drawings 4)
    (tracks 50)
    (zones 0)
    (modules 14)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.3)
    (user_trace_width 0.8)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 2)
    (user_trace_width 2.45)
    (user_trace_width 3)
    (user_trace_width 5)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.9)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x000a8_00000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GNDPWR)
  (net 2 GND)
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(L1-Pad1)")
  (net 5 "Net-(L2-Pad1)")
  (net 6 /Input)
  (net 7 /NettieNT1)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class CopperInFootprint ""
    (clearance 3)
    (trace_width 1)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /NettieNT1)
  )
  (net_class GND ""
    (clearance 1)
    (trace_width 5)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net GND)
  )
  (net_class GND-2 ""
    (clearance 2)
    (trace_width 2)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net GNDPWR)
  )
  (net_class coplanar50-Ohm ""
    (clearance 1)
    (trace_width 2.45)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class schmal ""
    (clearance 0.3)
    (trace_width 0.3)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class test-2 ""
    (clearance 1)
    (trace_width 1)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /Input)
    (add_net "Net-(L1-Pad1)")
  )
  (net_class test-3 ""
    (clearance 1.5)
    (trace_width 0.8)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(L2-Pad1)")
  )
  (module Oddities_RevA_10Mar2011:NetTie-I_Connected_SMD_RevA_20Mar2011 (layer F.Cu) (tedit 56C7657B)
    (at 184.404 64.897)
    (descr "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC.")
    (tags "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC.")
    (fp_text reference NT1 (at -0.254 -3.937) (layer F.SilkS))
    (fp_text value NET-TIE_07Mar2012 (at 1.016 2.413) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 0) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 6 /Input))
    (pad 2 smd rect (at 6.7 0) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad2)"))
  )
  (module Oddities_RevA_10Mar2011:NetTie-I_RevA_20Mar2011 (layer F.Cu) (tedit 56C75FB8)
    (at 184.15 78.74)
    (descr "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC. Make connection between 1 and 2 by yourself.")
    (tags "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC. Make connection between 1 and 2 by yourself.")
    (fp_text reference NT2 (at -0.254 -3.175) (layer F.SilkS))
    (fp_text value NET-TIE_07Mar2012 (at -0.254 5.715) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GNDPWR))
    (pad 2 thru_hole rect (at 2.54 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Dioden_ThroughHole_RevC:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 4D93C165)
    (at 160.02 69.85 90)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D1 (at 0 2.54 90) (layer F.SilkS))
    (fp_text value Z-Diode (at -1.016 -3.556 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 1 GNDPWR))
    (pad 2 thru_hole rect (at 5.08 0 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 6 /Input))
    (model discret/diode.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Dioden_ThroughHole_RevC:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 4D93C165)
    (at 207.01 69.85 90)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D2 (at 0 2.54 90) (layer F.SilkS))
    (fp_text value Z-Diode (at -1.016 -3.556 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 5.08 0 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D2-Pad2)"))
    (model discret/diode.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_SMD_RevB_28Dez2012:Choke_SMD_PISN_FASTRON (layer F.Cu) (tedit 4BF41A3D)
    (at 140.97 64.77 180)
    (descr "Choke, Drossel, PISN, SMD, Fastron,")
    (tags "Choke, Drossel, PISN, SMD, Fastron,")
    (fp_text reference L1 (at 0 -6.35 180) (layer F.SilkS))
    (fp_text value Drossel (at 1.27 7.62 180) (layer F.SilkS))
    (pad 2 smd rect (at -5.15112 0.01016 180) (size 2.99974 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 6 /Input))
    (pad 1 smd rect (at 5.1816 0 180) (size 2.99974 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(L1-Pad1)"))
  )
  (module Choke_SMD_RevB_28Dez2012:Choke_SMD_PISN_FASTRON (layer F.Cu) (tedit 4BF41A3D)
    (at 222.25 64.77)
    (descr "Choke, Drossel, PISN, SMD, Fastron,")
    (tags "Choke, Drossel, PISN, SMD, Fastron,")
    (fp_text reference L2 (at 0 -6.35) (layer F.SilkS))
    (fp_text value Drossel (at 1.27 7.62) (layer F.SilkS))
    (pad 2 smd rect (at -5.15112 0.01016) (size 2.99974 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at 5.1816 0) (size 2.99974 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(L2-Pad1)"))
  )
  (module Measurement_Point_RevA:Measurement_Point_Round-TH_Big (layer F.Cu) (tedit 4BBC4584)
    (at 127 64.77)
    (descr "Mesurement Point, Square, Trough Hole,  DM 3mm, Drill 1.5mm,")
    (tags "Mesurement Point, Square, Trough Hole, DM 3mm, Drill 1.5mm,")
    (fp_text reference X1 (at 0 -2.54) (layer F.SilkS))
    (fp_text value "+ IN" (at 0 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(L1-Pad1)"))
  )
  (module Measurement_Point_RevA:Measurement_Point_Round-TH_Big (layer F.Cu) (tedit 4BBC4584)
    (at 170.18 78.74)
    (descr "Mesurement Point, Square, Trough Hole,  DM 3mm, Drill 1.5mm,")
    (tags "Mesurement Point, Square, Trough Hole, DM 3mm, Drill 1.5mm,")
    (fp_text reference X2 (at 0 -2.54) (layer F.SilkS))
    (fp_text value -IN (at 0 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 1 GNDPWR))
  )
  (module Measurement_Point_RevA:Measurement_Point_Round-TH_Big (layer F.Cu) (tedit 4BBC4584)
    (at 170.18 59.69)
    (descr "Mesurement Point, Square, Trough Hole,  DM 3mm, Drill 1.5mm,")
    (tags "Mesurement Point, Square, Trough Hole, DM 3mm, Drill 1.5mm,")
    (fp_text reference X3 (at 0 -2.54) (layer F.SilkS))
    (fp_text value "+ OUT" (at 0 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 6 /Input))
  )
  (module Measurement_Point_RevA:Measurement_Point_Round-TH_Big (layer F.Cu) (tedit 4BBC4584)
    (at 127 78.74)
    (descr "Mesurement Point, Square, Trough Hole,  DM 3mm, Drill 1.5mm,")
    (tags "Mesurement Point, Square, Trough Hole, DM 3mm, Drill 1.5mm,")
    (fp_text reference X4 (at 0 -2.54) (layer F.SilkS))
    (fp_text value "- OUT" (at 0 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 1 GNDPWR))
  )
  (module Measurement_Point_RevA:Measurement_Point_Round-TH_Big (layer F.Cu) (tedit 4BBC4584)
    (at 199.39 59.69)
    (descr "Mesurement Point, Square, Trough Hole,  DM 3mm, Drill 1.5mm,")
    (tags "Mesurement Point, Square, Trough Hole, DM 3mm, Drill 1.5mm,")
    (fp_text reference X5 (at 0 -2.54) (layer F.SilkS))
    (fp_text value "+ OUT" (at 0 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D2-Pad2)"))
  )
  (module Measurement_Point_RevA:Measurement_Point_Round-TH_Big (layer F.Cu) (tedit 4BBC4584)
    (at 199.39 78.74)
    (descr "Mesurement Point, Square, Trough Hole,  DM 3mm, Drill 1.5mm,")
    (tags "Mesurement Point, Square, Trough Hole, DM 3mm, Drill 1.5mm,")
    (fp_text reference X6 (at 0 -2.54) (layer F.SilkS))
    (fp_text value "- OUT" (at 0 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Measurement_Point_RevA:Measurement_Point_Round-TH_Big (layer F.Cu) (tedit 56C758C4)
    (at 242.189 65.913)
    (descr "Mesurement Point, Square, Trough Hole,  DM 3mm, Drill 1.5mm,")
    (tags "Mesurement Point, Square, Trough Hole, DM 3mm, Drill 1.5mm,")
    (fp_text reference X7 (at 0.381 -4.953) (layer F.SilkS))
    (fp_text value "+ IN" (at 0 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0.381 -1.143) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(L2-Pad1)"))
  )
  (module Measurement_Point_RevA:Measurement_Point_Round-TH_Big (layer F.Cu) (tedit 4BBC4584)
    (at 242.57 78.74)
    (descr "Mesurement Point, Square, Trough Hole,  DM 3mm, Drill 1.5mm,")
    (tags "Mesurement Point, Square, Trough Hole, DM 3mm, Drill 1.5mm,")
    (fp_text reference X8 (at 0 -2.54) (layer F.SilkS))
    (fp_text value -IN (at 0 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (gr_line (start 245.11 85.09) (end 245.11 53.34) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 85.09) (end 245.11 85.09) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 53.34) (end 123.19 85.09) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 245.11 53.34) (end 123.19 53.34) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.19 53.34) (xy 245.11 53.34) (xy 245.11 85.09) (xy 123.19 85.09)
      )
    )
  )
  (zone (net 1) (net_name GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 245.11 85.09) (xy 123.19 85.09) (xy 123.19 53.34) (xy 245.11 53.34) (xy 245.11 85.09)
      )
    )
  )
)
