<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="2" y1="-116" x2="124" y2="-116" width="0" layer="20"/>
<wire x1="124" y1="-116" x2="124" y2="118" width="0" layer="20"/>
<wire x1="124" y1="118" x2="2" y2="118" width="0" layer="20"/>
<wire x1="2" y1="118" x2="2" y2="-116" width="0" layer="20"/>
</plain>
<libraries>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="IS42S16320D">
<packages>
<package name="TSOP54-II">
<description>&lt;b&gt;TSOP 54&lt;/b&gt; Type II&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="con-hirose">
<description>&lt;b&gt;Hirose Connectors&lt;/b&gt;&lt;p&gt;
www.hirose.co.jp&lt;p&gt;
Include : &lt;br&gt;
con-hirose-df12d(3.0)60dp0.5v80.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;
con-hirose.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;</description>
<packages>
<package name="FH12-40S-0.5SH">
<description>&lt;b&gt;0.5mm Pitch Connectors For FPC/FFC&lt;/b&gt;&lt;p&gt;
Source: &lt;a href= "http://www.hirose.co.jp/cataloge_hp/e58605370.pdf"&gt;Data sheet&lt;/a&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="IQD-Frequency-Products">
<description>&lt;b&gt;Crystals and Oscillators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by IQD Frequency Products&lt;/author&gt;</description>
<packages>
<package name="85SMX">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="7.0X5.0-4-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="20pin_header">
<packages>
<package name="TYCO_2-1761603-7">
</package>
</packages>
</library>
<library name="lm2576">
<packages>
<package name="TO220-5">
<description>&lt;b&gt;Molded Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-caps-electro-pol">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="063_025_2">
<description>&lt;b&gt;6.3mm diameter, 2.5mm lead spacing, 0.2" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rc-master-smd">
<description>&lt;b&gt;R/C MASTER-SMD! - v1.01 (07/03/2007)&lt;/b&gt;&lt;p&gt;
&lt;p&gt;This library is a collection of SMD ONLY resistors and capacitors by various manufacturers. The pad sizes, spacing and silkscreen widths have been tweaked for use in dense fine pitch layouts where space, alignment and precision are critical. In general these components are designed for routing in grid increments of 5 mils&lt;/p&gt;
&lt;p&gt;* Silkscreen line elements are a minimum of 8 mils in width. All components have text sizes of 0.032"  or 0.04".&lt;/p&gt;
&lt;p&gt;* A silkscreen text values use a ratio of 18 in all cases.&lt;/p&gt;
&lt;p&gt;* ALL PADS AND PART OUTLINES ARE SNAPPED TO A 5 MIL GRID!&lt;/p&gt;
&lt;p&gt;&lt;h4&gt;All components are prefixed using the following conventions:&lt;/h4&gt;&lt;/p&gt;
&lt;table width="380" border="1" bordercolor="#000000"&gt;
  &lt;tr&gt; 
    &lt;td width="81" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Prefix&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
    &lt;td width="289" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Description&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CBP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Bipolar Electrolytic Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CCA_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Chip Cap Array Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Electrolytic/Tantalum Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Non-Polarized Film / Chip Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;FB_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Ferrite Bead Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;L_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Chip Inductors&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;R_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Resistor Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;
&lt;p&gt;&lt;author&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;Copyright (C) 2007, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;
&lt;/author&gt;</description>
<packages>
<package name="C3216/T">
<description>&lt;b&gt;SMD CHIP TANT&lt;/b&gt;&lt;p&gt;
chip tantalum</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO-214AC">
<description>&lt;b&gt;SURFACE MOUNT GENERAL RECTIFIER&lt;/b&gt; JEDEC DO-214AC molded platic body&lt;p&gt;
Method 2026&lt;br&gt;
Source: http://www.kingtronics.com/SMD_M7/M7_SMD_4007.pdf</description>
</package>
</packages>
</library>
<library name="Panasonic-ELC">
<description>&lt;b&gt; Developed By element14 &lt;/b&gt;&lt;p&gt; 

For feedback and Technical support please contact reach from below:
&lt;br&gt; Tech Support e-mail  : &lt;a href="mailto:CAD_Tech@element14.com"&gt;CAD_Tech@element14.com&lt;/a&gt;
&lt;br&gt;Community website: &lt;a href=http://www.element14.com/community/community/knode/cad_tools/cadsoft_eagle/eagle_cad_libraries&gt;
EAGLE CAD Libraries on element14&lt;/a&gt;</description>
<packages>
<package name="IND_ELC16B">
</package>
</packages>
</library>
<library name="Panasonic-EE5">
<description>&lt;b&gt; Developed By element14 &lt;/b&gt;&lt;p&gt; 

For feedback and Technical support please contact reach from below:
&lt;br&gt; Tech Support e-mail  : &lt;a href="mailto:CAD_Tech@element14.com"&gt;CAD_Tech@element14.com&lt;/a&gt;
&lt;br&gt;Community website: &lt;a href=http://www.element14.com/community/community/knode/cad_tools/cadsoft_eagle/eagle_cad_libraries&gt;
EAGLE CAD Libraries on element14&lt;/a&gt;</description>
<packages>
<package name="CAPPR750-1600X4200">
</package>
</packages>
</library>
<library name="dp83848">
<packages>
<package name="QFP50P900X900X160-48N">
</package>
</packages>
</library>
<library name="CONNECTER">
<packages>
<package name="HR911105A">
</package>
</packages>
</library>
<library name="FFC_4Pin">
<packages>
<package name="FCI_SFW4R-3STE1LF">
</package>
</packages>
</library>
<library name="MAX3232CDR">
<packages>
<package name="SOIC127P600X175-16N">
</package>
</packages>
</library>
<library name="AD7606-4">
<packages>
<package name="QFP50P1200X1200X160-64N">
</package>
</packages>
</library>
<library name="STM32">
<packages>
<package name="LQFP208">
<description>&lt;b&gt;LQFP208&lt;/b&gt;&lt;p&gt;
28 x 28 mm, 208-pin low-profile quad flat package</description>
</package>
<package name="LQFP100">
<description>&lt;b&gt;LQFP100&lt;/b&gt;&lt;p&gt;
14 x 14 mm, 100-pin low-profile quad flat package</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C_C1" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C10" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C11" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C12" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C13" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C14" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C15" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C20" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C19" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C18" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C50" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C2" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C60" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C61" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C62" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C63" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C64" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C65" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C66" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C3" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C4" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C5" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C6" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C7" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C8" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C9" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="R1" library="eagle-ltspice" package="R0805" value="10k">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="RESET_SW" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="MPN" value="B3F-1000"/>
</element>
<element name="U$1" library="IS42S16320D" package="TSOP54-II" value="IS42S16320"/>
<element name="TFT_CON" library="con-hirose" package="FH12-40S-0.5SH" value="FH12-40S-0.5SH">
<attribute name="OC_NEWARK" value="34M6178"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1324556"/>
<attribute name="MPN" value="FH12-40S-0.5SH(55)"/>
</element>
<element name="769_BOOT_JMP" library="jumper" package="JP2" value=""/>
<element name="Y1" library="SparkFun-FreqCtrl" package="HC49UP" value="8MHz"/>
<element name="C_C40" library="eagle-ltspice" package="C0805" value="18pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C41" library="eagle-ltspice" package="C0805" value="18pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="R2" library="eagle-ltspice" package="R0805" value="220">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="X2" library="IQD-Frequency-Products" package="85SMX" value="32.768kHz"/>
<element name="C_C42" library="eagle-ltspice" package="C0805" value="12pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C43" library="eagle-ltspice" package="C0805" value="12pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C16" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C17" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="U1" library="20pin_header" package="TYCO_2-1761603-7" value="2-1761603-7">
<attribute name="MPN" value="2-1761603-7"/>
<attribute name="OC_FARNELL" value="1298789"/>
<attribute name="PACKAGE" value="20-Way Male Header"/>
<attribute name="SUPPLIER" value="TycoElectronics"/>
<attribute name="OC_NEWARK" value="42K6789"/>
</element>
<element name="LM2576-5" library="lm2576" package="TO220-5" value=""/>
<element name="LM2576-3.3" library="lm2576" package="TO220-5" value=""/>
<element name="C_A1_ESR" library="gm-caps-electro-pol" package="063_025_2" value="100µF"/>
<element name="C_A2_ESR" library="gm-caps-electro-pol" package="063_025_2" value="100µF"/>
<element name="C_T1" library="rc-master-smd" package="C3216/T" value="10µF"/>
<element name="C_T2" library="rc-master-smd" package="C3216/T" value="1µF"/>
<element name="C_T3" library="rc-master-smd" package="C3216/T" value="1µF"/>
<element name="C_T5" library="rc-master-smd" package="C3216/T" value="2.2µF"/>
<element name="C_T4" library="rc-master-smd" package="C3216/T" value="2.2µF"/>
<element name="D1" library="diode" package="DO-214AC" value="SK34"/>
<element name="D2" library="diode" package="DO-214AC" value="SK34"/>
<element name="L1" library="Panasonic-ELC" package="IND_ELC16B" value=" 100UH ">
<attribute name="MPN" value="ELC16B101L"/>
<attribute name="OC_NEWARK" value="32R9152"/>
<attribute name="CURRENTRATING" value=" 2.6A "/>
<attribute name="OC_FARNELL" value="1749179  "/>
<attribute name="PACKAGE" value="Radial Lead-TH"/>
<attribute name="SUPPLIER" value="PANASONIC"/>
</element>
<element name="L2" library="Panasonic-ELC" package="IND_ELC16B" value=" 100UH ">
<attribute name="MPN" value="ELC16B101L"/>
<attribute name="OC_NEWARK" value="32R9152"/>
<attribute name="CURRENTRATING" value=" 2.6A "/>
<attribute name="OC_FARNELL" value="1749179  "/>
<attribute name="PACKAGE" value="Radial Lead-TH"/>
<attribute name="SUPPLIER" value="PANASONIC"/>
</element>
<element name="C_A3_ESR" library="Panasonic-EE5" package="CAPPR750-1600X4200" value="2000UF">
<attribute name="MPN" value="EEUTP1E202S"/>
<attribute name="OC_NEWARK" value="47T2036 "/>
<attribute name="RATEDVOLTAGE" value="25V"/>
<attribute name="TOLERANCE" value="±20 %"/>
<attribute name="OC_FARNELL" value="1890547 "/>
<attribute name="SUPPLIER" value="PANASONIC "/>
</element>
<element name="C_A4_ESR" library="Panasonic-EE5" package="CAPPR750-1600X4200" value="2000UF">
<attribute name="MPN" value="EEUTP1E202S"/>
<attribute name="OC_NEWARK" value="47T2036 "/>
<attribute name="RATEDVOLTAGE" value="25V"/>
<attribute name="TOLERANCE" value="±20 %"/>
<attribute name="OC_FARNELL" value="1890547 "/>
<attribute name="SUPPLIER" value="PANASONIC "/>
</element>
<element name="R3" library="eagle-ltspice" package="R0805" value="10k">
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="R29" library="eagle-ltspice" package="R0805" value="1.5k">
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="U2" library="dp83848" package="QFP50P900X900X160-48N" value="DP83848IVV/NOPB">
<attribute name="PACKAGE" value="48LQFP"/>
<attribute name="OC_NEWARK" value="69K2089"/>
<attribute name="OC_FARNELL" value="2101289 "/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="MPN" value="DP83848IVV/NOPB"/>
</element>
<element name="RJ1" library="CONNECTER" package="HR911105A" value="HR911105A"/>
<element name="R20" library="eagle-ltspice" package="R0805" value="18">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R21" library="eagle-ltspice" package="R0805" value="18">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="C_C21" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="R22" library="eagle-ltspice" package="R0805" value="18">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R23" library="eagle-ltspice" package="R0805" value="18">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="C_C22" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C23" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C24" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="SG7050CAN" library="IQD-Frequency-Products" package="7.0X5.0-4-PAD" value="TCXO-CFPT-125"/>
<element name="C_T6" library="rc-master-smd" package="C3216/T" value="10µF"/>
<element name="C_C25" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C26" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C27" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="R40" library="eagle-ltspice" package="R0805" value="330">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R41" library="eagle-ltspice" package="R0805" value="330">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R24" library="eagle-ltspice" package="R0805" value="4.87k">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R25" library="eagle-ltspice" package="R0805" value="2.2k">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R26" library="eagle-ltspice" package="R0805" value="2.2k">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R28" library="eagle-ltspice" package="R0805" value="2.2k">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R27" library="eagle-ltspice" package="R0805" value="2.2k">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="C_C28" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C29" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C_C30" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="TOUCH_CON" library="FFC_4Pin" package="FCI_SFW4R-3STE1LF" value="SFW4S-2STE9LF">
<attribute name="SUPPLIER" value="FCI"/>
<attribute name="PACKAGE" value="CONNECTOR-4POS"/>
<attribute name="OC_FARNELL" value="1632059"/>
<attribute name="OC_NEWARK" value="06M0308"/>
<attribute name="MPN" value="SFW4R-3STE1LF"/>
</element>
<element name="R31" library="eagle-ltspice" package="R0805" value="1.5k">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R30" library="eagle-ltspice" package="R0805" value="1.5k">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="U3" library="MAX3232CDR" package="SOIC127P600X175-16N" value="MAX3232CDR">
<attribute name="SUPPLIER" value="TEXAS INSTRUMENTS"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="OC_FARNELL" value="1564957"/>
<attribute name="OC_NEWARK" value="35K4720"/>
<attribute name="MPN" value="MAX3232CDR"/>
</element>
<element name="C_T7" library="rc-master-smd" package="C3216/T" value="0.1µF"/>
<element name="C_T8" library="rc-master-smd" package="C3216/T" value="0.1µF"/>
<element name="C_T9" library="rc-master-smd" package="C3216/T" value="0.1µF"/>
<element name="C_T10" library="rc-master-smd" package="C3216/T" value="0.1µF"/>
<element name="C_T11" library="rc-master-smd" package="C3216/T" value="0.1µF"/>
<element name="RS232_CON" library="jumper" package="JP2" value=""/>
<element name="U4" library="AD7606-4" package="QFP50P1200X1200X160-64N" value="AD7606BSTZ-4">
<attribute name="OC_NEWARK" value="76R7616"/>
<attribute name="MPN" value="AD7606BSTZ-4"/>
<attribute name="OC_FARNELL" value="2295975"/>
<attribute name="SUPPLIER" value="Analog Devices"/>
<attribute name="PACKAGE" value="LQFP-64"/>
</element>
<element name="IC1" library="STM32" package="LQFP208" value="STM32F769BIT6"/>
<element name="IC2" library="STM32" package="LQFP100" value="STM32F767VIT6"/>
<element name="C_C92" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="C_C90" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="C_C91" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="R80" library="eagle-ltspice" package="R0805" value="10k">
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="767_BOOT_JMP" library="jumper" package="JP2" value=""/>
<element name="Y2" library="SparkFun-FreqCtrl" package="HC49UP" value="8MHz"/>
<element name="C_C93" library="eagle-ltspice" package="C0805" value="18pF">
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="C_C94" library="eagle-ltspice" package="C0805" value="18pF">
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="R81" library="eagle-ltspice" package="R0805" value="220">
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="C_T32" library="rc-master-smd" package="C3216/T" value="1µF"/>
<element name="C_T31" library="rc-master-smd" package="C3216/T" value="1µF"/>
<element name="C_T34" library="rc-master-smd" package="C3216/T" value="2.2µF"/>
<element name="C_T33" library="rc-master-smd" package="C3216/T" value="2.2µF"/>
<element name="C_C80" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="C_C81" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="C_C82" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="C_C83" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="C_C84" library="eagle-ltspice" package="C0805" value="100nF">
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="C_T30" library="rc-master-smd" package="C3216/T" value="10µF"/>
<element name="U5" library="20pin_header" package="TYCO_2-1761603-7" value="2-1761603-7">
<attribute name="PACKAGE" value="20-Way Male Header"/>
<attribute name="MPN" value="2-1761603-7"/>
<attribute name="OC_FARNELL" value="1298789"/>
<attribute name="OC_NEWARK" value="42K6789"/>
<attribute name="SUPPLIER" value="TycoElectronics"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="197"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="1"/>
<contactref element="769_BOOT_JMP" pad="2"/>
</signal>
<signal name="NRST">
<contactref element="RESET_SW" pad="1"/>
<contactref element="RESET_SW" pad="2"/>
<contactref element="C_C50" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="U2" pad="29"/>
<contactref element="IC1" pad="34"/>
<contactref element="IC2" pad="14"/>
<contactref element="U1" pad="15"/>
<contactref element="U5" pad="15"/>
</signal>
<signal name="RAM1_A0">
<contactref element="U$1" pad="23"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="RAM1_A2">
<contactref element="U$1" pad="25"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="RAM1_A3">
<contactref element="U$1" pad="26"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="RAM1_A4">
<contactref element="U$1" pad="29"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="RAM1_A5">
<contactref element="U$1" pad="30"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="RAM1_A6">
<contactref element="U$1" pad="31"/>
<contactref element="IC1" pad="71"/>
</signal>
<signal name="RAM1_A7">
<contactref element="U$1" pad="32"/>
<contactref element="IC1" pad="74"/>
</signal>
<signal name="RAM1_A8">
<contactref element="U$1" pad="33"/>
<contactref element="IC1" pad="75"/>
</signal>
<signal name="RAM1_A9">
<contactref element="U$1" pad="34"/>
<contactref element="IC1" pad="76"/>
</signal>
<signal name="RAM1_A10">
<contactref element="U$1" pad="22"/>
<contactref element="IC1" pad="77"/>
</signal>
<signal name="RAM1_A11">
<contactref element="U$1" pad="35"/>
<contactref element="IC1" pad="78"/>
</signal>
<signal name="RAM1_A12">
<contactref element="U$1" pad="36"/>
<contactref element="IC1" pad="129"/>
</signal>
<signal name="RAM1_D1">
<contactref element="U$1" pad="4"/>
<contactref element="IC1" pad="117"/>
</signal>
<signal name="RAM1_D0">
<contactref element="U$1" pad="2"/>
<contactref element="IC1" pad="116"/>
</signal>
<signal name="RAM1_D2">
<contactref element="U$1" pad="5"/>
<contactref element="IC1" pad="164"/>
</signal>
<signal name="RAM1_D3">
<contactref element="U$1" pad="7"/>
<contactref element="IC1" pad="165"/>
</signal>
<signal name="RAM1_D4">
<contactref element="U$1" pad="8"/>
<contactref element="IC1" pad="79"/>
</signal>
<signal name="RAM1_D5">
<contactref element="U$1" pad="10"/>
<contactref element="IC1" pad="80"/>
</signal>
<signal name="RAM1_D6">
<contactref element="U$1" pad="11"/>
<contactref element="IC1" pad="81"/>
</signal>
<signal name="RAM1_D7">
<contactref element="U$1" pad="13"/>
<contactref element="IC1" pad="84"/>
</signal>
<signal name="RAM1_D8">
<contactref element="U$1" pad="42"/>
<contactref element="IC1" pad="85"/>
</signal>
<signal name="RAM1_D9">
<contactref element="U$1" pad="44"/>
<contactref element="IC1" pad="86"/>
</signal>
<signal name="RAM1_D10">
<contactref element="U$1" pad="45"/>
<contactref element="IC1" pad="87"/>
</signal>
<signal name="RAM1_D11">
<contactref element="U$1" pad="47"/>
<contactref element="IC1" pad="88"/>
</signal>
<signal name="RAM1_D12">
<contactref element="U$1" pad="48"/>
<contactref element="IC1" pad="89"/>
</signal>
<signal name="RAM1_D13">
<contactref element="U$1" pad="50"/>
<contactref element="IC1" pad="108"/>
</signal>
<signal name="RAM1_D14">
<contactref element="U$1" pad="51"/>
<contactref element="IC1" pad="109"/>
</signal>
<signal name="RAM1_D15">
<contactref element="U$1" pad="53"/>
<contactref element="IC1" pad="110"/>
</signal>
<signal name="RAM1_A1">
<contactref element="U$1" pad="24"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="RAM1_BA0">
<contactref element="U$1" pad="20"/>
<contactref element="IC1" pad="131"/>
</signal>
<signal name="RAM1_BA1">
<contactref element="U$1" pad="21"/>
<contactref element="IC1" pad="132"/>
</signal>
<signal name="RAM1_DQML">
<contactref element="U$1" pad="15"/>
<contactref element="IC1" pad="200"/>
</signal>
<signal name="RAM1_DQMH">
<contactref element="U$1" pad="39"/>
<contactref element="IC1" pad="201"/>
</signal>
<signal name="RAM1_CLK">
<contactref element="U$1" pad="38"/>
<contactref element="IC1" pad="135"/>
</signal>
<signal name="RAM1_CKE">
<contactref element="U$1" pad="37"/>
<contactref element="IC1" pad="38"/>
</signal>
<signal name="RAM1_WE">
<contactref element="U$1" pad="16"/>
<contactref element="IC1" pad="35"/>
</signal>
<signal name="RAM1_CS">
<contactref element="U$1" pad="19"/>
<contactref element="IC1" pad="37"/>
</signal>
<signal name="RAM1_RAS">
<contactref element="U$1" pad="18"/>
<contactref element="IC1" pad="70"/>
</signal>
<signal name="RAM1_CAS">
<contactref element="U$1" pad="17" route="any" routetag="G$1.!CAS"/>
<contactref element="IC1" pad="191"/>
</signal>
<signal name="TFT_LEDPWM">
<contactref element="TFT_CON" pad="1"/>
</signal>
<signal name="+5V_D">
<contactref element="TFT_CON" pad="2"/>
</signal>
<signal name="TFT_VSYNC">
<contactref element="TFT_CON" pad="33"/>
<contactref element="IC1" pad="53"/>
</signal>
<signal name="TFT_DE">
<contactref element="TFT_CON" pad="34"/>
<contactref element="IC1" pad="190"/>
</signal>
<signal name="TFT_R0">
<contactref element="TFT_CON" pad="5"/>
<contactref element="IC1" pad="64"/>
</signal>
<signal name="TFT_R1">
<contactref element="TFT_CON" pad="6"/>
<contactref element="IC1" pad="65"/>
</signal>
<signal name="TFT_R2">
<contactref element="TFT_CON" pad="7"/>
<contactref element="IC1" pad="66"/>
</signal>
<signal name="TFT_R3">
<contactref element="TFT_CON" pad="8"/>
<contactref element="IC1" pad="67"/>
</signal>
<signal name="TFT_R4">
<contactref element="TFT_CON" pad="9"/>
<contactref element="IC1" pad="68"/>
</signal>
<signal name="TFT_R5">
<contactref element="TFT_CON" pad="10"/>
<contactref element="IC1" pad="69"/>
</signal>
<signal name="TFT_R6">
<contactref element="TFT_CON" pad="11"/>
<contactref element="IC1" pad="95"/>
</signal>
<signal name="TFT_R7">
<contactref element="TFT_CON" pad="12"/>
<contactref element="IC1" pad="133"/>
</signal>
<signal name="TFT_G0">
<contactref element="TFT_CON" pad="13"/>
<contactref element="IC1" pad="62"/>
</signal>
<signal name="TFT_G1">
<contactref element="TFT_CON" pad="14"/>
<contactref element="IC1" pad="61"/>
</signal>
<signal name="TFT_G2">
<contactref element="TFT_CON" pad="15"/>
<contactref element="IC1" pad="151"/>
</signal>
<signal name="TFT_G3">
<contactref element="TFT_CON" pad="16"/>
<contactref element="IC1" pad="152"/>
</signal>
<signal name="TFT_G4">
<contactref element="TFT_CON" pad="17"/>
<contactref element="IC1" pad="153"/>
</signal>
<signal name="TFT_G5">
<contactref element="TFT_CON" pad="18"/>
<contactref element="IC1" pad="154"/>
</signal>
<signal name="TFT_G6">
<contactref element="TFT_CON" pad="19"/>
<contactref element="IC1" pad="155"/>
</signal>
<signal name="TFT_G7">
<contactref element="TFT_CON" pad="20"/>
<contactref element="IC1" pad="156"/>
</signal>
<signal name="TFT_B0">
<contactref element="TFT_CON" pad="21"/>
<contactref element="IC1" pad="174"/>
</signal>
<signal name="TFT_B1">
<contactref element="TFT_CON" pad="22"/>
<contactref element="IC1" pad="175"/>
</signal>
<signal name="TFT_B3">
<contactref element="TFT_CON" pad="24"/>
<contactref element="IC1" pad="177"/>
</signal>
<signal name="TFT_B2">
<contactref element="TFT_CON" pad="23"/>
<contactref element="IC1" pad="176"/>
</signal>
<signal name="TFT_B4">
<contactref element="TFT_CON" pad="25"/>
<contactref element="IC1" pad="186"/>
</signal>
<signal name="TFT_B5">
<contactref element="TFT_CON" pad="26"/>
<contactref element="IC1" pad="187"/>
</signal>
<signal name="TFT_B6">
<contactref element="TFT_CON" pad="27"/>
<contactref element="IC1" pad="188"/>
</signal>
<signal name="TFT_B7">
<contactref element="TFT_CON" pad="28"/>
<contactref element="IC1" pad="189"/>
</signal>
<signal name="TFT_CLK">
<contactref element="TFT_CON" pad="30"/>
<contactref element="IC1" pad="134"/>
</signal>
<signal name="TFT_HSYNC">
<contactref element="TFT_CON" pad="32"/>
<contactref element="IC1" pad="138"/>
</signal>
<signal name="N$6">
<contactref element="Y1" pad="2"/>
<contactref element="C_C41" pad="2"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="N$8">
<contactref element="Y1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="C_C40" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="C_C43" pad="1"/>
<contactref element="X2" pad="1"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="N$10">
<contactref element="C_C42" pad="1"/>
<contactref element="X2" pad="4"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="33"/>
</signal>
<signal name="N$2">
<contactref element="C_T5" pad="+"/>
<contactref element="IC1" pad="92"/>
</signal>
<signal name="N$3">
<contactref element="C_T4" pad="+"/>
<contactref element="IC1" pad="148"/>
</signal>
<signal name="ETH_MDC">
<contactref element="U2" pad="31"/>
<contactref element="IC1" pad="36"/>
</signal>
<signal name="ETH_CLK">
<contactref element="U2" pad="34"/>
<contactref element="SG7050CAN" pad="3"/>
<contactref element="IC1" pad="44"/>
</signal>
<signal name="ETH_MDIO">
<contactref element="U2" pad="30"/>
<contactref element="R29" pad="1"/>
<contactref element="IC1" pad="45"/>
</signal>
<signal name="ETH_CRS_DV">
<contactref element="U2" pad="40"/>
<contactref element="R27" pad="1"/>
<contactref element="IC1" pad="56"/>
</signal>
<signal name="ETH_RXD0">
<contactref element="U2" pad="43"/>
<contactref element="IC1" pad="57"/>
</signal>
<signal name="ETH_RXD1">
<contactref element="U2" pad="44"/>
<contactref element="IC1" pad="58"/>
</signal>
<signal name="ETH_TX_EN">
<contactref element="U2" pad="2"/>
<contactref element="IC1" pad="91"/>
</signal>
<signal name="ETH_TXD0">
<contactref element="U2" pad="3"/>
<contactref element="IC1" pad="104"/>
</signal>
<signal name="ETH_TXD1">
<contactref element="U2" pad="4"/>
<contactref element="IC1" pad="105"/>
</signal>
<signal name="+15V">
<contactref element="LM2576-3.3" pad="1"/>
<contactref element="C_A2_ESR" pad="+"/>
<contactref element="LM2576-5" pad="1"/>
<contactref element="C_A1_ESR" pad="+"/>
</signal>
<signal name="GND">
<contactref element="C_C21" pad="2"/>
<contactref element="C_C22" pad="2"/>
<contactref element="RJ1" pad="GND"/>
<contactref element="SG7050CAN" pad="2"/>
<contactref element="RESET_SW" pad="4"/>
<contactref element="C_C50" pad="2"/>
<contactref element="RESET_SW" pad="3"/>
<contactref element="769_BOOT_JMP" pad="1"/>
<contactref element="C_T5" pad="-"/>
<contactref element="C_T4" pad="-"/>
<contactref element="C_C26" pad="2"/>
<contactref element="C_C27" pad="2"/>
<contactref element="C_T6" pad="-"/>
<contactref element="C_C25" pad="2"/>
<contactref element="R24" pad="1"/>
<contactref element="U2" pad="47"/>
<contactref element="U2" pad="19"/>
<contactref element="U2" pad="15"/>
<contactref element="U2" pad="36"/>
<contactref element="U2" pad="35"/>
<contactref element="C_C28" pad="2"/>
<contactref element="C_C29" pad="2"/>
<contactref element="C_C30" pad="2"/>
<contactref element="U3" pad="15"/>
<contactref element="C_T10" pad="-"/>
<contactref element="C_T9" pad="+"/>
<contactref element="C_T11" pad="-"/>
<contactref element="RS232_CON" pad="2"/>
<contactref element="TFT_CON" pad="3"/>
<contactref element="TFT_CON" pad="29"/>
<contactref element="TFT_CON" pad="36"/>
<contactref element="C_C15" pad="2"/>
<contactref element="C_C14" pad="2"/>
<contactref element="C_C13" pad="2"/>
<contactref element="C_C12" pad="2"/>
<contactref element="C_C11" pad="2"/>
<contactref element="C_C10" pad="2"/>
<contactref element="C_C9" pad="2"/>
<contactref element="C_C8" pad="2"/>
<contactref element="C_C7" pad="2"/>
<contactref element="C_C6" pad="2"/>
<contactref element="C_C5" pad="2"/>
<contactref element="C_C4" pad="2"/>
<contactref element="C_C3" pad="2"/>
<contactref element="C_C2" pad="2"/>
<contactref element="C_C1" pad="2"/>
<contactref element="C_C16" pad="2"/>
<contactref element="C_C17" pad="2"/>
<contactref element="C_T1" pad="-"/>
<contactref element="C_C19" pad="2"/>
<contactref element="C_C18" pad="2"/>
<contactref element="C_C20" pad="2"/>
<contactref element="C_T3" pad="-"/>
<contactref element="C_T2" pad="-"/>
<contactref element="C_C41" pad="1"/>
<contactref element="C_C40" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="10"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="16"/>
<contactref element="C_C43" pad="2"/>
<contactref element="C_C42" pad="2"/>
<contactref element="RJ1" pad="SHIELD0"/>
<contactref element="RJ1" pad="SHIELD1"/>
<contactref element="C_C23" pad="2"/>
<contactref element="C_C24" pad="2"/>
<contactref element="C_C66" pad="2"/>
<contactref element="C_C65" pad="2"/>
<contactref element="C_C64" pad="2"/>
<contactref element="C_C63" pad="2"/>
<contactref element="C_C62" pad="2"/>
<contactref element="C_C61" pad="2"/>
<contactref element="C_C60" pad="2"/>
<contactref element="U$1" pad="54"/>
<contactref element="U$1" pad="28"/>
<contactref element="U$1" pad="41"/>
<contactref element="U$1" pad="52"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="12"/>
<contactref element="U$1" pad="46"/>
<contactref element="IC1" pad="202"/>
<contactref element="IC1" pad="184"/>
<contactref element="IC1" pad="170"/>
<contactref element="IC1" pad="149"/>
<contactref element="IC1" pad="136"/>
<contactref element="IC1" pad="114"/>
<contactref element="IC1" pad="93"/>
<contactref element="IC1" pad="82"/>
<contactref element="IC1" pad="72"/>
<contactref element="IC1" pad="60"/>
<contactref element="IC1" pad="51"/>
<contactref element="IC1" pad="25"/>
<contactref element="IC1" pad="14"/>
<contactref element="IC1" pad="40"/>
<contactref element="IC1" pad="128"/>
<contactref element="IC1" pad="122"/>
<contactref element="767_BOOT_JMP" pad="1"/>
<contactref element="C_T33" pad="-"/>
<contactref element="C_T34" pad="-"/>
<contactref element="C_C90" pad="2"/>
<contactref element="C_C91" pad="2"/>
<contactref element="C_C92" pad="2"/>
<contactref element="C_T31" pad="-"/>
<contactref element="C_T32" pad="-"/>
<contactref element="C_C94" pad="1"/>
<contactref element="C_C93" pad="1"/>
<contactref element="IC2" pad="99"/>
<contactref element="IC2" pad="49"/>
<contactref element="IC2" pad="74"/>
<contactref element="IC2" pad="26"/>
<contactref element="IC2" pad="10"/>
<contactref element="C_C84" pad="2"/>
<contactref element="C_C83" pad="2"/>
<contactref element="C_C82" pad="2"/>
<contactref element="C_C81" pad="2"/>
<contactref element="C_C80" pad="2"/>
<contactref element="C_T30" pad="-"/>
<contactref element="IC2" pad="19"/>
<contactref element="U5" pad="6"/>
<contactref element="U5" pad="4"/>
<contactref element="U5" pad="8"/>
<contactref element="U5" pad="10"/>
<contactref element="U5" pad="12"/>
<contactref element="U5" pad="14"/>
<contactref element="U5" pad="20"/>
<contactref element="U5" pad="18"/>
<contactref element="U5" pad="16"/>
</signal>
<signal name="N$13">
<contactref element="LM2576-5" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="LM2576-3.3" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="L2" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="R3" pad="2"/>
<contactref element="R20" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="C_C21" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="R23" pad="2"/>
<contactref element="C_C22" pad="1"/>
<contactref element="C_C24" pad="1"/>
<contactref element="RJ1" pad="P5"/>
<contactref element="RJ1" pad="P4"/>
<contactref element="C_C23" pad="1"/>
<contactref element="C_C20" pad="1"/>
<contactref element="C_C19" pad="1"/>
<contactref element="C_C18" pad="1"/>
<contactref element="769_BOOT_JMP" pad="3"/>
<contactref element="C_T3" pad="+"/>
<contactref element="C_T2" pad="+"/>
<contactref element="RJ1" pad="Y+"/>
<contactref element="RJ1" pad="G+"/>
<contactref element="R29" pad="2"/>
<contactref element="SG7050CAN" pad="1"/>
<contactref element="SG7050CAN" pad="4"/>
<contactref element="U2" pad="32"/>
<contactref element="U2" pad="22"/>
<contactref element="U2" pad="48"/>
<contactref element="R28" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="C_C28" pad="1"/>
<contactref element="C_C29" pad="1"/>
<contactref element="C_C30" pad="1"/>
<contactref element="R31" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="TOUCH_CON" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="U3" pad="16"/>
<contactref element="C_T10" pad="+"/>
<contactref element="TFT_CON" pad="4"/>
<contactref element="TFT_CON" pad="31"/>
<contactref element="C_C15" pad="1"/>
<contactref element="C_C14" pad="1"/>
<contactref element="C_C13" pad="1"/>
<contactref element="C_C12" pad="1"/>
<contactref element="C_C11" pad="1"/>
<contactref element="C_C10" pad="1"/>
<contactref element="C_C9" pad="1"/>
<contactref element="C_C8" pad="1"/>
<contactref element="C_C7" pad="1"/>
<contactref element="C_C6" pad="1"/>
<contactref element="C_C5" pad="1"/>
<contactref element="C_C4" pad="1"/>
<contactref element="C_C3" pad="1"/>
<contactref element="C_C2" pad="1"/>
<contactref element="C_C1" pad="1"/>
<contactref element="C_C16" pad="1"/>
<contactref element="C_C17" pad="1"/>
<contactref element="C_T1" pad="+"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="C_C63" pad="1"/>
<contactref element="C_C64" pad="1"/>
<contactref element="C_C60" pad="1"/>
<contactref element="C_C61" pad="1"/>
<contactref element="C_C62" pad="1"/>
<contactref element="C_C65" pad="1"/>
<contactref element="C_C66" pad="1"/>
<contactref element="U$1" pad="27"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="14"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="49"/>
<contactref element="U$1" pad="43"/>
<contactref element="U$1" pad="9"/>
<contactref element="IC1" pad="204"/>
<contactref element="IC1" pad="185"/>
<contactref element="IC1" pad="150"/>
<contactref element="IC1" pad="115"/>
<contactref element="IC1" pad="94"/>
<contactref element="IC1" pad="83"/>
<contactref element="IC1" pad="73"/>
<contactref element="IC1" pad="59"/>
<contactref element="IC1" pad="52"/>
<contactref element="IC1" pad="26"/>
<contactref element="IC1" pad="15"/>
<contactref element="IC1" pad="158"/>
<contactref element="IC1" pad="103"/>
<contactref element="IC1" pad="39"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="41"/>
<contactref element="IC1" pad="42"/>
<contactref element="IC1" pad="203"/>
<contactref element="IC1" pad="118"/>
<contactref element="IC1" pad="137"/>
<contactref element="IC1" pad="171"/>
<contactref element="C_C92" pad="1"/>
<contactref element="C_C90" pad="1"/>
<contactref element="C_C91" pad="1"/>
<contactref element="767_BOOT_JMP" pad="3"/>
<contactref element="C_T31" pad="+"/>
<contactref element="C_T32" pad="+"/>
<contactref element="IC2" pad="100"/>
<contactref element="IC2" pad="50"/>
<contactref element="IC2" pad="75"/>
<contactref element="IC2" pad="27"/>
<contactref element="IC2" pad="11"/>
<contactref element="C_C84" pad="1"/>
<contactref element="C_C83" pad="1"/>
<contactref element="C_C82" pad="1"/>
<contactref element="C_C81" pad="1"/>
<contactref element="C_C80" pad="1"/>
<contactref element="C_T30" pad="+"/>
<contactref element="IC2" pad="6"/>
<contactref element="IC2" pad="20"/>
<contactref element="IC2" pad="21"/>
<contactref element="U5" pad="2"/>
<contactref element="U5" pad="1"/>
</signal>
<signal name="RJ45_TD-">
<contactref element="U2" pad="16"/>
<contactref element="R22" pad="2"/>
<contactref element="RJ1" pad="TD-"/>
</signal>
<signal name="RJ45_TD+">
<contactref element="U2" pad="17"/>
<contactref element="R23" pad="1"/>
<contactref element="RJ1" pad="TD+"/>
</signal>
<signal name="RJ45_RD+">
<contactref element="U2" pad="14"/>
<contactref element="R21" pad="1"/>
<contactref element="RJ1" pad="RD+"/>
</signal>
<signal name="RJ45_RD-">
<contactref element="U2" pad="13"/>
<contactref element="R20" pad="2"/>
<contactref element="RJ1" pad="RD-"/>
</signal>
<signal name="ETH_LINK">
<contactref element="U2" pad="28"/>
<contactref element="R41" pad="2"/>
<contactref element="IC1" pad="106"/>
</signal>
<signal name="LED_ACT">
<contactref element="U2" pad="26"/>
<contactref element="R40" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="RJ1" pad="G-"/>
<contactref element="R40" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="RJ1" pad="Y-"/>
<contactref element="R41" pad="1"/>
</signal>
<signal name="RES_2">
<contactref element="U2" pad="20"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="RES_1">
<contactref element="U2" pad="21"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="U2" pad="39"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="TOUCH_INT">
<contactref element="TOUCH_CON" pad="1"/>
<contactref element="IC1" pad="111"/>
</signal>
<signal name="TOUCH_I2C_SDA">
<contactref element="TOUCH_CON" pad="3"/>
<contactref element="R31" pad="1"/>
<contactref element="IC1" pad="113"/>
</signal>
<signal name="TOUCH_I2C_SCL">
<contactref element="TOUCH_CON" pad="4"/>
<contactref element="R30" pad="1"/>
<contactref element="IC1" pad="112"/>
</signal>
<signal name="N$26">
<contactref element="U3" pad="4"/>
<contactref element="C_T8" pad="+"/>
</signal>
<signal name="N$27">
<contactref element="U3" pad="5"/>
<contactref element="C_T8" pad="-"/>
</signal>
<signal name="N$22">
<contactref element="U3" pad="3"/>
<contactref element="C_T7" pad="-"/>
</signal>
<signal name="N$23">
<contactref element="U3" pad="1"/>
<contactref element="C_T7" pad="+"/>
</signal>
<signal name="N$24">
<contactref element="U3" pad="6"/>
<contactref element="C_T9" pad="-"/>
</signal>
<signal name="N$29">
<contactref element="U3" pad="2"/>
<contactref element="C_T11" pad="+"/>
</signal>
<signal name="UART_TX">
<contactref element="U3" pad="11"/>
<contactref element="IC1" pad="161"/>
</signal>
<signal name="UART_RX">
<contactref element="U3" pad="12"/>
<contactref element="IC1" pad="162"/>
</signal>
<signal name="RS232_RX">
<contactref element="U3" pad="13"/>
<contactref element="RS232_CON" pad="3"/>
</signal>
<signal name="RBIAS">
<contactref element="U2" pad="24"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="PFB">
<contactref element="U2" pad="18"/>
<contactref element="U2" pad="23"/>
<contactref element="C_C26" pad="1"/>
<contactref element="C_C27" pad="1"/>
<contactref element="C_T6" pad="+"/>
<contactref element="C_C25" pad="1"/>
<contactref element="U2" pad="37"/>
</signal>
<signal name="RS232_TX">
<contactref element="U3" pad="14"/>
<contactref element="RS232_CON" pad="1"/>
</signal>
<signal name="AVCC_2">
<contactref element="U4" pad="1"/>
</signal>
<signal name="AVCC_3">
<contactref element="U4" pad="38"/>
</signal>
<signal name="AVCC_4">
<contactref element="U4" pad="37"/>
</signal>
<signal name="AVCC">
<contactref element="U4" pad="48"/>
</signal>
<signal name="VDRIVE">
<contactref element="U4" pad="23"/>
</signal>
<signal name="ADC_DB0">
<contactref element="U4" pad="16"/>
<contactref element="IC2" pad="61"/>
</signal>
<signal name="ADC_DB1">
<contactref element="U4" pad="17"/>
<contactref element="IC2" pad="62"/>
</signal>
<signal name="ADC_DB2">
<contactref element="U4" pad="18"/>
<contactref element="IC2" pad="81"/>
</signal>
<signal name="ADC_DB3">
<contactref element="U4" pad="19"/>
<contactref element="IC2" pad="82"/>
</signal>
<signal name="ADC_DB4">
<contactref element="U4" pad="20"/>
<contactref element="IC2" pad="37"/>
</signal>
<signal name="ADC_DB5">
<contactref element="U4" pad="21"/>
<contactref element="IC2" pad="38"/>
</signal>
<signal name="ADC_DB6">
<contactref element="U4" pad="22"/>
<contactref element="IC2" pad="39"/>
</signal>
<signal name="ADC_DB9">
<contactref element="U4" pad="27"/>
<contactref element="IC2" pad="42"/>
</signal>
<signal name="ADC_DB10">
<contactref element="U4" pad="28"/>
<contactref element="IC2" pad="43"/>
</signal>
<signal name="ADC_DB11">
<contactref element="U4" pad="29"/>
<contactref element="IC2" pad="44"/>
</signal>
<signal name="ADC_DB12">
<contactref element="U4" pad="30"/>
<contactref element="IC2" pad="45"/>
</signal>
<signal name="ADC_DB13">
<contactref element="U4" pad="31"/>
<contactref element="IC2" pad="55"/>
</signal>
<signal name="ADC_DB14">
<contactref element="U4" pad="32"/>
<contactref element="IC2" pad="56"/>
</signal>
<signal name="ADC_DB7">
<contactref element="U4" pad="24"/>
<contactref element="IC2" pad="40"/>
</signal>
<signal name="ADC_DB15">
<contactref element="U4" pad="33"/>
<contactref element="IC2" pad="57"/>
</signal>
<signal name="ADC_DB8">
<contactref element="U4" pad="25"/>
<contactref element="IC2" pad="41"/>
</signal>
<signal name="QSPI_NCS">
<contactref element="IC1" pad="90"/>
</signal>
<signal name="QSPI_CLK">
<contactref element="IC1" pad="63"/>
</signal>
<signal name="QSPI_IO3">
<contactref element="IC1" pad="27"/>
</signal>
<signal name="QSPI_IO2">
<contactref element="IC1" pad="28"/>
</signal>
<signal name="QSPI_IO0">
<contactref element="IC1" pad="29"/>
</signal>
<signal name="QSPI_IO1">
<contactref element="IC1" pad="30"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="119"/>
<contactref element="IC1" pad="125"/>
</signal>
<signal name="N$16">
<contactref element="LM2576-3.3" pad="4"/>
<contactref element="L2" pad="1"/>
<contactref element="C_A4_ESR" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="LM2576-5" pad="4"/>
<contactref element="L1" pad="1"/>
<contactref element="C_A3_ESR" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="C_A2_ESR" pad="-"/>
<contactref element="LM2576-3.3" pad="3"/>
<contactref element="LM2576-3.3" pad="5"/>
<contactref element="D2" pad="A"/>
<contactref element="C_A4_ESR" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="C_A1_ESR" pad="-"/>
<contactref element="LM2576-5" pad="3"/>
<contactref element="LM2576-5" pad="5"/>
<contactref element="D1" pad="A"/>
<contactref element="C_A3_ESR" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="R80" pad="2"/>
<contactref element="IC2" pad="94"/>
</signal>
<signal name="N$30">
<contactref element="R80" pad="1"/>
<contactref element="767_BOOT_JMP" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="Y2" pad="2"/>
<contactref element="C_C94" pad="2"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="N$32">
<contactref element="Y2" pad="1"/>
<contactref element="R81" pad="1"/>
<contactref element="C_C93" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="R81" pad="2"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="N$34">
<contactref element="C_T34" pad="+"/>
<contactref element="IC2" pad="48"/>
</signal>
<signal name="N$35">
<contactref element="C_T33" pad="+"/>
<contactref element="IC2" pad="73"/>
</signal>
<signal name="767_DEBUG_SWDIO">
<contactref element="IC2" pad="72"/>
<contactref element="U5" pad="7"/>
</signal>
<signal name="767_DEBUG_SWCLK">
<contactref element="IC2" pad="76"/>
<contactref element="U5" pad="9"/>
</signal>
<signal name="767_DEBUG_SWO">
<contactref element="IC2" pad="89"/>
<contactref element="U5" pad="13"/>
</signal>
<signal name="769_DEBUG_SWDIO">
<contactref element="IC1" pad="147"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="769_DEBUG_SWCLK">
<contactref element="IC1" pad="159"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="769_DEBUG_SWO">
<contactref element="IC1" pad="192"/>
<contactref element="U1" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
