<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;ARM 32-bit Cortex™ MCUs&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by jb@jenszuhause.de&lt;/author&gt;&lt;p&gt;
&lt;b&gt;You are using this libary by your own risk.&lt;/b&gt;&lt;br&gt;
&lt;b&gt;Make sure to check everything well due to this libary before using it.&lt;/b&gt;</description>
<packages>
<package name="LFBGA100">
<description>&lt;b&gt;LFBGA100&lt;/b&gt;&lt;p&gt;
10 x 10 mm, 10 x 10-pin low profil 0.8 mm pitch ball grid array package</description>
</package>
<package name="LFBGA144">
<description>&lt;b&gt;LFBGA144&lt;/b&gt;&lt;p&gt;
10 x 10 mm, 12 x 12-pin low profil 0.8 mm pitch ball grid array package</description>
</package>
<package name="LQFP32">
<description>&lt;b&gt;LQFP32&lt;/b&gt;&lt;p&gt;
7 x 7 mm, 32-pin low-profile quad flat package</description>
</package>
<package name="LQFP48">
<description>&lt;b&gt;LQFP48&lt;/b&gt;&lt;p&gt;
7 x 7 mm, 48-pin low-profile quad flat package</description>
</package>
<package name="LQFP64">
<description>&lt;b&gt;LQFP64&lt;/b&gt;&lt;p&gt;
10 x 10 mm, 64-pin low-profile quad flat package</description>
</package>
<package name="LQFP100">
<description>&lt;b&gt;LQFP100&lt;/b&gt;&lt;p&gt;
14 x 14 mm, 100-pin low-profile quad flat package</description>
</package>
<package name="LQFP144">
<description>&lt;b&gt;LQFP144&lt;/b&gt;&lt;p&gt;
20 x 20 mm, 144-pin low-profile quad flat package</description>
</package>
<package name="LQFP176">
<description>&lt;b&gt;LQFP176&lt;/b&gt;&lt;p&gt;
24 x 24 mm, 176-pin low-profile quad flat package</description>
</package>
<package name="LQFP208">
<description>&lt;b&gt;LQFP208&lt;/b&gt;&lt;p&gt;
28 x 28 mm, 208-pin low-profile quad flat package</description>
</package>
<package name="TFBGA64">
<description>&lt;b&gt;TFBGA64&lt;/b&gt;&lt;p&gt;
5 x 5 mm, 8 x 8-pin thin  0.5 mm pitch ball grid array package</description>
</package>
<package name="TFBGA216">
<description>&lt;b&gt;TFBGA216&lt;/b&gt;&lt;p&gt;
13 x 13 mm, 15 x 15-pin thin fine 0.8 mm pitch ball grid array package</description>
</package>
<package name="TSSOP20-I">
<description>&lt;b&gt;TSSOP20-I&lt;/b&gt;&lt;p&gt;
20-pin thin shrink small outline package</description>
</package>
<package name="UFBGA100">
<description>&lt;b&gt;UFBGA100&lt;/b&gt;&lt;p&gt;
7 x 7 mm, 12 x 12-pin ultra fine 0.5 mm pitch ball grid array package</description>
</package>
<package name="UFBGA132">
<description>&lt;b&gt;UFBGA132&lt;/b&gt;&lt;p&gt;
7 x 7 mm, 12 x 12-pin ultra fine 0.5 mm pitch ball grid array package</description>
</package>
<package name="UFBGA176+25">
<description>&lt;b&gt;UFBGA176+25&lt;/b&gt;&lt;p&gt;
10 x 10 mm, 15 x 15-pin ultra fine 0.65 mm pitch ball grid array package</description>
</package>
<package name="UFQFPN28">
<description>&lt;b&gt;UFQFPN28&lt;/b&gt;&lt;p&gt;
4 x 4 mm, 28-pin ultra thin fine pitch quad flat no-lead package</description>
</package>
<package name="UFQFPN32">
<description>&lt;b&gt;UFQFPN32&lt;/b&gt;&lt;p&gt;
5 x 5 mm, 32-pin ultra thin fine pitch quad flat no-lead package</description>
</package>
<package name="UFQFPN48">
<description>&lt;b&gt;UFQFPN48&lt;/b&gt;&lt;p&gt;
7 x 7 mm, 48-pin ultra thin 0.5 mm pitch quad flat no-lead package</description>
</package>
<package name="VFQFPN36">
<description>&lt;b&gt;VFQFPN36&lt;/b&gt;&lt;p&gt;
6 x 6 mm, 36-pin very thin 0.5 mm pitch quad flat no-lead package</description>
</package>
<package name="VFQFPN40">
<description>&lt;b&gt;VFQFPN40&lt;/b&gt;&lt;p&gt;
6 x 6 mm, 40-pin very thin 0.5 mm pitch quad flat no-lead package</description>
</package>
<package name="VFQFPN48">
<description>&lt;b&gt;VFQFPN48&lt;/b&gt;&lt;p&gt;
7 x 7 mm, 48-pin very thin 0.5 mm pitch quad flat no-lead package</description>
</package>
<package name="WLCSP49">
<description>&lt;b&gt;WLCSP49&lt;/b&gt;&lt;p&gt;
2.965 x 2.965 mm, 7 x 7-pin 0.4 mm pitch wafer-level chip-scale package</description>
</package>
<package name="WLCSP63">
<description>&lt;b&gt;WLCSP63&lt;/b&gt;&lt;p&gt;
3.228 x 4.164 mm, 7 x 9-pin 0.4 mm pitch wafer-level chip-scale package</description>
</package>
<package name="WLCSP64">
<description>&lt;b&gt;WLCSP64&lt;/b&gt;&lt;p&gt;
4.466 x 4.395 mm, 8 x 8-pin 0.5 mm pitch wafer-level chip-scale package</description>
</package>
<package name="WLCSP64+2">
<description>&lt;b&gt;WLCSP64+2&lt;/b&gt;&lt;p&gt;
3.639 x 3.971 mm, 9 x 9-pin 0.4 mm pitch wafer-level chip-scale package</description>
</package>
<package name="WLCSP64_0.4MM">
<description>&lt;b&gt;WLCSP64&lt;/b&gt;&lt;p&gt;
4.539 x 4.911 mm, 8 x 8-pin 0.4 mm pitch wafer-level chip-scale package</description>
</package>
<package name="WLCSP66">
<description>&lt;b&gt;WLCSP66&lt;/b&gt;&lt;p&gt;
3.767 x 4.229 mm, 8 x 9-pin 0.4 mm pitch wafer-level chip-scale package</description>
</package>
<package name="WLCSP90">
<description>&lt;b&gt;WLCSP90&lt;/b&gt;&lt;p&gt;
4.218 x 3.969 mm, 10 x 9-pin 0.4 mm pitch wafer-level chip-scale package</description>
</package>
<package name="WLCSP143">
<description>&lt;b&gt;WLCSP143&lt;/b&gt;&lt;p&gt;
4.521 x 5.547 mm, 11 x 13-pin 0.4 mm pitch wafer-level chip-scale package</description>
</package>
<package name="UFBGA144">
<description>&lt;b&gt;UFBGA144&lt;/b&gt;&lt;p&gt;
7 x 7 mm, 12 x 12-pin ultra fine 0.5 mm pitch ball grid array package</description>
</package>
<package name="WLCSP72">
<description>&lt;b&gt;WLCSP72&lt;/b&gt;&lt;p&gt;
4,4084 x 3,7594 mm, 9 x 9-pin 0.4 mm pitch wafer-level chip-scale package</description>
</package>
</packages>
<symbols>
<symbol name="STM32_20PIN_TYP1">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB1"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
</symbol>
<symbol name="STM32_28PIN_TYP1">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
</symbol>
<symbol name="STM32_32PIN_TYP1">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
</symbol>
<symbol name="STM32_32PIN_TYP2">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
</symbol>
<symbol name="STM32_36PIN_TYP1">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="VSSA" direction="pwr"/>
</symbol>
<symbol name="STM32_48PIN_TYP1">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
</symbol>
<symbol name="STM32_48PIN_TYP2">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
</symbol>
<symbol name="STM32_48PIN_TYP3">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
</symbol>
<symbol name="STM32_48PIN_TYP4">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="NPOR" direction="in"/>
</symbol>
<symbol name="STM32_48PIN_TYP5">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PD8"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PF7"/>
<pin name="PF6"/>
<pin name="VREFSD+" direction="pwr"/>
<pin name="VREFSD-" direction="pwr"/>
<pin name="VDDSD" direction="pwr"/>
<pin name="PB2"/>
</symbol>
<symbol name="STM32_48PIN_TYP6">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PD8"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PF7"/>
<pin name="PF6"/>
<pin name="VREFSD+" direction="pwr"/>
<pin name="VREFSD-" direction="pwr"/>
<pin name="VDDSD" direction="pwr"/>
<pin name="NPOR" direction="in"/>
</symbol>
<symbol name="STM32_48PIN_TYP7">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VCAP1" direction="pwr"/>
</symbol>
<symbol name="STM32_48PIN_TYP8">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VLCD" direction="pwr"/>
</symbol>
<symbol name="STM32_49PIN_TYP1">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="PDR_ON" direction="in"/>
</symbol>
<symbol name="STM32_63PIN_TYP1">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VLCD" direction="pwr"/>
</symbol>
<symbol name="STM32_64PIN_TYP1">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
</symbol>
<symbol name="STM32_64PIN_TYP2">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="VBAT" direction="pwr"/>
</symbol>
<symbol name="STM32_64PIN_TYP3">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
</symbol>
<symbol name="STM32_64PIN_TYP4">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
</symbol>
<symbol name="STM32_64PIN_TYP5">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
</symbol>
<symbol name="STM32_64PIN_TYP6">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PF4"/>
</symbol>
<symbol name="STM32_64PIN_TYP7">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PF4"/>
<pin name="NPOR" direction="in"/>
</symbol>
<symbol name="STM32_64PIN_TYP8">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PD8"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PF7"/>
<pin name="PF6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VREFSD+" direction="pwr"/>
<pin name="VREFSD-" direction="pwr"/>
<pin name="VDDSD" direction="pwr"/>
</symbol>
<symbol name="STM32_64PIN_TYP9">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PD8"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PF7"/>
<pin name="PF6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VREFSD+" direction="pwr"/>
<pin name="VREFSD-" direction="pwr"/>
<pin name="VDDSD" direction="pwr"/>
<pin name="NPOR" direction="in"/>
</symbol>
<symbol name="STM32_64PIN_TYP10">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VCAP1" direction="pwr"/>
</symbol>
<symbol name="STM32_64PIN_TYP11">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VLCD" direction="pwr"/>
</symbol>
<symbol name="STM32_64PIN_TYP12">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VLCD" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
</symbol>
<symbol name="STM32_66PIN_TYP1">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VBAT" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
<pin name="IRROFF" direction="in"/>
<pin name="REGOFF" direction="in"/>
</symbol>
<symbol name="STM32_66PIN_TYP2">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PD8"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PF7"/>
<pin name="PF6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VREFSD+" direction="pwr"/>
<pin name="VREFSD-" direction="pwr"/>
<pin name="VDDSD" direction="pwr"/>
<pin name="NPOR" direction="in"/>
</symbol>
<symbol name="STM32_90PIN_TYP1">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PD8"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PI0"/>
<pin name="PI1"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
<pin name="PDR_ON" direction="in"/>
<pin name="BYPASS_REG" direction="in"/>
<pin name="PC0"/>
<pin name="PB10"/>
<pin name="PB2"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
</symbol>
<symbol name="STM32_100PIN_TYP1">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PD8"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB2"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF-" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
</symbol>
<symbol name="STM32_100PIN_TYP2">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PD8"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB2"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
<pin name="RFU" direction="in"/>
</symbol>
<symbol name="STM32_100PIN_TYP3">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PD8"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB2"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PF2"/>
<pin name="PF4"/>
<pin name="PF6"/>
<pin name="PF9"/>
<pin name="PF10"/>
</symbol>
<symbol name="STM32_100PIN_TYP4">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PD8"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PF2"/>
<pin name="PF4"/>
<pin name="PF6"/>
<pin name="PF9"/>
<pin name="PF10"/>
<pin name="NPOR" direction="in"/>
</symbol>
<symbol name="STM32_100PIN_TYP5">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PD8"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB2"/>
<pin name="PB10"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PF2"/>
<pin name="PF4"/>
<pin name="PF6"/>
<pin name="PF9"/>
<pin name="PF10"/>
<pin name="VREFSD+" direction="pwr"/>
<pin name="VREFSD-" direction="pwr"/>
<pin name="VDDSD12" direction="pwr"/>
<pin name="VDDSD3" direction="pwr"/>
<pin name="VSSSD" direction="pwr"/>
</symbol>
<symbol name="STM32_100PIN_TYP6">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PD8"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PF2"/>
<pin name="PF4"/>
<pin name="PF6"/>
<pin name="PF9"/>
<pin name="PF10"/>
<pin name="VREFSD+" direction="pwr"/>
<pin name="VREFSD-" direction="pwr"/>
<pin name="VDDSD12" direction="pwr"/>
<pin name="VDDSD3" direction="pwr"/>
<pin name="VSSSD" direction="pwr"/>
<pin name="NPOR" direction="in"/>
</symbol>
<symbol name="STM32_100PIN_TYP7">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PD8"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PB2"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
</symbol>
<symbol name="STM32_100PIN_TYP8">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PB2"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
<pin name="PB11"/>
<pin name="VREF-" direction="pwr"/>
<pin name="BYPASS_REG" direction="in"/>
<pin name="PDR_ON" direction="in"/>
</symbol>
<symbol name="STM32_100PIN_TYP9">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PB2"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
<pin name="PB11"/>
<pin name="PD8"/>
</symbol>
<symbol name="STM32_100PIN_TYP10">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VREF-" direction="pwr"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PB2"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="VLCD" direction="pwr"/>
<pin name="PB11"/>
<pin name="PD8"/>
<pin name="PH2"/>
</symbol>
<symbol name="STM32_132PIN_TYP1">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PB2"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="VLCD" direction="pwr"/>
<pin name="PB11"/>
<pin name="PD8"/>
<pin name="PH2"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="OPAMP1" direction="pwr"/>
<pin name="OPAMP2" direction="pwr"/>
<pin name="OPAMP3" direction="pwr"/>
<pin name="PC2"/>
</symbol>
<symbol name="STM32_143PIN_TYP1">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PB2"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="PB11"/>
<pin name="PD8"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PF10"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG11"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
<pin name="BYPASS_REG" direction="in"/>
<pin name="PDR_ON" direction="in"/>
</symbol>
<symbol name="STM32_144PIN_TYP1">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PB2"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB11"/>
<pin name="PD8"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PF10"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG11"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VREF-" direction="pwr"/>
</symbol>
<symbol name="STM32_144PIN_TYP2">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PB2"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB11"/>
<pin name="PD8"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PF10"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG11"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
<pin name="RFU" direction="in"/>
</symbol>
<symbol name="STM32_144PIN_TYP3">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PB2"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB11"/>
<pin name="PD8"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PF10"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG11"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
<pin name="PDR_ON" direction="in"/>
</symbol>
<symbol name="STM32_144PIN_TYP4">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PB2"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB11"/>
<pin name="PD8"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PF10"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG11"/>
<pin name="VREF-" direction="pwr"/>
<pin name="VLCD" direction="pwr"/>
<pin name="PH2"/>
</symbol>
<symbol name="STM32_144PIN_TYP5">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PB2"/>
<pin name="PD8"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PF10"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG11"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PH8"/>
<pin name="PH9"/>
<pin name="PH10"/>
<pin name="PH11"/>
<pin name="PH12"/>
<pin name="PH13"/>
<pin name="PH14"/>
<pin name="PH15"/>
<pin name="PI0"/>
<pin name="PI1"/>
<pin name="PI2"/>
<pin name="PI3"/>
<pin name="PI4"/>
<pin name="PI5"/>
<pin name="PI6"/>
<pin name="PI7"/>
<pin name="PI8"/>
<pin name="PI9"/>
<pin name="PI10"/>
<pin name="PI11"/>
<pin name="PI12"/>
<pin name="PI13"/>
<pin name="PI14"/>
<pin name="PI15"/>
<pin name="PH1"/>
<pin name="PH0"/>
</symbol>
<symbol name="STM32_176PIN_TYP1">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PB2"/>
<pin name="PD8"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PF10"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG11"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PH8"/>
<pin name="PH9"/>
<pin name="PH10"/>
<pin name="PH11"/>
<pin name="PH12"/>
<pin name="PH13"/>
<pin name="PH14"/>
<pin name="PH15"/>
<pin name="PI0"/>
<pin name="PI1"/>
<pin name="PI2"/>
<pin name="PI3"/>
<pin name="PI4"/>
<pin name="PI5"/>
<pin name="PI6"/>
<pin name="PI7"/>
<pin name="PI8"/>
<pin name="PI9"/>
<pin name="PI10"/>
<pin name="PI11"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
<pin name="PDR_ON" direction="in"/>
</symbol>
<symbol name="STM32_176PIN_TYP2">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PB2"/>
<pin name="PD8"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PF10"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG11"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PH8"/>
<pin name="PH9"/>
<pin name="PH10"/>
<pin name="PH11"/>
<pin name="PH12"/>
<pin name="PH13"/>
<pin name="PH14"/>
<pin name="PH15"/>
<pin name="PI0"/>
<pin name="PI1"/>
<pin name="PI2"/>
<pin name="PI3"/>
<pin name="PI4"/>
<pin name="PI5"/>
<pin name="PI6"/>
<pin name="PI7"/>
<pin name="PI8"/>
<pin name="PI9"/>
<pin name="PI10"/>
<pin name="PI11"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
<pin name="REGOFF" direction="in"/>
<pin name="VREF-" direction="pwr"/>
<pin name="RFU" direction="in"/>
</symbol>
<symbol name="STM32_176PIN_TYP3">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PB2"/>
<pin name="PD8"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PF10"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG11"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PH8"/>
<pin name="PH9"/>
<pin name="PH10"/>
<pin name="PH11"/>
<pin name="PH12"/>
<pin name="PH13"/>
<pin name="PH14"/>
<pin name="PH15"/>
<pin name="PI0"/>
<pin name="PI1"/>
<pin name="PI2"/>
<pin name="PI3"/>
<pin name="PI4"/>
<pin name="PI5"/>
<pin name="PI6"/>
<pin name="PI7"/>
<pin name="PI8"/>
<pin name="PI9"/>
<pin name="PI10"/>
<pin name="PI11"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
<pin name="BYPASS_REG" direction="in"/>
<pin name="PDR_ON" direction="in"/>
</symbol>
<symbol name="STM32_176PIN_TYP4">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PB2"/>
<pin name="PD8"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PF10"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG11"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PH8"/>
<pin name="PH9"/>
<pin name="PH10"/>
<pin name="PH11"/>
<pin name="PH12"/>
<pin name="PH13"/>
<pin name="PH14"/>
<pin name="PH15"/>
<pin name="PI0"/>
<pin name="PI1"/>
<pin name="PI2"/>
<pin name="PI3"/>
<pin name="PI4"/>
<pin name="PI5"/>
<pin name="PI6"/>
<pin name="PI7"/>
<pin name="PI8"/>
<pin name="PI9"/>
<pin name="PI10"/>
<pin name="PI11"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
<pin name="BYPASS_REG" direction="in"/>
<pin name="PDR_ON" direction="in"/>
<pin name="VREF-" direction="pwr"/>
</symbol>
<symbol name="STM32_176PIN_TYP5">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PB2"/>
<pin name="PD8"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PF10"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG11"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PH8"/>
<pin name="PH9"/>
<pin name="PH10"/>
<pin name="PH11"/>
<pin name="PH12"/>
<pin name="PH13"/>
<pin name="PH14"/>
<pin name="PH15"/>
<pin name="PI0"/>
<pin name="PI1"/>
<pin name="PI2"/>
<pin name="PI3"/>
<pin name="PI4"/>
<pin name="PI5"/>
<pin name="PI6"/>
<pin name="PI7"/>
<pin name="PI8"/>
<pin name="PI9"/>
<pin name="PI10"/>
<pin name="PI11"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
<pin name="BYPASS_REG" direction="in"/>
<pin name="PDR_ON" direction="in"/>
</symbol>
<symbol name="STM32_208PIN_TYP1">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PB2"/>
<pin name="PD8"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PF10"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG11"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PH8"/>
<pin name="PH9"/>
<pin name="PH10"/>
<pin name="PH11"/>
<pin name="PH12"/>
<pin name="PH13"/>
<pin name="PH14"/>
<pin name="PH15"/>
<pin name="PI0"/>
<pin name="PI1"/>
<pin name="PI2"/>
<pin name="PI3"/>
<pin name="PI4"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
<pin name="PDR_ON" direction="in"/>
<pin name="PI5"/>
<pin name="PI6"/>
<pin name="PI7"/>
<pin name="PI8"/>
<pin name="PI9"/>
<pin name="PI10"/>
<pin name="PI11"/>
<pin name="PI12"/>
<pin name="PI13"/>
<pin name="PI14"/>
<pin name="PI15"/>
<pin name="PJ0"/>
<pin name="PJ1"/>
<pin name="PJ2"/>
<pin name="PJ3"/>
<pin name="PJ4"/>
<pin name="PJ5"/>
<pin name="PJ6"/>
<pin name="PJ7"/>
<pin name="PJ8"/>
<pin name="PJ9"/>
<pin name="PJ10"/>
<pin name="PJ11"/>
<pin name="PJ12"/>
<pin name="PJ13"/>
<pin name="PJ14"/>
<pin name="PJ15"/>
<pin name="PK0"/>
<pin name="PK1"/>
<pin name="PK2"/>
<pin name="PK3"/>
<pin name="PK4"/>
<pin name="PK5"/>
<pin name="PK6"/>
<pin name="PK7"/>
</symbol>
<symbol name="STM32_216PIN_TYP1">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PB2"/>
<pin name="PD8"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PF10"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG11"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PH8"/>
<pin name="PH9"/>
<pin name="PH10"/>
<pin name="PH11"/>
<pin name="PH12"/>
<pin name="PH13"/>
<pin name="PH14"/>
<pin name="PH15"/>
<pin name="PI0"/>
<pin name="PI1"/>
<pin name="PI2"/>
<pin name="PI3"/>
<pin name="PI4"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VCAP1" direction="pwr"/>
<pin name="VCAP2" direction="pwr"/>
<pin name="PDR_ON" direction="in"/>
<pin name="PI5"/>
<pin name="PI6"/>
<pin name="PI7"/>
<pin name="PI8"/>
<pin name="PI9"/>
<pin name="PI10"/>
<pin name="PI11"/>
<pin name="PI12"/>
<pin name="PI13"/>
<pin name="PI14"/>
<pin name="PI15"/>
<pin name="PJ0"/>
<pin name="PJ1"/>
<pin name="PJ2"/>
<pin name="PJ3"/>
<pin name="PJ4"/>
<pin name="PJ5"/>
<pin name="PJ6"/>
<pin name="PJ7"/>
<pin name="PJ8"/>
<pin name="PJ9"/>
<pin name="PJ10"/>
<pin name="PJ11"/>
<pin name="PJ12"/>
<pin name="PJ13"/>
<pin name="PJ14"/>
<pin name="PJ15"/>
<pin name="PK0"/>
<pin name="PK1"/>
<pin name="PK2"/>
<pin name="PK3"/>
<pin name="PK4"/>
<pin name="PK5"/>
<pin name="PK6"/>
<pin name="PK7"/>
<pin name="VREF-" direction="pwr"/>
<pin name="BYPASS_REG" direction="in"/>
</symbol>
<symbol name="PWR_VDD1_VSS1">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD2_VSS1">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD2_VSS2">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD2_VSS3">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD3_VSS2">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD3_VSS3">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD3_VSS4">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD4_VSS2">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD4_VSS3">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD4_VSS4">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD5_VSS4">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD5_VSS5">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD6_VSS4">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD6_VSS5">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD7_VSS7">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD11_VSS11">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD12_VSS9">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD13_VSS6">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD13_VSS11">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD14_VSS12">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD14_VSS36">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
<pin name="VSS@27" direction="pwr"/>
<pin name="VSS@28" direction="pwr"/>
<pin name="VSS@29" direction="pwr"/>
<pin name="VSS@30" direction="pwr"/>
<pin name="VSS@31" direction="pwr"/>
<pin name="VSS@32" direction="pwr"/>
<pin name="VSS@33" direction="pwr"/>
<pin name="VSS@34" direction="pwr"/>
<pin name="VSS@35" direction="pwr"/>
<pin name="VSS@36" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD15_VSS11">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD17_VSS13">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@16" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD17_VSS14">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@16" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD19_VSS17">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@16" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VDD@18" direction="pwr"/>
<pin name="VDD@19" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD6_VSS3">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD15_VSS12">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
</symbol>
<symbol name="STM32_64PIN_TYP13">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PF4"/>
<pin name="VBAT" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD14_VSS11">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD19_VSS18">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@16" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VDD@18" direction="pwr"/>
<pin name="VDD@19" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
</symbol>
<symbol name="STM32W_48PIN">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="NRESET" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="SWCLK"/>
<pin name="RF_P"/>
<pin name="RF_N"/>
<pin name="RF_TX_ALT_P" direction="out"/>
<pin name="RF_TX_ALT_N" direction="out"/>
<pin name="BIAS_R" direction="in"/>
<pin name="VREG_OUT" direction="pwr"/>
<pin name="VDD_24MHZ" direction="pwr"/>
<pin name="VDD_VCO" direction="pwr"/>
<pin name="VDD_RF" direction="pwr"/>
<pin name="VDD_IF" direction="pwr"/>
<pin name="VDD_PADSA" direction="pwr"/>
<pin name="VDD_PADS@1" direction="pwr"/>
<pin name="VDD_PADS@2" direction="pwr"/>
<pin name="VDD_PADS@3" direction="pwr"/>
<pin name="VDD_PADS@4" direction="pwr"/>
<pin name="VDD_CORE@1" direction="pwr"/>
<pin name="VDD_CORE@2" direction="pwr"/>
<pin name="VDD_PRE" direction="pwr"/>
<pin name="VDD_SYNTH" direction="pwr"/>
<pin name="VDD_MEM" direction="pwr"/>
</symbol>
<symbol name="STM32W_40PIN">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="NRESET" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="SWCLK"/>
<pin name="RF_P"/>
<pin name="RF_N"/>
<pin name="RF_TX_ALT_P" direction="out"/>
<pin name="RF_TX_ALT_N" direction="out"/>
<pin name="BIAS_R" direction="in"/>
<pin name="VREG_OUT" direction="pwr"/>
<pin name="VDD_24MHZ" direction="pwr"/>
<pin name="VDD_VCO" direction="pwr"/>
<pin name="VDD_RF" direction="pwr"/>
<pin name="VDD_IF" direction="pwr"/>
<pin name="VDD_PADSA" direction="pwr"/>
<pin name="VDD_PADS@1" direction="pwr"/>
<pin name="VDD_PADS@2" direction="pwr"/>
<pin name="VDD_PADS@3" direction="pwr"/>
<pin name="VDD_CORE@1" direction="pwr"/>
<pin name="VDD_CORE@2" direction="pwr"/>
<pin name="VDD_PRE" direction="pwr"/>
<pin name="VDD_MEM" direction="pwr"/>
</symbol>
<symbol name="STM32_32PIN_TYP3">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="PC14-OSC_IN"/>
<pin name="PC15-OSC_OUT"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
</symbol>
<symbol name="STM32_48PIN_TYP9">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
</symbol>
<symbol name="STM32_48PIN_TYP10">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDD_USB" direction="pwr"/>
</symbol>
<symbol name="STM32_48PIN_TYP11">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDD_USB" direction="pwr"/>
<pin name="VLCD" direction="pwr"/>
</symbol>
<symbol name="STM32_64PIN_TYP14">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
</symbol>
<symbol name="STM32_64PIN_TYP15">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VREF+" direction="pwr"/>
</symbol>
<symbol name="STM32_64PIN_TYP16">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VDD_USB" direction="pwr"/>
</symbol>
<symbol name="STM32_64PIN_TYP18">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VDD_USB" direction="pwr"/>
<pin name="VLCD" direction="pwr"/>
</symbol>
<symbol name="STM32_64PIN_TYP17">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VDD_USB" direction="pwr"/>
</symbol>
<symbol name="STM32_64PIN_TYP19">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VDD_USB" direction="pwr"/>
<pin name="VLCD" direction="pwr"/>
</symbol>
<symbol name="STM32_32PIN_TYP4">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="PC14-OSC_IN"/>
<pin name="PC15-OSC_OUT"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
</symbol>
<symbol name="PWR_VDD6_VSS7">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
</symbol>
<symbol name="PWR_VDD9_VSS11">
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
</symbol>
<symbol name="STM32_144PIN_TYP6">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PB2"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB11"/>
<pin name="PD8"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PF10"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG11"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VREF-" direction="pwr"/>
<pin name="VDDIO2_2"/>
<pin name="VDDIO2_1"/>
<pin name="VDD_USB"/>
</symbol>
<symbol name="STM32_132PIN_TYP2">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PB2"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB11"/>
<pin name="PD8"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
<pin name="PG15"/>
<pin name="PG6"/>
<pin name="PG7"/>
<pin name="PG8"/>
<pin name="PG11"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VDDIO2_1"/>
<pin name="VDD_USB"/>
<pin name="OPAMP2"/>
<pin name="OPAMP1"/>
</symbol>
<symbol name="STM32_100PIN_TYP11">
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VREF-" direction="pwr"/>
<pin name="PE9"/>
<pin name="PE8"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD9"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PE7"/>
<pin name="PE10"/>
<pin name="PE11"/>
<pin name="PE12"/>
<pin name="PE13"/>
<pin name="PE14"/>
<pin name="PE15"/>
<pin name="PB10"/>
<pin name="PC0"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PD13"/>
<pin name="PD3"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="VREF+" direction="pwr"/>
<pin name="PB2"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="VDD_USB" direction="pwr"/>
<pin name="PB11"/>
<pin name="PD8"/>
<pin name="VBAT" direction="pwr"/>
</symbol>
<symbol name="STM32_72PIN_TYP1">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VREF+" direction="pwr"/>
<pin name="VDDIO2" direction="pwr"/>
<pin name="VDD_USB" direction="pwr"/>
<pin name="PB2"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PG9"/>
<pin name="PG10"/>
<pin name="PG11"/>
<pin name="PG12"/>
<pin name="PG13"/>
<pin name="PG14"/>
</symbol>
<symbol name="STM32_64PIN_TYP20">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PB0"/>
<pin name="VDDA" direction="pwr"/>
<pin name="BOOT0" direction="in"/>
<pin name="NRST" function="dot"/>
<pin name="OSC_IN" function="clk"/>
<pin name="OSC_OUT" function="clk"/>
<pin name="PA8"/>
<pin name="PA15"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PD2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VDD_USB" direction="pwr"/>
<pin name="PC3"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="STM32F030F*P" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0 CPU&lt;/b&gt;&lt;p&gt;
48 MHz maximum frequency&lt;br&gt;
16 Kbytes of Flash memory&lt;br&gt;
4 kbytes of SRAM&lt;br&gt;
15 GPIOs&lt;br&gt;
2.4 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_20PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD1_VSS1"/>
</gates>
<devices>
<device name="" package="TSSOP20-I">
<connects>
<connect gate="MCU" pin="BOOT0" pad="1"/>
<connect gate="MCU" pin="NRST" pad="4"/>
<connect gate="MCU" pin="OSC_IN" pad="2"/>
<connect gate="MCU" pin="OSC_OUT" pad="3"/>
<connect gate="MCU" pin="PA0-WKUP" pad="6"/>
<connect gate="MCU" pin="PA1" pad="7"/>
<connect gate="MCU" pin="PA10" pad="18"/>
<connect gate="MCU" pin="PA13" pad="19"/>
<connect gate="MCU" pin="PA14" pad="20"/>
<connect gate="MCU" pin="PA2" pad="8"/>
<connect gate="MCU" pin="PA3" pad="9"/>
<connect gate="MCU" pin="PA4" pad="10"/>
<connect gate="MCU" pin="PA5" pad="11"/>
<connect gate="MCU" pin="PA6" pad="12"/>
<connect gate="MCU" pin="PA7" pad="13"/>
<connect gate="MCU" pin="PA9" pad="17"/>
<connect gate="MCU" pin="PB1" pad="14"/>
<connect gate="MCU" pin="VDDA" pad="5"/>
<connect gate="PWR" pin="VDD@1" pad="16"/>
<connect gate="PWR" pin="VSS@1" pad="15"/>
</connects>
<technologies>
<technology name="4"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F030K*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0 CPU&lt;/b&gt;&lt;p&gt;
48 MHz maximum frequency&lt;br&gt;
32 Kbytes of Flash memory&lt;br&gt;
4 kbytes of SRAM&lt;br&gt;
26 GPIOs&lt;br&gt;
2.4 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_32PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD2_VSS2"/>
</gates>
<devices>
<device name="" package="LQFP32">
<connects>
<connect gate="MCU" pin="BOOT0" pad="31"/>
<connect gate="MCU" pin="NRST" pad="4"/>
<connect gate="MCU" pin="OSC_IN" pad="2"/>
<connect gate="MCU" pin="OSC_OUT" pad="3"/>
<connect gate="MCU" pin="PA0-WKUP" pad="6"/>
<connect gate="MCU" pin="PA1" pad="7"/>
<connect gate="MCU" pin="PA10" pad="20"/>
<connect gate="MCU" pin="PA11" pad="21"/>
<connect gate="MCU" pin="PA12" pad="22"/>
<connect gate="MCU" pin="PA13" pad="23"/>
<connect gate="MCU" pin="PA14" pad="24"/>
<connect gate="MCU" pin="PA15" pad="25"/>
<connect gate="MCU" pin="PA2" pad="8"/>
<connect gate="MCU" pin="PA3" pad="9"/>
<connect gate="MCU" pin="PA4" pad="10"/>
<connect gate="MCU" pin="PA5" pad="11"/>
<connect gate="MCU" pin="PA6" pad="12"/>
<connect gate="MCU" pin="PA7" pad="13"/>
<connect gate="MCU" pin="PA8" pad="18"/>
<connect gate="MCU" pin="PA9" pad="19"/>
<connect gate="MCU" pin="PB0" pad="14"/>
<connect gate="MCU" pin="PB1" pad="15"/>
<connect gate="MCU" pin="PB3" pad="26"/>
<connect gate="MCU" pin="PB4" pad="27"/>
<connect gate="MCU" pin="PB5" pad="28"/>
<connect gate="MCU" pin="PB6" pad="29"/>
<connect gate="MCU" pin="PB7" pad="30"/>
<connect gate="MCU" pin="VDDA" pad="5"/>
<connect gate="PWR" pin="VDD@1" pad="1"/>
<connect gate="PWR" pin="VDD@2" pad="17"/>
<connect gate="PWR" pin="VSS@1" pad="32"/>
<connect gate="PWR" pin="VSS@2" pad="16"/>
</connects>
<technologies>
<technology name="6"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F030C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0 CPU&lt;/b&gt;&lt;p&gt;
48 MHz maximum frequency&lt;br&gt;
32 to 64 Kbytes of Flash memory&lt;br&gt;
4 to 8 kbytes of SRAM&lt;br&gt;
39 GPIOs&lt;br&gt;
2.4 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD3_VSS2"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PF6" pad="35"/>
<connect gate="MCU" pin="PF7" pad="36"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="1"/>
<connect gate="PWR" pin="VDD@2" pad="24"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F030R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0 CPU&lt;/b&gt;&lt;p&gt;
48 MHz maximum frequency&lt;br&gt;
64 Kbytes of Flash memory&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
55 GPIOs&lt;br&gt;
2.4 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD3_VSS2"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="PF4" pad="18"/>
<connect gate="MCU" pin="PF5" pad="19"/>
<connect gate="MCU" pin="PF6" pad="47"/>
<connect gate="MCU" pin="PF7" pad="48"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="1"/>
<connect gate="PWR" pin="VDD@2" pad="32"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VSS@1" pad="31"/>
<connect gate="PWR" pin="VSS@2" pad="63"/>
</connects>
<technologies>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F050F*P" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0 CPU&lt;/b&gt;&lt;p&gt;
48 MHz maximum frequency&lt;br&gt;
16to 32 Kbytes of Flash memory&lt;br&gt;
4 kbytes of SRAM&lt;br&gt;
15 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_20PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD1_VSS1"/>
</gates>
<devices>
<device name="" package="TSSOP20-I">
<connects>
<connect gate="MCU" pin="BOOT0" pad="1"/>
<connect gate="MCU" pin="NRST" pad="4"/>
<connect gate="MCU" pin="OSC_IN" pad="2"/>
<connect gate="MCU" pin="OSC_OUT" pad="3"/>
<connect gate="MCU" pin="PA0-WKUP" pad="6"/>
<connect gate="MCU" pin="PA1" pad="7"/>
<connect gate="MCU" pin="PA10" pad="18"/>
<connect gate="MCU" pin="PA13" pad="19"/>
<connect gate="MCU" pin="PA14" pad="20"/>
<connect gate="MCU" pin="PA2" pad="8"/>
<connect gate="MCU" pin="PA3" pad="9"/>
<connect gate="MCU" pin="PA4" pad="10"/>
<connect gate="MCU" pin="PA5" pad="11"/>
<connect gate="MCU" pin="PA6" pad="12"/>
<connect gate="MCU" pin="PA7" pad="13"/>
<connect gate="MCU" pin="PA9" pad="17"/>
<connect gate="MCU" pin="PB1" pad="14"/>
<connect gate="MCU" pin="VDDA" pad="5"/>
<connect gate="PWR" pin="VDD@1" pad="16"/>
<connect gate="PWR" pin="VSS@1" pad="15"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F050G*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0 CPU&lt;/b&gt;&lt;p&gt;
48 MHz maximum frequency&lt;br&gt;
16 to 32 Kbytes of Flash memory&lt;br&gt;
4 kbytes of SRAM&lt;br&gt;
23 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_28PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD1_VSS1"/>
</gates>
<devices>
<device name="" package="UFQFPN28">
<connects>
<connect gate="MCU" pin="BOOT0" pad="1"/>
<connect gate="MCU" pin="NRST" pad="4"/>
<connect gate="MCU" pin="OSC_IN" pad="2"/>
<connect gate="MCU" pin="OSC_OUT" pad="3"/>
<connect gate="MCU" pin="PA0-WKUP" pad="6"/>
<connect gate="MCU" pin="PA1" pad="7"/>
<connect gate="MCU" pin="PA10" pad="20"/>
<connect gate="MCU" pin="PA13" pad="21"/>
<connect gate="MCU" pin="PA14" pad="22"/>
<connect gate="MCU" pin="PA15" pad="23"/>
<connect gate="MCU" pin="PA2" pad="8"/>
<connect gate="MCU" pin="PA3" pad="9"/>
<connect gate="MCU" pin="PA4" pad="10"/>
<connect gate="MCU" pin="PA5" pad="11"/>
<connect gate="MCU" pin="PA6" pad="12"/>
<connect gate="MCU" pin="PA7" pad="13"/>
<connect gate="MCU" pin="PA8" pad="18"/>
<connect gate="MCU" pin="PA9" pad="19"/>
<connect gate="MCU" pin="PB0" pad="14"/>
<connect gate="MCU" pin="PB1" pad="15"/>
<connect gate="MCU" pin="PB3" pad="24"/>
<connect gate="MCU" pin="PB4" pad="25"/>
<connect gate="MCU" pin="PB5" pad="26"/>
<connect gate="MCU" pin="PB6" pad="27"/>
<connect gate="MCU" pin="PB7" pad="28"/>
<connect gate="MCU" pin="VDDA" pad="5"/>
<connect gate="PWR" pin="VDD@1" pad="17"/>
<connect gate="PWR" pin="VSS@1" pad="16"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F050K*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0 CPU&lt;/b&gt;&lt;p&gt;
48 MHz maximum frequency&lt;br&gt;
16 to 32 Kbytes of Flash memory&lt;br&gt;
4 kbytes of SRAM&lt;br&gt;
27 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_32PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD2_VSS1"/>
</gates>
<devices>
<device name="" package="UFQFPN32">
<connects>
<connect gate="MCU" pin="BOOT0" pad="31"/>
<connect gate="MCU" pin="NRST" pad="4"/>
<connect gate="MCU" pin="OSC_IN" pad="2"/>
<connect gate="MCU" pin="OSC_OUT" pad="3"/>
<connect gate="MCU" pin="PA0-WKUP" pad="6"/>
<connect gate="MCU" pin="PA1" pad="7"/>
<connect gate="MCU" pin="PA10" pad="20"/>
<connect gate="MCU" pin="PA11" pad="21"/>
<connect gate="MCU" pin="PA12" pad="22"/>
<connect gate="MCU" pin="PA13" pad="23"/>
<connect gate="MCU" pin="PA14" pad="24"/>
<connect gate="MCU" pin="PA15" pad="25"/>
<connect gate="MCU" pin="PA2" pad="8"/>
<connect gate="MCU" pin="PA3" pad="9"/>
<connect gate="MCU" pin="PA4" pad="10"/>
<connect gate="MCU" pin="PA5" pad="11"/>
<connect gate="MCU" pin="PA6" pad="12"/>
<connect gate="MCU" pin="PA7" pad="13"/>
<connect gate="MCU" pin="PA8" pad="18"/>
<connect gate="MCU" pin="PA9" pad="19"/>
<connect gate="MCU" pin="PB0" pad="14"/>
<connect gate="MCU" pin="PB1" pad="15"/>
<connect gate="MCU" pin="PB2" pad="16"/>
<connect gate="MCU" pin="PB3" pad="26"/>
<connect gate="MCU" pin="PB4" pad="27"/>
<connect gate="MCU" pin="PB5" pad="28"/>
<connect gate="MCU" pin="PB6" pad="29"/>
<connect gate="MCU" pin="PB7" pad="30"/>
<connect gate="MCU" pin="PB8" pad="32"/>
<connect gate="MCU" pin="VDDA" pad="5"/>
<connect gate="PWR" pin="VDD@1" pad="1"/>
<connect gate="PWR" pin="VDD@2" pad="17"/>
<connect gate="PWR" pin="VSS@1" pad="VSS"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F050C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0 CPU&lt;/b&gt;&lt;p&gt;
48 MHz maximum frequency&lt;br&gt;
16 to 32 Kbytes of Flash memory&lt;br&gt;
4 kbytes of SRAM&lt;br&gt;
39 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD2_VSS2"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PF6" pad="35"/>
<connect gate="MCU" pin="PF7" pad="36"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="24"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F051K*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0 CPU&lt;/b&gt;&lt;p&gt;
48 MHz maximum frequency&lt;br&gt;
16 to 64 Kbytes of Flash memory&lt;br&gt;
4 to 8 kbytes of SRAM&lt;br&gt;
27 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_32PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD2_VSS1"/>
</gates>
<devices>
<device name="" package="UFQFPN32">
<connects>
<connect gate="MCU" pin="BOOT0" pad="31"/>
<connect gate="MCU" pin="NRST" pad="4"/>
<connect gate="MCU" pin="OSC_IN" pad="2"/>
<connect gate="MCU" pin="OSC_OUT" pad="3"/>
<connect gate="MCU" pin="PA0-WKUP" pad="6"/>
<connect gate="MCU" pin="PA1" pad="7"/>
<connect gate="MCU" pin="PA10" pad="20"/>
<connect gate="MCU" pin="PA11" pad="21"/>
<connect gate="MCU" pin="PA12" pad="22"/>
<connect gate="MCU" pin="PA13" pad="23"/>
<connect gate="MCU" pin="PA14" pad="24"/>
<connect gate="MCU" pin="PA15" pad="25"/>
<connect gate="MCU" pin="PA2" pad="8"/>
<connect gate="MCU" pin="PA3" pad="9"/>
<connect gate="MCU" pin="PA4" pad="10"/>
<connect gate="MCU" pin="PA5" pad="11"/>
<connect gate="MCU" pin="PA6" pad="12"/>
<connect gate="MCU" pin="PA7" pad="13"/>
<connect gate="MCU" pin="PA8" pad="18"/>
<connect gate="MCU" pin="PA9" pad="19"/>
<connect gate="MCU" pin="PB0" pad="14"/>
<connect gate="MCU" pin="PB1" pad="15"/>
<connect gate="MCU" pin="PB2" pad="16"/>
<connect gate="MCU" pin="PB3" pad="26"/>
<connect gate="MCU" pin="PB4" pad="27"/>
<connect gate="MCU" pin="PB5" pad="28"/>
<connect gate="MCU" pin="PB6" pad="29"/>
<connect gate="MCU" pin="PB7" pad="30"/>
<connect gate="MCU" pin="PB8" pad="32"/>
<connect gate="MCU" pin="VDDA" pad="5"/>
<connect gate="PWR" pin="VDD@1" pad="1"/>
<connect gate="PWR" pin="VDD@2" pad="17"/>
<connect gate="PWR" pin="VSS@1" pad="VSS"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F051K*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0 CPU&lt;/b&gt;&lt;p&gt;
48 MHz maximum frequency&lt;br&gt;
16 to 32 Kbytes of Flash memory&lt;br&gt;
4 kbytes of SRAM&lt;br&gt;
25 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_32PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD2_VSS2"/>
</gates>
<devices>
<device name="" package="LQFP32">
<connects>
<connect gate="MCU" pin="BOOT0" pad="31"/>
<connect gate="MCU" pin="NRST" pad="4"/>
<connect gate="MCU" pin="OSC_IN" pad="2"/>
<connect gate="MCU" pin="OSC_OUT" pad="3"/>
<connect gate="MCU" pin="PA0-WKUP" pad="6"/>
<connect gate="MCU" pin="PA1" pad="7"/>
<connect gate="MCU" pin="PA10" pad="20"/>
<connect gate="MCU" pin="PA11" pad="21"/>
<connect gate="MCU" pin="PA12" pad="22"/>
<connect gate="MCU" pin="PA13" pad="23"/>
<connect gate="MCU" pin="PA14" pad="24"/>
<connect gate="MCU" pin="PA15" pad="25"/>
<connect gate="MCU" pin="PA2" pad="8"/>
<connect gate="MCU" pin="PA3" pad="9"/>
<connect gate="MCU" pin="PA4" pad="10"/>
<connect gate="MCU" pin="PA5" pad="11"/>
<connect gate="MCU" pin="PA6" pad="12"/>
<connect gate="MCU" pin="PA7" pad="13"/>
<connect gate="MCU" pin="PA8" pad="18"/>
<connect gate="MCU" pin="PA9" pad="19"/>
<connect gate="MCU" pin="PB0" pad="14"/>
<connect gate="MCU" pin="PB1" pad="15"/>
<connect gate="MCU" pin="PB3" pad="26"/>
<connect gate="MCU" pin="PB4" pad="27"/>
<connect gate="MCU" pin="PB5" pad="28"/>
<connect gate="MCU" pin="PB6" pad="29"/>
<connect gate="MCU" pin="PB7" pad="30"/>
<connect gate="MCU" pin="VDDA" pad="5"/>
<connect gate="PWR" pin="VDD@1" pad="1"/>
<connect gate="PWR" pin="VDD@2" pad="17"/>
<connect gate="PWR" pin="VSS@1" pad="32"/>
<connect gate="PWR" pin="VSS@2" pad="16"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F051C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0 CPU&lt;/b&gt;&lt;p&gt;
48 MHz maximum frequency&lt;br&gt;
16 to 64 Kbytes of Flash memory&lt;br&gt;
4 to 8 kbytes of SRAM&lt;br&gt;
39 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD2_VSS2"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PF6" pad="35"/>
<connect gate="MCU" pin="PF7" pad="36"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="24"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F051R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0 CPU&lt;/b&gt;&lt;p&gt;
48 MHz maximum frequency&lt;br&gt;
16 to 64 Kbytes of Flash memory&lt;br&gt;
4 to 8 kbytes of SRAM&lt;br&gt;
55 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD2_VSS2"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="PF4" pad="18"/>
<connect gate="MCU" pin="PF5" pad="19"/>
<connect gate="MCU" pin="PF6" pad="47"/>
<connect gate="MCU" pin="PF7" pad="48"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="32"/>
<connect gate="PWR" pin="VDD@2" pad="64"/>
<connect gate="PWR" pin="VSS@1" pad="31"/>
<connect gate="PWR" pin="VSS@2" pad="63"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F100C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
24 MHz maximum frequency&lt;br&gt;
16 to 128 Kbytes of Flash memory&lt;br&gt;
4 to 8 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD3_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="24"/>
<connect gate="PWR" pin="VDD@2" pad="36"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="35"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F100R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
24 MHz maximum frequency&lt;br&gt;
16 to 512 Kbytes of Flash memory&lt;br&gt;
4 to 32 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="32"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="31"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
<connect gate="PWR" pin="VSS@3" pad="63"/>
<connect gate="PWR" pin="VSS@4" pad="18"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
<technology name="D"/>
<technology name="E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F100R*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
24 MHz maximum frequency&lt;br&gt;
16 to 128 Kbytes of Flash memory&lt;br&gt;
4 to 8 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="TFBGA64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="B4"/>
<connect gate="MCU" pin="NRST" pad="E1"/>
<connect gate="MCU" pin="OSC_IN" pad="C1"/>
<connect gate="MCU" pin="OSC_OUT" pad="D1"/>
<connect gate="MCU" pin="PA0-WKUP" pad="G2"/>
<connect gate="MCU" pin="PA1" pad="H2"/>
<connect gate="MCU" pin="PA10" pad="C6"/>
<connect gate="MCU" pin="PA11" pad="C8"/>
<connect gate="MCU" pin="PA12" pad="B8"/>
<connect gate="MCU" pin="PA13" pad="A8"/>
<connect gate="MCU" pin="PA14" pad="A7"/>
<connect gate="MCU" pin="PA15" pad="A6"/>
<connect gate="MCU" pin="PA2" pad="F3"/>
<connect gate="MCU" pin="PA3" pad="G3"/>
<connect gate="MCU" pin="PA4" pad="H3"/>
<connect gate="MCU" pin="PA5" pad="F4"/>
<connect gate="MCU" pin="PA6" pad="G4"/>
<connect gate="MCU" pin="PA7" pad="H4"/>
<connect gate="MCU" pin="PA8" pad="D7"/>
<connect gate="MCU" pin="PA9" pad="C7"/>
<connect gate="MCU" pin="PB0" pad="F5"/>
<connect gate="MCU" pin="PB1" pad="G5"/>
<connect gate="MCU" pin="PB10" pad="G7"/>
<connect gate="MCU" pin="PB11" pad="H7"/>
<connect gate="MCU" pin="PB12" pad="H8"/>
<connect gate="MCU" pin="PB13" pad="G8"/>
<connect gate="MCU" pin="PB14" pad="F8"/>
<connect gate="MCU" pin="PB15" pad="F7"/>
<connect gate="MCU" pin="PB2" pad="G6"/>
<connect gate="MCU" pin="PB3" pad="A5"/>
<connect gate="MCU" pin="PB4" pad="A4"/>
<connect gate="MCU" pin="PB5" pad="C4"/>
<connect gate="MCU" pin="PB6" pad="D3"/>
<connect gate="MCU" pin="PB7" pad="C3"/>
<connect gate="MCU" pin="PB8" pad="B3"/>
<connect gate="MCU" pin="PB9" pad="A3"/>
<connect gate="MCU" pin="PC0" pad="E3"/>
<connect gate="MCU" pin="PC1" pad="E2"/>
<connect gate="MCU" pin="PC10" pad="B7"/>
<connect gate="MCU" pin="PC11" pad="B6"/>
<connect gate="MCU" pin="PC12" pad="C5"/>
<connect gate="MCU" pin="PC13" pad="A2"/>
<connect gate="MCU" pin="PC14" pad="A1"/>
<connect gate="MCU" pin="PC15" pad="B1"/>
<connect gate="MCU" pin="PC2" pad="F2"/>
<connect gate="MCU" pin="PC4" pad="H5"/>
<connect gate="MCU" pin="PC5" pad="H6"/>
<connect gate="MCU" pin="PC6" pad="F6"/>
<connect gate="MCU" pin="PC7" pad="E7"/>
<connect gate="MCU" pin="PC8" pad="E8"/>
<connect gate="MCU" pin="PC9" pad="D8"/>
<connect gate="MCU" pin="PD2" pad="B5"/>
<connect gate="MCU" pin="VBAT" pad="B2"/>
<connect gate="MCU" pin="VDDA" pad="H1"/>
<connect gate="MCU" pin="VREF+" pad="G1"/>
<connect gate="MCU" pin="VSSA" pad="F1"/>
<connect gate="PWR" pin="VDD@1" pad="E6"/>
<connect gate="PWR" pin="VDD@2" pad="E5"/>
<connect gate="PWR" pin="VDD@3" pad="E4"/>
<connect gate="PWR" pin="VDD@4" pad="D2"/>
<connect gate="PWR" pin="VSS@1" pad="D6"/>
<connect gate="PWR" pin="VSS@2" pad="D5"/>
<connect gate="PWR" pin="VSS@3" pad="D4"/>
<connect gate="PWR" pin="VSS@4" pad="C2"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F100V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
24 MHz maximum frequency&lt;br&gt;
16 to 512 Kbytes of Flash memory&lt;br&gt;
4 to 32 kbytes of SRAM&lt;br&gt;
80 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD5_VSS5"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0-WKUP" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VREF-" pad="20"/>
<connect gate="MCU" pin="VSSA" pad="19"/>
<connect gate="PWR" pin="VDD@1" pad="50"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="100"/>
<connect gate="PWR" pin="VDD@4" pad="28"/>
<connect gate="PWR" pin="VDD@5" pad="11"/>
<connect gate="PWR" pin="VSS@1" pad="49"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
<connect gate="PWR" pin="VSS@3" pad="99"/>
<connect gate="PWR" pin="VSS@4" pad="27"/>
<connect gate="PWR" pin="VSS@5" pad="10"/>
</connects>
<technologies>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
<technology name="D"/>
<technology name="E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F100Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
24 MHz maximum frequency&lt;br&gt;
256 to 512 Kbytes of Flash memory&lt;br&gt;
24 to 32 kbytes of SRAM&lt;br&gt;
112 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD11_VSS11"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VREF-" pad="31"/>
<connect gate="MCU" pin="VSSA" pad="30"/>
<connect gate="PWR" pin="VDD@1" pad="72"/>
<connect gate="PWR" pin="VDD@10" pad="121"/>
<connect gate="PWR" pin="VDD@11" pad="131"/>
<connect gate="PWR" pin="VDD@2" pad="108"/>
<connect gate="PWR" pin="VDD@3" pad="144"/>
<connect gate="PWR" pin="VDD@4" pad="39"/>
<connect gate="PWR" pin="VDD@5" pad="17"/>
<connect gate="PWR" pin="VDD@6" pad="52"/>
<connect gate="PWR" pin="VDD@7" pad="62"/>
<connect gate="PWR" pin="VDD@8" pad="84"/>
<connect gate="PWR" pin="VDD@9" pad="95"/>
<connect gate="PWR" pin="VSS@1" pad="71"/>
<connect gate="PWR" pin="VSS@10" pad="120"/>
<connect gate="PWR" pin="VSS@11" pad="130"/>
<connect gate="PWR" pin="VSS@2" pad="107"/>
<connect gate="PWR" pin="VSS@3" pad="143"/>
<connect gate="PWR" pin="VSS@4" pad="38"/>
<connect gate="PWR" pin="VSS@5" pad="16"/>
<connect gate="PWR" pin="VSS@6" pad="51"/>
<connect gate="PWR" pin="VSS@7" pad="61"/>
<connect gate="PWR" pin="VSS@8" pad="83"/>
<connect gate="PWR" pin="VSS@9" pad="94"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="D"/>
<technology name="E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F101T*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
36 MHz maximum frequency&lt;br&gt;
16 to 128 Kbytes of Flash memory&lt;br&gt;
4 to 16 kbytes of SRAM&lt;br&gt;
26 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_36PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD3_VSS4"/>
</gates>
<devices>
<device name="" package="VFQFPN36">
<connects>
<connect gate="MCU" pin="BOOT0" pad="35"/>
<connect gate="MCU" pin="NRST" pad="4"/>
<connect gate="MCU" pin="OSC_IN" pad="2"/>
<connect gate="MCU" pin="OSC_OUT" pad="3"/>
<connect gate="MCU" pin="PA0-WKUP" pad="7"/>
<connect gate="MCU" pin="PA1" pad="8"/>
<connect gate="MCU" pin="PA10" pad="22"/>
<connect gate="MCU" pin="PA11" pad="23"/>
<connect gate="MCU" pin="PA12" pad="24"/>
<connect gate="MCU" pin="PA13" pad="25"/>
<connect gate="MCU" pin="PA14" pad="28"/>
<connect gate="MCU" pin="PA15" pad="29"/>
<connect gate="MCU" pin="PA2" pad="9"/>
<connect gate="MCU" pin="PA3" pad="10"/>
<connect gate="MCU" pin="PA4" pad="11"/>
<connect gate="MCU" pin="PA5" pad="12"/>
<connect gate="MCU" pin="PA6" pad="13"/>
<connect gate="MCU" pin="PA7" pad="14"/>
<connect gate="MCU" pin="PA8" pad="20"/>
<connect gate="MCU" pin="PA9" pad="21"/>
<connect gate="MCU" pin="PB0" pad="15"/>
<connect gate="MCU" pin="PB1" pad="16"/>
<connect gate="MCU" pin="PB2" pad="17"/>
<connect gate="MCU" pin="PB3" pad="30"/>
<connect gate="MCU" pin="PB4" pad="31"/>
<connect gate="MCU" pin="PB5" pad="32"/>
<connect gate="MCU" pin="PB6" pad="33"/>
<connect gate="MCU" pin="PB7" pad="34"/>
<connect gate="MCU" pin="VDDA" pad="6"/>
<connect gate="MCU" pin="VSSA" pad="5"/>
<connect gate="PWR" pin="VDD@1" pad="19"/>
<connect gate="PWR" pin="VDD@2" pad="27"/>
<connect gate="PWR" pin="VDD@3" pad="1"/>
<connect gate="PWR" pin="VSS@1" pad="18"/>
<connect gate="PWR" pin="VSS@2" pad="26"/>
<connect gate="PWR" pin="VSS@3" pad="36"/>
<connect gate="PWR" pin="VSS@4" pad="EXP"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F101C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
36 MHz maximum frequency&lt;br&gt;
16 to 128 Kbytes of Flash memory&lt;br&gt;
4 to 16 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD3_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="24"/>
<connect gate="PWR" pin="VDD@2" pad="36"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="35"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F101C*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
36 MHz maximum frequency&lt;br&gt;
16 to 128 Kbytes of Flash memory&lt;br&gt;
4 to 16 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD3_VSS4"/>
</gates>
<devices>
<device name="" package="UFQFPN48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="24"/>
<connect gate="PWR" pin="VDD@2" pad="36"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="35"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
<connect gate="PWR" pin="VSS@4" pad="EXP"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F101R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
36 MHz maximum frequency&lt;br&gt;
16 to 1024 Kbytes of Flash memory&lt;br&gt;
4 to 80 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="32"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="31"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
<connect gate="PWR" pin="VSS@3" pad="63"/>
<connect gate="PWR" pin="VSS@4" pad="18"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
<technology name="D"/>
<technology name="E"/>
<technology name="F"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F101V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
36 MHz maximum frequency&lt;br&gt;
64 to 1024 Kbytes of Flash memory&lt;br&gt;
10 to 80 kbytes of SRAM&lt;br&gt;
80 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD5_VSS5"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0-WKUP" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VREF-" pad="20"/>
<connect gate="MCU" pin="VSSA" pad="19"/>
<connect gate="PWR" pin="VDD@1" pad="50"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="100"/>
<connect gate="PWR" pin="VDD@4" pad="28"/>
<connect gate="PWR" pin="VDD@5" pad="11"/>
<connect gate="PWR" pin="VSS@1" pad="49"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
<connect gate="PWR" pin="VSS@3" pad="99"/>
<connect gate="PWR" pin="VSS@4" pad="27"/>
<connect gate="PWR" pin="VSS@5" pad="10"/>
</connects>
<technologies>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
<technology name="D"/>
<technology name="E"/>
<technology name="F"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F101Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
36 MHz maximum frequency&lt;br&gt;
256 to 1024 Kbytes of Flash memory&lt;br&gt;
32 to 80 kbytes of SRAM&lt;br&gt;
112 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD11_VSS11"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VREF-" pad="31"/>
<connect gate="MCU" pin="VSSA" pad="30"/>
<connect gate="PWR" pin="VDD@1" pad="72"/>
<connect gate="PWR" pin="VDD@10" pad="121"/>
<connect gate="PWR" pin="VDD@11" pad="131"/>
<connect gate="PWR" pin="VDD@2" pad="108"/>
<connect gate="PWR" pin="VDD@3" pad="144"/>
<connect gate="PWR" pin="VDD@4" pad="39"/>
<connect gate="PWR" pin="VDD@5" pad="17"/>
<connect gate="PWR" pin="VDD@6" pad="52"/>
<connect gate="PWR" pin="VDD@7" pad="62"/>
<connect gate="PWR" pin="VDD@8" pad="84"/>
<connect gate="PWR" pin="VDD@9" pad="95"/>
<connect gate="PWR" pin="VSS@1" pad="71"/>
<connect gate="PWR" pin="VSS@10" pad="120"/>
<connect gate="PWR" pin="VSS@11" pad="130"/>
<connect gate="PWR" pin="VSS@2" pad="107"/>
<connect gate="PWR" pin="VSS@3" pad="143"/>
<connect gate="PWR" pin="VSS@4" pad="38"/>
<connect gate="PWR" pin="VSS@5" pad="16"/>
<connect gate="PWR" pin="VSS@6" pad="51"/>
<connect gate="PWR" pin="VSS@7" pad="61"/>
<connect gate="PWR" pin="VSS@8" pad="83"/>
<connect gate="PWR" pin="VSS@9" pad="94"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="D"/>
<technology name="E"/>
<technology name="F"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F102C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
48 MHz maximum frequency&lt;br&gt;
16 to 128 Kbytes of Flash memory&lt;br&gt;
4 to 16 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD3_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="24"/>
<connect gate="PWR" pin="VDD@2" pad="36"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="35"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F102R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
48 MHz maximum frequency&lt;br&gt;
16 to 128 Kbytes of Flash memory&lt;br&gt;
4 to 16 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="32"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="31"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
<connect gate="PWR" pin="VSS@3" pad="63"/>
<connect gate="PWR" pin="VSS@4" pad="18"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F103T*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
16 to 128 Kbytes of Flash memory&lt;br&gt;
6 to 20 kbytes of SRAM&lt;br&gt;
26 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_36PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD3_VSS4"/>
</gates>
<devices>
<device name="" package="VFQFPN36">
<connects>
<connect gate="MCU" pin="BOOT0" pad="35"/>
<connect gate="MCU" pin="NRST" pad="4"/>
<connect gate="MCU" pin="OSC_IN" pad="2"/>
<connect gate="MCU" pin="OSC_OUT" pad="3"/>
<connect gate="MCU" pin="PA0-WKUP" pad="7"/>
<connect gate="MCU" pin="PA1" pad="8"/>
<connect gate="MCU" pin="PA10" pad="22"/>
<connect gate="MCU" pin="PA11" pad="23"/>
<connect gate="MCU" pin="PA12" pad="24"/>
<connect gate="MCU" pin="PA13" pad="25"/>
<connect gate="MCU" pin="PA14" pad="28"/>
<connect gate="MCU" pin="PA15" pad="29"/>
<connect gate="MCU" pin="PA2" pad="9"/>
<connect gate="MCU" pin="PA3" pad="10"/>
<connect gate="MCU" pin="PA4" pad="11"/>
<connect gate="MCU" pin="PA5" pad="12"/>
<connect gate="MCU" pin="PA6" pad="13"/>
<connect gate="MCU" pin="PA7" pad="14"/>
<connect gate="MCU" pin="PA8" pad="20"/>
<connect gate="MCU" pin="PA9" pad="21"/>
<connect gate="MCU" pin="PB0" pad="15"/>
<connect gate="MCU" pin="PB1" pad="16"/>
<connect gate="MCU" pin="PB2" pad="17"/>
<connect gate="MCU" pin="PB3" pad="30"/>
<connect gate="MCU" pin="PB4" pad="31"/>
<connect gate="MCU" pin="PB5" pad="32"/>
<connect gate="MCU" pin="PB6" pad="33"/>
<connect gate="MCU" pin="PB7" pad="34"/>
<connect gate="MCU" pin="VDDA" pad="6"/>
<connect gate="MCU" pin="VSSA" pad="5"/>
<connect gate="PWR" pin="VDD@1" pad="19"/>
<connect gate="PWR" pin="VDD@2" pad="27"/>
<connect gate="PWR" pin="VDD@3" pad="1"/>
<connect gate="PWR" pin="VSS@1" pad="18"/>
<connect gate="PWR" pin="VSS@2" pad="26"/>
<connect gate="PWR" pin="VSS@3" pad="36"/>
<connect gate="PWR" pin="VSS@4" pad="EXP"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F103C*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
16 to 128 Kbytes of Flash memory&lt;br&gt;
6 to 20 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD3_VSS4"/>
</gates>
<devices>
<device name="" package="UFQFPN48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="24"/>
<connect gate="PWR" pin="VDD@2" pad="36"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="35"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
<connect gate="PWR" pin="VSS@4" pad="EXP"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F103C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
16 to 128 Kbytes of Flash memory&lt;br&gt;
6 to 20 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD3_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="24"/>
<connect gate="PWR" pin="VDD@2" pad="36"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="35"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F103R*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
16 to 128 Kbytes of Flash memory&lt;br&gt;
6 to 20 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="TFBGA64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="B4"/>
<connect gate="MCU" pin="NRST" pad="E1"/>
<connect gate="MCU" pin="OSC_IN" pad="C1"/>
<connect gate="MCU" pin="OSC_OUT" pad="D1"/>
<connect gate="MCU" pin="PA0-WKUP" pad="G2"/>
<connect gate="MCU" pin="PA1" pad="H2"/>
<connect gate="MCU" pin="PA10" pad="C6"/>
<connect gate="MCU" pin="PA11" pad="C8"/>
<connect gate="MCU" pin="PA12" pad="B8"/>
<connect gate="MCU" pin="PA13" pad="A8"/>
<connect gate="MCU" pin="PA14" pad="A7"/>
<connect gate="MCU" pin="PA15" pad="A6"/>
<connect gate="MCU" pin="PA2" pad="F3"/>
<connect gate="MCU" pin="PA3" pad="G3"/>
<connect gate="MCU" pin="PA4" pad="H3"/>
<connect gate="MCU" pin="PA5" pad="F4"/>
<connect gate="MCU" pin="PA6" pad="G4"/>
<connect gate="MCU" pin="PA7" pad="H4"/>
<connect gate="MCU" pin="PA8" pad="D7"/>
<connect gate="MCU" pin="PA9" pad="C7"/>
<connect gate="MCU" pin="PB0" pad="F5"/>
<connect gate="MCU" pin="PB1" pad="G5"/>
<connect gate="MCU" pin="PB10" pad="G7"/>
<connect gate="MCU" pin="PB11" pad="H7"/>
<connect gate="MCU" pin="PB12" pad="H8"/>
<connect gate="MCU" pin="PB13" pad="G8"/>
<connect gate="MCU" pin="PB14" pad="F8"/>
<connect gate="MCU" pin="PB15" pad="F7"/>
<connect gate="MCU" pin="PB2" pad="G6"/>
<connect gate="MCU" pin="PB3" pad="A5"/>
<connect gate="MCU" pin="PB4" pad="A4"/>
<connect gate="MCU" pin="PB5" pad="C4"/>
<connect gate="MCU" pin="PB6" pad="D3"/>
<connect gate="MCU" pin="PB7" pad="C3"/>
<connect gate="MCU" pin="PB8" pad="B3"/>
<connect gate="MCU" pin="PB9" pad="A3"/>
<connect gate="MCU" pin="PC0" pad="E3"/>
<connect gate="MCU" pin="PC1" pad="E2"/>
<connect gate="MCU" pin="PC10" pad="B7"/>
<connect gate="MCU" pin="PC11" pad="B6"/>
<connect gate="MCU" pin="PC12" pad="C5"/>
<connect gate="MCU" pin="PC13" pad="A2"/>
<connect gate="MCU" pin="PC14" pad="A1"/>
<connect gate="MCU" pin="PC15" pad="B1"/>
<connect gate="MCU" pin="PC2" pad="F2"/>
<connect gate="MCU" pin="PC4" pad="H5"/>
<connect gate="MCU" pin="PC5" pad="H6"/>
<connect gate="MCU" pin="PC6" pad="F6"/>
<connect gate="MCU" pin="PC7" pad="E7"/>
<connect gate="MCU" pin="PC8" pad="E8"/>
<connect gate="MCU" pin="PC9" pad="D8"/>
<connect gate="MCU" pin="PD2" pad="B5"/>
<connect gate="MCU" pin="VBAT" pad="B2"/>
<connect gate="MCU" pin="VDDA" pad="H1"/>
<connect gate="MCU" pin="VREF+" pad="G1"/>
<connect gate="MCU" pin="VSSA" pad="F1"/>
<connect gate="PWR" pin="VDD@1" pad="E6"/>
<connect gate="PWR" pin="VDD@2" pad="E5"/>
<connect gate="PWR" pin="VDD@3" pad="E4"/>
<connect gate="PWR" pin="VDD@4" pad="D2"/>
<connect gate="PWR" pin="VSS@1" pad="D6"/>
<connect gate="PWR" pin="VSS@2" pad="D5"/>
<connect gate="PWR" pin="VSS@3" pad="D4"/>
<connect gate="PWR" pin="VSS@4" pad="C2"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F103R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
16 to 1024 Kbytes of Flash memory&lt;br&gt;
6 to 96 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="32"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="31"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
<connect gate="PWR" pin="VSS@3" pad="63"/>
<connect gate="PWR" pin="VSS@4" pad="18"/>
</connects>
<technologies>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
<technology name="D"/>
<technology name="E"/>
<technology name="F"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F103R*Y" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
256 to 512 Kbytes of Flash memory&lt;br&gt;
64 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="WLCSP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A6"/>
<connect gate="MCU" pin="NRST" pad="C7"/>
<connect gate="MCU" pin="OSC_IN" pad="D8"/>
<connect gate="MCU" pin="OSC_OUT" pad="D7"/>
<connect gate="MCU" pin="PA0-WKUP" pad="F6"/>
<connect gate="MCU" pin="PA1" pad="E6"/>
<connect gate="MCU" pin="PA10" pad="D3"/>
<connect gate="MCU" pin="PA11" pad="C1"/>
<connect gate="MCU" pin="PA12" pad="C2"/>
<connect gate="MCU" pin="PA13" pad="D4"/>
<connect gate="MCU" pin="PA14" pad="B2"/>
<connect gate="MCU" pin="PA15" pad="C3"/>
<connect gate="MCU" pin="PA2" pad="H8"/>
<connect gate="MCU" pin="PA3" pad="G7"/>
<connect gate="MCU" pin="PA4" pad="H7"/>
<connect gate="MCU" pin="PA5" pad="E5"/>
<connect gate="MCU" pin="PA6" pad="G5"/>
<connect gate="MCU" pin="PA7" pad="G4"/>
<connect gate="MCU" pin="PA8" pad="E4"/>
<connect gate="MCU" pin="PA9" pad="D2"/>
<connect gate="MCU" pin="PB0" pad="H4"/>
<connect gate="MCU" pin="PB1" pad="F4"/>
<connect gate="MCU" pin="PB10" pad="G3"/>
<connect gate="MCU" pin="PB11" pad="F3"/>
<connect gate="MCU" pin="PB12" pad="G2"/>
<connect gate="MCU" pin="PB13" pad="G1"/>
<connect gate="MCU" pin="PB14" pad="F2"/>
<connect gate="MCU" pin="PB15" pad="F1"/>
<connect gate="MCU" pin="PB2" pad="H3"/>
<connect gate="MCU" pin="PB3" pad="A4"/>
<connect gate="MCU" pin="PB4" pad="B4"/>
<connect gate="MCU" pin="PB5" pad="A5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="C5"/>
<connect gate="MCU" pin="PB8" pad="D5"/>
<connect gate="MCU" pin="PB9" pad="B6"/>
<connect gate="MCU" pin="PC0" pad="E8"/>
<connect gate="MCU" pin="PC1" pad="F8"/>
<connect gate="MCU" pin="PC10" pad="A2"/>
<connect gate="MCU" pin="PC11" pad="B3"/>
<connect gate="MCU" pin="PC12" pad="C4"/>
<connect gate="MCU" pin="PC13" pad="C8"/>
<connect gate="MCU" pin="PC14" pad="B8"/>
<connect gate="MCU" pin="PC15" pad="B7"/>
<connect gate="MCU" pin="PC2" pad="D6"/>
<connect gate="MCU" pin="PC4" pad="H6"/>
<connect gate="MCU" pin="PC5" pad="H5"/>
<connect gate="MCU" pin="PC6" pad="E1"/>
<connect gate="MCU" pin="PC7" pad="E2"/>
<connect gate="MCU" pin="PC8" pad="E3"/>
<connect gate="MCU" pin="PC9" pad="D1"/>
<connect gate="MCU" pin="PD2" pad="A3"/>
<connect gate="MCU" pin="VBAT" pad="C6"/>
<connect gate="MCU" pin="VDDA" pad="G8"/>
<connect gate="MCU" pin="VREF+" pad="F7"/>
<connect gate="MCU" pin="VSSA" pad="E7"/>
<connect gate="PWR" pin="VDD@1" pad="H1"/>
<connect gate="PWR" pin="VDD@2" pad="A1"/>
<connect gate="PWR" pin="VDD@3" pad="A8"/>
<connect gate="PWR" pin="VDD@4" pad="G6"/>
<connect gate="PWR" pin="VSS@1" pad="H2"/>
<connect gate="PWR" pin="VSS@2" pad="B1"/>
<connect gate="PWR" pin="VSS@3" pad="A7"/>
<connect gate="PWR" pin="VSS@4" pad="F5"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="D"/>
<technology name="E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F103V*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
64 to 512 Kbytes of Flash memory&lt;br&gt;
20 to 64 kbytes of SRAM&lt;br&gt;
80 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD5_VSS5"/>
</gates>
<devices>
<device name="" package="LFBGA100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="D5"/>
<connect gate="MCU" pin="NRST" pad="E1"/>
<connect gate="MCU" pin="OSC_IN" pad="C1"/>
<connect gate="MCU" pin="OSC_OUT" pad="D1"/>
<connect gate="MCU" pin="PA0-WKUP" pad="G2"/>
<connect gate="MCU" pin="PA1" pad="H2"/>
<connect gate="MCU" pin="PA10" pad="D10"/>
<connect gate="MCU" pin="PA11" pad="C10"/>
<connect gate="MCU" pin="PA12" pad="B10"/>
<connect gate="MCU" pin="PA13" pad="A10"/>
<connect gate="MCU" pin="PA14" pad="A9"/>
<connect gate="MCU" pin="PA15" pad="A8"/>
<connect gate="MCU" pin="PA2" pad="J2"/>
<connect gate="MCU" pin="PA3" pad="K2"/>
<connect gate="MCU" pin="PA4" pad="G3"/>
<connect gate="MCU" pin="PA5" pad="H3"/>
<connect gate="MCU" pin="PA6" pad="J3"/>
<connect gate="MCU" pin="PA7" pad="K3"/>
<connect gate="MCU" pin="PA8" pad="D9"/>
<connect gate="MCU" pin="PA9" pad="C9"/>
<connect gate="MCU" pin="PB0" pad="J4"/>
<connect gate="MCU" pin="PB1" pad="K4"/>
<connect gate="MCU" pin="PB10" pad="J7"/>
<connect gate="MCU" pin="PB11" pad="K7"/>
<connect gate="MCU" pin="PB12" pad="K8"/>
<connect gate="MCU" pin="PB13" pad="J8"/>
<connect gate="MCU" pin="PB14" pad="H8"/>
<connect gate="MCU" pin="PB15" pad="G8"/>
<connect gate="MCU" pin="PB2" pad="G5"/>
<connect gate="MCU" pin="PB3" pad="A7"/>
<connect gate="MCU" pin="PB4" pad="A6"/>
<connect gate="MCU" pin="PB5" pad="C5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="A5"/>
<connect gate="MCU" pin="PB8" pad="B4"/>
<connect gate="MCU" pin="PB9" pad="A4"/>
<connect gate="MCU" pin="PC0" pad="F1"/>
<connect gate="MCU" pin="PC1" pad="F2"/>
<connect gate="MCU" pin="PC10" pad="B9"/>
<connect gate="MCU" pin="PC11" pad="B8"/>
<connect gate="MCU" pin="PC12" pad="C8"/>
<connect gate="MCU" pin="PC13" pad="A2"/>
<connect gate="MCU" pin="PC14" pad="A1"/>
<connect gate="MCU" pin="PC15" pad="B1"/>
<connect gate="MCU" pin="PC2" pad="E2"/>
<connect gate="MCU" pin="PC3" pad="F3"/>
<connect gate="MCU" pin="PC4" pad="G4"/>
<connect gate="MCU" pin="PC5" pad="H4"/>
<connect gate="MCU" pin="PC6" pad="F10"/>
<connect gate="MCU" pin="PC7" pad="E10"/>
<connect gate="MCU" pin="PC8" pad="F9"/>
<connect gate="MCU" pin="PC9" pad="E9"/>
<connect gate="MCU" pin="PD0" pad="D8"/>
<connect gate="MCU" pin="PD1" pad="E8"/>
<connect gate="MCU" pin="PD10" pad="H9"/>
<connect gate="MCU" pin="PD11" pad="G9"/>
<connect gate="MCU" pin="PD12" pad="K10"/>
<connect gate="MCU" pin="PD13" pad="J10"/>
<connect gate="MCU" pin="PD14" pad="H10"/>
<connect gate="MCU" pin="PD15" pad="G10"/>
<connect gate="MCU" pin="PD2" pad="B7"/>
<connect gate="MCU" pin="PD3" pad="C7"/>
<connect gate="MCU" pin="PD4" pad="D7"/>
<connect gate="MCU" pin="PD5" pad="B6"/>
<connect gate="MCU" pin="PD6" pad="C6"/>
<connect gate="MCU" pin="PD7" pad="D6"/>
<connect gate="MCU" pin="PD8" pad="K9"/>
<connect gate="MCU" pin="PD9" pad="J9"/>
<connect gate="MCU" pin="PE0" pad="D4"/>
<connect gate="MCU" pin="PE1" pad="C4"/>
<connect gate="MCU" pin="PE10" pad="G6"/>
<connect gate="MCU" pin="PE11" pad="H6"/>
<connect gate="MCU" pin="PE12" pad="J6"/>
<connect gate="MCU" pin="PE13" pad="K6"/>
<connect gate="MCU" pin="PE14" pad="G7"/>
<connect gate="MCU" pin="PE15" pad="H7"/>
<connect gate="MCU" pin="PE2" pad="A3"/>
<connect gate="MCU" pin="PE3" pad="B3"/>
<connect gate="MCU" pin="PE4" pad="C3"/>
<connect gate="MCU" pin="PE5" pad="D3"/>
<connect gate="MCU" pin="PE6" pad="E3"/>
<connect gate="MCU" pin="PE7" pad="H5"/>
<connect gate="MCU" pin="PE8" pad="J5"/>
<connect gate="MCU" pin="PE9" pad="K5"/>
<connect gate="MCU" pin="VBAT" pad="B2"/>
<connect gate="MCU" pin="VDDA" pad="K1"/>
<connect gate="MCU" pin="VREF+" pad="J1"/>
<connect gate="MCU" pin="VREF-" pad="H1"/>
<connect gate="MCU" pin="VSSA" pad="G1"/>
<connect gate="PWR" pin="VDD@1" pad="F7"/>
<connect gate="PWR" pin="VDD@2" pad="F6"/>
<connect gate="PWR" pin="VDD@3" pad="F5"/>
<connect gate="PWR" pin="VDD@4" pad="F4"/>
<connect gate="PWR" pin="VDD@5" pad="D2"/>
<connect gate="PWR" pin="VSS@1" pad="E7"/>
<connect gate="PWR" pin="VSS@2" pad="E6"/>
<connect gate="PWR" pin="VSS@3" pad="E5"/>
<connect gate="PWR" pin="VSS@4" pad="E4"/>
<connect gate="PWR" pin="VSS@5" pad="C2"/>
</connects>
<technologies>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
<technology name="D"/>
<technology name="E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F103V*I" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
64 to 128 Kbytes of Flash memory&lt;br&gt;
20 kbytes of SRAM&lt;br&gt;
80 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD5_VSS5"/>
</gates>
<devices>
<device name="" package="UFBGA100">
<technologies>
<technology name="8"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F103V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
64 to 1028 Kbytes of Flash memory&lt;br&gt;
20 to 96 kbytes of SRAM&lt;br&gt;
80 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD5_VSS5"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0-WKUP" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VREF-" pad="20"/>
<connect gate="MCU" pin="VSSA" pad="19"/>
<connect gate="PWR" pin="VDD@1" pad="50"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="100"/>
<connect gate="PWR" pin="VDD@4" pad="28"/>
<connect gate="PWR" pin="VDD@5" pad="11"/>
<connect gate="PWR" pin="VSS@1" pad="49"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
<connect gate="PWR" pin="VSS@3" pad="99"/>
<connect gate="PWR" pin="VSS@4" pad="27"/>
<connect gate="PWR" pin="VSS@5" pad="10"/>
</connects>
<technologies>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
<technology name="D"/>
<technology name="E"/>
<technology name="F"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F103Z*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
256 to 1024 Kbytes of Flash memory&lt;br&gt;
48 to 96 kbytes of SRAM&lt;br&gt;
112 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD11_VSS11"/>
</gates>
<devices>
<device name="" package="LFBGA144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="D5"/>
<connect gate="MCU" pin="NRST" pad="F1"/>
<connect gate="MCU" pin="OSC_IN" pad="D1"/>
<connect gate="MCU" pin="OSC_OUT" pad="E1"/>
<connect gate="MCU" pin="PA0" pad="J2"/>
<connect gate="MCU" pin="PA1" pad="K2"/>
<connect gate="MCU" pin="PA10" pad="D11"/>
<connect gate="MCU" pin="PA11" pad="C12"/>
<connect gate="MCU" pin="PA12" pad="B12"/>
<connect gate="MCU" pin="PA13" pad="A12"/>
<connect gate="MCU" pin="PA14" pad="A11"/>
<connect gate="MCU" pin="PA15" pad="A10"/>
<connect gate="MCU" pin="PA2" pad="L2"/>
<connect gate="MCU" pin="PA3" pad="M2"/>
<connect gate="MCU" pin="PA4" pad="J3"/>
<connect gate="MCU" pin="PA5" pad="K3"/>
<connect gate="MCU" pin="PA6" pad="L3"/>
<connect gate="MCU" pin="PA7" pad="M3"/>
<connect gate="MCU" pin="PA8" pad="E12"/>
<connect gate="MCU" pin="PA9" pad="D12"/>
<connect gate="MCU" pin="PB0" pad="L4"/>
<connect gate="MCU" pin="PB1" pad="M4"/>
<connect gate="MCU" pin="PB10" pad="M9"/>
<connect gate="MCU" pin="PB11" pad="M10"/>
<connect gate="MCU" pin="PB12" pad="M11"/>
<connect gate="MCU" pin="PB13" pad="M12"/>
<connect gate="MCU" pin="PB14" pad="L11"/>
<connect gate="MCU" pin="PB15" pad="L12"/>
<connect gate="MCU" pin="PB2" pad="J5"/>
<connect gate="MCU" pin="PB3" pad="A7"/>
<connect gate="MCU" pin="PB4" pad="A6"/>
<connect gate="MCU" pin="PB5" pad="B6"/>
<connect gate="MCU" pin="PB6" pad="C6"/>
<connect gate="MCU" pin="PB7" pad="D6"/>
<connect gate="MCU" pin="PB8" pad="C5"/>
<connect gate="MCU" pin="PB9" pad="B5"/>
<connect gate="MCU" pin="PC0" pad="H1"/>
<connect gate="MCU" pin="PC1" pad="H2"/>
<connect gate="MCU" pin="PC10" pad="B11"/>
<connect gate="MCU" pin="PC11" pad="B10"/>
<connect gate="MCU" pin="PC12" pad="C10"/>
<connect gate="MCU" pin="PC13" pad="A1"/>
<connect gate="MCU" pin="PC14" pad="B1"/>
<connect gate="MCU" pin="PC15" pad="C1"/>
<connect gate="MCU" pin="PC2" pad="H3"/>
<connect gate="MCU" pin="PC3" pad="H4"/>
<connect gate="MCU" pin="PC4" pad="J4"/>
<connect gate="MCU" pin="PC5" pad="K4"/>
<connect gate="MCU" pin="PC6" pad="G12"/>
<connect gate="MCU" pin="PC7" pad="F12"/>
<connect gate="MCU" pin="PC8" pad="F11"/>
<connect gate="MCU" pin="PC9" pad="E11"/>
<connect gate="MCU" pin="PD0" pad="E10"/>
<connect gate="MCU" pin="PD1" pad="D10"/>
<connect gate="MCU" pin="PD10" pad="J9"/>
<connect gate="MCU" pin="PD11" pad="H9"/>
<connect gate="MCU" pin="PD12" pad="L10"/>
<connect gate="MCU" pin="PD13" pad="K10"/>
<connect gate="MCU" pin="PD14" pad="K11"/>
<connect gate="MCU" pin="PD15" pad="K12"/>
<connect gate="MCU" pin="PD2" pad="E9"/>
<connect gate="MCU" pin="PD3" pad="D9"/>
<connect gate="MCU" pin="PD4" pad="C9"/>
<connect gate="MCU" pin="PD5" pad="B9"/>
<connect gate="MCU" pin="PD6" pad="A8"/>
<connect gate="MCU" pin="PD7" pad="A9"/>
<connect gate="MCU" pin="PD8" pad="L9"/>
<connect gate="MCU" pin="PD9" pad="K9"/>
<connect gate="MCU" pin="PE0" pad="A5"/>
<connect gate="MCU" pin="PE1" pad="A4"/>
<connect gate="MCU" pin="PE10" pad="J7"/>
<connect gate="MCU" pin="PE11" pad="H8"/>
<connect gate="MCU" pin="PE12" pad="J8"/>
<connect gate="MCU" pin="PE13" pad="K8"/>
<connect gate="MCU" pin="PE14" pad="L8"/>
<connect gate="MCU" pin="PE15" pad="M8"/>
<connect gate="MCU" pin="PE2" pad="A3"/>
<connect gate="MCU" pin="PE3" pad="A2"/>
<connect gate="MCU" pin="PE4" pad="B2"/>
<connect gate="MCU" pin="PE5" pad="B3"/>
<connect gate="MCU" pin="PE6" pad="B4"/>
<connect gate="MCU" pin="PE7" pad="M7"/>
<connect gate="MCU" pin="PE8" pad="L7"/>
<connect gate="MCU" pin="PE9" pad="K7"/>
<connect gate="MCU" pin="PF0" pad="C3"/>
<connect gate="MCU" pin="PF1" pad="C4"/>
<connect gate="MCU" pin="PF10" pad="G1"/>
<connect gate="MCU" pin="PF11" pad="M5"/>
<connect gate="MCU" pin="PF12" pad="L5"/>
<connect gate="MCU" pin="PF13" pad="K5"/>
<connect gate="MCU" pin="PF14" pad="M6"/>
<connect gate="MCU" pin="PF15" pad="L6"/>
<connect gate="MCU" pin="PF2" pad="D4"/>
<connect gate="MCU" pin="PF3" pad="E2"/>
<connect gate="MCU" pin="PF4" pad="E3"/>
<connect gate="MCU" pin="PF5" pad="E4"/>
<connect gate="MCU" pin="PF6" pad="F3"/>
<connect gate="MCU" pin="PF7" pad="F2"/>
<connect gate="MCU" pin="PF8" pad="G3"/>
<connect gate="MCU" pin="PF9" pad="G2"/>
<connect gate="MCU" pin="PG0" pad="K6"/>
<connect gate="MCU" pin="PG1" pad="J6"/>
<connect gate="MCU" pin="PG10" pad="D8"/>
<connect gate="MCU" pin="PG11" pad="C8"/>
<connect gate="MCU" pin="PG12" pad="B8"/>
<connect gate="MCU" pin="PG13" pad="D7"/>
<connect gate="MCU" pin="PG14" pad="C7"/>
<connect gate="MCU" pin="PG15" pad="B7"/>
<connect gate="MCU" pin="PG2" pad="J12"/>
<connect gate="MCU" pin="PG3" pad="J11"/>
<connect gate="MCU" pin="PG4" pad="J10"/>
<connect gate="MCU" pin="PG5" pad="H12"/>
<connect gate="MCU" pin="PG6" pad="H11"/>
<connect gate="MCU" pin="PG7" pad="H10"/>
<connect gate="MCU" pin="PG8" pad="G11"/>
<connect gate="MCU" pin="PG9" pad="E8"/>
<connect gate="MCU" pin="VBAT" pad="C2"/>
<connect gate="MCU" pin="VDDA" pad="M1"/>
<connect gate="MCU" pin="VREF+" pad="L1"/>
<connect gate="MCU" pin="VREF-" pad="K1"/>
<connect gate="MCU" pin="VSSA" pad="J1"/>
<connect gate="PWR" pin="VDD@1" pad="G7"/>
<connect gate="PWR" pin="VDD@10" pad="F7"/>
<connect gate="PWR" pin="VDD@11" pad="F6"/>
<connect gate="PWR" pin="VDD@2" pad="F9"/>
<connect gate="PWR" pin="VDD@3" pad="F5"/>
<connect gate="PWR" pin="VDD@4" pad="F4"/>
<connect gate="PWR" pin="VDD@5" pad="D3"/>
<connect gate="PWR" pin="VDD@6" pad="G5"/>
<connect gate="PWR" pin="VDD@7" pad="G6"/>
<connect gate="PWR" pin="VDD@8" pad="F8"/>
<connect gate="PWR" pin="VDD@9" pad="F10"/>
<connect gate="PWR" pin="VSS@1" pad="H7"/>
<connect gate="PWR" pin="VSS@10" pad="E7"/>
<connect gate="PWR" pin="VSS@11" pad="E6"/>
<connect gate="PWR" pin="VSS@2" pad="G9"/>
<connect gate="PWR" pin="VSS@3" pad="E5"/>
<connect gate="PWR" pin="VSS@4" pad="G4"/>
<connect gate="PWR" pin="VSS@5" pad="D2"/>
<connect gate="PWR" pin="VSS@6" pad="H5"/>
<connect gate="PWR" pin="VSS@7" pad="H6"/>
<connect gate="PWR" pin="VSS@8" pad="G8"/>
<connect gate="PWR" pin="VSS@9" pad="G10"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="D"/>
<technology name="E"/>
<technology name="F"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F103Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
256 to 1024 Kbytes of Flash memory&lt;br&gt;
48 to 96 kbytes of SRAM&lt;br&gt;
112 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD11_VSS11"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VREF-" pad="31"/>
<connect gate="MCU" pin="VSSA" pad="30"/>
<connect gate="PWR" pin="VDD@1" pad="72"/>
<connect gate="PWR" pin="VDD@10" pad="121"/>
<connect gate="PWR" pin="VDD@11" pad="131"/>
<connect gate="PWR" pin="VDD@2" pad="108"/>
<connect gate="PWR" pin="VDD@3" pad="144"/>
<connect gate="PWR" pin="VDD@4" pad="39"/>
<connect gate="PWR" pin="VDD@5" pad="17"/>
<connect gate="PWR" pin="VDD@6" pad="52"/>
<connect gate="PWR" pin="VDD@7" pad="62"/>
<connect gate="PWR" pin="VDD@8" pad="84"/>
<connect gate="PWR" pin="VDD@9" pad="95"/>
<connect gate="PWR" pin="VSS@1" pad="71"/>
<connect gate="PWR" pin="VSS@10" pad="120"/>
<connect gate="PWR" pin="VSS@11" pad="130"/>
<connect gate="PWR" pin="VSS@2" pad="107"/>
<connect gate="PWR" pin="VSS@3" pad="143"/>
<connect gate="PWR" pin="VSS@4" pad="38"/>
<connect gate="PWR" pin="VSS@5" pad="16"/>
<connect gate="PWR" pin="VSS@6" pad="51"/>
<connect gate="PWR" pin="VSS@7" pad="61"/>
<connect gate="PWR" pin="VSS@8" pad="83"/>
<connect gate="PWR" pin="VSS@9" pad="94"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="D"/>
<technology name="E"/>
<technology name="F"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F105R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
64 to 256 Kbytes of Flash memory&lt;br&gt;
64 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="32"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="31"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
<connect gate="PWR" pin="VSS@3" pad="63"/>
<connect gate="PWR" pin="VSS@4" pad="18"/>
</connects>
<technologies>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F105V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
64 to 256 Kbytes of Flash memory&lt;br&gt;
64 kbytes of SRAM&lt;br&gt;
80 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD5_VSS5"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0-WKUP" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VREF-" pad="20"/>
<connect gate="MCU" pin="VSSA" pad="19"/>
<connect gate="PWR" pin="VDD@1" pad="50"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="100"/>
<connect gate="PWR" pin="VDD@4" pad="28"/>
<connect gate="PWR" pin="VDD@5" pad="11"/>
<connect gate="PWR" pin="VSS@1" pad="49"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
<connect gate="PWR" pin="VSS@3" pad="99"/>
<connect gate="PWR" pin="VSS@4" pad="27"/>
<connect gate="PWR" pin="VSS@5" pad="10"/>
</connects>
<technologies>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F105V*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
64 kbytes of SRAM&lt;br&gt;
80 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD5_VSS5"/>
</gates>
<devices>
<device name="" package="LFBGA100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="D5"/>
<connect gate="MCU" pin="NRST" pad="E1"/>
<connect gate="MCU" pin="OSC_IN" pad="C1"/>
<connect gate="MCU" pin="OSC_OUT" pad="D1"/>
<connect gate="MCU" pin="PA0-WKUP" pad="G2"/>
<connect gate="MCU" pin="PA1" pad="H2"/>
<connect gate="MCU" pin="PA10" pad="D10"/>
<connect gate="MCU" pin="PA11" pad="C10"/>
<connect gate="MCU" pin="PA12" pad="B10"/>
<connect gate="MCU" pin="PA13" pad="A10"/>
<connect gate="MCU" pin="PA14" pad="A9"/>
<connect gate="MCU" pin="PA15" pad="A8"/>
<connect gate="MCU" pin="PA2" pad="J2"/>
<connect gate="MCU" pin="PA3" pad="K2"/>
<connect gate="MCU" pin="PA4" pad="G3"/>
<connect gate="MCU" pin="PA5" pad="H3"/>
<connect gate="MCU" pin="PA6" pad="J3"/>
<connect gate="MCU" pin="PA7" pad="K3"/>
<connect gate="MCU" pin="PA8" pad="D9"/>
<connect gate="MCU" pin="PA9" pad="C9"/>
<connect gate="MCU" pin="PB0" pad="J4"/>
<connect gate="MCU" pin="PB1" pad="K4"/>
<connect gate="MCU" pin="PB10" pad="J7"/>
<connect gate="MCU" pin="PB11" pad="K7"/>
<connect gate="MCU" pin="PB12" pad="K8"/>
<connect gate="MCU" pin="PB13" pad="J8"/>
<connect gate="MCU" pin="PB14" pad="H8"/>
<connect gate="MCU" pin="PB15" pad="G8"/>
<connect gate="MCU" pin="PB2" pad="G5"/>
<connect gate="MCU" pin="PB3" pad="A7"/>
<connect gate="MCU" pin="PB4" pad="A6"/>
<connect gate="MCU" pin="PB5" pad="C5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="A5"/>
<connect gate="MCU" pin="PB8" pad="B4"/>
<connect gate="MCU" pin="PB9" pad="A4"/>
<connect gate="MCU" pin="PC0" pad="F1"/>
<connect gate="MCU" pin="PC1" pad="F2"/>
<connect gate="MCU" pin="PC10" pad="B9"/>
<connect gate="MCU" pin="PC11" pad="B8"/>
<connect gate="MCU" pin="PC12" pad="C8"/>
<connect gate="MCU" pin="PC13" pad="A2"/>
<connect gate="MCU" pin="PC14" pad="A1"/>
<connect gate="MCU" pin="PC15" pad="B1"/>
<connect gate="MCU" pin="PC2" pad="E2"/>
<connect gate="MCU" pin="PC3" pad="F3"/>
<connect gate="MCU" pin="PC4" pad="G4"/>
<connect gate="MCU" pin="PC5" pad="H4"/>
<connect gate="MCU" pin="PC6" pad="F10"/>
<connect gate="MCU" pin="PC7" pad="E10"/>
<connect gate="MCU" pin="PC8" pad="F9"/>
<connect gate="MCU" pin="PC9" pad="E9"/>
<connect gate="MCU" pin="PD0" pad="D8"/>
<connect gate="MCU" pin="PD1" pad="E8"/>
<connect gate="MCU" pin="PD10" pad="H9"/>
<connect gate="MCU" pin="PD11" pad="G9"/>
<connect gate="MCU" pin="PD12" pad="K10"/>
<connect gate="MCU" pin="PD13" pad="J10"/>
<connect gate="MCU" pin="PD14" pad="H10"/>
<connect gate="MCU" pin="PD15" pad="G10"/>
<connect gate="MCU" pin="PD2" pad="B7"/>
<connect gate="MCU" pin="PD3" pad="C7"/>
<connect gate="MCU" pin="PD4" pad="D7"/>
<connect gate="MCU" pin="PD5" pad="B6"/>
<connect gate="MCU" pin="PD6" pad="C6"/>
<connect gate="MCU" pin="PD7" pad="D6"/>
<connect gate="MCU" pin="PD8" pad="K9"/>
<connect gate="MCU" pin="PD9" pad="J9"/>
<connect gate="MCU" pin="PE0" pad="D4"/>
<connect gate="MCU" pin="PE1" pad="C4"/>
<connect gate="MCU" pin="PE10" pad="G6"/>
<connect gate="MCU" pin="PE11" pad="H6"/>
<connect gate="MCU" pin="PE12" pad="J6"/>
<connect gate="MCU" pin="PE13" pad="K6"/>
<connect gate="MCU" pin="PE14" pad="G7"/>
<connect gate="MCU" pin="PE15" pad="H7"/>
<connect gate="MCU" pin="PE2" pad="A3"/>
<connect gate="MCU" pin="PE3" pad="B3"/>
<connect gate="MCU" pin="PE4" pad="C3"/>
<connect gate="MCU" pin="PE5" pad="D3"/>
<connect gate="MCU" pin="PE6" pad="E3"/>
<connect gate="MCU" pin="PE7" pad="H5"/>
<connect gate="MCU" pin="PE8" pad="J5"/>
<connect gate="MCU" pin="PE9" pad="K5"/>
<connect gate="MCU" pin="VBAT" pad="B2"/>
<connect gate="MCU" pin="VDDA" pad="K1"/>
<connect gate="MCU" pin="VREF+" pad="J1"/>
<connect gate="MCU" pin="VREF-" pad="H1"/>
<connect gate="MCU" pin="VSSA" pad="G1"/>
<connect gate="PWR" pin="VDD@1" pad="F7"/>
<connect gate="PWR" pin="VDD@2" pad="F6"/>
<connect gate="PWR" pin="VDD@3" pad="F5"/>
<connect gate="PWR" pin="VDD@4" pad="F4"/>
<connect gate="PWR" pin="VDD@5" pad="D2"/>
<connect gate="PWR" pin="VSS@1" pad="E7"/>
<connect gate="PWR" pin="VSS@2" pad="E6"/>
<connect gate="PWR" pin="VSS@3" pad="E5"/>
<connect gate="PWR" pin="VSS@4" pad="E4"/>
<connect gate="PWR" pin="VSS@5" pad="C2"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F107R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
64 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="32"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="31"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
<connect gate="PWR" pin="VSS@3" pad="63"/>
<connect gate="PWR" pin="VSS@4" pad="18"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F107V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
64 kbytes of SRAM&lt;br&gt;
80 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD5_VSS5"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0-WKUP" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VREF-" pad="20"/>
<connect gate="MCU" pin="VSSA" pad="19"/>
<connect gate="PWR" pin="VDD@1" pad="50"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="100"/>
<connect gate="PWR" pin="VDD@4" pad="28"/>
<connect gate="PWR" pin="VDD@5" pad="11"/>
<connect gate="PWR" pin="VSS@1" pad="49"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
<connect gate="PWR" pin="VSS@3" pad="99"/>
<connect gate="PWR" pin="VSS@4" pad="27"/>
<connect gate="PWR" pin="VSS@5" pad="10"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F205R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
120 MHz maximum frequency&lt;br&gt;
128 to 1024 Kbytes of Flash memory&lt;br&gt;
64 to 128 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP5"/>
<gate name="PWR" symbol="PWR_VDD4_VSS2"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VCAP1" pad="31"/>
<connect gate="MCU" pin="VCAP2" pad="47"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="32"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="63"/>
<connect gate="PWR" pin="VSS@2" pad="18"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
<technology name="E"/>
<technology name="F"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F205R*Y" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
120 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_66PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD3_VSS4"/>
</gates>
<devices>
<device name="" package="WLCSP64+2">
<connects>
<connect gate="MCU" pin="BOOT0" pad="B6"/>
<connect gate="MCU" pin="IRROFF" pad="C8"/>
<connect gate="MCU" pin="NRST" pad="E8"/>
<connect gate="MCU" pin="OSC_IN" pad="E9"/>
<connect gate="MCU" pin="OSC_OUT" pad="F9"/>
<connect gate="MCU" pin="PA0-WKUP" pad="E7"/>
<connect gate="MCU" pin="PA1" pad="H8"/>
<connect gate="MCU" pin="PA10" pad="D3"/>
<connect gate="MCU" pin="PA11" pad="D2"/>
<connect gate="MCU" pin="PA12" pad="C1"/>
<connect gate="MCU" pin="PA13" pad="B2"/>
<connect gate="MCU" pin="PA14" pad="A1"/>
<connect gate="MCU" pin="PA15" pad="A2"/>
<connect gate="MCU" pin="PA2" pad="J9"/>
<connect gate="MCU" pin="PA3" pad="G7"/>
<connect gate="MCU" pin="PA4" pad="J8"/>
<connect gate="MCU" pin="PA5" pad="H6"/>
<connect gate="MCU" pin="PA6" pad="H5"/>
<connect gate="MCU" pin="PA7" pad="J7"/>
<connect gate="MCU" pin="PA8" pad="E2"/>
<connect gate="MCU" pin="PA9" pad="E3"/>
<connect gate="MCU" pin="PB0" pad="J6"/>
<connect gate="MCU" pin="PB1" pad="J5"/>
<connect gate="MCU" pin="PB10" pad="H3"/>
<connect gate="MCU" pin="PB11" pad="J2"/>
<connect gate="MCU" pin="PB12" pad="J1"/>
<connect gate="MCU" pin="PB13" pad="H2"/>
<connect gate="MCU" pin="PB14" pad="H1"/>
<connect gate="MCU" pin="PB15" pad="G1"/>
<connect gate="MCU" pin="PB2" pad="J4"/>
<connect gate="MCU" pin="PB3" pad="A4"/>
<connect gate="MCU" pin="PB4" pad="B4"/>
<connect gate="MCU" pin="PB5" pad="A5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="A6"/>
<connect gate="MCU" pin="PB8" pad="B7"/>
<connect gate="MCU" pin="PB9" pad="A7"/>
<connect gate="MCU" pin="PC0" pad="G9"/>
<connect gate="MCU" pin="PC1" pad="F8"/>
<connect gate="MCU" pin="PC10" pad="B3"/>
<connect gate="MCU" pin="PC11" pad="C3"/>
<connect gate="MCU" pin="PC12" pad="A3"/>
<connect gate="MCU" pin="PC13" pad="B8"/>
<connect gate="MCU" pin="PC14" pad="B9"/>
<connect gate="MCU" pin="PC15" pad="C9"/>
<connect gate="MCU" pin="PC2" pad="D7"/>
<connect gate="MCU" pin="PC3" pad="G8"/>
<connect gate="MCU" pin="PC4" pad="H4"/>
<connect gate="MCU" pin="PC5" pad="G3"/>
<connect gate="MCU" pin="PC6" pad="G2"/>
<connect gate="MCU" pin="PC7" pad="F2"/>
<connect gate="MCU" pin="PC8" pad="F3"/>
<connect gate="MCU" pin="PC9" pad="D1"/>
<connect gate="MCU" pin="PD2" pad="C7"/>
<connect gate="MCU" pin="REGOFF" pad="H7"/>
<connect gate="MCU" pin="VBAT" pad="A9"/>
<connect gate="MCU" pin="VCAP1" pad="J3"/>
<connect gate="MCU" pin="VCAP2" pad="C2"/>
<connect gate="MCU" pin="VREF+" pad="F7"/>
<connect gate="PWR" pin="VDD@1" pad="A8"/>
<connect gate="PWR" pin="VDD@2" pad="D9"/>
<connect gate="PWR" pin="VDD@3" pad="E1"/>
<connect gate="PWR" pin="VSS@1" pad="B1"/>
<connect gate="PWR" pin="VSS@2" pad="D8"/>
<connect gate="PWR" pin="VSS@3" pad="F1"/>
<connect gate="PWR" pin="VSS@4" pad="H9"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F205V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
120 MHz maximum frequency&lt;br&gt;
128 to 1024 Kbytes of Flash memory&lt;br&gt;
64 to 128 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD6_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0-WKUP" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="RFU" pad="99"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="49"/>
<connect gate="MCU" pin="VCAP2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="11"/>
<connect gate="PWR" pin="VDD@2" pad="19"/>
<connect gate="PWR" pin="VDD@3" pad="28"/>
<connect gate="PWR" pin="VDD@4" pad="50"/>
<connect gate="PWR" pin="VDD@5" pad="75"/>
<connect gate="PWR" pin="VDD@6" pad="100"/>
<connect gate="PWR" pin="VSS@1" pad="10"/>
<connect gate="PWR" pin="VSS@2" pad="27"/>
<connect gate="PWR" pin="VSS@3" pad="74"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
<technology name="E"/>
<technology name="F"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F205Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
120 MHz maximum frequency&lt;br&gt;
256 to 1024 Kbytes of Flash memory&lt;br&gt;
96 to 128 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD12_VSS9"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="RFU" pad="143"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="71"/>
<connect gate="MCU" pin="VCAP2" pad="106"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VSSA" pad="31"/>
<connect gate="PWR" pin="VDD@1" pad="17"/>
<connect gate="PWR" pin="VDD@10" pad="121"/>
<connect gate="PWR" pin="VDD@11" pad="131"/>
<connect gate="PWR" pin="VDD@12" pad="144"/>
<connect gate="PWR" pin="VDD@2" pad="30"/>
<connect gate="PWR" pin="VDD@3" pad="39"/>
<connect gate="PWR" pin="VDD@4" pad="52"/>
<connect gate="PWR" pin="VDD@5" pad="62"/>
<connect gate="PWR" pin="VDD@6" pad="72"/>
<connect gate="PWR" pin="VDD@7" pad="84"/>
<connect gate="PWR" pin="VDD@8" pad="95"/>
<connect gate="PWR" pin="VDD@9" pad="108"/>
<connect gate="PWR" pin="VSS@1" pad="16"/>
<connect gate="PWR" pin="VSS@2" pad="38"/>
<connect gate="PWR" pin="VSS@3" pad="51"/>
<connect gate="PWR" pin="VSS@4" pad="61"/>
<connect gate="PWR" pin="VSS@5" pad="83"/>
<connect gate="PWR" pin="VSS@6" pad="94"/>
<connect gate="PWR" pin="VSS@7" pad="107"/>
<connect gate="PWR" pin="VSS@8" pad="120"/>
<connect gate="PWR" pin="VSS@9" pad="130"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
<technology name="F"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F207V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
120 MHz maximum frequency&lt;br&gt;
256 to 1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD6_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0-WKUP" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="RFU" pad="99"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="49"/>
<connect gate="MCU" pin="VCAP2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="11"/>
<connect gate="PWR" pin="VDD@2" pad="19"/>
<connect gate="PWR" pin="VDD@3" pad="28"/>
<connect gate="PWR" pin="VDD@4" pad="50"/>
<connect gate="PWR" pin="VDD@5" pad="75"/>
<connect gate="PWR" pin="VDD@6" pad="100"/>
<connect gate="PWR" pin="VSS@1" pad="10"/>
<connect gate="PWR" pin="VSS@2" pad="27"/>
<connect gate="PWR" pin="VSS@3" pad="74"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
<technology name="F"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F207Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
120 MHz maximum frequency&lt;br&gt;
256 to 1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD12_VSS9"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="RFU" pad="143"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="71"/>
<connect gate="MCU" pin="VCAP2" pad="106"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VSSA" pad="31"/>
<connect gate="PWR" pin="VDD@1" pad="17"/>
<connect gate="PWR" pin="VDD@10" pad="121"/>
<connect gate="PWR" pin="VDD@11" pad="131"/>
<connect gate="PWR" pin="VDD@12" pad="144"/>
<connect gate="PWR" pin="VDD@2" pad="30"/>
<connect gate="PWR" pin="VDD@3" pad="39"/>
<connect gate="PWR" pin="VDD@4" pad="52"/>
<connect gate="PWR" pin="VDD@5" pad="62"/>
<connect gate="PWR" pin="VDD@6" pad="72"/>
<connect gate="PWR" pin="VDD@7" pad="84"/>
<connect gate="PWR" pin="VDD@8" pad="95"/>
<connect gate="PWR" pin="VDD@9" pad="108"/>
<connect gate="PWR" pin="VSS@1" pad="16"/>
<connect gate="PWR" pin="VSS@2" pad="38"/>
<connect gate="PWR" pin="VSS@3" pad="51"/>
<connect gate="PWR" pin="VSS@4" pad="61"/>
<connect gate="PWR" pin="VSS@5" pad="83"/>
<connect gate="PWR" pin="VSS@6" pad="94"/>
<connect gate="PWR" pin="VSS@7" pad="107"/>
<connect gate="PWR" pin="VSS@8" pad="120"/>
<connect gate="PWR" pin="VSS@9" pad="130"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
<technology name="F"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F207I*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
120 MHz maximum frequency&lt;br&gt;
256 to 1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD15_VSS12"/>
</gates>
<devices>
<device name="" package="LQFP176">
<connects>
<connect gate="MCU" pin="BOOT0" pad="166"/>
<connect gate="MCU" pin="NRST" pad="31"/>
<connect gate="MCU" pin="OSC_IN" pad="29"/>
<connect gate="MCU" pin="OSC_OUT" pad="30"/>
<connect gate="MCU" pin="PA0" pad="40"/>
<connect gate="MCU" pin="PA1" pad="41"/>
<connect gate="MCU" pin="PA10" pad="121"/>
<connect gate="MCU" pin="PA11" pad="122"/>
<connect gate="MCU" pin="PA12" pad="123"/>
<connect gate="MCU" pin="PA13" pad="124"/>
<connect gate="MCU" pin="PA14" pad="137"/>
<connect gate="MCU" pin="PA15" pad="138"/>
<connect gate="MCU" pin="PA2" pad="42"/>
<connect gate="MCU" pin="PA3" pad="47"/>
<connect gate="MCU" pin="PA4" pad="50"/>
<connect gate="MCU" pin="PA5" pad="51"/>
<connect gate="MCU" pin="PA6" pad="52"/>
<connect gate="MCU" pin="PA7" pad="53"/>
<connect gate="MCU" pin="PA8" pad="119"/>
<connect gate="MCU" pin="PA9" pad="120"/>
<connect gate="MCU" pin="PB0" pad="56"/>
<connect gate="MCU" pin="PB1" pad="57"/>
<connect gate="MCU" pin="PB10" pad="79"/>
<connect gate="MCU" pin="PB11" pad="80"/>
<connect gate="MCU" pin="PB12" pad="92"/>
<connect gate="MCU" pin="PB13" pad="93"/>
<connect gate="MCU" pin="PB14" pad="94"/>
<connect gate="MCU" pin="PB15" pad="95"/>
<connect gate="MCU" pin="PB2" pad="58"/>
<connect gate="MCU" pin="PB3" pad="161"/>
<connect gate="MCU" pin="PB4" pad="162"/>
<connect gate="MCU" pin="PB5" pad="163"/>
<connect gate="MCU" pin="PB6" pad="164"/>
<connect gate="MCU" pin="PB7" pad="165"/>
<connect gate="MCU" pin="PB8" pad="167"/>
<connect gate="MCU" pin="PB9" pad="168"/>
<connect gate="MCU" pin="PC0" pad="32"/>
<connect gate="MCU" pin="PC1" pad="33"/>
<connect gate="MCU" pin="PC10" pad="139"/>
<connect gate="MCU" pin="PC11" pad="140"/>
<connect gate="MCU" pin="PC12" pad="141"/>
<connect gate="MCU" pin="PC13" pad="8"/>
<connect gate="MCU" pin="PC14" pad="9"/>
<connect gate="MCU" pin="PC15" pad="10"/>
<connect gate="MCU" pin="PC2" pad="34"/>
<connect gate="MCU" pin="PC3" pad="35"/>
<connect gate="MCU" pin="PC4" pad="54"/>
<connect gate="MCU" pin="PC5" pad="55"/>
<connect gate="MCU" pin="PC6" pad="115"/>
<connect gate="MCU" pin="PC7" pad="116"/>
<connect gate="MCU" pin="PC8" pad="117"/>
<connect gate="MCU" pin="PC9" pad="118"/>
<connect gate="MCU" pin="PD0" pad="142"/>
<connect gate="MCU" pin="PD1" pad="143"/>
<connect gate="MCU" pin="PD10" pad="98"/>
<connect gate="MCU" pin="PD11" pad="99"/>
<connect gate="MCU" pin="PD12" pad="100"/>
<connect gate="MCU" pin="PD13" pad="101"/>
<connect gate="MCU" pin="PD14" pad="104"/>
<connect gate="MCU" pin="PD15" pad="105"/>
<connect gate="MCU" pin="PD2" pad="144"/>
<connect gate="MCU" pin="PD3" pad="145"/>
<connect gate="MCU" pin="PD4" pad="146"/>
<connect gate="MCU" pin="PD5" pad="147"/>
<connect gate="MCU" pin="PD6" pad="150"/>
<connect gate="MCU" pin="PD7" pad="151"/>
<connect gate="MCU" pin="PD8" pad="96"/>
<connect gate="MCU" pin="PD9" pad="97"/>
<connect gate="MCU" pin="PDR_ON" pad="171"/>
<connect gate="MCU" pin="PE0" pad="169"/>
<connect gate="MCU" pin="PE1" pad="170"/>
<connect gate="MCU" pin="PE10" pad="73"/>
<connect gate="MCU" pin="PE11" pad="74"/>
<connect gate="MCU" pin="PE12" pad="75"/>
<connect gate="MCU" pin="PE13" pad="76"/>
<connect gate="MCU" pin="PE14" pad="77"/>
<connect gate="MCU" pin="PE15" pad="78"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="68"/>
<connect gate="MCU" pin="PE8" pad="69"/>
<connect gate="MCU" pin="PE9" pad="70"/>
<connect gate="MCU" pin="PF0" pad="16"/>
<connect gate="MCU" pin="PF1" pad="17"/>
<connect gate="MCU" pin="PF10" pad="28"/>
<connect gate="MCU" pin="PF11" pad="59"/>
<connect gate="MCU" pin="PF12" pad="60"/>
<connect gate="MCU" pin="PF13" pad="63"/>
<connect gate="MCU" pin="PF14" pad="64"/>
<connect gate="MCU" pin="PF15" pad="65"/>
<connect gate="MCU" pin="PF2" pad="18"/>
<connect gate="MCU" pin="PF3" pad="19"/>
<connect gate="MCU" pin="PF4" pad="20"/>
<connect gate="MCU" pin="PF5" pad="21"/>
<connect gate="MCU" pin="PF6" pad="24"/>
<connect gate="MCU" pin="PF7" pad="25"/>
<connect gate="MCU" pin="PF8" pad="26"/>
<connect gate="MCU" pin="PF9" pad="27"/>
<connect gate="MCU" pin="PG0" pad="66"/>
<connect gate="MCU" pin="PG1" pad="67"/>
<connect gate="MCU" pin="PG10" pad="153"/>
<connect gate="MCU" pin="PG11" pad="154"/>
<connect gate="MCU" pin="PG12" pad="155"/>
<connect gate="MCU" pin="PG13" pad="156"/>
<connect gate="MCU" pin="PG14" pad="157"/>
<connect gate="MCU" pin="PG15" pad="160"/>
<connect gate="MCU" pin="PG2" pad="106"/>
<connect gate="MCU" pin="PG3" pad="107"/>
<connect gate="MCU" pin="PG4" pad="108"/>
<connect gate="MCU" pin="PG5" pad="109"/>
<connect gate="MCU" pin="PG6" pad="110"/>
<connect gate="MCU" pin="PG7" pad="111"/>
<connect gate="MCU" pin="PG8" pad="112"/>
<connect gate="MCU" pin="PG9" pad="152"/>
<connect gate="MCU" pin="PH10" pad="87"/>
<connect gate="MCU" pin="PH11" pad="88"/>
<connect gate="MCU" pin="PH12" pad="89"/>
<connect gate="MCU" pin="PH13" pad="128"/>
<connect gate="MCU" pin="PH14" pad="129"/>
<connect gate="MCU" pin="PH15" pad="130"/>
<connect gate="MCU" pin="PH2" pad="43"/>
<connect gate="MCU" pin="PH3" pad="44"/>
<connect gate="MCU" pin="PH4" pad="45"/>
<connect gate="MCU" pin="PH5" pad="46"/>
<connect gate="MCU" pin="PH6" pad="83"/>
<connect gate="MCU" pin="PH7" pad="84"/>
<connect gate="MCU" pin="PH8" pad="85"/>
<connect gate="MCU" pin="PH9" pad="86"/>
<connect gate="MCU" pin="PI0" pad="131"/>
<connect gate="MCU" pin="PI1" pad="132"/>
<connect gate="MCU" pin="PI10" pad="12"/>
<connect gate="MCU" pin="PI11" pad="13"/>
<connect gate="MCU" pin="PI2" pad="133"/>
<connect gate="MCU" pin="PI3" pad="134"/>
<connect gate="MCU" pin="PI4" pad="173"/>
<connect gate="MCU" pin="PI5" pad="174"/>
<connect gate="MCU" pin="PI6" pad="175"/>
<connect gate="MCU" pin="PI7" pad="176"/>
<connect gate="MCU" pin="PI8" pad="7"/>
<connect gate="MCU" pin="PI9" pad="11"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="81"/>
<connect gate="MCU" pin="VCAP2" pad="125"/>
<connect gate="MCU" pin="VDDA" pad="39"/>
<connect gate="MCU" pin="VREF+" pad="38"/>
<connect gate="MCU" pin="VSSA" pad="37"/>
<connect gate="PWR" pin="VDD@1" pad="15"/>
<connect gate="PWR" pin="VDD@10" pad="114"/>
<connect gate="PWR" pin="VDD@11" pad="127"/>
<connect gate="PWR" pin="VDD@12" pad="136"/>
<connect gate="PWR" pin="VDD@13" pad="149"/>
<connect gate="PWR" pin="VDD@14" pad="159"/>
<connect gate="PWR" pin="VDD@15" pad="172"/>
<connect gate="PWR" pin="VDD@2" pad="23"/>
<connect gate="PWR" pin="VDD@3" pad="36"/>
<connect gate="PWR" pin="VDD@4" pad="49"/>
<connect gate="PWR" pin="VDD@5" pad="62"/>
<connect gate="PWR" pin="VDD@6" pad="72"/>
<connect gate="PWR" pin="VDD@7" pad="82"/>
<connect gate="PWR" pin="VDD@8" pad="91"/>
<connect gate="PWR" pin="VDD@9" pad="103"/>
<connect gate="PWR" pin="VSS@1" pad="14"/>
<connect gate="PWR" pin="VSS@10" pad="135"/>
<connect gate="PWR" pin="VSS@11" pad="148"/>
<connect gate="PWR" pin="VSS@12" pad="158"/>
<connect gate="PWR" pin="VSS@2" pad="22"/>
<connect gate="PWR" pin="VSS@3" pad="48"/>
<connect gate="PWR" pin="VSS@4" pad="61"/>
<connect gate="PWR" pin="VSS@5" pad="71"/>
<connect gate="PWR" pin="VSS@6" pad="90"/>
<connect gate="PWR" pin="VSS@7" pad="102"/>
<connect gate="PWR" pin="VSS@8" pad="113"/>
<connect gate="PWR" pin="VSS@9" pad="126"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
<technology name="F"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F207I*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
120 MHz maximum frequency&lt;br&gt;
256 to 1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD14_VSS36"/>
</gates>
<devices>
<device name="" package="UFBGA176+25">
<connects>
<connect gate="MCU" pin="BOOT0" pad="D6"/>
<connect gate="MCU" pin="NRST" pad="J1"/>
<connect gate="MCU" pin="OSC_IN" pad="G1"/>
<connect gate="MCU" pin="OSC_OUT" pad="H1"/>
<connect gate="MCU" pin="PA0" pad="N3"/>
<connect gate="MCU" pin="PA1" pad="N2"/>
<connect gate="MCU" pin="PA10" pad="D15"/>
<connect gate="MCU" pin="PA11" pad="C15"/>
<connect gate="MCU" pin="PA12" pad="B15"/>
<connect gate="MCU" pin="PA13" pad="A15"/>
<connect gate="MCU" pin="PA14" pad="A14"/>
<connect gate="MCU" pin="PA15" pad="A13"/>
<connect gate="MCU" pin="PA2" pad="P2"/>
<connect gate="MCU" pin="PA3" pad="R2"/>
<connect gate="MCU" pin="PA4" pad="N4"/>
<connect gate="MCU" pin="PA5" pad="P4"/>
<connect gate="MCU" pin="PA6" pad="P3"/>
<connect gate="MCU" pin="PA7" pad="R3"/>
<connect gate="MCU" pin="PA8" pad="F15"/>
<connect gate="MCU" pin="PA9" pad="E15"/>
<connect gate="MCU" pin="PB0" pad="R5"/>
<connect gate="MCU" pin="PB1" pad="R4"/>
<connect gate="MCU" pin="PB10" pad="R12"/>
<connect gate="MCU" pin="PB11" pad="R13"/>
<connect gate="MCU" pin="PB12" pad="P12"/>
<connect gate="MCU" pin="PB13" pad="P13"/>
<connect gate="MCU" pin="PB14" pad="R14"/>
<connect gate="MCU" pin="PB15" pad="R15"/>
<connect gate="MCU" pin="PB2" pad="M6"/>
<connect gate="MCU" pin="PB3" pad="A10"/>
<connect gate="MCU" pin="PB4" pad="A9"/>
<connect gate="MCU" pin="PB5" pad="A6"/>
<connect gate="MCU" pin="PB6" pad="B6"/>
<connect gate="MCU" pin="PB7" pad="B5"/>
<connect gate="MCU" pin="PB8" pad="A5"/>
<connect gate="MCU" pin="PB9" pad="B4"/>
<connect gate="MCU" pin="PC0" pad="M2"/>
<connect gate="MCU" pin="PC1" pad="M3"/>
<connect gate="MCU" pin="PC10" pad="B14"/>
<connect gate="MCU" pin="PC11" pad="B13"/>
<connect gate="MCU" pin="PC12" pad="A12"/>
<connect gate="MCU" pin="PC13" pad="D1"/>
<connect gate="MCU" pin="PC14" pad="E1"/>
<connect gate="MCU" pin="PC15" pad="F1"/>
<connect gate="MCU" pin="PC2" pad="M4"/>
<connect gate="MCU" pin="PC3" pad="M5"/>
<connect gate="MCU" pin="PC4" pad="N5"/>
<connect gate="MCU" pin="PC5" pad="P5"/>
<connect gate="MCU" pin="PC6" pad="H15"/>
<connect gate="MCU" pin="PC7" pad="G15"/>
<connect gate="MCU" pin="PC8" pad="G14"/>
<connect gate="MCU" pin="PC9" pad="F14"/>
<connect gate="MCU" pin="PD0" pad="B12"/>
<connect gate="MCU" pin="PD1" pad="C12"/>
<connect gate="MCU" pin="PD10" pad="N15"/>
<connect gate="MCU" pin="PD11" pad="N14"/>
<connect gate="MCU" pin="PD12" pad="N13"/>
<connect gate="MCU" pin="PD13" pad="M15"/>
<connect gate="MCU" pin="PD14" pad="M14"/>
<connect gate="MCU" pin="PD15" pad="L14"/>
<connect gate="MCU" pin="PD2" pad="D12"/>
<connect gate="MCU" pin="PD3" pad="D11"/>
<connect gate="MCU" pin="PD4" pad="D10"/>
<connect gate="MCU" pin="PD5" pad="C11"/>
<connect gate="MCU" pin="PD6" pad="B11"/>
<connect gate="MCU" pin="PD7" pad="A11"/>
<connect gate="MCU" pin="PD8" pad="P15"/>
<connect gate="MCU" pin="PD9" pad="P14"/>
<connect gate="MCU" pin="PE0" pad="A4"/>
<connect gate="MCU" pin="PE1" pad="A3"/>
<connect gate="MCU" pin="PE10" pad="R9"/>
<connect gate="MCU" pin="PE11" pad="P10"/>
<connect gate="MCU" pin="PE12" pad="R10"/>
<connect gate="MCU" pin="PE13" pad="N11"/>
<connect gate="MCU" pin="PE14" pad="P11"/>
<connect gate="MCU" pin="PE15" pad="R11"/>
<connect gate="MCU" pin="PE2" pad="A2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="B2"/>
<connect gate="MCU" pin="PE6" pad="B3"/>
<connect gate="MCU" pin="PE7" pad="R8"/>
<connect gate="MCU" pin="PE8" pad="P8"/>
<connect gate="MCU" pin="PE9" pad="P9"/>
<connect gate="MCU" pin="PF0" pad="E2"/>
<connect gate="MCU" pin="PF1" pad="H3"/>
<connect gate="MCU" pin="PF10" pad="L1"/>
<connect gate="MCU" pin="PF11" pad="R6"/>
<connect gate="MCU" pin="PF12" pad="P6"/>
<connect gate="MCU" pin="PF13" pad="N6"/>
<connect gate="MCU" pin="PF14" pad="R7"/>
<connect gate="MCU" pin="PF15" pad="P7"/>
<connect gate="MCU" pin="PF2" pad="H2"/>
<connect gate="MCU" pin="PF3" pad="J2"/>
<connect gate="MCU" pin="PF4" pad="J3"/>
<connect gate="MCU" pin="PF5" pad="K3"/>
<connect gate="MCU" pin="PF6" pad="K2"/>
<connect gate="MCU" pin="PF7" pad="K1"/>
<connect gate="MCU" pin="PF8" pad="L3"/>
<connect gate="MCU" pin="PF9" pad="L2"/>
<connect gate="MCU" pin="PG0" pad="N7"/>
<connect gate="MCU" pin="PG1" pad="M7"/>
<connect gate="MCU" pin="PG10" pad="B10"/>
<connect gate="MCU" pin="PG11" pad="B9"/>
<connect gate="MCU" pin="PG12" pad="B8"/>
<connect gate="MCU" pin="PG13" pad="A8"/>
<connect gate="MCU" pin="PG14" pad="A7"/>
<connect gate="MCU" pin="PG15" pad="B7"/>
<connect gate="MCU" pin="PG2" pad="L15"/>
<connect gate="MCU" pin="PG3" pad="K15"/>
<connect gate="MCU" pin="PG4" pad="K14"/>
<connect gate="MCU" pin="PG5" pad="K13"/>
<connect gate="MCU" pin="PG6" pad="J15"/>
<connect gate="MCU" pin="PG7" pad="J14"/>
<connect gate="MCU" pin="PG8" pad="H14"/>
<connect gate="MCU" pin="PG9" pad="C10"/>
<connect gate="MCU" pin="PH10" pad="L13"/>
<connect gate="MCU" pin="PH11" pad="L12"/>
<connect gate="MCU" pin="PH12" pad="K12"/>
<connect gate="MCU" pin="PH13" pad="E12"/>
<connect gate="MCU" pin="PH14" pad="E13"/>
<connect gate="MCU" pin="PH15" pad="D13"/>
<connect gate="MCU" pin="PH2" pad="F4"/>
<connect gate="MCU" pin="PH3" pad="G4"/>
<connect gate="MCU" pin="PH4" pad="H4"/>
<connect gate="MCU" pin="PH5" pad="J4"/>
<connect gate="MCU" pin="PH6" pad="M11"/>
<connect gate="MCU" pin="PH7" pad="N12"/>
<connect gate="MCU" pin="PH8" pad="M12"/>
<connect gate="MCU" pin="PH9" pad="M13"/>
<connect gate="MCU" pin="PI0" pad="E14"/>
<connect gate="MCU" pin="PI1" pad="D14"/>
<connect gate="MCU" pin="PI10" pad="E3"/>
<connect gate="MCU" pin="PI11" pad="E4"/>
<connect gate="MCU" pin="PI2" pad="C14"/>
<connect gate="MCU" pin="PI3" pad="C13"/>
<connect gate="MCU" pin="PI4" pad="D4"/>
<connect gate="MCU" pin="PI5" pad="C4"/>
<connect gate="MCU" pin="PI6" pad="C3"/>
<connect gate="MCU" pin="PI7" pad="C2"/>
<connect gate="MCU" pin="PI8" pad="D2"/>
<connect gate="MCU" pin="PI9" pad="D3"/>
<connect gate="MCU" pin="REGOFF" pad="L4"/>
<connect gate="MCU" pin="RFU" pad="C6"/>
<connect gate="MCU" pin="VBAT" pad="C1"/>
<connect gate="MCU" pin="VCAP1" pad="M10"/>
<connect gate="MCU" pin="VCAP2" pad="F13"/>
<connect gate="MCU" pin="VDDA" pad="R1"/>
<connect gate="MCU" pin="VREF+" pad="P1"/>
<connect gate="MCU" pin="VREF-" pad="N1"/>
<connect gate="MCU" pin="VSSA" pad="M1"/>
<connect gate="PWR" pin="VDD@1" pad="C5"/>
<connect gate="PWR" pin="VDD@10" pad="J13"/>
<connect gate="PWR" pin="VDD@11" pad="K4"/>
<connect gate="PWR" pin="VDD@12" pad="N8"/>
<connect gate="PWR" pin="VDD@13" pad="N9"/>
<connect gate="PWR" pin="VDD@14" pad="N10"/>
<connect gate="PWR" pin="VDD@2" pad="C7"/>
<connect gate="PWR" pin="VDD@3" pad="C8"/>
<connect gate="PWR" pin="VDD@4" pad="C9"/>
<connect gate="PWR" pin="VDD@5" pad="F3"/>
<connect gate="PWR" pin="VDD@6" pad="G3"/>
<connect gate="PWR" pin="VDD@7" pad="G13"/>
<connect gate="PWR" pin="VDD@8" pad="H13"/>
<connect gate="PWR" pin="VDD@9" pad="J12"/>
<connect gate="PWR" pin="VSS@1" pad="D5"/>
<connect gate="PWR" pin="VSS@10" pad="M8"/>
<connect gate="PWR" pin="VSS@11" pad="M9"/>
<connect gate="PWR" pin="VSS@12" pad="VSS_1"/>
<connect gate="PWR" pin="VSS@13" pad="VSS_2"/>
<connect gate="PWR" pin="VSS@14" pad="VSS_3"/>
<connect gate="PWR" pin="VSS@15" pad="VSS_4"/>
<connect gate="PWR" pin="VSS@16" pad="VSS_5"/>
<connect gate="PWR" pin="VSS@17" pad="VSS_6"/>
<connect gate="PWR" pin="VSS@18" pad="VSS_7"/>
<connect gate="PWR" pin="VSS@19" pad="VSS_8"/>
<connect gate="PWR" pin="VSS@2" pad="D7"/>
<connect gate="PWR" pin="VSS@20" pad="VSS_9"/>
<connect gate="PWR" pin="VSS@21" pad="VSS_10"/>
<connect gate="PWR" pin="VSS@22" pad="VSS_11"/>
<connect gate="PWR" pin="VSS@23" pad="VSS_12"/>
<connect gate="PWR" pin="VSS@24" pad="VSS_13"/>
<connect gate="PWR" pin="VSS@25" pad="VSS_14"/>
<connect gate="PWR" pin="VSS@26" pad="VSS_15"/>
<connect gate="PWR" pin="VSS@27" pad="VSS_16"/>
<connect gate="PWR" pin="VSS@28" pad="VSS_17"/>
<connect gate="PWR" pin="VSS@29" pad="VSS_18"/>
<connect gate="PWR" pin="VSS@3" pad="D8"/>
<connect gate="PWR" pin="VSS@30" pad="VSS_19"/>
<connect gate="PWR" pin="VSS@31" pad="VSS_20"/>
<connect gate="PWR" pin="VSS@32" pad="VSS_21"/>
<connect gate="PWR" pin="VSS@33" pad="VSS_22"/>
<connect gate="PWR" pin="VSS@34" pad="VSS_23"/>
<connect gate="PWR" pin="VSS@35" pad="VSS_24"/>
<connect gate="PWR" pin="VSS@36" pad="VSS_25"/>
<connect gate="PWR" pin="VSS@4" pad="D9"/>
<connect gate="PWR" pin="VSS@5" pad="F2"/>
<connect gate="PWR" pin="VSS@6" pad="F12"/>
<connect gate="PWR" pin="VSS@7" pad="G2"/>
<connect gate="PWR" pin="VSS@8" pad="G12"/>
<connect gate="PWR" pin="VSS@9" pad="H12"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
<technology name="F"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F215R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
120 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP5"/>
<gate name="PWR" symbol="PWR_VDD4_VSS2"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VCAP1" pad="31"/>
<connect gate="MCU" pin="VCAP2" pad="47"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="19"/>
<connect gate="PWR" pin="VDD@2" pad="64"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VDD@4" pad="32"/>
<connect gate="PWR" pin="VSS@1" pad="18"/>
<connect gate="PWR" pin="VSS@2" pad="63"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F215V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
120 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD6_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0-WKUP" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="RFU" pad="99"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="49"/>
<connect gate="MCU" pin="VCAP2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="11"/>
<connect gate="PWR" pin="VDD@2" pad="19"/>
<connect gate="PWR" pin="VDD@3" pad="28"/>
<connect gate="PWR" pin="VDD@4" pad="50"/>
<connect gate="PWR" pin="VDD@5" pad="75"/>
<connect gate="PWR" pin="VDD@6" pad="100"/>
<connect gate="PWR" pin="VSS@1" pad="10"/>
<connect gate="PWR" pin="VSS@2" pad="27"/>
<connect gate="PWR" pin="VSS@3" pad="74"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F215Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
120 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD12_VSS9"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="RFU" pad="143"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="71"/>
<connect gate="MCU" pin="VCAP2" pad="106"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VSSA" pad="31"/>
<connect gate="PWR" pin="VDD@1" pad="17"/>
<connect gate="PWR" pin="VDD@10" pad="108"/>
<connect gate="PWR" pin="VDD@11" pad="131"/>
<connect gate="PWR" pin="VDD@12" pad="144"/>
<connect gate="PWR" pin="VDD@2" pad="30"/>
<connect gate="PWR" pin="VDD@3" pad="39"/>
<connect gate="PWR" pin="VDD@4" pad="52"/>
<connect gate="PWR" pin="VDD@5" pad="62"/>
<connect gate="PWR" pin="VDD@6" pad="72"/>
<connect gate="PWR" pin="VDD@7" pad="84"/>
<connect gate="PWR" pin="VDD@8" pad="121"/>
<connect gate="PWR" pin="VDD@9" pad="95"/>
<connect gate="PWR" pin="VSS@1" pad="16"/>
<connect gate="PWR" pin="VSS@2" pad="38"/>
<connect gate="PWR" pin="VSS@3" pad="51"/>
<connect gate="PWR" pin="VSS@4" pad="61"/>
<connect gate="PWR" pin="VSS@5" pad="83"/>
<connect gate="PWR" pin="VSS@6" pad="94"/>
<connect gate="PWR" pin="VSS@7" pad="107"/>
<connect gate="PWR" pin="VSS@8" pad="120"/>
<connect gate="PWR" pin="VSS@9" pad="130"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F217V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
120 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD6_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0-WKUP" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="RFU" pad="99"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="49"/>
<connect gate="MCU" pin="VCAP2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="11"/>
<connect gate="PWR" pin="VDD@2" pad="19"/>
<connect gate="PWR" pin="VDD@3" pad="28"/>
<connect gate="PWR" pin="VDD@4" pad="50"/>
<connect gate="PWR" pin="VDD@5" pad="75"/>
<connect gate="PWR" pin="VDD@6" pad="100"/>
<connect gate="PWR" pin="VSS@1" pad="10"/>
<connect gate="PWR" pin="VSS@2" pad="27"/>
<connect gate="PWR" pin="VSS@3" pad="74"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F217Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
120 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD12_VSS9"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="RFU" pad="143"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="71"/>
<connect gate="MCU" pin="VCAP2" pad="106"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VSSA" pad="31"/>
<connect gate="PWR" pin="VDD@1" pad="17"/>
<connect gate="PWR" pin="VDD@10" pad="121"/>
<connect gate="PWR" pin="VDD@11" pad="131"/>
<connect gate="PWR" pin="VDD@12" pad="144"/>
<connect gate="PWR" pin="VDD@2" pad="30"/>
<connect gate="PWR" pin="VDD@3" pad="39"/>
<connect gate="PWR" pin="VDD@4" pad="52"/>
<connect gate="PWR" pin="VDD@5" pad="62"/>
<connect gate="PWR" pin="VDD@6" pad="72"/>
<connect gate="PWR" pin="VDD@7" pad="84"/>
<connect gate="PWR" pin="VDD@8" pad="95"/>
<connect gate="PWR" pin="VDD@9" pad="108"/>
<connect gate="PWR" pin="VSS@1" pad="16"/>
<connect gate="PWR" pin="VSS@2" pad="38"/>
<connect gate="PWR" pin="VSS@3" pad="51"/>
<connect gate="PWR" pin="VSS@4" pad="61"/>
<connect gate="PWR" pin="VSS@5" pad="83"/>
<connect gate="PWR" pin="VSS@6" pad="94"/>
<connect gate="PWR" pin="VSS@7" pad="107"/>
<connect gate="PWR" pin="VSS@8" pad="120"/>
<connect gate="PWR" pin="VSS@9" pad="130"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F217I*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
120 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD15_VSS12"/>
</gates>
<devices>
<device name="" package="LQFP176">
<connects>
<connect gate="MCU" pin="BOOT0" pad="166"/>
<connect gate="MCU" pin="NRST" pad="31"/>
<connect gate="MCU" pin="OSC_IN" pad="29"/>
<connect gate="MCU" pin="OSC_OUT" pad="30"/>
<connect gate="MCU" pin="PA0" pad="40"/>
<connect gate="MCU" pin="PA1" pad="41"/>
<connect gate="MCU" pin="PA10" pad="121"/>
<connect gate="MCU" pin="PA11" pad="122"/>
<connect gate="MCU" pin="PA12" pad="123"/>
<connect gate="MCU" pin="PA13" pad="124"/>
<connect gate="MCU" pin="PA14" pad="137"/>
<connect gate="MCU" pin="PA15" pad="138"/>
<connect gate="MCU" pin="PA2" pad="42"/>
<connect gate="MCU" pin="PA3" pad="47"/>
<connect gate="MCU" pin="PA4" pad="50"/>
<connect gate="MCU" pin="PA5" pad="51"/>
<connect gate="MCU" pin="PA6" pad="52"/>
<connect gate="MCU" pin="PA7" pad="53"/>
<connect gate="MCU" pin="PA8" pad="119"/>
<connect gate="MCU" pin="PA9" pad="120"/>
<connect gate="MCU" pin="PB0" pad="56"/>
<connect gate="MCU" pin="PB1" pad="57"/>
<connect gate="MCU" pin="PB10" pad="79"/>
<connect gate="MCU" pin="PB11" pad="80"/>
<connect gate="MCU" pin="PB12" pad="92"/>
<connect gate="MCU" pin="PB13" pad="93"/>
<connect gate="MCU" pin="PB14" pad="94"/>
<connect gate="MCU" pin="PB15" pad="95"/>
<connect gate="MCU" pin="PB2" pad="58"/>
<connect gate="MCU" pin="PB3" pad="161"/>
<connect gate="MCU" pin="PB4" pad="162"/>
<connect gate="MCU" pin="PB5" pad="163"/>
<connect gate="MCU" pin="PB6" pad="164"/>
<connect gate="MCU" pin="PB7" pad="165"/>
<connect gate="MCU" pin="PB8" pad="167"/>
<connect gate="MCU" pin="PB9" pad="168"/>
<connect gate="MCU" pin="PC0" pad="32"/>
<connect gate="MCU" pin="PC1" pad="33"/>
<connect gate="MCU" pin="PC10" pad="139"/>
<connect gate="MCU" pin="PC11" pad="140"/>
<connect gate="MCU" pin="PC12" pad="141"/>
<connect gate="MCU" pin="PC13" pad="8"/>
<connect gate="MCU" pin="PC14" pad="9"/>
<connect gate="MCU" pin="PC15" pad="10"/>
<connect gate="MCU" pin="PC2" pad="34"/>
<connect gate="MCU" pin="PC3" pad="35"/>
<connect gate="MCU" pin="PC4" pad="54"/>
<connect gate="MCU" pin="PC5" pad="55"/>
<connect gate="MCU" pin="PC6" pad="115"/>
<connect gate="MCU" pin="PC7" pad="116"/>
<connect gate="MCU" pin="PC8" pad="117"/>
<connect gate="MCU" pin="PC9" pad="118"/>
<connect gate="MCU" pin="PD0" pad="142"/>
<connect gate="MCU" pin="PD1" pad="143"/>
<connect gate="MCU" pin="PD10" pad="98"/>
<connect gate="MCU" pin="PD11" pad="99"/>
<connect gate="MCU" pin="PD12" pad="100"/>
<connect gate="MCU" pin="PD13" pad="101"/>
<connect gate="MCU" pin="PD14" pad="104"/>
<connect gate="MCU" pin="PD15" pad="105"/>
<connect gate="MCU" pin="PD2" pad="144"/>
<connect gate="MCU" pin="PD3" pad="145"/>
<connect gate="MCU" pin="PD4" pad="146"/>
<connect gate="MCU" pin="PD5" pad="147"/>
<connect gate="MCU" pin="PD6" pad="150"/>
<connect gate="MCU" pin="PD7" pad="151"/>
<connect gate="MCU" pin="PD8" pad="96"/>
<connect gate="MCU" pin="PD9" pad="97"/>
<connect gate="MCU" pin="PDR_ON" pad="171"/>
<connect gate="MCU" pin="PE0" pad="169"/>
<connect gate="MCU" pin="PE1" pad="170"/>
<connect gate="MCU" pin="PE10" pad="73"/>
<connect gate="MCU" pin="PE11" pad="74"/>
<connect gate="MCU" pin="PE12" pad="75"/>
<connect gate="MCU" pin="PE13" pad="76"/>
<connect gate="MCU" pin="PE14" pad="77"/>
<connect gate="MCU" pin="PE15" pad="78"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="68"/>
<connect gate="MCU" pin="PE8" pad="69"/>
<connect gate="MCU" pin="PE9" pad="70"/>
<connect gate="MCU" pin="PF0" pad="16"/>
<connect gate="MCU" pin="PF1" pad="17"/>
<connect gate="MCU" pin="PF10" pad="28"/>
<connect gate="MCU" pin="PF11" pad="59"/>
<connect gate="MCU" pin="PF12" pad="60"/>
<connect gate="MCU" pin="PF13" pad="63"/>
<connect gate="MCU" pin="PF14" pad="64"/>
<connect gate="MCU" pin="PF15" pad="65"/>
<connect gate="MCU" pin="PF2" pad="18"/>
<connect gate="MCU" pin="PF3" pad="19"/>
<connect gate="MCU" pin="PF4" pad="20"/>
<connect gate="MCU" pin="PF5" pad="21"/>
<connect gate="MCU" pin="PF6" pad="24"/>
<connect gate="MCU" pin="PF7" pad="25"/>
<connect gate="MCU" pin="PF8" pad="26"/>
<connect gate="MCU" pin="PF9" pad="27"/>
<connect gate="MCU" pin="PG0" pad="66"/>
<connect gate="MCU" pin="PG1" pad="67"/>
<connect gate="MCU" pin="PG10" pad="153"/>
<connect gate="MCU" pin="PG11" pad="154"/>
<connect gate="MCU" pin="PG12" pad="155"/>
<connect gate="MCU" pin="PG13" pad="156"/>
<connect gate="MCU" pin="PG14" pad="157"/>
<connect gate="MCU" pin="PG15" pad="160"/>
<connect gate="MCU" pin="PG2" pad="106"/>
<connect gate="MCU" pin="PG3" pad="107"/>
<connect gate="MCU" pin="PG4" pad="108"/>
<connect gate="MCU" pin="PG5" pad="109"/>
<connect gate="MCU" pin="PG6" pad="110"/>
<connect gate="MCU" pin="PG7" pad="111"/>
<connect gate="MCU" pin="PG8" pad="112"/>
<connect gate="MCU" pin="PG9" pad="152"/>
<connect gate="MCU" pin="PH10" pad="87"/>
<connect gate="MCU" pin="PH11" pad="88"/>
<connect gate="MCU" pin="PH12" pad="89"/>
<connect gate="MCU" pin="PH13" pad="128"/>
<connect gate="MCU" pin="PH14" pad="129"/>
<connect gate="MCU" pin="PH15" pad="130"/>
<connect gate="MCU" pin="PH2" pad="43"/>
<connect gate="MCU" pin="PH3" pad="44"/>
<connect gate="MCU" pin="PH4" pad="45"/>
<connect gate="MCU" pin="PH5" pad="46"/>
<connect gate="MCU" pin="PH6" pad="83"/>
<connect gate="MCU" pin="PH7" pad="84"/>
<connect gate="MCU" pin="PH8" pad="85"/>
<connect gate="MCU" pin="PH9" pad="86"/>
<connect gate="MCU" pin="PI0" pad="131"/>
<connect gate="MCU" pin="PI1" pad="132"/>
<connect gate="MCU" pin="PI10" pad="12"/>
<connect gate="MCU" pin="PI11" pad="13"/>
<connect gate="MCU" pin="PI2" pad="133"/>
<connect gate="MCU" pin="PI3" pad="134"/>
<connect gate="MCU" pin="PI4" pad="173"/>
<connect gate="MCU" pin="PI5" pad="174"/>
<connect gate="MCU" pin="PI6" pad="175"/>
<connect gate="MCU" pin="PI7" pad="176"/>
<connect gate="MCU" pin="PI8" pad="7"/>
<connect gate="MCU" pin="PI9" pad="11"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="81"/>
<connect gate="MCU" pin="VCAP2" pad="125"/>
<connect gate="MCU" pin="VDDA" pad="39"/>
<connect gate="MCU" pin="VREF+" pad="38"/>
<connect gate="MCU" pin="VSSA" pad="37"/>
<connect gate="PWR" pin="VDD@1" pad="15"/>
<connect gate="PWR" pin="VDD@10" pad="114"/>
<connect gate="PWR" pin="VDD@11" pad="127"/>
<connect gate="PWR" pin="VDD@12" pad="136"/>
<connect gate="PWR" pin="VDD@13" pad="149"/>
<connect gate="PWR" pin="VDD@14" pad="159"/>
<connect gate="PWR" pin="VDD@15" pad="172"/>
<connect gate="PWR" pin="VDD@2" pad="23"/>
<connect gate="PWR" pin="VDD@3" pad="36"/>
<connect gate="PWR" pin="VDD@4" pad="49"/>
<connect gate="PWR" pin="VDD@5" pad="62"/>
<connect gate="PWR" pin="VDD@6" pad="72"/>
<connect gate="PWR" pin="VDD@7" pad="82"/>
<connect gate="PWR" pin="VDD@8" pad="91"/>
<connect gate="PWR" pin="VDD@9" pad="103"/>
<connect gate="PWR" pin="VSS@1" pad="14"/>
<connect gate="PWR" pin="VSS@10" pad="135"/>
<connect gate="PWR" pin="VSS@11" pad="148"/>
<connect gate="PWR" pin="VSS@12" pad="158"/>
<connect gate="PWR" pin="VSS@2" pad="22"/>
<connect gate="PWR" pin="VSS@3" pad="48"/>
<connect gate="PWR" pin="VSS@4" pad="61"/>
<connect gate="PWR" pin="VSS@5" pad="71"/>
<connect gate="PWR" pin="VSS@6" pad="90"/>
<connect gate="PWR" pin="VSS@7" pad="102"/>
<connect gate="PWR" pin="VSS@8" pad="113"/>
<connect gate="PWR" pin="VSS@9" pad="126"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F217I*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
120 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD14_VSS36"/>
</gates>
<devices>
<device name="" package="UFBGA176+25">
<connects>
<connect gate="MCU" pin="BOOT0" pad="D6"/>
<connect gate="MCU" pin="NRST" pad="J1"/>
<connect gate="MCU" pin="OSC_IN" pad="G1"/>
<connect gate="MCU" pin="OSC_OUT" pad="H1"/>
<connect gate="MCU" pin="PA0" pad="N3"/>
<connect gate="MCU" pin="PA1" pad="N2"/>
<connect gate="MCU" pin="PA10" pad="D15"/>
<connect gate="MCU" pin="PA11" pad="C15"/>
<connect gate="MCU" pin="PA12" pad="B15"/>
<connect gate="MCU" pin="PA13" pad="A15"/>
<connect gate="MCU" pin="PA14" pad="A14"/>
<connect gate="MCU" pin="PA15" pad="A13"/>
<connect gate="MCU" pin="PA2" pad="P2"/>
<connect gate="MCU" pin="PA3" pad="R2"/>
<connect gate="MCU" pin="PA4" pad="N4"/>
<connect gate="MCU" pin="PA5" pad="P4"/>
<connect gate="MCU" pin="PA6" pad="P3"/>
<connect gate="MCU" pin="PA7" pad="R3"/>
<connect gate="MCU" pin="PA8" pad="F15"/>
<connect gate="MCU" pin="PA9" pad="E15"/>
<connect gate="MCU" pin="PB0" pad="R5"/>
<connect gate="MCU" pin="PB1" pad="R4"/>
<connect gate="MCU" pin="PB10" pad="R12"/>
<connect gate="MCU" pin="PB11" pad="R13"/>
<connect gate="MCU" pin="PB12" pad="P12"/>
<connect gate="MCU" pin="PB13" pad="P13"/>
<connect gate="MCU" pin="PB14" pad="R14"/>
<connect gate="MCU" pin="PB15" pad="R15"/>
<connect gate="MCU" pin="PB2" pad="M6"/>
<connect gate="MCU" pin="PB3" pad="A10"/>
<connect gate="MCU" pin="PB4" pad="A9"/>
<connect gate="MCU" pin="PB5" pad="A6"/>
<connect gate="MCU" pin="PB6" pad="B6"/>
<connect gate="MCU" pin="PB7" pad="B5"/>
<connect gate="MCU" pin="PB8" pad="A5"/>
<connect gate="MCU" pin="PB9" pad="B4"/>
<connect gate="MCU" pin="PC0" pad="M2"/>
<connect gate="MCU" pin="PC1" pad="M3"/>
<connect gate="MCU" pin="PC10" pad="B14"/>
<connect gate="MCU" pin="PC11" pad="B13"/>
<connect gate="MCU" pin="PC12" pad="A12"/>
<connect gate="MCU" pin="PC13" pad="D1"/>
<connect gate="MCU" pin="PC14" pad="E1"/>
<connect gate="MCU" pin="PC15" pad="F1"/>
<connect gate="MCU" pin="PC2" pad="M4"/>
<connect gate="MCU" pin="PC3" pad="M5"/>
<connect gate="MCU" pin="PC4" pad="N5"/>
<connect gate="MCU" pin="PC5" pad="P5"/>
<connect gate="MCU" pin="PC6" pad="H15"/>
<connect gate="MCU" pin="PC7" pad="G15"/>
<connect gate="MCU" pin="PC8" pad="G14"/>
<connect gate="MCU" pin="PC9" pad="F14"/>
<connect gate="MCU" pin="PD0" pad="B12"/>
<connect gate="MCU" pin="PD1" pad="C12"/>
<connect gate="MCU" pin="PD10" pad="N15"/>
<connect gate="MCU" pin="PD11" pad="N14"/>
<connect gate="MCU" pin="PD12" pad="N13"/>
<connect gate="MCU" pin="PD13" pad="M15"/>
<connect gate="MCU" pin="PD14" pad="M14"/>
<connect gate="MCU" pin="PD15" pad="L14"/>
<connect gate="MCU" pin="PD2" pad="D12"/>
<connect gate="MCU" pin="PD3" pad="D11"/>
<connect gate="MCU" pin="PD4" pad="D10"/>
<connect gate="MCU" pin="PD5" pad="C11"/>
<connect gate="MCU" pin="PD6" pad="B11"/>
<connect gate="MCU" pin="PD7" pad="A11"/>
<connect gate="MCU" pin="PD8" pad="P15"/>
<connect gate="MCU" pin="PD9" pad="P14"/>
<connect gate="MCU" pin="PE0" pad="A4"/>
<connect gate="MCU" pin="PE1" pad="A3"/>
<connect gate="MCU" pin="PE10" pad="R9"/>
<connect gate="MCU" pin="PE11" pad="P10"/>
<connect gate="MCU" pin="PE12" pad="R10"/>
<connect gate="MCU" pin="PE13" pad="N11"/>
<connect gate="MCU" pin="PE14" pad="P11"/>
<connect gate="MCU" pin="PE15" pad="R11"/>
<connect gate="MCU" pin="PE2" pad="A2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="B2"/>
<connect gate="MCU" pin="PE6" pad="B3"/>
<connect gate="MCU" pin="PE7" pad="R8"/>
<connect gate="MCU" pin="PE8" pad="P8"/>
<connect gate="MCU" pin="PE9" pad="P9"/>
<connect gate="MCU" pin="PF0" pad="E2"/>
<connect gate="MCU" pin="PF1" pad="H3"/>
<connect gate="MCU" pin="PF10" pad="L1"/>
<connect gate="MCU" pin="PF11" pad="R6"/>
<connect gate="MCU" pin="PF12" pad="P6"/>
<connect gate="MCU" pin="PF13" pad="N6"/>
<connect gate="MCU" pin="PF14" pad="R7"/>
<connect gate="MCU" pin="PF15" pad="P7"/>
<connect gate="MCU" pin="PF2" pad="H2"/>
<connect gate="MCU" pin="PF3" pad="J2"/>
<connect gate="MCU" pin="PF4" pad="J3"/>
<connect gate="MCU" pin="PF5" pad="K3"/>
<connect gate="MCU" pin="PF6" pad="K2"/>
<connect gate="MCU" pin="PF7" pad="K1"/>
<connect gate="MCU" pin="PF8" pad="L3"/>
<connect gate="MCU" pin="PF9" pad="L2"/>
<connect gate="MCU" pin="PG0" pad="N7"/>
<connect gate="MCU" pin="PG1" pad="M7"/>
<connect gate="MCU" pin="PG10" pad="B10"/>
<connect gate="MCU" pin="PG11" pad="B9"/>
<connect gate="MCU" pin="PG12" pad="B8"/>
<connect gate="MCU" pin="PG13" pad="A8"/>
<connect gate="MCU" pin="PG14" pad="A7"/>
<connect gate="MCU" pin="PG15" pad="B7"/>
<connect gate="MCU" pin="PG2" pad="L15"/>
<connect gate="MCU" pin="PG3" pad="K15"/>
<connect gate="MCU" pin="PG4" pad="K14"/>
<connect gate="MCU" pin="PG5" pad="K13"/>
<connect gate="MCU" pin="PG6" pad="J15"/>
<connect gate="MCU" pin="PG7" pad="J14"/>
<connect gate="MCU" pin="PG8" pad="H14"/>
<connect gate="MCU" pin="PG9" pad="C10"/>
<connect gate="MCU" pin="PH10" pad="L13"/>
<connect gate="MCU" pin="PH11" pad="L12"/>
<connect gate="MCU" pin="PH12" pad="K12"/>
<connect gate="MCU" pin="PH13" pad="E12"/>
<connect gate="MCU" pin="PH14" pad="E13"/>
<connect gate="MCU" pin="PH15" pad="D13"/>
<connect gate="MCU" pin="PH2" pad="F4"/>
<connect gate="MCU" pin="PH3" pad="G4"/>
<connect gate="MCU" pin="PH4" pad="H4"/>
<connect gate="MCU" pin="PH5" pad="J4"/>
<connect gate="MCU" pin="PH6" pad="M11"/>
<connect gate="MCU" pin="PH7" pad="N12"/>
<connect gate="MCU" pin="PH8" pad="M12"/>
<connect gate="MCU" pin="PH9" pad="M13"/>
<connect gate="MCU" pin="PI0" pad="E14"/>
<connect gate="MCU" pin="PI1" pad="D14"/>
<connect gate="MCU" pin="PI10" pad="E3"/>
<connect gate="MCU" pin="PI11" pad="E4"/>
<connect gate="MCU" pin="PI2" pad="C14"/>
<connect gate="MCU" pin="PI3" pad="C13"/>
<connect gate="MCU" pin="PI4" pad="D4"/>
<connect gate="MCU" pin="PI5" pad="C4"/>
<connect gate="MCU" pin="PI6" pad="C3"/>
<connect gate="MCU" pin="PI7" pad="C2"/>
<connect gate="MCU" pin="PI8" pad="D2"/>
<connect gate="MCU" pin="PI9" pad="D3"/>
<connect gate="MCU" pin="REGOFF" pad="L4"/>
<connect gate="MCU" pin="RFU" pad="C6"/>
<connect gate="MCU" pin="VBAT" pad="C1"/>
<connect gate="MCU" pin="VCAP1" pad="M10"/>
<connect gate="MCU" pin="VCAP2" pad="F13"/>
<connect gate="MCU" pin="VDDA" pad="R1"/>
<connect gate="MCU" pin="VREF+" pad="P1"/>
<connect gate="MCU" pin="VREF-" pad="N1"/>
<connect gate="MCU" pin="VSSA" pad="M1"/>
<connect gate="PWR" pin="VDD@1" pad="C5"/>
<connect gate="PWR" pin="VDD@10" pad="J13"/>
<connect gate="PWR" pin="VDD@11" pad="K4"/>
<connect gate="PWR" pin="VDD@12" pad="N8"/>
<connect gate="PWR" pin="VDD@13" pad="N9"/>
<connect gate="PWR" pin="VDD@14" pad="N10"/>
<connect gate="PWR" pin="VDD@2" pad="C7"/>
<connect gate="PWR" pin="VDD@3" pad="C8"/>
<connect gate="PWR" pin="VDD@4" pad="C9"/>
<connect gate="PWR" pin="VDD@5" pad="F3"/>
<connect gate="PWR" pin="VDD@6" pad="G3"/>
<connect gate="PWR" pin="VDD@7" pad="G13"/>
<connect gate="PWR" pin="VDD@8" pad="H13"/>
<connect gate="PWR" pin="VDD@9" pad="J12"/>
<connect gate="PWR" pin="VSS@1" pad="D5"/>
<connect gate="PWR" pin="VSS@10" pad="M8"/>
<connect gate="PWR" pin="VSS@11" pad="M9"/>
<connect gate="PWR" pin="VSS@12" pad="VSS_1"/>
<connect gate="PWR" pin="VSS@13" pad="VSS_2"/>
<connect gate="PWR" pin="VSS@14" pad="VSS_3"/>
<connect gate="PWR" pin="VSS@15" pad="VSS_4"/>
<connect gate="PWR" pin="VSS@16" pad="VSS_5"/>
<connect gate="PWR" pin="VSS@17" pad="VSS_6"/>
<connect gate="PWR" pin="VSS@18" pad="VSS_7"/>
<connect gate="PWR" pin="VSS@19" pad="VSS_8"/>
<connect gate="PWR" pin="VSS@2" pad="D7"/>
<connect gate="PWR" pin="VSS@20" pad="VSS_9"/>
<connect gate="PWR" pin="VSS@21" pad="VSS_10"/>
<connect gate="PWR" pin="VSS@22" pad="VSS_11"/>
<connect gate="PWR" pin="VSS@23" pad="VSS_12"/>
<connect gate="PWR" pin="VSS@24" pad="VSS_13"/>
<connect gate="PWR" pin="VSS@25" pad="VSS_14"/>
<connect gate="PWR" pin="VSS@26" pad="VSS_15"/>
<connect gate="PWR" pin="VSS@27" pad="VSS_16"/>
<connect gate="PWR" pin="VSS@28" pad="VSS_17"/>
<connect gate="PWR" pin="VSS@29" pad="VSS_18"/>
<connect gate="PWR" pin="VSS@3" pad="D8"/>
<connect gate="PWR" pin="VSS@30" pad="VSS_19"/>
<connect gate="PWR" pin="VSS@31" pad="VSS_20"/>
<connect gate="PWR" pin="VSS@32" pad="VSS_21"/>
<connect gate="PWR" pin="VSS@33" pad="VSS_22"/>
<connect gate="PWR" pin="VSS@34" pad="VSS_23"/>
<connect gate="PWR" pin="VSS@35" pad="VSS_24"/>
<connect gate="PWR" pin="VSS@36" pad="VSS_25"/>
<connect gate="PWR" pin="VSS@4" pad="D9"/>
<connect gate="PWR" pin="VSS@5" pad="F2"/>
<connect gate="PWR" pin="VSS@6" pad="F12"/>
<connect gate="PWR" pin="VSS@7" pad="G2"/>
<connect gate="PWR" pin="VSS@8" pad="G12"/>
<connect gate="PWR" pin="VSS@9" pad="H12"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F302C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
24 to 32 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD3_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="48"/>
<connect gate="PWR" pin="VDD@2" pad="24"/>
<connect gate="PWR" pin="VDD@3" pad="36"/>
<connect gate="PWR" pin="VSS@1" pad="47"/>
<connect gate="PWR" pin="VSS@2" pad="23"/>
<connect gate="PWR" pin="VSS@3" pad="35"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F302R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
24 to 32 kbytes of SRAM&lt;br&gt;
52 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="PWR" symbol="PWR_VDD4_VSS3"/>
<gate name="MCU" symbol="STM32_64PIN_TYP13"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="PF4" pad="18"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="64"/>
<connect gate="PWR" pin="VDD@2" pad="32"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="63"/>
<connect gate="PWR" pin="VSS@2" pad="31"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F302V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
24 to 32 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD4_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0-WKUP" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="PF10" pad="11"/>
<connect gate="MCU" pin="PF2" pad="19"/>
<connect gate="MCU" pin="PF4" pad="27"/>
<connect gate="MCU" pin="PF6" pad="73"/>
<connect gate="MCU" pin="PF9" pad="10"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="100"/>
<connect gate="PWR" pin="VDD@2" pad="50"/>
<connect gate="PWR" pin="VDD@3" pad="75"/>
<connect gate="PWR" pin="VDD@4" pad="28"/>
<connect gate="PWR" pin="VSS@1" pad="99"/>
<connect gate="PWR" pin="VSS@2" pad="49"/>
<connect gate="PWR" pin="VSS@3" pad="74"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F303C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
32 to 40 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD3_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="48"/>
<connect gate="PWR" pin="VDD@2" pad="24"/>
<connect gate="PWR" pin="VDD@3" pad="36"/>
<connect gate="PWR" pin="VSS@1" pad="47"/>
<connect gate="PWR" pin="VSS@2" pad="23"/>
<connect gate="PWR" pin="VSS@3" pad="35"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F303R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
32 to 40 kbytes of SRAM&lt;br&gt;
52 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP13"/>
<gate name="PWR" symbol="PWR_VDD4_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="PF4" pad="18"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="64"/>
<connect gate="PWR" pin="VDD@2" pad="32"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="63"/>
<connect gate="PWR" pin="VSS@2" pad="31"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F303V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
32 to 40 kbytes of SRAM&lt;br&gt;
87 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD4_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0-WKUP" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="PF10" pad="11"/>
<connect gate="MCU" pin="PF2" pad="19"/>
<connect gate="MCU" pin="PF4" pad="27"/>
<connect gate="MCU" pin="PF6" pad="73"/>
<connect gate="MCU" pin="PF9" pad="10"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="100"/>
<connect gate="PWR" pin="VDD@2" pad="50"/>
<connect gate="PWR" pin="VDD@3" pad="75"/>
<connect gate="PWR" pin="VDD@4" pad="28"/>
<connect gate="PWR" pin="VSS@1" pad="99"/>
<connect gate="PWR" pin="VSS@2" pad="49"/>
<connect gate="PWR" pin="VSS@3" pad="74"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F313C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
32 to 40 kbytes of SRAM&lt;br&gt;
36 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD3_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NPOR" pad="20"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="48"/>
<connect gate="PWR" pin="VDD@2" pad="24"/>
<connect gate="PWR" pin="VDD@3" pad="36"/>
<connect gate="PWR" pin="VSS@1" pad="47"/>
<connect gate="PWR" pin="VSS@2" pad="23"/>
<connect gate="PWR" pin="VSS@3" pad="35"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F313R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
32 to 40 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP7"/>
<gate name="PWR" symbol="PWR_VDD4_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NPOR" pad="28"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="PF4" pad="18"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="64"/>
<connect gate="PWR" pin="VDD@2" pad="32"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="63"/>
<connect gate="PWR" pin="VSS@2" pad="31"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F313V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
32 to 40 kbytes of SRAM&lt;br&gt;
86 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD4_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NPOR" pad="37"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0-WKUP" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="PF10" pad="11"/>
<connect gate="MCU" pin="PF2" pad="19"/>
<connect gate="MCU" pin="PF4" pad="27"/>
<connect gate="MCU" pin="PF6" pad="73"/>
<connect gate="MCU" pin="PF9" pad="10"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="100"/>
<connect gate="PWR" pin="VDD@2" pad="50"/>
<connect gate="PWR" pin="VDD@3" pad="75"/>
<connect gate="PWR" pin="VDD@4" pad="28"/>
<connect gate="PWR" pin="VSS@1" pad="99"/>
<connect gate="PWR" pin="VSS@2" pad="49"/>
<connect gate="PWR" pin="VSS@3" pad="74"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F373C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
64 to 256 Kbytes of Flash memory&lt;br&gt;
16 to 32 kbytes of SRAM&lt;br&gt;
36 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP5"/>
<gate name="PWR" symbol="PWR_VDD2_VSS1"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB14" pad="26"/>
<connect gate="MCU" pin="PB15" pad="27"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PD8" pad="28"/>
<connect gate="MCU" pin="PE8" pad="21"/>
<connect gate="MCU" pin="PE9" pad="22"/>
<connect gate="MCU" pin="PF6" pad="35"/>
<connect gate="MCU" pin="PF7" pad="36"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VDDSD" pad="24"/>
<connect gate="MCU" pin="VREFSD+" pad="25"/>
<connect gate="MCU" pin="VREFSD-" pad="23"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="48"/>
<connect gate="PWR" pin="VDD@2" pad="17"/>
<connect gate="PWR" pin="VSS@1" pad="47"/>
</connects>
<technologies>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F373R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
64 to 256 Kbytes of Flash memory&lt;br&gt;
16 to 32 kbytes of SRAM&lt;br&gt;
52 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP8"/>
<gate name="PWR" symbol="PWR_VDD2_VSS1"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="18"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB14" pad="34"/>
<connect gate="MCU" pin="PB15" pad="35"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="PD8" pad="36"/>
<connect gate="MCU" pin="PE8" pad="29"/>
<connect gate="MCU" pin="PE9" pad="30"/>
<connect gate="MCU" pin="PF6" pad="47"/>
<connect gate="MCU" pin="PF7" pad="48"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VDDSD" pad="32"/>
<connect gate="MCU" pin="VREF+" pad="17"/>
<connect gate="MCU" pin="VREFSD+" pad="33"/>
<connect gate="MCU" pin="VREFSD-" pad="31"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="64"/>
<connect gate="PWR" pin="VDD@2" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="63"/>
</connects>
<technologies>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F373V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
64 to 256 Kbytes of Flash memory&lt;br&gt;
16 to 32 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP5"/>
<gate name="PWR" symbol="PWR_VDD3_VSS2"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="PF10" pad="11"/>
<connect gate="MCU" pin="PF2" pad="19"/>
<connect gate="MCU" pin="PF4" pad="27"/>
<connect gate="MCU" pin="PF6" pad="73"/>
<connect gate="MCU" pin="PF9" pad="10"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="21"/>
<connect gate="MCU" pin="VDDSD12" pad="50"/>
<connect gate="MCU" pin="VDDSD3" pad="51"/>
<connect gate="MCU" pin="VREF+" pad="22"/>
<connect gate="MCU" pin="VREFSD+" pad="52"/>
<connect gate="MCU" pin="VREFSD-" pad="48"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="MCU" pin="VSSSD" pad="49"/>
<connect gate="PWR" pin="VDD@1" pad="100"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="28"/>
<connect gate="PWR" pin="VSS@1" pad="99"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
</connects>
<technologies>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F373V*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
256 Kbytes of Flash memory&lt;br&gt;
32 kbytes of SRAM&lt;br&gt;
84 GPIOs&lt;br&gt;
2.0 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP5"/>
<gate name="PWR" symbol="PWR_VDD3_VSS2"/>
</gates>
<devices>
<device name="" package="UFBGA100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A4"/>
<connect gate="MCU" pin="NRST" pad="H2"/>
<connect gate="MCU" pin="OSC_IN" pad="F1"/>
<connect gate="MCU" pin="OSC_OUT" pad="G1"/>
<connect gate="MCU" pin="PA0" pad="L2"/>
<connect gate="MCU" pin="PA1" pad="M2"/>
<connect gate="MCU" pin="PA10" pad="C12"/>
<connect gate="MCU" pin="PA11" pad="B12"/>
<connect gate="MCU" pin="PA12" pad="A12"/>
<connect gate="MCU" pin="PA13" pad="A11"/>
<connect gate="MCU" pin="PA14" pad="A10"/>
<connect gate="MCU" pin="PA15" pad="A9"/>
<connect gate="MCU" pin="PA2" pad="K3"/>
<connect gate="MCU" pin="PA3" pad="L3"/>
<connect gate="MCU" pin="PA4" pad="M3"/>
<connect gate="MCU" pin="PA5" pad="K4"/>
<connect gate="MCU" pin="PA6" pad="L4"/>
<connect gate="MCU" pin="PA7" pad="M4"/>
<connect gate="MCU" pin="PA8" pad="D11"/>
<connect gate="MCU" pin="PA9" pad="D10"/>
<connect gate="MCU" pin="PB0" pad="M5"/>
<connect gate="MCU" pin="PB1" pad="M6"/>
<connect gate="MCU" pin="PB10" pad="L10"/>
<connect gate="MCU" pin="PB14" pad="K11"/>
<connect gate="MCU" pin="PB15" pad="K10"/>
<connect gate="MCU" pin="PB2" pad="L6"/>
<connect gate="MCU" pin="PB3" pad="A8"/>
<connect gate="MCU" pin="PB4" pad="A7"/>
<connect gate="MCU" pin="PB5" pad="C5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="B4"/>
<connect gate="MCU" pin="PB8" pad="A3"/>
<connect gate="MCU" pin="PB9" pad="B3"/>
<connect gate="MCU" pin="PC0" pad="H1"/>
<connect gate="MCU" pin="PC1" pad="J2"/>
<connect gate="MCU" pin="PC10" pad="B11"/>
<connect gate="MCU" pin="PC11" pad="C10"/>
<connect gate="MCU" pin="PC12" pad="B10"/>
<connect gate="MCU" pin="PC13" pad="C1"/>
<connect gate="MCU" pin="PC14" pad="D1"/>
<connect gate="MCU" pin="PC15" pad="E1"/>
<connect gate="MCU" pin="PC2" pad="J3"/>
<connect gate="MCU" pin="PC3" pad="K2"/>
<connect gate="MCU" pin="PC4" pad="K5"/>
<connect gate="MCU" pin="PC5" pad="L5"/>
<connect gate="MCU" pin="PC6" pad="E12"/>
<connect gate="MCU" pin="PC7" pad="E11"/>
<connect gate="MCU" pin="PC8" pad="E10"/>
<connect gate="MCU" pin="PC9" pad="D12"/>
<connect gate="MCU" pin="PD0" pad="C9"/>
<connect gate="MCU" pin="PD1" pad="B9"/>
<connect gate="MCU" pin="PD10" pad="J12"/>
<connect gate="MCU" pin="PD11" pad="J11"/>
<connect gate="MCU" pin="PD12" pad="J10"/>
<connect gate="MCU" pin="PD13" pad="H12"/>
<connect gate="MCU" pin="PD14" pad="H11"/>
<connect gate="MCU" pin="PD15" pad="H10"/>
<connect gate="MCU" pin="PD2" pad="C8"/>
<connect gate="MCU" pin="PD3" pad="B8"/>
<connect gate="MCU" pin="PD4" pad="B7"/>
<connect gate="MCU" pin="PD5" pad="A6"/>
<connect gate="MCU" pin="PD6" pad="B6"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD8" pad="K9"/>
<connect gate="MCU" pin="PD9" pad="K8"/>
<connect gate="MCU" pin="PE0" pad="C3"/>
<connect gate="MCU" pin="PE1" pad="A2"/>
<connect gate="MCU" pin="PE10" pad="L8"/>
<connect gate="MCU" pin="PE11" pad="M9"/>
<connect gate="MCU" pin="PE12" pad="L9"/>
<connect gate="MCU" pin="PE13" pad="M10"/>
<connect gate="MCU" pin="PE14" pad="M11"/>
<connect gate="MCU" pin="PE15" pad="M12"/>
<connect gate="MCU" pin="PE2" pad="B2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="C2"/>
<connect gate="MCU" pin="PE6" pad="D2"/>
<connect gate="MCU" pin="PE7" pad="M7"/>
<connect gate="MCU" pin="PE8" pad="L7"/>
<connect gate="MCU" pin="PE9" pad="M8"/>
<connect gate="MCU" pin="PF10" pad="G2"/>
<connect gate="MCU" pin="PF2" pad="J1"/>
<connect gate="MCU" pin="PF4" pad="E3"/>
<connect gate="MCU" pin="PF6" pad="C11"/>
<connect gate="MCU" pin="PF9" pad="F2"/>
<connect gate="MCU" pin="VBAT" pad="E2"/>
<connect gate="MCU" pin="VDDA" pad="M1"/>
<connect gate="MCU" pin="VDDSD12" pad="G12"/>
<connect gate="MCU" pin="VDDSD3" pad="L12"/>
<connect gate="MCU" pin="VREF+" pad="L1"/>
<connect gate="MCU" pin="VREFSD+" pad="K12"/>
<connect gate="MCU" pin="VREFSD-" pad="L11"/>
<connect gate="MCU" pin="VSSA" pad="K1"/>
<connect gate="MCU" pin="VSSSD" pad="F12"/>
<connect gate="PWR" pin="VDD@1" pad="C4"/>
<connect gate="PWR" pin="VDD@2" pad="H3"/>
<connect gate="PWR" pin="VDD@3" pad="G11"/>
<connect gate="PWR" pin="VSS@1" pad="D3"/>
<connect gate="PWR" pin="VSS@2" pad="F11"/>
</connects>
<technologies>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F383C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
64 to 256 Kbytes of Flash memory&lt;br&gt;
16 to 32 kbytes of SRAM&lt;br&gt;
36 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP6"/>
<gate name="PWR" symbol="PWR_VDD2_VSS1"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NPOR" pad="20"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB14" pad="26"/>
<connect gate="MCU" pin="PB15" pad="27"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PD8" pad="28"/>
<connect gate="MCU" pin="PE8" pad="21"/>
<connect gate="MCU" pin="PE9" pad="22"/>
<connect gate="MCU" pin="PF6" pad="35"/>
<connect gate="MCU" pin="PF7" pad="36"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VDDSD" pad="24"/>
<connect gate="MCU" pin="VREFSD+" pad="25"/>
<connect gate="MCU" pin="VREFSD-" pad="23"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="48"/>
<connect gate="PWR" pin="VDD@2" pad="17"/>
<connect gate="PWR" pin="VSS@1" pad="47"/>
</connects>
<technologies>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F383R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
64 to 256 Kbytes of Flash memory&lt;br&gt;
16 to 32 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP9"/>
<gate name="PWR" symbol="PWR_VDD2_VSS1"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NPOR" pad="28"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="18"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB14" pad="34"/>
<connect gate="MCU" pin="PB15" pad="35"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="PD8" pad="36"/>
<connect gate="MCU" pin="PE8" pad="29"/>
<connect gate="MCU" pin="PE9" pad="30"/>
<connect gate="MCU" pin="PF6" pad="47"/>
<connect gate="MCU" pin="PF7" pad="48"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VDDSD" pad="32"/>
<connect gate="MCU" pin="VREF+" pad="17"/>
<connect gate="MCU" pin="VREFSD+" pad="33"/>
<connect gate="MCU" pin="VREFSD-" pad="31"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="64"/>
<connect gate="PWR" pin="VDD@2" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="63"/>
</connects>
<technologies>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F383R*Y" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
64 to 256 Kbytes of Flash memory&lt;br&gt;
16 to 32 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_66PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD2_VSS3"/>
</gates>
<devices>
<device name="" package="WLCSP66">
<connects>
<connect gate="MCU" pin="BOOT0" pad="C7"/>
<connect gate="MCU" pin="NPOR" pad="G2"/>
<connect gate="MCU" pin="NRST" pad="E7"/>
<connect gate="MCU" pin="OSC_IN" pad="D7"/>
<connect gate="MCU" pin="OSC_OUT" pad="E8"/>
<connect gate="MCU" pin="PA0-WKUP" pad="H8"/>
<connect gate="MCU" pin="PA1" pad="H7"/>
<connect gate="MCU" pin="PA10" pad="C2"/>
<connect gate="MCU" pin="PA11" pad="C1"/>
<connect gate="MCU" pin="PA12" pad="C3"/>
<connect gate="MCU" pin="PA13" pad="C4"/>
<connect gate="MCU" pin="PA14" pad="A1"/>
<connect gate="MCU" pin="PA15" pad="A2"/>
<connect gate="MCU" pin="PA2" pad="J8"/>
<connect gate="MCU" pin="PA3" pad="H6"/>
<connect gate="MCU" pin="PA4" pad="J6"/>
<connect gate="MCU" pin="PA5" pad="H5"/>
<connect gate="MCU" pin="PA6" pad="J5"/>
<connect gate="MCU" pin="PA7" pad="G3"/>
<connect gate="MCU" pin="PA8" pad="D1"/>
<connect gate="MCU" pin="PA9" pad="D3"/>
<connect gate="MCU" pin="PB0" pad="H3"/>
<connect gate="MCU" pin="PB1" pad="J3"/>
<connect gate="MCU" pin="PB14" pad="F2"/>
<connect gate="MCU" pin="PB15" pad="F1"/>
<connect gate="MCU" pin="PB3" pad="C5"/>
<connect gate="MCU" pin="PB4" pad="B5"/>
<connect gate="MCU" pin="PB5" pad="A5"/>
<connect gate="MCU" pin="PB6" pad="B6"/>
<connect gate="MCU" pin="PB7" pad="A6"/>
<connect gate="MCU" pin="PB8" pad="B7"/>
<connect gate="MCU" pin="PB9" pad="A7"/>
<connect gate="MCU" pin="PC0" pad="E6"/>
<connect gate="MCU" pin="PC1" pad="F8"/>
<connect gate="MCU" pin="PC10" pad="B3"/>
<connect gate="MCU" pin="PC11" pad="A3"/>
<connect gate="MCU" pin="PC12" pad="B4"/>
<connect gate="MCU" pin="PC13" pad="B8"/>
<connect gate="MCU" pin="PC14" pad="C8"/>
<connect gate="MCU" pin="PC15" pad="D8"/>
<connect gate="MCU" pin="PC2" pad="F7"/>
<connect gate="MCU" pin="PC3" pad="F6"/>
<connect gate="MCU" pin="PC4" pad="H4"/>
<connect gate="MCU" pin="PC5" pad="J4"/>
<connect gate="MCU" pin="PC6" pad="E2"/>
<connect gate="MCU" pin="PC7" pad="E1"/>
<connect gate="MCU" pin="PC8" pad="E3"/>
<connect gate="MCU" pin="PC9" pad="D2"/>
<connect gate="MCU" pin="PD2" pad="A4"/>
<connect gate="MCU" pin="PD8" pad="F3"/>
<connect gate="MCU" pin="PE8" pad="H2"/>
<connect gate="MCU" pin="PE9" pad="J2"/>
<connect gate="MCU" pin="PF6" pad="B2"/>
<connect gate="MCU" pin="PF7" pad="B1"/>
<connect gate="MCU" pin="VBAT" pad="A8"/>
<connect gate="MCU" pin="VDDA" pad="G7"/>
<connect gate="MCU" pin="VDDSD" pad="H1"/>
<connect gate="MCU" pin="VREF+" pad="G6"/>
<connect gate="MCU" pin="VREFSD+" pad="G1"/>
<connect gate="MCU" pin="VREFSD-" pad="J1"/>
<connect gate="MCU" pin="VSSA" pad="G8"/>
<connect gate="PWR" pin="VDD@1" pad="D6"/>
<connect gate="PWR" pin="VDD@2" pad="J7"/>
<connect gate="PWR" pin="VSS@1" pad="C6"/>
<connect gate="PWR" pin="VSS@2" pad="G4"/>
<connect gate="PWR" pin="VSS@3" pad="G5"/>
</connects>
<technologies>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F383V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
64 to 256 Kbytes of Flash memory&lt;br&gt;
16 to 32 kbytes of SRAM&lt;br&gt;
81 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP6"/>
<gate name="PWR" symbol="PWR_VDD3_VSS2"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NPOR" pad="37"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="PF10" pad="11"/>
<connect gate="MCU" pin="PF2" pad="19"/>
<connect gate="MCU" pin="PF4" pad="27"/>
<connect gate="MCU" pin="PF6" pad="73"/>
<connect gate="MCU" pin="PF9" pad="10"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="21"/>
<connect gate="MCU" pin="VDDSD12" pad="50"/>
<connect gate="MCU" pin="VDDSD3" pad="51"/>
<connect gate="MCU" pin="VREF+" pad="22"/>
<connect gate="MCU" pin="VREFSD+" pad="52"/>
<connect gate="MCU" pin="VREFSD-" pad="48"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="MCU" pin="VSSSD" pad="49"/>
<connect gate="PWR" pin="VDD@1" pad="100"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="28"/>
<connect gate="PWR" pin="VSS@1" pad="99"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
</connects>
<technologies>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F383V*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
256 Kbytes of Flash memory&lt;br&gt;
32 kbytes of SRAM&lt;br&gt;
81 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP6"/>
<gate name="PWR" symbol="PWR_VDD3_VSS2"/>
</gates>
<devices>
<device name="" package="UFBGA100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A4"/>
<connect gate="MCU" pin="NPOR" pad="L6"/>
<connect gate="MCU" pin="NRST" pad="H2"/>
<connect gate="MCU" pin="OSC_IN" pad="F1"/>
<connect gate="MCU" pin="OSC_OUT" pad="G1"/>
<connect gate="MCU" pin="PA0" pad="L2"/>
<connect gate="MCU" pin="PA1" pad="M2"/>
<connect gate="MCU" pin="PA10" pad="C12"/>
<connect gate="MCU" pin="PA11" pad="B12"/>
<connect gate="MCU" pin="PA12" pad="A12"/>
<connect gate="MCU" pin="PA13" pad="A11"/>
<connect gate="MCU" pin="PA14" pad="A10"/>
<connect gate="MCU" pin="PA15" pad="A9"/>
<connect gate="MCU" pin="PA2" pad="K3"/>
<connect gate="MCU" pin="PA3" pad="L3"/>
<connect gate="MCU" pin="PA4" pad="M3"/>
<connect gate="MCU" pin="PA5" pad="K4"/>
<connect gate="MCU" pin="PA6" pad="L4"/>
<connect gate="MCU" pin="PA7" pad="M4"/>
<connect gate="MCU" pin="PA8" pad="D11"/>
<connect gate="MCU" pin="PA9" pad="D10"/>
<connect gate="MCU" pin="PB0" pad="M5"/>
<connect gate="MCU" pin="PB1" pad="M6"/>
<connect gate="MCU" pin="PB10" pad="L10"/>
<connect gate="MCU" pin="PB14" pad="K11"/>
<connect gate="MCU" pin="PB15" pad="K10"/>
<connect gate="MCU" pin="PB3" pad="A8"/>
<connect gate="MCU" pin="PB4" pad="A7"/>
<connect gate="MCU" pin="PB5" pad="C5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="B4"/>
<connect gate="MCU" pin="PB8" pad="A3"/>
<connect gate="MCU" pin="PB9" pad="B3"/>
<connect gate="MCU" pin="PC0" pad="H1"/>
<connect gate="MCU" pin="PC1" pad="J2"/>
<connect gate="MCU" pin="PC10" pad="B11"/>
<connect gate="MCU" pin="PC11" pad="C10"/>
<connect gate="MCU" pin="PC12" pad="B10"/>
<connect gate="MCU" pin="PC13" pad="C1"/>
<connect gate="MCU" pin="PC14" pad="D1"/>
<connect gate="MCU" pin="PC15" pad="E1"/>
<connect gate="MCU" pin="PC2" pad="J3"/>
<connect gate="MCU" pin="PC3" pad="K2"/>
<connect gate="MCU" pin="PC4" pad="K5"/>
<connect gate="MCU" pin="PC5" pad="L5"/>
<connect gate="MCU" pin="PC6" pad="E12"/>
<connect gate="MCU" pin="PC7" pad="E11"/>
<connect gate="MCU" pin="PC8" pad="E10"/>
<connect gate="MCU" pin="PC9" pad="D12"/>
<connect gate="MCU" pin="PD0" pad="C9"/>
<connect gate="MCU" pin="PD1" pad="B9"/>
<connect gate="MCU" pin="PD10" pad="J12"/>
<connect gate="MCU" pin="PD11" pad="J11"/>
<connect gate="MCU" pin="PD12" pad="J10"/>
<connect gate="MCU" pin="PD13" pad="H12"/>
<connect gate="MCU" pin="PD14" pad="H11"/>
<connect gate="MCU" pin="PD15" pad="H10"/>
<connect gate="MCU" pin="PD2" pad="C8"/>
<connect gate="MCU" pin="PD3" pad="B8"/>
<connect gate="MCU" pin="PD4" pad="B7"/>
<connect gate="MCU" pin="PD5" pad="A6"/>
<connect gate="MCU" pin="PD6" pad="B6"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD8" pad="K9"/>
<connect gate="MCU" pin="PD9" pad="K8"/>
<connect gate="MCU" pin="PE0" pad="C3"/>
<connect gate="MCU" pin="PE1" pad="A2"/>
<connect gate="MCU" pin="PE10" pad="L8"/>
<connect gate="MCU" pin="PE11" pad="M9"/>
<connect gate="MCU" pin="PE12" pad="L9"/>
<connect gate="MCU" pin="PE13" pad="M10"/>
<connect gate="MCU" pin="PE14" pad="M11"/>
<connect gate="MCU" pin="PE15" pad="M12"/>
<connect gate="MCU" pin="PE2" pad="B2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="C2"/>
<connect gate="MCU" pin="PE6" pad="D2"/>
<connect gate="MCU" pin="PE7" pad="M7"/>
<connect gate="MCU" pin="PE8" pad="L7"/>
<connect gate="MCU" pin="PE9" pad="M8"/>
<connect gate="MCU" pin="PF10" pad="G2"/>
<connect gate="MCU" pin="PF2" pad="J1"/>
<connect gate="MCU" pin="PF4" pad="E3"/>
<connect gate="MCU" pin="PF6" pad="C11"/>
<connect gate="MCU" pin="PF9" pad="F2"/>
<connect gate="MCU" pin="VBAT" pad="E2"/>
<connect gate="MCU" pin="VDDA" pad="M1"/>
<connect gate="MCU" pin="VDDSD12" pad="G12"/>
<connect gate="MCU" pin="VDDSD3" pad="L12"/>
<connect gate="MCU" pin="VREF+" pad="L1"/>
<connect gate="MCU" pin="VREFSD+" pad="K12"/>
<connect gate="MCU" pin="VREFSD-" pad="L11"/>
<connect gate="MCU" pin="VSSA" pad="K1"/>
<connect gate="MCU" pin="VSSSD" pad="F12"/>
<connect gate="PWR" pin="VDD@1" pad="C4"/>
<connect gate="PWR" pin="VDD@2" pad="H3"/>
<connect gate="PWR" pin="VDD@3" pad="G11"/>
<connect gate="PWR" pin="VSS@1" pad="D3"/>
<connect gate="PWR" pin="VSS@2" pad="F11"/>
</connects>
<technologies>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F401C*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
84 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
64 kbytes of SRAM&lt;br&gt;
36 GPIOs&lt;br&gt;
1.7 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP7"/>
<gate name="PWR" symbol="PWR_VDD3_VSS3"/>
</gates>
<devices>
<device name="" package="UFQFPN48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VCAP1" pad="22"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="48"/>
<connect gate="PWR" pin="VDD@2" pad="36"/>
<connect gate="PWR" pin="VDD@3" pad="24"/>
<connect gate="PWR" pin="VSS@1" pad="47"/>
<connect gate="PWR" pin="VSS@2" pad="35"/>
<connect gate="PWR" pin="VSS@3" pad="23"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F401C*Y" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
84 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
64 kbytes of SRAM&lt;br&gt;
36 GPIOs&lt;br&gt;
1.7 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_49PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD3_VSS3"/>
</gates>
<devices>
<device name="" package="WLCSP49">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A5"/>
<connect gate="MCU" pin="NRST" pad="E7"/>
<connect gate="MCU" pin="OSC_IN" pad="D7"/>
<connect gate="MCU" pin="OSC_OUT" pad="D6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="F6"/>
<connect gate="MCU" pin="PA1" pad="G7"/>
<connect gate="MCU" pin="PA10" pad="C2"/>
<connect gate="MCU" pin="PA11" pad="C1"/>
<connect gate="MCU" pin="PA12" pad="C3"/>
<connect gate="MCU" pin="PA13" pad="B3"/>
<connect gate="MCU" pin="PA14" pad="A1"/>
<connect gate="MCU" pin="PA15" pad="A2"/>
<connect gate="MCU" pin="PA2" pad="E5"/>
<connect gate="MCU" pin="PA3" pad="E4"/>
<connect gate="MCU" pin="PA4" pad="G6"/>
<connect gate="MCU" pin="PA5" pad="F5"/>
<connect gate="MCU" pin="PA6" pad="F4"/>
<connect gate="MCU" pin="PA7" pad="F3"/>
<connect gate="MCU" pin="PA8" pad="D1"/>
<connect gate="MCU" pin="PA9" pad="D2"/>
<connect gate="MCU" pin="PB0" pad="G5"/>
<connect gate="MCU" pin="PB1" pad="G4"/>
<connect gate="MCU" pin="PB10" pad="E3"/>
<connect gate="MCU" pin="PB12" pad="E2"/>
<connect gate="MCU" pin="PB13" pad="G1"/>
<connect gate="MCU" pin="PB14" pad="F1"/>
<connect gate="MCU" pin="PB15" pad="E1"/>
<connect gate="MCU" pin="PB2" pad="G3"/>
<connect gate="MCU" pin="PB3" pad="A3"/>
<connect gate="MCU" pin="PB4" pad="A4"/>
<connect gate="MCU" pin="PB5" pad="B4"/>
<connect gate="MCU" pin="PB6" pad="C4"/>
<connect gate="MCU" pin="PB7" pad="D4"/>
<connect gate="MCU" pin="PB8" pad="B5"/>
<connect gate="MCU" pin="PB9" pad="C5"/>
<connect gate="MCU" pin="PC13" pad="D5"/>
<connect gate="MCU" pin="PC14" pad="C7"/>
<connect gate="MCU" pin="PC15" pad="C6"/>
<connect gate="MCU" pin="PDR_ON" pad="B6"/>
<connect gate="MCU" pin="VBAT" pad="B7"/>
<connect gate="MCU" pin="VCAP1" pad="G2"/>
<connect gate="MCU" pin="VDDA" pad="F7"/>
<connect gate="MCU" pin="VSSA" pad="E6"/>
<connect gate="PWR" pin="VDD@1" pad="A7"/>
<connect gate="PWR" pin="VDD@2" pad="B2"/>
<connect gate="PWR" pin="VDD@3" pad="F2"/>
<connect gate="PWR" pin="VSS@1" pad="A6"/>
<connect gate="PWR" pin="VSS@2" pad="B1"/>
<connect gate="PWR" pin="VSS@3" pad="D3"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F401R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
84 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
64 kbytes of SRAM&lt;br&gt;
50 GPIOs&lt;br&gt;
1.7 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP10"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VCAP1" pad="30"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="64"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VDD@3" pad="32"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="63"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
<connect gate="PWR" pin="VSS@3" pad="31"/>
<connect gate="PWR" pin="VSS@4" pad="18"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F401V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
84 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
64 kbytes of SRAM&lt;br&gt;
81 GPIOs&lt;br&gt;
1.7 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP7"/>
<gate name="PWR" symbol="PWR_VDD6_VSS5"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="48"/>
<connect gate="MCU" pin="VCAP2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="11"/>
<connect gate="PWR" pin="VDD@2" pad="28"/>
<connect gate="PWR" pin="VDD@3" pad="50"/>
<connect gate="PWR" pin="VDD@4" pad="75"/>
<connect gate="PWR" pin="VDD@5" pad="100"/>
<connect gate="PWR" pin="VDD@6" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="10"/>
<connect gate="PWR" pin="VSS@2" pad="27"/>
<connect gate="PWR" pin="VSS@3" pad="49"/>
<connect gate="PWR" pin="VSS@4" pad="74"/>
<connect gate="PWR" pin="VSS@5" pad="99"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F401V*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
84 MHz maximum frequency&lt;br&gt;
128 to 256 Kbytes of Flash memory&lt;br&gt;
64 kbytes of SRAM&lt;br&gt;
81 GPIOs&lt;br&gt;
1.7 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP8"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="UFBGA100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A4"/>
<connect gate="MCU" pin="BYPASS_REG" pad="E3"/>
<connect gate="MCU" pin="NRST" pad="H2"/>
<connect gate="MCU" pin="OSC_IN" pad="F1"/>
<connect gate="MCU" pin="OSC_OUT" pad="G1"/>
<connect gate="MCU" pin="PA0" pad="L2"/>
<connect gate="MCU" pin="PA1" pad="M2"/>
<connect gate="MCU" pin="PA10" pad="C12"/>
<connect gate="MCU" pin="PA11" pad="B12"/>
<connect gate="MCU" pin="PA12" pad="A12"/>
<connect gate="MCU" pin="PA13" pad="A11"/>
<connect gate="MCU" pin="PA14" pad="A10"/>
<connect gate="MCU" pin="PA15" pad="A9"/>
<connect gate="MCU" pin="PA2" pad="K3"/>
<connect gate="MCU" pin="PA3" pad="L3"/>
<connect gate="MCU" pin="PA4" pad="M3"/>
<connect gate="MCU" pin="PA5" pad="K4"/>
<connect gate="MCU" pin="PA6" pad="L4"/>
<connect gate="MCU" pin="PA7" pad="M4"/>
<connect gate="MCU" pin="PA8" pad="D11"/>
<connect gate="MCU" pin="PA9" pad="D10"/>
<connect gate="MCU" pin="PB0" pad="M5"/>
<connect gate="MCU" pin="PB1" pad="M6"/>
<connect gate="MCU" pin="PB10" pad="L10"/>
<connect gate="MCU" pin="PB11" pad="K9"/>
<connect gate="MCU" pin="PB12" pad="L12"/>
<connect gate="MCU" pin="PB13" pad="K12"/>
<connect gate="MCU" pin="PB14" pad="K11"/>
<connect gate="MCU" pin="PB15" pad="K10"/>
<connect gate="MCU" pin="PB2" pad="L6"/>
<connect gate="MCU" pin="PB3" pad="A8"/>
<connect gate="MCU" pin="PB4" pad="A7"/>
<connect gate="MCU" pin="PB5" pad="C5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="B4"/>
<connect gate="MCU" pin="PB8" pad="A3"/>
<connect gate="MCU" pin="PB9" pad="B3"/>
<connect gate="MCU" pin="PC0" pad="H1"/>
<connect gate="MCU" pin="PC1" pad="J2"/>
<connect gate="MCU" pin="PC10" pad="B11"/>
<connect gate="MCU" pin="PC11" pad="C10"/>
<connect gate="MCU" pin="PC12" pad="B10"/>
<connect gate="MCU" pin="PC13" pad="C1"/>
<connect gate="MCU" pin="PC14" pad="D1"/>
<connect gate="MCU" pin="PC15" pad="E1"/>
<connect gate="MCU" pin="PC2" pad="J3"/>
<connect gate="MCU" pin="PC3" pad="K2"/>
<connect gate="MCU" pin="PC4" pad="K5"/>
<connect gate="MCU" pin="PC5" pad="L5"/>
<connect gate="MCU" pin="PC6" pad="E12"/>
<connect gate="MCU" pin="PC7" pad="E11"/>
<connect gate="MCU" pin="PC8" pad="E10"/>
<connect gate="MCU" pin="PC9" pad="D12"/>
<connect gate="MCU" pin="PD0" pad="C9"/>
<connect gate="MCU" pin="PD1" pad="B9"/>
<connect gate="MCU" pin="PD10" pad="J12"/>
<connect gate="MCU" pin="PD11" pad="J11"/>
<connect gate="MCU" pin="PD12" pad="J10"/>
<connect gate="MCU" pin="PD13" pad="H12"/>
<connect gate="MCU" pin="PD14" pad="H11"/>
<connect gate="MCU" pin="PD15" pad="H10"/>
<connect gate="MCU" pin="PD2" pad="C8"/>
<connect gate="MCU" pin="PD3" pad="B8"/>
<connect gate="MCU" pin="PD4" pad="B7"/>
<connect gate="MCU" pin="PD5" pad="A6"/>
<connect gate="MCU" pin="PD6" pad="B6"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD9" pad="K8"/>
<connect gate="MCU" pin="PDR_ON" pad="H3"/>
<connect gate="MCU" pin="PE0" pad="C3"/>
<connect gate="MCU" pin="PE1" pad="A2"/>
<connect gate="MCU" pin="PE10" pad="L8"/>
<connect gate="MCU" pin="PE11" pad="M9"/>
<connect gate="MCU" pin="PE12" pad="L9"/>
<connect gate="MCU" pin="PE13" pad="M10"/>
<connect gate="MCU" pin="PE14" pad="M11"/>
<connect gate="MCU" pin="PE15" pad="M12"/>
<connect gate="MCU" pin="PE2" pad="B2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="C2"/>
<connect gate="MCU" pin="PE6" pad="D2"/>
<connect gate="MCU" pin="PE7" pad="M7"/>
<connect gate="MCU" pin="PE8" pad="L7"/>
<connect gate="MCU" pin="PE9" pad="M8"/>
<connect gate="MCU" pin="VBAT" pad="E2"/>
<connect gate="MCU" pin="VCAP1" pad="L11"/>
<connect gate="MCU" pin="VCAP2" pad="C11"/>
<connect gate="MCU" pin="VDDA" pad="M1"/>
<connect gate="MCU" pin="VREF+" pad="L1"/>
<connect gate="MCU" pin="VREF-" pad="K1"/>
<connect gate="MCU" pin="VSSA" pad="J1"/>
<connect gate="PWR" pin="VDD@1" pad="C4"/>
<connect gate="PWR" pin="VDD@2" pad="G2"/>
<connect gate="PWR" pin="VDD@3" pad="G11"/>
<connect gate="PWR" pin="VDD@4" pad="G12"/>
<connect gate="PWR" pin="VSS@1" pad="D3"/>
<connect gate="PWR" pin="VSS@2" pad="F2"/>
<connect gate="PWR" pin="VSS@3" pad="F11"/>
<connect gate="PWR" pin="VSS@4" pad="F12"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F405R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP5"/>
<gate name="PWR" symbol="PWR_VDD4_VSS2"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VCAP1" pad="31"/>
<connect gate="MCU" pin="VCAP2" pad="47"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="64"/>
<connect gate="PWR" pin="VDD@2" pad="19"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VDD@4" pad="32"/>
<connect gate="PWR" pin="VSS@1" pad="63"/>
<connect gate="PWR" pin="VSS@2" pad="18"/>
</connects>
<technologies>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F405O*Y" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
72 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_90PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD5_VSS4"/>
</gates>
<devices>
<device name="" package="WLCSP90">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A7"/>
<connect gate="MCU" pin="BYPASS_REG" pad="D9"/>
<connect gate="MCU" pin="NRST" pad="G10"/>
<connect gate="MCU" pin="OSC_IN" pad="F10"/>
<connect gate="MCU" pin="OSC_OUT" pad="F9"/>
<connect gate="MCU" pin="PA0-WKUP" pad="C10"/>
<connect gate="MCU" pin="PA1" pad="F8"/>
<connect gate="MCU" pin="PA10" pad="D3"/>
<connect gate="MCU" pin="PA11" pad="C1"/>
<connect gate="MCU" pin="PA12" pad="C2"/>
<connect gate="MCU" pin="PA13" pad="D4"/>
<connect gate="MCU" pin="PA14" pad="A2"/>
<connect gate="MCU" pin="PA15" pad="B3"/>
<connect gate="MCU" pin="PA2" pad="J10"/>
<connect gate="MCU" pin="PA3" pad="H9"/>
<connect gate="MCU" pin="PA4" pad="J9"/>
<connect gate="MCU" pin="PA5" pad="G8"/>
<connect gate="MCU" pin="PA6" pad="H8"/>
<connect gate="MCU" pin="PA7" pad="J8"/>
<connect gate="MCU" pin="PA8" pad="D1"/>
<connect gate="MCU" pin="PA9" pad="D2"/>
<connect gate="MCU" pin="PB0" pad="G7"/>
<connect gate="MCU" pin="PB1" pad="H7"/>
<connect gate="MCU" pin="PB10" pad="H4"/>
<connect gate="MCU" pin="PB11" pad="J4"/>
<connect gate="MCU" pin="PB12" pad="J3"/>
<connect gate="MCU" pin="PB13" pad="J1"/>
<connect gate="MCU" pin="PB14" pad="J2"/>
<connect gate="MCU" pin="PB15" pad="H1"/>
<connect gate="MCU" pin="PB2" pad="J7"/>
<connect gate="MCU" pin="PB3" pad="B6"/>
<connect gate="MCU" pin="PB4" pad="A6"/>
<connect gate="MCU" pin="PB5" pad="D7"/>
<connect gate="MCU" pin="PB6" pad="C7"/>
<connect gate="MCU" pin="PB7" pad="B7"/>
<connect gate="MCU" pin="PB8" pad="D8"/>
<connect gate="MCU" pin="PB9" pad="C8"/>
<connect gate="MCU" pin="PC0" pad="E10"/>
<connect gate="MCU" pin="PC10" pad="D5"/>
<connect gate="MCU" pin="PC11" pad="C4"/>
<connect gate="MCU" pin="PC12" pad="A3"/>
<connect gate="MCU" pin="PC13" pad="A9"/>
<connect gate="MCU" pin="PC14" pad="B10"/>
<connect gate="MCU" pin="PC15" pad="B9"/>
<connect gate="MCU" pin="PC2" pad="D10"/>
<connect gate="MCU" pin="PC3" pad="E9"/>
<connect gate="MCU" pin="PC6" pad="F3"/>
<connect gate="MCU" pin="PC7" pad="E1"/>
<connect gate="MCU" pin="PC8" pad="E2"/>
<connect gate="MCU" pin="PC9" pad="E3"/>
<connect gate="MCU" pin="PD0" pad="D6"/>
<connect gate="MCU" pin="PD1" pad="C5"/>
<connect gate="MCU" pin="PD10" pad="G3"/>
<connect gate="MCU" pin="PD11" pad="G1"/>
<connect gate="MCU" pin="PD12" pad="G2"/>
<connect gate="MCU" pin="PD14" pad="F2"/>
<connect gate="MCU" pin="PD15" pad="F1"/>
<connect gate="MCU" pin="PD2" pad="B4"/>
<connect gate="MCU" pin="PD4" pad="A4"/>
<connect gate="MCU" pin="PD5" pad="C6"/>
<connect gate="MCU" pin="PD6" pad="B5"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD8" pad="H2"/>
<connect gate="MCU" pin="PD9" pad="H3"/>
<connect gate="MCU" pin="PDR_ON" pad="A8"/>
<connect gate="MCU" pin="PE10" pad="F6"/>
<connect gate="MCU" pin="PE11" pad="J5"/>
<connect gate="MCU" pin="PE12" pad="H5"/>
<connect gate="MCU" pin="PE13" pad="G5"/>
<connect gate="MCU" pin="PE14" pad="F5"/>
<connect gate="MCU" pin="PE15" pad="G4"/>
<connect gate="MCU" pin="PE7" pad="G6"/>
<connect gate="MCU" pin="PE8" pad="H6"/>
<connect gate="MCU" pin="PE9" pad="J6"/>
<connect gate="MCU" pin="PI0" pad="C3"/>
<connect gate="MCU" pin="PI1" pad="B2"/>
<connect gate="MCU" pin="VBAT" pad="A10"/>
<connect gate="MCU" pin="VCAP1" pad="F4"/>
<connect gate="MCU" pin="VCAP2" pad="B1"/>
<connect gate="MCU" pin="VDDA" pad="G9"/>
<connect gate="MCU" pin="VSSA" pad="H10"/>
<connect gate="PWR" pin="VDD@1" pad="A1"/>
<connect gate="PWR" pin="VDD@2" pad="B8"/>
<connect gate="PWR" pin="VDD@3" pad="E4"/>
<connect gate="PWR" pin="VDD@4" pad="E6"/>
<connect gate="PWR" pin="VDD@5" pad="F7"/>
<connect gate="PWR" pin="VSS@1" pad="C9"/>
<connect gate="PWR" pin="VSS@2" pad="E5"/>
<connect gate="PWR" pin="VSS@3" pad="E7"/>
<connect gate="PWR" pin="VSS@4" pad="E8"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F405V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP9"/>
<gate name="PWR" symbol="PWR_VDD6_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="49"/>
<connect gate="MCU" pin="VCAP2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="11"/>
<connect gate="PWR" pin="VDD@2" pad="28"/>
<connect gate="PWR" pin="VDD@3" pad="75"/>
<connect gate="PWR" pin="VDD@4" pad="100"/>
<connect gate="PWR" pin="VDD@5" pad="19"/>
<connect gate="PWR" pin="VDD@6" pad="50"/>
<connect gate="PWR" pin="VSS@1" pad="10"/>
<connect gate="PWR" pin="VSS@2" pad="27"/>
<connect gate="PWR" pin="VSS@3" pad="74"/>
<connect gate="PWR" pin="VSS@4" pad="99"/>
</connects>
<technologies>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F405Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD12_VSS9"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PDR_ON" pad="143"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="71"/>
<connect gate="MCU" pin="VCAP2" pad="106"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VSSA" pad="31"/>
<connect gate="PWR" pin="VDD@1" pad="17"/>
<connect gate="PWR" pin="VDD@10" pad="144"/>
<connect gate="PWR" pin="VDD@11" pad="72"/>
<connect gate="PWR" pin="VDD@12" pad="30"/>
<connect gate="PWR" pin="VDD@2" pad="39"/>
<connect gate="PWR" pin="VDD@3" pad="52"/>
<connect gate="PWR" pin="VDD@4" pad="62"/>
<connect gate="PWR" pin="VDD@5" pad="84"/>
<connect gate="PWR" pin="VDD@6" pad="95"/>
<connect gate="PWR" pin="VDD@7" pad="108"/>
<connect gate="PWR" pin="VDD@8" pad="121"/>
<connect gate="PWR" pin="VDD@9" pad="131"/>
<connect gate="PWR" pin="VSS@1" pad="16"/>
<connect gate="PWR" pin="VSS@2" pad="38"/>
<connect gate="PWR" pin="VSS@3" pad="51"/>
<connect gate="PWR" pin="VSS@4" pad="61"/>
<connect gate="PWR" pin="VSS@5" pad="83"/>
<connect gate="PWR" pin="VSS@6" pad="94"/>
<connect gate="PWR" pin="VSS@7" pad="107"/>
<connect gate="PWR" pin="VSS@8" pad="120"/>
<connect gate="PWR" pin="VSS@9" pad="130"/>
</connects>
<technologies>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F407V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP9"/>
<gate name="PWR" symbol="PWR_VDD6_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="49"/>
<connect gate="MCU" pin="VCAP2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="11"/>
<connect gate="PWR" pin="VDD@2" pad="28"/>
<connect gate="PWR" pin="VDD@3" pad="75"/>
<connect gate="PWR" pin="VDD@4" pad="100"/>
<connect gate="PWR" pin="VDD@5" pad="50"/>
<connect gate="PWR" pin="VDD@6" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="10"/>
<connect gate="PWR" pin="VSS@2" pad="27"/>
<connect gate="PWR" pin="VSS@3" pad="74"/>
<connect gate="PWR" pin="VSS@4" pad="99"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F407Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD12_VSS9"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PDR_ON" pad="143"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="71"/>
<connect gate="MCU" pin="VCAP2" pad="106"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VSSA" pad="31"/>
<connect gate="PWR" pin="VDD@1" pad="17"/>
<connect gate="PWR" pin="VDD@10" pad="144"/>
<connect gate="PWR" pin="VDD@11" pad="72"/>
<connect gate="PWR" pin="VDD@12" pad="30"/>
<connect gate="PWR" pin="VDD@2" pad="39"/>
<connect gate="PWR" pin="VDD@3" pad="52"/>
<connect gate="PWR" pin="VDD@4" pad="62"/>
<connect gate="PWR" pin="VDD@5" pad="84"/>
<connect gate="PWR" pin="VDD@6" pad="95"/>
<connect gate="PWR" pin="VDD@7" pad="108"/>
<connect gate="PWR" pin="VDD@8" pad="121"/>
<connect gate="PWR" pin="VDD@9" pad="131"/>
<connect gate="PWR" pin="VSS@1" pad="16"/>
<connect gate="PWR" pin="VSS@2" pad="38"/>
<connect gate="PWR" pin="VSS@3" pad="51"/>
<connect gate="PWR" pin="VSS@4" pad="61"/>
<connect gate="PWR" pin="VSS@5" pad="83"/>
<connect gate="PWR" pin="VSS@6" pad="94"/>
<connect gate="PWR" pin="VSS@7" pad="107"/>
<connect gate="PWR" pin="VSS@8" pad="120"/>
<connect gate="PWR" pin="VSS@9" pad="130"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F407I*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD15_VSS11"/>
</gates>
<devices>
<device name="" package="LQFP176">
<connects>
<connect gate="MCU" pin="BOOT0" pad="166"/>
<connect gate="MCU" pin="BYPASS_REG" pad="48"/>
<connect gate="MCU" pin="NRST" pad="31"/>
<connect gate="MCU" pin="OSC_IN" pad="29"/>
<connect gate="MCU" pin="OSC_OUT" pad="30"/>
<connect gate="MCU" pin="PA0" pad="40"/>
<connect gate="MCU" pin="PA1" pad="41"/>
<connect gate="MCU" pin="PA10" pad="121"/>
<connect gate="MCU" pin="PA11" pad="122"/>
<connect gate="MCU" pin="PA12" pad="123"/>
<connect gate="MCU" pin="PA13" pad="124"/>
<connect gate="MCU" pin="PA14" pad="137"/>
<connect gate="MCU" pin="PA15" pad="138"/>
<connect gate="MCU" pin="PA2" pad="42"/>
<connect gate="MCU" pin="PA3" pad="47"/>
<connect gate="MCU" pin="PA4" pad="50"/>
<connect gate="MCU" pin="PA5" pad="51"/>
<connect gate="MCU" pin="PA6" pad="52"/>
<connect gate="MCU" pin="PA7" pad="53"/>
<connect gate="MCU" pin="PA8" pad="119"/>
<connect gate="MCU" pin="PA9" pad="120"/>
<connect gate="MCU" pin="PB0" pad="56"/>
<connect gate="MCU" pin="PB1" pad="57"/>
<connect gate="MCU" pin="PB10" pad="79"/>
<connect gate="MCU" pin="PB11" pad="80"/>
<connect gate="MCU" pin="PB12" pad="92"/>
<connect gate="MCU" pin="PB13" pad="93"/>
<connect gate="MCU" pin="PB14" pad="94"/>
<connect gate="MCU" pin="PB15" pad="95"/>
<connect gate="MCU" pin="PB2" pad="58"/>
<connect gate="MCU" pin="PB3" pad="161"/>
<connect gate="MCU" pin="PB4" pad="162"/>
<connect gate="MCU" pin="PB5" pad="163"/>
<connect gate="MCU" pin="PB6" pad="164"/>
<connect gate="MCU" pin="PB7" pad="165"/>
<connect gate="MCU" pin="PB8" pad="167"/>
<connect gate="MCU" pin="PB9" pad="168"/>
<connect gate="MCU" pin="PC0" pad="32"/>
<connect gate="MCU" pin="PC1" pad="33"/>
<connect gate="MCU" pin="PC10" pad="139"/>
<connect gate="MCU" pin="PC11" pad="140"/>
<connect gate="MCU" pin="PC12" pad="141"/>
<connect gate="MCU" pin="PC13" pad="8"/>
<connect gate="MCU" pin="PC14" pad="9"/>
<connect gate="MCU" pin="PC15" pad="10"/>
<connect gate="MCU" pin="PC2" pad="34"/>
<connect gate="MCU" pin="PC3" pad="35"/>
<connect gate="MCU" pin="PC4" pad="54"/>
<connect gate="MCU" pin="PC5" pad="55"/>
<connect gate="MCU" pin="PC6" pad="115"/>
<connect gate="MCU" pin="PC7" pad="116"/>
<connect gate="MCU" pin="PC8" pad="117"/>
<connect gate="MCU" pin="PC9" pad="118"/>
<connect gate="MCU" pin="PD0" pad="142"/>
<connect gate="MCU" pin="PD1" pad="143"/>
<connect gate="MCU" pin="PD10" pad="98"/>
<connect gate="MCU" pin="PD11" pad="99"/>
<connect gate="MCU" pin="PD12" pad="100"/>
<connect gate="MCU" pin="PD13" pad="101"/>
<connect gate="MCU" pin="PD14" pad="104"/>
<connect gate="MCU" pin="PD15" pad="105"/>
<connect gate="MCU" pin="PD2" pad="144"/>
<connect gate="MCU" pin="PD3" pad="145"/>
<connect gate="MCU" pin="PD4" pad="146"/>
<connect gate="MCU" pin="PD5" pad="147"/>
<connect gate="MCU" pin="PD6" pad="150"/>
<connect gate="MCU" pin="PD7" pad="151"/>
<connect gate="MCU" pin="PD8" pad="96"/>
<connect gate="MCU" pin="PD9" pad="97"/>
<connect gate="MCU" pin="PDR_ON" pad="171"/>
<connect gate="MCU" pin="PE0" pad="169"/>
<connect gate="MCU" pin="PE1" pad="170"/>
<connect gate="MCU" pin="PE10" pad="73"/>
<connect gate="MCU" pin="PE11" pad="74"/>
<connect gate="MCU" pin="PE12" pad="75"/>
<connect gate="MCU" pin="PE13" pad="76"/>
<connect gate="MCU" pin="PE14" pad="77"/>
<connect gate="MCU" pin="PE15" pad="78"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="68"/>
<connect gate="MCU" pin="PE8" pad="69"/>
<connect gate="MCU" pin="PE9" pad="70"/>
<connect gate="MCU" pin="PF0" pad="16"/>
<connect gate="MCU" pin="PF1" pad="17"/>
<connect gate="MCU" pin="PF10" pad="28"/>
<connect gate="MCU" pin="PF11" pad="59"/>
<connect gate="MCU" pin="PF12" pad="60"/>
<connect gate="MCU" pin="PF13" pad="63"/>
<connect gate="MCU" pin="PF14" pad="64"/>
<connect gate="MCU" pin="PF15" pad="65"/>
<connect gate="MCU" pin="PF2" pad="18"/>
<connect gate="MCU" pin="PF3" pad="19"/>
<connect gate="MCU" pin="PF4" pad="20"/>
<connect gate="MCU" pin="PF5" pad="21"/>
<connect gate="MCU" pin="PF6" pad="24"/>
<connect gate="MCU" pin="PF7" pad="25"/>
<connect gate="MCU" pin="PF8" pad="26"/>
<connect gate="MCU" pin="PF9" pad="27"/>
<connect gate="MCU" pin="PG0" pad="66"/>
<connect gate="MCU" pin="PG1" pad="67"/>
<connect gate="MCU" pin="PG10" pad="153"/>
<connect gate="MCU" pin="PG11" pad="154"/>
<connect gate="MCU" pin="PG12" pad="155"/>
<connect gate="MCU" pin="PG13" pad="156"/>
<connect gate="MCU" pin="PG14" pad="157"/>
<connect gate="MCU" pin="PG15" pad="160"/>
<connect gate="MCU" pin="PG2" pad="106"/>
<connect gate="MCU" pin="PG3" pad="107"/>
<connect gate="MCU" pin="PG4" pad="108"/>
<connect gate="MCU" pin="PG5" pad="109"/>
<connect gate="MCU" pin="PG6" pad="110"/>
<connect gate="MCU" pin="PG7" pad="111"/>
<connect gate="MCU" pin="PG8" pad="112"/>
<connect gate="MCU" pin="PG9" pad="152"/>
<connect gate="MCU" pin="PH10" pad="87"/>
<connect gate="MCU" pin="PH11" pad="88"/>
<connect gate="MCU" pin="PH12" pad="89"/>
<connect gate="MCU" pin="PH13" pad="128"/>
<connect gate="MCU" pin="PH14" pad="129"/>
<connect gate="MCU" pin="PH15" pad="130"/>
<connect gate="MCU" pin="PH2" pad="43"/>
<connect gate="MCU" pin="PH3" pad="44"/>
<connect gate="MCU" pin="PH4" pad="45"/>
<connect gate="MCU" pin="PH5" pad="46"/>
<connect gate="MCU" pin="PH6" pad="83"/>
<connect gate="MCU" pin="PH7" pad="84"/>
<connect gate="MCU" pin="PH8" pad="85"/>
<connect gate="MCU" pin="PH9" pad="86"/>
<connect gate="MCU" pin="PI0" pad="131"/>
<connect gate="MCU" pin="PI1" pad="132"/>
<connect gate="MCU" pin="PI10" pad="12"/>
<connect gate="MCU" pin="PI11" pad="13"/>
<connect gate="MCU" pin="PI2" pad="133"/>
<connect gate="MCU" pin="PI3" pad="134"/>
<connect gate="MCU" pin="PI4" pad="173"/>
<connect gate="MCU" pin="PI5" pad="174"/>
<connect gate="MCU" pin="PI6" pad="175"/>
<connect gate="MCU" pin="PI7" pad="176"/>
<connect gate="MCU" pin="PI8" pad="7"/>
<connect gate="MCU" pin="PI9" pad="11"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="81"/>
<connect gate="MCU" pin="VCAP2" pad="125"/>
<connect gate="MCU" pin="VDDA" pad="39"/>
<connect gate="MCU" pin="VREF+" pad="38"/>
<connect gate="MCU" pin="VSSA" pad="37"/>
<connect gate="PWR" pin="VDD@1" pad="15"/>
<connect gate="PWR" pin="VDD@10" pad="149"/>
<connect gate="PWR" pin="VDD@11" pad="159"/>
<connect gate="PWR" pin="VDD@12" pad="172"/>
<connect gate="PWR" pin="VDD@13" pad="82"/>
<connect gate="PWR" pin="VDD@14" pad="49"/>
<connect gate="PWR" pin="VDD@15" pad="36"/>
<connect gate="PWR" pin="VDD@2" pad="23"/>
<connect gate="PWR" pin="VDD@3" pad="62"/>
<connect gate="PWR" pin="VDD@4" pad="72"/>
<connect gate="PWR" pin="VDD@5" pad="91"/>
<connect gate="PWR" pin="VDD@6" pad="103"/>
<connect gate="PWR" pin="VDD@7" pad="114"/>
<connect gate="PWR" pin="VDD@8" pad="127"/>
<connect gate="PWR" pin="VDD@9" pad="136"/>
<connect gate="PWR" pin="VSS@1" pad="14"/>
<connect gate="PWR" pin="VSS@10" pad="148"/>
<connect gate="PWR" pin="VSS@11" pad="158"/>
<connect gate="PWR" pin="VSS@2" pad="22"/>
<connect gate="PWR" pin="VSS@3" pad="61"/>
<connect gate="PWR" pin="VSS@4" pad="71"/>
<connect gate="PWR" pin="VSS@5" pad="90"/>
<connect gate="PWR" pin="VSS@6" pad="102"/>
<connect gate="PWR" pin="VSS@7" pad="113"/>
<connect gate="PWR" pin="VSS@8" pad="126"/>
<connect gate="PWR" pin="VSS@9" pad="135"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F407I*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD14_VSS36"/>
</gates>
<devices>
<device name="" package="UFBGA176+25">
<connects>
<connect gate="MCU" pin="BOOT0" pad="D6"/>
<connect gate="MCU" pin="BYPASS_REG" pad="L4"/>
<connect gate="MCU" pin="NRST" pad="J1"/>
<connect gate="MCU" pin="OSC_IN" pad="G1"/>
<connect gate="MCU" pin="OSC_OUT" pad="H1"/>
<connect gate="MCU" pin="PA0" pad="N3"/>
<connect gate="MCU" pin="PA1" pad="N2"/>
<connect gate="MCU" pin="PA10" pad="D15"/>
<connect gate="MCU" pin="PA11" pad="C15"/>
<connect gate="MCU" pin="PA12" pad="B15"/>
<connect gate="MCU" pin="PA13" pad="A15"/>
<connect gate="MCU" pin="PA14" pad="A14"/>
<connect gate="MCU" pin="PA15" pad="A13"/>
<connect gate="MCU" pin="PA2" pad="P2"/>
<connect gate="MCU" pin="PA3" pad="R2"/>
<connect gate="MCU" pin="PA4" pad="N4"/>
<connect gate="MCU" pin="PA5" pad="P4"/>
<connect gate="MCU" pin="PA6" pad="P3"/>
<connect gate="MCU" pin="PA7" pad="R3"/>
<connect gate="MCU" pin="PA8" pad="F15"/>
<connect gate="MCU" pin="PA9" pad="E15"/>
<connect gate="MCU" pin="PB0" pad="R5"/>
<connect gate="MCU" pin="PB1" pad="R4"/>
<connect gate="MCU" pin="PB10" pad="R12"/>
<connect gate="MCU" pin="PB11" pad="R13"/>
<connect gate="MCU" pin="PB12" pad="P12"/>
<connect gate="MCU" pin="PB13" pad="P13"/>
<connect gate="MCU" pin="PB14" pad="R14"/>
<connect gate="MCU" pin="PB15" pad="R15"/>
<connect gate="MCU" pin="PB2" pad="M6"/>
<connect gate="MCU" pin="PB3" pad="A10"/>
<connect gate="MCU" pin="PB4" pad="A9"/>
<connect gate="MCU" pin="PB5" pad="A6"/>
<connect gate="MCU" pin="PB6" pad="B6"/>
<connect gate="MCU" pin="PB7" pad="B5"/>
<connect gate="MCU" pin="PB8" pad="A5"/>
<connect gate="MCU" pin="PB9" pad="B4"/>
<connect gate="MCU" pin="PC0" pad="M2"/>
<connect gate="MCU" pin="PC1" pad="M3"/>
<connect gate="MCU" pin="PC10" pad="B14"/>
<connect gate="MCU" pin="PC11" pad="B13"/>
<connect gate="MCU" pin="PC12" pad="A12"/>
<connect gate="MCU" pin="PC13" pad="D1"/>
<connect gate="MCU" pin="PC14" pad="E1"/>
<connect gate="MCU" pin="PC15" pad="F1"/>
<connect gate="MCU" pin="PC2" pad="M4"/>
<connect gate="MCU" pin="PC3" pad="M5"/>
<connect gate="MCU" pin="PC4" pad="N5"/>
<connect gate="MCU" pin="PC5" pad="P5"/>
<connect gate="MCU" pin="PC6" pad="H15"/>
<connect gate="MCU" pin="PC7" pad="G15"/>
<connect gate="MCU" pin="PC8" pad="G14"/>
<connect gate="MCU" pin="PC9" pad="F14"/>
<connect gate="MCU" pin="PD0" pad="B12"/>
<connect gate="MCU" pin="PD1" pad="C12"/>
<connect gate="MCU" pin="PD10" pad="N15"/>
<connect gate="MCU" pin="PD11" pad="N14"/>
<connect gate="MCU" pin="PD12" pad="N13"/>
<connect gate="MCU" pin="PD13" pad="M15"/>
<connect gate="MCU" pin="PD14" pad="M14"/>
<connect gate="MCU" pin="PD15" pad="L14"/>
<connect gate="MCU" pin="PD2" pad="D12"/>
<connect gate="MCU" pin="PD3" pad="D11"/>
<connect gate="MCU" pin="PD4" pad="D10"/>
<connect gate="MCU" pin="PD5" pad="C11"/>
<connect gate="MCU" pin="PD6" pad="B11"/>
<connect gate="MCU" pin="PD7" pad="A11"/>
<connect gate="MCU" pin="PD8" pad="P15"/>
<connect gate="MCU" pin="PD9" pad="P14"/>
<connect gate="MCU" pin="PDR_ON" pad="C6"/>
<connect gate="MCU" pin="PE0" pad="A4"/>
<connect gate="MCU" pin="PE1" pad="A3"/>
<connect gate="MCU" pin="PE10" pad="R9"/>
<connect gate="MCU" pin="PE11" pad="P10"/>
<connect gate="MCU" pin="PE12" pad="R10"/>
<connect gate="MCU" pin="PE13" pad="N11"/>
<connect gate="MCU" pin="PE14" pad="P11"/>
<connect gate="MCU" pin="PE15" pad="R11"/>
<connect gate="MCU" pin="PE2" pad="A2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="B2"/>
<connect gate="MCU" pin="PE6" pad="B3"/>
<connect gate="MCU" pin="PE7" pad="R8"/>
<connect gate="MCU" pin="PE8" pad="P8"/>
<connect gate="MCU" pin="PE9" pad="P9"/>
<connect gate="MCU" pin="PF0" pad="E2"/>
<connect gate="MCU" pin="PF1" pad="H3"/>
<connect gate="MCU" pin="PF10" pad="L1"/>
<connect gate="MCU" pin="PF11" pad="R6"/>
<connect gate="MCU" pin="PF12" pad="P6"/>
<connect gate="MCU" pin="PF13" pad="N6"/>
<connect gate="MCU" pin="PF14" pad="R7"/>
<connect gate="MCU" pin="PF15" pad="P7"/>
<connect gate="MCU" pin="PF2" pad="H2"/>
<connect gate="MCU" pin="PF3" pad="J2"/>
<connect gate="MCU" pin="PF4" pad="J3"/>
<connect gate="MCU" pin="PF5" pad="K3"/>
<connect gate="MCU" pin="PF6" pad="K2"/>
<connect gate="MCU" pin="PF7" pad="K1"/>
<connect gate="MCU" pin="PF8" pad="L3"/>
<connect gate="MCU" pin="PF9" pad="L2"/>
<connect gate="MCU" pin="PG0" pad="N7"/>
<connect gate="MCU" pin="PG1" pad="M7"/>
<connect gate="MCU" pin="PG10" pad="B10"/>
<connect gate="MCU" pin="PG11" pad="B9"/>
<connect gate="MCU" pin="PG12" pad="B8"/>
<connect gate="MCU" pin="PG13" pad="A8"/>
<connect gate="MCU" pin="PG14" pad="A7"/>
<connect gate="MCU" pin="PG15" pad="B7"/>
<connect gate="MCU" pin="PG2" pad="L15"/>
<connect gate="MCU" pin="PG3" pad="K15"/>
<connect gate="MCU" pin="PG4" pad="K14"/>
<connect gate="MCU" pin="PG5" pad="K13"/>
<connect gate="MCU" pin="PG6" pad="J15"/>
<connect gate="MCU" pin="PG7" pad="J14"/>
<connect gate="MCU" pin="PG8" pad="H14"/>
<connect gate="MCU" pin="PG9" pad="C10"/>
<connect gate="MCU" pin="PH10" pad="L13"/>
<connect gate="MCU" pin="PH11" pad="L12"/>
<connect gate="MCU" pin="PH12" pad="K12"/>
<connect gate="MCU" pin="PH13" pad="E12"/>
<connect gate="MCU" pin="PH14" pad="E13"/>
<connect gate="MCU" pin="PH15" pad="D13"/>
<connect gate="MCU" pin="PH2" pad="F4"/>
<connect gate="MCU" pin="PH3" pad="G4"/>
<connect gate="MCU" pin="PH4" pad="H4"/>
<connect gate="MCU" pin="PH5" pad="J4"/>
<connect gate="MCU" pin="PH6" pad="M11"/>
<connect gate="MCU" pin="PH7" pad="N12"/>
<connect gate="MCU" pin="PH8" pad="M12"/>
<connect gate="MCU" pin="PH9" pad="M13"/>
<connect gate="MCU" pin="PI0" pad="E14"/>
<connect gate="MCU" pin="PI1" pad="D14"/>
<connect gate="MCU" pin="PI10" pad="E3"/>
<connect gate="MCU" pin="PI11" pad="E4"/>
<connect gate="MCU" pin="PI2" pad="C14"/>
<connect gate="MCU" pin="PI3" pad="C13"/>
<connect gate="MCU" pin="PI4" pad="D4"/>
<connect gate="MCU" pin="PI5" pad="C4"/>
<connect gate="MCU" pin="PI6" pad="C3"/>
<connect gate="MCU" pin="PI7" pad="C2"/>
<connect gate="MCU" pin="PI8" pad="D2"/>
<connect gate="MCU" pin="PI9" pad="D3"/>
<connect gate="MCU" pin="VBAT" pad="C1"/>
<connect gate="MCU" pin="VCAP1" pad="M10"/>
<connect gate="MCU" pin="VCAP2" pad="F13"/>
<connect gate="MCU" pin="VDDA" pad="R1"/>
<connect gate="MCU" pin="VREF+" pad="P1"/>
<connect gate="MCU" pin="VREF-" pad="N1"/>
<connect gate="MCU" pin="VSSA" pad="M1"/>
<connect gate="PWR" pin="VDD@1" pad="C5"/>
<connect gate="PWR" pin="VDD@10" pad="J13"/>
<connect gate="PWR" pin="VDD@11" pad="K4"/>
<connect gate="PWR" pin="VDD@12" pad="N8"/>
<connect gate="PWR" pin="VDD@13" pad="N9"/>
<connect gate="PWR" pin="VDD@14" pad="N10"/>
<connect gate="PWR" pin="VDD@2" pad="C7"/>
<connect gate="PWR" pin="VDD@3" pad="C8"/>
<connect gate="PWR" pin="VDD@4" pad="C9"/>
<connect gate="PWR" pin="VDD@5" pad="F3"/>
<connect gate="PWR" pin="VDD@6" pad="G3"/>
<connect gate="PWR" pin="VDD@7" pad="G13"/>
<connect gate="PWR" pin="VDD@8" pad="H13"/>
<connect gate="PWR" pin="VDD@9" pad="J12"/>
<connect gate="PWR" pin="VSS@1" pad="D5"/>
<connect gate="PWR" pin="VSS@10" pad="M8"/>
<connect gate="PWR" pin="VSS@11" pad="M9"/>
<connect gate="PWR" pin="VSS@12" pad="VSS_1"/>
<connect gate="PWR" pin="VSS@13" pad="VSS_2"/>
<connect gate="PWR" pin="VSS@14" pad="VSS_3"/>
<connect gate="PWR" pin="VSS@15" pad="VSS_4"/>
<connect gate="PWR" pin="VSS@16" pad="VSS_5"/>
<connect gate="PWR" pin="VSS@17" pad="VSS_6"/>
<connect gate="PWR" pin="VSS@18" pad="VSS_7"/>
<connect gate="PWR" pin="VSS@19" pad="VSS_8"/>
<connect gate="PWR" pin="VSS@2" pad="D7"/>
<connect gate="PWR" pin="VSS@20" pad="VSS_9"/>
<connect gate="PWR" pin="VSS@21" pad="VSS_10"/>
<connect gate="PWR" pin="VSS@22" pad="VSS_11"/>
<connect gate="PWR" pin="VSS@23" pad="VSS_12"/>
<connect gate="PWR" pin="VSS@24" pad="VSS_13"/>
<connect gate="PWR" pin="VSS@25" pad="VSS_14"/>
<connect gate="PWR" pin="VSS@26" pad="VSS_15"/>
<connect gate="PWR" pin="VSS@27" pad="VSS_16"/>
<connect gate="PWR" pin="VSS@28" pad="VSS_17"/>
<connect gate="PWR" pin="VSS@29" pad="VSS_18"/>
<connect gate="PWR" pin="VSS@3" pad="D8"/>
<connect gate="PWR" pin="VSS@30" pad="VSS_19"/>
<connect gate="PWR" pin="VSS@31" pad="VSS_20"/>
<connect gate="PWR" pin="VSS@32" pad="VSS_21"/>
<connect gate="PWR" pin="VSS@33" pad="VSS_22"/>
<connect gate="PWR" pin="VSS@34" pad="VSS_23"/>
<connect gate="PWR" pin="VSS@35" pad="VSS_24"/>
<connect gate="PWR" pin="VSS@36" pad="VSS_25"/>
<connect gate="PWR" pin="VSS@4" pad="D9"/>
<connect gate="PWR" pin="VSS@5" pad="F2"/>
<connect gate="PWR" pin="VSS@6" pad="F12"/>
<connect gate="PWR" pin="VSS@7" pad="G2"/>
<connect gate="PWR" pin="VSS@8" pad="G12"/>
<connect gate="PWR" pin="VSS@9" pad="H12"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F415R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP5"/>
<gate name="PWR" symbol="PWR_VDD4_VSS2"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VCAP1" pad="31"/>
<connect gate="MCU" pin="VCAP2" pad="47"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="64"/>
<connect gate="PWR" pin="VDD@2" pad="19"/>
<connect gate="PWR" pin="VDD@3" pad="32"/>
<connect gate="PWR" pin="VDD@4" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="63"/>
<connect gate="PWR" pin="VSS@2" pad="18"/>
</connects>
<technologies>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F415O*Y" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
72 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_90PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD5_VSS4"/>
</gates>
<devices>
<device name="" package="WLCSP90">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A7"/>
<connect gate="MCU" pin="BYPASS_REG" pad="D9"/>
<connect gate="MCU" pin="NRST" pad="G10"/>
<connect gate="MCU" pin="OSC_IN" pad="F10"/>
<connect gate="MCU" pin="OSC_OUT" pad="F9"/>
<connect gate="MCU" pin="PA0-WKUP" pad="C10"/>
<connect gate="MCU" pin="PA1" pad="F8"/>
<connect gate="MCU" pin="PA10" pad="D3"/>
<connect gate="MCU" pin="PA11" pad="C1"/>
<connect gate="MCU" pin="PA12" pad="C2"/>
<connect gate="MCU" pin="PA13" pad="D4"/>
<connect gate="MCU" pin="PA14" pad="A2"/>
<connect gate="MCU" pin="PA15" pad="B3"/>
<connect gate="MCU" pin="PA2" pad="J10"/>
<connect gate="MCU" pin="PA3" pad="H9"/>
<connect gate="MCU" pin="PA4" pad="J9"/>
<connect gate="MCU" pin="PA5" pad="G8"/>
<connect gate="MCU" pin="PA6" pad="H8"/>
<connect gate="MCU" pin="PA7" pad="J8"/>
<connect gate="MCU" pin="PA8" pad="D1"/>
<connect gate="MCU" pin="PA9" pad="D2"/>
<connect gate="MCU" pin="PB0" pad="G7"/>
<connect gate="MCU" pin="PB1" pad="H7"/>
<connect gate="MCU" pin="PB10" pad="H4"/>
<connect gate="MCU" pin="PB11" pad="J4"/>
<connect gate="MCU" pin="PB12" pad="J3"/>
<connect gate="MCU" pin="PB13" pad="J1"/>
<connect gate="MCU" pin="PB14" pad="J2"/>
<connect gate="MCU" pin="PB15" pad="H1"/>
<connect gate="MCU" pin="PB2" pad="J7"/>
<connect gate="MCU" pin="PB3" pad="B6"/>
<connect gate="MCU" pin="PB4" pad="A6"/>
<connect gate="MCU" pin="PB5" pad="D7"/>
<connect gate="MCU" pin="PB6" pad="C7"/>
<connect gate="MCU" pin="PB7" pad="B7"/>
<connect gate="MCU" pin="PB8" pad="D8"/>
<connect gate="MCU" pin="PB9" pad="C8"/>
<connect gate="MCU" pin="PC0" pad="E10"/>
<connect gate="MCU" pin="PC10" pad="D5"/>
<connect gate="MCU" pin="PC11" pad="C4"/>
<connect gate="MCU" pin="PC12" pad="A3"/>
<connect gate="MCU" pin="PC13" pad="A9"/>
<connect gate="MCU" pin="PC14" pad="B10"/>
<connect gate="MCU" pin="PC15" pad="B9"/>
<connect gate="MCU" pin="PC2" pad="D10"/>
<connect gate="MCU" pin="PC3" pad="E9"/>
<connect gate="MCU" pin="PC6" pad="F3"/>
<connect gate="MCU" pin="PC7" pad="E1"/>
<connect gate="MCU" pin="PC8" pad="E2"/>
<connect gate="MCU" pin="PC9" pad="E3"/>
<connect gate="MCU" pin="PD0" pad="D6"/>
<connect gate="MCU" pin="PD1" pad="C5"/>
<connect gate="MCU" pin="PD10" pad="G3"/>
<connect gate="MCU" pin="PD11" pad="G1"/>
<connect gate="MCU" pin="PD12" pad="G2"/>
<connect gate="MCU" pin="PD14" pad="F2"/>
<connect gate="MCU" pin="PD15" pad="F1"/>
<connect gate="MCU" pin="PD2" pad="B4"/>
<connect gate="MCU" pin="PD4" pad="A4"/>
<connect gate="MCU" pin="PD5" pad="C6"/>
<connect gate="MCU" pin="PD6" pad="B5"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD8" pad="H2"/>
<connect gate="MCU" pin="PD9" pad="H3"/>
<connect gate="MCU" pin="PDR_ON" pad="A8"/>
<connect gate="MCU" pin="PE10" pad="F6"/>
<connect gate="MCU" pin="PE11" pad="J5"/>
<connect gate="MCU" pin="PE12" pad="H5"/>
<connect gate="MCU" pin="PE13" pad="G5"/>
<connect gate="MCU" pin="PE14" pad="F5"/>
<connect gate="MCU" pin="PE15" pad="G4"/>
<connect gate="MCU" pin="PE7" pad="G6"/>
<connect gate="MCU" pin="PE8" pad="H6"/>
<connect gate="MCU" pin="PE9" pad="J6"/>
<connect gate="MCU" pin="PI0" pad="C3"/>
<connect gate="MCU" pin="PI1" pad="B2"/>
<connect gate="MCU" pin="VBAT" pad="A10"/>
<connect gate="MCU" pin="VCAP1" pad="F4"/>
<connect gate="MCU" pin="VCAP2" pad="B1"/>
<connect gate="MCU" pin="VDDA" pad="G9"/>
<connect gate="MCU" pin="VSSA" pad="H10"/>
<connect gate="PWR" pin="VDD@1" pad="A1"/>
<connect gate="PWR" pin="VDD@2" pad="B8"/>
<connect gate="PWR" pin="VDD@3" pad="E4"/>
<connect gate="PWR" pin="VDD@4" pad="E6"/>
<connect gate="PWR" pin="VDD@5" pad="F7"/>
<connect gate="PWR" pin="VSS@1" pad="C9"/>
<connect gate="PWR" pin="VSS@2" pad="E5"/>
<connect gate="PWR" pin="VSS@3" pad="E7"/>
<connect gate="PWR" pin="VSS@4" pad="E8"/>
</connects>
<technologies>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F415V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP9"/>
<gate name="PWR" symbol="PWR_VDD6_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="49"/>
<connect gate="MCU" pin="VCAP2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="100"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="28"/>
<connect gate="PWR" pin="VDD@4" pad="11"/>
<connect gate="PWR" pin="VDD@5" pad="50"/>
<connect gate="PWR" pin="VDD@6" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="99"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
<connect gate="PWR" pin="VSS@3" pad="27"/>
<connect gate="PWR" pin="VSS@4" pad="10"/>
</connects>
<technologies>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F415Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD12_VSS9"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PDR_ON" pad="143"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="71"/>
<connect gate="MCU" pin="VCAP2" pad="106"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VSSA" pad="31"/>
<connect gate="PWR" pin="VDD@1" pad="131"/>
<connect gate="PWR" pin="VDD@10" pad="144"/>
<connect gate="PWR" pin="VDD@11" pad="72"/>
<connect gate="PWR" pin="VDD@12" pad="30"/>
<connect gate="PWR" pin="VDD@2" pad="121"/>
<connect gate="PWR" pin="VDD@3" pad="108"/>
<connect gate="PWR" pin="VDD@4" pad="95"/>
<connect gate="PWR" pin="VDD@5" pad="84"/>
<connect gate="PWR" pin="VDD@6" pad="62"/>
<connect gate="PWR" pin="VDD@7" pad="52"/>
<connect gate="PWR" pin="VDD@8" pad="39"/>
<connect gate="PWR" pin="VDD@9" pad="17"/>
<connect gate="PWR" pin="VSS@1" pad="130"/>
<connect gate="PWR" pin="VSS@2" pad="120"/>
<connect gate="PWR" pin="VSS@3" pad="107"/>
<connect gate="PWR" pin="VSS@4" pad="94"/>
<connect gate="PWR" pin="VSS@5" pad="83"/>
<connect gate="PWR" pin="VSS@6" pad="61"/>
<connect gate="PWR" pin="VSS@7" pad="51"/>
<connect gate="PWR" pin="VSS@8" pad="38"/>
<connect gate="PWR" pin="VSS@9" pad="16"/>
</connects>
<technologies>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F417V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP9"/>
<gate name="PWR" symbol="PWR_VDD6_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="49"/>
<connect gate="MCU" pin="VCAP2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="100"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="28"/>
<connect gate="PWR" pin="VDD@4" pad="11"/>
<connect gate="PWR" pin="VDD@5" pad="50"/>
<connect gate="PWR" pin="VDD@6" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="99"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
<connect gate="PWR" pin="VSS@3" pad="27"/>
<connect gate="PWR" pin="VSS@4" pad="10"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F417Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD12_VSS9"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PDR_ON" pad="143"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="71"/>
<connect gate="MCU" pin="VCAP2" pad="106"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VSSA" pad="31"/>
<connect gate="PWR" pin="VDD@1" pad="131"/>
<connect gate="PWR" pin="VDD@10" pad="144"/>
<connect gate="PWR" pin="VDD@11" pad="72"/>
<connect gate="PWR" pin="VDD@12" pad="30"/>
<connect gate="PWR" pin="VDD@2" pad="121"/>
<connect gate="PWR" pin="VDD@3" pad="108"/>
<connect gate="PWR" pin="VDD@4" pad="95"/>
<connect gate="PWR" pin="VDD@5" pad="84"/>
<connect gate="PWR" pin="VDD@6" pad="62"/>
<connect gate="PWR" pin="VDD@7" pad="52"/>
<connect gate="PWR" pin="VDD@8" pad="39"/>
<connect gate="PWR" pin="VDD@9" pad="17"/>
<connect gate="PWR" pin="VSS@1" pad="130"/>
<connect gate="PWR" pin="VSS@2" pad="120"/>
<connect gate="PWR" pin="VSS@3" pad="107"/>
<connect gate="PWR" pin="VSS@4" pad="94"/>
<connect gate="PWR" pin="VSS@5" pad="83"/>
<connect gate="PWR" pin="VSS@6" pad="61"/>
<connect gate="PWR" pin="VSS@7" pad="51"/>
<connect gate="PWR" pin="VSS@8" pad="38"/>
<connect gate="PWR" pin="VSS@9" pad="16"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F417I*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD15_VSS11"/>
</gates>
<devices>
<device name="" package="LQFP176">
<connects>
<connect gate="MCU" pin="BOOT0" pad="166"/>
<connect gate="MCU" pin="BYPASS_REG" pad="48"/>
<connect gate="MCU" pin="NRST" pad="31"/>
<connect gate="MCU" pin="OSC_IN" pad="29"/>
<connect gate="MCU" pin="OSC_OUT" pad="30"/>
<connect gate="MCU" pin="PA0" pad="40"/>
<connect gate="MCU" pin="PA1" pad="41"/>
<connect gate="MCU" pin="PA10" pad="121"/>
<connect gate="MCU" pin="PA11" pad="122"/>
<connect gate="MCU" pin="PA12" pad="123"/>
<connect gate="MCU" pin="PA13" pad="124"/>
<connect gate="MCU" pin="PA14" pad="137"/>
<connect gate="MCU" pin="PA15" pad="138"/>
<connect gate="MCU" pin="PA2" pad="42"/>
<connect gate="MCU" pin="PA3" pad="47"/>
<connect gate="MCU" pin="PA4" pad="50"/>
<connect gate="MCU" pin="PA5" pad="51"/>
<connect gate="MCU" pin="PA6" pad="52"/>
<connect gate="MCU" pin="PA7" pad="53"/>
<connect gate="MCU" pin="PA8" pad="119"/>
<connect gate="MCU" pin="PA9" pad="120"/>
<connect gate="MCU" pin="PB0" pad="56"/>
<connect gate="MCU" pin="PB1" pad="57"/>
<connect gate="MCU" pin="PB10" pad="79"/>
<connect gate="MCU" pin="PB11" pad="80"/>
<connect gate="MCU" pin="PB12" pad="92"/>
<connect gate="MCU" pin="PB13" pad="93"/>
<connect gate="MCU" pin="PB14" pad="94"/>
<connect gate="MCU" pin="PB15" pad="95"/>
<connect gate="MCU" pin="PB2" pad="58"/>
<connect gate="MCU" pin="PB3" pad="161"/>
<connect gate="MCU" pin="PB4" pad="162"/>
<connect gate="MCU" pin="PB5" pad="163"/>
<connect gate="MCU" pin="PB6" pad="164"/>
<connect gate="MCU" pin="PB7" pad="165"/>
<connect gate="MCU" pin="PB8" pad="167"/>
<connect gate="MCU" pin="PB9" pad="168"/>
<connect gate="MCU" pin="PC0" pad="32"/>
<connect gate="MCU" pin="PC1" pad="33"/>
<connect gate="MCU" pin="PC10" pad="139"/>
<connect gate="MCU" pin="PC11" pad="140"/>
<connect gate="MCU" pin="PC12" pad="141"/>
<connect gate="MCU" pin="PC13" pad="8"/>
<connect gate="MCU" pin="PC14" pad="9"/>
<connect gate="MCU" pin="PC15" pad="10"/>
<connect gate="MCU" pin="PC2" pad="34"/>
<connect gate="MCU" pin="PC3" pad="35"/>
<connect gate="MCU" pin="PC4" pad="54"/>
<connect gate="MCU" pin="PC5" pad="55"/>
<connect gate="MCU" pin="PC6" pad="115"/>
<connect gate="MCU" pin="PC7" pad="116"/>
<connect gate="MCU" pin="PC8" pad="117"/>
<connect gate="MCU" pin="PC9" pad="118"/>
<connect gate="MCU" pin="PD0" pad="142"/>
<connect gate="MCU" pin="PD1" pad="143"/>
<connect gate="MCU" pin="PD10" pad="98"/>
<connect gate="MCU" pin="PD11" pad="99"/>
<connect gate="MCU" pin="PD12" pad="100"/>
<connect gate="MCU" pin="PD13" pad="101"/>
<connect gate="MCU" pin="PD14" pad="104"/>
<connect gate="MCU" pin="PD15" pad="105"/>
<connect gate="MCU" pin="PD2" pad="144"/>
<connect gate="MCU" pin="PD3" pad="145"/>
<connect gate="MCU" pin="PD4" pad="146"/>
<connect gate="MCU" pin="PD5" pad="147"/>
<connect gate="MCU" pin="PD6" pad="150"/>
<connect gate="MCU" pin="PD7" pad="151"/>
<connect gate="MCU" pin="PD8" pad="96"/>
<connect gate="MCU" pin="PD9" pad="97"/>
<connect gate="MCU" pin="PDR_ON" pad="171"/>
<connect gate="MCU" pin="PE0" pad="169"/>
<connect gate="MCU" pin="PE1" pad="170"/>
<connect gate="MCU" pin="PE10" pad="73"/>
<connect gate="MCU" pin="PE11" pad="74"/>
<connect gate="MCU" pin="PE12" pad="75"/>
<connect gate="MCU" pin="PE13" pad="76"/>
<connect gate="MCU" pin="PE14" pad="77"/>
<connect gate="MCU" pin="PE15" pad="78"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="68"/>
<connect gate="MCU" pin="PE8" pad="69"/>
<connect gate="MCU" pin="PE9" pad="70"/>
<connect gate="MCU" pin="PF0" pad="16"/>
<connect gate="MCU" pin="PF1" pad="17"/>
<connect gate="MCU" pin="PF10" pad="28"/>
<connect gate="MCU" pin="PF11" pad="59"/>
<connect gate="MCU" pin="PF12" pad="60"/>
<connect gate="MCU" pin="PF13" pad="63"/>
<connect gate="MCU" pin="PF14" pad="64"/>
<connect gate="MCU" pin="PF15" pad="65"/>
<connect gate="MCU" pin="PF2" pad="18"/>
<connect gate="MCU" pin="PF3" pad="19"/>
<connect gate="MCU" pin="PF4" pad="20"/>
<connect gate="MCU" pin="PF5" pad="21"/>
<connect gate="MCU" pin="PF6" pad="24"/>
<connect gate="MCU" pin="PF7" pad="25"/>
<connect gate="MCU" pin="PF8" pad="26"/>
<connect gate="MCU" pin="PF9" pad="27"/>
<connect gate="MCU" pin="PG0" pad="66"/>
<connect gate="MCU" pin="PG1" pad="67"/>
<connect gate="MCU" pin="PG10" pad="153"/>
<connect gate="MCU" pin="PG11" pad="154"/>
<connect gate="MCU" pin="PG12" pad="155"/>
<connect gate="MCU" pin="PG13" pad="156"/>
<connect gate="MCU" pin="PG14" pad="157"/>
<connect gate="MCU" pin="PG15" pad="160"/>
<connect gate="MCU" pin="PG2" pad="106"/>
<connect gate="MCU" pin="PG3" pad="107"/>
<connect gate="MCU" pin="PG4" pad="108"/>
<connect gate="MCU" pin="PG5" pad="109"/>
<connect gate="MCU" pin="PG6" pad="110"/>
<connect gate="MCU" pin="PG7" pad="111"/>
<connect gate="MCU" pin="PG8" pad="112"/>
<connect gate="MCU" pin="PG9" pad="152"/>
<connect gate="MCU" pin="PH10" pad="87"/>
<connect gate="MCU" pin="PH11" pad="88"/>
<connect gate="MCU" pin="PH12" pad="89"/>
<connect gate="MCU" pin="PH13" pad="128"/>
<connect gate="MCU" pin="PH14" pad="129"/>
<connect gate="MCU" pin="PH15" pad="130"/>
<connect gate="MCU" pin="PH2" pad="43"/>
<connect gate="MCU" pin="PH3" pad="44"/>
<connect gate="MCU" pin="PH4" pad="45"/>
<connect gate="MCU" pin="PH5" pad="46"/>
<connect gate="MCU" pin="PH6" pad="83"/>
<connect gate="MCU" pin="PH7" pad="84"/>
<connect gate="MCU" pin="PH8" pad="85"/>
<connect gate="MCU" pin="PH9" pad="86"/>
<connect gate="MCU" pin="PI0" pad="131"/>
<connect gate="MCU" pin="PI1" pad="132"/>
<connect gate="MCU" pin="PI10" pad="12"/>
<connect gate="MCU" pin="PI11" pad="13"/>
<connect gate="MCU" pin="PI2" pad="133"/>
<connect gate="MCU" pin="PI3" pad="134"/>
<connect gate="MCU" pin="PI4" pad="173"/>
<connect gate="MCU" pin="PI5" pad="174"/>
<connect gate="MCU" pin="PI6" pad="175"/>
<connect gate="MCU" pin="PI7" pad="176"/>
<connect gate="MCU" pin="PI8" pad="7"/>
<connect gate="MCU" pin="PI9" pad="11"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="81"/>
<connect gate="MCU" pin="VCAP2" pad="125"/>
<connect gate="MCU" pin="VDDA" pad="39"/>
<connect gate="MCU" pin="VREF+" pad="38"/>
<connect gate="MCU" pin="VSSA" pad="37"/>
<connect gate="PWR" pin="VDD@1" pad="159"/>
<connect gate="PWR" pin="VDD@10" pad="23"/>
<connect gate="PWR" pin="VDD@11" pad="15"/>
<connect gate="PWR" pin="VDD@12" pad="172"/>
<connect gate="PWR" pin="VDD@13" pad="82"/>
<connect gate="PWR" pin="VDD@14" pad="49"/>
<connect gate="PWR" pin="VDD@15" pad="36"/>
<connect gate="PWR" pin="VDD@2" pad="149"/>
<connect gate="PWR" pin="VDD@3" pad="136"/>
<connect gate="PWR" pin="VDD@4" pad="127"/>
<connect gate="PWR" pin="VDD@5" pad="114"/>
<connect gate="PWR" pin="VDD@6" pad="103"/>
<connect gate="PWR" pin="VDD@7" pad="91"/>
<connect gate="PWR" pin="VDD@8" pad="72"/>
<connect gate="PWR" pin="VDD@9" pad="62"/>
<connect gate="PWR" pin="VSS@1" pad="158"/>
<connect gate="PWR" pin="VSS@10" pad="22"/>
<connect gate="PWR" pin="VSS@11" pad="14"/>
<connect gate="PWR" pin="VSS@2" pad="148"/>
<connect gate="PWR" pin="VSS@3" pad="135"/>
<connect gate="PWR" pin="VSS@4" pad="126"/>
<connect gate="PWR" pin="VSS@5" pad="113"/>
<connect gate="PWR" pin="VSS@6" pad="102"/>
<connect gate="PWR" pin="VSS@7" pad="90"/>
<connect gate="PWR" pin="VSS@8" pad="71"/>
<connect gate="PWR" pin="VSS@9" pad="61"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F417I*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
168 MHz maximum frequency&lt;br&gt;
512 to 1024 Kbytes of Flash memory&lt;br&gt;
192 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD14_VSS36"/>
</gates>
<devices>
<device name="" package="UFBGA176+25">
<connects>
<connect gate="MCU" pin="BOOT0" pad="D6"/>
<connect gate="MCU" pin="BYPASS_REG" pad="L4"/>
<connect gate="MCU" pin="NRST" pad="J1"/>
<connect gate="MCU" pin="OSC_IN" pad="G1"/>
<connect gate="MCU" pin="OSC_OUT" pad="H1"/>
<connect gate="MCU" pin="PA0" pad="N3"/>
<connect gate="MCU" pin="PA1" pad="N2"/>
<connect gate="MCU" pin="PA10" pad="D15"/>
<connect gate="MCU" pin="PA11" pad="C15"/>
<connect gate="MCU" pin="PA12" pad="B15"/>
<connect gate="MCU" pin="PA13" pad="A15"/>
<connect gate="MCU" pin="PA14" pad="A14"/>
<connect gate="MCU" pin="PA15" pad="A13"/>
<connect gate="MCU" pin="PA2" pad="P2"/>
<connect gate="MCU" pin="PA3" pad="R2"/>
<connect gate="MCU" pin="PA4" pad="N4"/>
<connect gate="MCU" pin="PA5" pad="P4"/>
<connect gate="MCU" pin="PA6" pad="P3"/>
<connect gate="MCU" pin="PA7" pad="R3"/>
<connect gate="MCU" pin="PA8" pad="F15"/>
<connect gate="MCU" pin="PA9" pad="E15"/>
<connect gate="MCU" pin="PB0" pad="R5"/>
<connect gate="MCU" pin="PB1" pad="R4"/>
<connect gate="MCU" pin="PB10" pad="R12"/>
<connect gate="MCU" pin="PB11" pad="R13"/>
<connect gate="MCU" pin="PB12" pad="P12"/>
<connect gate="MCU" pin="PB13" pad="P13"/>
<connect gate="MCU" pin="PB14" pad="R14"/>
<connect gate="MCU" pin="PB15" pad="R15"/>
<connect gate="MCU" pin="PB2" pad="M6"/>
<connect gate="MCU" pin="PB3" pad="A10"/>
<connect gate="MCU" pin="PB4" pad="A9"/>
<connect gate="MCU" pin="PB5" pad="A6"/>
<connect gate="MCU" pin="PB6" pad="B6"/>
<connect gate="MCU" pin="PB7" pad="B5"/>
<connect gate="MCU" pin="PB8" pad="A5"/>
<connect gate="MCU" pin="PB9" pad="B4"/>
<connect gate="MCU" pin="PC0" pad="M2"/>
<connect gate="MCU" pin="PC1" pad="M3"/>
<connect gate="MCU" pin="PC10" pad="B14"/>
<connect gate="MCU" pin="PC11" pad="B13"/>
<connect gate="MCU" pin="PC12" pad="A12"/>
<connect gate="MCU" pin="PC13" pad="D1"/>
<connect gate="MCU" pin="PC14" pad="E1"/>
<connect gate="MCU" pin="PC15" pad="F1"/>
<connect gate="MCU" pin="PC2" pad="M4"/>
<connect gate="MCU" pin="PC3" pad="M5"/>
<connect gate="MCU" pin="PC4" pad="N5"/>
<connect gate="MCU" pin="PC5" pad="P5"/>
<connect gate="MCU" pin="PC6" pad="H15"/>
<connect gate="MCU" pin="PC7" pad="G15"/>
<connect gate="MCU" pin="PC8" pad="G14"/>
<connect gate="MCU" pin="PC9" pad="F14"/>
<connect gate="MCU" pin="PD0" pad="B12"/>
<connect gate="MCU" pin="PD1" pad="C12"/>
<connect gate="MCU" pin="PD10" pad="N15"/>
<connect gate="MCU" pin="PD11" pad="N14"/>
<connect gate="MCU" pin="PD12" pad="N13"/>
<connect gate="MCU" pin="PD13" pad="M15"/>
<connect gate="MCU" pin="PD14" pad="M14"/>
<connect gate="MCU" pin="PD15" pad="L14"/>
<connect gate="MCU" pin="PD2" pad="D12"/>
<connect gate="MCU" pin="PD3" pad="D11"/>
<connect gate="MCU" pin="PD4" pad="D10"/>
<connect gate="MCU" pin="PD5" pad="C11"/>
<connect gate="MCU" pin="PD6" pad="B11"/>
<connect gate="MCU" pin="PD7" pad="A11"/>
<connect gate="MCU" pin="PD8" pad="P15"/>
<connect gate="MCU" pin="PD9" pad="P14"/>
<connect gate="MCU" pin="PDR_ON" pad="C6"/>
<connect gate="MCU" pin="PE0" pad="A4"/>
<connect gate="MCU" pin="PE1" pad="A3"/>
<connect gate="MCU" pin="PE10" pad="R9"/>
<connect gate="MCU" pin="PE11" pad="P10"/>
<connect gate="MCU" pin="PE12" pad="R10"/>
<connect gate="MCU" pin="PE13" pad="N11"/>
<connect gate="MCU" pin="PE14" pad="P11"/>
<connect gate="MCU" pin="PE15" pad="R11"/>
<connect gate="MCU" pin="PE2" pad="A2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="B2"/>
<connect gate="MCU" pin="PE6" pad="B3"/>
<connect gate="MCU" pin="PE7" pad="R8"/>
<connect gate="MCU" pin="PE8" pad="P8"/>
<connect gate="MCU" pin="PE9" pad="P9"/>
<connect gate="MCU" pin="PF0" pad="E2"/>
<connect gate="MCU" pin="PF1" pad="H3"/>
<connect gate="MCU" pin="PF10" pad="L1"/>
<connect gate="MCU" pin="PF11" pad="R6"/>
<connect gate="MCU" pin="PF12" pad="P6"/>
<connect gate="MCU" pin="PF13" pad="N6"/>
<connect gate="MCU" pin="PF14" pad="R7"/>
<connect gate="MCU" pin="PF15" pad="P7"/>
<connect gate="MCU" pin="PF2" pad="H2"/>
<connect gate="MCU" pin="PF3" pad="J2"/>
<connect gate="MCU" pin="PF4" pad="J3"/>
<connect gate="MCU" pin="PF5" pad="K3"/>
<connect gate="MCU" pin="PF6" pad="K2"/>
<connect gate="MCU" pin="PF7" pad="K1"/>
<connect gate="MCU" pin="PF8" pad="L3"/>
<connect gate="MCU" pin="PF9" pad="L2"/>
<connect gate="MCU" pin="PG0" pad="N7"/>
<connect gate="MCU" pin="PG1" pad="M7"/>
<connect gate="MCU" pin="PG10" pad="B10"/>
<connect gate="MCU" pin="PG11" pad="B9"/>
<connect gate="MCU" pin="PG12" pad="B8"/>
<connect gate="MCU" pin="PG13" pad="A8"/>
<connect gate="MCU" pin="PG14" pad="A7"/>
<connect gate="MCU" pin="PG15" pad="B7"/>
<connect gate="MCU" pin="PG2" pad="L15"/>
<connect gate="MCU" pin="PG3" pad="K15"/>
<connect gate="MCU" pin="PG4" pad="K14"/>
<connect gate="MCU" pin="PG5" pad="K13"/>
<connect gate="MCU" pin="PG6" pad="J15"/>
<connect gate="MCU" pin="PG7" pad="J14"/>
<connect gate="MCU" pin="PG8" pad="H14"/>
<connect gate="MCU" pin="PG9" pad="C10"/>
<connect gate="MCU" pin="PH10" pad="L13"/>
<connect gate="MCU" pin="PH11" pad="L12"/>
<connect gate="MCU" pin="PH12" pad="K12"/>
<connect gate="MCU" pin="PH13" pad="E12"/>
<connect gate="MCU" pin="PH14" pad="E13"/>
<connect gate="MCU" pin="PH15" pad="D13"/>
<connect gate="MCU" pin="PH2" pad="F4"/>
<connect gate="MCU" pin="PH3" pad="G4"/>
<connect gate="MCU" pin="PH4" pad="H4"/>
<connect gate="MCU" pin="PH5" pad="J4"/>
<connect gate="MCU" pin="PH6" pad="M11"/>
<connect gate="MCU" pin="PH7" pad="N12"/>
<connect gate="MCU" pin="PH8" pad="M12"/>
<connect gate="MCU" pin="PH9" pad="M13"/>
<connect gate="MCU" pin="PI0" pad="E14"/>
<connect gate="MCU" pin="PI1" pad="D14"/>
<connect gate="MCU" pin="PI10" pad="E3"/>
<connect gate="MCU" pin="PI11" pad="E4"/>
<connect gate="MCU" pin="PI2" pad="C14"/>
<connect gate="MCU" pin="PI3" pad="C13"/>
<connect gate="MCU" pin="PI4" pad="D4"/>
<connect gate="MCU" pin="PI5" pad="C4"/>
<connect gate="MCU" pin="PI6" pad="C3"/>
<connect gate="MCU" pin="PI7" pad="C2"/>
<connect gate="MCU" pin="PI8" pad="D2"/>
<connect gate="MCU" pin="PI9" pad="D3"/>
<connect gate="MCU" pin="VBAT" pad="C1"/>
<connect gate="MCU" pin="VCAP1" pad="M10"/>
<connect gate="MCU" pin="VCAP2" pad="F13"/>
<connect gate="MCU" pin="VDDA" pad="R1"/>
<connect gate="MCU" pin="VREF+" pad="P1"/>
<connect gate="MCU" pin="VREF-" pad="N1"/>
<connect gate="MCU" pin="VSSA" pad="M1"/>
<connect gate="PWR" pin="VDD@1" pad="C5"/>
<connect gate="PWR" pin="VDD@10" pad="J13"/>
<connect gate="PWR" pin="VDD@11" pad="K4"/>
<connect gate="PWR" pin="VDD@12" pad="N8"/>
<connect gate="PWR" pin="VDD@13" pad="N9"/>
<connect gate="PWR" pin="VDD@14" pad="N10"/>
<connect gate="PWR" pin="VDD@2" pad="C7"/>
<connect gate="PWR" pin="VDD@3" pad="C8"/>
<connect gate="PWR" pin="VDD@4" pad="C9"/>
<connect gate="PWR" pin="VDD@5" pad="F3"/>
<connect gate="PWR" pin="VDD@6" pad="G3"/>
<connect gate="PWR" pin="VDD@7" pad="G13"/>
<connect gate="PWR" pin="VDD@8" pad="H13"/>
<connect gate="PWR" pin="VDD@9" pad="J12"/>
<connect gate="PWR" pin="VSS@1" pad="D5"/>
<connect gate="PWR" pin="VSS@10" pad="M8"/>
<connect gate="PWR" pin="VSS@11" pad="M9"/>
<connect gate="PWR" pin="VSS@12" pad="VSS_1"/>
<connect gate="PWR" pin="VSS@13" pad="VSS_2"/>
<connect gate="PWR" pin="VSS@14" pad="VSS_3"/>
<connect gate="PWR" pin="VSS@15" pad="VSS_4"/>
<connect gate="PWR" pin="VSS@16" pad="VSS_5"/>
<connect gate="PWR" pin="VSS@17" pad="VSS_6"/>
<connect gate="PWR" pin="VSS@18" pad="VSS_7"/>
<connect gate="PWR" pin="VSS@19" pad="VSS_8"/>
<connect gate="PWR" pin="VSS@2" pad="D7"/>
<connect gate="PWR" pin="VSS@20" pad="VSS_9"/>
<connect gate="PWR" pin="VSS@21" pad="VSS_10"/>
<connect gate="PWR" pin="VSS@22" pad="VSS_11"/>
<connect gate="PWR" pin="VSS@23" pad="VSS_12"/>
<connect gate="PWR" pin="VSS@24" pad="VSS_13"/>
<connect gate="PWR" pin="VSS@25" pad="VSS_14"/>
<connect gate="PWR" pin="VSS@26" pad="VSS_15"/>
<connect gate="PWR" pin="VSS@27" pad="VSS_16"/>
<connect gate="PWR" pin="VSS@28" pad="VSS_17"/>
<connect gate="PWR" pin="VSS@29" pad="VSS_18"/>
<connect gate="PWR" pin="VSS@3" pad="D8"/>
<connect gate="PWR" pin="VSS@30" pad="VSS_19"/>
<connect gate="PWR" pin="VSS@31" pad="VSS_20"/>
<connect gate="PWR" pin="VSS@32" pad="VSS_21"/>
<connect gate="PWR" pin="VSS@33" pad="VSS_22"/>
<connect gate="PWR" pin="VSS@34" pad="VSS_23"/>
<connect gate="PWR" pin="VSS@35" pad="VSS_24"/>
<connect gate="PWR" pin="VSS@36" pad="VSS_25"/>
<connect gate="PWR" pin="VSS@4" pad="D9"/>
<connect gate="PWR" pin="VSS@5" pad="F2"/>
<connect gate="PWR" pin="VSS@6" pad="F12"/>
<connect gate="PWR" pin="VSS@7" pad="G2"/>
<connect gate="PWR" pin="VSS@8" pad="G12"/>
<connect gate="PWR" pin="VSS@9" pad="H12"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F427V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP9"/>
<gate name="PWR" symbol="PWR_VDD6_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="49"/>
<connect gate="MCU" pin="VCAP2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="100"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="28"/>
<connect gate="PWR" pin="VDD@4" pad="11"/>
<connect gate="PWR" pin="VDD@5" pad="50"/>
<connect gate="PWR" pin="VDD@6" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="99"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
<connect gate="PWR" pin="VSS@3" pad="27"/>
<connect gate="PWR" pin="VSS@4" pad="10"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F427Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD12_VSS9"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PDR_ON" pad="143"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="71"/>
<connect gate="MCU" pin="VCAP2" pad="106"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VSSA" pad="31"/>
<connect gate="PWR" pin="VDD@1" pad="131"/>
<connect gate="PWR" pin="VDD@10" pad="144"/>
<connect gate="PWR" pin="VDD@11" pad="72"/>
<connect gate="PWR" pin="VDD@12" pad="30"/>
<connect gate="PWR" pin="VDD@2" pad="121"/>
<connect gate="PWR" pin="VDD@3" pad="108"/>
<connect gate="PWR" pin="VDD@4" pad="95"/>
<connect gate="PWR" pin="VDD@5" pad="84"/>
<connect gate="PWR" pin="VDD@6" pad="62"/>
<connect gate="PWR" pin="VDD@7" pad="52"/>
<connect gate="PWR" pin="VDD@8" pad="39"/>
<connect gate="PWR" pin="VDD@9" pad="17"/>
<connect gate="PWR" pin="VSS@1" pad="130"/>
<connect gate="PWR" pin="VSS@2" pad="120"/>
<connect gate="PWR" pin="VSS@3" pad="107"/>
<connect gate="PWR" pin="VSS@4" pad="94"/>
<connect gate="PWR" pin="VSS@5" pad="83"/>
<connect gate="PWR" pin="VSS@6" pad="61"/>
<connect gate="PWR" pin="VSS@7" pad="51"/>
<connect gate="PWR" pin="VSS@8" pad="38"/>
<connect gate="PWR" pin="VSS@9" pad="16"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F427Z*Y" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_143PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD13_VSS6"/>
</gates>
<devices>
<device name="" package="WLCSP143">
<connects>
<connect gate="MCU" pin="BOOT0" pad="C9"/>
<connect gate="MCU" pin="BYPASS_REG" pad="N11"/>
<connect gate="MCU" pin="NRST" pad="H9"/>
<connect gate="MCU" pin="OSC_IN" pad="J11"/>
<connect gate="MCU" pin="OSC_OUT" pad="H10"/>
<connect gate="MCU" pin="PA0" pad="K9"/>
<connect gate="MCU" pin="PA1" pad="K8"/>
<connect gate="MCU" pin="PA10" pad="D5"/>
<connect gate="MCU" pin="PA11" pad="D4"/>
<connect gate="MCU" pin="PA12" pad="E1"/>
<connect gate="MCU" pin="PA13" pad="D3"/>
<connect gate="MCU" pin="PA14" pad="B1"/>
<connect gate="MCU" pin="PA15" pad="C2"/>
<connect gate="MCU" pin="PA2" pad="L9"/>
<connect gate="MCU" pin="PA3" pad="M11"/>
<connect gate="MCU" pin="PA4" pad="M10"/>
<connect gate="MCU" pin="PA5" pad="M9"/>
<connect gate="MCU" pin="PA6" pad="N10"/>
<connect gate="MCU" pin="PA7" pad="L8"/>
<connect gate="MCU" pin="PA8" pad="F1"/>
<connect gate="MCU" pin="PA9" pad="E2"/>
<connect gate="MCU" pin="PB0" pad="N8"/>
<connect gate="MCU" pin="PB1" pad="K7"/>
<connect gate="MCU" pin="PB10" pad="M3"/>
<connect gate="MCU" pin="PB11" pad="N3"/>
<connect gate="MCU" pin="PB12" pad="M2"/>
<connect gate="MCU" pin="PB13" pad="N1"/>
<connect gate="MCU" pin="PB14" pad="K3"/>
<connect gate="MCU" pin="PB15" pad="J3"/>
<connect gate="MCU" pin="PB2" pad="L7"/>
<connect gate="MCU" pin="PB3" pad="B7"/>
<connect gate="MCU" pin="PB4" pad="C7"/>
<connect gate="MCU" pin="PB5" pad="C8"/>
<connect gate="MCU" pin="PB6" pad="A8"/>
<connect gate="MCU" pin="PB7" pad="B8"/>
<connect gate="MCU" pin="PB8" pad="A9"/>
<connect gate="MCU" pin="PB9" pad="B9"/>
<connect gate="MCU" pin="PC0" pad="H8"/>
<connect gate="MCU" pin="PC1" pad="K11"/>
<connect gate="MCU" pin="PC10" pad="A2"/>
<connect gate="MCU" pin="PC11" pad="B2"/>
<connect gate="MCU" pin="PC12" pad="C3"/>
<connect gate="MCU" pin="PC13" pad="D10"/>
<connect gate="MCU" pin="PC14" pad="D11"/>
<connect gate="MCU" pin="PC15" pad="E11"/>
<connect gate="MCU" pin="PC2" pad="J10"/>
<connect gate="MCU" pin="PC3" pad="J9"/>
<connect gate="MCU" pin="PC4" pad="M8"/>
<connect gate="MCU" pin="PC5" pad="N9"/>
<connect gate="MCU" pin="PC6" pad="F2"/>
<connect gate="MCU" pin="PC7" pad="F3"/>
<connect gate="MCU" pin="PC8" pad="E4"/>
<connect gate="MCU" pin="PC9" pad="E3"/>
<connect gate="MCU" pin="PD0" pad="B3"/>
<connect gate="MCU" pin="PD1" pad="C4"/>
<connect gate="MCU" pin="PD10" pad="H4"/>
<connect gate="MCU" pin="PD11" pad="K2"/>
<connect gate="MCU" pin="PD12" pad="H6"/>
<connect gate="MCU" pin="PD13" pad="H5"/>
<connect gate="MCU" pin="PD14" pad="J2"/>
<connect gate="MCU" pin="PD15" pad="K1"/>
<connect gate="MCU" pin="PD2" pad="A3"/>
<connect gate="MCU" pin="PD3" pad="B4"/>
<connect gate="MCU" pin="PD4" pad="B5"/>
<connect gate="MCU" pin="PD5" pad="A4"/>
<connect gate="MCU" pin="PD6" pad="F4"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD8" pad="L2"/>
<connect gate="MCU" pin="PD9" pad="M1"/>
<connect gate="MCU" pin="PDR_ON" pad="A11"/>
<connect gate="MCU" pin="PE0" pad="B10"/>
<connect gate="MCU" pin="PE1" pad="A10"/>
<connect gate="MCU" pin="PE10" pad="J4"/>
<connect gate="MCU" pin="PE11" pad="K4"/>
<connect gate="MCU" pin="PE12" pad="L4"/>
<connect gate="MCU" pin="PE13" pad="N4"/>
<connect gate="MCU" pin="PE14" pad="M4"/>
<connect gate="MCU" pin="PE15" pad="L3"/>
<connect gate="MCU" pin="PE2" pad="D8"/>
<connect gate="MCU" pin="PE3" pad="C10"/>
<connect gate="MCU" pin="PE4" pad="B11"/>
<connect gate="MCU" pin="PE5" pad="D9"/>
<connect gate="MCU" pin="PE6" pad="E8"/>
<connect gate="MCU" pin="PE7" pad="L5"/>
<connect gate="MCU" pin="PE8" pad="M5"/>
<connect gate="MCU" pin="PE9" pad="N5"/>
<connect gate="MCU" pin="PF0" pad="F11"/>
<connect gate="MCU" pin="PF1" pad="E9"/>
<connect gate="MCU" pin="PF10" pad="G9"/>
<connect gate="MCU" pin="PF11" pad="M7"/>
<connect gate="MCU" pin="PF12" pad="N7"/>
<connect gate="MCU" pin="PF13" pad="K6"/>
<connect gate="MCU" pin="PF14" pad="L6"/>
<connect gate="MCU" pin="PF15" pad="M6"/>
<connect gate="MCU" pin="PF2" pad="F10"/>
<connect gate="MCU" pin="PF3" pad="G11"/>
<connect gate="MCU" pin="PF4" pad="F9"/>
<connect gate="MCU" pin="PF5" pad="F8"/>
<connect gate="MCU" pin="PF6" pad="G10"/>
<connect gate="MCU" pin="PF7" pad="F7"/>
<connect gate="MCU" pin="PF8" pad="H11"/>
<connect gate="MCU" pin="PF9" pad="G8"/>
<connect gate="MCU" pin="PG0" pad="N6"/>
<connect gate="MCU" pin="PG1" pad="K5"/>
<connect gate="MCU" pin="PG10" pad="C6"/>
<connect gate="MCU" pin="PG11" pad="B6"/>
<connect gate="MCU" pin="PG12" pad="A6"/>
<connect gate="MCU" pin="PG13" pad="D6"/>
<connect gate="MCU" pin="PG14" pad="F6"/>
<connect gate="MCU" pin="PG15" pad="A7"/>
<connect gate="MCU" pin="PG2" pad="J1"/>
<connect gate="MCU" pin="PG3" pad="G3"/>
<connect gate="MCU" pin="PG4" pad="G5"/>
<connect gate="MCU" pin="PG5" pad="G6"/>
<connect gate="MCU" pin="PG6" pad="G4"/>
<connect gate="MCU" pin="PG7" pad="H1"/>
<connect gate="MCU" pin="PG8" pad="G2"/>
<connect gate="MCU" pin="PG9" pad="E5"/>
<connect gate="MCU" pin="VBAT" pad="C11"/>
<connect gate="MCU" pin="VCAP1" pad="N2"/>
<connect gate="MCU" pin="VCAP2" pad="D1"/>
<connect gate="MCU" pin="VDDA" pad="L10"/>
<connect gate="MCU" pin="VREF+" pad="L11"/>
<connect gate="MCU" pin="VSSA" pad="K10"/>
<connect gate="PWR" pin="VDD@1" pad="A1"/>
<connect gate="PWR" pin="VDD@10" pad="J6"/>
<connect gate="PWR" pin="VDD@11" pad="J7"/>
<connect gate="PWR" pin="VDD@12" pad="J8"/>
<connect gate="PWR" pin="VDD@13" pad="L1"/>
<connect gate="PWR" pin="VDD@2" pad="C1"/>
<connect gate="PWR" pin="VDD@3" pad="C5"/>
<connect gate="PWR" pin="VDD@4" pad="D7"/>
<connect gate="PWR" pin="VDD@5" pad="E6"/>
<connect gate="PWR" pin="VDD@6" pad="E10"/>
<connect gate="PWR" pin="VDD@7" pad="G1"/>
<connect gate="PWR" pin="VDD@8" pad="G7"/>
<connect gate="PWR" pin="VDD@9" pad="J5"/>
<connect gate="PWR" pin="VSS@1" pad="D2"/>
<connect gate="PWR" pin="VSS@2" pad="E7"/>
<connect gate="PWR" pin="VSS@3" pad="F5"/>
<connect gate="PWR" pin="VSS@4" pad="H2"/>
<connect gate="PWR" pin="VSS@5" pad="H3"/>
<connect gate="PWR" pin="VSS@6" pad="H7"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F427I*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD15_VSS11"/>
</gates>
<devices>
<device name="" package="LQFP176">
<connects>
<connect gate="MCU" pin="BOOT0" pad="166"/>
<connect gate="MCU" pin="BYPASS_REG" pad="48"/>
<connect gate="MCU" pin="NRST" pad="31"/>
<connect gate="MCU" pin="OSC_IN" pad="29"/>
<connect gate="MCU" pin="OSC_OUT" pad="30"/>
<connect gate="MCU" pin="PA0" pad="40"/>
<connect gate="MCU" pin="PA1" pad="41"/>
<connect gate="MCU" pin="PA10" pad="121"/>
<connect gate="MCU" pin="PA11" pad="122"/>
<connect gate="MCU" pin="PA12" pad="123"/>
<connect gate="MCU" pin="PA13" pad="124"/>
<connect gate="MCU" pin="PA14" pad="137"/>
<connect gate="MCU" pin="PA15" pad="138"/>
<connect gate="MCU" pin="PA2" pad="42"/>
<connect gate="MCU" pin="PA3" pad="47"/>
<connect gate="MCU" pin="PA4" pad="50"/>
<connect gate="MCU" pin="PA5" pad="51"/>
<connect gate="MCU" pin="PA6" pad="52"/>
<connect gate="MCU" pin="PA7" pad="53"/>
<connect gate="MCU" pin="PA8" pad="119"/>
<connect gate="MCU" pin="PA9" pad="120"/>
<connect gate="MCU" pin="PB0" pad="56"/>
<connect gate="MCU" pin="PB1" pad="57"/>
<connect gate="MCU" pin="PB10" pad="79"/>
<connect gate="MCU" pin="PB11" pad="80"/>
<connect gate="MCU" pin="PB12" pad="92"/>
<connect gate="MCU" pin="PB13" pad="93"/>
<connect gate="MCU" pin="PB14" pad="94"/>
<connect gate="MCU" pin="PB15" pad="95"/>
<connect gate="MCU" pin="PB2" pad="58"/>
<connect gate="MCU" pin="PB3" pad="161"/>
<connect gate="MCU" pin="PB4" pad="162"/>
<connect gate="MCU" pin="PB5" pad="163"/>
<connect gate="MCU" pin="PB6" pad="164"/>
<connect gate="MCU" pin="PB7" pad="165"/>
<connect gate="MCU" pin="PB8" pad="167"/>
<connect gate="MCU" pin="PB9" pad="168"/>
<connect gate="MCU" pin="PC0" pad="32"/>
<connect gate="MCU" pin="PC1" pad="33"/>
<connect gate="MCU" pin="PC10" pad="139"/>
<connect gate="MCU" pin="PC11" pad="140"/>
<connect gate="MCU" pin="PC12" pad="141"/>
<connect gate="MCU" pin="PC13" pad="8"/>
<connect gate="MCU" pin="PC14" pad="9"/>
<connect gate="MCU" pin="PC15" pad="10"/>
<connect gate="MCU" pin="PC2" pad="34"/>
<connect gate="MCU" pin="PC3" pad="35"/>
<connect gate="MCU" pin="PC4" pad="54"/>
<connect gate="MCU" pin="PC5" pad="55"/>
<connect gate="MCU" pin="PC6" pad="115"/>
<connect gate="MCU" pin="PC7" pad="116"/>
<connect gate="MCU" pin="PC8" pad="117"/>
<connect gate="MCU" pin="PC9" pad="118"/>
<connect gate="MCU" pin="PD0" pad="142"/>
<connect gate="MCU" pin="PD1" pad="143"/>
<connect gate="MCU" pin="PD10" pad="98"/>
<connect gate="MCU" pin="PD11" pad="99"/>
<connect gate="MCU" pin="PD12" pad="100"/>
<connect gate="MCU" pin="PD13" pad="101"/>
<connect gate="MCU" pin="PD14" pad="104"/>
<connect gate="MCU" pin="PD15" pad="105"/>
<connect gate="MCU" pin="PD2" pad="144"/>
<connect gate="MCU" pin="PD3" pad="145"/>
<connect gate="MCU" pin="PD4" pad="146"/>
<connect gate="MCU" pin="PD5" pad="147"/>
<connect gate="MCU" pin="PD6" pad="150"/>
<connect gate="MCU" pin="PD7" pad="151"/>
<connect gate="MCU" pin="PD8" pad="96"/>
<connect gate="MCU" pin="PD9" pad="97"/>
<connect gate="MCU" pin="PDR_ON" pad="171"/>
<connect gate="MCU" pin="PE0" pad="169"/>
<connect gate="MCU" pin="PE1" pad="170"/>
<connect gate="MCU" pin="PE10" pad="73"/>
<connect gate="MCU" pin="PE11" pad="74"/>
<connect gate="MCU" pin="PE12" pad="75"/>
<connect gate="MCU" pin="PE13" pad="76"/>
<connect gate="MCU" pin="PE14" pad="77"/>
<connect gate="MCU" pin="PE15" pad="78"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="68"/>
<connect gate="MCU" pin="PE8" pad="69"/>
<connect gate="MCU" pin="PE9" pad="70"/>
<connect gate="MCU" pin="PF0" pad="16"/>
<connect gate="MCU" pin="PF1" pad="17"/>
<connect gate="MCU" pin="PF10" pad="28"/>
<connect gate="MCU" pin="PF11" pad="59"/>
<connect gate="MCU" pin="PF12" pad="60"/>
<connect gate="MCU" pin="PF13" pad="63"/>
<connect gate="MCU" pin="PF14" pad="64"/>
<connect gate="MCU" pin="PF15" pad="65"/>
<connect gate="MCU" pin="PF2" pad="18"/>
<connect gate="MCU" pin="PF3" pad="19"/>
<connect gate="MCU" pin="PF4" pad="20"/>
<connect gate="MCU" pin="PF5" pad="21"/>
<connect gate="MCU" pin="PF6" pad="24"/>
<connect gate="MCU" pin="PF7" pad="25"/>
<connect gate="MCU" pin="PF8" pad="26"/>
<connect gate="MCU" pin="PF9" pad="27"/>
<connect gate="MCU" pin="PG0" pad="66"/>
<connect gate="MCU" pin="PG1" pad="67"/>
<connect gate="MCU" pin="PG10" pad="153"/>
<connect gate="MCU" pin="PG11" pad="154"/>
<connect gate="MCU" pin="PG12" pad="155"/>
<connect gate="MCU" pin="PG13" pad="156"/>
<connect gate="MCU" pin="PG14" pad="157"/>
<connect gate="MCU" pin="PG15" pad="160"/>
<connect gate="MCU" pin="PG2" pad="106"/>
<connect gate="MCU" pin="PG3" pad="107"/>
<connect gate="MCU" pin="PG4" pad="108"/>
<connect gate="MCU" pin="PG5" pad="109"/>
<connect gate="MCU" pin="PG6" pad="110"/>
<connect gate="MCU" pin="PG7" pad="111"/>
<connect gate="MCU" pin="PG8" pad="112"/>
<connect gate="MCU" pin="PG9" pad="152"/>
<connect gate="MCU" pin="PH10" pad="87"/>
<connect gate="MCU" pin="PH11" pad="88"/>
<connect gate="MCU" pin="PH12" pad="89"/>
<connect gate="MCU" pin="PH13" pad="128"/>
<connect gate="MCU" pin="PH14" pad="129"/>
<connect gate="MCU" pin="PH15" pad="130"/>
<connect gate="MCU" pin="PH2" pad="43"/>
<connect gate="MCU" pin="PH3" pad="44"/>
<connect gate="MCU" pin="PH4" pad="45"/>
<connect gate="MCU" pin="PH5" pad="46"/>
<connect gate="MCU" pin="PH6" pad="83"/>
<connect gate="MCU" pin="PH7" pad="84"/>
<connect gate="MCU" pin="PH8" pad="85"/>
<connect gate="MCU" pin="PH9" pad="86"/>
<connect gate="MCU" pin="PI0" pad="131"/>
<connect gate="MCU" pin="PI1" pad="132"/>
<connect gate="MCU" pin="PI10" pad="12"/>
<connect gate="MCU" pin="PI11" pad="13"/>
<connect gate="MCU" pin="PI2" pad="133"/>
<connect gate="MCU" pin="PI3" pad="134"/>
<connect gate="MCU" pin="PI4" pad="173"/>
<connect gate="MCU" pin="PI5" pad="174"/>
<connect gate="MCU" pin="PI6" pad="175"/>
<connect gate="MCU" pin="PI7" pad="176"/>
<connect gate="MCU" pin="PI8" pad="7"/>
<connect gate="MCU" pin="PI9" pad="11"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="81"/>
<connect gate="MCU" pin="VCAP2" pad="125"/>
<connect gate="MCU" pin="VDDA" pad="39"/>
<connect gate="MCU" pin="VREF+" pad="38"/>
<connect gate="MCU" pin="VSSA" pad="37"/>
<connect gate="PWR" pin="VDD@1" pad="159"/>
<connect gate="PWR" pin="VDD@10" pad="23"/>
<connect gate="PWR" pin="VDD@11" pad="15"/>
<connect gate="PWR" pin="VDD@12" pad="172"/>
<connect gate="PWR" pin="VDD@13" pad="82"/>
<connect gate="PWR" pin="VDD@14" pad="49"/>
<connect gate="PWR" pin="VDD@15" pad="36"/>
<connect gate="PWR" pin="VDD@2" pad="149"/>
<connect gate="PWR" pin="VDD@3" pad="136"/>
<connect gate="PWR" pin="VDD@4" pad="127"/>
<connect gate="PWR" pin="VDD@5" pad="114"/>
<connect gate="PWR" pin="VDD@6" pad="103"/>
<connect gate="PWR" pin="VDD@7" pad="91"/>
<connect gate="PWR" pin="VDD@8" pad="72"/>
<connect gate="PWR" pin="VDD@9" pad="62"/>
<connect gate="PWR" pin="VSS@1" pad="158"/>
<connect gate="PWR" pin="VSS@10" pad="22"/>
<connect gate="PWR" pin="VSS@11" pad="14"/>
<connect gate="PWR" pin="VSS@2" pad="148"/>
<connect gate="PWR" pin="VSS@3" pad="135"/>
<connect gate="PWR" pin="VSS@4" pad="126"/>
<connect gate="PWR" pin="VSS@5" pad="113"/>
<connect gate="PWR" pin="VSS@6" pad="102"/>
<connect gate="PWR" pin="VSS@7" pad="90"/>
<connect gate="PWR" pin="VSS@8" pad="71"/>
<connect gate="PWR" pin="VSS@9" pad="61"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F427I*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD14_VSS36"/>
</gates>
<devices>
<device name="" package="UFBGA176+25">
<connects>
<connect gate="MCU" pin="BOOT0" pad="D6"/>
<connect gate="MCU" pin="BYPASS_REG" pad="L4"/>
<connect gate="MCU" pin="NRST" pad="J1"/>
<connect gate="MCU" pin="OSC_IN" pad="G1"/>
<connect gate="MCU" pin="OSC_OUT" pad="H1"/>
<connect gate="MCU" pin="PA0" pad="N3"/>
<connect gate="MCU" pin="PA1" pad="N2"/>
<connect gate="MCU" pin="PA10" pad="D15"/>
<connect gate="MCU" pin="PA11" pad="C15"/>
<connect gate="MCU" pin="PA12" pad="B15"/>
<connect gate="MCU" pin="PA13" pad="A15"/>
<connect gate="MCU" pin="PA14" pad="A14"/>
<connect gate="MCU" pin="PA15" pad="A13"/>
<connect gate="MCU" pin="PA2" pad="P2"/>
<connect gate="MCU" pin="PA3" pad="R2"/>
<connect gate="MCU" pin="PA4" pad="N4"/>
<connect gate="MCU" pin="PA5" pad="P4"/>
<connect gate="MCU" pin="PA6" pad="P3"/>
<connect gate="MCU" pin="PA7" pad="R3"/>
<connect gate="MCU" pin="PA8" pad="F15"/>
<connect gate="MCU" pin="PA9" pad="E15"/>
<connect gate="MCU" pin="PB0" pad="R5"/>
<connect gate="MCU" pin="PB1" pad="R4"/>
<connect gate="MCU" pin="PB10" pad="R12"/>
<connect gate="MCU" pin="PB11" pad="R13"/>
<connect gate="MCU" pin="PB12" pad="P12"/>
<connect gate="MCU" pin="PB13" pad="P13"/>
<connect gate="MCU" pin="PB14" pad="R14"/>
<connect gate="MCU" pin="PB15" pad="R15"/>
<connect gate="MCU" pin="PB2" pad="M6"/>
<connect gate="MCU" pin="PB3" pad="A10"/>
<connect gate="MCU" pin="PB4" pad="A9"/>
<connect gate="MCU" pin="PB5" pad="A6"/>
<connect gate="MCU" pin="PB6" pad="B6"/>
<connect gate="MCU" pin="PB7" pad="B5"/>
<connect gate="MCU" pin="PB8" pad="A5"/>
<connect gate="MCU" pin="PB9" pad="B4"/>
<connect gate="MCU" pin="PC0" pad="M2"/>
<connect gate="MCU" pin="PC1" pad="M3"/>
<connect gate="MCU" pin="PC10" pad="B14"/>
<connect gate="MCU" pin="PC11" pad="B13"/>
<connect gate="MCU" pin="PC12" pad="A12"/>
<connect gate="MCU" pin="PC13" pad="D1"/>
<connect gate="MCU" pin="PC14" pad="E1"/>
<connect gate="MCU" pin="PC15" pad="F1"/>
<connect gate="MCU" pin="PC2" pad="M4"/>
<connect gate="MCU" pin="PC3" pad="M5"/>
<connect gate="MCU" pin="PC4" pad="N5"/>
<connect gate="MCU" pin="PC5" pad="P5"/>
<connect gate="MCU" pin="PC6" pad="H15"/>
<connect gate="MCU" pin="PC7" pad="G15"/>
<connect gate="MCU" pin="PC8" pad="G14"/>
<connect gate="MCU" pin="PC9" pad="F14"/>
<connect gate="MCU" pin="PD0" pad="B12"/>
<connect gate="MCU" pin="PD1" pad="C12"/>
<connect gate="MCU" pin="PD10" pad="N15"/>
<connect gate="MCU" pin="PD11" pad="N14"/>
<connect gate="MCU" pin="PD12" pad="N13"/>
<connect gate="MCU" pin="PD13" pad="M15"/>
<connect gate="MCU" pin="PD14" pad="M14"/>
<connect gate="MCU" pin="PD15" pad="L14"/>
<connect gate="MCU" pin="PD2" pad="D12"/>
<connect gate="MCU" pin="PD3" pad="D11"/>
<connect gate="MCU" pin="PD4" pad="D10"/>
<connect gate="MCU" pin="PD5" pad="C11"/>
<connect gate="MCU" pin="PD6" pad="B11"/>
<connect gate="MCU" pin="PD7" pad="A11"/>
<connect gate="MCU" pin="PD8" pad="P15"/>
<connect gate="MCU" pin="PD9" pad="P14"/>
<connect gate="MCU" pin="PDR_ON" pad="C6"/>
<connect gate="MCU" pin="PE0" pad="A4"/>
<connect gate="MCU" pin="PE1" pad="A3"/>
<connect gate="MCU" pin="PE10" pad="R9"/>
<connect gate="MCU" pin="PE11" pad="P10"/>
<connect gate="MCU" pin="PE12" pad="R10"/>
<connect gate="MCU" pin="PE13" pad="N11"/>
<connect gate="MCU" pin="PE14" pad="P11"/>
<connect gate="MCU" pin="PE15" pad="R11"/>
<connect gate="MCU" pin="PE2" pad="A2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="B2"/>
<connect gate="MCU" pin="PE6" pad="B3"/>
<connect gate="MCU" pin="PE7" pad="R8"/>
<connect gate="MCU" pin="PE8" pad="P8"/>
<connect gate="MCU" pin="PE9" pad="P9"/>
<connect gate="MCU" pin="PF0" pad="E2"/>
<connect gate="MCU" pin="PF1" pad="H3"/>
<connect gate="MCU" pin="PF10" pad="L1"/>
<connect gate="MCU" pin="PF11" pad="R6"/>
<connect gate="MCU" pin="PF12" pad="P6"/>
<connect gate="MCU" pin="PF13" pad="N6"/>
<connect gate="MCU" pin="PF14" pad="R7"/>
<connect gate="MCU" pin="PF15" pad="P7"/>
<connect gate="MCU" pin="PF2" pad="H2"/>
<connect gate="MCU" pin="PF3" pad="J2"/>
<connect gate="MCU" pin="PF4" pad="J3"/>
<connect gate="MCU" pin="PF5" pad="K3"/>
<connect gate="MCU" pin="PF6" pad="K2"/>
<connect gate="MCU" pin="PF7" pad="K1"/>
<connect gate="MCU" pin="PF8" pad="L3"/>
<connect gate="MCU" pin="PF9" pad="L2"/>
<connect gate="MCU" pin="PG0" pad="N7"/>
<connect gate="MCU" pin="PG1" pad="M7"/>
<connect gate="MCU" pin="PG10" pad="B10"/>
<connect gate="MCU" pin="PG11" pad="B9"/>
<connect gate="MCU" pin="PG12" pad="B8"/>
<connect gate="MCU" pin="PG13" pad="A8"/>
<connect gate="MCU" pin="PG14" pad="A7"/>
<connect gate="MCU" pin="PG15" pad="B7"/>
<connect gate="MCU" pin="PG2" pad="L15"/>
<connect gate="MCU" pin="PG3" pad="K15"/>
<connect gate="MCU" pin="PG4" pad="K14"/>
<connect gate="MCU" pin="PG5" pad="K13"/>
<connect gate="MCU" pin="PG6" pad="J15"/>
<connect gate="MCU" pin="PG7" pad="J14"/>
<connect gate="MCU" pin="PG8" pad="H14"/>
<connect gate="MCU" pin="PG9" pad="C10"/>
<connect gate="MCU" pin="PH10" pad="L13"/>
<connect gate="MCU" pin="PH11" pad="L12"/>
<connect gate="MCU" pin="PH12" pad="K12"/>
<connect gate="MCU" pin="PH13" pad="E12"/>
<connect gate="MCU" pin="PH14" pad="E13"/>
<connect gate="MCU" pin="PH15" pad="D13"/>
<connect gate="MCU" pin="PH2" pad="F4"/>
<connect gate="MCU" pin="PH3" pad="G4"/>
<connect gate="MCU" pin="PH4" pad="H4"/>
<connect gate="MCU" pin="PH5" pad="J4"/>
<connect gate="MCU" pin="PH6" pad="M11"/>
<connect gate="MCU" pin="PH7" pad="N12"/>
<connect gate="MCU" pin="PH8" pad="M12"/>
<connect gate="MCU" pin="PH9" pad="M13"/>
<connect gate="MCU" pin="PI0" pad="E14"/>
<connect gate="MCU" pin="PI1" pad="D14"/>
<connect gate="MCU" pin="PI10" pad="E3"/>
<connect gate="MCU" pin="PI11" pad="E4"/>
<connect gate="MCU" pin="PI2" pad="C14"/>
<connect gate="MCU" pin="PI3" pad="C13"/>
<connect gate="MCU" pin="PI4" pad="D4"/>
<connect gate="MCU" pin="PI5" pad="C4"/>
<connect gate="MCU" pin="PI6" pad="C3"/>
<connect gate="MCU" pin="PI7" pad="C2"/>
<connect gate="MCU" pin="PI8" pad="D2"/>
<connect gate="MCU" pin="PI9" pad="D3"/>
<connect gate="MCU" pin="VBAT" pad="C1"/>
<connect gate="MCU" pin="VCAP1" pad="M10"/>
<connect gate="MCU" pin="VCAP2" pad="F13"/>
<connect gate="MCU" pin="VDDA" pad="R1"/>
<connect gate="MCU" pin="VREF+" pad="P1"/>
<connect gate="MCU" pin="VREF-" pad="N1"/>
<connect gate="MCU" pin="VSSA" pad="M1"/>
<connect gate="PWR" pin="VDD@1" pad="C5"/>
<connect gate="PWR" pin="VDD@10" pad="J13"/>
<connect gate="PWR" pin="VDD@11" pad="K4"/>
<connect gate="PWR" pin="VDD@12" pad="N8"/>
<connect gate="PWR" pin="VDD@13" pad="N9"/>
<connect gate="PWR" pin="VDD@14" pad="N10"/>
<connect gate="PWR" pin="VDD@2" pad="C7"/>
<connect gate="PWR" pin="VDD@3" pad="C8"/>
<connect gate="PWR" pin="VDD@4" pad="C9"/>
<connect gate="PWR" pin="VDD@5" pad="F3"/>
<connect gate="PWR" pin="VDD@6" pad="G3"/>
<connect gate="PWR" pin="VDD@7" pad="G13"/>
<connect gate="PWR" pin="VDD@8" pad="H13"/>
<connect gate="PWR" pin="VDD@9" pad="J12"/>
<connect gate="PWR" pin="VSS@1" pad="D5"/>
<connect gate="PWR" pin="VSS@10" pad="M8"/>
<connect gate="PWR" pin="VSS@11" pad="M9"/>
<connect gate="PWR" pin="VSS@12" pad="VSS_1"/>
<connect gate="PWR" pin="VSS@13" pad="VSS_2"/>
<connect gate="PWR" pin="VSS@14" pad="VSS_3"/>
<connect gate="PWR" pin="VSS@15" pad="VSS_4"/>
<connect gate="PWR" pin="VSS@16" pad="VSS_5"/>
<connect gate="PWR" pin="VSS@17" pad="VSS_6"/>
<connect gate="PWR" pin="VSS@18" pad="VSS_7"/>
<connect gate="PWR" pin="VSS@19" pad="VSS_8"/>
<connect gate="PWR" pin="VSS@2" pad="D7"/>
<connect gate="PWR" pin="VSS@20" pad="VSS_9"/>
<connect gate="PWR" pin="VSS@21" pad="VSS_10"/>
<connect gate="PWR" pin="VSS@22" pad="VSS_11"/>
<connect gate="PWR" pin="VSS@23" pad="VSS_12"/>
<connect gate="PWR" pin="VSS@24" pad="VSS_13"/>
<connect gate="PWR" pin="VSS@25" pad="VSS_14"/>
<connect gate="PWR" pin="VSS@26" pad="VSS_15"/>
<connect gate="PWR" pin="VSS@27" pad="VSS_16"/>
<connect gate="PWR" pin="VSS@28" pad="VSS_17"/>
<connect gate="PWR" pin="VSS@29" pad="VSS_18"/>
<connect gate="PWR" pin="VSS@3" pad="D8"/>
<connect gate="PWR" pin="VSS@30" pad="VSS_19"/>
<connect gate="PWR" pin="VSS@31" pad="VSS_20"/>
<connect gate="PWR" pin="VSS@32" pad="VSS_21"/>
<connect gate="PWR" pin="VSS@33" pad="VSS_22"/>
<connect gate="PWR" pin="VSS@34" pad="VSS_23"/>
<connect gate="PWR" pin="VSS@35" pad="VSS_24"/>
<connect gate="PWR" pin="VSS@36" pad="VSS_25"/>
<connect gate="PWR" pin="VSS@4" pad="D9"/>
<connect gate="PWR" pin="VSS@5" pad="F2"/>
<connect gate="PWR" pin="VSS@6" pad="F12"/>
<connect gate="PWR" pin="VSS@7" pad="G2"/>
<connect gate="PWR" pin="VSS@8" pad="G12"/>
<connect gate="PWR" pin="VSS@9" pad="H12"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F429V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP9"/>
<gate name="PWR" symbol="PWR_VDD6_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="49"/>
<connect gate="MCU" pin="VCAP2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="100"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="28"/>
<connect gate="PWR" pin="VDD@4" pad="11"/>
<connect gate="PWR" pin="VDD@5" pad="50"/>
<connect gate="PWR" pin="VDD@6" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="99"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
<connect gate="PWR" pin="VSS@3" pad="27"/>
<connect gate="PWR" pin="VSS@4" pad="10"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F429Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD12_VSS9"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PDR_ON" pad="143"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="71"/>
<connect gate="MCU" pin="VCAP2" pad="106"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VSSA" pad="31"/>
<connect gate="PWR" pin="VDD@1" pad="131"/>
<connect gate="PWR" pin="VDD@10" pad="144"/>
<connect gate="PWR" pin="VDD@11" pad="72"/>
<connect gate="PWR" pin="VDD@12" pad="30"/>
<connect gate="PWR" pin="VDD@2" pad="121"/>
<connect gate="PWR" pin="VDD@3" pad="108"/>
<connect gate="PWR" pin="VDD@4" pad="95"/>
<connect gate="PWR" pin="VDD@5" pad="84"/>
<connect gate="PWR" pin="VDD@6" pad="62"/>
<connect gate="PWR" pin="VDD@7" pad="52"/>
<connect gate="PWR" pin="VDD@8" pad="39"/>
<connect gate="PWR" pin="VDD@9" pad="17"/>
<connect gate="PWR" pin="VSS@1" pad="130"/>
<connect gate="PWR" pin="VSS@2" pad="120"/>
<connect gate="PWR" pin="VSS@3" pad="107"/>
<connect gate="PWR" pin="VSS@4" pad="94"/>
<connect gate="PWR" pin="VSS@5" pad="83"/>
<connect gate="PWR" pin="VSS@6" pad="61"/>
<connect gate="PWR" pin="VSS@7" pad="51"/>
<connect gate="PWR" pin="VSS@8" pad="38"/>
<connect gate="PWR" pin="VSS@9" pad="16"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F429Z*Y" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_143PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD13_VSS6"/>
</gates>
<devices>
<device name="" package="WLCSP143">
<connects>
<connect gate="MCU" pin="BOOT0" pad="C9"/>
<connect gate="MCU" pin="BYPASS_REG" pad="N11"/>
<connect gate="MCU" pin="NRST" pad="H9"/>
<connect gate="MCU" pin="OSC_IN" pad="J11"/>
<connect gate="MCU" pin="OSC_OUT" pad="H10"/>
<connect gate="MCU" pin="PA0" pad="K9"/>
<connect gate="MCU" pin="PA1" pad="K8"/>
<connect gate="MCU" pin="PA10" pad="D5"/>
<connect gate="MCU" pin="PA11" pad="D4"/>
<connect gate="MCU" pin="PA12" pad="E1"/>
<connect gate="MCU" pin="PA13" pad="D3"/>
<connect gate="MCU" pin="PA14" pad="B1"/>
<connect gate="MCU" pin="PA15" pad="C2"/>
<connect gate="MCU" pin="PA2" pad="L9"/>
<connect gate="MCU" pin="PA3" pad="M11"/>
<connect gate="MCU" pin="PA4" pad="M10"/>
<connect gate="MCU" pin="PA5" pad="M9"/>
<connect gate="MCU" pin="PA6" pad="N10"/>
<connect gate="MCU" pin="PA7" pad="L8"/>
<connect gate="MCU" pin="PA8" pad="F1"/>
<connect gate="MCU" pin="PA9" pad="E2"/>
<connect gate="MCU" pin="PB0" pad="N8"/>
<connect gate="MCU" pin="PB1" pad="K7"/>
<connect gate="MCU" pin="PB10" pad="M3"/>
<connect gate="MCU" pin="PB11" pad="N3"/>
<connect gate="MCU" pin="PB12" pad="M2"/>
<connect gate="MCU" pin="PB13" pad="N1"/>
<connect gate="MCU" pin="PB14" pad="K3"/>
<connect gate="MCU" pin="PB15" pad="J3"/>
<connect gate="MCU" pin="PB2" pad="L7"/>
<connect gate="MCU" pin="PB3" pad="B7"/>
<connect gate="MCU" pin="PB4" pad="C7"/>
<connect gate="MCU" pin="PB5" pad="C8"/>
<connect gate="MCU" pin="PB6" pad="A8"/>
<connect gate="MCU" pin="PB7" pad="B8"/>
<connect gate="MCU" pin="PB8" pad="A9"/>
<connect gate="MCU" pin="PB9" pad="B9"/>
<connect gate="MCU" pin="PC0" pad="H8"/>
<connect gate="MCU" pin="PC1" pad="K11"/>
<connect gate="MCU" pin="PC10" pad="A2"/>
<connect gate="MCU" pin="PC11" pad="B2"/>
<connect gate="MCU" pin="PC12" pad="C3"/>
<connect gate="MCU" pin="PC13" pad="D10"/>
<connect gate="MCU" pin="PC14" pad="D11"/>
<connect gate="MCU" pin="PC15" pad="E11"/>
<connect gate="MCU" pin="PC2" pad="J10"/>
<connect gate="MCU" pin="PC3" pad="J9"/>
<connect gate="MCU" pin="PC4" pad="M8"/>
<connect gate="MCU" pin="PC5" pad="N9"/>
<connect gate="MCU" pin="PC6" pad="F2"/>
<connect gate="MCU" pin="PC7" pad="F3"/>
<connect gate="MCU" pin="PC8" pad="E4"/>
<connect gate="MCU" pin="PC9" pad="E3"/>
<connect gate="MCU" pin="PD0" pad="B3"/>
<connect gate="MCU" pin="PD1" pad="C4"/>
<connect gate="MCU" pin="PD10" pad="H4"/>
<connect gate="MCU" pin="PD11" pad="K2"/>
<connect gate="MCU" pin="PD12" pad="H6"/>
<connect gate="MCU" pin="PD13" pad="H5"/>
<connect gate="MCU" pin="PD14" pad="J2"/>
<connect gate="MCU" pin="PD15" pad="K1"/>
<connect gate="MCU" pin="PD2" pad="A3"/>
<connect gate="MCU" pin="PD3" pad="B4"/>
<connect gate="MCU" pin="PD4" pad="B5"/>
<connect gate="MCU" pin="PD5" pad="A4"/>
<connect gate="MCU" pin="PD6" pad="F4"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD8" pad="L2"/>
<connect gate="MCU" pin="PD9" pad="M1"/>
<connect gate="MCU" pin="PDR_ON" pad="A11"/>
<connect gate="MCU" pin="PE0" pad="B10"/>
<connect gate="MCU" pin="PE1" pad="A10"/>
<connect gate="MCU" pin="PE10" pad="J4"/>
<connect gate="MCU" pin="PE11" pad="K4"/>
<connect gate="MCU" pin="PE12" pad="L4"/>
<connect gate="MCU" pin="PE13" pad="N4"/>
<connect gate="MCU" pin="PE14" pad="M4"/>
<connect gate="MCU" pin="PE15" pad="L3"/>
<connect gate="MCU" pin="PE2" pad="D8"/>
<connect gate="MCU" pin="PE3" pad="C10"/>
<connect gate="MCU" pin="PE4" pad="B11"/>
<connect gate="MCU" pin="PE5" pad="D9"/>
<connect gate="MCU" pin="PE6" pad="E8"/>
<connect gate="MCU" pin="PE7" pad="L5"/>
<connect gate="MCU" pin="PE8" pad="M5"/>
<connect gate="MCU" pin="PE9" pad="N5"/>
<connect gate="MCU" pin="PF0" pad="F11"/>
<connect gate="MCU" pin="PF1" pad="E9"/>
<connect gate="MCU" pin="PF10" pad="G9"/>
<connect gate="MCU" pin="PF11" pad="M7"/>
<connect gate="MCU" pin="PF12" pad="N7"/>
<connect gate="MCU" pin="PF13" pad="K6"/>
<connect gate="MCU" pin="PF14" pad="L6"/>
<connect gate="MCU" pin="PF15" pad="M6"/>
<connect gate="MCU" pin="PF2" pad="F10"/>
<connect gate="MCU" pin="PF3" pad="G11"/>
<connect gate="MCU" pin="PF4" pad="F9"/>
<connect gate="MCU" pin="PF5" pad="F8"/>
<connect gate="MCU" pin="PF6" pad="G10"/>
<connect gate="MCU" pin="PF7" pad="F7"/>
<connect gate="MCU" pin="PF8" pad="H11"/>
<connect gate="MCU" pin="PF9" pad="G8"/>
<connect gate="MCU" pin="PG0" pad="N6"/>
<connect gate="MCU" pin="PG1" pad="K5"/>
<connect gate="MCU" pin="PG10" pad="C6"/>
<connect gate="MCU" pin="PG11" pad="B6"/>
<connect gate="MCU" pin="PG12" pad="A6"/>
<connect gate="MCU" pin="PG13" pad="D6"/>
<connect gate="MCU" pin="PG14" pad="F6"/>
<connect gate="MCU" pin="PG15" pad="A7"/>
<connect gate="MCU" pin="PG2" pad="J1"/>
<connect gate="MCU" pin="PG3" pad="G3"/>
<connect gate="MCU" pin="PG4" pad="G5"/>
<connect gate="MCU" pin="PG5" pad="G6"/>
<connect gate="MCU" pin="PG6" pad="G4"/>
<connect gate="MCU" pin="PG7" pad="H1"/>
<connect gate="MCU" pin="PG8" pad="G2"/>
<connect gate="MCU" pin="PG9" pad="E5"/>
<connect gate="MCU" pin="VBAT" pad="C11"/>
<connect gate="MCU" pin="VCAP1" pad="N2"/>
<connect gate="MCU" pin="VCAP2" pad="D1"/>
<connect gate="MCU" pin="VDDA" pad="L10"/>
<connect gate="MCU" pin="VREF+" pad="L11"/>
<connect gate="MCU" pin="VSSA" pad="K10"/>
<connect gate="PWR" pin="VDD@1" pad="A1"/>
<connect gate="PWR" pin="VDD@10" pad="J6"/>
<connect gate="PWR" pin="VDD@11" pad="J7"/>
<connect gate="PWR" pin="VDD@12" pad="J8"/>
<connect gate="PWR" pin="VDD@13" pad="L1"/>
<connect gate="PWR" pin="VDD@2" pad="C1"/>
<connect gate="PWR" pin="VDD@3" pad="C5"/>
<connect gate="PWR" pin="VDD@4" pad="D7"/>
<connect gate="PWR" pin="VDD@5" pad="E6"/>
<connect gate="PWR" pin="VDD@6" pad="E10"/>
<connect gate="PWR" pin="VDD@7" pad="G1"/>
<connect gate="PWR" pin="VDD@8" pad="G7"/>
<connect gate="PWR" pin="VDD@9" pad="J5"/>
<connect gate="PWR" pin="VSS@1" pad="D2"/>
<connect gate="PWR" pin="VSS@2" pad="E7"/>
<connect gate="PWR" pin="VSS@3" pad="F5"/>
<connect gate="PWR" pin="VSS@4" pad="H2"/>
<connect gate="PWR" pin="VSS@5" pad="H3"/>
<connect gate="PWR" pin="VSS@6" pad="H7"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F429I*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD15_VSS11"/>
</gates>
<devices>
<device name="" package="LQFP176">
<connects>
<connect gate="MCU" pin="BOOT0" pad="166"/>
<connect gate="MCU" pin="BYPASS_REG" pad="48"/>
<connect gate="MCU" pin="NRST" pad="31"/>
<connect gate="MCU" pin="OSC_IN" pad="29"/>
<connect gate="MCU" pin="OSC_OUT" pad="30"/>
<connect gate="MCU" pin="PA0" pad="40"/>
<connect gate="MCU" pin="PA1" pad="41"/>
<connect gate="MCU" pin="PA10" pad="121"/>
<connect gate="MCU" pin="PA11" pad="122"/>
<connect gate="MCU" pin="PA12" pad="123"/>
<connect gate="MCU" pin="PA13" pad="124"/>
<connect gate="MCU" pin="PA14" pad="137"/>
<connect gate="MCU" pin="PA15" pad="138"/>
<connect gate="MCU" pin="PA2" pad="42"/>
<connect gate="MCU" pin="PA3" pad="47"/>
<connect gate="MCU" pin="PA4" pad="50"/>
<connect gate="MCU" pin="PA5" pad="51"/>
<connect gate="MCU" pin="PA6" pad="52"/>
<connect gate="MCU" pin="PA7" pad="53"/>
<connect gate="MCU" pin="PA8" pad="119"/>
<connect gate="MCU" pin="PA9" pad="120"/>
<connect gate="MCU" pin="PB0" pad="56"/>
<connect gate="MCU" pin="PB1" pad="57"/>
<connect gate="MCU" pin="PB10" pad="79"/>
<connect gate="MCU" pin="PB11" pad="80"/>
<connect gate="MCU" pin="PB12" pad="92"/>
<connect gate="MCU" pin="PB13" pad="93"/>
<connect gate="MCU" pin="PB14" pad="94"/>
<connect gate="MCU" pin="PB15" pad="95"/>
<connect gate="MCU" pin="PB2" pad="58"/>
<connect gate="MCU" pin="PB3" pad="161"/>
<connect gate="MCU" pin="PB4" pad="162"/>
<connect gate="MCU" pin="PB5" pad="163"/>
<connect gate="MCU" pin="PB6" pad="164"/>
<connect gate="MCU" pin="PB7" pad="165"/>
<connect gate="MCU" pin="PB8" pad="167"/>
<connect gate="MCU" pin="PB9" pad="168"/>
<connect gate="MCU" pin="PC0" pad="32"/>
<connect gate="MCU" pin="PC1" pad="33"/>
<connect gate="MCU" pin="PC10" pad="139"/>
<connect gate="MCU" pin="PC11" pad="140"/>
<connect gate="MCU" pin="PC12" pad="141"/>
<connect gate="MCU" pin="PC13" pad="8"/>
<connect gate="MCU" pin="PC14" pad="9"/>
<connect gate="MCU" pin="PC15" pad="10"/>
<connect gate="MCU" pin="PC2" pad="34"/>
<connect gate="MCU" pin="PC3" pad="35"/>
<connect gate="MCU" pin="PC4" pad="54"/>
<connect gate="MCU" pin="PC5" pad="55"/>
<connect gate="MCU" pin="PC6" pad="115"/>
<connect gate="MCU" pin="PC7" pad="116"/>
<connect gate="MCU" pin="PC8" pad="117"/>
<connect gate="MCU" pin="PC9" pad="118"/>
<connect gate="MCU" pin="PD0" pad="142"/>
<connect gate="MCU" pin="PD1" pad="143"/>
<connect gate="MCU" pin="PD10" pad="98"/>
<connect gate="MCU" pin="PD11" pad="99"/>
<connect gate="MCU" pin="PD12" pad="100"/>
<connect gate="MCU" pin="PD13" pad="101"/>
<connect gate="MCU" pin="PD14" pad="104"/>
<connect gate="MCU" pin="PD15" pad="105"/>
<connect gate="MCU" pin="PD2" pad="144"/>
<connect gate="MCU" pin="PD3" pad="145"/>
<connect gate="MCU" pin="PD4" pad="146"/>
<connect gate="MCU" pin="PD5" pad="147"/>
<connect gate="MCU" pin="PD6" pad="150"/>
<connect gate="MCU" pin="PD7" pad="151"/>
<connect gate="MCU" pin="PD8" pad="96"/>
<connect gate="MCU" pin="PD9" pad="97"/>
<connect gate="MCU" pin="PDR_ON" pad="171"/>
<connect gate="MCU" pin="PE0" pad="169"/>
<connect gate="MCU" pin="PE1" pad="170"/>
<connect gate="MCU" pin="PE10" pad="73"/>
<connect gate="MCU" pin="PE11" pad="74"/>
<connect gate="MCU" pin="PE12" pad="75"/>
<connect gate="MCU" pin="PE13" pad="76"/>
<connect gate="MCU" pin="PE14" pad="77"/>
<connect gate="MCU" pin="PE15" pad="78"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="68"/>
<connect gate="MCU" pin="PE8" pad="69"/>
<connect gate="MCU" pin="PE9" pad="70"/>
<connect gate="MCU" pin="PF0" pad="16"/>
<connect gate="MCU" pin="PF1" pad="17"/>
<connect gate="MCU" pin="PF10" pad="28"/>
<connect gate="MCU" pin="PF11" pad="59"/>
<connect gate="MCU" pin="PF12" pad="60"/>
<connect gate="MCU" pin="PF13" pad="63"/>
<connect gate="MCU" pin="PF14" pad="64"/>
<connect gate="MCU" pin="PF15" pad="65"/>
<connect gate="MCU" pin="PF2" pad="18"/>
<connect gate="MCU" pin="PF3" pad="19"/>
<connect gate="MCU" pin="PF4" pad="20"/>
<connect gate="MCU" pin="PF5" pad="21"/>
<connect gate="MCU" pin="PF6" pad="24"/>
<connect gate="MCU" pin="PF7" pad="25"/>
<connect gate="MCU" pin="PF8" pad="26"/>
<connect gate="MCU" pin="PF9" pad="27"/>
<connect gate="MCU" pin="PG0" pad="66"/>
<connect gate="MCU" pin="PG1" pad="67"/>
<connect gate="MCU" pin="PG10" pad="153"/>
<connect gate="MCU" pin="PG11" pad="154"/>
<connect gate="MCU" pin="PG12" pad="155"/>
<connect gate="MCU" pin="PG13" pad="156"/>
<connect gate="MCU" pin="PG14" pad="157"/>
<connect gate="MCU" pin="PG15" pad="160"/>
<connect gate="MCU" pin="PG2" pad="106"/>
<connect gate="MCU" pin="PG3" pad="107"/>
<connect gate="MCU" pin="PG4" pad="108"/>
<connect gate="MCU" pin="PG5" pad="109"/>
<connect gate="MCU" pin="PG6" pad="110"/>
<connect gate="MCU" pin="PG7" pad="111"/>
<connect gate="MCU" pin="PG8" pad="112"/>
<connect gate="MCU" pin="PG9" pad="152"/>
<connect gate="MCU" pin="PH10" pad="87"/>
<connect gate="MCU" pin="PH11" pad="88"/>
<connect gate="MCU" pin="PH12" pad="89"/>
<connect gate="MCU" pin="PH13" pad="128"/>
<connect gate="MCU" pin="PH14" pad="129"/>
<connect gate="MCU" pin="PH15" pad="130"/>
<connect gate="MCU" pin="PH2" pad="43"/>
<connect gate="MCU" pin="PH3" pad="44"/>
<connect gate="MCU" pin="PH4" pad="45"/>
<connect gate="MCU" pin="PH5" pad="46"/>
<connect gate="MCU" pin="PH6" pad="83"/>
<connect gate="MCU" pin="PH7" pad="84"/>
<connect gate="MCU" pin="PH8" pad="85"/>
<connect gate="MCU" pin="PH9" pad="86"/>
<connect gate="MCU" pin="PI0" pad="131"/>
<connect gate="MCU" pin="PI1" pad="132"/>
<connect gate="MCU" pin="PI10" pad="12"/>
<connect gate="MCU" pin="PI11" pad="13"/>
<connect gate="MCU" pin="PI2" pad="133"/>
<connect gate="MCU" pin="PI3" pad="134"/>
<connect gate="MCU" pin="PI4" pad="173"/>
<connect gate="MCU" pin="PI5" pad="174"/>
<connect gate="MCU" pin="PI6" pad="175"/>
<connect gate="MCU" pin="PI7" pad="176"/>
<connect gate="MCU" pin="PI8" pad="7"/>
<connect gate="MCU" pin="PI9" pad="11"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="81"/>
<connect gate="MCU" pin="VCAP2" pad="125"/>
<connect gate="MCU" pin="VDDA" pad="39"/>
<connect gate="MCU" pin="VREF+" pad="38"/>
<connect gate="MCU" pin="VSSA" pad="37"/>
<connect gate="PWR" pin="VDD@1" pad="159"/>
<connect gate="PWR" pin="VDD@10" pad="23"/>
<connect gate="PWR" pin="VDD@11" pad="15"/>
<connect gate="PWR" pin="VDD@12" pad="172"/>
<connect gate="PWR" pin="VDD@13" pad="82"/>
<connect gate="PWR" pin="VDD@14" pad="49"/>
<connect gate="PWR" pin="VDD@15" pad="36"/>
<connect gate="PWR" pin="VDD@2" pad="149"/>
<connect gate="PWR" pin="VDD@3" pad="136"/>
<connect gate="PWR" pin="VDD@4" pad="127"/>
<connect gate="PWR" pin="VDD@5" pad="114"/>
<connect gate="PWR" pin="VDD@6" pad="103"/>
<connect gate="PWR" pin="VDD@7" pad="91"/>
<connect gate="PWR" pin="VDD@8" pad="72"/>
<connect gate="PWR" pin="VDD@9" pad="62"/>
<connect gate="PWR" pin="VSS@1" pad="158"/>
<connect gate="PWR" pin="VSS@10" pad="22"/>
<connect gate="PWR" pin="VSS@11" pad="14"/>
<connect gate="PWR" pin="VSS@2" pad="148"/>
<connect gate="PWR" pin="VSS@3" pad="135"/>
<connect gate="PWR" pin="VSS@4" pad="126"/>
<connect gate="PWR" pin="VSS@5" pad="113"/>
<connect gate="PWR" pin="VSS@6" pad="102"/>
<connect gate="PWR" pin="VSS@7" pad="90"/>
<connect gate="PWR" pin="VSS@8" pad="71"/>
<connect gate="PWR" pin="VSS@9" pad="61"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F429I*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD14_VSS36"/>
</gates>
<devices>
<device name="" package="UFBGA176+25">
<connects>
<connect gate="MCU" pin="BOOT0" pad="D6"/>
<connect gate="MCU" pin="BYPASS_REG" pad="L4"/>
<connect gate="MCU" pin="NRST" pad="J1"/>
<connect gate="MCU" pin="OSC_IN" pad="G1"/>
<connect gate="MCU" pin="OSC_OUT" pad="H1"/>
<connect gate="MCU" pin="PA0" pad="N3"/>
<connect gate="MCU" pin="PA1" pad="N2"/>
<connect gate="MCU" pin="PA10" pad="D15"/>
<connect gate="MCU" pin="PA11" pad="C15"/>
<connect gate="MCU" pin="PA12" pad="B15"/>
<connect gate="MCU" pin="PA13" pad="A15"/>
<connect gate="MCU" pin="PA14" pad="A14"/>
<connect gate="MCU" pin="PA15" pad="A13"/>
<connect gate="MCU" pin="PA2" pad="P2"/>
<connect gate="MCU" pin="PA3" pad="R2"/>
<connect gate="MCU" pin="PA4" pad="N4"/>
<connect gate="MCU" pin="PA5" pad="P4"/>
<connect gate="MCU" pin="PA6" pad="P3"/>
<connect gate="MCU" pin="PA7" pad="R3"/>
<connect gate="MCU" pin="PA8" pad="F15"/>
<connect gate="MCU" pin="PA9" pad="E15"/>
<connect gate="MCU" pin="PB0" pad="R5"/>
<connect gate="MCU" pin="PB1" pad="R4"/>
<connect gate="MCU" pin="PB10" pad="R12"/>
<connect gate="MCU" pin="PB11" pad="R13"/>
<connect gate="MCU" pin="PB12" pad="P12"/>
<connect gate="MCU" pin="PB13" pad="P13"/>
<connect gate="MCU" pin="PB14" pad="R14"/>
<connect gate="MCU" pin="PB15" pad="R15"/>
<connect gate="MCU" pin="PB2" pad="M6"/>
<connect gate="MCU" pin="PB3" pad="A10"/>
<connect gate="MCU" pin="PB4" pad="A9"/>
<connect gate="MCU" pin="PB5" pad="A6"/>
<connect gate="MCU" pin="PB6" pad="B6"/>
<connect gate="MCU" pin="PB7" pad="B5"/>
<connect gate="MCU" pin="PB8" pad="A5"/>
<connect gate="MCU" pin="PB9" pad="B4"/>
<connect gate="MCU" pin="PC0" pad="M2"/>
<connect gate="MCU" pin="PC1" pad="M3"/>
<connect gate="MCU" pin="PC10" pad="B14"/>
<connect gate="MCU" pin="PC11" pad="B13"/>
<connect gate="MCU" pin="PC12" pad="A12"/>
<connect gate="MCU" pin="PC13" pad="D1"/>
<connect gate="MCU" pin="PC14" pad="E1"/>
<connect gate="MCU" pin="PC15" pad="F1"/>
<connect gate="MCU" pin="PC2" pad="M4"/>
<connect gate="MCU" pin="PC3" pad="M5"/>
<connect gate="MCU" pin="PC4" pad="N5"/>
<connect gate="MCU" pin="PC5" pad="P5"/>
<connect gate="MCU" pin="PC6" pad="H15"/>
<connect gate="MCU" pin="PC7" pad="G15"/>
<connect gate="MCU" pin="PC8" pad="G14"/>
<connect gate="MCU" pin="PC9" pad="F14"/>
<connect gate="MCU" pin="PD0" pad="B12"/>
<connect gate="MCU" pin="PD1" pad="C12"/>
<connect gate="MCU" pin="PD10" pad="N15"/>
<connect gate="MCU" pin="PD11" pad="N14"/>
<connect gate="MCU" pin="PD12" pad="N13"/>
<connect gate="MCU" pin="PD13" pad="M15"/>
<connect gate="MCU" pin="PD14" pad="M14"/>
<connect gate="MCU" pin="PD15" pad="L14"/>
<connect gate="MCU" pin="PD2" pad="D12"/>
<connect gate="MCU" pin="PD3" pad="D11"/>
<connect gate="MCU" pin="PD4" pad="D10"/>
<connect gate="MCU" pin="PD5" pad="C11"/>
<connect gate="MCU" pin="PD6" pad="B11"/>
<connect gate="MCU" pin="PD7" pad="A11"/>
<connect gate="MCU" pin="PD8" pad="P15"/>
<connect gate="MCU" pin="PD9" pad="P14"/>
<connect gate="MCU" pin="PDR_ON" pad="C6"/>
<connect gate="MCU" pin="PE0" pad="A4"/>
<connect gate="MCU" pin="PE1" pad="A3"/>
<connect gate="MCU" pin="PE10" pad="R9"/>
<connect gate="MCU" pin="PE11" pad="P10"/>
<connect gate="MCU" pin="PE12" pad="R10"/>
<connect gate="MCU" pin="PE13" pad="N11"/>
<connect gate="MCU" pin="PE14" pad="P11"/>
<connect gate="MCU" pin="PE15" pad="R11"/>
<connect gate="MCU" pin="PE2" pad="A2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="B2"/>
<connect gate="MCU" pin="PE6" pad="B3"/>
<connect gate="MCU" pin="PE7" pad="R8"/>
<connect gate="MCU" pin="PE8" pad="P8"/>
<connect gate="MCU" pin="PE9" pad="P9"/>
<connect gate="MCU" pin="PF0" pad="E2"/>
<connect gate="MCU" pin="PF1" pad="H3"/>
<connect gate="MCU" pin="PF10" pad="L1"/>
<connect gate="MCU" pin="PF11" pad="R6"/>
<connect gate="MCU" pin="PF12" pad="P6"/>
<connect gate="MCU" pin="PF13" pad="N6"/>
<connect gate="MCU" pin="PF14" pad="R7"/>
<connect gate="MCU" pin="PF15" pad="P7"/>
<connect gate="MCU" pin="PF2" pad="H2"/>
<connect gate="MCU" pin="PF3" pad="J2"/>
<connect gate="MCU" pin="PF4" pad="J3"/>
<connect gate="MCU" pin="PF5" pad="K3"/>
<connect gate="MCU" pin="PF6" pad="K2"/>
<connect gate="MCU" pin="PF7" pad="K1"/>
<connect gate="MCU" pin="PF8" pad="L3"/>
<connect gate="MCU" pin="PF9" pad="L2"/>
<connect gate="MCU" pin="PG0" pad="N7"/>
<connect gate="MCU" pin="PG1" pad="M7"/>
<connect gate="MCU" pin="PG10" pad="B10"/>
<connect gate="MCU" pin="PG11" pad="B9"/>
<connect gate="MCU" pin="PG12" pad="B8"/>
<connect gate="MCU" pin="PG13" pad="A8"/>
<connect gate="MCU" pin="PG14" pad="A7"/>
<connect gate="MCU" pin="PG15" pad="B7"/>
<connect gate="MCU" pin="PG2" pad="L15"/>
<connect gate="MCU" pin="PG3" pad="K15"/>
<connect gate="MCU" pin="PG4" pad="K14"/>
<connect gate="MCU" pin="PG5" pad="K13"/>
<connect gate="MCU" pin="PG6" pad="J15"/>
<connect gate="MCU" pin="PG7" pad="J14"/>
<connect gate="MCU" pin="PG8" pad="H14"/>
<connect gate="MCU" pin="PG9" pad="C10"/>
<connect gate="MCU" pin="PH10" pad="L13"/>
<connect gate="MCU" pin="PH11" pad="L12"/>
<connect gate="MCU" pin="PH12" pad="K12"/>
<connect gate="MCU" pin="PH13" pad="E12"/>
<connect gate="MCU" pin="PH14" pad="E13"/>
<connect gate="MCU" pin="PH15" pad="D13"/>
<connect gate="MCU" pin="PH2" pad="F4"/>
<connect gate="MCU" pin="PH3" pad="G4"/>
<connect gate="MCU" pin="PH4" pad="H4"/>
<connect gate="MCU" pin="PH5" pad="J4"/>
<connect gate="MCU" pin="PH6" pad="M11"/>
<connect gate="MCU" pin="PH7" pad="N12"/>
<connect gate="MCU" pin="PH8" pad="M12"/>
<connect gate="MCU" pin="PH9" pad="M13"/>
<connect gate="MCU" pin="PI0" pad="E14"/>
<connect gate="MCU" pin="PI1" pad="D14"/>
<connect gate="MCU" pin="PI10" pad="E3"/>
<connect gate="MCU" pin="PI11" pad="E4"/>
<connect gate="MCU" pin="PI2" pad="C14"/>
<connect gate="MCU" pin="PI3" pad="C13"/>
<connect gate="MCU" pin="PI4" pad="D4"/>
<connect gate="MCU" pin="PI5" pad="C4"/>
<connect gate="MCU" pin="PI6" pad="C3"/>
<connect gate="MCU" pin="PI7" pad="C2"/>
<connect gate="MCU" pin="PI8" pad="D2"/>
<connect gate="MCU" pin="PI9" pad="D3"/>
<connect gate="MCU" pin="VBAT" pad="C1"/>
<connect gate="MCU" pin="VCAP1" pad="M10"/>
<connect gate="MCU" pin="VCAP2" pad="F13"/>
<connect gate="MCU" pin="VDDA" pad="R1"/>
<connect gate="MCU" pin="VREF+" pad="P1"/>
<connect gate="MCU" pin="VREF-" pad="N1"/>
<connect gate="MCU" pin="VSSA" pad="M1"/>
<connect gate="PWR" pin="VDD@1" pad="C5"/>
<connect gate="PWR" pin="VDD@10" pad="J13"/>
<connect gate="PWR" pin="VDD@11" pad="K4"/>
<connect gate="PWR" pin="VDD@12" pad="N8"/>
<connect gate="PWR" pin="VDD@13" pad="N9"/>
<connect gate="PWR" pin="VDD@14" pad="N10"/>
<connect gate="PWR" pin="VDD@2" pad="C7"/>
<connect gate="PWR" pin="VDD@3" pad="C8"/>
<connect gate="PWR" pin="VDD@4" pad="C9"/>
<connect gate="PWR" pin="VDD@5" pad="F3"/>
<connect gate="PWR" pin="VDD@6" pad="G3"/>
<connect gate="PWR" pin="VDD@7" pad="G13"/>
<connect gate="PWR" pin="VDD@8" pad="H13"/>
<connect gate="PWR" pin="VDD@9" pad="J12"/>
<connect gate="PWR" pin="VSS@1" pad="D5"/>
<connect gate="PWR" pin="VSS@10" pad="M8"/>
<connect gate="PWR" pin="VSS@11" pad="M9"/>
<connect gate="PWR" pin="VSS@12" pad="VSS_1"/>
<connect gate="PWR" pin="VSS@13" pad="VSS_2"/>
<connect gate="PWR" pin="VSS@14" pad="VSS_3"/>
<connect gate="PWR" pin="VSS@15" pad="VSS_4"/>
<connect gate="PWR" pin="VSS@16" pad="VSS_5"/>
<connect gate="PWR" pin="VSS@17" pad="VSS_6"/>
<connect gate="PWR" pin="VSS@18" pad="VSS_7"/>
<connect gate="PWR" pin="VSS@19" pad="VSS_8"/>
<connect gate="PWR" pin="VSS@2" pad="D7"/>
<connect gate="PWR" pin="VSS@20" pad="VSS_9"/>
<connect gate="PWR" pin="VSS@21" pad="VSS_10"/>
<connect gate="PWR" pin="VSS@22" pad="VSS_11"/>
<connect gate="PWR" pin="VSS@23" pad="VSS_12"/>
<connect gate="PWR" pin="VSS@24" pad="VSS_13"/>
<connect gate="PWR" pin="VSS@25" pad="VSS_14"/>
<connect gate="PWR" pin="VSS@26" pad="VSS_15"/>
<connect gate="PWR" pin="VSS@27" pad="VSS_16"/>
<connect gate="PWR" pin="VSS@28" pad="VSS_17"/>
<connect gate="PWR" pin="VSS@29" pad="VSS_18"/>
<connect gate="PWR" pin="VSS@3" pad="D8"/>
<connect gate="PWR" pin="VSS@30" pad="VSS_19"/>
<connect gate="PWR" pin="VSS@31" pad="VSS_20"/>
<connect gate="PWR" pin="VSS@32" pad="VSS_21"/>
<connect gate="PWR" pin="VSS@33" pad="VSS_22"/>
<connect gate="PWR" pin="VSS@34" pad="VSS_23"/>
<connect gate="PWR" pin="VSS@35" pad="VSS_24"/>
<connect gate="PWR" pin="VSS@36" pad="VSS_25"/>
<connect gate="PWR" pin="VSS@4" pad="D9"/>
<connect gate="PWR" pin="VSS@5" pad="F2"/>
<connect gate="PWR" pin="VSS@6" pad="F12"/>
<connect gate="PWR" pin="VSS@7" pad="G2"/>
<connect gate="PWR" pin="VSS@8" pad="G12"/>
<connect gate="PWR" pin="VSS@9" pad="H12"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F429B*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
168 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_208PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD17_VSS14"/>
</gates>
<devices>
<device name="" package="LQFP208">
<connects>
<connect gate="MCU" pin="BOOT0" pad="197"/>
<connect gate="MCU" pin="NRST" pad="34"/>
<connect gate="MCU" pin="OSC_IN" pad="32"/>
<connect gate="MCU" pin="OSC_OUT" pad="33"/>
<connect gate="MCU" pin="PA0" pad="43"/>
<connect gate="MCU" pin="PA1" pad="44"/>
<connect gate="MCU" pin="PA10" pad="144"/>
<connect gate="MCU" pin="PA11" pad="145"/>
<connect gate="MCU" pin="PA12" pad="146"/>
<connect gate="MCU" pin="PA13" pad="147"/>
<connect gate="MCU" pin="PA14" pad="159"/>
<connect gate="MCU" pin="PA15" pad="160"/>
<connect gate="MCU" pin="PA2" pad="45"/>
<connect gate="MCU" pin="PA3" pad="50"/>
<connect gate="MCU" pin="PA4" pad="53"/>
<connect gate="MCU" pin="PA5" pad="54"/>
<connect gate="MCU" pin="PA6" pad="55"/>
<connect gate="MCU" pin="PA7" pad="56"/>
<connect gate="MCU" pin="PA8" pad="142"/>
<connect gate="MCU" pin="PA9" pad="143"/>
<connect gate="MCU" pin="PB0" pad="61"/>
<connect gate="MCU" pin="PB1" pad="62"/>
<connect gate="MCU" pin="PB10" pad="90"/>
<connect gate="MCU" pin="PB11" pad="91"/>
<connect gate="MCU" pin="PB12" pad="104"/>
<connect gate="MCU" pin="PB13" pad="105"/>
<connect gate="MCU" pin="PB14" pad="106"/>
<connect gate="MCU" pin="PB15" pad="107"/>
<connect gate="MCU" pin="PB2" pad="63"/>
<connect gate="MCU" pin="PB3" pad="192"/>
<connect gate="MCU" pin="PB4" pad="193"/>
<connect gate="MCU" pin="PB5" pad="194"/>
<connect gate="MCU" pin="PB6" pad="195"/>
<connect gate="MCU" pin="PB7" pad="196"/>
<connect gate="MCU" pin="PB8" pad="198"/>
<connect gate="MCU" pin="PB9" pad="199"/>
<connect gate="MCU" pin="PC0" pad="35"/>
<connect gate="MCU" pin="PC1" pad="36"/>
<connect gate="MCU" pin="PC10" pad="161"/>
<connect gate="MCU" pin="PC11" pad="162"/>
<connect gate="MCU" pin="PC12" pad="163"/>
<connect gate="MCU" pin="PC13" pad="8"/>
<connect gate="MCU" pin="PC14" pad="9"/>
<connect gate="MCU" pin="PC15" pad="10"/>
<connect gate="MCU" pin="PC2" pad="37"/>
<connect gate="MCU" pin="PC3" pad="38"/>
<connect gate="MCU" pin="PC4" pad="57"/>
<connect gate="MCU" pin="PC5" pad="58"/>
<connect gate="MCU" pin="PC6" pad="138"/>
<connect gate="MCU" pin="PC7" pad="139"/>
<connect gate="MCU" pin="PC8" pad="140"/>
<connect gate="MCU" pin="PC9" pad="141"/>
<connect gate="MCU" pin="PD0" pad="164"/>
<connect gate="MCU" pin="PD1" pad="165"/>
<connect gate="MCU" pin="PD10" pad="110"/>
<connect gate="MCU" pin="PD11" pad="111"/>
<connect gate="MCU" pin="PD12" pad="112"/>
<connect gate="MCU" pin="PD13" pad="113"/>
<connect gate="MCU" pin="PD14" pad="116"/>
<connect gate="MCU" pin="PD15" pad="117"/>
<connect gate="MCU" pin="PD2" pad="166"/>
<connect gate="MCU" pin="PD3" pad="167"/>
<connect gate="MCU" pin="PD4" pad="168"/>
<connect gate="MCU" pin="PD5" pad="169"/>
<connect gate="MCU" pin="PD6" pad="172"/>
<connect gate="MCU" pin="PD7" pad="173"/>
<connect gate="MCU" pin="PD8" pad="108"/>
<connect gate="MCU" pin="PD9" pad="109"/>
<connect gate="MCU" pin="PDR_ON" pad="203"/>
<connect gate="MCU" pin="PE0" pad="200"/>
<connect gate="MCU" pin="PE1" pad="201"/>
<connect gate="MCU" pin="PE10" pad="84"/>
<connect gate="MCU" pin="PE11" pad="85"/>
<connect gate="MCU" pin="PE12" pad="86"/>
<connect gate="MCU" pin="PE13" pad="87"/>
<connect gate="MCU" pin="PE14" pad="88"/>
<connect gate="MCU" pin="PE15" pad="89"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="79"/>
<connect gate="MCU" pin="PE8" pad="80"/>
<connect gate="MCU" pin="PE9" pad="81"/>
<connect gate="MCU" pin="PF0" pad="16"/>
<connect gate="MCU" pin="PF1" pad="17"/>
<connect gate="MCU" pin="PF10" pad="31"/>
<connect gate="MCU" pin="PF11" pad="70"/>
<connect gate="MCU" pin="PF12" pad="71"/>
<connect gate="MCU" pin="PF13" pad="74"/>
<connect gate="MCU" pin="PF14" pad="75"/>
<connect gate="MCU" pin="PF15" pad="76"/>
<connect gate="MCU" pin="PF2" pad="18"/>
<connect gate="MCU" pin="PF3" pad="22"/>
<connect gate="MCU" pin="PF4" pad="23"/>
<connect gate="MCU" pin="PF5" pad="24"/>
<connect gate="MCU" pin="PF6" pad="27"/>
<connect gate="MCU" pin="PF7" pad="28"/>
<connect gate="MCU" pin="PF8" pad="29"/>
<connect gate="MCU" pin="PF9" pad="30"/>
<connect gate="MCU" pin="PG0" pad="77"/>
<connect gate="MCU" pin="PG1" pad="78"/>
<connect gate="MCU" pin="PG10" pad="179"/>
<connect gate="MCU" pin="PG11" pad="180"/>
<connect gate="MCU" pin="PG12" pad="181"/>
<connect gate="MCU" pin="PG13" pad="182"/>
<connect gate="MCU" pin="PG14" pad="183"/>
<connect gate="MCU" pin="PG15" pad="191"/>
<connect gate="MCU" pin="PG2" pad="129"/>
<connect gate="MCU" pin="PG3" pad="130"/>
<connect gate="MCU" pin="PG4" pad="131"/>
<connect gate="MCU" pin="PG5" pad="132"/>
<connect gate="MCU" pin="PG6" pad="133"/>
<connect gate="MCU" pin="PG7" pad="134"/>
<connect gate="MCU" pin="PG8" pad="135"/>
<connect gate="MCU" pin="PG9" pad="178"/>
<connect gate="MCU" pin="PH10" pad="100"/>
<connect gate="MCU" pin="PH11" pad="101"/>
<connect gate="MCU" pin="PH12" pad="102"/>
<connect gate="MCU" pin="PH13" pad="151"/>
<connect gate="MCU" pin="PH14" pad="152"/>
<connect gate="MCU" pin="PH15" pad="153"/>
<connect gate="MCU" pin="PH2" pad="46"/>
<connect gate="MCU" pin="PH3" pad="47"/>
<connect gate="MCU" pin="PH4" pad="48"/>
<connect gate="MCU" pin="PH5" pad="49"/>
<connect gate="MCU" pin="PH6" pad="96"/>
<connect gate="MCU" pin="PH7" pad="97"/>
<connect gate="MCU" pin="PH8" pad="98"/>
<connect gate="MCU" pin="PH9" pad="99"/>
<connect gate="MCU" pin="PI0" pad="154"/>
<connect gate="MCU" pin="PI1" pad="155"/>
<connect gate="MCU" pin="PI10" pad="12"/>
<connect gate="MCU" pin="PI11" pad="13"/>
<connect gate="MCU" pin="PI12" pad="19"/>
<connect gate="MCU" pin="PI13" pad="20"/>
<connect gate="MCU" pin="PI14" pad="21"/>
<connect gate="MCU" pin="PI15" pad="64"/>
<connect gate="MCU" pin="PI2" pad="156"/>
<connect gate="MCU" pin="PI3" pad="157"/>
<connect gate="MCU" pin="PI4" pad="205"/>
<connect gate="MCU" pin="PI5" pad="206"/>
<connect gate="MCU" pin="PI6" pad="207"/>
<connect gate="MCU" pin="PI7" pad="208"/>
<connect gate="MCU" pin="PI8" pad="7"/>
<connect gate="MCU" pin="PI9" pad="11"/>
<connect gate="MCU" pin="PJ0" pad="65"/>
<connect gate="MCU" pin="PJ1" pad="66"/>
<connect gate="MCU" pin="PJ10" pad="122"/>
<connect gate="MCU" pin="PJ11" pad="123"/>
<connect gate="MCU" pin="PJ12" pad="174"/>
<connect gate="MCU" pin="PJ13" pad="175"/>
<connect gate="MCU" pin="PJ14" pad="176"/>
<connect gate="MCU" pin="PJ15" pad="177"/>
<connect gate="MCU" pin="PJ2" pad="67"/>
<connect gate="MCU" pin="PJ3" pad="68"/>
<connect gate="MCU" pin="PJ4" pad="69"/>
<connect gate="MCU" pin="PJ5" pad="95"/>
<connect gate="MCU" pin="PJ6" pad="118"/>
<connect gate="MCU" pin="PJ7" pad="119"/>
<connect gate="MCU" pin="PJ8" pad="120"/>
<connect gate="MCU" pin="PJ9" pad="121"/>
<connect gate="MCU" pin="PK0" pad="126"/>
<connect gate="MCU" pin="PK1" pad="127"/>
<connect gate="MCU" pin="PK2" pad="128"/>
<connect gate="MCU" pin="PK3" pad="186"/>
<connect gate="MCU" pin="PK4" pad="187"/>
<connect gate="MCU" pin="PK5" pad="188"/>
<connect gate="MCU" pin="PK6" pad="189"/>
<connect gate="MCU" pin="PK7" pad="190"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="92"/>
<connect gate="MCU" pin="VCAP2" pad="148"/>
<connect gate="MCU" pin="VDDA" pad="42"/>
<connect gate="MCU" pin="VREF+" pad="41"/>
<connect gate="MCU" pin="VSSA" pad="40"/>
<connect gate="PWR" pin="VDD@1" pad="204"/>
<connect gate="PWR" pin="VDD@10" pad="73"/>
<connect gate="PWR" pin="VDD@11" pad="59"/>
<connect gate="PWR" pin="VDD@12" pad="52"/>
<connect gate="PWR" pin="VDD@13" pad="26"/>
<connect gate="PWR" pin="VDD@14" pad="15"/>
<connect gate="PWR" pin="VDD@15" pad="158"/>
<connect gate="PWR" pin="VDD@16" pad="103"/>
<connect gate="PWR" pin="VDD@17" pad="39"/>
<connect gate="PWR" pin="VDD@2" pad="185"/>
<connect gate="PWR" pin="VDD@3" pad="171"/>
<connect gate="PWR" pin="VDD@4" pad="150"/>
<connect gate="PWR" pin="VDD@5" pad="137"/>
<connect gate="PWR" pin="VDD@6" pad="124"/>
<connect gate="PWR" pin="VDD@7" pad="115"/>
<connect gate="PWR" pin="VDD@8" pad="94"/>
<connect gate="PWR" pin="VDD@9" pad="83"/>
<connect gate="PWR" pin="VSS@1" pad="202"/>
<connect gate="PWR" pin="VSS@10" pad="72"/>
<connect gate="PWR" pin="VSS@11" pad="60"/>
<connect gate="PWR" pin="VSS@12" pad="51"/>
<connect gate="PWR" pin="VSS@13" pad="25"/>
<connect gate="PWR" pin="VSS@14" pad="14"/>
<connect gate="PWR" pin="VSS@2" pad="184"/>
<connect gate="PWR" pin="VSS@3" pad="170"/>
<connect gate="PWR" pin="VSS@4" pad="149"/>
<connect gate="PWR" pin="VSS@5" pad="136"/>
<connect gate="PWR" pin="VSS@6" pad="125"/>
<connect gate="PWR" pin="VSS@7" pad="114"/>
<connect gate="PWR" pin="VSS@8" pad="93"/>
<connect gate="PWR" pin="VSS@9" pad="82"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F429N*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
168 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_216PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD19_VSS18"/>
</gates>
<devices>
<device name="" package="TFBGA216">
<connects>
<connect gate="MCU" pin="BOOT0" pad="E6"/>
<connect gate="MCU" pin="BYPASS_REG" pad="L5"/>
<connect gate="MCU" pin="NRST" pad="J1"/>
<connect gate="MCU" pin="OSC_IN" pad="G1"/>
<connect gate="MCU" pin="OSC_OUT" pad="H1"/>
<connect gate="MCU" pin="PA0" pad="N3"/>
<connect gate="MCU" pin="PA1" pad="N2"/>
<connect gate="MCU" pin="PA10" pad="D15"/>
<connect gate="MCU" pin="PA11" pad="C15"/>
<connect gate="MCU" pin="PA12" pad="B15"/>
<connect gate="MCU" pin="PA13" pad="A15"/>
<connect gate="MCU" pin="PA14" pad="A14"/>
<connect gate="MCU" pin="PA15" pad="A13"/>
<connect gate="MCU" pin="PA2" pad="P2"/>
<connect gate="MCU" pin="PA3" pad="R2"/>
<connect gate="MCU" pin="PA4" pad="N4"/>
<connect gate="MCU" pin="PA5" pad="P4"/>
<connect gate="MCU" pin="PA6" pad="P3"/>
<connect gate="MCU" pin="PA7" pad="R3"/>
<connect gate="MCU" pin="PA8" pad="F15"/>
<connect gate="MCU" pin="PA9" pad="E15"/>
<connect gate="MCU" pin="PB0" pad="R5"/>
<connect gate="MCU" pin="PB1" pad="R4"/>
<connect gate="MCU" pin="PB10" pad="P12"/>
<connect gate="MCU" pin="PB11" pad="R13"/>
<connect gate="MCU" pin="PB12" pad="L13"/>
<connect gate="MCU" pin="PB13" pad="K14"/>
<connect gate="MCU" pin="PB14" pad="R14"/>
<connect gate="MCU" pin="PB15" pad="R15"/>
<connect gate="MCU" pin="PB2" pad="M5"/>
<connect gate="MCU" pin="PB3" pad="A10"/>
<connect gate="MCU" pin="PB4" pad="A9"/>
<connect gate="MCU" pin="PB5" pad="A8"/>
<connect gate="MCU" pin="PB6" pad="B6"/>
<connect gate="MCU" pin="PB7" pad="B5"/>
<connect gate="MCU" pin="PB8" pad="A7"/>
<connect gate="MCU" pin="PB9" pad="B4"/>
<connect gate="MCU" pin="PC0" pad="M2"/>
<connect gate="MCU" pin="PC1" pad="M3"/>
<connect gate="MCU" pin="PC10" pad="B14"/>
<connect gate="MCU" pin="PC11" pad="B13"/>
<connect gate="MCU" pin="PC12" pad="A12"/>
<connect gate="MCU" pin="PC13" pad="D1"/>
<connect gate="MCU" pin="PC14" pad="E1"/>
<connect gate="MCU" pin="PC15" pad="F1"/>
<connect gate="MCU" pin="PC2" pad="M4"/>
<connect gate="MCU" pin="PC3" pad="L4"/>
<connect gate="MCU" pin="PC4" pad="N5"/>
<connect gate="MCU" pin="PC5" pad="P5"/>
<connect gate="MCU" pin="PC6" pad="H15"/>
<connect gate="MCU" pin="PC7" pad="G15"/>
<connect gate="MCU" pin="PC8" pad="G14"/>
<connect gate="MCU" pin="PC9" pad="F14"/>
<connect gate="MCU" pin="PD0" pad="B12"/>
<connect gate="MCU" pin="PD1" pad="C12"/>
<connect gate="MCU" pin="PD10" pad="K15"/>
<connect gate="MCU" pin="PD11" pad="N10"/>
<connect gate="MCU" pin="PD12" pad="M10"/>
<connect gate="MCU" pin="PD13" pad="M11"/>
<connect gate="MCU" pin="PD14" pad="L12"/>
<connect gate="MCU" pin="PD15" pad="K13"/>
<connect gate="MCU" pin="PD2" pad="D12"/>
<connect gate="MCU" pin="PD3" pad="C11"/>
<connect gate="MCU" pin="PD4" pad="D11"/>
<connect gate="MCU" pin="PD5" pad="C10"/>
<connect gate="MCU" pin="PD6" pad="B11"/>
<connect gate="MCU" pin="PD7" pad="A11"/>
<connect gate="MCU" pin="PD8" pad="L15"/>
<connect gate="MCU" pin="PD9" pad="L14"/>
<connect gate="MCU" pin="PDR_ON" pad="E5"/>
<connect gate="MCU" pin="PE0" pad="A6"/>
<connect gate="MCU" pin="PE1" pad="A5"/>
<connect gate="MCU" pin="PE10" pad="R9"/>
<connect gate="MCU" pin="PE11" pad="P10"/>
<connect gate="MCU" pin="PE12" pad="R10"/>
<connect gate="MCU" pin="PE13" pad="R12"/>
<connect gate="MCU" pin="PE14" pad="P11"/>
<connect gate="MCU" pin="PE15" pad="R11"/>
<connect gate="MCU" pin="PE2" pad="A3"/>
<connect gate="MCU" pin="PE3" pad="A2"/>
<connect gate="MCU" pin="PE4" pad="A1"/>
<connect gate="MCU" pin="PE5" pad="B1"/>
<connect gate="MCU" pin="PE6" pad="B2"/>
<connect gate="MCU" pin="PE7" pad="R8"/>
<connect gate="MCU" pin="PE8" pad="N9"/>
<connect gate="MCU" pin="PE9" pad="P9"/>
<connect gate="MCU" pin="PF0" pad="D2"/>
<connect gate="MCU" pin="PF1" pad="E2"/>
<connect gate="MCU" pin="PF10" pad="L1"/>
<connect gate="MCU" pin="PF11" pad="P8"/>
<connect gate="MCU" pin="PF12" pad="M6"/>
<connect gate="MCU" pin="PF13" pad="N6"/>
<connect gate="MCU" pin="PF14" pad="P6"/>
<connect gate="MCU" pin="PF15" pad="M8"/>
<connect gate="MCU" pin="PF2" pad="G2"/>
<connect gate="MCU" pin="PF3" pad="H2"/>
<connect gate="MCU" pin="PF4" pad="J2"/>
<connect gate="MCU" pin="PF5" pad="K3"/>
<connect gate="MCU" pin="PF6" pad="K2"/>
<connect gate="MCU" pin="PF7" pad="K1"/>
<connect gate="MCU" pin="PF8" pad="L3"/>
<connect gate="MCU" pin="PF9" pad="L2"/>
<connect gate="MCU" pin="PG0" pad="N7"/>
<connect gate="MCU" pin="PG1" pad="M7"/>
<connect gate="MCU" pin="PG10" pad="C8"/>
<connect gate="MCU" pin="PG11" pad="B8"/>
<connect gate="MCU" pin="PG12" pad="C7"/>
<connect gate="MCU" pin="PG13" pad="B3"/>
<connect gate="MCU" pin="PG14" pad="A4"/>
<connect gate="MCU" pin="PG15" pad="B7"/>
<connect gate="MCU" pin="PG2" pad="M13"/>
<connect gate="MCU" pin="PG3" pad="M12"/>
<connect gate="MCU" pin="PG4" pad="N12"/>
<connect gate="MCU" pin="PG5" pad="N11"/>
<connect gate="MCU" pin="PG6" pad="J15"/>
<connect gate="MCU" pin="PG7" pad="J14"/>
<connect gate="MCU" pin="PG8" pad="H14"/>
<connect gate="MCU" pin="PG9" pad="D9"/>
<connect gate="MCU" pin="PH10" pad="P15"/>
<connect gate="MCU" pin="PH11" pad="N15"/>
<connect gate="MCU" pin="PH12" pad="M15"/>
<connect gate="MCU" pin="PH13" pad="E12"/>
<connect gate="MCU" pin="PH14" pad="E13"/>
<connect gate="MCU" pin="PH15" pad="D13"/>
<connect gate="MCU" pin="PH2" pad="K4"/>
<connect gate="MCU" pin="PH3" pad="J4"/>
<connect gate="MCU" pin="PH4" pad="H4"/>
<connect gate="MCU" pin="PH5" pad="J3"/>
<connect gate="MCU" pin="PH6" pad="P13"/>
<connect gate="MCU" pin="PH7" pad="N13"/>
<connect gate="MCU" pin="PH8" pad="P14"/>
<connect gate="MCU" pin="PH9" pad="N14"/>
<connect gate="MCU" pin="PI0" pad="E14"/>
<connect gate="MCU" pin="PI1" pad="D14"/>
<connect gate="MCU" pin="PI10" pad="D5"/>
<connect gate="MCU" pin="PI11" pad="F3"/>
<connect gate="MCU" pin="PI12" pad="E3"/>
<connect gate="MCU" pin="PI13" pad="G3"/>
<connect gate="MCU" pin="PI14" pad="H3"/>
<connect gate="MCU" pin="PI15" pad="G4"/>
<connect gate="MCU" pin="PI2" pad="C14"/>
<connect gate="MCU" pin="PI3" pad="C13"/>
<connect gate="MCU" pin="PI4" pad="C3"/>
<connect gate="MCU" pin="PI5" pad="D3"/>
<connect gate="MCU" pin="PI6" pad="D6"/>
<connect gate="MCU" pin="PI7" pad="D4"/>
<connect gate="MCU" pin="PI8" pad="C2"/>
<connect gate="MCU" pin="PI9" pad="E4"/>
<connect gate="MCU" pin="PJ0" pad="R6"/>
<connect gate="MCU" pin="PJ1" pad="R7"/>
<connect gate="MCU" pin="PJ10" pad="H13"/>
<connect gate="MCU" pin="PJ11" pad="G12"/>
<connect gate="MCU" pin="PJ12" pad="B10"/>
<connect gate="MCU" pin="PJ13" pad="B9"/>
<connect gate="MCU" pin="PJ14" pad="C9"/>
<connect gate="MCU" pin="PJ15" pad="D10"/>
<connect gate="MCU" pin="PJ2" pad="P7"/>
<connect gate="MCU" pin="PJ3" pad="N8"/>
<connect gate="MCU" pin="PJ4" pad="M9"/>
<connect gate="MCU" pin="PJ5" pad="M14"/>
<connect gate="MCU" pin="PJ6" pad="K12"/>
<connect gate="MCU" pin="PJ7" pad="J12"/>
<connect gate="MCU" pin="PJ8" pad="H12"/>
<connect gate="MCU" pin="PJ9" pad="J13"/>
<connect gate="MCU" pin="PK0" pad="G13"/>
<connect gate="MCU" pin="PK1" pad="F12"/>
<connect gate="MCU" pin="PK2" pad="F13"/>
<connect gate="MCU" pin="PK3" pad="D8"/>
<connect gate="MCU" pin="PK4" pad="D7"/>
<connect gate="MCU" pin="PK5" pad="C6"/>
<connect gate="MCU" pin="PK6" pad="C5"/>
<connect gate="MCU" pin="PK7" pad="C4"/>
<connect gate="MCU" pin="VBAT" pad="C1"/>
<connect gate="MCU" pin="VCAP1" pad="L11"/>
<connect gate="MCU" pin="VCAP2" pad="E11"/>
<connect gate="MCU" pin="VDDA" pad="R1"/>
<connect gate="MCU" pin="VREF+" pad="P1"/>
<connect gate="MCU" pin="VREF-" pad="N1"/>
<connect gate="MCU" pin="VSSA" pad="M1"/>
<connect gate="PWR" pin="VDD@1" pad="E7"/>
<connect gate="PWR" pin="VDD@10" pad="H5"/>
<connect gate="PWR" pin="VDD@11" pad="H11"/>
<connect gate="PWR" pin="VDD@12" pad="J5"/>
<connect gate="PWR" pin="VDD@13" pad="J11"/>
<connect gate="PWR" pin="VDD@14" pad="K5"/>
<connect gate="PWR" pin="VDD@15" pad="K11"/>
<connect gate="PWR" pin="VDD@16" pad="L7"/>
<connect gate="PWR" pin="VDD@17" pad="L8"/>
<connect gate="PWR" pin="VDD@18" pad="L9"/>
<connect gate="PWR" pin="VDD@19" pad="L10"/>
<connect gate="PWR" pin="VDD@2" pad="E8"/>
<connect gate="PWR" pin="VDD@3" pad="E9"/>
<connect gate="PWR" pin="VDD@4" pad="E10"/>
<connect gate="PWR" pin="VDD@5" pad="F4"/>
<connect gate="PWR" pin="VDD@6" pad="F5"/>
<connect gate="PWR" pin="VDD@7" pad="F11"/>
<connect gate="PWR" pin="VDD@8" pad="G5"/>
<connect gate="PWR" pin="VDD@9" pad="G11"/>
<connect gate="PWR" pin="VSS@1" pad="F2"/>
<connect gate="PWR" pin="VSS@10" pad="H10"/>
<connect gate="PWR" pin="VSS@11" pad="J6"/>
<connect gate="PWR" pin="VSS@12" pad="J10"/>
<connect gate="PWR" pin="VSS@13" pad="K6"/>
<connect gate="PWR" pin="VSS@14" pad="K7"/>
<connect gate="PWR" pin="VSS@15" pad="K8"/>
<connect gate="PWR" pin="VSS@16" pad="K9"/>
<connect gate="PWR" pin="VSS@17" pad="K10"/>
<connect gate="PWR" pin="VSS@18" pad="L6"/>
<connect gate="PWR" pin="VSS@2" pad="F6"/>
<connect gate="PWR" pin="VSS@3" pad="F7"/>
<connect gate="PWR" pin="VSS@4" pad="F8"/>
<connect gate="PWR" pin="VSS@5" pad="F9"/>
<connect gate="PWR" pin="VSS@6" pad="F10"/>
<connect gate="PWR" pin="VSS@7" pad="G6"/>
<connect gate="PWR" pin="VSS@8" pad="G10"/>
<connect gate="PWR" pin="VSS@9" pad="H6"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F437V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP9"/>
<gate name="PWR" symbol="PWR_VDD6_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="49"/>
<connect gate="MCU" pin="VCAP2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="100"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="28"/>
<connect gate="PWR" pin="VDD@4" pad="11"/>
<connect gate="PWR" pin="VDD@5" pad="50"/>
<connect gate="PWR" pin="VDD@6" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="99"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
<connect gate="PWR" pin="VSS@3" pad="27"/>
<connect gate="PWR" pin="VSS@4" pad="10"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F437Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD12_VSS9"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PDR_ON" pad="143"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="71"/>
<connect gate="MCU" pin="VCAP2" pad="106"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VSSA" pad="31"/>
<connect gate="PWR" pin="VDD@1" pad="131"/>
<connect gate="PWR" pin="VDD@10" pad="144"/>
<connect gate="PWR" pin="VDD@11" pad="72"/>
<connect gate="PWR" pin="VDD@12" pad="30"/>
<connect gate="PWR" pin="VDD@2" pad="121"/>
<connect gate="PWR" pin="VDD@3" pad="108"/>
<connect gate="PWR" pin="VDD@4" pad="95"/>
<connect gate="PWR" pin="VDD@5" pad="84"/>
<connect gate="PWR" pin="VDD@6" pad="62"/>
<connect gate="PWR" pin="VDD@7" pad="52"/>
<connect gate="PWR" pin="VDD@8" pad="39"/>
<connect gate="PWR" pin="VDD@9" pad="17"/>
<connect gate="PWR" pin="VSS@1" pad="130"/>
<connect gate="PWR" pin="VSS@2" pad="120"/>
<connect gate="PWR" pin="VSS@3" pad="107"/>
<connect gate="PWR" pin="VSS@4" pad="94"/>
<connect gate="PWR" pin="VSS@5" pad="83"/>
<connect gate="PWR" pin="VSS@6" pad="61"/>
<connect gate="PWR" pin="VSS@7" pad="51"/>
<connect gate="PWR" pin="VSS@8" pad="38"/>
<connect gate="PWR" pin="VSS@9" pad="16"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F437Z*Y" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_143PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD13_VSS6"/>
</gates>
<devices>
<device name="" package="WLCSP143">
<connects>
<connect gate="MCU" pin="BOOT0" pad="C9"/>
<connect gate="MCU" pin="BYPASS_REG" pad="N11"/>
<connect gate="MCU" pin="NRST" pad="H9"/>
<connect gate="MCU" pin="OSC_IN" pad="J11"/>
<connect gate="MCU" pin="OSC_OUT" pad="H10"/>
<connect gate="MCU" pin="PA0" pad="K9"/>
<connect gate="MCU" pin="PA1" pad="K8"/>
<connect gate="MCU" pin="PA10" pad="D5"/>
<connect gate="MCU" pin="PA11" pad="D4"/>
<connect gate="MCU" pin="PA12" pad="E1"/>
<connect gate="MCU" pin="PA13" pad="D3"/>
<connect gate="MCU" pin="PA14" pad="B1"/>
<connect gate="MCU" pin="PA15" pad="C2"/>
<connect gate="MCU" pin="PA2" pad="L9"/>
<connect gate="MCU" pin="PA3" pad="M11"/>
<connect gate="MCU" pin="PA4" pad="M10"/>
<connect gate="MCU" pin="PA5" pad="M9"/>
<connect gate="MCU" pin="PA6" pad="N10"/>
<connect gate="MCU" pin="PA7" pad="L8"/>
<connect gate="MCU" pin="PA8" pad="F1"/>
<connect gate="MCU" pin="PA9" pad="E2"/>
<connect gate="MCU" pin="PB0" pad="N8"/>
<connect gate="MCU" pin="PB1" pad="K7"/>
<connect gate="MCU" pin="PB10" pad="M3"/>
<connect gate="MCU" pin="PB11" pad="N3"/>
<connect gate="MCU" pin="PB12" pad="M2"/>
<connect gate="MCU" pin="PB13" pad="N1"/>
<connect gate="MCU" pin="PB14" pad="K3"/>
<connect gate="MCU" pin="PB15" pad="J3"/>
<connect gate="MCU" pin="PB2" pad="L7"/>
<connect gate="MCU" pin="PB3" pad="B7"/>
<connect gate="MCU" pin="PB4" pad="C7"/>
<connect gate="MCU" pin="PB5" pad="C8"/>
<connect gate="MCU" pin="PB6" pad="A8"/>
<connect gate="MCU" pin="PB7" pad="B8"/>
<connect gate="MCU" pin="PB8" pad="A9"/>
<connect gate="MCU" pin="PB9" pad="B9"/>
<connect gate="MCU" pin="PC0" pad="H8"/>
<connect gate="MCU" pin="PC1" pad="K11"/>
<connect gate="MCU" pin="PC10" pad="A2"/>
<connect gate="MCU" pin="PC11" pad="B2"/>
<connect gate="MCU" pin="PC12" pad="C3"/>
<connect gate="MCU" pin="PC13" pad="D10"/>
<connect gate="MCU" pin="PC14" pad="D11"/>
<connect gate="MCU" pin="PC15" pad="E11"/>
<connect gate="MCU" pin="PC2" pad="J10"/>
<connect gate="MCU" pin="PC3" pad="J9"/>
<connect gate="MCU" pin="PC4" pad="M8"/>
<connect gate="MCU" pin="PC5" pad="N9"/>
<connect gate="MCU" pin="PC6" pad="F2"/>
<connect gate="MCU" pin="PC7" pad="F3"/>
<connect gate="MCU" pin="PC8" pad="E4"/>
<connect gate="MCU" pin="PC9" pad="E3"/>
<connect gate="MCU" pin="PD0" pad="B3"/>
<connect gate="MCU" pin="PD1" pad="C4"/>
<connect gate="MCU" pin="PD10" pad="H4"/>
<connect gate="MCU" pin="PD11" pad="K2"/>
<connect gate="MCU" pin="PD12" pad="H6"/>
<connect gate="MCU" pin="PD13" pad="H5"/>
<connect gate="MCU" pin="PD14" pad="J2"/>
<connect gate="MCU" pin="PD15" pad="K1"/>
<connect gate="MCU" pin="PD2" pad="A3"/>
<connect gate="MCU" pin="PD3" pad="B4"/>
<connect gate="MCU" pin="PD4" pad="B5"/>
<connect gate="MCU" pin="PD5" pad="A4"/>
<connect gate="MCU" pin="PD6" pad="F4"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD8" pad="L2"/>
<connect gate="MCU" pin="PD9" pad="M1"/>
<connect gate="MCU" pin="PDR_ON" pad="A11"/>
<connect gate="MCU" pin="PE0" pad="B10"/>
<connect gate="MCU" pin="PE1" pad="A10"/>
<connect gate="MCU" pin="PE10" pad="J4"/>
<connect gate="MCU" pin="PE11" pad="K4"/>
<connect gate="MCU" pin="PE12" pad="L4"/>
<connect gate="MCU" pin="PE13" pad="N4"/>
<connect gate="MCU" pin="PE14" pad="M4"/>
<connect gate="MCU" pin="PE15" pad="L3"/>
<connect gate="MCU" pin="PE2" pad="D8"/>
<connect gate="MCU" pin="PE3" pad="C10"/>
<connect gate="MCU" pin="PE4" pad="B11"/>
<connect gate="MCU" pin="PE5" pad="D9"/>
<connect gate="MCU" pin="PE6" pad="E8"/>
<connect gate="MCU" pin="PE7" pad="L5"/>
<connect gate="MCU" pin="PE8" pad="M5"/>
<connect gate="MCU" pin="PE9" pad="N5"/>
<connect gate="MCU" pin="PF0" pad="F11"/>
<connect gate="MCU" pin="PF1" pad="E9"/>
<connect gate="MCU" pin="PF10" pad="G9"/>
<connect gate="MCU" pin="PF11" pad="M7"/>
<connect gate="MCU" pin="PF12" pad="N7"/>
<connect gate="MCU" pin="PF13" pad="K6"/>
<connect gate="MCU" pin="PF14" pad="L6"/>
<connect gate="MCU" pin="PF15" pad="M6"/>
<connect gate="MCU" pin="PF2" pad="F10"/>
<connect gate="MCU" pin="PF3" pad="G11"/>
<connect gate="MCU" pin="PF4" pad="F9"/>
<connect gate="MCU" pin="PF5" pad="F8"/>
<connect gate="MCU" pin="PF6" pad="G10"/>
<connect gate="MCU" pin="PF7" pad="F7"/>
<connect gate="MCU" pin="PF8" pad="H11"/>
<connect gate="MCU" pin="PF9" pad="G8"/>
<connect gate="MCU" pin="PG0" pad="N6"/>
<connect gate="MCU" pin="PG1" pad="K5"/>
<connect gate="MCU" pin="PG10" pad="C6"/>
<connect gate="MCU" pin="PG11" pad="B6"/>
<connect gate="MCU" pin="PG12" pad="A6"/>
<connect gate="MCU" pin="PG13" pad="D6"/>
<connect gate="MCU" pin="PG14" pad="F6"/>
<connect gate="MCU" pin="PG15" pad="A7"/>
<connect gate="MCU" pin="PG2" pad="J1"/>
<connect gate="MCU" pin="PG3" pad="G3"/>
<connect gate="MCU" pin="PG4" pad="G5"/>
<connect gate="MCU" pin="PG5" pad="G6"/>
<connect gate="MCU" pin="PG6" pad="G4"/>
<connect gate="MCU" pin="PG7" pad="H1"/>
<connect gate="MCU" pin="PG8" pad="G2"/>
<connect gate="MCU" pin="PG9" pad="E5"/>
<connect gate="MCU" pin="VBAT" pad="C11"/>
<connect gate="MCU" pin="VCAP1" pad="N2"/>
<connect gate="MCU" pin="VCAP2" pad="D1"/>
<connect gate="MCU" pin="VDDA" pad="L10"/>
<connect gate="MCU" pin="VREF+" pad="L11"/>
<connect gate="MCU" pin="VSSA" pad="K10"/>
<connect gate="PWR" pin="VDD@1" pad="A1"/>
<connect gate="PWR" pin="VDD@10" pad="J6"/>
<connect gate="PWR" pin="VDD@11" pad="J7"/>
<connect gate="PWR" pin="VDD@12" pad="J8"/>
<connect gate="PWR" pin="VDD@13" pad="L1"/>
<connect gate="PWR" pin="VDD@2" pad="C1"/>
<connect gate="PWR" pin="VDD@3" pad="C5"/>
<connect gate="PWR" pin="VDD@4" pad="D7"/>
<connect gate="PWR" pin="VDD@5" pad="E6"/>
<connect gate="PWR" pin="VDD@6" pad="E10"/>
<connect gate="PWR" pin="VDD@7" pad="G1"/>
<connect gate="PWR" pin="VDD@8" pad="G7"/>
<connect gate="PWR" pin="VDD@9" pad="J5"/>
<connect gate="PWR" pin="VSS@1" pad="D2"/>
<connect gate="PWR" pin="VSS@2" pad="E7"/>
<connect gate="PWR" pin="VSS@3" pad="F5"/>
<connect gate="PWR" pin="VSS@4" pad="H2"/>
<connect gate="PWR" pin="VSS@5" pad="H3"/>
<connect gate="PWR" pin="VSS@6" pad="H7"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F437I*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD15_VSS11"/>
</gates>
<devices>
<device name="" package="LQFP176">
<connects>
<connect gate="MCU" pin="BOOT0" pad="166"/>
<connect gate="MCU" pin="BYPASS_REG" pad="48"/>
<connect gate="MCU" pin="NRST" pad="31"/>
<connect gate="MCU" pin="OSC_IN" pad="29"/>
<connect gate="MCU" pin="OSC_OUT" pad="30"/>
<connect gate="MCU" pin="PA0" pad="40"/>
<connect gate="MCU" pin="PA1" pad="41"/>
<connect gate="MCU" pin="PA10" pad="121"/>
<connect gate="MCU" pin="PA11" pad="122"/>
<connect gate="MCU" pin="PA12" pad="123"/>
<connect gate="MCU" pin="PA13" pad="124"/>
<connect gate="MCU" pin="PA14" pad="137"/>
<connect gate="MCU" pin="PA15" pad="138"/>
<connect gate="MCU" pin="PA2" pad="42"/>
<connect gate="MCU" pin="PA3" pad="47"/>
<connect gate="MCU" pin="PA4" pad="50"/>
<connect gate="MCU" pin="PA5" pad="51"/>
<connect gate="MCU" pin="PA6" pad="52"/>
<connect gate="MCU" pin="PA7" pad="53"/>
<connect gate="MCU" pin="PA8" pad="119"/>
<connect gate="MCU" pin="PA9" pad="120"/>
<connect gate="MCU" pin="PB0" pad="56"/>
<connect gate="MCU" pin="PB1" pad="57"/>
<connect gate="MCU" pin="PB10" pad="79"/>
<connect gate="MCU" pin="PB11" pad="80"/>
<connect gate="MCU" pin="PB12" pad="92"/>
<connect gate="MCU" pin="PB13" pad="93"/>
<connect gate="MCU" pin="PB14" pad="94"/>
<connect gate="MCU" pin="PB15" pad="95"/>
<connect gate="MCU" pin="PB2" pad="58"/>
<connect gate="MCU" pin="PB3" pad="161"/>
<connect gate="MCU" pin="PB4" pad="162"/>
<connect gate="MCU" pin="PB5" pad="163"/>
<connect gate="MCU" pin="PB6" pad="164"/>
<connect gate="MCU" pin="PB7" pad="165"/>
<connect gate="MCU" pin="PB8" pad="167"/>
<connect gate="MCU" pin="PB9" pad="168"/>
<connect gate="MCU" pin="PC0" pad="32"/>
<connect gate="MCU" pin="PC1" pad="33"/>
<connect gate="MCU" pin="PC10" pad="139"/>
<connect gate="MCU" pin="PC11" pad="140"/>
<connect gate="MCU" pin="PC12" pad="141"/>
<connect gate="MCU" pin="PC13" pad="8"/>
<connect gate="MCU" pin="PC14" pad="9"/>
<connect gate="MCU" pin="PC15" pad="10"/>
<connect gate="MCU" pin="PC2" pad="34"/>
<connect gate="MCU" pin="PC3" pad="35"/>
<connect gate="MCU" pin="PC4" pad="54"/>
<connect gate="MCU" pin="PC5" pad="55"/>
<connect gate="MCU" pin="PC6" pad="115"/>
<connect gate="MCU" pin="PC7" pad="116"/>
<connect gate="MCU" pin="PC8" pad="117"/>
<connect gate="MCU" pin="PC9" pad="118"/>
<connect gate="MCU" pin="PD0" pad="142"/>
<connect gate="MCU" pin="PD1" pad="143"/>
<connect gate="MCU" pin="PD10" pad="98"/>
<connect gate="MCU" pin="PD11" pad="99"/>
<connect gate="MCU" pin="PD12" pad="100"/>
<connect gate="MCU" pin="PD13" pad="101"/>
<connect gate="MCU" pin="PD14" pad="104"/>
<connect gate="MCU" pin="PD15" pad="105"/>
<connect gate="MCU" pin="PD2" pad="144"/>
<connect gate="MCU" pin="PD3" pad="145"/>
<connect gate="MCU" pin="PD4" pad="146"/>
<connect gate="MCU" pin="PD5" pad="147"/>
<connect gate="MCU" pin="PD6" pad="150"/>
<connect gate="MCU" pin="PD7" pad="151"/>
<connect gate="MCU" pin="PD8" pad="96"/>
<connect gate="MCU" pin="PD9" pad="97"/>
<connect gate="MCU" pin="PDR_ON" pad="171"/>
<connect gate="MCU" pin="PE0" pad="169"/>
<connect gate="MCU" pin="PE1" pad="170"/>
<connect gate="MCU" pin="PE10" pad="73"/>
<connect gate="MCU" pin="PE11" pad="74"/>
<connect gate="MCU" pin="PE12" pad="75"/>
<connect gate="MCU" pin="PE13" pad="76"/>
<connect gate="MCU" pin="PE14" pad="77"/>
<connect gate="MCU" pin="PE15" pad="78"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="68"/>
<connect gate="MCU" pin="PE8" pad="69"/>
<connect gate="MCU" pin="PE9" pad="70"/>
<connect gate="MCU" pin="PF0" pad="16"/>
<connect gate="MCU" pin="PF1" pad="17"/>
<connect gate="MCU" pin="PF10" pad="28"/>
<connect gate="MCU" pin="PF11" pad="59"/>
<connect gate="MCU" pin="PF12" pad="60"/>
<connect gate="MCU" pin="PF13" pad="63"/>
<connect gate="MCU" pin="PF14" pad="64"/>
<connect gate="MCU" pin="PF15" pad="65"/>
<connect gate="MCU" pin="PF2" pad="18"/>
<connect gate="MCU" pin="PF3" pad="19"/>
<connect gate="MCU" pin="PF4" pad="20"/>
<connect gate="MCU" pin="PF5" pad="21"/>
<connect gate="MCU" pin="PF6" pad="24"/>
<connect gate="MCU" pin="PF7" pad="25"/>
<connect gate="MCU" pin="PF8" pad="26"/>
<connect gate="MCU" pin="PF9" pad="27"/>
<connect gate="MCU" pin="PG0" pad="66"/>
<connect gate="MCU" pin="PG1" pad="67"/>
<connect gate="MCU" pin="PG10" pad="153"/>
<connect gate="MCU" pin="PG11" pad="154"/>
<connect gate="MCU" pin="PG12" pad="155"/>
<connect gate="MCU" pin="PG13" pad="156"/>
<connect gate="MCU" pin="PG14" pad="157"/>
<connect gate="MCU" pin="PG15" pad="160"/>
<connect gate="MCU" pin="PG2" pad="106"/>
<connect gate="MCU" pin="PG3" pad="107"/>
<connect gate="MCU" pin="PG4" pad="108"/>
<connect gate="MCU" pin="PG5" pad="109"/>
<connect gate="MCU" pin="PG6" pad="110"/>
<connect gate="MCU" pin="PG7" pad="111"/>
<connect gate="MCU" pin="PG8" pad="112"/>
<connect gate="MCU" pin="PG9" pad="152"/>
<connect gate="MCU" pin="PH10" pad="87"/>
<connect gate="MCU" pin="PH11" pad="88"/>
<connect gate="MCU" pin="PH12" pad="89"/>
<connect gate="MCU" pin="PH13" pad="128"/>
<connect gate="MCU" pin="PH14" pad="129"/>
<connect gate="MCU" pin="PH15" pad="130"/>
<connect gate="MCU" pin="PH2" pad="43"/>
<connect gate="MCU" pin="PH3" pad="44"/>
<connect gate="MCU" pin="PH4" pad="45"/>
<connect gate="MCU" pin="PH5" pad="46"/>
<connect gate="MCU" pin="PH6" pad="83"/>
<connect gate="MCU" pin="PH7" pad="84"/>
<connect gate="MCU" pin="PH8" pad="85"/>
<connect gate="MCU" pin="PH9" pad="86"/>
<connect gate="MCU" pin="PI0" pad="131"/>
<connect gate="MCU" pin="PI1" pad="132"/>
<connect gate="MCU" pin="PI10" pad="12"/>
<connect gate="MCU" pin="PI11" pad="13"/>
<connect gate="MCU" pin="PI2" pad="133"/>
<connect gate="MCU" pin="PI3" pad="134"/>
<connect gate="MCU" pin="PI4" pad="173"/>
<connect gate="MCU" pin="PI5" pad="174"/>
<connect gate="MCU" pin="PI6" pad="175"/>
<connect gate="MCU" pin="PI7" pad="176"/>
<connect gate="MCU" pin="PI8" pad="7"/>
<connect gate="MCU" pin="PI9" pad="11"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="81"/>
<connect gate="MCU" pin="VCAP2" pad="125"/>
<connect gate="MCU" pin="VDDA" pad="39"/>
<connect gate="MCU" pin="VREF+" pad="38"/>
<connect gate="MCU" pin="VSSA" pad="37"/>
<connect gate="PWR" pin="VDD@1" pad="159"/>
<connect gate="PWR" pin="VDD@10" pad="23"/>
<connect gate="PWR" pin="VDD@11" pad="15"/>
<connect gate="PWR" pin="VDD@12" pad="172"/>
<connect gate="PWR" pin="VDD@13" pad="82"/>
<connect gate="PWR" pin="VDD@14" pad="49"/>
<connect gate="PWR" pin="VDD@15" pad="36"/>
<connect gate="PWR" pin="VDD@2" pad="149"/>
<connect gate="PWR" pin="VDD@3" pad="136"/>
<connect gate="PWR" pin="VDD@4" pad="127"/>
<connect gate="PWR" pin="VDD@5" pad="114"/>
<connect gate="PWR" pin="VDD@6" pad="103"/>
<connect gate="PWR" pin="VDD@7" pad="91"/>
<connect gate="PWR" pin="VDD@8" pad="72"/>
<connect gate="PWR" pin="VDD@9" pad="62"/>
<connect gate="PWR" pin="VSS@1" pad="158"/>
<connect gate="PWR" pin="VSS@10" pad="22"/>
<connect gate="PWR" pin="VSS@11" pad="14"/>
<connect gate="PWR" pin="VSS@2" pad="148"/>
<connect gate="PWR" pin="VSS@3" pad="135"/>
<connect gate="PWR" pin="VSS@4" pad="126"/>
<connect gate="PWR" pin="VSS@5" pad="113"/>
<connect gate="PWR" pin="VSS@6" pad="102"/>
<connect gate="PWR" pin="VSS@7" pad="90"/>
<connect gate="PWR" pin="VSS@8" pad="71"/>
<connect gate="PWR" pin="VSS@9" pad="61"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F437I*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD14_VSS36"/>
</gates>
<devices>
<device name="" package="UFBGA176+25">
<connects>
<connect gate="MCU" pin="BOOT0" pad="D6"/>
<connect gate="MCU" pin="BYPASS_REG" pad="L4"/>
<connect gate="MCU" pin="NRST" pad="J1"/>
<connect gate="MCU" pin="OSC_IN" pad="G1"/>
<connect gate="MCU" pin="OSC_OUT" pad="H1"/>
<connect gate="MCU" pin="PA0" pad="N3"/>
<connect gate="MCU" pin="PA1" pad="N2"/>
<connect gate="MCU" pin="PA10" pad="D15"/>
<connect gate="MCU" pin="PA11" pad="C15"/>
<connect gate="MCU" pin="PA12" pad="B15"/>
<connect gate="MCU" pin="PA13" pad="A15"/>
<connect gate="MCU" pin="PA14" pad="A14"/>
<connect gate="MCU" pin="PA15" pad="A13"/>
<connect gate="MCU" pin="PA2" pad="P2"/>
<connect gate="MCU" pin="PA3" pad="R2"/>
<connect gate="MCU" pin="PA4" pad="N4"/>
<connect gate="MCU" pin="PA5" pad="P4"/>
<connect gate="MCU" pin="PA6" pad="P3"/>
<connect gate="MCU" pin="PA7" pad="R3"/>
<connect gate="MCU" pin="PA8" pad="F15"/>
<connect gate="MCU" pin="PA9" pad="E15"/>
<connect gate="MCU" pin="PB0" pad="R5"/>
<connect gate="MCU" pin="PB1" pad="R4"/>
<connect gate="MCU" pin="PB10" pad="R12"/>
<connect gate="MCU" pin="PB11" pad="R13"/>
<connect gate="MCU" pin="PB12" pad="P12"/>
<connect gate="MCU" pin="PB13" pad="P13"/>
<connect gate="MCU" pin="PB14" pad="R14"/>
<connect gate="MCU" pin="PB15" pad="R15"/>
<connect gate="MCU" pin="PB2" pad="M6"/>
<connect gate="MCU" pin="PB3" pad="A10"/>
<connect gate="MCU" pin="PB4" pad="A9"/>
<connect gate="MCU" pin="PB5" pad="A6"/>
<connect gate="MCU" pin="PB6" pad="B6"/>
<connect gate="MCU" pin="PB7" pad="B5"/>
<connect gate="MCU" pin="PB8" pad="A5"/>
<connect gate="MCU" pin="PB9" pad="B4"/>
<connect gate="MCU" pin="PC0" pad="M2"/>
<connect gate="MCU" pin="PC1" pad="M3"/>
<connect gate="MCU" pin="PC10" pad="B14"/>
<connect gate="MCU" pin="PC11" pad="B13"/>
<connect gate="MCU" pin="PC12" pad="A12"/>
<connect gate="MCU" pin="PC13" pad="D1"/>
<connect gate="MCU" pin="PC14" pad="E1"/>
<connect gate="MCU" pin="PC15" pad="F1"/>
<connect gate="MCU" pin="PC2" pad="M4"/>
<connect gate="MCU" pin="PC3" pad="M5"/>
<connect gate="MCU" pin="PC4" pad="N5"/>
<connect gate="MCU" pin="PC5" pad="P5"/>
<connect gate="MCU" pin="PC6" pad="H15"/>
<connect gate="MCU" pin="PC7" pad="G15"/>
<connect gate="MCU" pin="PC8" pad="G14"/>
<connect gate="MCU" pin="PC9" pad="F14"/>
<connect gate="MCU" pin="PD0" pad="B12"/>
<connect gate="MCU" pin="PD1" pad="C12"/>
<connect gate="MCU" pin="PD10" pad="N15"/>
<connect gate="MCU" pin="PD11" pad="N14"/>
<connect gate="MCU" pin="PD12" pad="N13"/>
<connect gate="MCU" pin="PD13" pad="M15"/>
<connect gate="MCU" pin="PD14" pad="M14"/>
<connect gate="MCU" pin="PD15" pad="L14"/>
<connect gate="MCU" pin="PD2" pad="D12"/>
<connect gate="MCU" pin="PD3" pad="D11"/>
<connect gate="MCU" pin="PD4" pad="D10"/>
<connect gate="MCU" pin="PD5" pad="C11"/>
<connect gate="MCU" pin="PD6" pad="B11"/>
<connect gate="MCU" pin="PD7" pad="A11"/>
<connect gate="MCU" pin="PD8" pad="P15"/>
<connect gate="MCU" pin="PD9" pad="P14"/>
<connect gate="MCU" pin="PDR_ON" pad="C6"/>
<connect gate="MCU" pin="PE0" pad="A4"/>
<connect gate="MCU" pin="PE1" pad="A3"/>
<connect gate="MCU" pin="PE10" pad="R9"/>
<connect gate="MCU" pin="PE11" pad="P10"/>
<connect gate="MCU" pin="PE12" pad="R10"/>
<connect gate="MCU" pin="PE13" pad="N11"/>
<connect gate="MCU" pin="PE14" pad="P11"/>
<connect gate="MCU" pin="PE15" pad="R11"/>
<connect gate="MCU" pin="PE2" pad="A2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="B2"/>
<connect gate="MCU" pin="PE6" pad="B3"/>
<connect gate="MCU" pin="PE7" pad="R8"/>
<connect gate="MCU" pin="PE8" pad="P8"/>
<connect gate="MCU" pin="PE9" pad="P9"/>
<connect gate="MCU" pin="PF0" pad="E2"/>
<connect gate="MCU" pin="PF1" pad="H3"/>
<connect gate="MCU" pin="PF10" pad="L1"/>
<connect gate="MCU" pin="PF11" pad="R6"/>
<connect gate="MCU" pin="PF12" pad="P6"/>
<connect gate="MCU" pin="PF13" pad="N6"/>
<connect gate="MCU" pin="PF14" pad="R7"/>
<connect gate="MCU" pin="PF15" pad="P7"/>
<connect gate="MCU" pin="PF2" pad="H2"/>
<connect gate="MCU" pin="PF3" pad="J2"/>
<connect gate="MCU" pin="PF4" pad="J3"/>
<connect gate="MCU" pin="PF5" pad="K3"/>
<connect gate="MCU" pin="PF6" pad="K2"/>
<connect gate="MCU" pin="PF7" pad="K1"/>
<connect gate="MCU" pin="PF8" pad="L3"/>
<connect gate="MCU" pin="PF9" pad="L2"/>
<connect gate="MCU" pin="PG0" pad="N7"/>
<connect gate="MCU" pin="PG1" pad="M7"/>
<connect gate="MCU" pin="PG10" pad="B10"/>
<connect gate="MCU" pin="PG11" pad="B9"/>
<connect gate="MCU" pin="PG12" pad="B8"/>
<connect gate="MCU" pin="PG13" pad="A8"/>
<connect gate="MCU" pin="PG14" pad="A7"/>
<connect gate="MCU" pin="PG15" pad="B7"/>
<connect gate="MCU" pin="PG2" pad="L15"/>
<connect gate="MCU" pin="PG3" pad="K15"/>
<connect gate="MCU" pin="PG4" pad="K14"/>
<connect gate="MCU" pin="PG5" pad="K13"/>
<connect gate="MCU" pin="PG6" pad="J15"/>
<connect gate="MCU" pin="PG7" pad="J14"/>
<connect gate="MCU" pin="PG8" pad="H14"/>
<connect gate="MCU" pin="PG9" pad="C10"/>
<connect gate="MCU" pin="PH10" pad="L13"/>
<connect gate="MCU" pin="PH11" pad="L12"/>
<connect gate="MCU" pin="PH12" pad="K12"/>
<connect gate="MCU" pin="PH13" pad="E12"/>
<connect gate="MCU" pin="PH14" pad="E13"/>
<connect gate="MCU" pin="PH15" pad="D13"/>
<connect gate="MCU" pin="PH2" pad="F4"/>
<connect gate="MCU" pin="PH3" pad="G4"/>
<connect gate="MCU" pin="PH4" pad="H4"/>
<connect gate="MCU" pin="PH5" pad="J4"/>
<connect gate="MCU" pin="PH6" pad="M11"/>
<connect gate="MCU" pin="PH7" pad="N12"/>
<connect gate="MCU" pin="PH8" pad="M12"/>
<connect gate="MCU" pin="PH9" pad="M13"/>
<connect gate="MCU" pin="PI0" pad="E14"/>
<connect gate="MCU" pin="PI1" pad="D14"/>
<connect gate="MCU" pin="PI10" pad="E3"/>
<connect gate="MCU" pin="PI11" pad="E4"/>
<connect gate="MCU" pin="PI2" pad="C14"/>
<connect gate="MCU" pin="PI3" pad="C13"/>
<connect gate="MCU" pin="PI4" pad="D4"/>
<connect gate="MCU" pin="PI5" pad="C4"/>
<connect gate="MCU" pin="PI6" pad="C3"/>
<connect gate="MCU" pin="PI7" pad="C2"/>
<connect gate="MCU" pin="PI8" pad="D2"/>
<connect gate="MCU" pin="PI9" pad="D3"/>
<connect gate="MCU" pin="VBAT" pad="C1"/>
<connect gate="MCU" pin="VCAP1" pad="M10"/>
<connect gate="MCU" pin="VCAP2" pad="F13"/>
<connect gate="MCU" pin="VDDA" pad="R1"/>
<connect gate="MCU" pin="VREF+" pad="P1"/>
<connect gate="MCU" pin="VREF-" pad="N1"/>
<connect gate="MCU" pin="VSSA" pad="M1"/>
<connect gate="PWR" pin="VDD@1" pad="C5"/>
<connect gate="PWR" pin="VDD@10" pad="J13"/>
<connect gate="PWR" pin="VDD@11" pad="K4"/>
<connect gate="PWR" pin="VDD@12" pad="N8"/>
<connect gate="PWR" pin="VDD@13" pad="N9"/>
<connect gate="PWR" pin="VDD@14" pad="N10"/>
<connect gate="PWR" pin="VDD@2" pad="C7"/>
<connect gate="PWR" pin="VDD@3" pad="C8"/>
<connect gate="PWR" pin="VDD@4" pad="C9"/>
<connect gate="PWR" pin="VDD@5" pad="F3"/>
<connect gate="PWR" pin="VDD@6" pad="G3"/>
<connect gate="PWR" pin="VDD@7" pad="G13"/>
<connect gate="PWR" pin="VDD@8" pad="H13"/>
<connect gate="PWR" pin="VDD@9" pad="J12"/>
<connect gate="PWR" pin="VSS@1" pad="D5"/>
<connect gate="PWR" pin="VSS@10" pad="M8"/>
<connect gate="PWR" pin="VSS@11" pad="M9"/>
<connect gate="PWR" pin="VSS@12" pad="VSS_1"/>
<connect gate="PWR" pin="VSS@13" pad="VSS_2"/>
<connect gate="PWR" pin="VSS@14" pad="VSS_3"/>
<connect gate="PWR" pin="VSS@15" pad="VSS_4"/>
<connect gate="PWR" pin="VSS@16" pad="VSS_5"/>
<connect gate="PWR" pin="VSS@17" pad="VSS_6"/>
<connect gate="PWR" pin="VSS@18" pad="VSS_7"/>
<connect gate="PWR" pin="VSS@19" pad="VSS_8"/>
<connect gate="PWR" pin="VSS@2" pad="D7"/>
<connect gate="PWR" pin="VSS@20" pad="VSS_9"/>
<connect gate="PWR" pin="VSS@21" pad="VSS_10"/>
<connect gate="PWR" pin="VSS@22" pad="VSS_11"/>
<connect gate="PWR" pin="VSS@23" pad="VSS_12"/>
<connect gate="PWR" pin="VSS@24" pad="VSS_13"/>
<connect gate="PWR" pin="VSS@25" pad="VSS_14"/>
<connect gate="PWR" pin="VSS@26" pad="VSS_15"/>
<connect gate="PWR" pin="VSS@27" pad="VSS_16"/>
<connect gate="PWR" pin="VSS@28" pad="VSS_17"/>
<connect gate="PWR" pin="VSS@29" pad="VSS_18"/>
<connect gate="PWR" pin="VSS@3" pad="D8"/>
<connect gate="PWR" pin="VSS@30" pad="VSS_19"/>
<connect gate="PWR" pin="VSS@31" pad="VSS_20"/>
<connect gate="PWR" pin="VSS@32" pad="VSS_21"/>
<connect gate="PWR" pin="VSS@33" pad="VSS_22"/>
<connect gate="PWR" pin="VSS@34" pad="VSS_23"/>
<connect gate="PWR" pin="VSS@35" pad="VSS_24"/>
<connect gate="PWR" pin="VSS@36" pad="VSS_25"/>
<connect gate="PWR" pin="VSS@4" pad="D9"/>
<connect gate="PWR" pin="VSS@5" pad="F2"/>
<connect gate="PWR" pin="VSS@6" pad="F12"/>
<connect gate="PWR" pin="VSS@7" pad="G2"/>
<connect gate="PWR" pin="VSS@8" pad="G12"/>
<connect gate="PWR" pin="VSS@9" pad="H12"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F439V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP9"/>
<gate name="PWR" symbol="PWR_VDD6_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="49"/>
<connect gate="MCU" pin="VCAP2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VSSA" pad="20"/>
<connect gate="PWR" pin="VDD@1" pad="100"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="28"/>
<connect gate="PWR" pin="VDD@4" pad="11"/>
<connect gate="PWR" pin="VDD@5" pad="50"/>
<connect gate="PWR" pin="VDD@6" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="99"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
<connect gate="PWR" pin="VSS@3" pad="27"/>
<connect gate="PWR" pin="VSS@4" pad="10"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F439Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD12_VSS9"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PDR_ON" pad="143"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="71"/>
<connect gate="MCU" pin="VCAP2" pad="106"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VSSA" pad="31"/>
<connect gate="PWR" pin="VDD@1" pad="131"/>
<connect gate="PWR" pin="VDD@10" pad="144"/>
<connect gate="PWR" pin="VDD@11" pad="72"/>
<connect gate="PWR" pin="VDD@12" pad="30"/>
<connect gate="PWR" pin="VDD@2" pad="121"/>
<connect gate="PWR" pin="VDD@3" pad="108"/>
<connect gate="PWR" pin="VDD@4" pad="95"/>
<connect gate="PWR" pin="VDD@5" pad="84"/>
<connect gate="PWR" pin="VDD@6" pad="62"/>
<connect gate="PWR" pin="VDD@7" pad="52"/>
<connect gate="PWR" pin="VDD@8" pad="39"/>
<connect gate="PWR" pin="VDD@9" pad="17"/>
<connect gate="PWR" pin="VSS@1" pad="130"/>
<connect gate="PWR" pin="VSS@2" pad="120"/>
<connect gate="PWR" pin="VSS@3" pad="107"/>
<connect gate="PWR" pin="VSS@4" pad="94"/>
<connect gate="PWR" pin="VSS@5" pad="83"/>
<connect gate="PWR" pin="VSS@6" pad="61"/>
<connect gate="PWR" pin="VSS@7" pad="51"/>
<connect gate="PWR" pin="VSS@8" pad="38"/>
<connect gate="PWR" pin="VSS@9" pad="16"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F439Z*Y" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
114 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_143PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD13_VSS6"/>
</gates>
<devices>
<device name="" package="WLCSP143">
<connects>
<connect gate="MCU" pin="BOOT0" pad="C9"/>
<connect gate="MCU" pin="BYPASS_REG" pad="N11"/>
<connect gate="MCU" pin="NRST" pad="H9"/>
<connect gate="MCU" pin="OSC_IN" pad="J11"/>
<connect gate="MCU" pin="OSC_OUT" pad="H10"/>
<connect gate="MCU" pin="PA0" pad="K9"/>
<connect gate="MCU" pin="PA1" pad="K8"/>
<connect gate="MCU" pin="PA10" pad="D5"/>
<connect gate="MCU" pin="PA11" pad="D4"/>
<connect gate="MCU" pin="PA12" pad="E1"/>
<connect gate="MCU" pin="PA13" pad="D3"/>
<connect gate="MCU" pin="PA14" pad="B1"/>
<connect gate="MCU" pin="PA15" pad="C2"/>
<connect gate="MCU" pin="PA2" pad="L9"/>
<connect gate="MCU" pin="PA3" pad="M11"/>
<connect gate="MCU" pin="PA4" pad="M10"/>
<connect gate="MCU" pin="PA5" pad="M9"/>
<connect gate="MCU" pin="PA6" pad="N10"/>
<connect gate="MCU" pin="PA7" pad="L8"/>
<connect gate="MCU" pin="PA8" pad="F1"/>
<connect gate="MCU" pin="PA9" pad="E2"/>
<connect gate="MCU" pin="PB0" pad="N8"/>
<connect gate="MCU" pin="PB1" pad="K7"/>
<connect gate="MCU" pin="PB10" pad="M3"/>
<connect gate="MCU" pin="PB11" pad="N3"/>
<connect gate="MCU" pin="PB12" pad="M2"/>
<connect gate="MCU" pin="PB13" pad="N1"/>
<connect gate="MCU" pin="PB14" pad="K3"/>
<connect gate="MCU" pin="PB15" pad="J3"/>
<connect gate="MCU" pin="PB2" pad="L7"/>
<connect gate="MCU" pin="PB3" pad="B7"/>
<connect gate="MCU" pin="PB4" pad="C7"/>
<connect gate="MCU" pin="PB5" pad="C8"/>
<connect gate="MCU" pin="PB6" pad="A8"/>
<connect gate="MCU" pin="PB7" pad="B8"/>
<connect gate="MCU" pin="PB8" pad="A9"/>
<connect gate="MCU" pin="PB9" pad="B9"/>
<connect gate="MCU" pin="PC0" pad="H8"/>
<connect gate="MCU" pin="PC1" pad="K11"/>
<connect gate="MCU" pin="PC10" pad="A2"/>
<connect gate="MCU" pin="PC11" pad="B2"/>
<connect gate="MCU" pin="PC12" pad="C3"/>
<connect gate="MCU" pin="PC13" pad="D10"/>
<connect gate="MCU" pin="PC14" pad="D11"/>
<connect gate="MCU" pin="PC15" pad="E11"/>
<connect gate="MCU" pin="PC2" pad="J10"/>
<connect gate="MCU" pin="PC3" pad="J9"/>
<connect gate="MCU" pin="PC4" pad="M8"/>
<connect gate="MCU" pin="PC5" pad="N9"/>
<connect gate="MCU" pin="PC6" pad="F2"/>
<connect gate="MCU" pin="PC7" pad="F3"/>
<connect gate="MCU" pin="PC8" pad="E4"/>
<connect gate="MCU" pin="PC9" pad="E3"/>
<connect gate="MCU" pin="PD0" pad="B3"/>
<connect gate="MCU" pin="PD1" pad="C4"/>
<connect gate="MCU" pin="PD10" pad="H4"/>
<connect gate="MCU" pin="PD11" pad="K2"/>
<connect gate="MCU" pin="PD12" pad="H6"/>
<connect gate="MCU" pin="PD13" pad="H5"/>
<connect gate="MCU" pin="PD14" pad="J2"/>
<connect gate="MCU" pin="PD15" pad="K1"/>
<connect gate="MCU" pin="PD2" pad="A3"/>
<connect gate="MCU" pin="PD3" pad="B4"/>
<connect gate="MCU" pin="PD4" pad="B5"/>
<connect gate="MCU" pin="PD5" pad="A4"/>
<connect gate="MCU" pin="PD6" pad="F4"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD8" pad="L2"/>
<connect gate="MCU" pin="PD9" pad="M1"/>
<connect gate="MCU" pin="PDR_ON" pad="A11"/>
<connect gate="MCU" pin="PE0" pad="B10"/>
<connect gate="MCU" pin="PE1" pad="A10"/>
<connect gate="MCU" pin="PE10" pad="J4"/>
<connect gate="MCU" pin="PE11" pad="K4"/>
<connect gate="MCU" pin="PE12" pad="L4"/>
<connect gate="MCU" pin="PE13" pad="N4"/>
<connect gate="MCU" pin="PE14" pad="M4"/>
<connect gate="MCU" pin="PE15" pad="L3"/>
<connect gate="MCU" pin="PE2" pad="D8"/>
<connect gate="MCU" pin="PE3" pad="C10"/>
<connect gate="MCU" pin="PE4" pad="B11"/>
<connect gate="MCU" pin="PE5" pad="D9"/>
<connect gate="MCU" pin="PE6" pad="E8"/>
<connect gate="MCU" pin="PE7" pad="L5"/>
<connect gate="MCU" pin="PE8" pad="M5"/>
<connect gate="MCU" pin="PE9" pad="N5"/>
<connect gate="MCU" pin="PF0" pad="F11"/>
<connect gate="MCU" pin="PF1" pad="E9"/>
<connect gate="MCU" pin="PF10" pad="G9"/>
<connect gate="MCU" pin="PF11" pad="M7"/>
<connect gate="MCU" pin="PF12" pad="N7"/>
<connect gate="MCU" pin="PF13" pad="K6"/>
<connect gate="MCU" pin="PF14" pad="L6"/>
<connect gate="MCU" pin="PF15" pad="M6"/>
<connect gate="MCU" pin="PF2" pad="F10"/>
<connect gate="MCU" pin="PF3" pad="G11"/>
<connect gate="MCU" pin="PF4" pad="F9"/>
<connect gate="MCU" pin="PF5" pad="F8"/>
<connect gate="MCU" pin="PF6" pad="G10"/>
<connect gate="MCU" pin="PF7" pad="F7"/>
<connect gate="MCU" pin="PF8" pad="H11"/>
<connect gate="MCU" pin="PF9" pad="G8"/>
<connect gate="MCU" pin="PG0" pad="N6"/>
<connect gate="MCU" pin="PG1" pad="K5"/>
<connect gate="MCU" pin="PG10" pad="C6"/>
<connect gate="MCU" pin="PG11" pad="B6"/>
<connect gate="MCU" pin="PG12" pad="A6"/>
<connect gate="MCU" pin="PG13" pad="D6"/>
<connect gate="MCU" pin="PG14" pad="F6"/>
<connect gate="MCU" pin="PG15" pad="A7"/>
<connect gate="MCU" pin="PG2" pad="J1"/>
<connect gate="MCU" pin="PG3" pad="G3"/>
<connect gate="MCU" pin="PG4" pad="G5"/>
<connect gate="MCU" pin="PG5" pad="G6"/>
<connect gate="MCU" pin="PG6" pad="G4"/>
<connect gate="MCU" pin="PG7" pad="H1"/>
<connect gate="MCU" pin="PG8" pad="G2"/>
<connect gate="MCU" pin="PG9" pad="E5"/>
<connect gate="MCU" pin="VBAT" pad="C11"/>
<connect gate="MCU" pin="VCAP1" pad="N2"/>
<connect gate="MCU" pin="VCAP2" pad="D1"/>
<connect gate="MCU" pin="VDDA" pad="L10"/>
<connect gate="MCU" pin="VREF+" pad="L11"/>
<connect gate="MCU" pin="VSSA" pad="K10"/>
<connect gate="PWR" pin="VDD@1" pad="A1"/>
<connect gate="PWR" pin="VDD@10" pad="J6"/>
<connect gate="PWR" pin="VDD@11" pad="J7"/>
<connect gate="PWR" pin="VDD@12" pad="J8"/>
<connect gate="PWR" pin="VDD@13" pad="L1"/>
<connect gate="PWR" pin="VDD@2" pad="C1"/>
<connect gate="PWR" pin="VDD@3" pad="C5"/>
<connect gate="PWR" pin="VDD@4" pad="D7"/>
<connect gate="PWR" pin="VDD@5" pad="E6"/>
<connect gate="PWR" pin="VDD@6" pad="E10"/>
<connect gate="PWR" pin="VDD@7" pad="G1"/>
<connect gate="PWR" pin="VDD@8" pad="G7"/>
<connect gate="PWR" pin="VDD@9" pad="J5"/>
<connect gate="PWR" pin="VSS@1" pad="D2"/>
<connect gate="PWR" pin="VSS@2" pad="E7"/>
<connect gate="PWR" pin="VSS@3" pad="F5"/>
<connect gate="PWR" pin="VSS@4" pad="H2"/>
<connect gate="PWR" pin="VSS@5" pad="H3"/>
<connect gate="PWR" pin="VSS@6" pad="H7"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F439I*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD15_VSS11"/>
</gates>
<devices>
<device name="" package="LQFP176">
<connects>
<connect gate="MCU" pin="BOOT0" pad="166"/>
<connect gate="MCU" pin="BYPASS_REG" pad="48"/>
<connect gate="MCU" pin="NRST" pad="31"/>
<connect gate="MCU" pin="OSC_IN" pad="29"/>
<connect gate="MCU" pin="OSC_OUT" pad="30"/>
<connect gate="MCU" pin="PA0" pad="40"/>
<connect gate="MCU" pin="PA1" pad="41"/>
<connect gate="MCU" pin="PA10" pad="121"/>
<connect gate="MCU" pin="PA11" pad="122"/>
<connect gate="MCU" pin="PA12" pad="123"/>
<connect gate="MCU" pin="PA13" pad="124"/>
<connect gate="MCU" pin="PA14" pad="137"/>
<connect gate="MCU" pin="PA15" pad="138"/>
<connect gate="MCU" pin="PA2" pad="42"/>
<connect gate="MCU" pin="PA3" pad="47"/>
<connect gate="MCU" pin="PA4" pad="50"/>
<connect gate="MCU" pin="PA5" pad="51"/>
<connect gate="MCU" pin="PA6" pad="52"/>
<connect gate="MCU" pin="PA7" pad="53"/>
<connect gate="MCU" pin="PA8" pad="119"/>
<connect gate="MCU" pin="PA9" pad="120"/>
<connect gate="MCU" pin="PB0" pad="56"/>
<connect gate="MCU" pin="PB1" pad="57"/>
<connect gate="MCU" pin="PB10" pad="79"/>
<connect gate="MCU" pin="PB11" pad="80"/>
<connect gate="MCU" pin="PB12" pad="92"/>
<connect gate="MCU" pin="PB13" pad="93"/>
<connect gate="MCU" pin="PB14" pad="94"/>
<connect gate="MCU" pin="PB15" pad="95"/>
<connect gate="MCU" pin="PB2" pad="58"/>
<connect gate="MCU" pin="PB3" pad="161"/>
<connect gate="MCU" pin="PB4" pad="162"/>
<connect gate="MCU" pin="PB5" pad="163"/>
<connect gate="MCU" pin="PB6" pad="164"/>
<connect gate="MCU" pin="PB7" pad="165"/>
<connect gate="MCU" pin="PB8" pad="167"/>
<connect gate="MCU" pin="PB9" pad="168"/>
<connect gate="MCU" pin="PC0" pad="32"/>
<connect gate="MCU" pin="PC1" pad="33"/>
<connect gate="MCU" pin="PC10" pad="139"/>
<connect gate="MCU" pin="PC11" pad="140"/>
<connect gate="MCU" pin="PC12" pad="141"/>
<connect gate="MCU" pin="PC13" pad="8"/>
<connect gate="MCU" pin="PC14" pad="9"/>
<connect gate="MCU" pin="PC15" pad="10"/>
<connect gate="MCU" pin="PC2" pad="34"/>
<connect gate="MCU" pin="PC3" pad="35"/>
<connect gate="MCU" pin="PC4" pad="54"/>
<connect gate="MCU" pin="PC5" pad="55"/>
<connect gate="MCU" pin="PC6" pad="115"/>
<connect gate="MCU" pin="PC7" pad="116"/>
<connect gate="MCU" pin="PC8" pad="117"/>
<connect gate="MCU" pin="PC9" pad="118"/>
<connect gate="MCU" pin="PD0" pad="142"/>
<connect gate="MCU" pin="PD1" pad="143"/>
<connect gate="MCU" pin="PD10" pad="98"/>
<connect gate="MCU" pin="PD11" pad="99"/>
<connect gate="MCU" pin="PD12" pad="100"/>
<connect gate="MCU" pin="PD13" pad="101"/>
<connect gate="MCU" pin="PD14" pad="104"/>
<connect gate="MCU" pin="PD15" pad="105"/>
<connect gate="MCU" pin="PD2" pad="144"/>
<connect gate="MCU" pin="PD3" pad="145"/>
<connect gate="MCU" pin="PD4" pad="146"/>
<connect gate="MCU" pin="PD5" pad="147"/>
<connect gate="MCU" pin="PD6" pad="150"/>
<connect gate="MCU" pin="PD7" pad="151"/>
<connect gate="MCU" pin="PD8" pad="96"/>
<connect gate="MCU" pin="PD9" pad="97"/>
<connect gate="MCU" pin="PDR_ON" pad="171"/>
<connect gate="MCU" pin="PE0" pad="169"/>
<connect gate="MCU" pin="PE1" pad="170"/>
<connect gate="MCU" pin="PE10" pad="73"/>
<connect gate="MCU" pin="PE11" pad="74"/>
<connect gate="MCU" pin="PE12" pad="75"/>
<connect gate="MCU" pin="PE13" pad="76"/>
<connect gate="MCU" pin="PE14" pad="77"/>
<connect gate="MCU" pin="PE15" pad="78"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="68"/>
<connect gate="MCU" pin="PE8" pad="69"/>
<connect gate="MCU" pin="PE9" pad="70"/>
<connect gate="MCU" pin="PF0" pad="16"/>
<connect gate="MCU" pin="PF1" pad="17"/>
<connect gate="MCU" pin="PF10" pad="28"/>
<connect gate="MCU" pin="PF11" pad="59"/>
<connect gate="MCU" pin="PF12" pad="60"/>
<connect gate="MCU" pin="PF13" pad="63"/>
<connect gate="MCU" pin="PF14" pad="64"/>
<connect gate="MCU" pin="PF15" pad="65"/>
<connect gate="MCU" pin="PF2" pad="18"/>
<connect gate="MCU" pin="PF3" pad="19"/>
<connect gate="MCU" pin="PF4" pad="20"/>
<connect gate="MCU" pin="PF5" pad="21"/>
<connect gate="MCU" pin="PF6" pad="24"/>
<connect gate="MCU" pin="PF7" pad="25"/>
<connect gate="MCU" pin="PF8" pad="26"/>
<connect gate="MCU" pin="PF9" pad="27"/>
<connect gate="MCU" pin="PG0" pad="66"/>
<connect gate="MCU" pin="PG1" pad="67"/>
<connect gate="MCU" pin="PG10" pad="153"/>
<connect gate="MCU" pin="PG11" pad="154"/>
<connect gate="MCU" pin="PG12" pad="155"/>
<connect gate="MCU" pin="PG13" pad="156"/>
<connect gate="MCU" pin="PG14" pad="157"/>
<connect gate="MCU" pin="PG15" pad="160"/>
<connect gate="MCU" pin="PG2" pad="106"/>
<connect gate="MCU" pin="PG3" pad="107"/>
<connect gate="MCU" pin="PG4" pad="108"/>
<connect gate="MCU" pin="PG5" pad="109"/>
<connect gate="MCU" pin="PG6" pad="110"/>
<connect gate="MCU" pin="PG7" pad="111"/>
<connect gate="MCU" pin="PG8" pad="112"/>
<connect gate="MCU" pin="PG9" pad="152"/>
<connect gate="MCU" pin="PH10" pad="87"/>
<connect gate="MCU" pin="PH11" pad="88"/>
<connect gate="MCU" pin="PH12" pad="89"/>
<connect gate="MCU" pin="PH13" pad="128"/>
<connect gate="MCU" pin="PH14" pad="129"/>
<connect gate="MCU" pin="PH15" pad="130"/>
<connect gate="MCU" pin="PH2" pad="43"/>
<connect gate="MCU" pin="PH3" pad="44"/>
<connect gate="MCU" pin="PH4" pad="45"/>
<connect gate="MCU" pin="PH5" pad="46"/>
<connect gate="MCU" pin="PH6" pad="83"/>
<connect gate="MCU" pin="PH7" pad="84"/>
<connect gate="MCU" pin="PH8" pad="85"/>
<connect gate="MCU" pin="PH9" pad="86"/>
<connect gate="MCU" pin="PI0" pad="131"/>
<connect gate="MCU" pin="PI1" pad="132"/>
<connect gate="MCU" pin="PI10" pad="12"/>
<connect gate="MCU" pin="PI11" pad="13"/>
<connect gate="MCU" pin="PI2" pad="133"/>
<connect gate="MCU" pin="PI3" pad="134"/>
<connect gate="MCU" pin="PI4" pad="173"/>
<connect gate="MCU" pin="PI5" pad="174"/>
<connect gate="MCU" pin="PI6" pad="175"/>
<connect gate="MCU" pin="PI7" pad="176"/>
<connect gate="MCU" pin="PI8" pad="7"/>
<connect gate="MCU" pin="PI9" pad="11"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="81"/>
<connect gate="MCU" pin="VCAP2" pad="125"/>
<connect gate="MCU" pin="VDDA" pad="39"/>
<connect gate="MCU" pin="VREF+" pad="38"/>
<connect gate="MCU" pin="VSSA" pad="37"/>
<connect gate="PWR" pin="VDD@1" pad="159"/>
<connect gate="PWR" pin="VDD@10" pad="23"/>
<connect gate="PWR" pin="VDD@11" pad="15"/>
<connect gate="PWR" pin="VDD@12" pad="172"/>
<connect gate="PWR" pin="VDD@13" pad="82"/>
<connect gate="PWR" pin="VDD@14" pad="49"/>
<connect gate="PWR" pin="VDD@15" pad="36"/>
<connect gate="PWR" pin="VDD@2" pad="149"/>
<connect gate="PWR" pin="VDD@3" pad="136"/>
<connect gate="PWR" pin="VDD@4" pad="127"/>
<connect gate="PWR" pin="VDD@5" pad="114"/>
<connect gate="PWR" pin="VDD@6" pad="103"/>
<connect gate="PWR" pin="VDD@7" pad="91"/>
<connect gate="PWR" pin="VDD@8" pad="72"/>
<connect gate="PWR" pin="VDD@9" pad="62"/>
<connect gate="PWR" pin="VSS@1" pad="158"/>
<connect gate="PWR" pin="VSS@10" pad="22"/>
<connect gate="PWR" pin="VSS@11" pad="14"/>
<connect gate="PWR" pin="VSS@2" pad="148"/>
<connect gate="PWR" pin="VSS@3" pad="135"/>
<connect gate="PWR" pin="VSS@4" pad="126"/>
<connect gate="PWR" pin="VSS@5" pad="113"/>
<connect gate="PWR" pin="VSS@6" pad="102"/>
<connect gate="PWR" pin="VSS@7" pad="90"/>
<connect gate="PWR" pin="VSS@8" pad="71"/>
<connect gate="PWR" pin="VSS@9" pad="61"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F439I*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
140 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_176PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD14_VSS36"/>
</gates>
<devices>
<device name="" package="UFBGA176+25">
<connects>
<connect gate="MCU" pin="BOOT0" pad="D6"/>
<connect gate="MCU" pin="BYPASS_REG" pad="L4"/>
<connect gate="MCU" pin="NRST" pad="J1"/>
<connect gate="MCU" pin="OSC_IN" pad="G1"/>
<connect gate="MCU" pin="OSC_OUT" pad="H1"/>
<connect gate="MCU" pin="PA0" pad="N3"/>
<connect gate="MCU" pin="PA1" pad="N2"/>
<connect gate="MCU" pin="PA10" pad="D15"/>
<connect gate="MCU" pin="PA11" pad="C15"/>
<connect gate="MCU" pin="PA12" pad="B15"/>
<connect gate="MCU" pin="PA13" pad="A15"/>
<connect gate="MCU" pin="PA14" pad="A14"/>
<connect gate="MCU" pin="PA15" pad="A13"/>
<connect gate="MCU" pin="PA2" pad="P2"/>
<connect gate="MCU" pin="PA3" pad="R2"/>
<connect gate="MCU" pin="PA4" pad="N4"/>
<connect gate="MCU" pin="PA5" pad="P4"/>
<connect gate="MCU" pin="PA6" pad="P3"/>
<connect gate="MCU" pin="PA7" pad="R3"/>
<connect gate="MCU" pin="PA8" pad="F15"/>
<connect gate="MCU" pin="PA9" pad="E15"/>
<connect gate="MCU" pin="PB0" pad="R5"/>
<connect gate="MCU" pin="PB1" pad="R4"/>
<connect gate="MCU" pin="PB10" pad="R12"/>
<connect gate="MCU" pin="PB11" pad="R13"/>
<connect gate="MCU" pin="PB12" pad="P12"/>
<connect gate="MCU" pin="PB13" pad="P13"/>
<connect gate="MCU" pin="PB14" pad="R14"/>
<connect gate="MCU" pin="PB15" pad="R15"/>
<connect gate="MCU" pin="PB2" pad="M6"/>
<connect gate="MCU" pin="PB3" pad="A10"/>
<connect gate="MCU" pin="PB4" pad="A9"/>
<connect gate="MCU" pin="PB5" pad="A6"/>
<connect gate="MCU" pin="PB6" pad="B6"/>
<connect gate="MCU" pin="PB7" pad="B5"/>
<connect gate="MCU" pin="PB8" pad="A5"/>
<connect gate="MCU" pin="PB9" pad="B4"/>
<connect gate="MCU" pin="PC0" pad="M2"/>
<connect gate="MCU" pin="PC1" pad="M3"/>
<connect gate="MCU" pin="PC10" pad="B14"/>
<connect gate="MCU" pin="PC11" pad="B13"/>
<connect gate="MCU" pin="PC12" pad="A12"/>
<connect gate="MCU" pin="PC13" pad="D1"/>
<connect gate="MCU" pin="PC14" pad="E1"/>
<connect gate="MCU" pin="PC15" pad="F1"/>
<connect gate="MCU" pin="PC2" pad="M4"/>
<connect gate="MCU" pin="PC3" pad="M5"/>
<connect gate="MCU" pin="PC4" pad="N5"/>
<connect gate="MCU" pin="PC5" pad="P5"/>
<connect gate="MCU" pin="PC6" pad="H15"/>
<connect gate="MCU" pin="PC7" pad="G15"/>
<connect gate="MCU" pin="PC8" pad="G14"/>
<connect gate="MCU" pin="PC9" pad="F14"/>
<connect gate="MCU" pin="PD0" pad="B12"/>
<connect gate="MCU" pin="PD1" pad="C12"/>
<connect gate="MCU" pin="PD10" pad="N15"/>
<connect gate="MCU" pin="PD11" pad="N14"/>
<connect gate="MCU" pin="PD12" pad="N13"/>
<connect gate="MCU" pin="PD13" pad="M15"/>
<connect gate="MCU" pin="PD14" pad="M14"/>
<connect gate="MCU" pin="PD15" pad="L14"/>
<connect gate="MCU" pin="PD2" pad="D12"/>
<connect gate="MCU" pin="PD3" pad="D11"/>
<connect gate="MCU" pin="PD4" pad="D10"/>
<connect gate="MCU" pin="PD5" pad="C11"/>
<connect gate="MCU" pin="PD6" pad="B11"/>
<connect gate="MCU" pin="PD7" pad="A11"/>
<connect gate="MCU" pin="PD8" pad="P15"/>
<connect gate="MCU" pin="PD9" pad="P14"/>
<connect gate="MCU" pin="PDR_ON" pad="C6"/>
<connect gate="MCU" pin="PE0" pad="A4"/>
<connect gate="MCU" pin="PE1" pad="A3"/>
<connect gate="MCU" pin="PE10" pad="R9"/>
<connect gate="MCU" pin="PE11" pad="P10"/>
<connect gate="MCU" pin="PE12" pad="R10"/>
<connect gate="MCU" pin="PE13" pad="N11"/>
<connect gate="MCU" pin="PE14" pad="P11"/>
<connect gate="MCU" pin="PE15" pad="R11"/>
<connect gate="MCU" pin="PE2" pad="A2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="B2"/>
<connect gate="MCU" pin="PE6" pad="B3"/>
<connect gate="MCU" pin="PE7" pad="R8"/>
<connect gate="MCU" pin="PE8" pad="P8"/>
<connect gate="MCU" pin="PE9" pad="P9"/>
<connect gate="MCU" pin="PF0" pad="E2"/>
<connect gate="MCU" pin="PF1" pad="H3"/>
<connect gate="MCU" pin="PF10" pad="L1"/>
<connect gate="MCU" pin="PF11" pad="R6"/>
<connect gate="MCU" pin="PF12" pad="P6"/>
<connect gate="MCU" pin="PF13" pad="N6"/>
<connect gate="MCU" pin="PF14" pad="R7"/>
<connect gate="MCU" pin="PF15" pad="P7"/>
<connect gate="MCU" pin="PF2" pad="H2"/>
<connect gate="MCU" pin="PF3" pad="J2"/>
<connect gate="MCU" pin="PF4" pad="J3"/>
<connect gate="MCU" pin="PF5" pad="K3"/>
<connect gate="MCU" pin="PF6" pad="K2"/>
<connect gate="MCU" pin="PF7" pad="K1"/>
<connect gate="MCU" pin="PF8" pad="L3"/>
<connect gate="MCU" pin="PF9" pad="L2"/>
<connect gate="MCU" pin="PG0" pad="N7"/>
<connect gate="MCU" pin="PG1" pad="M7"/>
<connect gate="MCU" pin="PG10" pad="B10"/>
<connect gate="MCU" pin="PG11" pad="B9"/>
<connect gate="MCU" pin="PG12" pad="B8"/>
<connect gate="MCU" pin="PG13" pad="A8"/>
<connect gate="MCU" pin="PG14" pad="A7"/>
<connect gate="MCU" pin="PG15" pad="B7"/>
<connect gate="MCU" pin="PG2" pad="L15"/>
<connect gate="MCU" pin="PG3" pad="K15"/>
<connect gate="MCU" pin="PG4" pad="K14"/>
<connect gate="MCU" pin="PG5" pad="K13"/>
<connect gate="MCU" pin="PG6" pad="J15"/>
<connect gate="MCU" pin="PG7" pad="J14"/>
<connect gate="MCU" pin="PG8" pad="H14"/>
<connect gate="MCU" pin="PG9" pad="C10"/>
<connect gate="MCU" pin="PH10" pad="L13"/>
<connect gate="MCU" pin="PH11" pad="L12"/>
<connect gate="MCU" pin="PH12" pad="K12"/>
<connect gate="MCU" pin="PH13" pad="E12"/>
<connect gate="MCU" pin="PH14" pad="E13"/>
<connect gate="MCU" pin="PH15" pad="D13"/>
<connect gate="MCU" pin="PH2" pad="F4"/>
<connect gate="MCU" pin="PH3" pad="G4"/>
<connect gate="MCU" pin="PH4" pad="H4"/>
<connect gate="MCU" pin="PH5" pad="J4"/>
<connect gate="MCU" pin="PH6" pad="M11"/>
<connect gate="MCU" pin="PH7" pad="N12"/>
<connect gate="MCU" pin="PH8" pad="M12"/>
<connect gate="MCU" pin="PH9" pad="M13"/>
<connect gate="MCU" pin="PI0" pad="E14"/>
<connect gate="MCU" pin="PI1" pad="D14"/>
<connect gate="MCU" pin="PI10" pad="E3"/>
<connect gate="MCU" pin="PI11" pad="E4"/>
<connect gate="MCU" pin="PI2" pad="C14"/>
<connect gate="MCU" pin="PI3" pad="C13"/>
<connect gate="MCU" pin="PI4" pad="D4"/>
<connect gate="MCU" pin="PI5" pad="C4"/>
<connect gate="MCU" pin="PI6" pad="C3"/>
<connect gate="MCU" pin="PI7" pad="C2"/>
<connect gate="MCU" pin="PI8" pad="D2"/>
<connect gate="MCU" pin="PI9" pad="D3"/>
<connect gate="MCU" pin="VBAT" pad="C1"/>
<connect gate="MCU" pin="VCAP1" pad="M10"/>
<connect gate="MCU" pin="VCAP2" pad="F13"/>
<connect gate="MCU" pin="VDDA" pad="R1"/>
<connect gate="MCU" pin="VREF+" pad="P1"/>
<connect gate="MCU" pin="VREF-" pad="N1"/>
<connect gate="MCU" pin="VSSA" pad="M1"/>
<connect gate="PWR" pin="VDD@1" pad="C5"/>
<connect gate="PWR" pin="VDD@10" pad="J13"/>
<connect gate="PWR" pin="VDD@11" pad="K4"/>
<connect gate="PWR" pin="VDD@12" pad="N8"/>
<connect gate="PWR" pin="VDD@13" pad="N9"/>
<connect gate="PWR" pin="VDD@14" pad="N10"/>
<connect gate="PWR" pin="VDD@2" pad="C7"/>
<connect gate="PWR" pin="VDD@3" pad="C8"/>
<connect gate="PWR" pin="VDD@4" pad="C9"/>
<connect gate="PWR" pin="VDD@5" pad="F3"/>
<connect gate="PWR" pin="VDD@6" pad="G3"/>
<connect gate="PWR" pin="VDD@7" pad="G13"/>
<connect gate="PWR" pin="VDD@8" pad="H13"/>
<connect gate="PWR" pin="VDD@9" pad="J12"/>
<connect gate="PWR" pin="VSS@1" pad="D5"/>
<connect gate="PWR" pin="VSS@10" pad="M8"/>
<connect gate="PWR" pin="VSS@11" pad="M9"/>
<connect gate="PWR" pin="VSS@12" pad="VSS_1"/>
<connect gate="PWR" pin="VSS@13" pad="VSS_2"/>
<connect gate="PWR" pin="VSS@14" pad="VSS_3"/>
<connect gate="PWR" pin="VSS@15" pad="VSS_4"/>
<connect gate="PWR" pin="VSS@16" pad="VSS_5"/>
<connect gate="PWR" pin="VSS@17" pad="VSS_6"/>
<connect gate="PWR" pin="VSS@18" pad="VSS_7"/>
<connect gate="PWR" pin="VSS@19" pad="VSS_8"/>
<connect gate="PWR" pin="VSS@2" pad="D7"/>
<connect gate="PWR" pin="VSS@20" pad="VSS_9"/>
<connect gate="PWR" pin="VSS@21" pad="VSS_10"/>
<connect gate="PWR" pin="VSS@22" pad="VSS_11"/>
<connect gate="PWR" pin="VSS@23" pad="VSS_12"/>
<connect gate="PWR" pin="VSS@24" pad="VSS_13"/>
<connect gate="PWR" pin="VSS@25" pad="VSS_14"/>
<connect gate="PWR" pin="VSS@26" pad="VSS_15"/>
<connect gate="PWR" pin="VSS@27" pad="VSS_16"/>
<connect gate="PWR" pin="VSS@28" pad="VSS_17"/>
<connect gate="PWR" pin="VSS@29" pad="VSS_18"/>
<connect gate="PWR" pin="VSS@3" pad="D8"/>
<connect gate="PWR" pin="VSS@30" pad="VSS_19"/>
<connect gate="PWR" pin="VSS@31" pad="VSS_20"/>
<connect gate="PWR" pin="VSS@32" pad="VSS_21"/>
<connect gate="PWR" pin="VSS@33" pad="VSS_22"/>
<connect gate="PWR" pin="VSS@34" pad="VSS_23"/>
<connect gate="PWR" pin="VSS@35" pad="VSS_24"/>
<connect gate="PWR" pin="VSS@36" pad="VSS_25"/>
<connect gate="PWR" pin="VSS@4" pad="D9"/>
<connect gate="PWR" pin="VSS@5" pad="F2"/>
<connect gate="PWR" pin="VSS@6" pad="F12"/>
<connect gate="PWR" pin="VSS@7" pad="G2"/>
<connect gate="PWR" pin="VSS@8" pad="G12"/>
<connect gate="PWR" pin="VSS@9" pad="H12"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F439B*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
168 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_208PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD17_VSS14"/>
</gates>
<devices>
<device name="" package="LQFP208">
<connects>
<connect gate="MCU" pin="BOOT0" pad="197"/>
<connect gate="MCU" pin="NRST" pad="34"/>
<connect gate="MCU" pin="OSC_IN" pad="32"/>
<connect gate="MCU" pin="OSC_OUT" pad="33"/>
<connect gate="MCU" pin="PA0" pad="43"/>
<connect gate="MCU" pin="PA1" pad="44"/>
<connect gate="MCU" pin="PA10" pad="144"/>
<connect gate="MCU" pin="PA11" pad="145"/>
<connect gate="MCU" pin="PA12" pad="146"/>
<connect gate="MCU" pin="PA13" pad="147"/>
<connect gate="MCU" pin="PA14" pad="159"/>
<connect gate="MCU" pin="PA15" pad="160"/>
<connect gate="MCU" pin="PA2" pad="45"/>
<connect gate="MCU" pin="PA3" pad="50"/>
<connect gate="MCU" pin="PA4" pad="53"/>
<connect gate="MCU" pin="PA5" pad="54"/>
<connect gate="MCU" pin="PA6" pad="55"/>
<connect gate="MCU" pin="PA7" pad="56"/>
<connect gate="MCU" pin="PA8" pad="142"/>
<connect gate="MCU" pin="PA9" pad="143"/>
<connect gate="MCU" pin="PB0" pad="61"/>
<connect gate="MCU" pin="PB1" pad="62"/>
<connect gate="MCU" pin="PB10" pad="90"/>
<connect gate="MCU" pin="PB11" pad="91"/>
<connect gate="MCU" pin="PB12" pad="104"/>
<connect gate="MCU" pin="PB13" pad="105"/>
<connect gate="MCU" pin="PB14" pad="106"/>
<connect gate="MCU" pin="PB15" pad="107"/>
<connect gate="MCU" pin="PB2" pad="63"/>
<connect gate="MCU" pin="PB3" pad="192"/>
<connect gate="MCU" pin="PB4" pad="193"/>
<connect gate="MCU" pin="PB5" pad="194"/>
<connect gate="MCU" pin="PB6" pad="195"/>
<connect gate="MCU" pin="PB7" pad="196"/>
<connect gate="MCU" pin="PB8" pad="198"/>
<connect gate="MCU" pin="PB9" pad="199"/>
<connect gate="MCU" pin="PC0" pad="35"/>
<connect gate="MCU" pin="PC1" pad="36"/>
<connect gate="MCU" pin="PC10" pad="161"/>
<connect gate="MCU" pin="PC11" pad="162"/>
<connect gate="MCU" pin="PC12" pad="163"/>
<connect gate="MCU" pin="PC13" pad="8"/>
<connect gate="MCU" pin="PC14" pad="9"/>
<connect gate="MCU" pin="PC15" pad="10"/>
<connect gate="MCU" pin="PC2" pad="37"/>
<connect gate="MCU" pin="PC3" pad="38"/>
<connect gate="MCU" pin="PC4" pad="57"/>
<connect gate="MCU" pin="PC5" pad="58"/>
<connect gate="MCU" pin="PC6" pad="138"/>
<connect gate="MCU" pin="PC7" pad="139"/>
<connect gate="MCU" pin="PC8" pad="140"/>
<connect gate="MCU" pin="PC9" pad="141"/>
<connect gate="MCU" pin="PD0" pad="164"/>
<connect gate="MCU" pin="PD1" pad="165"/>
<connect gate="MCU" pin="PD10" pad="110"/>
<connect gate="MCU" pin="PD11" pad="111"/>
<connect gate="MCU" pin="PD12" pad="112"/>
<connect gate="MCU" pin="PD13" pad="113"/>
<connect gate="MCU" pin="PD14" pad="116"/>
<connect gate="MCU" pin="PD15" pad="117"/>
<connect gate="MCU" pin="PD2" pad="166"/>
<connect gate="MCU" pin="PD3" pad="167"/>
<connect gate="MCU" pin="PD4" pad="168"/>
<connect gate="MCU" pin="PD5" pad="169"/>
<connect gate="MCU" pin="PD6" pad="172"/>
<connect gate="MCU" pin="PD7" pad="173"/>
<connect gate="MCU" pin="PD8" pad="108"/>
<connect gate="MCU" pin="PD9" pad="109"/>
<connect gate="MCU" pin="PDR_ON" pad="203"/>
<connect gate="MCU" pin="PE0" pad="200"/>
<connect gate="MCU" pin="PE1" pad="201"/>
<connect gate="MCU" pin="PE10" pad="84"/>
<connect gate="MCU" pin="PE11" pad="85"/>
<connect gate="MCU" pin="PE12" pad="86"/>
<connect gate="MCU" pin="PE13" pad="87"/>
<connect gate="MCU" pin="PE14" pad="88"/>
<connect gate="MCU" pin="PE15" pad="89"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="79"/>
<connect gate="MCU" pin="PE8" pad="80"/>
<connect gate="MCU" pin="PE9" pad="81"/>
<connect gate="MCU" pin="PF0" pad="16"/>
<connect gate="MCU" pin="PF1" pad="17"/>
<connect gate="MCU" pin="PF10" pad="31"/>
<connect gate="MCU" pin="PF11" pad="70"/>
<connect gate="MCU" pin="PF12" pad="71"/>
<connect gate="MCU" pin="PF13" pad="74"/>
<connect gate="MCU" pin="PF14" pad="75"/>
<connect gate="MCU" pin="PF15" pad="76"/>
<connect gate="MCU" pin="PF2" pad="18"/>
<connect gate="MCU" pin="PF3" pad="22"/>
<connect gate="MCU" pin="PF4" pad="23"/>
<connect gate="MCU" pin="PF5" pad="24"/>
<connect gate="MCU" pin="PF6" pad="27"/>
<connect gate="MCU" pin="PF7" pad="28"/>
<connect gate="MCU" pin="PF8" pad="29"/>
<connect gate="MCU" pin="PF9" pad="30"/>
<connect gate="MCU" pin="PG0" pad="77"/>
<connect gate="MCU" pin="PG1" pad="78"/>
<connect gate="MCU" pin="PG10" pad="179"/>
<connect gate="MCU" pin="PG11" pad="180"/>
<connect gate="MCU" pin="PG12" pad="181"/>
<connect gate="MCU" pin="PG13" pad="182"/>
<connect gate="MCU" pin="PG14" pad="183"/>
<connect gate="MCU" pin="PG15" pad="191"/>
<connect gate="MCU" pin="PG2" pad="129"/>
<connect gate="MCU" pin="PG3" pad="130"/>
<connect gate="MCU" pin="PG4" pad="131"/>
<connect gate="MCU" pin="PG5" pad="132"/>
<connect gate="MCU" pin="PG6" pad="133"/>
<connect gate="MCU" pin="PG7" pad="134"/>
<connect gate="MCU" pin="PG8" pad="135"/>
<connect gate="MCU" pin="PG9" pad="178"/>
<connect gate="MCU" pin="PH10" pad="100"/>
<connect gate="MCU" pin="PH11" pad="101"/>
<connect gate="MCU" pin="PH12" pad="102"/>
<connect gate="MCU" pin="PH13" pad="151"/>
<connect gate="MCU" pin="PH14" pad="152"/>
<connect gate="MCU" pin="PH15" pad="153"/>
<connect gate="MCU" pin="PH2" pad="46"/>
<connect gate="MCU" pin="PH3" pad="47"/>
<connect gate="MCU" pin="PH4" pad="48"/>
<connect gate="MCU" pin="PH5" pad="49"/>
<connect gate="MCU" pin="PH6" pad="96"/>
<connect gate="MCU" pin="PH7" pad="97"/>
<connect gate="MCU" pin="PH8" pad="98"/>
<connect gate="MCU" pin="PH9" pad="99"/>
<connect gate="MCU" pin="PI0" pad="154"/>
<connect gate="MCU" pin="PI1" pad="155"/>
<connect gate="MCU" pin="PI10" pad="12"/>
<connect gate="MCU" pin="PI11" pad="13"/>
<connect gate="MCU" pin="PI12" pad="19"/>
<connect gate="MCU" pin="PI13" pad="20"/>
<connect gate="MCU" pin="PI14" pad="21"/>
<connect gate="MCU" pin="PI15" pad="64"/>
<connect gate="MCU" pin="PI2" pad="156"/>
<connect gate="MCU" pin="PI3" pad="157"/>
<connect gate="MCU" pin="PI4" pad="205"/>
<connect gate="MCU" pin="PI5" pad="206"/>
<connect gate="MCU" pin="PI6" pad="207"/>
<connect gate="MCU" pin="PI7" pad="208"/>
<connect gate="MCU" pin="PI8" pad="7"/>
<connect gate="MCU" pin="PI9" pad="11"/>
<connect gate="MCU" pin="PJ0" pad="65"/>
<connect gate="MCU" pin="PJ1" pad="66"/>
<connect gate="MCU" pin="PJ10" pad="122"/>
<connect gate="MCU" pin="PJ11" pad="123"/>
<connect gate="MCU" pin="PJ12" pad="174"/>
<connect gate="MCU" pin="PJ13" pad="175"/>
<connect gate="MCU" pin="PJ14" pad="176"/>
<connect gate="MCU" pin="PJ15" pad="177"/>
<connect gate="MCU" pin="PJ2" pad="67"/>
<connect gate="MCU" pin="PJ3" pad="68"/>
<connect gate="MCU" pin="PJ4" pad="69"/>
<connect gate="MCU" pin="PJ5" pad="95"/>
<connect gate="MCU" pin="PJ6" pad="118"/>
<connect gate="MCU" pin="PJ7" pad="119"/>
<connect gate="MCU" pin="PJ8" pad="120"/>
<connect gate="MCU" pin="PJ9" pad="121"/>
<connect gate="MCU" pin="PK0" pad="126"/>
<connect gate="MCU" pin="PK1" pad="127"/>
<connect gate="MCU" pin="PK2" pad="128"/>
<connect gate="MCU" pin="PK3" pad="186"/>
<connect gate="MCU" pin="PK4" pad="187"/>
<connect gate="MCU" pin="PK5" pad="188"/>
<connect gate="MCU" pin="PK6" pad="189"/>
<connect gate="MCU" pin="PK7" pad="190"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VCAP1" pad="92"/>
<connect gate="MCU" pin="VCAP2" pad="148"/>
<connect gate="MCU" pin="VDDA" pad="42"/>
<connect gate="MCU" pin="VREF+" pad="41"/>
<connect gate="MCU" pin="VSSA" pad="40"/>
<connect gate="PWR" pin="VDD@1" pad="204"/>
<connect gate="PWR" pin="VDD@10" pad="73"/>
<connect gate="PWR" pin="VDD@11" pad="59"/>
<connect gate="PWR" pin="VDD@12" pad="52"/>
<connect gate="PWR" pin="VDD@13" pad="26"/>
<connect gate="PWR" pin="VDD@14" pad="15"/>
<connect gate="PWR" pin="VDD@15" pad="158"/>
<connect gate="PWR" pin="VDD@16" pad="103"/>
<connect gate="PWR" pin="VDD@17" pad="39"/>
<connect gate="PWR" pin="VDD@2" pad="185"/>
<connect gate="PWR" pin="VDD@3" pad="171"/>
<connect gate="PWR" pin="VDD@4" pad="150"/>
<connect gate="PWR" pin="VDD@5" pad="137"/>
<connect gate="PWR" pin="VDD@6" pad="124"/>
<connect gate="PWR" pin="VDD@7" pad="115"/>
<connect gate="PWR" pin="VDD@8" pad="94"/>
<connect gate="PWR" pin="VDD@9" pad="83"/>
<connect gate="PWR" pin="VSS@1" pad="202"/>
<connect gate="PWR" pin="VSS@10" pad="72"/>
<connect gate="PWR" pin="VSS@11" pad="60"/>
<connect gate="PWR" pin="VSS@12" pad="51"/>
<connect gate="PWR" pin="VSS@13" pad="25"/>
<connect gate="PWR" pin="VSS@14" pad="14"/>
<connect gate="PWR" pin="VSS@2" pad="184"/>
<connect gate="PWR" pin="VSS@3" pad="170"/>
<connect gate="PWR" pin="VSS@4" pad="149"/>
<connect gate="PWR" pin="VSS@5" pad="136"/>
<connect gate="PWR" pin="VSS@6" pad="125"/>
<connect gate="PWR" pin="VSS@7" pad="114"/>
<connect gate="PWR" pin="VSS@8" pad="93"/>
<connect gate="PWR" pin="VSS@9" pad="82"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32F439N*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
180 MHz maximum frequency&lt;br&gt;
1024 to 2048 Kbytes of Flash memory&lt;br&gt;
256 kbytes of SRAM&lt;br&gt;
168 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_216PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD19_VSS18"/>
</gates>
<devices>
<device name="" package="TFBGA216">
<connects>
<connect gate="MCU" pin="BOOT0" pad="E6"/>
<connect gate="MCU" pin="BYPASS_REG" pad="L5"/>
<connect gate="MCU" pin="NRST" pad="J1"/>
<connect gate="MCU" pin="OSC_IN" pad="G1"/>
<connect gate="MCU" pin="OSC_OUT" pad="H1"/>
<connect gate="MCU" pin="PA0" pad="N3"/>
<connect gate="MCU" pin="PA1" pad="N2"/>
<connect gate="MCU" pin="PA10" pad="D15"/>
<connect gate="MCU" pin="PA11" pad="C15"/>
<connect gate="MCU" pin="PA12" pad="B15"/>
<connect gate="MCU" pin="PA13" pad="A15"/>
<connect gate="MCU" pin="PA14" pad="A14"/>
<connect gate="MCU" pin="PA15" pad="A13"/>
<connect gate="MCU" pin="PA2" pad="P2"/>
<connect gate="MCU" pin="PA3" pad="R2"/>
<connect gate="MCU" pin="PA4" pad="N4"/>
<connect gate="MCU" pin="PA5" pad="P4"/>
<connect gate="MCU" pin="PA6" pad="P3"/>
<connect gate="MCU" pin="PA7" pad="R3"/>
<connect gate="MCU" pin="PA8" pad="F15"/>
<connect gate="MCU" pin="PA9" pad="E15"/>
<connect gate="MCU" pin="PB0" pad="R5"/>
<connect gate="MCU" pin="PB1" pad="R4"/>
<connect gate="MCU" pin="PB10" pad="P12"/>
<connect gate="MCU" pin="PB11" pad="R13"/>
<connect gate="MCU" pin="PB12" pad="L13"/>
<connect gate="MCU" pin="PB13" pad="K14"/>
<connect gate="MCU" pin="PB14" pad="R14"/>
<connect gate="MCU" pin="PB15" pad="R15"/>
<connect gate="MCU" pin="PB2" pad="M5"/>
<connect gate="MCU" pin="PB3" pad="A10"/>
<connect gate="MCU" pin="PB4" pad="A9"/>
<connect gate="MCU" pin="PB5" pad="A8"/>
<connect gate="MCU" pin="PB6" pad="B6"/>
<connect gate="MCU" pin="PB7" pad="B5"/>
<connect gate="MCU" pin="PB8" pad="A7"/>
<connect gate="MCU" pin="PB9" pad="B4"/>
<connect gate="MCU" pin="PC0" pad="M2"/>
<connect gate="MCU" pin="PC1" pad="M3"/>
<connect gate="MCU" pin="PC10" pad="B14"/>
<connect gate="MCU" pin="PC11" pad="B13"/>
<connect gate="MCU" pin="PC12" pad="A12"/>
<connect gate="MCU" pin="PC13" pad="D1"/>
<connect gate="MCU" pin="PC14" pad="E1"/>
<connect gate="MCU" pin="PC15" pad="F1"/>
<connect gate="MCU" pin="PC2" pad="M4"/>
<connect gate="MCU" pin="PC3" pad="L4"/>
<connect gate="MCU" pin="PC4" pad="N5"/>
<connect gate="MCU" pin="PC5" pad="P5"/>
<connect gate="MCU" pin="PC6" pad="H15"/>
<connect gate="MCU" pin="PC7" pad="G15"/>
<connect gate="MCU" pin="PC8" pad="G14"/>
<connect gate="MCU" pin="PC9" pad="F14"/>
<connect gate="MCU" pin="PD0" pad="B12"/>
<connect gate="MCU" pin="PD1" pad="C12"/>
<connect gate="MCU" pin="PD10" pad="K15"/>
<connect gate="MCU" pin="PD11" pad="N10"/>
<connect gate="MCU" pin="PD12" pad="M10"/>
<connect gate="MCU" pin="PD13" pad="M11"/>
<connect gate="MCU" pin="PD14" pad="L12"/>
<connect gate="MCU" pin="PD15" pad="K13"/>
<connect gate="MCU" pin="PD2" pad="D12"/>
<connect gate="MCU" pin="PD3" pad="C11"/>
<connect gate="MCU" pin="PD4" pad="D11"/>
<connect gate="MCU" pin="PD5" pad="C10"/>
<connect gate="MCU" pin="PD6" pad="B11"/>
<connect gate="MCU" pin="PD7" pad="A11"/>
<connect gate="MCU" pin="PD8" pad="L15"/>
<connect gate="MCU" pin="PD9" pad="L14"/>
<connect gate="MCU" pin="PDR_ON" pad="E5"/>
<connect gate="MCU" pin="PE0" pad="A6"/>
<connect gate="MCU" pin="PE1" pad="A5"/>
<connect gate="MCU" pin="PE10" pad="R9"/>
<connect gate="MCU" pin="PE11" pad="P10"/>
<connect gate="MCU" pin="PE12" pad="R10"/>
<connect gate="MCU" pin="PE13" pad="R12"/>
<connect gate="MCU" pin="PE14" pad="P11"/>
<connect gate="MCU" pin="PE15" pad="R11"/>
<connect gate="MCU" pin="PE2" pad="A3"/>
<connect gate="MCU" pin="PE3" pad="A2"/>
<connect gate="MCU" pin="PE4" pad="A1"/>
<connect gate="MCU" pin="PE5" pad="B1"/>
<connect gate="MCU" pin="PE6" pad="B2"/>
<connect gate="MCU" pin="PE7" pad="R8"/>
<connect gate="MCU" pin="PE8" pad="N9"/>
<connect gate="MCU" pin="PE9" pad="P9"/>
<connect gate="MCU" pin="PF0" pad="D2"/>
<connect gate="MCU" pin="PF1" pad="E2"/>
<connect gate="MCU" pin="PF10" pad="L1"/>
<connect gate="MCU" pin="PF11" pad="P8"/>
<connect gate="MCU" pin="PF12" pad="M6"/>
<connect gate="MCU" pin="PF13" pad="N6"/>
<connect gate="MCU" pin="PF14" pad="P6"/>
<connect gate="MCU" pin="PF15" pad="M8"/>
<connect gate="MCU" pin="PF2" pad="G2"/>
<connect gate="MCU" pin="PF3" pad="H2"/>
<connect gate="MCU" pin="PF4" pad="J2"/>
<connect gate="MCU" pin="PF5" pad="K3"/>
<connect gate="MCU" pin="PF6" pad="K2"/>
<connect gate="MCU" pin="PF7" pad="K1"/>
<connect gate="MCU" pin="PF8" pad="L3"/>
<connect gate="MCU" pin="PF9" pad="L2"/>
<connect gate="MCU" pin="PG0" pad="N7"/>
<connect gate="MCU" pin="PG1" pad="M7"/>
<connect gate="MCU" pin="PG10" pad="C8"/>
<connect gate="MCU" pin="PG11" pad="B8"/>
<connect gate="MCU" pin="PG12" pad="C7"/>
<connect gate="MCU" pin="PG13" pad="B3"/>
<connect gate="MCU" pin="PG14" pad="A4"/>
<connect gate="MCU" pin="PG15" pad="B7"/>
<connect gate="MCU" pin="PG2" pad="M13"/>
<connect gate="MCU" pin="PG3" pad="M12"/>
<connect gate="MCU" pin="PG4" pad="N12"/>
<connect gate="MCU" pin="PG5" pad="N11"/>
<connect gate="MCU" pin="PG6" pad="J15"/>
<connect gate="MCU" pin="PG7" pad="J14"/>
<connect gate="MCU" pin="PG8" pad="H14"/>
<connect gate="MCU" pin="PG9" pad="D9"/>
<connect gate="MCU" pin="PH10" pad="P15"/>
<connect gate="MCU" pin="PH11" pad="N15"/>
<connect gate="MCU" pin="PH12" pad="M15"/>
<connect gate="MCU" pin="PH13" pad="E12"/>
<connect gate="MCU" pin="PH14" pad="E13"/>
<connect gate="MCU" pin="PH15" pad="D13"/>
<connect gate="MCU" pin="PH2" pad="K4"/>
<connect gate="MCU" pin="PH3" pad="J4"/>
<connect gate="MCU" pin="PH4" pad="H4"/>
<connect gate="MCU" pin="PH5" pad="J3"/>
<connect gate="MCU" pin="PH6" pad="P13"/>
<connect gate="MCU" pin="PH7" pad="N13"/>
<connect gate="MCU" pin="PH8" pad="P14"/>
<connect gate="MCU" pin="PH9" pad="N14"/>
<connect gate="MCU" pin="PI0" pad="E14"/>
<connect gate="MCU" pin="PI1" pad="D14"/>
<connect gate="MCU" pin="PI10" pad="D5"/>
<connect gate="MCU" pin="PI11" pad="F3"/>
<connect gate="MCU" pin="PI12" pad="E3"/>
<connect gate="MCU" pin="PI13" pad="G3"/>
<connect gate="MCU" pin="PI14" pad="H3"/>
<connect gate="MCU" pin="PI15" pad="G4"/>
<connect gate="MCU" pin="PI2" pad="C14"/>
<connect gate="MCU" pin="PI3" pad="C13"/>
<connect gate="MCU" pin="PI4" pad="C3"/>
<connect gate="MCU" pin="PI5" pad="D3"/>
<connect gate="MCU" pin="PI6" pad="D6"/>
<connect gate="MCU" pin="PI7" pad="D4"/>
<connect gate="MCU" pin="PI8" pad="C2"/>
<connect gate="MCU" pin="PI9" pad="E4"/>
<connect gate="MCU" pin="PJ0" pad="R6"/>
<connect gate="MCU" pin="PJ1" pad="R7"/>
<connect gate="MCU" pin="PJ10" pad="H13"/>
<connect gate="MCU" pin="PJ11" pad="G12"/>
<connect gate="MCU" pin="PJ12" pad="B10"/>
<connect gate="MCU" pin="PJ13" pad="B9"/>
<connect gate="MCU" pin="PJ14" pad="C9"/>
<connect gate="MCU" pin="PJ15" pad="D10"/>
<connect gate="MCU" pin="PJ2" pad="P7"/>
<connect gate="MCU" pin="PJ3" pad="N8"/>
<connect gate="MCU" pin="PJ4" pad="M9"/>
<connect gate="MCU" pin="PJ5" pad="M14"/>
<connect gate="MCU" pin="PJ6" pad="K12"/>
<connect gate="MCU" pin="PJ7" pad="J12"/>
<connect gate="MCU" pin="PJ8" pad="H12"/>
<connect gate="MCU" pin="PJ9" pad="J13"/>
<connect gate="MCU" pin="PK0" pad="G13"/>
<connect gate="MCU" pin="PK1" pad="F12"/>
<connect gate="MCU" pin="PK2" pad="F13"/>
<connect gate="MCU" pin="PK3" pad="D8"/>
<connect gate="MCU" pin="PK4" pad="D7"/>
<connect gate="MCU" pin="PK5" pad="C6"/>
<connect gate="MCU" pin="PK6" pad="C5"/>
<connect gate="MCU" pin="PK7" pad="C4"/>
<connect gate="MCU" pin="VBAT" pad="C1"/>
<connect gate="MCU" pin="VCAP1" pad="L11"/>
<connect gate="MCU" pin="VCAP2" pad="E11"/>
<connect gate="MCU" pin="VDDA" pad="R1"/>
<connect gate="MCU" pin="VREF+" pad="P1"/>
<connect gate="MCU" pin="VREF-" pad="N1"/>
<connect gate="MCU" pin="VSSA" pad="M1"/>
<connect gate="PWR" pin="VDD@1" pad="E7"/>
<connect gate="PWR" pin="VDD@10" pad="H5"/>
<connect gate="PWR" pin="VDD@11" pad="H11"/>
<connect gate="PWR" pin="VDD@12" pad="J5"/>
<connect gate="PWR" pin="VDD@13" pad="J11"/>
<connect gate="PWR" pin="VDD@14" pad="K5"/>
<connect gate="PWR" pin="VDD@15" pad="K11"/>
<connect gate="PWR" pin="VDD@16" pad="L7"/>
<connect gate="PWR" pin="VDD@17" pad="L8"/>
<connect gate="PWR" pin="VDD@18" pad="L9"/>
<connect gate="PWR" pin="VDD@19" pad="L10"/>
<connect gate="PWR" pin="VDD@2" pad="E8"/>
<connect gate="PWR" pin="VDD@3" pad="E9"/>
<connect gate="PWR" pin="VDD@4" pad="E10"/>
<connect gate="PWR" pin="VDD@5" pad="F4"/>
<connect gate="PWR" pin="VDD@6" pad="F5"/>
<connect gate="PWR" pin="VDD@7" pad="F11"/>
<connect gate="PWR" pin="VDD@8" pad="G5"/>
<connect gate="PWR" pin="VDD@9" pad="G11"/>
<connect gate="PWR" pin="VSS@1" pad="F2"/>
<connect gate="PWR" pin="VSS@10" pad="H10"/>
<connect gate="PWR" pin="VSS@11" pad="J6"/>
<connect gate="PWR" pin="VSS@12" pad="J10"/>
<connect gate="PWR" pin="VSS@13" pad="K6"/>
<connect gate="PWR" pin="VSS@14" pad="K7"/>
<connect gate="PWR" pin="VSS@15" pad="K8"/>
<connect gate="PWR" pin="VSS@16" pad="K9"/>
<connect gate="PWR" pin="VSS@17" pad="K10"/>
<connect gate="PWR" pin="VSS@18" pad="L6"/>
<connect gate="PWR" pin="VSS@2" pad="F6"/>
<connect gate="PWR" pin="VSS@3" pad="F7"/>
<connect gate="PWR" pin="VSS@4" pad="F8"/>
<connect gate="PWR" pin="VSS@5" pad="F9"/>
<connect gate="PWR" pin="VSS@6" pad="F10"/>
<connect gate="PWR" pin="VSS@7" pad="G6"/>
<connect gate="PWR" pin="VSS@8" pad="G10"/>
<connect gate="PWR" pin="VSS@9" pad="H6"/>
</connects>
<technologies>
<technology name="G"/>
<technology name="I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L100C*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 Kbytes of Flash memory&lt;br&gt;
2 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP8"/>
<gate name="PWR" symbol="PWR_VDD3_VSS3"/>
</gates>
<devices>
<device name="" package="UFQFPN48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VLCD" pad="1"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="24"/>
<connect gate="PWR" pin="VDD@2" pad="36"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="35"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
</connects>
<technologies>
<technology name="6"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L100R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 256 Kbytes of Flash memory&lt;br&gt;
2 to 4 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP11"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VLCD" pad="1"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="32"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="31"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
<connect gate="PWR" pin="VSS@3" pad="63"/>
<connect gate="PWR" pin="VSS@4" pad="18"/>
</connects>
<technologies>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L151C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 256 Kbytes of Flash memory&lt;br&gt;
4 to 8 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP8"/>
<gate name="PWR" symbol="PWR_VDD3_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VLCD" pad="1"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="24"/>
<connect gate="PWR" pin="VDD@2" pad="36"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="35"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L151C*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 256 Kbytes of Flash memory&lt;br&gt;
4 to 8 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP8"/>
<gate name="PWR" symbol="PWR_VDD3_VSS3"/>
</gates>
<devices>
<device name="" package="UFQFPN48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VLCD" pad="1"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="24"/>
<connect gate="PWR" pin="VDD@2" pad="36"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="35"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L151R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 384 Kbytes of Flash memory&lt;br&gt;
4 to 12 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP11"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VLCD" pad="1"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="32"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="31"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
<connect gate="PWR" pin="VSS@3" pad="63"/>
<connect gate="PWR" pin="VSS@4" pad="18"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
<technology name="D"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L151R*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 128 Kbytes of Flash memory&lt;br&gt;
4 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP12"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="TFBGA64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="B4"/>
<connect gate="MCU" pin="NRST" pad="E1"/>
<connect gate="MCU" pin="OSC_IN" pad="C1"/>
<connect gate="MCU" pin="OSC_OUT" pad="D1"/>
<connect gate="MCU" pin="PA0-WKUP" pad="G2"/>
<connect gate="MCU" pin="PA1" pad="H2"/>
<connect gate="MCU" pin="PA10" pad="C6"/>
<connect gate="MCU" pin="PA11" pad="C8"/>
<connect gate="MCU" pin="PA12" pad="B8"/>
<connect gate="MCU" pin="PA13" pad="A8"/>
<connect gate="MCU" pin="PA14" pad="A7"/>
<connect gate="MCU" pin="PA15" pad="A6"/>
<connect gate="MCU" pin="PA2" pad="F3"/>
<connect gate="MCU" pin="PA3" pad="G3"/>
<connect gate="MCU" pin="PA4" pad="H3"/>
<connect gate="MCU" pin="PA5" pad="F4"/>
<connect gate="MCU" pin="PA6" pad="G4"/>
<connect gate="MCU" pin="PA7" pad="H4"/>
<connect gate="MCU" pin="PA8" pad="D7"/>
<connect gate="MCU" pin="PA9" pad="C7"/>
<connect gate="MCU" pin="PB0" pad="F5"/>
<connect gate="MCU" pin="PB1" pad="G5"/>
<connect gate="MCU" pin="PB10" pad="G7"/>
<connect gate="MCU" pin="PB11" pad="H7"/>
<connect gate="MCU" pin="PB12" pad="H8"/>
<connect gate="MCU" pin="PB13" pad="G8"/>
<connect gate="MCU" pin="PB14" pad="F8"/>
<connect gate="MCU" pin="PB15" pad="F7"/>
<connect gate="MCU" pin="PB2" pad="G6"/>
<connect gate="MCU" pin="PB3" pad="A5"/>
<connect gate="MCU" pin="PB4" pad="A4"/>
<connect gate="MCU" pin="PB5" pad="C4"/>
<connect gate="MCU" pin="PB6" pad="D3"/>
<connect gate="MCU" pin="PB7" pad="C3"/>
<connect gate="MCU" pin="PB8" pad="B3"/>
<connect gate="MCU" pin="PB9" pad="A3"/>
<connect gate="MCU" pin="PC0" pad="E3"/>
<connect gate="MCU" pin="PC1" pad="E2"/>
<connect gate="MCU" pin="PC10" pad="B7"/>
<connect gate="MCU" pin="PC11" pad="B6"/>
<connect gate="MCU" pin="PC12" pad="C5"/>
<connect gate="MCU" pin="PC13" pad="A2"/>
<connect gate="MCU" pin="PC14" pad="A1"/>
<connect gate="MCU" pin="PC15" pad="B1"/>
<connect gate="MCU" pin="PC2" pad="F2"/>
<connect gate="MCU" pin="PC4" pad="H5"/>
<connect gate="MCU" pin="PC5" pad="H6"/>
<connect gate="MCU" pin="PC6" pad="F6"/>
<connect gate="MCU" pin="PC7" pad="E7"/>
<connect gate="MCU" pin="PC8" pad="E8"/>
<connect gate="MCU" pin="PC9" pad="D8"/>
<connect gate="MCU" pin="PD2" pad="B5"/>
<connect gate="MCU" pin="VDDA" pad="H1"/>
<connect gate="MCU" pin="VLCD" pad="B2"/>
<connect gate="MCU" pin="VREF+" pad="G1"/>
<connect gate="MCU" pin="VSSA" pad="F1"/>
<connect gate="PWR" pin="VDD@1" pad="E6"/>
<connect gate="PWR" pin="VDD@2" pad="E5"/>
<connect gate="PWR" pin="VDD@3" pad="E4"/>
<connect gate="PWR" pin="VDD@4" pad="D2"/>
<connect gate="PWR" pin="VSS@1" pad="D6"/>
<connect gate="PWR" pin="VSS@2" pad="D5"/>
<connect gate="PWR" pin="VSS@3" pad="D4"/>
<connect gate="PWR" pin="VSS@4" pad="C2"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L151R*Y">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
384 Kbytes of Flash memory&lt;br&gt;
12 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP11"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="WLCSP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A6"/>
<connect gate="MCU" pin="NRST" pad="C7"/>
<connect gate="MCU" pin="OSC_IN" pad="D8"/>
<connect gate="MCU" pin="OSC_OUT" pad="D7"/>
<connect gate="MCU" pin="PA0-WKUP" pad="F6"/>
<connect gate="MCU" pin="PA1" pad="E6"/>
<connect gate="MCU" pin="PA10" pad="D3"/>
<connect gate="MCU" pin="PA11" pad="C1"/>
<connect gate="MCU" pin="PA12" pad="C2"/>
<connect gate="MCU" pin="PA13" pad="D4"/>
<connect gate="MCU" pin="PA14" pad="B2"/>
<connect gate="MCU" pin="PA15" pad="C3"/>
<connect gate="MCU" pin="PA2" pad="H8"/>
<connect gate="MCU" pin="PA3" pad="G7"/>
<connect gate="MCU" pin="PA4" pad="H7"/>
<connect gate="MCU" pin="PA5" pad="E5"/>
<connect gate="MCU" pin="PA6" pad="G5"/>
<connect gate="MCU" pin="PA7" pad="G4"/>
<connect gate="MCU" pin="PA8" pad="E4"/>
<connect gate="MCU" pin="PA9" pad="D2"/>
<connect gate="MCU" pin="PB0" pad="H4"/>
<connect gate="MCU" pin="PB1" pad="F4"/>
<connect gate="MCU" pin="PB10" pad="G3"/>
<connect gate="MCU" pin="PB11" pad="F3"/>
<connect gate="MCU" pin="PB12" pad="G2"/>
<connect gate="MCU" pin="PB13" pad="G1"/>
<connect gate="MCU" pin="PB14" pad="F2"/>
<connect gate="MCU" pin="PB15" pad="F1"/>
<connect gate="MCU" pin="PB2" pad="H3"/>
<connect gate="MCU" pin="PB3" pad="A4"/>
<connect gate="MCU" pin="PB4" pad="B4"/>
<connect gate="MCU" pin="PB5" pad="A5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="C5"/>
<connect gate="MCU" pin="PB8" pad="D5"/>
<connect gate="MCU" pin="PB9" pad="B6"/>
<connect gate="MCU" pin="PC0" pad="E8"/>
<connect gate="MCU" pin="PC1" pad="F8"/>
<connect gate="MCU" pin="PC10" pad="A2"/>
<connect gate="MCU" pin="PC11" pad="B3"/>
<connect gate="MCU" pin="PC12" pad="C4"/>
<connect gate="MCU" pin="PC13" pad="C8"/>
<connect gate="MCU" pin="PC14" pad="B8"/>
<connect gate="MCU" pin="PC15" pad="B7"/>
<connect gate="MCU" pin="PC2" pad="D6"/>
<connect gate="MCU" pin="PC3" pad="F7"/>
<connect gate="MCU" pin="PC4" pad="H6"/>
<connect gate="MCU" pin="PC5" pad="H5"/>
<connect gate="MCU" pin="PC6" pad="E1"/>
<connect gate="MCU" pin="PC7" pad="E2"/>
<connect gate="MCU" pin="PC8" pad="E3"/>
<connect gate="MCU" pin="PC9" pad="D1"/>
<connect gate="MCU" pin="PD2" pad="A3"/>
<connect gate="MCU" pin="VDDA" pad="G8"/>
<connect gate="MCU" pin="VLCD" pad="C6"/>
<connect gate="MCU" pin="VSSA" pad="E7"/>
<connect gate="PWR" pin="VDD@1" pad="H1"/>
<connect gate="PWR" pin="VDD@2" pad="A1"/>
<connect gate="PWR" pin="VDD@3" pad="A8"/>
<connect gate="PWR" pin="VDD@4" pad="G6"/>
<connect gate="PWR" pin="VSS@1" pad="H2"/>
<connect gate="PWR" pin="VSS@2" pad="B1"/>
<connect gate="PWR" pin="VSS@3" pad="A7"/>
<connect gate="PWR" pin="VSS@4" pad="F5"/>
</connects>
<technologies>
<technology name="D"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L151U*Y" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
256 Kbytes of Flash memory&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_63PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD3_VSS4"/>
</gates>
<devices>
<device name="" package="WLCSP63">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A6"/>
<connect gate="MCU" pin="NRST" pad="E7"/>
<connect gate="MCU" pin="OSC_IN" pad="F6"/>
<connect gate="MCU" pin="OSC_OUT" pad="F7"/>
<connect gate="MCU" pin="PA0-WKUP" pad="E4"/>
<connect gate="MCU" pin="PA1" pad="G5"/>
<connect gate="MCU" pin="PA10" pad="D2"/>
<connect gate="MCU" pin="PA11" pad="B1"/>
<connect gate="MCU" pin="PA12" pad="D3"/>
<connect gate="MCU" pin="PA13" pad="C2"/>
<connect gate="MCU" pin="PA14" pad="C3"/>
<connect gate="MCU" pin="PA15" pad="A2"/>
<connect gate="MCU" pin="PA2" pad="H6"/>
<connect gate="MCU" pin="PA3" pad="J7"/>
<connect gate="MCU" pin="PA4" pad="J6"/>
<connect gate="MCU" pin="PA5" pad="H4"/>
<connect gate="MCU" pin="PA6" pad="G4"/>
<connect gate="MCU" pin="PA7" pad="J5"/>
<connect gate="MCU" pin="PA8" pad="E3"/>
<connect gate="MCU" pin="PA9" pad="C1"/>
<connect gate="MCU" pin="PB0" pad="J3"/>
<connect gate="MCU" pin="PB1" pad="H3"/>
<connect gate="MCU" pin="PB10" pad="J2"/>
<connect gate="MCU" pin="PB11" pad="H2"/>
<connect gate="MCU" pin="PB12" pad="G2"/>
<connect gate="MCU" pin="PB13" pad="G1"/>
<connect gate="MCU" pin="PB14" pad="F3"/>
<connect gate="MCU" pin="PB15" pad="F2"/>
<connect gate="MCU" pin="PB2" pad="G3"/>
<connect gate="MCU" pin="PB3" pad="C4"/>
<connect gate="MCU" pin="PB4" pad="D4"/>
<connect gate="MCU" pin="PB5" pad="A5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="C5"/>
<connect gate="MCU" pin="PB8" pad="B6"/>
<connect gate="MCU" pin="PB9" pad="C6"/>
<connect gate="MCU" pin="PC0" pad="E6"/>
<connect gate="MCU" pin="PC1" pad="E5"/>
<connect gate="MCU" pin="PC10" pad="B3"/>
<connect gate="MCU" pin="PC11" pad="A3"/>
<connect gate="MCU" pin="PC12" pad="B4"/>
<connect gate="MCU" pin="PC13" pad="D5"/>
<connect gate="MCU" pin="PC14" pad="D7"/>
<connect gate="MCU" pin="PC15" pad="D6"/>
<connect gate="MCU" pin="PC2" pad="G7"/>
<connect gate="MCU" pin="PC3" pad="G6"/>
<connect gate="MCU" pin="PC4" pad="F4"/>
<connect gate="MCU" pin="PC5" pad="J4"/>
<connect gate="MCU" pin="PC6" pad="F1"/>
<connect gate="MCU" pin="PC7" pad="E1"/>
<connect gate="MCU" pin="PC8" pad="D1"/>
<connect gate="MCU" pin="PC9" pad="E2"/>
<connect gate="MCU" pin="PD2" pad="A4"/>
<connect gate="MCU" pin="VDDA" pad="H7"/>
<connect gate="MCU" pin="VLCD" pad="C7"/>
<connect gate="MCU" pin="VSSA" pad="F5"/>
<connect gate="PWR" pin="VDD@1" pad="H1"/>
<connect gate="PWR" pin="VDD@2" pad="B2"/>
<connect gate="PWR" pin="VDD@3" pad="B7"/>
<connect gate="PWR" pin="VSS@1" pad="J1"/>
<connect gate="PWR" pin="VSS@2" pad="A1"/>
<connect gate="PWR" pin="VSS@3" pad="A7"/>
<connect gate="PWR" pin="VSS@4" pad="H5"/>
</connects>
<technologies>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L151V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 384 Kbytes of Flash memory&lt;br&gt;
4 to 12 kbytes of SRAM&lt;br&gt;
83 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP10"/>
<gate name="PWR" symbol="PWR_VDD5_VSS5"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="PH2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VLCD" pad="6"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VREF-" pad="20"/>
<connect gate="MCU" pin="VSSA" pad="19"/>
<connect gate="PWR" pin="VDD@1" pad="50"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="100"/>
<connect gate="PWR" pin="VDD@4" pad="28"/>
<connect gate="PWR" pin="VDD@5" pad="11"/>
<connect gate="PWR" pin="VSS@1" pad="49"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
<connect gate="PWR" pin="VSS@3" pad="99"/>
<connect gate="PWR" pin="VSS@4" pad="27"/>
<connect gate="PWR" pin="VSS@5" pad="10"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
<technology name="D"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L151V*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 256 Kbytes of Flash memory&lt;br&gt;
4 to 8 kbytes of SRAM&lt;br&gt;
83 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP10"/>
<gate name="PWR" symbol="PWR_VDD5_VSS5"/>
</gates>
<devices>
<device name="" package="UFBGA100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A4"/>
<connect gate="MCU" pin="NRST" pad="H2"/>
<connect gate="MCU" pin="OSC_IN" pad="F1"/>
<connect gate="MCU" pin="OSC_OUT" pad="G1"/>
<connect gate="MCU" pin="PA0" pad="L2"/>
<connect gate="MCU" pin="PA1" pad="M2"/>
<connect gate="MCU" pin="PA10" pad="C12"/>
<connect gate="MCU" pin="PA11" pad="B12"/>
<connect gate="MCU" pin="PA12" pad="A12"/>
<connect gate="MCU" pin="PA13" pad="A11"/>
<connect gate="MCU" pin="PA14" pad="A10"/>
<connect gate="MCU" pin="PA15" pad="A9"/>
<connect gate="MCU" pin="PA2" pad="K3"/>
<connect gate="MCU" pin="PA3" pad="L3"/>
<connect gate="MCU" pin="PA4" pad="M3"/>
<connect gate="MCU" pin="PA5" pad="K4"/>
<connect gate="MCU" pin="PA6" pad="L4"/>
<connect gate="MCU" pin="PA7" pad="M4"/>
<connect gate="MCU" pin="PA8" pad="D11"/>
<connect gate="MCU" pin="PA9" pad="D10"/>
<connect gate="MCU" pin="PB0" pad="M5"/>
<connect gate="MCU" pin="PB1" pad="M6"/>
<connect gate="MCU" pin="PB10" pad="L10"/>
<connect gate="MCU" pin="PB11" pad="L11"/>
<connect gate="MCU" pin="PB12" pad="L12"/>
<connect gate="MCU" pin="PB13" pad="K12"/>
<connect gate="MCU" pin="PB14" pad="K11"/>
<connect gate="MCU" pin="PB15" pad="K10"/>
<connect gate="MCU" pin="PB2" pad="L6"/>
<connect gate="MCU" pin="PB3" pad="A8"/>
<connect gate="MCU" pin="PB4" pad="A7"/>
<connect gate="MCU" pin="PB5" pad="C5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="B4"/>
<connect gate="MCU" pin="PB8" pad="A3"/>
<connect gate="MCU" pin="PB9" pad="B3"/>
<connect gate="MCU" pin="PC0" pad="H1"/>
<connect gate="MCU" pin="PC1" pad="J2"/>
<connect gate="MCU" pin="PC10" pad="B11"/>
<connect gate="MCU" pin="PC11" pad="C10"/>
<connect gate="MCU" pin="PC12" pad="B10"/>
<connect gate="MCU" pin="PC13" pad="C1"/>
<connect gate="MCU" pin="PC14" pad="D1"/>
<connect gate="MCU" pin="PC15" pad="E1"/>
<connect gate="MCU" pin="PC2" pad="J3"/>
<connect gate="MCU" pin="PC3" pad="K2"/>
<connect gate="MCU" pin="PC4" pad="K5"/>
<connect gate="MCU" pin="PC5" pad="L5"/>
<connect gate="MCU" pin="PC6" pad="E12"/>
<connect gate="MCU" pin="PC7" pad="E11"/>
<connect gate="MCU" pin="PC8" pad="E10"/>
<connect gate="MCU" pin="PC9" pad="D12"/>
<connect gate="MCU" pin="PD0" pad="C9"/>
<connect gate="MCU" pin="PD1" pad="B9"/>
<connect gate="MCU" pin="PD10" pad="J12"/>
<connect gate="MCU" pin="PD11" pad="J11"/>
<connect gate="MCU" pin="PD12" pad="J10"/>
<connect gate="MCU" pin="PD13" pad="H12"/>
<connect gate="MCU" pin="PD14" pad="H11"/>
<connect gate="MCU" pin="PD15" pad="H10"/>
<connect gate="MCU" pin="PD2" pad="C8"/>
<connect gate="MCU" pin="PD3" pad="B8"/>
<connect gate="MCU" pin="PD4" pad="B7"/>
<connect gate="MCU" pin="PD5" pad="A6"/>
<connect gate="MCU" pin="PD6" pad="B6"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD8" pad="K9"/>
<connect gate="MCU" pin="PD9" pad="K8"/>
<connect gate="MCU" pin="PE0" pad="C3"/>
<connect gate="MCU" pin="PE1" pad="A2"/>
<connect gate="MCU" pin="PE10" pad="L8"/>
<connect gate="MCU" pin="PE11" pad="M9"/>
<connect gate="MCU" pin="PE12" pad="L9"/>
<connect gate="MCU" pin="PE13" pad="M10"/>
<connect gate="MCU" pin="PE14" pad="M11"/>
<connect gate="MCU" pin="PE15" pad="M12"/>
<connect gate="MCU" pin="PE2" pad="B2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="C2"/>
<connect gate="MCU" pin="PE6" pad="D2"/>
<connect gate="MCU" pin="PE7" pad="M7"/>
<connect gate="MCU" pin="PE8" pad="L7"/>
<connect gate="MCU" pin="PE9" pad="M8"/>
<connect gate="MCU" pin="PH2" pad="C11"/>
<connect gate="MCU" pin="VDDA" pad="M1"/>
<connect gate="MCU" pin="VLCD" pad="E2"/>
<connect gate="MCU" pin="VREF+" pad="L1"/>
<connect gate="MCU" pin="VREF-" pad="K1"/>
<connect gate="MCU" pin="VSSA" pad="J1"/>
<connect gate="PWR" pin="VDD@1" pad="G12"/>
<connect gate="PWR" pin="VDD@2" pad="G11"/>
<connect gate="PWR" pin="VDD@3" pad="C4"/>
<connect gate="PWR" pin="VDD@4" pad="H3"/>
<connect gate="PWR" pin="VDD@5" pad="G2"/>
<connect gate="PWR" pin="VSS@1" pad="F12"/>
<connect gate="PWR" pin="VSS@2" pad="F11"/>
<connect gate="PWR" pin="VSS@3" pad="D3"/>
<connect gate="PWR" pin="VSS@4" pad="E3"/>
<connect gate="PWR" pin="VSS@5" pad="F2"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L151Q*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
384 Kbytes of Flash memory&lt;br&gt;
12 kbytes of SRAM&lt;br&gt;
109 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_132PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD7_VSS7"/>
</gates>
<devices>
<device name="" package="UFBGA132">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A4"/>
<connect gate="MCU" pin="NRST" pad="H2"/>
<connect gate="MCU" pin="OPAMP1" pad="M3"/>
<connect gate="MCU" pin="OPAMP2" pad="M4"/>
<connect gate="MCU" pin="OPAMP3" pad="K1"/>
<connect gate="MCU" pin="OSC_IN" pad="F1"/>
<connect gate="MCU" pin="OSC_OUT" pad="G1"/>
<connect gate="MCU" pin="PA0" pad="L2"/>
<connect gate="MCU" pin="PA1" pad="M2"/>
<connect gate="MCU" pin="PA10" pad="C12"/>
<connect gate="MCU" pin="PA11" pad="B12"/>
<connect gate="MCU" pin="PA12" pad="A12"/>
<connect gate="MCU" pin="PA13" pad="A11"/>
<connect gate="MCU" pin="PA14" pad="A10"/>
<connect gate="MCU" pin="PA15" pad="A9"/>
<connect gate="MCU" pin="PA2" pad="K3"/>
<connect gate="MCU" pin="PA3" pad="L3"/>
<connect gate="MCU" pin="PA4" pad="J4"/>
<connect gate="MCU" pin="PA5" pad="K4"/>
<connect gate="MCU" pin="PA6" pad="L4"/>
<connect gate="MCU" pin="PA7" pad="J5"/>
<connect gate="MCU" pin="PA8" pad="D11"/>
<connect gate="MCU" pin="PA9" pad="D10"/>
<connect gate="MCU" pin="PB0" pad="M5"/>
<connect gate="MCU" pin="PB1" pad="M6"/>
<connect gate="MCU" pin="PB10" pad="L10"/>
<connect gate="MCU" pin="PB11" pad="L11"/>
<connect gate="MCU" pin="PB12" pad="L12"/>
<connect gate="MCU" pin="PB13" pad="K12"/>
<connect gate="MCU" pin="PB14" pad="K11"/>
<connect gate="MCU" pin="PB15" pad="K10"/>
<connect gate="MCU" pin="PB2" pad="L6"/>
<connect gate="MCU" pin="PB3" pad="A8"/>
<connect gate="MCU" pin="PB4" pad="A7"/>
<connect gate="MCU" pin="PB5" pad="C5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="B4"/>
<connect gate="MCU" pin="PB8" pad="A3"/>
<connect gate="MCU" pin="PB9" pad="B3"/>
<connect gate="MCU" pin="PC0" pad="H1"/>
<connect gate="MCU" pin="PC1" pad="J2"/>
<connect gate="MCU" pin="PC10" pad="B11"/>
<connect gate="MCU" pin="PC11" pad="C10"/>
<connect gate="MCU" pin="PC12" pad="B10"/>
<connect gate="MCU" pin="PC13" pad="C1"/>
<connect gate="MCU" pin="PC14" pad="D1"/>
<connect gate="MCU" pin="PC15" pad="E1"/>
<connect gate="MCU" pin="PC2" pad="J3"/>
<connect gate="MCU" pin="PC3" pad="K2"/>
<connect gate="MCU" pin="PC4" pad="K5"/>
<connect gate="MCU" pin="PC5" pad="L5"/>
<connect gate="MCU" pin="PC6" pad="E12"/>
<connect gate="MCU" pin="PC7" pad="E11"/>
<connect gate="MCU" pin="PC8" pad="E10"/>
<connect gate="MCU" pin="PC9" pad="D12"/>
<connect gate="MCU" pin="PD0" pad="C9"/>
<connect gate="MCU" pin="PD1" pad="B9"/>
<connect gate="MCU" pin="PD10" pad="J12"/>
<connect gate="MCU" pin="PD11" pad="J11"/>
<connect gate="MCU" pin="PD12" pad="J10"/>
<connect gate="MCU" pin="PD13" pad="H12"/>
<connect gate="MCU" pin="PD14" pad="H11"/>
<connect gate="MCU" pin="PD15" pad="H10"/>
<connect gate="MCU" pin="PD2" pad="C8"/>
<connect gate="MCU" pin="PD3" pad="B8"/>
<connect gate="MCU" pin="PD4" pad="B7"/>
<connect gate="MCU" pin="PD5" pad="A6"/>
<connect gate="MCU" pin="PD6" pad="B6"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD8" pad="K9"/>
<connect gate="MCU" pin="PD9" pad="K8"/>
<connect gate="MCU" pin="PE0" pad="C3"/>
<connect gate="MCU" pin="PE1" pad="A2"/>
<connect gate="MCU" pin="PE10" pad="L8"/>
<connect gate="MCU" pin="PE11" pad="M9"/>
<connect gate="MCU" pin="PE12" pad="L9"/>
<connect gate="MCU" pin="PE13" pad="M10"/>
<connect gate="MCU" pin="PE14" pad="M11"/>
<connect gate="MCU" pin="PE15" pad="M12"/>
<connect gate="MCU" pin="PE2" pad="B2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="C2"/>
<connect gate="MCU" pin="PE6" pad="D2"/>
<connect gate="MCU" pin="PE7" pad="M7"/>
<connect gate="MCU" pin="PE8" pad="L7"/>
<connect gate="MCU" pin="PE9" pad="M8"/>
<connect gate="MCU" pin="PF0" pad="D6"/>
<connect gate="MCU" pin="PF1" pad="D5"/>
<connect gate="MCU" pin="PF11" pad="K6"/>
<connect gate="MCU" pin="PF12" pad="J7"/>
<connect gate="MCU" pin="PF13" pad="K7"/>
<connect gate="MCU" pin="PF14" pad="J8"/>
<connect gate="MCU" pin="PF15" pad="J9"/>
<connect gate="MCU" pin="PF2" pad="D4"/>
<connect gate="MCU" pin="PF3" pad="E4"/>
<connect gate="MCU" pin="PF4" pad="F3"/>
<connect gate="MCU" pin="PF5" pad="F4"/>
<connect gate="MCU" pin="PF6" pad="G3"/>
<connect gate="MCU" pin="PF7" pad="G4"/>
<connect gate="MCU" pin="PF8" pad="H4"/>
<connect gate="MCU" pin="PF9" pad="J6"/>
<connect gate="MCU" pin="PG0" pad="H9"/>
<connect gate="MCU" pin="PG1" pad="G9"/>
<connect gate="MCU" pin="PG10" pad="D8"/>
<connect gate="MCU" pin="PG12" pad="D7"/>
<connect gate="MCU" pin="PG13" pad="C7"/>
<connect gate="MCU" pin="PG14" pad="C6"/>
<connect gate="MCU" pin="PG2" pad="G10"/>
<connect gate="MCU" pin="PG3" pad="F9"/>
<connect gate="MCU" pin="PG4" pad="F10"/>
<connect gate="MCU" pin="PG5" pad="E9"/>
<connect gate="MCU" pin="PG9" pad="D9"/>
<connect gate="MCU" pin="PH2" pad="C11"/>
<connect gate="MCU" pin="VDDA" pad="M1"/>
<connect gate="MCU" pin="VLCD" pad="E2"/>
<connect gate="MCU" pin="VREF+" pad="L1"/>
<connect gate="MCU" pin="VSSA" pad="J1"/>
<connect gate="PWR" pin="VDD@1" pad="G12"/>
<connect gate="PWR" pin="VDD@2" pad="G11"/>
<connect gate="PWR" pin="VDD@3" pad="C4"/>
<connect gate="PWR" pin="VDD@4" pad="G7"/>
<connect gate="PWR" pin="VDD@5" pad="G2"/>
<connect gate="PWR" pin="VDD@6" pad="H3"/>
<connect gate="PWR" pin="VDD@7" pad="G6"/>
<connect gate="PWR" pin="VSS@1" pad="F12"/>
<connect gate="PWR" pin="VSS@2" pad="F11"/>
<connect gate="PWR" pin="VSS@3" pad="D3"/>
<connect gate="PWR" pin="VSS@4" pad="F7"/>
<connect gate="PWR" pin="VSS@5" pad="F2"/>
<connect gate="PWR" pin="VSS@6" pad="E3"/>
<connect gate="PWR" pin="VSS@7" pad="F6"/>
</connects>
<technologies>
<technology name="D"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L151Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
384 Kbytes of Flash memory&lt;br&gt;
12 kbytes of SRAM&lt;br&gt;
115 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD11_VSS11"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="PH2" pad="106"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VLCD" pad="6"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VREF-" pad="31"/>
<connect gate="MCU" pin="VSSA" pad="30"/>
<connect gate="PWR" pin="VDD@1" pad="72"/>
<connect gate="PWR" pin="VDD@10" pad="121"/>
<connect gate="PWR" pin="VDD@11" pad="131"/>
<connect gate="PWR" pin="VDD@2" pad="108"/>
<connect gate="PWR" pin="VDD@3" pad="144"/>
<connect gate="PWR" pin="VDD@4" pad="39"/>
<connect gate="PWR" pin="VDD@5" pad="17"/>
<connect gate="PWR" pin="VDD@6" pad="52"/>
<connect gate="PWR" pin="VDD@7" pad="62"/>
<connect gate="PWR" pin="VDD@8" pad="84"/>
<connect gate="PWR" pin="VDD@9" pad="95"/>
<connect gate="PWR" pin="VSS@1" pad="71"/>
<connect gate="PWR" pin="VSS@10" pad="120"/>
<connect gate="PWR" pin="VSS@11" pad="130"/>
<connect gate="PWR" pin="VSS@2" pad="107"/>
<connect gate="PWR" pin="VSS@3" pad="143"/>
<connect gate="PWR" pin="VSS@4" pad="38"/>
<connect gate="PWR" pin="VSS@5" pad="16"/>
<connect gate="PWR" pin="VSS@6" pad="51"/>
<connect gate="PWR" pin="VSS@7" pad="61"/>
<connect gate="PWR" pin="VSS@8" pad="83"/>
<connect gate="PWR" pin="VSS@9" pad="94"/>
</connects>
<technologies>
<technology name="D"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L152C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 256 Kbytes of Flash memory&lt;br&gt;
4 to 8 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP8"/>
<gate name="PWR" symbol="PWR_VDD3_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VLCD" pad="1"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="24"/>
<connect gate="PWR" pin="VDD@2" pad="36"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="35"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L152C*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 256 Kbytes of Flash memory&lt;br&gt;
4 to 8 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP8"/>
<gate name="PWR" symbol="PWR_VDD3_VSS3"/>
</gates>
<devices>
<device name="" package="UFQFPN48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VLCD" pad="1"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="24"/>
<connect gate="PWR" pin="VDD@2" pad="36"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="35"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L152R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 384 Kbytes of Flash memory&lt;br&gt;
4 to 12 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP11"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VLCD" pad="1"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="32"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="31"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
<connect gate="PWR" pin="VSS@3" pad="63"/>
<connect gate="PWR" pin="VSS@4" pad="18"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
<technology name="D"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L152R*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 128 Kbytes of Flash memory&lt;br&gt;
4 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP12"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="TFBGA64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="B4"/>
<connect gate="MCU" pin="NRST" pad="E1"/>
<connect gate="MCU" pin="OSC_IN" pad="C1"/>
<connect gate="MCU" pin="OSC_OUT" pad="D1"/>
<connect gate="MCU" pin="PA0-WKUP" pad="G2"/>
<connect gate="MCU" pin="PA1" pad="H2"/>
<connect gate="MCU" pin="PA10" pad="C6"/>
<connect gate="MCU" pin="PA11" pad="C8"/>
<connect gate="MCU" pin="PA12" pad="B8"/>
<connect gate="MCU" pin="PA13" pad="A8"/>
<connect gate="MCU" pin="PA14" pad="A7"/>
<connect gate="MCU" pin="PA15" pad="A6"/>
<connect gate="MCU" pin="PA2" pad="F3"/>
<connect gate="MCU" pin="PA3" pad="G3"/>
<connect gate="MCU" pin="PA4" pad="H3"/>
<connect gate="MCU" pin="PA5" pad="F4"/>
<connect gate="MCU" pin="PA6" pad="G4"/>
<connect gate="MCU" pin="PA7" pad="H4"/>
<connect gate="MCU" pin="PA8" pad="D7"/>
<connect gate="MCU" pin="PA9" pad="C7"/>
<connect gate="MCU" pin="PB0" pad="F5"/>
<connect gate="MCU" pin="PB1" pad="G5"/>
<connect gate="MCU" pin="PB10" pad="G7"/>
<connect gate="MCU" pin="PB11" pad="H7"/>
<connect gate="MCU" pin="PB12" pad="H8"/>
<connect gate="MCU" pin="PB13" pad="G8"/>
<connect gate="MCU" pin="PB14" pad="F8"/>
<connect gate="MCU" pin="PB15" pad="F7"/>
<connect gate="MCU" pin="PB2" pad="G6"/>
<connect gate="MCU" pin="PB3" pad="A5"/>
<connect gate="MCU" pin="PB4" pad="A4"/>
<connect gate="MCU" pin="PB5" pad="C4"/>
<connect gate="MCU" pin="PB6" pad="D3"/>
<connect gate="MCU" pin="PB7" pad="C3"/>
<connect gate="MCU" pin="PB8" pad="B3"/>
<connect gate="MCU" pin="PB9" pad="A3"/>
<connect gate="MCU" pin="PC0" pad="E3"/>
<connect gate="MCU" pin="PC1" pad="E2"/>
<connect gate="MCU" pin="PC10" pad="B7"/>
<connect gate="MCU" pin="PC11" pad="B6"/>
<connect gate="MCU" pin="PC12" pad="C5"/>
<connect gate="MCU" pin="PC13" pad="A2"/>
<connect gate="MCU" pin="PC14" pad="A1"/>
<connect gate="MCU" pin="PC15" pad="B1"/>
<connect gate="MCU" pin="PC2" pad="F2"/>
<connect gate="MCU" pin="PC4" pad="H5"/>
<connect gate="MCU" pin="PC5" pad="H6"/>
<connect gate="MCU" pin="PC6" pad="F6"/>
<connect gate="MCU" pin="PC7" pad="E7"/>
<connect gate="MCU" pin="PC8" pad="E8"/>
<connect gate="MCU" pin="PC9" pad="D8"/>
<connect gate="MCU" pin="PD2" pad="B5"/>
<connect gate="MCU" pin="VDDA" pad="H1"/>
<connect gate="MCU" pin="VLCD" pad="B2"/>
<connect gate="MCU" pin="VREF+" pad="G1"/>
<connect gate="MCU" pin="VSSA" pad="F1"/>
<connect gate="PWR" pin="VDD@1" pad="E6"/>
<connect gate="PWR" pin="VDD@2" pad="E5"/>
<connect gate="PWR" pin="VDD@3" pad="E4"/>
<connect gate="PWR" pin="VDD@4" pad="D2"/>
<connect gate="PWR" pin="VSS@1" pad="D6"/>
<connect gate="PWR" pin="VSS@2" pad="D5"/>
<connect gate="PWR" pin="VSS@3" pad="D4"/>
<connect gate="PWR" pin="VSS@4" pad="C2"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L152R*Y">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
384 Kbytes of Flash memory&lt;br&gt;
12 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP11"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="WLCSP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A6"/>
<connect gate="MCU" pin="NRST" pad="C7"/>
<connect gate="MCU" pin="OSC_IN" pad="D8"/>
<connect gate="MCU" pin="OSC_OUT" pad="D7"/>
<connect gate="MCU" pin="PA0-WKUP" pad="F6"/>
<connect gate="MCU" pin="PA1" pad="E6"/>
<connect gate="MCU" pin="PA10" pad="D3"/>
<connect gate="MCU" pin="PA11" pad="C1"/>
<connect gate="MCU" pin="PA12" pad="C2"/>
<connect gate="MCU" pin="PA13" pad="D4"/>
<connect gate="MCU" pin="PA14" pad="B2"/>
<connect gate="MCU" pin="PA15" pad="C3"/>
<connect gate="MCU" pin="PA2" pad="H8"/>
<connect gate="MCU" pin="PA3" pad="G7"/>
<connect gate="MCU" pin="PA4" pad="H7"/>
<connect gate="MCU" pin="PA5" pad="E5"/>
<connect gate="MCU" pin="PA6" pad="G5"/>
<connect gate="MCU" pin="PA7" pad="G4"/>
<connect gate="MCU" pin="PA8" pad="E4"/>
<connect gate="MCU" pin="PA9" pad="D2"/>
<connect gate="MCU" pin="PB0" pad="H4"/>
<connect gate="MCU" pin="PB1" pad="F4"/>
<connect gate="MCU" pin="PB10" pad="G3"/>
<connect gate="MCU" pin="PB11" pad="F3"/>
<connect gate="MCU" pin="PB12" pad="G2"/>
<connect gate="MCU" pin="PB13" pad="G1"/>
<connect gate="MCU" pin="PB14" pad="F2"/>
<connect gate="MCU" pin="PB15" pad="F1"/>
<connect gate="MCU" pin="PB2" pad="H3"/>
<connect gate="MCU" pin="PB3" pad="A4"/>
<connect gate="MCU" pin="PB4" pad="B4"/>
<connect gate="MCU" pin="PB5" pad="A5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="C5"/>
<connect gate="MCU" pin="PB8" pad="D5"/>
<connect gate="MCU" pin="PB9" pad="B6"/>
<connect gate="MCU" pin="PC0" pad="E8"/>
<connect gate="MCU" pin="PC1" pad="F8"/>
<connect gate="MCU" pin="PC10" pad="A2"/>
<connect gate="MCU" pin="PC11" pad="B3"/>
<connect gate="MCU" pin="PC12" pad="C4"/>
<connect gate="MCU" pin="PC13" pad="C8"/>
<connect gate="MCU" pin="PC14" pad="B8"/>
<connect gate="MCU" pin="PC15" pad="B7"/>
<connect gate="MCU" pin="PC2" pad="D6"/>
<connect gate="MCU" pin="PC3" pad="F7"/>
<connect gate="MCU" pin="PC4" pad="H6"/>
<connect gate="MCU" pin="PC5" pad="H5"/>
<connect gate="MCU" pin="PC6" pad="E1"/>
<connect gate="MCU" pin="PC7" pad="E2"/>
<connect gate="MCU" pin="PC8" pad="E3"/>
<connect gate="MCU" pin="PC9" pad="D1"/>
<connect gate="MCU" pin="PD2" pad="A3"/>
<connect gate="MCU" pin="VDDA" pad="G8"/>
<connect gate="MCU" pin="VLCD" pad="C6"/>
<connect gate="MCU" pin="VSSA" pad="E7"/>
<connect gate="PWR" pin="VDD@1" pad="H1"/>
<connect gate="PWR" pin="VDD@2" pad="A1"/>
<connect gate="PWR" pin="VDD@3" pad="A8"/>
<connect gate="PWR" pin="VDD@4" pad="G6"/>
<connect gate="PWR" pin="VSS@1" pad="H2"/>
<connect gate="PWR" pin="VSS@2" pad="B1"/>
<connect gate="PWR" pin="VSS@3" pad="A7"/>
<connect gate="PWR" pin="VSS@4" pad="F5"/>
</connects>
<technologies>
<technology name="D"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L152U*Y" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
256 Kbytes of Flash memory&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_63PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD3_VSS4"/>
</gates>
<devices>
<device name="" package="WLCSP63">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A6"/>
<connect gate="MCU" pin="NRST" pad="E7"/>
<connect gate="MCU" pin="OSC_IN" pad="F6"/>
<connect gate="MCU" pin="OSC_OUT" pad="F7"/>
<connect gate="MCU" pin="PA0-WKUP" pad="E4"/>
<connect gate="MCU" pin="PA1" pad="G5"/>
<connect gate="MCU" pin="PA10" pad="D2"/>
<connect gate="MCU" pin="PA11" pad="B1"/>
<connect gate="MCU" pin="PA12" pad="D3"/>
<connect gate="MCU" pin="PA13" pad="C2"/>
<connect gate="MCU" pin="PA14" pad="C3"/>
<connect gate="MCU" pin="PA15" pad="A2"/>
<connect gate="MCU" pin="PA2" pad="H6"/>
<connect gate="MCU" pin="PA3" pad="J7"/>
<connect gate="MCU" pin="PA4" pad="J6"/>
<connect gate="MCU" pin="PA5" pad="H4"/>
<connect gate="MCU" pin="PA6" pad="G4"/>
<connect gate="MCU" pin="PA7" pad="J5"/>
<connect gate="MCU" pin="PA8" pad="E3"/>
<connect gate="MCU" pin="PA9" pad="C1"/>
<connect gate="MCU" pin="PB0" pad="J3"/>
<connect gate="MCU" pin="PB1" pad="H3"/>
<connect gate="MCU" pin="PB10" pad="J2"/>
<connect gate="MCU" pin="PB11" pad="H2"/>
<connect gate="MCU" pin="PB12" pad="G2"/>
<connect gate="MCU" pin="PB13" pad="G1"/>
<connect gate="MCU" pin="PB14" pad="F3"/>
<connect gate="MCU" pin="PB15" pad="F2"/>
<connect gate="MCU" pin="PB2" pad="G3"/>
<connect gate="MCU" pin="PB3" pad="C4"/>
<connect gate="MCU" pin="PB4" pad="D4"/>
<connect gate="MCU" pin="PB5" pad="A5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="C5"/>
<connect gate="MCU" pin="PB8" pad="B6"/>
<connect gate="MCU" pin="PB9" pad="C6"/>
<connect gate="MCU" pin="PC0" pad="E6"/>
<connect gate="MCU" pin="PC1" pad="E5"/>
<connect gate="MCU" pin="PC10" pad="B3"/>
<connect gate="MCU" pin="PC11" pad="A3"/>
<connect gate="MCU" pin="PC12" pad="B4"/>
<connect gate="MCU" pin="PC13" pad="D5"/>
<connect gate="MCU" pin="PC14" pad="D7"/>
<connect gate="MCU" pin="PC15" pad="D6"/>
<connect gate="MCU" pin="PC2" pad="G7"/>
<connect gate="MCU" pin="PC3" pad="G6"/>
<connect gate="MCU" pin="PC4" pad="F4"/>
<connect gate="MCU" pin="PC5" pad="J4"/>
<connect gate="MCU" pin="PC6" pad="F1"/>
<connect gate="MCU" pin="PC7" pad="E1"/>
<connect gate="MCU" pin="PC8" pad="D1"/>
<connect gate="MCU" pin="PC9" pad="E2"/>
<connect gate="MCU" pin="PD2" pad="A4"/>
<connect gate="MCU" pin="VDDA" pad="H7"/>
<connect gate="MCU" pin="VLCD" pad="C7"/>
<connect gate="MCU" pin="VSSA" pad="F5"/>
<connect gate="PWR" pin="VDD@1" pad="H1"/>
<connect gate="PWR" pin="VDD@2" pad="B2"/>
<connect gate="PWR" pin="VDD@3" pad="B7"/>
<connect gate="PWR" pin="VSS@1" pad="J1"/>
<connect gate="PWR" pin="VSS@2" pad="A1"/>
<connect gate="PWR" pin="VSS@3" pad="A7"/>
<connect gate="PWR" pin="VSS@4" pad="H5"/>
</connects>
<technologies>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L152V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 384 Kbytes of Flash memory&lt;br&gt;
4 to 12 kbytes of SRAM&lt;br&gt;
83 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP10"/>
<gate name="PWR" symbol="PWR_VDD5_VSS5"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="PH2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VLCD" pad="6"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VREF-" pad="20"/>
<connect gate="MCU" pin="VSSA" pad="19"/>
<connect gate="PWR" pin="VDD@1" pad="50"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="100"/>
<connect gate="PWR" pin="VDD@4" pad="28"/>
<connect gate="PWR" pin="VDD@5" pad="11"/>
<connect gate="PWR" pin="VSS@1" pad="49"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
<connect gate="PWR" pin="VSS@3" pad="99"/>
<connect gate="PWR" pin="VSS@4" pad="27"/>
<connect gate="PWR" pin="VSS@5" pad="10"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
<technology name="D"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L152V*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 256 Kbytes of Flash memory&lt;br&gt;
4 to 8 kbytes of SRAM&lt;br&gt;
83 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP10"/>
<gate name="PWR" symbol="PWR_VDD5_VSS5"/>
</gates>
<devices>
<device name="" package="UFBGA100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A4"/>
<connect gate="MCU" pin="NRST" pad="H2"/>
<connect gate="MCU" pin="OSC_IN" pad="F1"/>
<connect gate="MCU" pin="OSC_OUT" pad="G1"/>
<connect gate="MCU" pin="PA0" pad="L2"/>
<connect gate="MCU" pin="PA1" pad="M2"/>
<connect gate="MCU" pin="PA10" pad="C12"/>
<connect gate="MCU" pin="PA11" pad="B12"/>
<connect gate="MCU" pin="PA12" pad="A12"/>
<connect gate="MCU" pin="PA13" pad="A11"/>
<connect gate="MCU" pin="PA14" pad="A10"/>
<connect gate="MCU" pin="PA15" pad="A9"/>
<connect gate="MCU" pin="PA2" pad="K3"/>
<connect gate="MCU" pin="PA3" pad="L3"/>
<connect gate="MCU" pin="PA4" pad="M3"/>
<connect gate="MCU" pin="PA5" pad="K4"/>
<connect gate="MCU" pin="PA6" pad="L4"/>
<connect gate="MCU" pin="PA7" pad="M4"/>
<connect gate="MCU" pin="PA8" pad="D11"/>
<connect gate="MCU" pin="PA9" pad="D10"/>
<connect gate="MCU" pin="PB0" pad="M5"/>
<connect gate="MCU" pin="PB1" pad="M6"/>
<connect gate="MCU" pin="PB10" pad="L10"/>
<connect gate="MCU" pin="PB11" pad="L11"/>
<connect gate="MCU" pin="PB12" pad="L12"/>
<connect gate="MCU" pin="PB13" pad="K12"/>
<connect gate="MCU" pin="PB14" pad="K11"/>
<connect gate="MCU" pin="PB15" pad="K10"/>
<connect gate="MCU" pin="PB2" pad="L6"/>
<connect gate="MCU" pin="PB3" pad="A8"/>
<connect gate="MCU" pin="PB4" pad="A7"/>
<connect gate="MCU" pin="PB5" pad="C5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="B4"/>
<connect gate="MCU" pin="PB8" pad="A3"/>
<connect gate="MCU" pin="PB9" pad="B3"/>
<connect gate="MCU" pin="PC0" pad="H1"/>
<connect gate="MCU" pin="PC1" pad="J2"/>
<connect gate="MCU" pin="PC10" pad="B11"/>
<connect gate="MCU" pin="PC11" pad="C10"/>
<connect gate="MCU" pin="PC12" pad="B10"/>
<connect gate="MCU" pin="PC13" pad="C1"/>
<connect gate="MCU" pin="PC14" pad="D1"/>
<connect gate="MCU" pin="PC15" pad="E1"/>
<connect gate="MCU" pin="PC2" pad="J3"/>
<connect gate="MCU" pin="PC3" pad="K2"/>
<connect gate="MCU" pin="PC4" pad="K5"/>
<connect gate="MCU" pin="PC5" pad="L5"/>
<connect gate="MCU" pin="PC6" pad="E12"/>
<connect gate="MCU" pin="PC7" pad="E11"/>
<connect gate="MCU" pin="PC8" pad="E10"/>
<connect gate="MCU" pin="PC9" pad="D12"/>
<connect gate="MCU" pin="PD0" pad="C9"/>
<connect gate="MCU" pin="PD1" pad="B9"/>
<connect gate="MCU" pin="PD10" pad="J12"/>
<connect gate="MCU" pin="PD11" pad="J11"/>
<connect gate="MCU" pin="PD12" pad="J10"/>
<connect gate="MCU" pin="PD13" pad="H12"/>
<connect gate="MCU" pin="PD14" pad="H11"/>
<connect gate="MCU" pin="PD15" pad="H10"/>
<connect gate="MCU" pin="PD2" pad="C8"/>
<connect gate="MCU" pin="PD3" pad="B8"/>
<connect gate="MCU" pin="PD4" pad="B7"/>
<connect gate="MCU" pin="PD5" pad="A6"/>
<connect gate="MCU" pin="PD6" pad="B6"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD8" pad="K9"/>
<connect gate="MCU" pin="PD9" pad="K8"/>
<connect gate="MCU" pin="PE0" pad="C3"/>
<connect gate="MCU" pin="PE1" pad="A2"/>
<connect gate="MCU" pin="PE10" pad="L8"/>
<connect gate="MCU" pin="PE11" pad="M9"/>
<connect gate="MCU" pin="PE12" pad="L9"/>
<connect gate="MCU" pin="PE13" pad="M10"/>
<connect gate="MCU" pin="PE14" pad="M11"/>
<connect gate="MCU" pin="PE15" pad="M12"/>
<connect gate="MCU" pin="PE2" pad="B2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="C2"/>
<connect gate="MCU" pin="PE6" pad="D2"/>
<connect gate="MCU" pin="PE7" pad="M7"/>
<connect gate="MCU" pin="PE8" pad="L7"/>
<connect gate="MCU" pin="PE9" pad="M8"/>
<connect gate="MCU" pin="PH2" pad="C11"/>
<connect gate="MCU" pin="VDDA" pad="M1"/>
<connect gate="MCU" pin="VLCD" pad="E2"/>
<connect gate="MCU" pin="VREF+" pad="L1"/>
<connect gate="MCU" pin="VREF-" pad="K1"/>
<connect gate="MCU" pin="VSSA" pad="J1"/>
<connect gate="PWR" pin="VDD@1" pad="G12"/>
<connect gate="PWR" pin="VDD@2" pad="G11"/>
<connect gate="PWR" pin="VDD@3" pad="C4"/>
<connect gate="PWR" pin="VDD@4" pad="H3"/>
<connect gate="PWR" pin="VDD@5" pad="G2"/>
<connect gate="PWR" pin="VSS@1" pad="F12"/>
<connect gate="PWR" pin="VSS@2" pad="F11"/>
<connect gate="PWR" pin="VSS@3" pad="D3"/>
<connect gate="PWR" pin="VSS@4" pad="E3"/>
<connect gate="PWR" pin="VSS@5" pad="F2"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L152Q*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
384 Kbytes of Flash memory&lt;br&gt;
12 kbytes of SRAM&lt;br&gt;
109 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_132PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD7_VSS7"/>
</gates>
<devices>
<device name="" package="UFBGA132">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A4"/>
<connect gate="MCU" pin="NRST" pad="H2"/>
<connect gate="MCU" pin="OPAMP1" pad="M3"/>
<connect gate="MCU" pin="OPAMP2" pad="M4"/>
<connect gate="MCU" pin="OPAMP3" pad="K1"/>
<connect gate="MCU" pin="OSC_IN" pad="F1"/>
<connect gate="MCU" pin="OSC_OUT" pad="G1"/>
<connect gate="MCU" pin="PA0" pad="L2"/>
<connect gate="MCU" pin="PA1" pad="M2"/>
<connect gate="MCU" pin="PA10" pad="C12"/>
<connect gate="MCU" pin="PA11" pad="B12"/>
<connect gate="MCU" pin="PA12" pad="A12"/>
<connect gate="MCU" pin="PA13" pad="A11"/>
<connect gate="MCU" pin="PA14" pad="A10"/>
<connect gate="MCU" pin="PA15" pad="A9"/>
<connect gate="MCU" pin="PA2" pad="K3"/>
<connect gate="MCU" pin="PA3" pad="L3"/>
<connect gate="MCU" pin="PA4" pad="J4"/>
<connect gate="MCU" pin="PA5" pad="K4"/>
<connect gate="MCU" pin="PA6" pad="L4"/>
<connect gate="MCU" pin="PA7" pad="J5"/>
<connect gate="MCU" pin="PA8" pad="D11"/>
<connect gate="MCU" pin="PA9" pad="D10"/>
<connect gate="MCU" pin="PB0" pad="M5"/>
<connect gate="MCU" pin="PB1" pad="M6"/>
<connect gate="MCU" pin="PB10" pad="L10"/>
<connect gate="MCU" pin="PB11" pad="L11"/>
<connect gate="MCU" pin="PB12" pad="L12"/>
<connect gate="MCU" pin="PB13" pad="K12"/>
<connect gate="MCU" pin="PB14" pad="K11"/>
<connect gate="MCU" pin="PB15" pad="K10"/>
<connect gate="MCU" pin="PB2" pad="L6"/>
<connect gate="MCU" pin="PB3" pad="A8"/>
<connect gate="MCU" pin="PB4" pad="A7"/>
<connect gate="MCU" pin="PB5" pad="C5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="B4"/>
<connect gate="MCU" pin="PB8" pad="A3"/>
<connect gate="MCU" pin="PB9" pad="B3"/>
<connect gate="MCU" pin="PC0" pad="H1"/>
<connect gate="MCU" pin="PC1" pad="J2"/>
<connect gate="MCU" pin="PC10" pad="B11"/>
<connect gate="MCU" pin="PC11" pad="C10"/>
<connect gate="MCU" pin="PC12" pad="B10"/>
<connect gate="MCU" pin="PC13" pad="C1"/>
<connect gate="MCU" pin="PC14" pad="D1"/>
<connect gate="MCU" pin="PC15" pad="E1"/>
<connect gate="MCU" pin="PC2" pad="J3"/>
<connect gate="MCU" pin="PC3" pad="K2"/>
<connect gate="MCU" pin="PC4" pad="K5"/>
<connect gate="MCU" pin="PC5" pad="L5"/>
<connect gate="MCU" pin="PC6" pad="E12"/>
<connect gate="MCU" pin="PC7" pad="E11"/>
<connect gate="MCU" pin="PC8" pad="E10"/>
<connect gate="MCU" pin="PC9" pad="D12"/>
<connect gate="MCU" pin="PD0" pad="C9"/>
<connect gate="MCU" pin="PD1" pad="B9"/>
<connect gate="MCU" pin="PD10" pad="J12"/>
<connect gate="MCU" pin="PD11" pad="J11"/>
<connect gate="MCU" pin="PD12" pad="J10"/>
<connect gate="MCU" pin="PD13" pad="H12"/>
<connect gate="MCU" pin="PD14" pad="H11"/>
<connect gate="MCU" pin="PD15" pad="H10"/>
<connect gate="MCU" pin="PD2" pad="C8"/>
<connect gate="MCU" pin="PD3" pad="B8"/>
<connect gate="MCU" pin="PD4" pad="B7"/>
<connect gate="MCU" pin="PD5" pad="A6"/>
<connect gate="MCU" pin="PD6" pad="B6"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD8" pad="K9"/>
<connect gate="MCU" pin="PD9" pad="K8"/>
<connect gate="MCU" pin="PE0" pad="C3"/>
<connect gate="MCU" pin="PE1" pad="A2"/>
<connect gate="MCU" pin="PE10" pad="L8"/>
<connect gate="MCU" pin="PE11" pad="M9"/>
<connect gate="MCU" pin="PE12" pad="L9"/>
<connect gate="MCU" pin="PE13" pad="M10"/>
<connect gate="MCU" pin="PE14" pad="M11"/>
<connect gate="MCU" pin="PE15" pad="M12"/>
<connect gate="MCU" pin="PE2" pad="B2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="C2"/>
<connect gate="MCU" pin="PE6" pad="D2"/>
<connect gate="MCU" pin="PE7" pad="M7"/>
<connect gate="MCU" pin="PE8" pad="L7"/>
<connect gate="MCU" pin="PE9" pad="M8"/>
<connect gate="MCU" pin="PF0" pad="D6"/>
<connect gate="MCU" pin="PF1" pad="D5"/>
<connect gate="MCU" pin="PF11" pad="K6"/>
<connect gate="MCU" pin="PF12" pad="J7"/>
<connect gate="MCU" pin="PF13" pad="K7"/>
<connect gate="MCU" pin="PF14" pad="J8"/>
<connect gate="MCU" pin="PF15" pad="J9"/>
<connect gate="MCU" pin="PF2" pad="D4"/>
<connect gate="MCU" pin="PF3" pad="E4"/>
<connect gate="MCU" pin="PF4" pad="F3"/>
<connect gate="MCU" pin="PF5" pad="F4"/>
<connect gate="MCU" pin="PF6" pad="G3"/>
<connect gate="MCU" pin="PF7" pad="G4"/>
<connect gate="MCU" pin="PF8" pad="H4"/>
<connect gate="MCU" pin="PF9" pad="J6"/>
<connect gate="MCU" pin="PG0" pad="H9"/>
<connect gate="MCU" pin="PG1" pad="G9"/>
<connect gate="MCU" pin="PG10" pad="D8"/>
<connect gate="MCU" pin="PG12" pad="D7"/>
<connect gate="MCU" pin="PG13" pad="C7"/>
<connect gate="MCU" pin="PG14" pad="C6"/>
<connect gate="MCU" pin="PG2" pad="G10"/>
<connect gate="MCU" pin="PG3" pad="F9"/>
<connect gate="MCU" pin="PG4" pad="F10"/>
<connect gate="MCU" pin="PG5" pad="E9"/>
<connect gate="MCU" pin="PG9" pad="D9"/>
<connect gate="MCU" pin="PH2" pad="C11"/>
<connect gate="MCU" pin="VDDA" pad="M1"/>
<connect gate="MCU" pin="VLCD" pad="E2"/>
<connect gate="MCU" pin="VREF+" pad="L1"/>
<connect gate="MCU" pin="VSSA" pad="J1"/>
<connect gate="PWR" pin="VDD@1" pad="G12"/>
<connect gate="PWR" pin="VDD@2" pad="G11"/>
<connect gate="PWR" pin="VDD@3" pad="C4"/>
<connect gate="PWR" pin="VDD@4" pad="G7"/>
<connect gate="PWR" pin="VDD@5" pad="G2"/>
<connect gate="PWR" pin="VDD@6" pad="H3"/>
<connect gate="PWR" pin="VDD@7" pad="G6"/>
<connect gate="PWR" pin="VSS@1" pad="F12"/>
<connect gate="PWR" pin="VSS@2" pad="F11"/>
<connect gate="PWR" pin="VSS@3" pad="D3"/>
<connect gate="PWR" pin="VSS@4" pad="F7"/>
<connect gate="PWR" pin="VSS@5" pad="F2"/>
<connect gate="PWR" pin="VSS@6" pad="E3"/>
<connect gate="PWR" pin="VSS@7" pad="F6"/>
</connects>
<technologies>
<technology name="D"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L152Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
384 Kbytes of Flash memory&lt;br&gt;
12 kbytes of SRAM&lt;br&gt;
115 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD11_VSS11"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="PH2" pad="106"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VLCD" pad="6"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VREF-" pad="31"/>
<connect gate="MCU" pin="VSSA" pad="30"/>
<connect gate="PWR" pin="VDD@1" pad="72"/>
<connect gate="PWR" pin="VDD@10" pad="121"/>
<connect gate="PWR" pin="VDD@11" pad="131"/>
<connect gate="PWR" pin="VDD@2" pad="108"/>
<connect gate="PWR" pin="VDD@3" pad="144"/>
<connect gate="PWR" pin="VDD@4" pad="39"/>
<connect gate="PWR" pin="VDD@5" pad="17"/>
<connect gate="PWR" pin="VDD@6" pad="52"/>
<connect gate="PWR" pin="VDD@7" pad="62"/>
<connect gate="PWR" pin="VDD@8" pad="84"/>
<connect gate="PWR" pin="VDD@9" pad="95"/>
<connect gate="PWR" pin="VSS@1" pad="71"/>
<connect gate="PWR" pin="VSS@10" pad="120"/>
<connect gate="PWR" pin="VSS@11" pad="130"/>
<connect gate="PWR" pin="VSS@2" pad="107"/>
<connect gate="PWR" pin="VSS@3" pad="143"/>
<connect gate="PWR" pin="VSS@4" pad="38"/>
<connect gate="PWR" pin="VSS@5" pad="16"/>
<connect gate="PWR" pin="VSS@6" pad="51"/>
<connect gate="PWR" pin="VSS@7" pad="61"/>
<connect gate="PWR" pin="VSS@8" pad="83"/>
<connect gate="PWR" pin="VSS@9" pad="94"/>
</connects>
<technologies>
<technology name="D"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L162R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
256 to 384 Kbytes of Flash memory&lt;br&gt;
8 to12 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP11"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VLCD" pad="1"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="32"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VSS@1" pad="31"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
<connect gate="PWR" pin="VSS@3" pad="63"/>
<connect gate="PWR" pin="VSS@4" pad="18"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="D"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L162R*Y" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
384 Kbytes of Flash memory&lt;br&gt;
12 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP11"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="WLCSP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A6"/>
<connect gate="MCU" pin="NRST" pad="C7"/>
<connect gate="MCU" pin="OSC_IN" pad="D8"/>
<connect gate="MCU" pin="OSC_OUT" pad="D7"/>
<connect gate="MCU" pin="PA0-WKUP" pad="F6"/>
<connect gate="MCU" pin="PA1" pad="E6"/>
<connect gate="MCU" pin="PA10" pad="D3"/>
<connect gate="MCU" pin="PA11" pad="C1"/>
<connect gate="MCU" pin="PA12" pad="C2"/>
<connect gate="MCU" pin="PA13" pad="D4"/>
<connect gate="MCU" pin="PA14" pad="B2"/>
<connect gate="MCU" pin="PA15" pad="C3"/>
<connect gate="MCU" pin="PA2" pad="H8"/>
<connect gate="MCU" pin="PA3" pad="G7"/>
<connect gate="MCU" pin="PA4" pad="H7"/>
<connect gate="MCU" pin="PA5" pad="E5"/>
<connect gate="MCU" pin="PA6" pad="G5"/>
<connect gate="MCU" pin="PA7" pad="G4"/>
<connect gate="MCU" pin="PA8" pad="E4"/>
<connect gate="MCU" pin="PA9" pad="D2"/>
<connect gate="MCU" pin="PB0" pad="H4"/>
<connect gate="MCU" pin="PB1" pad="F4"/>
<connect gate="MCU" pin="PB10" pad="G3"/>
<connect gate="MCU" pin="PB11" pad="F3"/>
<connect gate="MCU" pin="PB12" pad="G2"/>
<connect gate="MCU" pin="PB13" pad="G1"/>
<connect gate="MCU" pin="PB14" pad="F2"/>
<connect gate="MCU" pin="PB15" pad="F1"/>
<connect gate="MCU" pin="PB2" pad="H3"/>
<connect gate="MCU" pin="PB3" pad="A4"/>
<connect gate="MCU" pin="PB4" pad="B4"/>
<connect gate="MCU" pin="PB5" pad="A5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="C5"/>
<connect gate="MCU" pin="PB8" pad="D5"/>
<connect gate="MCU" pin="PB9" pad="B6"/>
<connect gate="MCU" pin="PC0" pad="E8"/>
<connect gate="MCU" pin="PC1" pad="F8"/>
<connect gate="MCU" pin="PC10" pad="A2"/>
<connect gate="MCU" pin="PC11" pad="B3"/>
<connect gate="MCU" pin="PC12" pad="C4"/>
<connect gate="MCU" pin="PC13" pad="C8"/>
<connect gate="MCU" pin="PC14" pad="B8"/>
<connect gate="MCU" pin="PC15" pad="B7"/>
<connect gate="MCU" pin="PC2" pad="D6"/>
<connect gate="MCU" pin="PC3" pad="F7"/>
<connect gate="MCU" pin="PC4" pad="H6"/>
<connect gate="MCU" pin="PC5" pad="H5"/>
<connect gate="MCU" pin="PC6" pad="E1"/>
<connect gate="MCU" pin="PC7" pad="E2"/>
<connect gate="MCU" pin="PC8" pad="E3"/>
<connect gate="MCU" pin="PC9" pad="D1"/>
<connect gate="MCU" pin="PD2" pad="A3"/>
<connect gate="MCU" pin="VDDA" pad="G8"/>
<connect gate="MCU" pin="VLCD" pad="C6"/>
<connect gate="MCU" pin="VSSA" pad="E7"/>
<connect gate="PWR" pin="VDD@1" pad="H1"/>
<connect gate="PWR" pin="VDD@2" pad="A1"/>
<connect gate="PWR" pin="VDD@3" pad="A8"/>
<connect gate="PWR" pin="VDD@4" pad="G6"/>
<connect gate="PWR" pin="VSS@1" pad="H2"/>
<connect gate="PWR" pin="VSS@2" pad="B1"/>
<connect gate="PWR" pin="VSS@3" pad="A7"/>
<connect gate="PWR" pin="VSS@4" pad="F5"/>
</connects>
<technologies>
<technology name="D"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L162V*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
256 to 384 Kbytes of Flash memory&lt;br&gt;
8 to 12 kbytes of SRAM&lt;br&gt;
83 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP10"/>
<gate name="PWR" symbol="PWR_VDD5_VSS5"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="PH2" pad="73"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VLCD" pad="6"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VREF-" pad="20"/>
<connect gate="MCU" pin="VSSA" pad="19"/>
<connect gate="PWR" pin="VDD@1" pad="50"/>
<connect gate="PWR" pin="VDD@2" pad="75"/>
<connect gate="PWR" pin="VDD@3" pad="100"/>
<connect gate="PWR" pin="VDD@4" pad="28"/>
<connect gate="PWR" pin="VDD@5" pad="11"/>
<connect gate="PWR" pin="VSS@1" pad="49"/>
<connect gate="PWR" pin="VSS@2" pad="74"/>
<connect gate="PWR" pin="VSS@3" pad="99"/>
<connect gate="PWR" pin="VSS@4" pad="27"/>
<connect gate="PWR" pin="VSS@5" pad="10"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="D"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L162Q*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
384 Kbytes of Flash memory&lt;br&gt;
12 kbytes of SRAM&lt;br&gt;
109 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_132PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD7_VSS7"/>
</gates>
<devices>
<device name="" package="UFBGA132">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A4"/>
<connect gate="MCU" pin="NRST" pad="H2"/>
<connect gate="MCU" pin="OPAMP1" pad="M3"/>
<connect gate="MCU" pin="OPAMP2" pad="M4"/>
<connect gate="MCU" pin="OPAMP3" pad="K1"/>
<connect gate="MCU" pin="OSC_IN" pad="F1"/>
<connect gate="MCU" pin="OSC_OUT" pad="G1"/>
<connect gate="MCU" pin="PA0" pad="L2"/>
<connect gate="MCU" pin="PA1" pad="M2"/>
<connect gate="MCU" pin="PA10" pad="C12"/>
<connect gate="MCU" pin="PA11" pad="B12"/>
<connect gate="MCU" pin="PA12" pad="A12"/>
<connect gate="MCU" pin="PA13" pad="A11"/>
<connect gate="MCU" pin="PA14" pad="A10"/>
<connect gate="MCU" pin="PA15" pad="A9"/>
<connect gate="MCU" pin="PA2" pad="K3"/>
<connect gate="MCU" pin="PA3" pad="L3"/>
<connect gate="MCU" pin="PA4" pad="J4"/>
<connect gate="MCU" pin="PA5" pad="K4"/>
<connect gate="MCU" pin="PA6" pad="L4"/>
<connect gate="MCU" pin="PA7" pad="J5"/>
<connect gate="MCU" pin="PA8" pad="D11"/>
<connect gate="MCU" pin="PA9" pad="D10"/>
<connect gate="MCU" pin="PB0" pad="M5"/>
<connect gate="MCU" pin="PB1" pad="M6"/>
<connect gate="MCU" pin="PB10" pad="L10"/>
<connect gate="MCU" pin="PB11" pad="L11"/>
<connect gate="MCU" pin="PB12" pad="L12"/>
<connect gate="MCU" pin="PB13" pad="K12"/>
<connect gate="MCU" pin="PB14" pad="K11"/>
<connect gate="MCU" pin="PB15" pad="K10"/>
<connect gate="MCU" pin="PB2" pad="L6"/>
<connect gate="MCU" pin="PB3" pad="A8"/>
<connect gate="MCU" pin="PB4" pad="A7"/>
<connect gate="MCU" pin="PB5" pad="C5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="B4"/>
<connect gate="MCU" pin="PB8" pad="A3"/>
<connect gate="MCU" pin="PB9" pad="B3"/>
<connect gate="MCU" pin="PC0" pad="H1"/>
<connect gate="MCU" pin="PC1" pad="J2"/>
<connect gate="MCU" pin="PC10" pad="B11"/>
<connect gate="MCU" pin="PC11" pad="C10"/>
<connect gate="MCU" pin="PC12" pad="B10"/>
<connect gate="MCU" pin="PC13" pad="C1"/>
<connect gate="MCU" pin="PC14" pad="D1"/>
<connect gate="MCU" pin="PC15" pad="E1"/>
<connect gate="MCU" pin="PC2" pad="J3"/>
<connect gate="MCU" pin="PC3" pad="K2"/>
<connect gate="MCU" pin="PC4" pad="K5"/>
<connect gate="MCU" pin="PC5" pad="L5"/>
<connect gate="MCU" pin="PC6" pad="E12"/>
<connect gate="MCU" pin="PC7" pad="E11"/>
<connect gate="MCU" pin="PC8" pad="E10"/>
<connect gate="MCU" pin="PC9" pad="D12"/>
<connect gate="MCU" pin="PD0" pad="C9"/>
<connect gate="MCU" pin="PD1" pad="B9"/>
<connect gate="MCU" pin="PD10" pad="J12"/>
<connect gate="MCU" pin="PD11" pad="J11"/>
<connect gate="MCU" pin="PD12" pad="J10"/>
<connect gate="MCU" pin="PD13" pad="H12"/>
<connect gate="MCU" pin="PD14" pad="H11"/>
<connect gate="MCU" pin="PD15" pad="H10"/>
<connect gate="MCU" pin="PD2" pad="C8"/>
<connect gate="MCU" pin="PD3" pad="B8"/>
<connect gate="MCU" pin="PD4" pad="B7"/>
<connect gate="MCU" pin="PD5" pad="A6"/>
<connect gate="MCU" pin="PD6" pad="B6"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD8" pad="K9"/>
<connect gate="MCU" pin="PD9" pad="K8"/>
<connect gate="MCU" pin="PE0" pad="C3"/>
<connect gate="MCU" pin="PE1" pad="A2"/>
<connect gate="MCU" pin="PE10" pad="L8"/>
<connect gate="MCU" pin="PE11" pad="M9"/>
<connect gate="MCU" pin="PE12" pad="L9"/>
<connect gate="MCU" pin="PE13" pad="M10"/>
<connect gate="MCU" pin="PE14" pad="M11"/>
<connect gate="MCU" pin="PE15" pad="M12"/>
<connect gate="MCU" pin="PE2" pad="B2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="C2"/>
<connect gate="MCU" pin="PE6" pad="D2"/>
<connect gate="MCU" pin="PE7" pad="M7"/>
<connect gate="MCU" pin="PE8" pad="L7"/>
<connect gate="MCU" pin="PE9" pad="M8"/>
<connect gate="MCU" pin="PF0" pad="D6"/>
<connect gate="MCU" pin="PF1" pad="D5"/>
<connect gate="MCU" pin="PF11" pad="K6"/>
<connect gate="MCU" pin="PF12" pad="J7"/>
<connect gate="MCU" pin="PF13" pad="K7"/>
<connect gate="MCU" pin="PF14" pad="J8"/>
<connect gate="MCU" pin="PF15" pad="J9"/>
<connect gate="MCU" pin="PF2" pad="D4"/>
<connect gate="MCU" pin="PF3" pad="E4"/>
<connect gate="MCU" pin="PF4" pad="F3"/>
<connect gate="MCU" pin="PF5" pad="F4"/>
<connect gate="MCU" pin="PF6" pad="G3"/>
<connect gate="MCU" pin="PF7" pad="G4"/>
<connect gate="MCU" pin="PF8" pad="H4"/>
<connect gate="MCU" pin="PF9" pad="J6"/>
<connect gate="MCU" pin="PG0" pad="H9"/>
<connect gate="MCU" pin="PG1" pad="G9"/>
<connect gate="MCU" pin="PG10" pad="D8"/>
<connect gate="MCU" pin="PG12" pad="D7"/>
<connect gate="MCU" pin="PG13" pad="C7"/>
<connect gate="MCU" pin="PG14" pad="C6"/>
<connect gate="MCU" pin="PG2" pad="G10"/>
<connect gate="MCU" pin="PG3" pad="F9"/>
<connect gate="MCU" pin="PG4" pad="F10"/>
<connect gate="MCU" pin="PG5" pad="E9"/>
<connect gate="MCU" pin="PG9" pad="D9"/>
<connect gate="MCU" pin="PH2" pad="C11"/>
<connect gate="MCU" pin="VDDA" pad="M1"/>
<connect gate="MCU" pin="VLCD" pad="E2"/>
<connect gate="MCU" pin="VREF+" pad="L1"/>
<connect gate="MCU" pin="VSSA" pad="J1"/>
<connect gate="PWR" pin="VDD@1" pad="G12"/>
<connect gate="PWR" pin="VDD@2" pad="G11"/>
<connect gate="PWR" pin="VDD@3" pad="C4"/>
<connect gate="PWR" pin="VDD@4" pad="G7"/>
<connect gate="PWR" pin="VDD@5" pad="G2"/>
<connect gate="PWR" pin="VDD@6" pad="H3"/>
<connect gate="PWR" pin="VDD@7" pad="G6"/>
<connect gate="PWR" pin="VSS@1" pad="F12"/>
<connect gate="PWR" pin="VSS@2" pad="F11"/>
<connect gate="PWR" pin="VSS@3" pad="D3"/>
<connect gate="PWR" pin="VSS@4" pad="F7"/>
<connect gate="PWR" pin="VSS@5" pad="F2"/>
<connect gate="PWR" pin="VSS@6" pad="E3"/>
<connect gate="PWR" pin="VSS@7" pad="F6"/>
</connects>
<technologies>
<technology name="D"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L162Z*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
384 Kbytes of Flash memory&lt;br&gt;
12 kbytes of SRAM&lt;br&gt;
115 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD11_VSS11"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="PH2" pad="106"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VLCD" pad="6"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VREF-" pad="31"/>
<connect gate="MCU" pin="VSSA" pad="30"/>
<connect gate="PWR" pin="VDD@1" pad="72"/>
<connect gate="PWR" pin="VDD@10" pad="121"/>
<connect gate="PWR" pin="VDD@11" pad="131"/>
<connect gate="PWR" pin="VDD@2" pad="108"/>
<connect gate="PWR" pin="VDD@3" pad="144"/>
<connect gate="PWR" pin="VDD@4" pad="39"/>
<connect gate="PWR" pin="VDD@5" pad="17"/>
<connect gate="PWR" pin="VDD@6" pad="52"/>
<connect gate="PWR" pin="VDD@7" pad="62"/>
<connect gate="PWR" pin="VDD@8" pad="84"/>
<connect gate="PWR" pin="VDD@9" pad="95"/>
<connect gate="PWR" pin="VSS@1" pad="71"/>
<connect gate="PWR" pin="VSS@10" pad="120"/>
<connect gate="PWR" pin="VSS@11" pad="130"/>
<connect gate="PWR" pin="VSS@2" pad="107"/>
<connect gate="PWR" pin="VSS@3" pad="143"/>
<connect gate="PWR" pin="VSS@4" pad="38"/>
<connect gate="PWR" pin="VSS@5" pad="16"/>
<connect gate="PWR" pin="VSS@6" pad="51"/>
<connect gate="PWR" pin="VSS@7" pad="61"/>
<connect gate="PWR" pin="VSS@8" pad="83"/>
<connect gate="PWR" pin="VSS@9" pad="94"/>
</connects>
<technologies>
<technology name="D"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32TS60ZH" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
72 MHz maximum frequency&lt;br&gt;
32 Kbytes of Flash memory&lt;br&gt;
10 kbytes of SRAM&lt;br&gt;
138 GPIOs&lt;br&gt;
2.4 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP5"/>
<gate name="PWR" symbol="PWR_VDD2_VSS2"/>
</gates>
<devices>
<device name="" package="UFBGA144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="G6"/>
<connect gate="MCU" pin="NRST" pad="K7"/>
<connect gate="MCU" pin="PA0" pad="A8"/>
<connect gate="MCU" pin="PA1" pad="C9"/>
<connect gate="MCU" pin="PA10" pad="E9"/>
<connect gate="MCU" pin="PA11" pad="C6"/>
<connect gate="MCU" pin="PA12" pad="B6"/>
<connect gate="MCU" pin="PA13" pad="H7"/>
<connect gate="MCU" pin="PA14" pad="H6"/>
<connect gate="MCU" pin="PA15" pad="L8"/>
<connect gate="MCU" pin="PA2" pad="B8"/>
<connect gate="MCU" pin="PA3" pad="D7"/>
<connect gate="MCU" pin="PA4" pad="D8"/>
<connect gate="MCU" pin="PA5" pad="B7"/>
<connect gate="MCU" pin="PA6" pad="C8"/>
<connect gate="MCU" pin="PA7" pad="D6"/>
<connect gate="MCU" pin="PA8" pad="C7"/>
<connect gate="MCU" pin="PA9" pad="G7"/>
<connect gate="MCU" pin="PB0" pad="G8"/>
<connect gate="MCU" pin="PB1" pad="E10"/>
<connect gate="MCU" pin="PB2" pad="G9"/>
<connect gate="MCU" pin="PB3" pad="K8"/>
<connect gate="MCU" pin="PB4" pad="J7"/>
<connect gate="MCU" pin="PB5" pad="M8"/>
<connect gate="MCU" pin="PB6" pad="D5"/>
<connect gate="MCU" pin="PB7" pad="F10"/>
<connect gate="MCU" pin="PB8" pad="D9"/>
<connect gate="MCU" pin="PB9" pad="E5"/>
<connect gate="MCU" pin="PC0" pad="E6"/>
<connect gate="MCU" pin="PC1" pad="E7"/>
<connect gate="MCU" pin="PC10" pad="J6"/>
<connect gate="MCU" pin="PC11" pad="F6"/>
<connect gate="MCU" pin="PC12" pad="C5"/>
<connect gate="MCU" pin="PC13" pad="K6"/>
<connect gate="MCU" pin="PC14" pad="L7"/>
<connect gate="MCU" pin="PC15" pad="L6"/>
<connect gate="MCU" pin="PC2" pad="F5"/>
<connect gate="MCU" pin="PC3" pad="G5"/>
<connect gate="MCU" pin="PC4" pad="H5"/>
<connect gate="MCU" pin="PC5" pad="J5"/>
<connect gate="MCU" pin="PC6" pad="K5"/>
<connect gate="MCU" pin="PC7" pad="M5"/>
<connect gate="MCU" pin="PC8" pad="L5"/>
<connect gate="MCU" pin="PC9" pad="F7"/>
<connect gate="MCU" pin="PD0" pad="K2"/>
<connect gate="MCU" pin="PD1" pad="J4"/>
<connect gate="MCU" pin="PD10" pad="M2"/>
<connect gate="MCU" pin="PD11" pad="L2"/>
<connect gate="MCU" pin="PD12" pad="L3"/>
<connect gate="MCU" pin="PD13" pad="M3"/>
<connect gate="MCU" pin="PD14" pad="L4"/>
<connect gate="MCU" pin="PD15" pad="M4"/>
<connect gate="MCU" pin="PD2" pad="J3"/>
<connect gate="MCU" pin="PD3" pad="J1"/>
<connect gate="MCU" pin="PD4" pad="J2"/>
<connect gate="MCU" pin="PD5" pad="K1"/>
<connect gate="MCU" pin="PD6" pad="L1"/>
<connect gate="MCU" pin="PD7" pad="K3"/>
<connect gate="MCU" pin="PD8" pad="M1"/>
<connect gate="MCU" pin="PD9" pad="K4"/>
<connect gate="MCU" pin="PE0" pad="E1"/>
<connect gate="MCU" pin="PE1" pad="F2"/>
<connect gate="MCU" pin="PE10" pad="G3"/>
<connect gate="MCU" pin="PE11" pad="G1"/>
<connect gate="MCU" pin="PE12" pad="G2"/>
<connect gate="MCU" pin="PE13" pad="H2"/>
<connect gate="MCU" pin="PE14" pad="H3"/>
<connect gate="MCU" pin="PE15" pad="H1"/>
<connect gate="MCU" pin="PE2" pad="F3"/>
<connect gate="MCU" pin="PE3" pad="F4"/>
<connect gate="MCU" pin="PE4" pad="E2"/>
<connect gate="MCU" pin="PE5" pad="E4"/>
<connect gate="MCU" pin="PE6" pad="E3"/>
<connect gate="MCU" pin="PE7" pad="H4"/>
<connect gate="MCU" pin="PE8" pad="F1"/>
<connect gate="MCU" pin="PE9" pad="G4"/>
<connect gate="MCU" pin="PF0" pad="D11"/>
<connect gate="MCU" pin="PF1" pad="A9"/>
<connect gate="MCU" pin="PF10" pad="C11"/>
<connect gate="MCU" pin="PF11" pad="B11"/>
<connect gate="MCU" pin="PF12" pad="B12"/>
<connect gate="MCU" pin="PF13" pad="B10"/>
<connect gate="MCU" pin="PF14" pad="E12"/>
<connect gate="MCU" pin="PF15" pad="C10"/>
<connect gate="MCU" pin="PF2" pad="E11"/>
<connect gate="MCU" pin="PF3" pad="A10"/>
<connect gate="MCU" pin="PF4" pad="D12"/>
<connect gate="MCU" pin="PF5" pad="A11"/>
<connect gate="MCU" pin="PF6" pad="D10"/>
<connect gate="MCU" pin="PF7" pad="A12"/>
<connect gate="MCU" pin="PF8" pad="C12"/>
<connect gate="MCU" pin="PF9" pad="B9"/>
<connect gate="MCU" pin="PG0" pad="E8"/>
<connect gate="MCU" pin="PG1" pad="J8"/>
<connect gate="MCU" pin="PG10" pad="F11"/>
<connect gate="MCU" pin="PG11" pad="F8"/>
<connect gate="MCU" pin="PG12" pad="F12"/>
<connect gate="MCU" pin="PG13" pad="F9"/>
<connect gate="MCU" pin="PG14" pad="G10"/>
<connect gate="MCU" pin="PG15" pad="G12"/>
<connect gate="MCU" pin="PG2" pad="H8"/>
<connect gate="MCU" pin="PG3" pad="H9"/>
<connect gate="MCU" pin="PG4" pad="G11"/>
<connect gate="MCU" pin="PG5" pad="H11"/>
<connect gate="MCU" pin="PG6" pad="A5"/>
<connect gate="MCU" pin="PG7" pad="H10"/>
<connect gate="MCU" pin="PG8" pad="B5"/>
<connect gate="MCU" pin="PG9" pad="H12"/>
<connect gate="MCU" pin="PH0" pad="L9"/>
<connect gate="MCU" pin="PH1" pad="M9"/>
<connect gate="MCU" pin="PH10" pad="L10"/>
<connect gate="MCU" pin="PH11" pad="K11"/>
<connect gate="MCU" pin="PH12" pad="L12"/>
<connect gate="MCU" pin="PH13" pad="J9"/>
<connect gate="MCU" pin="PH14" pad="J12"/>
<connect gate="MCU" pin="PH15" pad="K12"/>
<connect gate="MCU" pin="PH2" pad="J11"/>
<connect gate="MCU" pin="PH3" pad="M12"/>
<connect gate="MCU" pin="PH4" pad="L11"/>
<connect gate="MCU" pin="PH5" pad="M10"/>
<connect gate="MCU" pin="PH6" pad="M11"/>
<connect gate="MCU" pin="PH7" pad="J10"/>
<connect gate="MCU" pin="PH8" pad="K9"/>
<connect gate="MCU" pin="PH9" pad="K10"/>
<connect gate="MCU" pin="PI0" pad="B2"/>
<connect gate="MCU" pin="PI1" pad="D1"/>
<connect gate="MCU" pin="PI10" pad="C4"/>
<connect gate="MCU" pin="PI11" pad="D4"/>
<connect gate="MCU" pin="PI12" pad="A2"/>
<connect gate="MCU" pin="PI13" pad="C1"/>
<connect gate="MCU" pin="PI14" pad="A3"/>
<connect gate="MCU" pin="PI15" pad="B1"/>
<connect gate="MCU" pin="PI2" pad="D2"/>
<connect gate="MCU" pin="PI3" pad="A4"/>
<connect gate="MCU" pin="PI4" pad="B4"/>
<connect gate="MCU" pin="PI5" pad="B3"/>
<connect gate="MCU" pin="PI6" pad="A1"/>
<connect gate="MCU" pin="PI7" pad="C2"/>
<connect gate="MCU" pin="PI8" pad="C3"/>
<connect gate="MCU" pin="PI9" pad="D3"/>
<connect gate="PWR" pin="VDD@1" pad="A6"/>
<connect gate="PWR" pin="VDD@2" pad="M6"/>
<connect gate="PWR" pin="VSS@1" pad="A7"/>
<connect gate="PWR" pin="VSS@2" pad="M7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32W108H*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
24 MHz maximum frequency&lt;br&gt;
128 Kbytes of Flash memory&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
2.1 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32W_40PIN"/>
</gates>
<devices>
<device name="" package="VFQFPN40">
<connects>
<connect gate="MCU" pin="BIAS_R" pad="8"/>
<connect gate="MCU" pin="GND" pad="EXP"/>
<connect gate="MCU" pin="NRESET" pad="11"/>
<connect gate="MCU" pin="OSC_IN" pad="38"/>
<connect gate="MCU" pin="OSC_OUT" pad="39"/>
<connect gate="MCU" pin="PA0" pad="17"/>
<connect gate="MCU" pin="PA1" pad="18"/>
<connect gate="MCU" pin="PA2" pad="20"/>
<connect gate="MCU" pin="PA3" pad="21"/>
<connect gate="MCU" pin="PA4" pad="22"/>
<connect gate="MCU" pin="PA5" pad="23"/>
<connect gate="MCU" pin="PB1" pad="25"/>
<connect gate="MCU" pin="PB2" pad="26"/>
<connect gate="MCU" pin="PB3" pad="15"/>
<connect gate="MCU" pin="PB4" pad="16"/>
<connect gate="MCU" pin="PB6" pad="35"/>
<connect gate="MCU" pin="PB7" pad="34"/>
<connect gate="MCU" pin="PC0" pad="33"/>
<connect gate="MCU" pin="PC1" pad="31"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="30"/>
<connect gate="MCU" pin="PC5" pad="10"/>
<connect gate="MCU" pin="RF_N" pad="3"/>
<connect gate="MCU" pin="RF_P" pad="2"/>
<connect gate="MCU" pin="RF_TX_ALT_N" pad="6"/>
<connect gate="MCU" pin="RF_TX_ALT_P" pad="5"/>
<connect gate="MCU" pin="SWCLK" pad="27"/>
<connect gate="MCU" pin="VDD_24MHZ" pad="40"/>
<connect gate="MCU" pin="VDD_CORE@1" pad="14"/>
<connect gate="MCU" pin="VDD_CORE@2" pad="36"/>
<connect gate="MCU" pin="VDD_IF" pad="7"/>
<connect gate="MCU" pin="VDD_MEM" pad="32"/>
<connect gate="MCU" pin="VDD_PADS@1" pad="13"/>
<connect gate="MCU" pin="VDD_PADS@2" pad="19"/>
<connect gate="MCU" pin="VDD_PADS@3" pad="24"/>
<connect gate="MCU" pin="VDD_PADSA" pad="9"/>
<connect gate="MCU" pin="VDD_PRE" pad="37"/>
<connect gate="MCU" pin="VDD_RF" pad="4"/>
<connect gate="MCU" pin="VDD_VCO" pad="1"/>
<connect gate="MCU" pin="VREG_OUT" pad="12"/>
</connects>
<technologies>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32W108C*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M3 CPU&lt;/b&gt;&lt;p&gt;
24 MHz maximum frequency&lt;br&gt;
128 to 192 Kbytes of Flash memory&lt;br&gt;
8 to 16 kbytes of SRAM&lt;br&gt;
2.1 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32W_48PIN"/>
</gates>
<devices>
<device name="" package="UFQFPN48">
<connects>
<connect gate="MCU" pin="BIAS_R" pad="9"/>
<connect gate="MCU" pin="GND" pad="EXP"/>
<connect gate="MCU" pin="NRESET" pad="12"/>
<connect gate="MCU" pin="OSC_IN" pad="47"/>
<connect gate="MCU" pin="OSC_OUT" pad="48"/>
<connect gate="MCU" pin="PA0" pad="21"/>
<connect gate="MCU" pin="PA1" pad="22"/>
<connect gate="MCU" pin="PA2" pad="24"/>
<connect gate="MCU" pin="PA3" pad="25"/>
<connect gate="MCU" pin="PA4" pad="26"/>
<connect gate="MCU" pin="PA5" pad="27"/>
<connect gate="MCU" pin="PA6" pad="29"/>
<connect gate="MCU" pin="PA7" pad="18"/>
<connect gate="MCU" pin="PB0" pad="36"/>
<connect gate="MCU" pin="PB1" pad="30"/>
<connect gate="MCU" pin="PB2" pad="31"/>
<connect gate="MCU" pin="PB3" pad="19"/>
<connect gate="MCU" pin="PB4" pad="20"/>
<connect gate="MCU" pin="PB5" pad="43"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="41"/>
<connect gate="MCU" pin="PC0" pad="40"/>
<connect gate="MCU" pin="PC1" pad="38"/>
<connect gate="MCU" pin="PC2" pad="33"/>
<connect gate="MCU" pin="PC3" pad="34"/>
<connect gate="MCU" pin="PC4" pad="35"/>
<connect gate="MCU" pin="PC5" pad="11"/>
<connect gate="MCU" pin="PC6" pad="13"/>
<connect gate="MCU" pin="PC7" pad="14"/>
<connect gate="MCU" pin="RF_N" pad="4"/>
<connect gate="MCU" pin="RF_P" pad="3"/>
<connect gate="MCU" pin="RF_TX_ALT_N" pad="7"/>
<connect gate="MCU" pin="RF_TX_ALT_P" pad="6"/>
<connect gate="MCU" pin="SWCLK" pad="32"/>
<connect gate="MCU" pin="VDD_24MHZ" pad="1"/>
<connect gate="MCU" pin="VDD_CORE@1" pad="17"/>
<connect gate="MCU" pin="VDD_CORE@2" pad="44"/>
<connect gate="MCU" pin="VDD_IF" pad="8"/>
<connect gate="MCU" pin="VDD_MEM" pad="39"/>
<connect gate="MCU" pin="VDD_PADS@1" pad="16"/>
<connect gate="MCU" pin="VDD_PADS@2" pad="23"/>
<connect gate="MCU" pin="VDD_PADS@3" pad="28"/>
<connect gate="MCU" pin="VDD_PADS@4" pad="37"/>
<connect gate="MCU" pin="VDD_PADSA" pad="10"/>
<connect gate="MCU" pin="VDD_PRE" pad="45"/>
<connect gate="MCU" pin="VDD_RF" pad="5"/>
<connect gate="MCU" pin="VDD_SYNTH" pad="46"/>
<connect gate="MCU" pin="VDD_VCO" pad="2"/>
<connect gate="MCU" pin="VREG_OUT" pad="15"/>
</connects>
<technologies>
<technology name="8"/>
<technology name="B"/>
<technology name="C"/>
<technology name="Z"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L051K*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
27 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_32PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD2_VSS2"/>
</gates>
<devices>
<device name="" package="LQFP32">
<connects>
<connect gate="MCU" pin="BOOT0" pad="31"/>
<connect gate="MCU" pin="NRST" pad="4"/>
<connect gate="MCU" pin="PA0" pad="6"/>
<connect gate="MCU" pin="PA1" pad="7"/>
<connect gate="MCU" pin="PA10" pad="20"/>
<connect gate="MCU" pin="PA11" pad="21"/>
<connect gate="MCU" pin="PA12" pad="22"/>
<connect gate="MCU" pin="PA13" pad="23"/>
<connect gate="MCU" pin="PA14" pad="24"/>
<connect gate="MCU" pin="PA15" pad="25"/>
<connect gate="MCU" pin="PA2" pad="8"/>
<connect gate="MCU" pin="PA3" pad="9"/>
<connect gate="MCU" pin="PA4" pad="10"/>
<connect gate="MCU" pin="PA5" pad="11"/>
<connect gate="MCU" pin="PA6" pad="12"/>
<connect gate="MCU" pin="PA7" pad="13"/>
<connect gate="MCU" pin="PA8" pad="18"/>
<connect gate="MCU" pin="PA9" pad="19"/>
<connect gate="MCU" pin="PB0" pad="14"/>
<connect gate="MCU" pin="PB1" pad="15"/>
<connect gate="MCU" pin="PB3" pad="26"/>
<connect gate="MCU" pin="PB4" pad="27"/>
<connect gate="MCU" pin="PB5" pad="28"/>
<connect gate="MCU" pin="PB6" pad="29"/>
<connect gate="MCU" pin="PB7" pad="30"/>
<connect gate="MCU" pin="PC14-OSC_IN" pad="2"/>
<connect gate="MCU" pin="PC15-OSC_OUT" pad="3"/>
<connect gate="MCU" pin="VDDA" pad="5"/>
<connect gate="PWR" pin="VDD@1" pad="17"/>
<connect gate="PWR" pin="VDD@2" pad="1"/>
<connect gate="PWR" pin="VSS@1" pad="16"/>
<connect gate="PWR" pin="VSS@2" pad="32"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L051K*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
27 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_32PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD2_VSS1"/>
</gates>
<devices>
<device name="" package="UFQFPN32">
<connects>
<connect gate="MCU" pin="BOOT0" pad="31"/>
<connect gate="MCU" pin="NRST" pad="4"/>
<connect gate="MCU" pin="PA0" pad="6"/>
<connect gate="MCU" pin="PA1" pad="7"/>
<connect gate="MCU" pin="PA10" pad="20"/>
<connect gate="MCU" pin="PA11" pad="21"/>
<connect gate="MCU" pin="PA12" pad="22"/>
<connect gate="MCU" pin="PA13" pad="23"/>
<connect gate="MCU" pin="PA14" pad="24"/>
<connect gate="MCU" pin="PA15" pad="25"/>
<connect gate="MCU" pin="PA2" pad="8"/>
<connect gate="MCU" pin="PA3" pad="9"/>
<connect gate="MCU" pin="PA4" pad="10"/>
<connect gate="MCU" pin="PA5" pad="11"/>
<connect gate="MCU" pin="PA6" pad="12"/>
<connect gate="MCU" pin="PA7" pad="13"/>
<connect gate="MCU" pin="PA8" pad="18"/>
<connect gate="MCU" pin="PA9" pad="19"/>
<connect gate="MCU" pin="PB0" pad="14"/>
<connect gate="MCU" pin="PB1" pad="15"/>
<connect gate="MCU" pin="PB2" pad="16"/>
<connect gate="MCU" pin="PB3" pad="26"/>
<connect gate="MCU" pin="PB4" pad="27"/>
<connect gate="MCU" pin="PB5" pad="28"/>
<connect gate="MCU" pin="PB6" pad="29"/>
<connect gate="MCU" pin="PB7" pad="30"/>
<connect gate="MCU" pin="PB8" pad="32"/>
<connect gate="MCU" pin="PC14-OSC_IN" pad="2"/>
<connect gate="MCU" pin="PC15-OSC_OUT" pad="3"/>
<connect gate="MCU" pin="VDDA" pad="5"/>
<connect gate="PWR" pin="VDD@1" pad="17"/>
<connect gate="PWR" pin="VDD@2" pad="1"/>
<connect gate="PWR" pin="VSS@1" pad="VSS"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L051C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP9"/>
<gate name="PWR" symbol="PWR_VDD4_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="1"/>
<connect gate="PWR" pin="VDD@2" pad="24"/>
<connect gate="PWR" pin="VDD@3" pad="36"/>
<connect gate="PWR" pin="VDD@4" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="35"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L051R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP14"/>
<gate name="PWR" symbol="PWR_VDD5_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="64"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VDD@3" pad="32"/>
<connect gate="PWR" pin="VDD@4" pad="19"/>
<connect gate="PWR" pin="VDD@5" pad="1"/>
<connect gate="PWR" pin="VSS@1" pad="63"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
<connect gate="PWR" pin="VSS@3" pad="31"/>
<connect gate="PWR" pin="VSS@4" pad="18"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L051R*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP15"/>
<gate name="PWR" symbol="PWR_VDD5_VSS4"/>
</gates>
<devices>
<device name="" package="TFBGA64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="B4"/>
<connect gate="MCU" pin="NRST" pad="E1"/>
<connect gate="MCU" pin="OSC_IN" pad="C1"/>
<connect gate="MCU" pin="OSC_OUT" pad="D1"/>
<connect gate="MCU" pin="PA0-WKUP" pad="G2"/>
<connect gate="MCU" pin="PA1" pad="H2"/>
<connect gate="MCU" pin="PA10" pad="C6"/>
<connect gate="MCU" pin="PA11" pad="C8"/>
<connect gate="MCU" pin="PA12" pad="B8"/>
<connect gate="MCU" pin="PA13" pad="A8"/>
<connect gate="MCU" pin="PA14" pad="A7"/>
<connect gate="MCU" pin="PA15" pad="A6"/>
<connect gate="MCU" pin="PA2" pad="F3"/>
<connect gate="MCU" pin="PA3" pad="G3"/>
<connect gate="MCU" pin="PA4" pad="H3"/>
<connect gate="MCU" pin="PA5" pad="F4"/>
<connect gate="MCU" pin="PA6" pad="G4"/>
<connect gate="MCU" pin="PA7" pad="H4"/>
<connect gate="MCU" pin="PA8" pad="D7"/>
<connect gate="MCU" pin="PA9" pad="C7"/>
<connect gate="MCU" pin="PB0" pad="F5"/>
<connect gate="MCU" pin="PB1" pad="G5"/>
<connect gate="MCU" pin="PB10" pad="G7"/>
<connect gate="MCU" pin="PB11" pad="H7"/>
<connect gate="MCU" pin="PB12" pad="H8"/>
<connect gate="MCU" pin="PB13" pad="G8"/>
<connect gate="MCU" pin="PB14" pad="F8"/>
<connect gate="MCU" pin="PB15" pad="F7"/>
<connect gate="MCU" pin="PB2" pad="G6"/>
<connect gate="MCU" pin="PB3" pad="A5"/>
<connect gate="MCU" pin="PB4" pad="A4"/>
<connect gate="MCU" pin="PB5" pad="C4"/>
<connect gate="MCU" pin="PB6" pad="D3"/>
<connect gate="MCU" pin="PB7" pad="C3"/>
<connect gate="MCU" pin="PB8" pad="B3"/>
<connect gate="MCU" pin="PB9" pad="A3"/>
<connect gate="MCU" pin="PC0" pad="E3"/>
<connect gate="MCU" pin="PC1" pad="E2"/>
<connect gate="MCU" pin="PC10" pad="B7"/>
<connect gate="MCU" pin="PC11" pad="B6"/>
<connect gate="MCU" pin="PC12" pad="C5"/>
<connect gate="MCU" pin="PC13" pad="A2"/>
<connect gate="MCU" pin="PC14" pad="A1"/>
<connect gate="MCU" pin="PC15" pad="B1"/>
<connect gate="MCU" pin="PC2" pad="F2"/>
<connect gate="MCU" pin="PC4" pad="H5"/>
<connect gate="MCU" pin="PC5" pad="H6"/>
<connect gate="MCU" pin="PC6" pad="F6"/>
<connect gate="MCU" pin="PC7" pad="E7"/>
<connect gate="MCU" pin="PC8" pad="E8"/>
<connect gate="MCU" pin="PC9" pad="D8"/>
<connect gate="MCU" pin="PD2" pad="B5"/>
<connect gate="MCU" pin="VDDA" pad="H1"/>
<connect gate="MCU" pin="VREF+" pad="G1"/>
<connect gate="MCU" pin="VSSA" pad="F1"/>
<connect gate="PWR" pin="VDD@1" pad="B2"/>
<connect gate="PWR" pin="VDD@2" pad="D2"/>
<connect gate="PWR" pin="VDD@3" pad="E4"/>
<connect gate="PWR" pin="VDD@4" pad="E5"/>
<connect gate="PWR" pin="VDD@5" pad="E6"/>
<connect gate="PWR" pin="VSS@1" pad="C2"/>
<connect gate="PWR" pin="VSS@2" pad="D4"/>
<connect gate="PWR" pin="VSS@3" pad="D5"/>
<connect gate="PWR" pin="VSS@4" pad="D6"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L052K*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
27 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_32PIN_TYP4"/>
<gate name="PWR" symbol="PWR_VDD2_VSS2"/>
</gates>
<devices>
<device name="" package="LQFP32">
<connects>
<connect gate="MCU" pin="BOOT0" pad="31"/>
<connect gate="MCU" pin="NRST" pad="4"/>
<connect gate="MCU" pin="PA0" pad="6"/>
<connect gate="MCU" pin="PA1" pad="7"/>
<connect gate="MCU" pin="PA10" pad="20"/>
<connect gate="MCU" pin="PA11" pad="21"/>
<connect gate="MCU" pin="PA12" pad="22"/>
<connect gate="MCU" pin="PA13" pad="23"/>
<connect gate="MCU" pin="PA14" pad="24"/>
<connect gate="MCU" pin="PA15" pad="25"/>
<connect gate="MCU" pin="PA2" pad="8"/>
<connect gate="MCU" pin="PA3" pad="9"/>
<connect gate="MCU" pin="PA4" pad="10"/>
<connect gate="MCU" pin="PA5" pad="11"/>
<connect gate="MCU" pin="PA6" pad="12"/>
<connect gate="MCU" pin="PA7" pad="13"/>
<connect gate="MCU" pin="PA8" pad="18"/>
<connect gate="MCU" pin="PA9" pad="19"/>
<connect gate="MCU" pin="PB0" pad="14"/>
<connect gate="MCU" pin="PB1" pad="15"/>
<connect gate="MCU" pin="PB3" pad="26"/>
<connect gate="MCU" pin="PB4" pad="27"/>
<connect gate="MCU" pin="PB5" pad="28"/>
<connect gate="MCU" pin="PB6" pad="29"/>
<connect gate="MCU" pin="PB7" pad="30"/>
<connect gate="MCU" pin="PC14-OSC_IN" pad="2"/>
<connect gate="MCU" pin="PC15-OSC_OUT" pad="3"/>
<connect gate="MCU" pin="VDDA" pad="5"/>
<connect gate="PWR" pin="VDD@1" pad="17"/>
<connect gate="PWR" pin="VDD@2" pad="1"/>
<connect gate="PWR" pin="VSS@1" pad="16"/>
<connect gate="PWR" pin="VSS@2" pad="32"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L052K*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
27 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_32PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD2_VSS1"/>
</gates>
<devices>
<device name="" package="UFQFPN32">
<connects>
<connect gate="MCU" pin="BOOT0" pad="31"/>
<connect gate="MCU" pin="NRST" pad="4"/>
<connect gate="MCU" pin="PA0" pad="6"/>
<connect gate="MCU" pin="PA1" pad="7"/>
<connect gate="MCU" pin="PA10" pad="20"/>
<connect gate="MCU" pin="PA11" pad="21"/>
<connect gate="MCU" pin="PA12" pad="22"/>
<connect gate="MCU" pin="PA13" pad="23"/>
<connect gate="MCU" pin="PA14" pad="24"/>
<connect gate="MCU" pin="PA15" pad="25"/>
<connect gate="MCU" pin="PA2" pad="8"/>
<connect gate="MCU" pin="PA3" pad="9"/>
<connect gate="MCU" pin="PA4" pad="10"/>
<connect gate="MCU" pin="PA5" pad="11"/>
<connect gate="MCU" pin="PA6" pad="12"/>
<connect gate="MCU" pin="PA7" pad="13"/>
<connect gate="MCU" pin="PA8" pad="18"/>
<connect gate="MCU" pin="PA9" pad="19"/>
<connect gate="MCU" pin="PB0" pad="14"/>
<connect gate="MCU" pin="PB1" pad="15"/>
<connect gate="MCU" pin="PB2" pad="16"/>
<connect gate="MCU" pin="PB3" pad="26"/>
<connect gate="MCU" pin="PB4" pad="27"/>
<connect gate="MCU" pin="PB5" pad="28"/>
<connect gate="MCU" pin="PB6" pad="29"/>
<connect gate="MCU" pin="PB7" pad="30"/>
<connect gate="MCU" pin="PB8" pad="32"/>
<connect gate="MCU" pin="PC14-OSC_IN" pad="2"/>
<connect gate="MCU" pin="PC15-OSC_OUT" pad="3"/>
<connect gate="MCU" pin="VDDA" pad="5"/>
<connect gate="PWR" pin="VDD@1" pad="17"/>
<connect gate="PWR" pin="VDD@2" pad="1"/>
<connect gate="PWR" pin="VSS@1" pad="VSS"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L052C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP10"/>
<gate name="PWR" symbol="PWR_VDD3_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VDD_USB" pad="36"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="1"/>
<connect gate="PWR" pin="VDD@2" pad="24"/>
<connect gate="PWR" pin="VDD@3" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="35"/>
<connect gate="PWR" pin="VSS@2" pad="23"/>
<connect gate="PWR" pin="VSS@3" pad="47"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L052R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP16"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VDD_USB" pad="48"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="1"/>
<connect gate="PWR" pin="VDD@2" pad="19"/>
<connect gate="PWR" pin="VDD@3" pad="32"/>
<connect gate="PWR" pin="VDD@4" pad="64"/>
<connect gate="PWR" pin="VSS@1" pad="47"/>
<connect gate="PWR" pin="VSS@2" pad="18"/>
<connect gate="PWR" pin="VSS@3" pad="31"/>
<connect gate="PWR" pin="VSS@4" pad="63"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L052R*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP17"/>
<gate name="PWR" symbol="PWR_VDD4_VSS4"/>
</gates>
<devices>
<device name="" package="TFBGA64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="B4"/>
<connect gate="MCU" pin="NRST" pad="E1"/>
<connect gate="MCU" pin="OSC_IN" pad="C1"/>
<connect gate="MCU" pin="OSC_OUT" pad="D1"/>
<connect gate="MCU" pin="PA0-WKUP" pad="G2"/>
<connect gate="MCU" pin="PA1" pad="H2"/>
<connect gate="MCU" pin="PA10" pad="C6"/>
<connect gate="MCU" pin="PA11" pad="C8"/>
<connect gate="MCU" pin="PA12" pad="B8"/>
<connect gate="MCU" pin="PA13" pad="A8"/>
<connect gate="MCU" pin="PA14" pad="A7"/>
<connect gate="MCU" pin="PA15" pad="A6"/>
<connect gate="MCU" pin="PA2" pad="F3"/>
<connect gate="MCU" pin="PA3" pad="G3"/>
<connect gate="MCU" pin="PA4" pad="H3"/>
<connect gate="MCU" pin="PA5" pad="F4"/>
<connect gate="MCU" pin="PA6" pad="G4"/>
<connect gate="MCU" pin="PA7" pad="H4"/>
<connect gate="MCU" pin="PA8" pad="D7"/>
<connect gate="MCU" pin="PA9" pad="C7"/>
<connect gate="MCU" pin="PB0" pad="F5"/>
<connect gate="MCU" pin="PB1" pad="G5"/>
<connect gate="MCU" pin="PB10" pad="G7"/>
<connect gate="MCU" pin="PB11" pad="H7"/>
<connect gate="MCU" pin="PB12" pad="H8"/>
<connect gate="MCU" pin="PB13" pad="G8"/>
<connect gate="MCU" pin="PB14" pad="F8"/>
<connect gate="MCU" pin="PB15" pad="F7"/>
<connect gate="MCU" pin="PB2" pad="G6"/>
<connect gate="MCU" pin="PB3" pad="A5"/>
<connect gate="MCU" pin="PB4" pad="A4"/>
<connect gate="MCU" pin="PB5" pad="C4"/>
<connect gate="MCU" pin="PB6" pad="D3"/>
<connect gate="MCU" pin="PB7" pad="C3"/>
<connect gate="MCU" pin="PB8" pad="B3"/>
<connect gate="MCU" pin="PB9" pad="A3"/>
<connect gate="MCU" pin="PC0" pad="E3"/>
<connect gate="MCU" pin="PC1" pad="E2"/>
<connect gate="MCU" pin="PC10" pad="B7"/>
<connect gate="MCU" pin="PC11" pad="B6"/>
<connect gate="MCU" pin="PC12" pad="C5"/>
<connect gate="MCU" pin="PC13" pad="A2"/>
<connect gate="MCU" pin="PC14" pad="A1"/>
<connect gate="MCU" pin="PC15" pad="B1"/>
<connect gate="MCU" pin="PC2" pad="F2"/>
<connect gate="MCU" pin="PC4" pad="H5"/>
<connect gate="MCU" pin="PC5" pad="H6"/>
<connect gate="MCU" pin="PC6" pad="F6"/>
<connect gate="MCU" pin="PC7" pad="E7"/>
<connect gate="MCU" pin="PC8" pad="E8"/>
<connect gate="MCU" pin="PC9" pad="D8"/>
<connect gate="MCU" pin="PD2" pad="B5"/>
<connect gate="MCU" pin="VDDA" pad="H1"/>
<connect gate="MCU" pin="VDD_USB" pad="E6"/>
<connect gate="MCU" pin="VREF+" pad="G1"/>
<connect gate="MCU" pin="VSSA" pad="F1"/>
<connect gate="PWR" pin="VDD@1" pad="B2"/>
<connect gate="PWR" pin="VDD@2" pad="D2"/>
<connect gate="PWR" pin="VDD@3" pad="E4"/>
<connect gate="PWR" pin="VDD@4" pad="E5"/>
<connect gate="PWR" pin="VSS@1" pad="C2"/>
<connect gate="PWR" pin="VSS@2" pad="D4"/>
<connect gate="PWR" pin="VSS@3" pad="D5"/>
<connect gate="PWR" pin="VSS@4" pad="D6"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L053C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP11"/>
<gate name="PWR" symbol="PWR_VDD2_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VDD_USB" pad="36"/>
<connect gate="MCU" pin="VLCD" pad="1"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="24"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
<connect gate="PWR" pin="VSS@3" pad="35"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L053R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP18"/>
<gate name="PWR" symbol="PWR_VDD3_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VDD_USB" pad="48"/>
<connect gate="MCU" pin="VLCD" pad="1"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="19"/>
<connect gate="PWR" pin="VDD@2" pad="32"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VSS@1" pad="18"/>
<connect gate="PWR" pin="VSS@2" pad="31"/>
<connect gate="PWR" pin="VSS@3" pad="63"/>
<connect gate="PWR" pin="VSS@4" pad="47"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L053R*H" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
32 to 64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP19"/>
<gate name="PWR" symbol="PWR_VDD3_VSS4"/>
</gates>
<devices>
<device name="" package="TFBGA64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="B4"/>
<connect gate="MCU" pin="NRST" pad="E1"/>
<connect gate="MCU" pin="OSC_IN" pad="C1"/>
<connect gate="MCU" pin="OSC_OUT" pad="D1"/>
<connect gate="MCU" pin="PA0-WKUP" pad="G2"/>
<connect gate="MCU" pin="PA1" pad="H2"/>
<connect gate="MCU" pin="PA10" pad="C6"/>
<connect gate="MCU" pin="PA11" pad="C8"/>
<connect gate="MCU" pin="PA12" pad="B8"/>
<connect gate="MCU" pin="PA13" pad="A8"/>
<connect gate="MCU" pin="PA14" pad="A7"/>
<connect gate="MCU" pin="PA15" pad="A6"/>
<connect gate="MCU" pin="PA2" pad="F3"/>
<connect gate="MCU" pin="PA3" pad="G3"/>
<connect gate="MCU" pin="PA4" pad="H3"/>
<connect gate="MCU" pin="PA5" pad="F4"/>
<connect gate="MCU" pin="PA6" pad="G4"/>
<connect gate="MCU" pin="PA7" pad="H4"/>
<connect gate="MCU" pin="PA8" pad="D7"/>
<connect gate="MCU" pin="PA9" pad="C7"/>
<connect gate="MCU" pin="PB0" pad="F5"/>
<connect gate="MCU" pin="PB1" pad="G5"/>
<connect gate="MCU" pin="PB10" pad="G7"/>
<connect gate="MCU" pin="PB11" pad="H7"/>
<connect gate="MCU" pin="PB12" pad="H8"/>
<connect gate="MCU" pin="PB13" pad="G8"/>
<connect gate="MCU" pin="PB14" pad="F8"/>
<connect gate="MCU" pin="PB15" pad="F7"/>
<connect gate="MCU" pin="PB2" pad="G6"/>
<connect gate="MCU" pin="PB3" pad="A5"/>
<connect gate="MCU" pin="PB4" pad="A4"/>
<connect gate="MCU" pin="PB5" pad="C4"/>
<connect gate="MCU" pin="PB6" pad="D3"/>
<connect gate="MCU" pin="PB7" pad="C3"/>
<connect gate="MCU" pin="PB8" pad="B3"/>
<connect gate="MCU" pin="PB9" pad="A3"/>
<connect gate="MCU" pin="PC0" pad="E3"/>
<connect gate="MCU" pin="PC1" pad="E2"/>
<connect gate="MCU" pin="PC10" pad="B7"/>
<connect gate="MCU" pin="PC11" pad="B6"/>
<connect gate="MCU" pin="PC12" pad="C5"/>
<connect gate="MCU" pin="PC13" pad="A2"/>
<connect gate="MCU" pin="PC14" pad="A1"/>
<connect gate="MCU" pin="PC15" pad="B1"/>
<connect gate="MCU" pin="PC2" pad="F2"/>
<connect gate="MCU" pin="PC4" pad="H5"/>
<connect gate="MCU" pin="PC5" pad="H6"/>
<connect gate="MCU" pin="PC6" pad="F6"/>
<connect gate="MCU" pin="PC7" pad="E7"/>
<connect gate="MCU" pin="PC8" pad="E8"/>
<connect gate="MCU" pin="PC9" pad="D8"/>
<connect gate="MCU" pin="PD2" pad="B5"/>
<connect gate="MCU" pin="VDDA" pad="H1"/>
<connect gate="MCU" pin="VDD_USB" pad="E6"/>
<connect gate="MCU" pin="VLCD" pad="B2"/>
<connect gate="MCU" pin="VREF+" pad="G1"/>
<connect gate="MCU" pin="VSSA" pad="F1"/>
<connect gate="PWR" pin="VDD@1" pad="D2"/>
<connect gate="PWR" pin="VDD@2" pad="E4"/>
<connect gate="PWR" pin="VDD@3" pad="E5"/>
<connect gate="PWR" pin="VSS@1" pad="C2"/>
<connect gate="PWR" pin="VSS@2" pad="D4"/>
<connect gate="PWR" pin="VSS@3" pad="D5"/>
<connect gate="PWR" pin="VSS@4" pad="D6"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L062K*U" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
27 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_32PIN_TYP3"/>
<gate name="PWR" symbol="PWR_VDD2_VSS1"/>
</gates>
<devices>
<device name="" package="UFQFPN32">
<connects>
<connect gate="MCU" pin="BOOT0" pad="31"/>
<connect gate="MCU" pin="NRST" pad="4"/>
<connect gate="MCU" pin="PA0" pad="6"/>
<connect gate="MCU" pin="PA1" pad="7"/>
<connect gate="MCU" pin="PA10" pad="20"/>
<connect gate="MCU" pin="PA11" pad="21"/>
<connect gate="MCU" pin="PA12" pad="22"/>
<connect gate="MCU" pin="PA13" pad="23"/>
<connect gate="MCU" pin="PA14" pad="24"/>
<connect gate="MCU" pin="PA15" pad="25"/>
<connect gate="MCU" pin="PA2" pad="8"/>
<connect gate="MCU" pin="PA3" pad="9"/>
<connect gate="MCU" pin="PA4" pad="10"/>
<connect gate="MCU" pin="PA5" pad="11"/>
<connect gate="MCU" pin="PA6" pad="12"/>
<connect gate="MCU" pin="PA7" pad="13"/>
<connect gate="MCU" pin="PA8" pad="18"/>
<connect gate="MCU" pin="PA9" pad="19"/>
<connect gate="MCU" pin="PB0" pad="14"/>
<connect gate="MCU" pin="PB1" pad="15"/>
<connect gate="MCU" pin="PB2" pad="16"/>
<connect gate="MCU" pin="PB3" pad="26"/>
<connect gate="MCU" pin="PB4" pad="27"/>
<connect gate="MCU" pin="PB5" pad="28"/>
<connect gate="MCU" pin="PB6" pad="29"/>
<connect gate="MCU" pin="PB7" pad="30"/>
<connect gate="MCU" pin="PB8" pad="32"/>
<connect gate="MCU" pin="PC14-OSC_IN" pad="2"/>
<connect gate="MCU" pin="PC15-OSC_OUT" pad="3"/>
<connect gate="MCU" pin="VDDA" pad="5"/>
<connect gate="PWR" pin="VDD@1" pad="1"/>
<connect gate="PWR" pin="VDD@2" pad="17"/>
<connect gate="PWR" pin="VSS@1" pad="VSS"/>
</connects>
<technologies>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L063C*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
37 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_48PIN_TYP11"/>
<gate name="PWR" symbol="PWR_VDD2_VSS3"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="MCU" pin="BOOT0" pad="44"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0" pad="10"/>
<connect gate="MCU" pin="PA1" pad="11"/>
<connect gate="MCU" pin="PA10" pad="31"/>
<connect gate="MCU" pin="PA11" pad="32"/>
<connect gate="MCU" pin="PA12" pad="33"/>
<connect gate="MCU" pin="PA13" pad="34"/>
<connect gate="MCU" pin="PA14" pad="37"/>
<connect gate="MCU" pin="PA15" pad="38"/>
<connect gate="MCU" pin="PA2" pad="12"/>
<connect gate="MCU" pin="PA3" pad="13"/>
<connect gate="MCU" pin="PA4" pad="14"/>
<connect gate="MCU" pin="PA5" pad="15"/>
<connect gate="MCU" pin="PA6" pad="16"/>
<connect gate="MCU" pin="PA7" pad="17"/>
<connect gate="MCU" pin="PA8" pad="29"/>
<connect gate="MCU" pin="PA9" pad="30"/>
<connect gate="MCU" pin="PB0" pad="18"/>
<connect gate="MCU" pin="PB1" pad="19"/>
<connect gate="MCU" pin="PB10" pad="21"/>
<connect gate="MCU" pin="PB11" pad="22"/>
<connect gate="MCU" pin="PB12" pad="25"/>
<connect gate="MCU" pin="PB13" pad="26"/>
<connect gate="MCU" pin="PB14" pad="27"/>
<connect gate="MCU" pin="PB15" pad="28"/>
<connect gate="MCU" pin="PB2" pad="20"/>
<connect gate="MCU" pin="PB3" pad="39"/>
<connect gate="MCU" pin="PB4" pad="40"/>
<connect gate="MCU" pin="PB5" pad="41"/>
<connect gate="MCU" pin="PB6" pad="42"/>
<connect gate="MCU" pin="PB7" pad="43"/>
<connect gate="MCU" pin="PB8" pad="45"/>
<connect gate="MCU" pin="PB9" pad="46"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="VDDA" pad="9"/>
<connect gate="MCU" pin="VDD_USB" pad="36"/>
<connect gate="MCU" pin="VLCD" pad="1"/>
<connect gate="MCU" pin="VSSA" pad="8"/>
<connect gate="PWR" pin="VDD@1" pad="24"/>
<connect gate="PWR" pin="VDD@2" pad="48"/>
<connect gate="PWR" pin="VSS@1" pad="23"/>
<connect gate="PWR" pin="VSS@2" pad="47"/>
<connect gate="PWR" pin="VSS@3" pad="35"/>
</connects>
<technologies>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L063R*T" prefix="IC">
<description>&lt;b&gt;ARM 32-bit Cortex™-M0+ CPU&lt;/b&gt;&lt;p&gt;
32 MHz maximum frequency&lt;br&gt;
64 Kbytes of Flash memory&lt;br&gt;
2 kbyte of Data EEPROM&lt;br&gt;
8 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.8 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP18"/>
<gate name="PWR" symbol="PWR_VDD3_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VDD_USB" pad="48"/>
<connect gate="MCU" pin="VLCD" pad="1"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="19"/>
<connect gate="PWR" pin="VDD@2" pad="32"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VSS@1" pad="18"/>
<connect gate="PWR" pin="VSS@2" pad="31"/>
<connect gate="PWR" pin="VSS@3" pad="63"/>
<connect gate="PWR" pin="VSS@4" pad="47"/>
</connects>
<technologies>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L476Z*T">
<description>&lt;b&gt;ARM 32-bit Cortex™-M4 CPU&lt;/b&gt;&lt;p&gt;
80 MHz maximum frequency&lt;br&gt;
512..1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
115 GPIOs&lt;br&gt;
1.71 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP6"/>
<gate name="PWR" symbol="PWR_VDD9_VSS11"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VDDIO2_1" pad="95"/>
<connect gate="MCU" pin="VDDIO2_2" pad="131"/>
<connect gate="MCU" pin="VDD_USB" pad="106"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VREF-" pad="31"/>
<connect gate="MCU" pin="VSSA" pad="30"/>
<connect gate="PWR" pin="VDD@1" pad="17"/>
<connect gate="PWR" pin="VDD@2" pad="39"/>
<connect gate="PWR" pin="VDD@3" pad="52"/>
<connect gate="PWR" pin="VDD@4" pad="62"/>
<connect gate="PWR" pin="VDD@5" pad="72"/>
<connect gate="PWR" pin="VDD@6" pad="84"/>
<connect gate="PWR" pin="VDD@7" pad="108"/>
<connect gate="PWR" pin="VDD@8" pad="121"/>
<connect gate="PWR" pin="VDD@9" pad="144"/>
<connect gate="PWR" pin="VSS@1" pad="16"/>
<connect gate="PWR" pin="VSS@10" pad="130"/>
<connect gate="PWR" pin="VSS@11" pad="94"/>
<connect gate="PWR" pin="VSS@2" pad="38"/>
<connect gate="PWR" pin="VSS@3" pad="51"/>
<connect gate="PWR" pin="VSS@4" pad="61"/>
<connect gate="PWR" pin="VSS@5" pad="71"/>
<connect gate="PWR" pin="VSS@6" pad="83"/>
<connect gate="PWR" pin="VSS@7" pad="107"/>
<connect gate="PWR" pin="VSS@8" pad="120"/>
<connect gate="PWR" pin="VSS@9" pad="143"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L476V*T">
<description>&lt;b&gt;ARM 32-bit Cortex™-M4 CPU&lt;/b&gt;&lt;p&gt;
80 MHz maximum frequency&lt;br&gt;
256..1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
1.71 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP11"/>
<gate name="PWR" symbol="PWR_VDD5_VSS5"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VDD_USB" pad="73"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VREF-" pad="20"/>
<connect gate="MCU" pin="VSSA" pad="19"/>
<connect gate="PWR" pin="VDD@1" pad="11"/>
<connect gate="PWR" pin="VDD@2" pad="28"/>
<connect gate="PWR" pin="VDD@3" pad="50"/>
<connect gate="PWR" pin="VDD@4" pad="75"/>
<connect gate="PWR" pin="VDD@5" pad="100"/>
<connect gate="PWR" pin="VSS@1" pad="10"/>
<connect gate="PWR" pin="VSS@2" pad="27"/>
<connect gate="PWR" pin="VSS@3" pad="49"/>
<connect gate="PWR" pin="VSS@4" pad="74"/>
<connect gate="PWR" pin="VSS@5" pad="99"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L476J*Y">
<description>&lt;b&gt;ARM 32-bit Cortex™-M4 CPU&lt;/b&gt;&lt;p&gt;
80 MHz maximum frequency&lt;br&gt;
512..1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
57 GPIOs&lt;br&gt;
1.71 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_72PIN_TYP1"/>
<gate name="PWR" symbol="PWR_VDD3_VSS4"/>
</gates>
<devices>
<device name="" package="WLCSP72">
<connects>
<connect gate="MCU" pin="BOOT0" pad="D7"/>
<connect gate="MCU" pin="NRST" pad="E9"/>
<connect gate="MCU" pin="OSC_IN" pad="D9"/>
<connect gate="MCU" pin="OSC_OUT" pad="D8"/>
<connect gate="MCU" pin="PA0-WKUP" pad="H8"/>
<connect gate="MCU" pin="PA1" pad="G4"/>
<connect gate="MCU" pin="PA10" pad="D2"/>
<connect gate="MCU" pin="PA11" pad="D1"/>
<connect gate="MCU" pin="PA12" pad="C1"/>
<connect gate="MCU" pin="PA13" pad="C2"/>
<connect gate="MCU" pin="PA14" pad="B2"/>
<connect gate="MCU" pin="PA15" pad="A2"/>
<connect gate="MCU" pin="PA2" pad="G6"/>
<connect gate="MCU" pin="PA3" pad="H7"/>
<connect gate="MCU" pin="PA4" pad="G5"/>
<connect gate="MCU" pin="PA5" pad="H6"/>
<connect gate="MCU" pin="PA6" pad="H5"/>
<connect gate="MCU" pin="PA7" pad="H4"/>
<connect gate="MCU" pin="PA8" pad="E2"/>
<connect gate="MCU" pin="PA9" pad="E3"/>
<connect gate="MCU" pin="PB0" pad="J5"/>
<connect gate="MCU" pin="PB1" pad="J4"/>
<connect gate="MCU" pin="PB10" pad="H3"/>
<connect gate="MCU" pin="PB11" pad="G3"/>
<connect gate="MCU" pin="PB12" pad="H1"/>
<connect gate="MCU" pin="PB13" pad="H2"/>
<connect gate="MCU" pin="PB14" pad="G2"/>
<connect gate="MCU" pin="PB15" pad="G1"/>
<connect gate="MCU" pin="PB2" pad="J3"/>
<connect gate="MCU" pin="PB3" pad="A6"/>
<connect gate="MCU" pin="PB4" pad="C6"/>
<connect gate="MCU" pin="PB5" pad="C7"/>
<connect gate="MCU" pin="PB6" pad="B7"/>
<connect gate="MCU" pin="PB7" pad="A7"/>
<connect gate="MCU" pin="PB8" pad="E7"/>
<connect gate="MCU" pin="PB9" pad="E8"/>
<connect gate="MCU" pin="PC0" pad="F9"/>
<connect gate="MCU" pin="PC1" pad="F8"/>
<connect gate="MCU" pin="PC10" pad="D3"/>
<connect gate="MCU" pin="PC11" pad="C3"/>
<connect gate="MCU" pin="PC12" pad="B3"/>
<connect gate="MCU" pin="PC13" pad="B8"/>
<connect gate="MCU" pin="PC14" pad="C9"/>
<connect gate="MCU" pin="PC15" pad="C8"/>
<connect gate="MCU" pin="PC2" pad="F7"/>
<connect gate="MCU" pin="PC3" pad="G7"/>
<connect gate="MCU" pin="PC4" pad="J7"/>
<connect gate="MCU" pin="PC5" pad="J6"/>
<connect gate="MCU" pin="PC6" pad="F3"/>
<connect gate="MCU" pin="PC7" pad="F1"/>
<connect gate="MCU" pin="PC8" pad="F2"/>
<connect gate="MCU" pin="PC9" pad="E1"/>
<connect gate="MCU" pin="PD2" pad="A3"/>
<connect gate="MCU" pin="PG10" pad="B4"/>
<connect gate="MCU" pin="PG11" pad="C4"/>
<connect gate="MCU" pin="PG12" pad="C5"/>
<connect gate="MCU" pin="PG13" pad="B5"/>
<connect gate="MCU" pin="PG14" pad="A5"/>
<connect gate="MCU" pin="PG9" pad="A4"/>
<connect gate="MCU" pin="VBAT" pad="B9"/>
<connect gate="MCU" pin="VDDA" pad="H9"/>
<connect gate="MCU" pin="VDDIO2" pad="B6"/>
<connect gate="MCU" pin="VDD_USB" pad="A1"/>
<connect gate="MCU" pin="VREF+" pad="G8"/>
<connect gate="MCU" pin="VSSA" pad="G9"/>
<connect gate="PWR" pin="VDD@1" pad="A9"/>
<connect gate="PWR" pin="VDD@2" pad="J1"/>
<connect gate="PWR" pin="VDD@3" pad="J8"/>
<connect gate="PWR" pin="VSS@1" pad="A8"/>
<connect gate="PWR" pin="VSS@2" pad="B1"/>
<connect gate="PWR" pin="VSS@3" pad="J2"/>
<connect gate="PWR" pin="VSS@4" pad="J9"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L476Q*I">
<description>&lt;b&gt;ARM 32-bit Cortex™-M4 CPU&lt;/b&gt;&lt;p&gt;
80 MHz maximum frequency&lt;br&gt;
512..1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
109 GPIOs&lt;br&gt;
1.71 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_132PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD6_VSS7"/>
</gates>
<devices>
<device name="" package="UFBGA132">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A4"/>
<connect gate="MCU" pin="NRST" pad="H2"/>
<connect gate="MCU" pin="OPAMP1" pad="M3"/>
<connect gate="MCU" pin="OPAMP2" pad="M4"/>
<connect gate="MCU" pin="OSC_IN" pad="F1"/>
<connect gate="MCU" pin="OSC_OUT" pad="G1"/>
<connect gate="MCU" pin="PA0" pad="L2"/>
<connect gate="MCU" pin="PA1" pad="M2"/>
<connect gate="MCU" pin="PA10" pad="C12"/>
<connect gate="MCU" pin="PA11" pad="B12"/>
<connect gate="MCU" pin="PA12" pad="A12"/>
<connect gate="MCU" pin="PA13" pad="A11"/>
<connect gate="MCU" pin="PA14" pad="A10"/>
<connect gate="MCU" pin="PA15" pad="A9"/>
<connect gate="MCU" pin="PA2" pad="K3"/>
<connect gate="MCU" pin="PA3" pad="L3"/>
<connect gate="MCU" pin="PA4" pad="J4"/>
<connect gate="MCU" pin="PA5" pad="K4"/>
<connect gate="MCU" pin="PA6" pad="L4"/>
<connect gate="MCU" pin="PA7" pad="J5"/>
<connect gate="MCU" pin="PA8" pad="D11"/>
<connect gate="MCU" pin="PA9" pad="D10"/>
<connect gate="MCU" pin="PB0" pad="M5"/>
<connect gate="MCU" pin="PB1" pad="M6"/>
<connect gate="MCU" pin="PB10" pad="L10"/>
<connect gate="MCU" pin="PB11" pad="L11"/>
<connect gate="MCU" pin="PB12" pad="L12"/>
<connect gate="MCU" pin="PB13" pad="K12"/>
<connect gate="MCU" pin="PB14" pad="K11"/>
<connect gate="MCU" pin="PB15" pad="K10"/>
<connect gate="MCU" pin="PB2" pad="L6"/>
<connect gate="MCU" pin="PB3" pad="A8"/>
<connect gate="MCU" pin="PB4" pad="A7"/>
<connect gate="MCU" pin="PB5" pad="C5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="B4"/>
<connect gate="MCU" pin="PB8" pad="A3"/>
<connect gate="MCU" pin="PB9" pad="B3"/>
<connect gate="MCU" pin="PC0" pad="H1"/>
<connect gate="MCU" pin="PC1" pad="J2"/>
<connect gate="MCU" pin="PC10" pad="B11"/>
<connect gate="MCU" pin="PC11" pad="C10"/>
<connect gate="MCU" pin="PC12" pad="B10"/>
<connect gate="MCU" pin="PC13" pad="C1"/>
<connect gate="MCU" pin="PC14" pad="D1"/>
<connect gate="MCU" pin="PC15" pad="E1"/>
<connect gate="MCU" pin="PC2" pad="J3"/>
<connect gate="MCU" pin="PC3" pad="K2"/>
<connect gate="MCU" pin="PC4" pad="K5"/>
<connect gate="MCU" pin="PC5" pad="L5"/>
<connect gate="MCU" pin="PC6" pad="E12"/>
<connect gate="MCU" pin="PC7" pad="E11"/>
<connect gate="MCU" pin="PC8" pad="E10"/>
<connect gate="MCU" pin="PC9" pad="D12"/>
<connect gate="MCU" pin="PD0" pad="C9"/>
<connect gate="MCU" pin="PD1" pad="B9"/>
<connect gate="MCU" pin="PD10" pad="J12"/>
<connect gate="MCU" pin="PD11" pad="J11"/>
<connect gate="MCU" pin="PD12" pad="J10"/>
<connect gate="MCU" pin="PD13" pad="H12"/>
<connect gate="MCU" pin="PD14" pad="H11"/>
<connect gate="MCU" pin="PD15" pad="H10"/>
<connect gate="MCU" pin="PD2" pad="C8"/>
<connect gate="MCU" pin="PD3" pad="B8"/>
<connect gate="MCU" pin="PD4" pad="B7"/>
<connect gate="MCU" pin="PD5" pad="A6"/>
<connect gate="MCU" pin="PD6" pad="B6"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD8" pad="K9"/>
<connect gate="MCU" pin="PD9" pad="K8"/>
<connect gate="MCU" pin="PE0" pad="C3"/>
<connect gate="MCU" pin="PE1" pad="A2"/>
<connect gate="MCU" pin="PE10" pad="L8"/>
<connect gate="MCU" pin="PE11" pad="M9"/>
<connect gate="MCU" pin="PE12" pad="L9"/>
<connect gate="MCU" pin="PE13" pad="M10"/>
<connect gate="MCU" pin="PE14" pad="M11"/>
<connect gate="MCU" pin="PE15" pad="M12"/>
<connect gate="MCU" pin="PE2" pad="B2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="C2"/>
<connect gate="MCU" pin="PE6" pad="D2"/>
<connect gate="MCU" pin="PE7" pad="M7"/>
<connect gate="MCU" pin="PE8" pad="L7"/>
<connect gate="MCU" pin="PE9" pad="M8"/>
<connect gate="MCU" pin="PF0" pad="D6"/>
<connect gate="MCU" pin="PF1" pad="D5"/>
<connect gate="MCU" pin="PF11" pad="K6"/>
<connect gate="MCU" pin="PF12" pad="J7"/>
<connect gate="MCU" pin="PF13" pad="K7"/>
<connect gate="MCU" pin="PF14" pad="J8"/>
<connect gate="MCU" pin="PF15" pad="J9"/>
<connect gate="MCU" pin="PF2" pad="D4"/>
<connect gate="MCU" pin="PF3" pad="E4"/>
<connect gate="MCU" pin="PF4" pad="F3"/>
<connect gate="MCU" pin="PF5" pad="F4"/>
<connect gate="MCU" pin="PG0" pad="H9"/>
<connect gate="MCU" pin="PG1" pad="G9"/>
<connect gate="MCU" pin="PG10" pad="D8"/>
<connect gate="MCU" pin="PG11" pad="G3"/>
<connect gate="MCU" pin="PG12" pad="D7"/>
<connect gate="MCU" pin="PG13" pad="C7"/>
<connect gate="MCU" pin="PG14" pad="C6"/>
<connect gate="MCU" pin="PG15" pad="K1"/>
<connect gate="MCU" pin="PG2" pad="G10"/>
<connect gate="MCU" pin="PG3" pad="F9"/>
<connect gate="MCU" pin="PG4" pad="F10"/>
<connect gate="MCU" pin="PG5" pad="E9"/>
<connect gate="MCU" pin="PG6" pad="G4"/>
<connect gate="MCU" pin="PG7" pad="H4"/>
<connect gate="MCU" pin="PG8" pad="J6"/>
<connect gate="MCU" pin="PG9" pad="D9"/>
<connect gate="MCU" pin="VBAT" pad="E2"/>
<connect gate="MCU" pin="VDDA" pad="M1"/>
<connect gate="MCU" pin="VDDIO2_1" pad="G7"/>
<connect gate="MCU" pin="VDD_USB" pad="C11"/>
<connect gate="MCU" pin="VREF+" pad="L1"/>
<connect gate="MCU" pin="VSSA" pad="J1"/>
<connect gate="PWR" pin="VDD@1" pad="C4"/>
<connect gate="PWR" pin="VDD@2" pad="G2"/>
<connect gate="PWR" pin="VDD@3" pad="G6"/>
<connect gate="PWR" pin="VDD@4" pad="G11"/>
<connect gate="PWR" pin="VDD@5" pad="G12"/>
<connect gate="PWR" pin="VDD@6" pad="H3"/>
<connect gate="PWR" pin="VSS@1" pad="D3"/>
<connect gate="PWR" pin="VSS@2" pad="E3"/>
<connect gate="PWR" pin="VSS@3" pad="F2"/>
<connect gate="PWR" pin="VSS@4" pad="F6"/>
<connect gate="PWR" pin="VSS@5" pad="F7"/>
<connect gate="PWR" pin="VSS@6" pad="F11"/>
<connect gate="PWR" pin="VSS@7" pad="F12"/>
</connects>
<technologies>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L476R*T">
<description>&lt;b&gt;ARM 32-bit Cortex™-M4 CPU&lt;/b&gt;&lt;p&gt;
80 MHz maximum frequency&lt;br&gt;
256..1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.71 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP20"/>
<gate name="PWR" symbol="PWR_VDD3_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VDD_USB" pad="48"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="19"/>
<connect gate="PWR" pin="VDD@2" pad="32"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VSS@1" pad="18"/>
<connect gate="PWR" pin="VSS@2" pad="31"/>
<connect gate="PWR" pin="VSS@3" pad="63"/>
<connect gate="PWR" pin="VSS@4" pad="47"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L486Z*T">
<description>&lt;b&gt;ARM 32-bit Cortex™-M4 CPU&lt;/b&gt;&lt;p&gt;
80 MHz maximum frequency&lt;br&gt;
1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
115 GPIOs&lt;br&gt;
1.71 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_144PIN_TYP6"/>
<gate name="PWR" symbol="PWR_VDD9_VSS11"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="MCU" pin="BOOT0" pad="138"/>
<connect gate="MCU" pin="NRST" pad="25"/>
<connect gate="MCU" pin="OSC_IN" pad="23"/>
<connect gate="MCU" pin="OSC_OUT" pad="24"/>
<connect gate="MCU" pin="PA0" pad="34"/>
<connect gate="MCU" pin="PA1" pad="35"/>
<connect gate="MCU" pin="PA10" pad="102"/>
<connect gate="MCU" pin="PA11" pad="103"/>
<connect gate="MCU" pin="PA12" pad="104"/>
<connect gate="MCU" pin="PA13" pad="105"/>
<connect gate="MCU" pin="PA14" pad="109"/>
<connect gate="MCU" pin="PA15" pad="110"/>
<connect gate="MCU" pin="PA2" pad="36"/>
<connect gate="MCU" pin="PA3" pad="37"/>
<connect gate="MCU" pin="PA4" pad="40"/>
<connect gate="MCU" pin="PA5" pad="41"/>
<connect gate="MCU" pin="PA6" pad="42"/>
<connect gate="MCU" pin="PA7" pad="43"/>
<connect gate="MCU" pin="PA8" pad="100"/>
<connect gate="MCU" pin="PA9" pad="101"/>
<connect gate="MCU" pin="PB0" pad="46"/>
<connect gate="MCU" pin="PB1" pad="47"/>
<connect gate="MCU" pin="PB10" pad="69"/>
<connect gate="MCU" pin="PB11" pad="70"/>
<connect gate="MCU" pin="PB12" pad="73"/>
<connect gate="MCU" pin="PB13" pad="74"/>
<connect gate="MCU" pin="PB14" pad="75"/>
<connect gate="MCU" pin="PB15" pad="76"/>
<connect gate="MCU" pin="PB2" pad="48"/>
<connect gate="MCU" pin="PB3" pad="133"/>
<connect gate="MCU" pin="PB4" pad="134"/>
<connect gate="MCU" pin="PB5" pad="135"/>
<connect gate="MCU" pin="PB6" pad="136"/>
<connect gate="MCU" pin="PB7" pad="137"/>
<connect gate="MCU" pin="PB8" pad="139"/>
<connect gate="MCU" pin="PB9" pad="140"/>
<connect gate="MCU" pin="PC0" pad="26"/>
<connect gate="MCU" pin="PC1" pad="27"/>
<connect gate="MCU" pin="PC10" pad="111"/>
<connect gate="MCU" pin="PC11" pad="112"/>
<connect gate="MCU" pin="PC12" pad="113"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="28"/>
<connect gate="MCU" pin="PC3" pad="29"/>
<connect gate="MCU" pin="PC4" pad="44"/>
<connect gate="MCU" pin="PC5" pad="45"/>
<connect gate="MCU" pin="PC6" pad="96"/>
<connect gate="MCU" pin="PC7" pad="97"/>
<connect gate="MCU" pin="PC8" pad="98"/>
<connect gate="MCU" pin="PC9" pad="99"/>
<connect gate="MCU" pin="PD0" pad="114"/>
<connect gate="MCU" pin="PD1" pad="115"/>
<connect gate="MCU" pin="PD10" pad="79"/>
<connect gate="MCU" pin="PD11" pad="80"/>
<connect gate="MCU" pin="PD12" pad="81"/>
<connect gate="MCU" pin="PD13" pad="82"/>
<connect gate="MCU" pin="PD14" pad="85"/>
<connect gate="MCU" pin="PD15" pad="86"/>
<connect gate="MCU" pin="PD2" pad="116"/>
<connect gate="MCU" pin="PD3" pad="117"/>
<connect gate="MCU" pin="PD4" pad="118"/>
<connect gate="MCU" pin="PD5" pad="119"/>
<connect gate="MCU" pin="PD6" pad="122"/>
<connect gate="MCU" pin="PD7" pad="123"/>
<connect gate="MCU" pin="PD8" pad="77"/>
<connect gate="MCU" pin="PD9" pad="78"/>
<connect gate="MCU" pin="PE0" pad="141"/>
<connect gate="MCU" pin="PE1" pad="142"/>
<connect gate="MCU" pin="PE10" pad="63"/>
<connect gate="MCU" pin="PE11" pad="64"/>
<connect gate="MCU" pin="PE12" pad="65"/>
<connect gate="MCU" pin="PE13" pad="66"/>
<connect gate="MCU" pin="PE14" pad="67"/>
<connect gate="MCU" pin="PE15" pad="68"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="58"/>
<connect gate="MCU" pin="PE8" pad="59"/>
<connect gate="MCU" pin="PE9" pad="60"/>
<connect gate="MCU" pin="PF0" pad="10"/>
<connect gate="MCU" pin="PF1" pad="11"/>
<connect gate="MCU" pin="PF10" pad="22"/>
<connect gate="MCU" pin="PF11" pad="49"/>
<connect gate="MCU" pin="PF12" pad="50"/>
<connect gate="MCU" pin="PF13" pad="53"/>
<connect gate="MCU" pin="PF14" pad="54"/>
<connect gate="MCU" pin="PF15" pad="55"/>
<connect gate="MCU" pin="PF2" pad="12"/>
<connect gate="MCU" pin="PF3" pad="13"/>
<connect gate="MCU" pin="PF4" pad="14"/>
<connect gate="MCU" pin="PF5" pad="15"/>
<connect gate="MCU" pin="PF6" pad="18"/>
<connect gate="MCU" pin="PF7" pad="19"/>
<connect gate="MCU" pin="PF8" pad="20"/>
<connect gate="MCU" pin="PF9" pad="21"/>
<connect gate="MCU" pin="PG0" pad="56"/>
<connect gate="MCU" pin="PG1" pad="57"/>
<connect gate="MCU" pin="PG10" pad="125"/>
<connect gate="MCU" pin="PG11" pad="126"/>
<connect gate="MCU" pin="PG12" pad="127"/>
<connect gate="MCU" pin="PG13" pad="128"/>
<connect gate="MCU" pin="PG14" pad="129"/>
<connect gate="MCU" pin="PG15" pad="132"/>
<connect gate="MCU" pin="PG2" pad="87"/>
<connect gate="MCU" pin="PG3" pad="88"/>
<connect gate="MCU" pin="PG4" pad="89"/>
<connect gate="MCU" pin="PG5" pad="90"/>
<connect gate="MCU" pin="PG6" pad="91"/>
<connect gate="MCU" pin="PG7" pad="92"/>
<connect gate="MCU" pin="PG8" pad="93"/>
<connect gate="MCU" pin="PG9" pad="124"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="33"/>
<connect gate="MCU" pin="VDDIO2_1" pad="95"/>
<connect gate="MCU" pin="VDDIO2_2" pad="131"/>
<connect gate="MCU" pin="VDD_USB" pad="106"/>
<connect gate="MCU" pin="VREF+" pad="32"/>
<connect gate="MCU" pin="VREF-" pad="31"/>
<connect gate="MCU" pin="VSSA" pad="30"/>
<connect gate="PWR" pin="VDD@1" pad="17"/>
<connect gate="PWR" pin="VDD@2" pad="39"/>
<connect gate="PWR" pin="VDD@3" pad="52"/>
<connect gate="PWR" pin="VDD@4" pad="62"/>
<connect gate="PWR" pin="VDD@5" pad="72"/>
<connect gate="PWR" pin="VDD@6" pad="84"/>
<connect gate="PWR" pin="VDD@7" pad="108"/>
<connect gate="PWR" pin="VDD@8" pad="121"/>
<connect gate="PWR" pin="VDD@9" pad="144"/>
<connect gate="PWR" pin="VSS@1" pad="16"/>
<connect gate="PWR" pin="VSS@10" pad="130"/>
<connect gate="PWR" pin="VSS@11" pad="94"/>
<connect gate="PWR" pin="VSS@2" pad="38"/>
<connect gate="PWR" pin="VSS@3" pad="51"/>
<connect gate="PWR" pin="VSS@4" pad="61"/>
<connect gate="PWR" pin="VSS@5" pad="71"/>
<connect gate="PWR" pin="VSS@6" pad="83"/>
<connect gate="PWR" pin="VSS@7" pad="107"/>
<connect gate="PWR" pin="VSS@8" pad="120"/>
<connect gate="PWR" pin="VSS@9" pad="143"/>
</connects>
<technologies>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L486Q*I">
<description>&lt;b&gt;ARM 32-bit Cortex™-M4 CPU&lt;/b&gt;&lt;p&gt;
80 MHz maximum frequency&lt;br&gt;
1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
109 GPIOs&lt;br&gt;
1.71 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_132PIN_TYP2"/>
<gate name="PWR" symbol="PWR_VDD6_VSS7"/>
</gates>
<devices>
<device name="" package="UFBGA132">
<connects>
<connect gate="MCU" pin="BOOT0" pad="A4"/>
<connect gate="MCU" pin="NRST" pad="H2"/>
<connect gate="MCU" pin="OPAMP1" pad="M3"/>
<connect gate="MCU" pin="OPAMP2" pad="M4"/>
<connect gate="MCU" pin="OSC_IN" pad="F1"/>
<connect gate="MCU" pin="OSC_OUT" pad="G1"/>
<connect gate="MCU" pin="PA0" pad="L2"/>
<connect gate="MCU" pin="PA1" pad="M2"/>
<connect gate="MCU" pin="PA10" pad="C12"/>
<connect gate="MCU" pin="PA11" pad="B12"/>
<connect gate="MCU" pin="PA12" pad="A12"/>
<connect gate="MCU" pin="PA13" pad="A11"/>
<connect gate="MCU" pin="PA14" pad="A10"/>
<connect gate="MCU" pin="PA15" pad="A9"/>
<connect gate="MCU" pin="PA2" pad="K3"/>
<connect gate="MCU" pin="PA3" pad="L3"/>
<connect gate="MCU" pin="PA4" pad="J4"/>
<connect gate="MCU" pin="PA5" pad="K4"/>
<connect gate="MCU" pin="PA6" pad="L4"/>
<connect gate="MCU" pin="PA7" pad="J5"/>
<connect gate="MCU" pin="PA8" pad="D11"/>
<connect gate="MCU" pin="PA9" pad="D10"/>
<connect gate="MCU" pin="PB0" pad="M5"/>
<connect gate="MCU" pin="PB1" pad="M6"/>
<connect gate="MCU" pin="PB10" pad="L10"/>
<connect gate="MCU" pin="PB11" pad="L11"/>
<connect gate="MCU" pin="PB12" pad="L12"/>
<connect gate="MCU" pin="PB13" pad="K12"/>
<connect gate="MCU" pin="PB14" pad="K11"/>
<connect gate="MCU" pin="PB15" pad="K10"/>
<connect gate="MCU" pin="PB2" pad="L6"/>
<connect gate="MCU" pin="PB3" pad="A8"/>
<connect gate="MCU" pin="PB4" pad="A7"/>
<connect gate="MCU" pin="PB5" pad="C5"/>
<connect gate="MCU" pin="PB6" pad="B5"/>
<connect gate="MCU" pin="PB7" pad="B4"/>
<connect gate="MCU" pin="PB8" pad="A3"/>
<connect gate="MCU" pin="PB9" pad="B3"/>
<connect gate="MCU" pin="PC0" pad="H1"/>
<connect gate="MCU" pin="PC1" pad="J2"/>
<connect gate="MCU" pin="PC10" pad="B11"/>
<connect gate="MCU" pin="PC11" pad="C10"/>
<connect gate="MCU" pin="PC12" pad="B10"/>
<connect gate="MCU" pin="PC13" pad="C1"/>
<connect gate="MCU" pin="PC14" pad="D1"/>
<connect gate="MCU" pin="PC15" pad="E1"/>
<connect gate="MCU" pin="PC2" pad="J3"/>
<connect gate="MCU" pin="PC3" pad="K2"/>
<connect gate="MCU" pin="PC4" pad="K5"/>
<connect gate="MCU" pin="PC5" pad="L5"/>
<connect gate="MCU" pin="PC6" pad="E12"/>
<connect gate="MCU" pin="PC7" pad="E11"/>
<connect gate="MCU" pin="PC8" pad="E10"/>
<connect gate="MCU" pin="PC9" pad="D12"/>
<connect gate="MCU" pin="PD0" pad="C9"/>
<connect gate="MCU" pin="PD1" pad="B9"/>
<connect gate="MCU" pin="PD10" pad="J12"/>
<connect gate="MCU" pin="PD11" pad="J11"/>
<connect gate="MCU" pin="PD12" pad="J10"/>
<connect gate="MCU" pin="PD13" pad="H12"/>
<connect gate="MCU" pin="PD14" pad="H11"/>
<connect gate="MCU" pin="PD15" pad="H10"/>
<connect gate="MCU" pin="PD2" pad="C8"/>
<connect gate="MCU" pin="PD3" pad="B8"/>
<connect gate="MCU" pin="PD4" pad="B7"/>
<connect gate="MCU" pin="PD5" pad="A6"/>
<connect gate="MCU" pin="PD6" pad="B6"/>
<connect gate="MCU" pin="PD7" pad="A5"/>
<connect gate="MCU" pin="PD8" pad="K9"/>
<connect gate="MCU" pin="PD9" pad="K8"/>
<connect gate="MCU" pin="PE0" pad="C3"/>
<connect gate="MCU" pin="PE1" pad="A2"/>
<connect gate="MCU" pin="PE10" pad="L8"/>
<connect gate="MCU" pin="PE11" pad="M9"/>
<connect gate="MCU" pin="PE12" pad="L9"/>
<connect gate="MCU" pin="PE13" pad="M10"/>
<connect gate="MCU" pin="PE14" pad="M11"/>
<connect gate="MCU" pin="PE15" pad="M12"/>
<connect gate="MCU" pin="PE2" pad="B2"/>
<connect gate="MCU" pin="PE3" pad="A1"/>
<connect gate="MCU" pin="PE4" pad="B1"/>
<connect gate="MCU" pin="PE5" pad="C2"/>
<connect gate="MCU" pin="PE6" pad="D2"/>
<connect gate="MCU" pin="PE7" pad="M7"/>
<connect gate="MCU" pin="PE8" pad="L7"/>
<connect gate="MCU" pin="PE9" pad="M8"/>
<connect gate="MCU" pin="PF0" pad="D6"/>
<connect gate="MCU" pin="PF1" pad="D5"/>
<connect gate="MCU" pin="PF11" pad="K6"/>
<connect gate="MCU" pin="PF12" pad="J7"/>
<connect gate="MCU" pin="PF13" pad="K7"/>
<connect gate="MCU" pin="PF14" pad="J8"/>
<connect gate="MCU" pin="PF15" pad="J9"/>
<connect gate="MCU" pin="PF2" pad="D4"/>
<connect gate="MCU" pin="PF3" pad="E4"/>
<connect gate="MCU" pin="PF4" pad="F3"/>
<connect gate="MCU" pin="PF5" pad="F4"/>
<connect gate="MCU" pin="PG0" pad="H9"/>
<connect gate="MCU" pin="PG1" pad="G9"/>
<connect gate="MCU" pin="PG10" pad="D8"/>
<connect gate="MCU" pin="PG11" pad="G3"/>
<connect gate="MCU" pin="PG12" pad="D7"/>
<connect gate="MCU" pin="PG13" pad="C7"/>
<connect gate="MCU" pin="PG14" pad="C6"/>
<connect gate="MCU" pin="PG15" pad="K1"/>
<connect gate="MCU" pin="PG2" pad="G10"/>
<connect gate="MCU" pin="PG3" pad="F9"/>
<connect gate="MCU" pin="PG4" pad="F10"/>
<connect gate="MCU" pin="PG5" pad="E9"/>
<connect gate="MCU" pin="PG6" pad="G4"/>
<connect gate="MCU" pin="PG7" pad="H4"/>
<connect gate="MCU" pin="PG8" pad="J6"/>
<connect gate="MCU" pin="PG9" pad="D9"/>
<connect gate="MCU" pin="VBAT" pad="E2"/>
<connect gate="MCU" pin="VDDA" pad="M1"/>
<connect gate="MCU" pin="VDDIO2_1" pad="G7"/>
<connect gate="MCU" pin="VDD_USB" pad="C11"/>
<connect gate="MCU" pin="VREF+" pad="L1"/>
<connect gate="MCU" pin="VSSA" pad="J1"/>
<connect gate="PWR" pin="VDD@1" pad="C4"/>
<connect gate="PWR" pin="VDD@2" pad="G2"/>
<connect gate="PWR" pin="VDD@3" pad="G6"/>
<connect gate="PWR" pin="VDD@4" pad="G11"/>
<connect gate="PWR" pin="VDD@5" pad="G12"/>
<connect gate="PWR" pin="VDD@6" pad="H3"/>
<connect gate="PWR" pin="VSS@1" pad="D3"/>
<connect gate="PWR" pin="VSS@2" pad="E3"/>
<connect gate="PWR" pin="VSS@3" pad="F2"/>
<connect gate="PWR" pin="VSS@4" pad="F6"/>
<connect gate="PWR" pin="VSS@5" pad="F7"/>
<connect gate="PWR" pin="VSS@6" pad="F11"/>
<connect gate="PWR" pin="VSS@7" pad="F12"/>
</connects>
<technologies>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L486V*T">
<description>&lt;b&gt;ARM 32-bit Cortex™-M4 CPU&lt;/b&gt;&lt;p&gt;
80 MHz maximum frequency&lt;br&gt;
1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
82 GPIOs&lt;br&gt;
1.71 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_100PIN_TYP11"/>
<gate name="PWD" symbol="PWR_VDD5_VSS5"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="MCU" pin="BOOT0" pad="94"/>
<connect gate="MCU" pin="NRST" pad="14"/>
<connect gate="MCU" pin="OSC_IN" pad="12"/>
<connect gate="MCU" pin="OSC_OUT" pad="13"/>
<connect gate="MCU" pin="PA0" pad="23"/>
<connect gate="MCU" pin="PA1" pad="24"/>
<connect gate="MCU" pin="PA10" pad="69"/>
<connect gate="MCU" pin="PA11" pad="70"/>
<connect gate="MCU" pin="PA12" pad="71"/>
<connect gate="MCU" pin="PA13" pad="72"/>
<connect gate="MCU" pin="PA14" pad="76"/>
<connect gate="MCU" pin="PA15" pad="77"/>
<connect gate="MCU" pin="PA2" pad="25"/>
<connect gate="MCU" pin="PA3" pad="26"/>
<connect gate="MCU" pin="PA4" pad="29"/>
<connect gate="MCU" pin="PA5" pad="30"/>
<connect gate="MCU" pin="PA6" pad="31"/>
<connect gate="MCU" pin="PA7" pad="32"/>
<connect gate="MCU" pin="PA8" pad="67"/>
<connect gate="MCU" pin="PA9" pad="68"/>
<connect gate="MCU" pin="PB0" pad="35"/>
<connect gate="MCU" pin="PB1" pad="36"/>
<connect gate="MCU" pin="PB10" pad="47"/>
<connect gate="MCU" pin="PB11" pad="48"/>
<connect gate="MCU" pin="PB12" pad="51"/>
<connect gate="MCU" pin="PB13" pad="52"/>
<connect gate="MCU" pin="PB14" pad="53"/>
<connect gate="MCU" pin="PB15" pad="54"/>
<connect gate="MCU" pin="PB2" pad="37"/>
<connect gate="MCU" pin="PB3" pad="89"/>
<connect gate="MCU" pin="PB4" pad="90"/>
<connect gate="MCU" pin="PB5" pad="91"/>
<connect gate="MCU" pin="PB6" pad="92"/>
<connect gate="MCU" pin="PB7" pad="93"/>
<connect gate="MCU" pin="PB8" pad="95"/>
<connect gate="MCU" pin="PB9" pad="96"/>
<connect gate="MCU" pin="PC0" pad="15"/>
<connect gate="MCU" pin="PC1" pad="16"/>
<connect gate="MCU" pin="PC10" pad="78"/>
<connect gate="MCU" pin="PC11" pad="79"/>
<connect gate="MCU" pin="PC12" pad="80"/>
<connect gate="MCU" pin="PC13" pad="7"/>
<connect gate="MCU" pin="PC14" pad="8"/>
<connect gate="MCU" pin="PC15" pad="9"/>
<connect gate="MCU" pin="PC2" pad="17"/>
<connect gate="MCU" pin="PC3" pad="18"/>
<connect gate="MCU" pin="PC4" pad="33"/>
<connect gate="MCU" pin="PC5" pad="34"/>
<connect gate="MCU" pin="PC6" pad="63"/>
<connect gate="MCU" pin="PC7" pad="64"/>
<connect gate="MCU" pin="PC8" pad="65"/>
<connect gate="MCU" pin="PC9" pad="66"/>
<connect gate="MCU" pin="PD0" pad="81"/>
<connect gate="MCU" pin="PD1" pad="82"/>
<connect gate="MCU" pin="PD10" pad="57"/>
<connect gate="MCU" pin="PD11" pad="58"/>
<connect gate="MCU" pin="PD12" pad="59"/>
<connect gate="MCU" pin="PD13" pad="60"/>
<connect gate="MCU" pin="PD14" pad="61"/>
<connect gate="MCU" pin="PD15" pad="62"/>
<connect gate="MCU" pin="PD2" pad="83"/>
<connect gate="MCU" pin="PD3" pad="84"/>
<connect gate="MCU" pin="PD4" pad="85"/>
<connect gate="MCU" pin="PD5" pad="86"/>
<connect gate="MCU" pin="PD6" pad="87"/>
<connect gate="MCU" pin="PD7" pad="88"/>
<connect gate="MCU" pin="PD8" pad="55"/>
<connect gate="MCU" pin="PD9" pad="56"/>
<connect gate="MCU" pin="PE0" pad="97"/>
<connect gate="MCU" pin="PE1" pad="98"/>
<connect gate="MCU" pin="PE10" pad="41"/>
<connect gate="MCU" pin="PE11" pad="42"/>
<connect gate="MCU" pin="PE12" pad="43"/>
<connect gate="MCU" pin="PE13" pad="44"/>
<connect gate="MCU" pin="PE14" pad="45"/>
<connect gate="MCU" pin="PE15" pad="46"/>
<connect gate="MCU" pin="PE2" pad="1"/>
<connect gate="MCU" pin="PE3" pad="2"/>
<connect gate="MCU" pin="PE4" pad="3"/>
<connect gate="MCU" pin="PE5" pad="4"/>
<connect gate="MCU" pin="PE6" pad="5"/>
<connect gate="MCU" pin="PE7" pad="38"/>
<connect gate="MCU" pin="PE8" pad="39"/>
<connect gate="MCU" pin="PE9" pad="40"/>
<connect gate="MCU" pin="VBAT" pad="6"/>
<connect gate="MCU" pin="VDDA" pad="22"/>
<connect gate="MCU" pin="VDD_USB" pad="73"/>
<connect gate="MCU" pin="VREF+" pad="21"/>
<connect gate="MCU" pin="VREF-" pad="20"/>
<connect gate="MCU" pin="VSSA" pad="19"/>
<connect gate="PWD" pin="VDD@1" pad="11"/>
<connect gate="PWD" pin="VDD@2" pad="28"/>
<connect gate="PWD" pin="VDD@3" pad="50"/>
<connect gate="PWD" pin="VDD@4" pad="75"/>
<connect gate="PWD" pin="VDD@5" pad="100"/>
<connect gate="PWD" pin="VSS@1" pad="10"/>
<connect gate="PWD" pin="VSS@2" pad="27"/>
<connect gate="PWD" pin="VSS@3" pad="49"/>
<connect gate="PWD" pin="VSS@4" pad="74"/>
<connect gate="PWD" pin="VSS@5" pad="99"/>
</connects>
<technologies>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L486J*Y">
<description>&lt;b&gt;ARM 32-bit Cortex™-M4 CPU&lt;/b&gt;&lt;p&gt;
80 MHz maximum frequency&lt;br&gt;
1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
57 GPIOs&lt;br&gt;
1.71 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_72PIN_TYP1"/>
<gate name="PWD" symbol="PWR_VDD3_VSS4"/>
</gates>
<devices>
<device name="" package="WLCSP72">
<connects>
<connect gate="MCU" pin="BOOT0" pad="D7"/>
<connect gate="MCU" pin="NRST" pad="E9"/>
<connect gate="MCU" pin="OSC_IN" pad="D9"/>
<connect gate="MCU" pin="OSC_OUT" pad="D8"/>
<connect gate="MCU" pin="PA0-WKUP" pad="H8"/>
<connect gate="MCU" pin="PA1" pad="G4"/>
<connect gate="MCU" pin="PA10" pad="D2"/>
<connect gate="MCU" pin="PA11" pad="D1"/>
<connect gate="MCU" pin="PA12" pad="C1"/>
<connect gate="MCU" pin="PA13" pad="C2"/>
<connect gate="MCU" pin="PA14" pad="B2"/>
<connect gate="MCU" pin="PA15" pad="A2"/>
<connect gate="MCU" pin="PA2" pad="G6"/>
<connect gate="MCU" pin="PA3" pad="H7"/>
<connect gate="MCU" pin="PA4" pad="G5"/>
<connect gate="MCU" pin="PA5" pad="H6"/>
<connect gate="MCU" pin="PA6" pad="H5"/>
<connect gate="MCU" pin="PA7" pad="H4"/>
<connect gate="MCU" pin="PA8" pad="E2"/>
<connect gate="MCU" pin="PA9" pad="E3"/>
<connect gate="MCU" pin="PB0" pad="J5"/>
<connect gate="MCU" pin="PB1" pad="J4"/>
<connect gate="MCU" pin="PB10" pad="H3"/>
<connect gate="MCU" pin="PB11" pad="G3"/>
<connect gate="MCU" pin="PB12" pad="H1"/>
<connect gate="MCU" pin="PB13" pad="H2"/>
<connect gate="MCU" pin="PB14" pad="G2"/>
<connect gate="MCU" pin="PB15" pad="G1"/>
<connect gate="MCU" pin="PB2" pad="J3"/>
<connect gate="MCU" pin="PB3" pad="A6"/>
<connect gate="MCU" pin="PB4" pad="C6"/>
<connect gate="MCU" pin="PB5" pad="C7"/>
<connect gate="MCU" pin="PB6" pad="B7"/>
<connect gate="MCU" pin="PB7" pad="A7"/>
<connect gate="MCU" pin="PB8" pad="E7"/>
<connect gate="MCU" pin="PB9" pad="E8"/>
<connect gate="MCU" pin="PC0" pad="F9"/>
<connect gate="MCU" pin="PC1" pad="F8"/>
<connect gate="MCU" pin="PC10" pad="D3"/>
<connect gate="MCU" pin="PC11" pad="C3"/>
<connect gate="MCU" pin="PC12" pad="B3"/>
<connect gate="MCU" pin="PC13" pad="B8"/>
<connect gate="MCU" pin="PC14" pad="C9"/>
<connect gate="MCU" pin="PC15" pad="C8"/>
<connect gate="MCU" pin="PC2" pad="F7"/>
<connect gate="MCU" pin="PC3" pad="G7"/>
<connect gate="MCU" pin="PC4" pad="J7"/>
<connect gate="MCU" pin="PC5" pad="J6"/>
<connect gate="MCU" pin="PC6" pad="F3"/>
<connect gate="MCU" pin="PC7" pad="F1"/>
<connect gate="MCU" pin="PC8" pad="F2"/>
<connect gate="MCU" pin="PC9" pad="E1"/>
<connect gate="MCU" pin="PD2" pad="A3"/>
<connect gate="MCU" pin="PG10" pad="B4"/>
<connect gate="MCU" pin="PG11" pad="C4"/>
<connect gate="MCU" pin="PG12" pad="C5"/>
<connect gate="MCU" pin="PG13" pad="B5"/>
<connect gate="MCU" pin="PG14" pad="A5"/>
<connect gate="MCU" pin="PG9" pad="A4"/>
<connect gate="MCU" pin="VBAT" pad="B9"/>
<connect gate="MCU" pin="VDDA" pad="H9"/>
<connect gate="MCU" pin="VDDIO2" pad="B6"/>
<connect gate="MCU" pin="VDD_USB" pad="A1"/>
<connect gate="MCU" pin="VREF+" pad="G8"/>
<connect gate="MCU" pin="VSSA" pad="G9"/>
<connect gate="PWD" pin="VDD@1" pad="A9"/>
<connect gate="PWD" pin="VDD@2" pad="J1"/>
<connect gate="PWD" pin="VDD@3" pad="J8"/>
<connect gate="PWD" pin="VSS@1" pad="A8"/>
<connect gate="PWD" pin="VSS@2" pad="B1"/>
<connect gate="PWD" pin="VSS@3" pad="J2"/>
<connect gate="PWD" pin="VSS@4" pad="J9"/>
</connects>
<technologies>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM32L486R*T">
<description>&lt;b&gt;ARM 32-bit Cortex™-M4 CPU&lt;/b&gt;&lt;p&gt;
80 MHz maximum frequency&lt;br&gt;
1024 Kbytes of Flash memory&lt;br&gt;
128 kbytes of SRAM&lt;br&gt;
51 GPIOs&lt;br&gt;
1.71 to 3.6 V application supply&lt;br&gt;</description>
<gates>
<gate name="MCU" symbol="STM32_64PIN_TYP20"/>
<gate name="PWR" symbol="PWR_VDD3_VSS4"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="MCU" pin="BOOT0" pad="60"/>
<connect gate="MCU" pin="NRST" pad="7"/>
<connect gate="MCU" pin="OSC_IN" pad="5"/>
<connect gate="MCU" pin="OSC_OUT" pad="6"/>
<connect gate="MCU" pin="PA0-WKUP" pad="14"/>
<connect gate="MCU" pin="PA1" pad="15"/>
<connect gate="MCU" pin="PA10" pad="43"/>
<connect gate="MCU" pin="PA11" pad="44"/>
<connect gate="MCU" pin="PA12" pad="45"/>
<connect gate="MCU" pin="PA13" pad="46"/>
<connect gate="MCU" pin="PA14" pad="49"/>
<connect gate="MCU" pin="PA15" pad="50"/>
<connect gate="MCU" pin="PA2" pad="16"/>
<connect gate="MCU" pin="PA3" pad="17"/>
<connect gate="MCU" pin="PA4" pad="20"/>
<connect gate="MCU" pin="PA5" pad="21"/>
<connect gate="MCU" pin="PA6" pad="22"/>
<connect gate="MCU" pin="PA7" pad="23"/>
<connect gate="MCU" pin="PA8" pad="41"/>
<connect gate="MCU" pin="PA9" pad="42"/>
<connect gate="MCU" pin="PB0" pad="26"/>
<connect gate="MCU" pin="PB1" pad="27"/>
<connect gate="MCU" pin="PB10" pad="29"/>
<connect gate="MCU" pin="PB11" pad="30"/>
<connect gate="MCU" pin="PB12" pad="33"/>
<connect gate="MCU" pin="PB13" pad="34"/>
<connect gate="MCU" pin="PB14" pad="35"/>
<connect gate="MCU" pin="PB15" pad="36"/>
<connect gate="MCU" pin="PB2" pad="28"/>
<connect gate="MCU" pin="PB3" pad="55"/>
<connect gate="MCU" pin="PB4" pad="56"/>
<connect gate="MCU" pin="PB5" pad="57"/>
<connect gate="MCU" pin="PB6" pad="58"/>
<connect gate="MCU" pin="PB7" pad="59"/>
<connect gate="MCU" pin="PB8" pad="61"/>
<connect gate="MCU" pin="PB9" pad="62"/>
<connect gate="MCU" pin="PC0" pad="8"/>
<connect gate="MCU" pin="PC1" pad="9"/>
<connect gate="MCU" pin="PC10" pad="51"/>
<connect gate="MCU" pin="PC11" pad="52"/>
<connect gate="MCU" pin="PC12" pad="53"/>
<connect gate="MCU" pin="PC13" pad="2"/>
<connect gate="MCU" pin="PC14" pad="3"/>
<connect gate="MCU" pin="PC15" pad="4"/>
<connect gate="MCU" pin="PC2" pad="10"/>
<connect gate="MCU" pin="PC3" pad="11"/>
<connect gate="MCU" pin="PC4" pad="24"/>
<connect gate="MCU" pin="PC5" pad="25"/>
<connect gate="MCU" pin="PC6" pad="37"/>
<connect gate="MCU" pin="PC7" pad="38"/>
<connect gate="MCU" pin="PC8" pad="39"/>
<connect gate="MCU" pin="PC9" pad="40"/>
<connect gate="MCU" pin="PD2" pad="54"/>
<connect gate="MCU" pin="VBAT" pad="1"/>
<connect gate="MCU" pin="VDDA" pad="13"/>
<connect gate="MCU" pin="VDD_USB" pad="48"/>
<connect gate="MCU" pin="VSSA" pad="12"/>
<connect gate="PWR" pin="VDD@1" pad="19"/>
<connect gate="PWR" pin="VDD@2" pad="32"/>
<connect gate="PWR" pin="VDD@3" pad="64"/>
<connect gate="PWR" pin="VSS@1" pad="18"/>
<connect gate="PWR" pin="VSS@2" pad="31"/>
<connect gate="PWR" pin="VSS@3" pad="63"/>
<connect gate="PWR" pin="VSS@4" pad="47"/>
</connects>
<technologies>
<technology name="G"/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
