(kicad_pcb (version 4) (host pcbnew "(2016-07-06 BZR 6970, Git 61e886e)-product")
  (general
    (links 512)
    (no_connects 16)
    (area 19.924999 19.924999 133.714287 127.745001)
    (thickness 1.6)
    (drawings 15)
    (tracks 1440)
    (zones 0)
    (modules 260)
    (nets 257)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.15)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.15)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (blind_buried_vias_allowed yes)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF7FF)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(FLUXL1-Pad1)")
  (net 2 "Net-(FLUXL2-Pad1)")
  (net 3 "Net-(FLUXL3-Pad1)")
  (net 4 "Net-(FLUXL4-Pad1)")
  (net 5 "Net-(FLUXL5-Pad1)")
  (net 6 "Net-(FLUXL6-Pad1)")
  (net 7 "Net-(FLUXL7-Pad1)")
  (net 8 "Net-(FLUXL8-Pad1)")
  (net 9 "Net-(FLUXL9-Pad1)")
  (net 10 "Net-(FLUXL10-Pad1)")
  (net 11 "Net-(FLUXL11-Pad1)")
  (net 12 "Net-(FLUXL12-Pad1)")
  (net 13 "Net-(FLUXL13-Pad1)")
  (net 14 "Net-(FLUXL14-Pad1)")
  (net 15 "Net-(FLUXL15-Pad1)")
  (net 16 "Net-(FLUXL16-Pad1)")
  (net 17 "Net-(FLUXL17-Pad1)")
  (net 18 "Net-(FLUXL18-Pad1)")
  (net 19 "Net-(FLUXL19-Pad1)")
  (net 20 "Net-(FLUXL20-Pad1)")
  (net 21 "Net-(FLUXL21-Pad1)")
  (net 22 "Net-(FLUXL22-Pad1)")
  (net 23 "Net-(FLUXL23-Pad1)")
  (net 24 "Net-(FLUXL24-Pad1)")
  (net 25 "Net-(FLUXL25-Pad1)")
  (net 26 "Net-(FLUXL26-Pad1)")
  (net 27 "Net-(FLUXL27-Pad1)")
  (net 28 "Net-(FLUXL28-Pad1)")
  (net 29 "Net-(FLUXL29-Pad1)")
  (net 30 "Net-(FLUXL30-Pad1)")
  (net 31 "Net-(FLUXL31-Pad1)")
  (net 32 "Net-(FLUXL32-Pad1)")
  (net 33 "Net-(FLUXL33-Pad1)")
  (net 34 "Net-(FLUXL34-Pad1)")
  (net 35 "Net-(FLUXL35-Pad1)")
  (net 36 "Net-(FLUXL36-Pad1)")
  (net 37 "Net-(FLUXL37-Pad1)")
  (net 38 "Net-(FLUXL38-Pad1)")
  (net 39 "Net-(FLUXL39-Pad1)")
  (net 40 "Net-(FLUXL40-Pad1)")
  (net 41 "Net-(FLUXL41-Pad1)")
  (net 42 "Net-(FLUXL42-Pad1)")
  (net 43 "Net-(FLUXL43-Pad1)")
  (net 44 "Net-(FLUXL44-Pad1)")
  (net 45 "Net-(FLUXL45-Pad1)")
  (net 46 "Net-(FLUXL46-Pad1)")
  (net 47 "Net-(FLUXL47-Pad1)")
  (net 48 "Net-(FLUXL48-Pad1)")
  (net 49 "Net-(FLUXL49-Pad1)")
  (net 50 "Net-(FLUXL50-Pad1)")
  (net 51 "Net-(FLUXL51-Pad1)")
  (net 52 "Net-(FLUXL52-Pad1)")
  (net 53 "Net-(FLUXL53-Pad1)")
  (net 54 "Net-(FLUXL54-Pad1)")
  (net 55 "Net-(FLUXL55-Pad1)")
  (net 56 "Net-(FLUXL56-Pad1)")
  (net 57 "Net-(FLUXL57-Pad1)")
  (net 58 "Net-(FLUXL58-Pad1)")
  (net 59 "Net-(FLUXL59-Pad1)")
  (net 60 "Net-(FLUXL60-Pad1)")
  (net 61 "Net-(FLUXL61-Pad1)")
  (net 62 "Net-(FLUXL62-Pad1)")
  (net 63 "Net-(FLUXL63-Pad1)")
  (net 64 "Net-(FLUXL64-Pad1)")
  (net 65 "Net-(FLUXL65-Pad1)")
  (net 66 "Net-(FLUXL66-Pad1)")
  (net 67 "Net-(FLUXL67-Pad1)")
  (net 68 "Net-(FLUXL68-Pad1)")
  (net 69 "Net-(FLUXL69-Pad1)")
  (net 70 "Net-(FLUXL70-Pad1)")
  (net 71 "Net-(FLUXL71-Pad1)")
  (net 72 "Net-(FLUXL72-Pad1)")
  (net 73 "Net-(FLUXL73-Pad1)")
  (net 74 "Net-(FLUXL74-Pad1)")
  (net 75 "Net-(FLUXL75-Pad1)")
  (net 76 "Net-(FLUXL76-Pad1)")
  (net 77 "Net-(FLUXL77-Pad1)")
  (net 78 "Net-(FLUXL78-Pad1)")
  (net 79 "Net-(FLUXL79-Pad1)")
  (net 80 "Net-(FLUXL80-Pad1)")
  (net 81 "Net-(FLUXL81-Pad1)")
  (net 82 "Net-(FLUXL82-Pad1)")
  (net 83 "Net-(FLUXL83-Pad1)")
  (net 84 "Net-(FLUXL84-Pad1)")
  (net 85 "Net-(FLUXL85-Pad1)")
  (net 86 "Net-(FLUXL86-Pad1)")
  (net 87 "Net-(FLUXL87-Pad1)")
  (net 88 "Net-(FLUXL88-Pad1)")
  (net 89 "Net-(FLUXL89-Pad1)")
  (net 90 "Net-(FLUXL90-Pad1)")
  (net 91 "Net-(FLUXL91-Pad1)")
  (net 92 "Net-(FLUXL92-Pad1)")
  (net 93 "Net-(FLUXL93-Pad1)")
  (net 94 "Net-(FLUXL94-Pad1)")
  (net 95 "Net-(FLUXL95-Pad1)")
  (net 96 "Net-(FLUXL96-Pad1)")
  (net 97 "Net-(FLUXL97-Pad1)")
  (net 98 "Net-(FLUXL98-Pad1)")
  (net 99 "Net-(FLUXL99-Pad1)")
  (net 100 "Net-(FLUXL100-Pad1)")
  (net 101 "Net-(FLUXL101-Pad1)")
  (net 102 "Net-(FLUXL102-Pad1)")
  (net 103 "Net-(FLUXL103-Pad1)")
  (net 104 "Net-(FLUXL104-Pad1)")
  (net 105 "Net-(FLUXL105-Pad1)")
  (net 106 "Net-(FLUXL106-Pad1)")
  (net 107 "Net-(FLUXL107-Pad1)")
  (net 108 "Net-(FLUXL108-Pad1)")
  (net 109 "Net-(FLUXL109-Pad1)")
  (net 110 "Net-(FLUXL110-Pad1)")
  (net 111 "Net-(FLUXL111-Pad1)")
  (net 112 "Net-(FLUXL112-Pad1)")
  (net 113 "Net-(FLUXL113-Pad1)")
  (net 114 "Net-(FLUXL114-Pad1)")
  (net 115 "Net-(FLUXL115-Pad1)")
  (net 116 "Net-(FLUXL116-Pad1)")
  (net 117 "Net-(FLUXL117-Pad1)")
  (net 118 "Net-(FLUXL118-Pad1)")
  (net 119 "Net-(FLUXL119-Pad1)")
  (net 120 "Net-(FLUXL120-Pad1)")
  (net 121 "Net-(FLUXL121-Pad1)")
  (net 122 "Net-(FLUXL122-Pad1)")
  (net 123 "Net-(FLUXL123-Pad1)")
  (net 124 "Net-(FLUXL124-Pad1)")
  (net 125 "Net-(FLUXL125-Pad1)")
  (net 126 "Net-(FLUXL126-Pad1)")
  (net 127 "Net-(FLUXL127-Pad1)")
  (net 128 "Net-(FLUXL128-Pad1)")
  (net 129 "Net-(FLUXL129-Pad1)")
  (net 130 "Net-(FLUXL130-Pad1)")
  (net 131 "Net-(FLUXL131-Pad1)")
  (net 132 "Net-(FLUXL132-Pad1)")
  (net 133 "Net-(FLUXL133-Pad1)")
  (net 134 "Net-(FLUXL134-Pad1)")
  (net 135 "Net-(FLUXL135-Pad1)")
  (net 136 "Net-(FLUXL136-Pad1)")
  (net 137 "Net-(FLUXL137-Pad1)")
  (net 138 "Net-(FLUXL138-Pad1)")
  (net 139 "Net-(FLUXL139-Pad1)")
  (net 140 "Net-(FLUXL140-Pad1)")
  (net 141 "Net-(FLUXL141-Pad1)")
  (net 142 "Net-(FLUXL142-Pad1)")
  (net 143 "Net-(FLUXL143-Pad1)")
  (net 144 "Net-(FLUXL144-Pad1)")
  (net 145 "Net-(FLUXL145-Pad1)")
  (net 146 "Net-(FLUXL146-Pad1)")
  (net 147 "Net-(FLUXL147-Pad1)")
  (net 148 "Net-(FLUXL148-Pad1)")
  (net 149 "Net-(FLUXL149-Pad1)")
  (net 150 "Net-(FLUXL150-Pad1)")
  (net 151 "Net-(FLUXL151-Pad1)")
  (net 152 "Net-(FLUXL152-Pad1)")
  (net 153 "Net-(FLUXL153-Pad1)")
  (net 154 "Net-(FLUXL154-Pad1)")
  (net 155 "Net-(FLUXL155-Pad1)")
  (net 156 "Net-(FLUXL156-Pad1)")
  (net 157 "Net-(FLUXL157-Pad1)")
  (net 158 "Net-(FLUXL158-Pad1)")
  (net 159 "Net-(FLUXL159-Pad1)")
  (net 160 "Net-(FLUXL160-Pad1)")
  (net 161 "Net-(FLUXL161-Pad1)")
  (net 162 "Net-(FLUXL162-Pad1)")
  (net 163 "Net-(FLUXL163-Pad1)")
  (net 164 "Net-(FLUXL164-Pad1)")
  (net 165 "Net-(FLUXL165-Pad1)")
  (net 166 "Net-(FLUXL166-Pad1)")
  (net 167 "Net-(FLUXL167-Pad1)")
  (net 168 "Net-(FLUXL168-Pad1)")
  (net 169 "Net-(FLUXL169-Pad1)")
  (net 170 "Net-(FLUXL170-Pad1)")
  (net 171 "Net-(FLUXL171-Pad1)")
  (net 172 "Net-(FLUXL172-Pad1)")
  (net 173 "Net-(FLUXL173-Pad1)")
  (net 174 "Net-(FLUXL174-Pad1)")
  (net 175 "Net-(FLUXL175-Pad1)")
  (net 176 "Net-(FLUXL176-Pad1)")
  (net 177 "Net-(FLUXL177-Pad1)")
  (net 178 "Net-(FLUXL178-Pad1)")
  (net 179 "Net-(FLUXL179-Pad1)")
  (net 180 "Net-(FLUXL180-Pad1)")
  (net 181 "Net-(FLUXL181-Pad1)")
  (net 182 "Net-(FLUXL182-Pad1)")
  (net 183 "Net-(FLUXL183-Pad1)")
  (net 184 "Net-(FLUXL184-Pad1)")
  (net 185 "Net-(FLUXL185-Pad1)")
  (net 186 "Net-(FLUXL186-Pad1)")
  (net 187 "Net-(FLUXL187-Pad1)")
  (net 188 "Net-(FLUXL188-Pad1)")
  (net 189 "Net-(FLUXL189-Pad1)")
  (net 190 "Net-(FLUXL190-Pad1)")
  (net 191 "Net-(FLUXL191-Pad1)")
  (net 192 "Net-(FLUXL192-Pad1)")
  (net 193 "Net-(FLUXL193-Pad1)")
  (net 194 "Net-(FLUXL194-Pad1)")
  (net 195 "Net-(FLUXL195-Pad1)")
  (net 196 "Net-(FLUXL196-Pad1)")
  (net 197 "Net-(FLUXL197-Pad1)")
  (net 198 "Net-(FLUXL198-Pad1)")
  (net 199 "Net-(FLUXL199-Pad1)")
  (net 200 "Net-(FLUXL200-Pad1)")
  (net 201 "Net-(FLUXL201-Pad1)")
  (net 202 "Net-(FLUXL202-Pad1)")
  (net 203 "Net-(FLUXL203-Pad1)")
  (net 204 "Net-(FLUXL204-Pad1)")
  (net 205 "Net-(FLUXL205-Pad1)")
  (net 206 "Net-(FLUXL206-Pad1)")
  (net 207 "Net-(FLUXL207-Pad1)")
  (net 208 "Net-(FLUXL208-Pad1)")
  (net 209 "Net-(FLUXL209-Pad1)")
  (net 210 "Net-(FLUXL210-Pad1)")
  (net 211 "Net-(FLUXL211-Pad1)")
  (net 212 "Net-(FLUXL212-Pad1)")
  (net 213 "Net-(FLUXL213-Pad1)")
  (net 214 "Net-(FLUXL214-Pad1)")
  (net 215 "Net-(FLUXL215-Pad1)")
  (net 216 "Net-(FLUXL216-Pad1)")
  (net 217 "Net-(FLUXL217-Pad1)")
  (net 218 "Net-(FLUXL218-Pad1)")
  (net 219 "Net-(FLUXL219-Pad1)")
  (net 220 "Net-(FLUXL220-Pad1)")
  (net 221 "Net-(FLUXL221-Pad1)")
  (net 222 "Net-(FLUXL222-Pad1)")
  (net 223 "Net-(FLUXL223-Pad1)")
  (net 224 "Net-(FLUXL224-Pad1)")
  (net 225 "Net-(FLUXL225-Pad1)")
  (net 226 "Net-(FLUXL226-Pad1)")
  (net 227 "Net-(FLUXL227-Pad1)")
  (net 228 "Net-(FLUXL228-Pad1)")
  (net 229 "Net-(FLUXL229-Pad1)")
  (net 230 "Net-(FLUXL230-Pad1)")
  (net 231 "Net-(FLUXL231-Pad1)")
  (net 232 "Net-(FLUXL232-Pad1)")
  (net 233 "Net-(FLUXL233-Pad1)")
  (net 234 "Net-(FLUXL234-Pad1)")
  (net 235 "Net-(FLUXL235-Pad1)")
  (net 236 "Net-(FLUXL236-Pad1)")
  (net 237 "Net-(FLUXL237-Pad1)")
  (net 238 "Net-(FLUXL238-Pad1)")
  (net 239 "Net-(FLUXL239-Pad1)")
  (net 240 "Net-(FLUXL240-Pad1)")
  (net 241 "Net-(FLUXL241-Pad1)")
  (net 242 "Net-(FLUXL242-Pad1)")
  (net 243 "Net-(FLUXL243-Pad1)")
  (net 244 "Net-(FLUXL244-Pad1)")
  (net 245 "Net-(FLUXL245-Pad1)")
  (net 246 "Net-(FLUXL246-Pad1)")
  (net 247 "Net-(FLUXL247-Pad1)")
  (net 248 "Net-(FLUXL248-Pad1)")
  (net 249 "Net-(FLUXL249-Pad1)")
  (net 250 "Net-(FLUXL250-Pad1)")
  (net 251 "Net-(FLUXL251-Pad1)")
  (net 252 "Net-(FLUXL252-Pad1)")
  (net 253 "Net-(FLUXL253-Pad1)")
  (net 254 "Net-(FLUXL254-Pad1)")
  (net 255 "Net-(FLUXL255-Pad1)")
  (net 256 "Net-(FLUXL256-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.15)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(FLUXL1-Pad1)")
    (add_net "Net-(FLUXL10-Pad1)")
    (add_net "Net-(FLUXL100-Pad1)")
    (add_net "Net-(FLUXL101-Pad1)")
    (add_net "Net-(FLUXL102-Pad1)")
    (add_net "Net-(FLUXL103-Pad1)")
    (add_net "Net-(FLUXL104-Pad1)")
    (add_net "Net-(FLUXL105-Pad1)")
    (add_net "Net-(FLUXL106-Pad1)")
    (add_net "Net-(FLUXL107-Pad1)")
    (add_net "Net-(FLUXL108-Pad1)")
    (add_net "Net-(FLUXL109-Pad1)")
    (add_net "Net-(FLUXL11-Pad1)")
    (add_net "Net-(FLUXL110-Pad1)")
    (add_net "Net-(FLUXL111-Pad1)")
    (add_net "Net-(FLUXL112-Pad1)")
    (add_net "Net-(FLUXL113-Pad1)")
    (add_net "Net-(FLUXL114-Pad1)")
    (add_net "Net-(FLUXL115-Pad1)")
    (add_net "Net-(FLUXL116-Pad1)")
    (add_net "Net-(FLUXL117-Pad1)")
    (add_net "Net-(FLUXL118-Pad1)")
    (add_net "Net-(FLUXL119-Pad1)")
    (add_net "Net-(FLUXL12-Pad1)")
    (add_net "Net-(FLUXL120-Pad1)")
    (add_net "Net-(FLUXL121-Pad1)")
    (add_net "Net-(FLUXL122-Pad1)")
    (add_net "Net-(FLUXL123-Pad1)")
    (add_net "Net-(FLUXL124-Pad1)")
    (add_net "Net-(FLUXL125-Pad1)")
    (add_net "Net-(FLUXL126-Pad1)")
    (add_net "Net-(FLUXL127-Pad1)")
    (add_net "Net-(FLUXL128-Pad1)")
    (add_net "Net-(FLUXL129-Pad1)")
    (add_net "Net-(FLUXL13-Pad1)")
    (add_net "Net-(FLUXL130-Pad1)")
    (add_net "Net-(FLUXL131-Pad1)")
    (add_net "Net-(FLUXL132-Pad1)")
    (add_net "Net-(FLUXL133-Pad1)")
    (add_net "Net-(FLUXL134-Pad1)")
    (add_net "Net-(FLUXL135-Pad1)")
    (add_net "Net-(FLUXL136-Pad1)")
    (add_net "Net-(FLUXL137-Pad1)")
    (add_net "Net-(FLUXL138-Pad1)")
    (add_net "Net-(FLUXL139-Pad1)")
    (add_net "Net-(FLUXL14-Pad1)")
    (add_net "Net-(FLUXL140-Pad1)")
    (add_net "Net-(FLUXL141-Pad1)")
    (add_net "Net-(FLUXL142-Pad1)")
    (add_net "Net-(FLUXL143-Pad1)")
    (add_net "Net-(FLUXL144-Pad1)")
    (add_net "Net-(FLUXL145-Pad1)")
    (add_net "Net-(FLUXL146-Pad1)")
    (add_net "Net-(FLUXL147-Pad1)")
    (add_net "Net-(FLUXL148-Pad1)")
    (add_net "Net-(FLUXL149-Pad1)")
    (add_net "Net-(FLUXL15-Pad1)")
    (add_net "Net-(FLUXL150-Pad1)")
    (add_net "Net-(FLUXL151-Pad1)")
    (add_net "Net-(FLUXL152-Pad1)")
    (add_net "Net-(FLUXL153-Pad1)")
    (add_net "Net-(FLUXL154-Pad1)")
    (add_net "Net-(FLUXL155-Pad1)")
    (add_net "Net-(FLUXL156-Pad1)")
    (add_net "Net-(FLUXL157-Pad1)")
    (add_net "Net-(FLUXL158-Pad1)")
    (add_net "Net-(FLUXL159-Pad1)")
    (add_net "Net-(FLUXL16-Pad1)")
    (add_net "Net-(FLUXL160-Pad1)")
    (add_net "Net-(FLUXL161-Pad1)")
    (add_net "Net-(FLUXL162-Pad1)")
    (add_net "Net-(FLUXL163-Pad1)")
    (add_net "Net-(FLUXL164-Pad1)")
    (add_net "Net-(FLUXL165-Pad1)")
    (add_net "Net-(FLUXL166-Pad1)")
    (add_net "Net-(FLUXL167-Pad1)")
    (add_net "Net-(FLUXL168-Pad1)")
    (add_net "Net-(FLUXL169-Pad1)")
    (add_net "Net-(FLUXL17-Pad1)")
    (add_net "Net-(FLUXL170-Pad1)")
    (add_net "Net-(FLUXL171-Pad1)")
    (add_net "Net-(FLUXL172-Pad1)")
    (add_net "Net-(FLUXL173-Pad1)")
    (add_net "Net-(FLUXL174-Pad1)")
    (add_net "Net-(FLUXL175-Pad1)")
    (add_net "Net-(FLUXL176-Pad1)")
    (add_net "Net-(FLUXL177-Pad1)")
    (add_net "Net-(FLUXL178-Pad1)")
    (add_net "Net-(FLUXL179-Pad1)")
    (add_net "Net-(FLUXL18-Pad1)")
    (add_net "Net-(FLUXL180-Pad1)")
    (add_net "Net-(FLUXL181-Pad1)")
    (add_net "Net-(FLUXL182-Pad1)")
    (add_net "Net-(FLUXL183-Pad1)")
    (add_net "Net-(FLUXL184-Pad1)")
    (add_net "Net-(FLUXL185-Pad1)")
    (add_net "Net-(FLUXL186-Pad1)")
    (add_net "Net-(FLUXL187-Pad1)")
    (add_net "Net-(FLUXL188-Pad1)")
    (add_net "Net-(FLUXL189-Pad1)")
    (add_net "Net-(FLUXL19-Pad1)")
    (add_net "Net-(FLUXL190-Pad1)")
    (add_net "Net-(FLUXL191-Pad1)")
    (add_net "Net-(FLUXL192-Pad1)")
    (add_net "Net-(FLUXL193-Pad1)")
    (add_net "Net-(FLUXL194-Pad1)")
    (add_net "Net-(FLUXL195-Pad1)")
    (add_net "Net-(FLUXL196-Pad1)")
    (add_net "Net-(FLUXL197-Pad1)")
    (add_net "Net-(FLUXL198-Pad1)")
    (add_net "Net-(FLUXL199-Pad1)")
    (add_net "Net-(FLUXL2-Pad1)")
    (add_net "Net-(FLUXL20-Pad1)")
    (add_net "Net-(FLUXL200-Pad1)")
    (add_net "Net-(FLUXL201-Pad1)")
    (add_net "Net-(FLUXL202-Pad1)")
    (add_net "Net-(FLUXL203-Pad1)")
    (add_net "Net-(FLUXL204-Pad1)")
    (add_net "Net-(FLUXL205-Pad1)")
    (add_net "Net-(FLUXL206-Pad1)")
    (add_net "Net-(FLUXL207-Pad1)")
    (add_net "Net-(FLUXL208-Pad1)")
    (add_net "Net-(FLUXL209-Pad1)")
    (add_net "Net-(FLUXL21-Pad1)")
    (add_net "Net-(FLUXL210-Pad1)")
    (add_net "Net-(FLUXL211-Pad1)")
    (add_net "Net-(FLUXL212-Pad1)")
    (add_net "Net-(FLUXL213-Pad1)")
    (add_net "Net-(FLUXL214-Pad1)")
    (add_net "Net-(FLUXL215-Pad1)")
    (add_net "Net-(FLUXL216-Pad1)")
    (add_net "Net-(FLUXL217-Pad1)")
    (add_net "Net-(FLUXL218-Pad1)")
    (add_net "Net-(FLUXL219-Pad1)")
    (add_net "Net-(FLUXL22-Pad1)")
    (add_net "Net-(FLUXL220-Pad1)")
    (add_net "Net-(FLUXL221-Pad1)")
    (add_net "Net-(FLUXL222-Pad1)")
    (add_net "Net-(FLUXL223-Pad1)")
    (add_net "Net-(FLUXL224-Pad1)")
    (add_net "Net-(FLUXL225-Pad1)")
    (add_net "Net-(FLUXL226-Pad1)")
    (add_net "Net-(FLUXL227-Pad1)")
    (add_net "Net-(FLUXL228-Pad1)")
    (add_net "Net-(FLUXL229-Pad1)")
    (add_net "Net-(FLUXL23-Pad1)")
    (add_net "Net-(FLUXL230-Pad1)")
    (add_net "Net-(FLUXL231-Pad1)")
    (add_net "Net-(FLUXL232-Pad1)")
    (add_net "Net-(FLUXL233-Pad1)")
    (add_net "Net-(FLUXL234-Pad1)")
    (add_net "Net-(FLUXL235-Pad1)")
    (add_net "Net-(FLUXL236-Pad1)")
    (add_net "Net-(FLUXL237-Pad1)")
    (add_net "Net-(FLUXL238-Pad1)")
    (add_net "Net-(FLUXL239-Pad1)")
    (add_net "Net-(FLUXL24-Pad1)")
    (add_net "Net-(FLUXL240-Pad1)")
    (add_net "Net-(FLUXL241-Pad1)")
    (add_net "Net-(FLUXL242-Pad1)")
    (add_net "Net-(FLUXL243-Pad1)")
    (add_net "Net-(FLUXL244-Pad1)")
    (add_net "Net-(FLUXL245-Pad1)")
    (add_net "Net-(FLUXL246-Pad1)")
    (add_net "Net-(FLUXL247-Pad1)")
    (add_net "Net-(FLUXL248-Pad1)")
    (add_net "Net-(FLUXL249-Pad1)")
    (add_net "Net-(FLUXL25-Pad1)")
    (add_net "Net-(FLUXL250-Pad1)")
    (add_net "Net-(FLUXL251-Pad1)")
    (add_net "Net-(FLUXL252-Pad1)")
    (add_net "Net-(FLUXL253-Pad1)")
    (add_net "Net-(FLUXL254-Pad1)")
    (add_net "Net-(FLUXL255-Pad1)")
    (add_net "Net-(FLUXL256-Pad1)")
    (add_net "Net-(FLUXL26-Pad1)")
    (add_net "Net-(FLUXL27-Pad1)")
    (add_net "Net-(FLUXL28-Pad1)")
    (add_net "Net-(FLUXL29-Pad1)")
    (add_net "Net-(FLUXL3-Pad1)")
    (add_net "Net-(FLUXL30-Pad1)")
    (add_net "Net-(FLUXL31-Pad1)")
    (add_net "Net-(FLUXL32-Pad1)")
    (add_net "Net-(FLUXL33-Pad1)")
    (add_net "Net-(FLUXL34-Pad1)")
    (add_net "Net-(FLUXL35-Pad1)")
    (add_net "Net-(FLUXL36-Pad1)")
    (add_net "Net-(FLUXL37-Pad1)")
    (add_net "Net-(FLUXL38-Pad1)")
    (add_net "Net-(FLUXL39-Pad1)")
    (add_net "Net-(FLUXL4-Pad1)")
    (add_net "Net-(FLUXL40-Pad1)")
    (add_net "Net-(FLUXL41-Pad1)")
    (add_net "Net-(FLUXL42-Pad1)")
    (add_net "Net-(FLUXL43-Pad1)")
    (add_net "Net-(FLUXL44-Pad1)")
    (add_net "Net-(FLUXL45-Pad1)")
    (add_net "Net-(FLUXL46-Pad1)")
    (add_net "Net-(FLUXL47-Pad1)")
    (add_net "Net-(FLUXL48-Pad1)")
    (add_net "Net-(FLUXL49-Pad1)")
    (add_net "Net-(FLUXL5-Pad1)")
    (add_net "Net-(FLUXL50-Pad1)")
    (add_net "Net-(FLUXL51-Pad1)")
    (add_net "Net-(FLUXL52-Pad1)")
    (add_net "Net-(FLUXL53-Pad1)")
    (add_net "Net-(FLUXL54-Pad1)")
    (add_net "Net-(FLUXL55-Pad1)")
    (add_net "Net-(FLUXL56-Pad1)")
    (add_net "Net-(FLUXL57-Pad1)")
    (add_net "Net-(FLUXL58-Pad1)")
    (add_net "Net-(FLUXL59-Pad1)")
    (add_net "Net-(FLUXL6-Pad1)")
    (add_net "Net-(FLUXL60-Pad1)")
    (add_net "Net-(FLUXL61-Pad1)")
    (add_net "Net-(FLUXL62-Pad1)")
    (add_net "Net-(FLUXL63-Pad1)")
    (add_net "Net-(FLUXL64-Pad1)")
    (add_net "Net-(FLUXL65-Pad1)")
    (add_net "Net-(FLUXL66-Pad1)")
    (add_net "Net-(FLUXL67-Pad1)")
    (add_net "Net-(FLUXL68-Pad1)")
    (add_net "Net-(FLUXL69-Pad1)")
    (add_net "Net-(FLUXL7-Pad1)")
    (add_net "Net-(FLUXL70-Pad1)")
    (add_net "Net-(FLUXL71-Pad1)")
    (add_net "Net-(FLUXL72-Pad1)")
    (add_net "Net-(FLUXL73-Pad1)")
    (add_net "Net-(FLUXL74-Pad1)")
    (add_net "Net-(FLUXL75-Pad1)")
    (add_net "Net-(FLUXL76-Pad1)")
    (add_net "Net-(FLUXL77-Pad1)")
    (add_net "Net-(FLUXL78-Pad1)")
    (add_net "Net-(FLUXL79-Pad1)")
    (add_net "Net-(FLUXL8-Pad1)")
    (add_net "Net-(FLUXL80-Pad1)")
    (add_net "Net-(FLUXL81-Pad1)")
    (add_net "Net-(FLUXL82-Pad1)")
    (add_net "Net-(FLUXL83-Pad1)")
    (add_net "Net-(FLUXL84-Pad1)")
    (add_net "Net-(FLUXL85-Pad1)")
    (add_net "Net-(FLUXL86-Pad1)")
    (add_net "Net-(FLUXL87-Pad1)")
    (add_net "Net-(FLUXL88-Pad1)")
    (add_net "Net-(FLUXL89-Pad1)")
    (add_net "Net-(FLUXL9-Pad1)")
    (add_net "Net-(FLUXL90-Pad1)")
    (add_net "Net-(FLUXL91-Pad1)")
    (add_net "Net-(FLUXL92-Pad1)")
    (add_net "Net-(FLUXL93-Pad1)")
    (add_net "Net-(FLUXL94-Pad1)")
    (add_net "Net-(FLUXL95-Pad1)")
    (add_net "Net-(FLUXL96-Pad1)")
    (add_net "Net-(FLUXL97-Pad1)")
    (add_net "Net-(FLUXL98-Pad1)")
    (add_net "Net-(FLUXL99-Pad1)")
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 87.875)
    (fp_text reference FLUXL256 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 256 "Net-(FLUXL256-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 256 "Net-(FLUXL256-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 85.125)
    (fp_text reference FLUXL255 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 255 "Net-(FLUXL255-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 255 "Net-(FLUXL255-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 82.375)
    (fp_text reference FLUXL254 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 254 "Net-(FLUXL254-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 254 "Net-(FLUXL254-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 79.625)
    (fp_text reference FLUXL253 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 253 "Net-(FLUXL253-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 253 "Net-(FLUXL253-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 79.625)
    (fp_text reference FLUXL252 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 252 "Net-(FLUXL252-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 252 "Net-(FLUXL252-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 76.875)
    (fp_text reference FLUXL251 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 251 "Net-(FLUXL251-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 251 "Net-(FLUXL251-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 76.875)
    (fp_text reference FLUXL250 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 250 "Net-(FLUXL250-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 250 "Net-(FLUXL250-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 76.875)
    (fp_text reference FLUXL249 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 249 "Net-(FLUXL249-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 249 "Net-(FLUXL249-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 74.125)
    (fp_text reference FLUXL248 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 248 "Net-(FLUXL248-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 248 "Net-(FLUXL248-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 74.125)
    (fp_text reference FLUXL247 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 247 "Net-(FLUXL247-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 247 "Net-(FLUXL247-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 74.125)
    (fp_text reference FLUXL246 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 246 "Net-(FLUXL246-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 246 "Net-(FLUXL246-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 71.375)
    (fp_text reference FLUXL245 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 245 "Net-(FLUXL245-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 245 "Net-(FLUXL245-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 71.375)
    (fp_text reference FLUXL244 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 244 "Net-(FLUXL244-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 244 "Net-(FLUXL244-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 71.375)
    (fp_text reference FLUXL243 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 243 "Net-(FLUXL243-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 243 "Net-(FLUXL243-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 68.625)
    (fp_text reference FLUXL242 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 242 "Net-(FLUXL242-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 242 "Net-(FLUXL242-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 68.625)
    (fp_text reference FLUXL241 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 241 "Net-(FLUXL241-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 241 "Net-(FLUXL241-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 68.625)
    (fp_text reference FLUXL240 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 240 "Net-(FLUXL240-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 240 "Net-(FLUXL240-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 68.625)
    (fp_text reference FLUXL239 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 239 "Net-(FLUXL239-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 239 "Net-(FLUXL239-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 65.875)
    (fp_text reference FLUXL238 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 238 "Net-(FLUXL238-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 238 "Net-(FLUXL238-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 65.875)
    (fp_text reference FLUXL237 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 237 "Net-(FLUXL237-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 237 "Net-(FLUXL237-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 65.875)
    (fp_text reference FLUXL236 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 236 "Net-(FLUXL236-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 236 "Net-(FLUXL236-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 65.875)
    (fp_text reference FLUXL235 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 235 "Net-(FLUXL235-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 235 "Net-(FLUXL235-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 63.125)
    (fp_text reference FLUXL234 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 234 "Net-(FLUXL234-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 234 "Net-(FLUXL234-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 63.125)
    (fp_text reference FLUXL233 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 233 "Net-(FLUXL233-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 233 "Net-(FLUXL233-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 63.125)
    (fp_text reference FLUXL232 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 232 "Net-(FLUXL232-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 232 "Net-(FLUXL232-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 60.375)
    (fp_text reference FLUXL231 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 231 "Net-(FLUXL231-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 231 "Net-(FLUXL231-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 60.375)
    (fp_text reference FLUXL230 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 230 "Net-(FLUXL230-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 230 "Net-(FLUXL230-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 57.625)
    (fp_text reference FLUXL229 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 229 "Net-(FLUXL229-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 229 "Net-(FLUXL229-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 57.625)
    (fp_text reference FLUXL228 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 228 "Net-(FLUXL228-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 228 "Net-(FLUXL228-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 54.875)
    (fp_text reference FLUXL227 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 227 "Net-(FLUXL227-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 227 "Net-(FLUXL227-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 54.875)
    (fp_text reference FLUXL226 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 226 "Net-(FLUXL226-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 226 "Net-(FLUXL226-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 52.125)
    (fp_text reference FLUXL225 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 225 "Net-(FLUXL225-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 225 "Net-(FLUXL225-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 85.125)
    (fp_text reference FLUXL224 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 224 "Net-(FLUXL224-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 224 "Net-(FLUXL224-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 82.375)
    (fp_text reference FLUXL223 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 223 "Net-(FLUXL223-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 223 "Net-(FLUXL223-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 82.375)
    (fp_text reference FLUXL222 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 222 "Net-(FLUXL222-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 222 "Net-(FLUXL222-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 79.625)
    (fp_text reference FLUXL221 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 221 "Net-(FLUXL221-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 221 "Net-(FLUXL221-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 79.625)
    (fp_text reference FLUXL220 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 220 "Net-(FLUXL220-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 220 "Net-(FLUXL220-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 76.875)
    (fp_text reference FLUXL219 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 219 "Net-(FLUXL219-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 219 "Net-(FLUXL219-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 76.875)
    (fp_text reference FLUXL218 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 218 "Net-(FLUXL218-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 218 "Net-(FLUXL218-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 74.125)
    (fp_text reference FLUXL217 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 217 "Net-(FLUXL217-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 217 "Net-(FLUXL217-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 74.125)
    (fp_text reference FLUXL216 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 216 "Net-(FLUXL216-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 216 "Net-(FLUXL216-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 74.125)
    (fp_text reference FLUXL215 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 215 "Net-(FLUXL215-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 215 "Net-(FLUXL215-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 71.375)
    (fp_text reference FLUXL214 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 214 "Net-(FLUXL214-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 214 "Net-(FLUXL214-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 71.375)
    (fp_text reference FLUXL213 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 213 "Net-(FLUXL213-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 213 "Net-(FLUXL213-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 71.375)
    (fp_text reference FLUXL212 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 212 "Net-(FLUXL212-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 212 "Net-(FLUXL212-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 71.375)
    (fp_text reference FLUXL211 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 211 "Net-(FLUXL211-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 211 "Net-(FLUXL211-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 68.625)
    (fp_text reference FLUXL210 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 210 "Net-(FLUXL210-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 210 "Net-(FLUXL210-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 68.625)
    (fp_text reference FLUXL209 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 209 "Net-(FLUXL209-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 209 "Net-(FLUXL209-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 68.625)
    (fp_text reference FLUXL208 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 208 "Net-(FLUXL208-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 208 "Net-(FLUXL208-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 68.625)
    (fp_text reference FLUXL207 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 207 "Net-(FLUXL207-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 207 "Net-(FLUXL207-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 65.875)
    (fp_text reference FLUXL206 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 206 "Net-(FLUXL206-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 206 "Net-(FLUXL206-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 65.875)
    (fp_text reference FLUXL205 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 205 "Net-(FLUXL205-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 205 "Net-(FLUXL205-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 65.875)
    (fp_text reference FLUXL204 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 204 "Net-(FLUXL204-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 204 "Net-(FLUXL204-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 63.125)
    (fp_text reference FLUXL203 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 203 "Net-(FLUXL203-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 203 "Net-(FLUXL203-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 63.125)
    (fp_text reference FLUXL202 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 202 "Net-(FLUXL202-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 202 "Net-(FLUXL202-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 63.125)
    (fp_text reference FLUXL201 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 201 "Net-(FLUXL201-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 201 "Net-(FLUXL201-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 60.375)
    (fp_text reference FLUXL200 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 200 "Net-(FLUXL200-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 200 "Net-(FLUXL200-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 60.375)
    (fp_text reference FLUXL199 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 199 "Net-(FLUXL199-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 199 "Net-(FLUXL199-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 60.375)
    (fp_text reference FLUXL198 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 198 "Net-(FLUXL198-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 198 "Net-(FLUXL198-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 57.625)
    (fp_text reference FLUXL197 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 197 "Net-(FLUXL197-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 197 "Net-(FLUXL197-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 57.625)
    (fp_text reference FLUXL196 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 196 "Net-(FLUXL196-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 196 "Net-(FLUXL196-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 54.875)
    (fp_text reference FLUXL195 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 195 "Net-(FLUXL195-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 195 "Net-(FLUXL195-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 52.125)
    (fp_text reference FLUXL194 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 194 "Net-(FLUXL194-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 194 "Net-(FLUXL194-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 49.375)
    (fp_text reference FLUXL193 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 193 "Net-(FLUXL193-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 193 "Net-(FLUXL193-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 49.375)
    (fp_text reference FLUXL192 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 192 "Net-(FLUXL192-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 192 "Net-(FLUXL192-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 52.125)
    (fp_text reference FLUXL191 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 191 "Net-(FLUXL191-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 191 "Net-(FLUXL191-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 52.125)
    (fp_text reference FLUXL190 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 190 "Net-(FLUXL190-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 190 "Net-(FLUXL190-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 49.375)
    (fp_text reference FLUXL189 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 189 "Net-(FLUXL189-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 189 "Net-(FLUXL189-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 54.875)
    (fp_text reference FLUXL188 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 188 "Net-(FLUXL188-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 188 "Net-(FLUXL188-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 49.375)
    (fp_text reference FLUXL187 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 187 "Net-(FLUXL187-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 187 "Net-(FLUXL187-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 54.875)
    (fp_text reference FLUXL186 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 186 "Net-(FLUXL186-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 186 "Net-(FLUXL186-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 60.375)
    (fp_text reference FLUXL185 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 185 "Net-(FLUXL185-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 185 "Net-(FLUXL185-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 52.125)
    (fp_text reference FLUXL184 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 184 "Net-(FLUXL184-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 184 "Net-(FLUXL184-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 57.625)
    (fp_text reference FLUXL183 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 183 "Net-(FLUXL183-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 183 "Net-(FLUXL183-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 63.125)
    (fp_text reference FLUXL182 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 182 "Net-(FLUXL182-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 182 "Net-(FLUXL182-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 52.125)
    (fp_text reference FLUXL181 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 181 "Net-(FLUXL181-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 181 "Net-(FLUXL181-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 57.625)
    (fp_text reference FLUXL180 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 180 "Net-(FLUXL180-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 180 "Net-(FLUXL180-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 63.125)
    (fp_text reference FLUXL179 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 179 "Net-(FLUXL179-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 179 "Net-(FLUXL179-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 49.375)
    (fp_text reference FLUXL178 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 178 "Net-(FLUXL178-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 178 "Net-(FLUXL178-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 54.875)
    (fp_text reference FLUXL177 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 177 "Net-(FLUXL177-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 177 "Net-(FLUXL177-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 60.375)
    (fp_text reference FLUXL176 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 176 "Net-(FLUXL176-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 176 "Net-(FLUXL176-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 65.875)
    (fp_text reference FLUXL175 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 175 "Net-(FLUXL175-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 175 "Net-(FLUXL175-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 49.375)
    (fp_text reference FLUXL174 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 174 "Net-(FLUXL174-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 174 "Net-(FLUXL174-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 54.875)
    (fp_text reference FLUXL173 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 173 "Net-(FLUXL173-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 173 "Net-(FLUXL173-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 60.375)
    (fp_text reference FLUXL172 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 172 "Net-(FLUXL172-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 172 "Net-(FLUXL172-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 65.875)
    (fp_text reference FLUXL171 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 171 "Net-(FLUXL171-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 171 "Net-(FLUXL171-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 52.125)
    (fp_text reference FLUXL170 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 170 "Net-(FLUXL170-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 170 "Net-(FLUXL170-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 57.625)
    (fp_text reference FLUXL169 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 169 "Net-(FLUXL169-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 169 "Net-(FLUXL169-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 63.125)
    (fp_text reference FLUXL168 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 168 "Net-(FLUXL168-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 168 "Net-(FLUXL168-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 52.125)
    (fp_text reference FLUXL167 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 167 "Net-(FLUXL167-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 167 "Net-(FLUXL167-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 57.625)
    (fp_text reference FLUXL166 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 166 "Net-(FLUXL166-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 166 "Net-(FLUXL166-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 49.375)
    (fp_text reference FLUXL165 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 165 "Net-(FLUXL165-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 165 "Net-(FLUXL165-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 54.875)
    (fp_text reference FLUXL164 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 164 "Net-(FLUXL164-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 164 "Net-(FLUXL164-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 49.375)
    (fp_text reference FLUXL163 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 163 "Net-(FLUXL163-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 163 "Net-(FLUXL163-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 54.875)
    (fp_text reference FLUXL162 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 162 "Net-(FLUXL162-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 162 "Net-(FLUXL162-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 52.125)
    (fp_text reference FLUXL161 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 161 "Net-(FLUXL161-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 161 "Net-(FLUXL161-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 49.375)
    (fp_text reference FLUXL160 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 160 "Net-(FLUXL160-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 160 "Net-(FLUXL160-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 49.375)
    (fp_text reference FLUXL159 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 159 "Net-(FLUXL159-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 159 "Net-(FLUXL159-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 54.875)
    (fp_text reference FLUXL158 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 158 "Net-(FLUXL158-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 158 "Net-(FLUXL158-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 52.125)
    (fp_text reference FLUXL157 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 157 "Net-(FLUXL157-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 157 "Net-(FLUXL157-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 57.625)
    (fp_text reference FLUXL156 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 156 "Net-(FLUXL156-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 156 "Net-(FLUXL156-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 52.125)
    (fp_text reference FLUXL155 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 155 "Net-(FLUXL155-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 155 "Net-(FLUXL155-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 57.625)
    (fp_text reference FLUXL154 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 154 "Net-(FLUXL154-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 154 "Net-(FLUXL154-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 49.375)
    (fp_text reference FLUXL153 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 153 "Net-(FLUXL153-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 153 "Net-(FLUXL153-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 54.875)
    (fp_text reference FLUXL152 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 152 "Net-(FLUXL152-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 152 "Net-(FLUXL152-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 60.375)
    (fp_text reference FLUXL151 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 151 "Net-(FLUXL151-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 151 "Net-(FLUXL151-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 49.375)
    (fp_text reference FLUXL150 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 150 "Net-(FLUXL150-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 150 "Net-(FLUXL150-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 54.875)
    (fp_text reference FLUXL149 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 149 "Net-(FLUXL149-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 149 "Net-(FLUXL149-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 60.375)
    (fp_text reference FLUXL148 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 148 "Net-(FLUXL148-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 148 "Net-(FLUXL148-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 65.875)
    (fp_text reference FLUXL147 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 147 "Net-(FLUXL147-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 147 "Net-(FLUXL147-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 52.125)
    (fp_text reference FLUXL146 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 146 "Net-(FLUXL146-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 146 "Net-(FLUXL146-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 57.625)
    (fp_text reference FLUXL145 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 145 "Net-(FLUXL145-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 145 "Net-(FLUXL145-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 63.125)
    (fp_text reference FLUXL144 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 144 "Net-(FLUXL144-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 144 "Net-(FLUXL144-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 68.625)
    (fp_text reference FLUXL143 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 143 "Net-(FLUXL143-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 143 "Net-(FLUXL143-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 52.125)
    (fp_text reference FLUXL142 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 142 "Net-(FLUXL142-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 142 "Net-(FLUXL142-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 57.625)
    (fp_text reference FLUXL141 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 141 "Net-(FLUXL141-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 141 "Net-(FLUXL141-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 63.125)
    (fp_text reference FLUXL140 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 140 "Net-(FLUXL140-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 140 "Net-(FLUXL140-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 49.375)
    (fp_text reference FLUXL139 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 139 "Net-(FLUXL139-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 139 "Net-(FLUXL139-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 54.875)
    (fp_text reference FLUXL138 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 138 "Net-(FLUXL138-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 138 "Net-(FLUXL138-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 60.375)
    (fp_text reference FLUXL137 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 137 "Net-(FLUXL137-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 137 "Net-(FLUXL137-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 49.375)
    (fp_text reference FLUXL136 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 136 "Net-(FLUXL136-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 136 "Net-(FLUXL136-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 54.875)
    (fp_text reference FLUXL135 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 135 "Net-(FLUXL135-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 135 "Net-(FLUXL135-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 60.375)
    (fp_text reference FLUXL134 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 134 "Net-(FLUXL134-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 134 "Net-(FLUXL134-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 52.125)
    (fp_text reference FLUXL133 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 133 "Net-(FLUXL133-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 133 "Net-(FLUXL133-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 57.625)
    (fp_text reference FLUXL132 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 132 "Net-(FLUXL132-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 132 "Net-(FLUXL132-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 52.125)
    (fp_text reference FLUXL131 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 131 "Net-(FLUXL131-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 131 "Net-(FLUXL131-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 49.375)
    (fp_text reference FLUXL130 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 130 "Net-(FLUXL130-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 130 "Net-(FLUXL130-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 49.375)
    (fp_text reference FLUXL129 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 129 "Net-(FLUXL129-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 129 "Net-(FLUXL129-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 90.625)
    (fp_text reference FLUXL128 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 128 "Net-(FLUXL128-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 128 "Net-(FLUXL128-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 87.875)
    (fp_text reference FLUXL127 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 127 "Net-(FLUXL127-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 127 "Net-(FLUXL127-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 87.875)
    (fp_text reference FLUXL126 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 126 "Net-(FLUXL126-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 126 "Net-(FLUXL126-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 90.625)
    (fp_text reference FLUXL125 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 125 "Net-(FLUXL125-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 125 "Net-(FLUXL125-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 85.125)
    (fp_text reference FLUXL124 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 124 "Net-(FLUXL124-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 124 "Net-(FLUXL124-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 90.625)
    (fp_text reference FLUXL123 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 123 "Net-(FLUXL123-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 123 "Net-(FLUXL123-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 85.125)
    (fp_text reference FLUXL122 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 122 "Net-(FLUXL122-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 122 "Net-(FLUXL122-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 79.625)
    (fp_text reference FLUXL121 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 121 "Net-(FLUXL121-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(FLUXL121-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 87.875)
    (fp_text reference FLUXL120 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 120 "Net-(FLUXL120-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 120 "Net-(FLUXL120-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 82.375)
    (fp_text reference FLUXL119 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 119 "Net-(FLUXL119-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 119 "Net-(FLUXL119-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 76.875)
    (fp_text reference FLUXL118 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 118 "Net-(FLUXL118-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 118 "Net-(FLUXL118-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 87.875)
    (fp_text reference FLUXL117 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 117 "Net-(FLUXL117-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 117 "Net-(FLUXL117-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 82.375)
    (fp_text reference FLUXL116 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 116 "Net-(FLUXL116-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(FLUXL116-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 76.875)
    (fp_text reference FLUXL115 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 115 "Net-(FLUXL115-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(FLUXL115-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 90.625)
    (fp_text reference FLUXL114 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 114 "Net-(FLUXL114-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(FLUXL114-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 85.125)
    (fp_text reference FLUXL113 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 113 "Net-(FLUXL113-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(FLUXL113-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 79.625)
    (fp_text reference FLUXL112 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 112 "Net-(FLUXL112-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(FLUXL112-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 74.125)
    (fp_text reference FLUXL111 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 111 "Net-(FLUXL111-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(FLUXL111-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 90.625)
    (fp_text reference FLUXL110 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 110 "Net-(FLUXL110-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(FLUXL110-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 85.125)
    (fp_text reference FLUXL109 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 109 "Net-(FLUXL109-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(FLUXL109-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 79.625)
    (fp_text reference FLUXL108 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 108 "Net-(FLUXL108-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(FLUXL108-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 74.125)
    (fp_text reference FLUXL107 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 107 "Net-(FLUXL107-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(FLUXL107-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 87.875)
    (fp_text reference FLUXL106 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 106 "Net-(FLUXL106-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(FLUXL106-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 82.375)
    (fp_text reference FLUXL105 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 105 "Net-(FLUXL105-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(FLUXL105-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 76.875)
    (fp_text reference FLUXL104 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 104 "Net-(FLUXL104-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(FLUXL104-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 87.875)
    (fp_text reference FLUXL103 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 103 "Net-(FLUXL103-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(FLUXL103-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 82.375)
    (fp_text reference FLUXL102 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 102 "Net-(FLUXL102-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(FLUXL102-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 90.625)
    (fp_text reference FLUXL101 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 101 "Net-(FLUXL101-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(FLUXL101-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 85.125)
    (fp_text reference FLUXL100 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 100 "Net-(FLUXL100-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(FLUXL100-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 90.625)
    (fp_text reference FLUXL99 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 99 "Net-(FLUXL99-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(FLUXL99-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 85.125)
    (fp_text reference FLUXL98 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 98 "Net-(FLUXL98-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(FLUXL98-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 87.875)
    (fp_text reference FLUXL97 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 97 "Net-(FLUXL97-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 97 "Net-(FLUXL97-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 90.625)
    (fp_text reference FLUXL96 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 96 "Net-(FLUXL96-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(FLUXL96-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 90.625)
    (fp_text reference FLUXL95 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 95 "Net-(FLUXL95-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 95 "Net-(FLUXL95-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 85.125)
    (fp_text reference FLUXL94 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 94 "Net-(FLUXL94-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(FLUXL94-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 87.875)
    (fp_text reference FLUXL93 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 93 "Net-(FLUXL93-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(FLUXL93-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 82.375)
    (fp_text reference FLUXL92 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 92 "Net-(FLUXL92-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(FLUXL92-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 87.875)
    (fp_text reference FLUXL91 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 91 "Net-(FLUXL91-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(FLUXL91-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 82.375)
    (fp_text reference FLUXL90 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 90 "Net-(FLUXL90-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(FLUXL90-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 90.625)
    (fp_text reference FLUXL89 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 89 "Net-(FLUXL89-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(FLUXL89-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 85.125)
    (fp_text reference FLUXL88 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 88 "Net-(FLUXL88-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(FLUXL88-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 79.625)
    (fp_text reference FLUXL87 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 87 "Net-(FLUXL87-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(FLUXL87-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 90.625)
    (fp_text reference FLUXL86 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 86 "Net-(FLUXL86-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(FLUXL86-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 85.125)
    (fp_text reference FLUXL85 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 85 "Net-(FLUXL85-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(FLUXL85-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 79.625)
    (fp_text reference FLUXL84 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 84 "Net-(FLUXL84-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(FLUXL84-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 74.125)
    (fp_text reference FLUXL83 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 83 "Net-(FLUXL83-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(FLUXL83-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 87.875)
    (fp_text reference FLUXL82 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 82 "Net-(FLUXL82-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(FLUXL82-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 82.375)
    (fp_text reference FLUXL81 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 81 "Net-(FLUXL81-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(FLUXL81-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 76.875)
    (fp_text reference FLUXL80 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 80 "Net-(FLUXL80-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(FLUXL80-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 68.625 71.375)
    (fp_text reference FLUXL79 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 79 "Net-(FLUXL79-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(FLUXL79-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 87.875)
    (fp_text reference FLUXL78 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 78 "Net-(FLUXL78-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(FLUXL78-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 82.375)
    (fp_text reference FLUXL77 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 77 "Net-(FLUXL77-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(FLUXL77-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 65.875 76.875)
    (fp_text reference FLUXL76 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 76 "Net-(FLUXL76-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(FLUXL76-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 90.625)
    (fp_text reference FLUXL75 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 75 "Net-(FLUXL75-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(FLUXL75-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 85.125)
    (fp_text reference FLUXL74 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 74 "Net-(FLUXL74-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(FLUXL74-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 63.125 79.625)
    (fp_text reference FLUXL73 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 73 "Net-(FLUXL73-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(FLUXL73-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 90.625)
    (fp_text reference FLUXL72 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 72 "Net-(FLUXL72-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(FLUXL72-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 85.125)
    (fp_text reference FLUXL71 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 71 "Net-(FLUXL71-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(FLUXL71-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 60.375 79.625)
    (fp_text reference FLUXL70 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 70 "Net-(FLUXL70-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(FLUXL70-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 87.875)
    (fp_text reference FLUXL69 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 69 "Net-(FLUXL69-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(FLUXL69-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 57.625 82.375)
    (fp_text reference FLUXL68 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 68 "Net-(FLUXL68-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(FLUXL68-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 54.875 87.875)
    (fp_text reference FLUXL67 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 67 "Net-(FLUXL67-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(FLUXL67-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 52.125 90.625)
    (fp_text reference FLUXL66 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 66 "Net-(FLUXL66-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(FLUXL66-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 49.375 90.625)
    (fp_text reference FLUXL65 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 65 "Net-(FLUXL65-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(FLUXL65-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 52.125)
    (fp_text reference FLUXL64 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 64 "Net-(FLUXL64-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(FLUXL64-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 54.875)
    (fp_text reference FLUXL63 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 63 "Net-(FLUXL63-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(FLUXL63-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 57.625)
    (fp_text reference FLUXL62 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 62 "Net-(FLUXL62-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(FLUXL62-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 60.375)
    (fp_text reference FLUXL61 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 61 "Net-(FLUXL61-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(FLUXL61-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 60.375)
    (fp_text reference FLUXL60 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 60 "Net-(FLUXL60-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(FLUXL60-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 63.125)
    (fp_text reference FLUXL59 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 59 "Net-(FLUXL59-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(FLUXL59-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 63.125)
    (fp_text reference FLUXL58 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 58 "Net-(FLUXL58-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(FLUXL58-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 63.125)
    (fp_text reference FLUXL57 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 57 "Net-(FLUXL57-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(FLUXL57-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 65.875)
    (fp_text reference FLUXL56 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 56 "Net-(FLUXL56-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(FLUXL56-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 65.875)
    (fp_text reference FLUXL55 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 55 "Net-(FLUXL55-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(FLUXL55-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 65.875)
    (fp_text reference FLUXL54 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 54 "Net-(FLUXL54-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(FLUXL54-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 68.625)
    (fp_text reference FLUXL53 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 53 "Net-(FLUXL53-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(FLUXL53-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 68.625)
    (fp_text reference FLUXL52 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 52 "Net-(FLUXL52-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(FLUXL52-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 68.625)
    (fp_text reference FLUXL51 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 51 "Net-(FLUXL51-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(FLUXL51-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 71.375)
    (fp_text reference FLUXL50 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 50 "Net-(FLUXL50-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(FLUXL50-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 71.375)
    (fp_text reference FLUXL49 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 49 "Net-(FLUXL49-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(FLUXL49-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 71.375)
    (fp_text reference FLUXL48 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 48 "Net-(FLUXL48-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(FLUXL48-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 71.375)
    (fp_text reference FLUXL47 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 47 "Net-(FLUXL47-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(FLUXL47-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 74.125)
    (fp_text reference FLUXL46 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 46 "Net-(FLUXL46-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(FLUXL46-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 74.125)
    (fp_text reference FLUXL45 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 45 "Net-(FLUXL45-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(FLUXL45-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 74.125)
    (fp_text reference FLUXL44 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 44 "Net-(FLUXL44-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(FLUXL44-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 74.125)
    (fp_text reference FLUXL43 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 43 "Net-(FLUXL43-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(FLUXL43-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 76.875)
    (fp_text reference FLUXL42 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 42 "Net-(FLUXL42-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(FLUXL42-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 76.875)
    (fp_text reference FLUXL41 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 41 "Net-(FLUXL41-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(FLUXL41-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 76.875)
    (fp_text reference FLUXL40 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 40 "Net-(FLUXL40-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(FLUXL40-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 79.625)
    (fp_text reference FLUXL39 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 39 "Net-(FLUXL39-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(FLUXL39-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 79.625)
    (fp_text reference FLUXL38 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 38 "Net-(FLUXL38-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(FLUXL38-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 82.375)
    (fp_text reference FLUXL37 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 37 "Net-(FLUXL37-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(FLUXL37-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 82.375)
    (fp_text reference FLUXL36 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 36 "Net-(FLUXL36-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(FLUXL36-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 85.125)
    (fp_text reference FLUXL35 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 35 "Net-(FLUXL35-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(FLUXL35-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 85.125)
    (fp_text reference FLUXL34 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 34 "Net-(FLUXL34-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(FLUXL34-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 87.875)
    (fp_text reference FLUXL33 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 33 "Net-(FLUXL33-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(FLUXL33-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 54.875)
    (fp_text reference FLUXL32 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 32 "Net-(FLUXL32-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(FLUXL32-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 57.625)
    (fp_text reference FLUXL31 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 31 "Net-(FLUXL31-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(FLUXL31-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 57.625)
    (fp_text reference FLUXL30 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 30 "Net-(FLUXL30-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(FLUXL30-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 60.375)
    (fp_text reference FLUXL29 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 29 "Net-(FLUXL29-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(FLUXL29-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 60.375)
    (fp_text reference FLUXL28 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 28 "Net-(FLUXL28-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(FLUXL28-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 63.125)
    (fp_text reference FLUXL27 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 27 "Net-(FLUXL27-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(FLUXL27-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 63.125)
    (fp_text reference FLUXL26 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 26 "Net-(FLUXL26-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(FLUXL26-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 65.875)
    (fp_text reference FLUXL25 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 25 "Net-(FLUXL25-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(FLUXL25-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 65.875)
    (fp_text reference FLUXL24 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 24 "Net-(FLUXL24-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(FLUXL24-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 65.875)
    (fp_text reference FLUXL23 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 23 "Net-(FLUXL23-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(FLUXL23-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 68.625)
    (fp_text reference FLUXL22 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 22 "Net-(FLUXL22-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(FLUXL22-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 68.625)
    (fp_text reference FLUXL21 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 21 "Net-(FLUXL21-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(FLUXL21-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 68.625)
    (fp_text reference FLUXL20 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 20 "Net-(FLUXL20-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(FLUXL20-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 74.125 68.625)
    (fp_text reference FLUXL19 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 19 "Net-(FLUXL19-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(FLUXL19-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 71.375)
    (fp_text reference FLUXL18 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 18 "Net-(FLUXL18-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(FLUXL18-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 71.375)
    (fp_text reference FLUXL17 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 17 "Net-(FLUXL17-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(FLUXL17-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 71.375)
    (fp_text reference FLUXL16 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 16 "Net-(FLUXL16-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(FLUXL16-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 71.375 71.375)
    (fp_text reference FLUXL15 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 15 "Net-(FLUXL15-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(FLUXL15-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 74.125)
    (fp_text reference FLUXL14 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 14 "Net-(FLUXL14-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(FLUXL14-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 74.125)
    (fp_text reference FLUXL13 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 13 "Net-(FLUXL13-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(FLUXL13-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 76.875 74.125)
    (fp_text reference FLUXL12 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 12 "Net-(FLUXL12-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(FLUXL12-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 76.875)
    (fp_text reference FLUXL11 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 11 "Net-(FLUXL11-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(FLUXL11-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 76.875)
    (fp_text reference FLUXL10 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 10 "Net-(FLUXL10-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(FLUXL10-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 76.875)
    (fp_text reference FLUXL9 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 9 "Net-(FLUXL9-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(FLUXL9-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 79.625)
    (fp_text reference FLUXL8 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 8 "Net-(FLUXL8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(FLUXL8-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 85.125 79.625)
    (fp_text reference FLUXL7 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 7 "Net-(FLUXL7-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(FLUXL7-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 79.625 79.625)
    (fp_text reference FLUXL6 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 6 "Net-(FLUXL6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(FLUXL6-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 82.375)
    (fp_text reference FLUXL5 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 5 "Net-(FLUXL5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(FLUXL5-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 82.375 82.375)
    (fp_text reference FLUXL4 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 4 "Net-(FLUXL4-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(FLUXL4-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 87.875 85.125)
    (fp_text reference FLUXL3 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 3 "Net-(FLUXL3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(FLUXL3-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 87.875)
    (fp_text reference FLUXL2 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 2 "Net-(FLUXL2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(FLUXL2-Pad1)"))
  )
  (module GaudiLabsFootPrints:FLUXPAD_2_75_4MIL_4_5 (layer F.Cu) (tedit 57332E01)
    (at 90.625 90.625)
    (fp_text reference FLUXL1 (at 0.49 2.21) (layer F.SilkS) hide)
    (fp_text value FX (at 1.14 -2.07) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.27 2.27) (drill 0.3) (layers F.Cu F.SilkS F.Mask)
      (net 1 "Net-(FLUXL1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 0.6048 0.6048) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(FLUXL1-Pad1)"))
  )
  (module Malu:Pin_Header_Straight_2x32_TH locked (layer B.Cu) (tedit 0)
    (at 70 116 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -1.27 44.47 270) (layer B.SilkS))
    (fp_text value CONN_02X32 (at -1.27 42.47 270) (layer B.Fab))
    (pad 1 thru_hole rect (at -1.27 39.37 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 65 "Net-(FLUXL65-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 39.37 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 97 "Net-(FLUXL97-Pad1)"))
    (pad 3 thru_hole oval (at -1.27 36.83 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 66 "Net-(FLUXL66-Pad1)"))
    (pad 4 thru_hole oval (at 1.27 36.83 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 98 "Net-(FLUXL98-Pad1)"))
    (pad 5 thru_hole oval (at -1.27 34.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 67 "Net-(FLUXL67-Pad1)"))
    (pad 6 thru_hole oval (at 1.27 34.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 99 "Net-(FLUXL99-Pad1)"))
    (pad 7 thru_hole oval (at -1.27 31.75 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 68 "Net-(FLUXL68-Pad1)"))
    (pad 8 thru_hole oval (at 1.27 31.75 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 100 "Net-(FLUXL100-Pad1)"))
    (pad 9 thru_hole oval (at -1.27 29.21 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 69 "Net-(FLUXL69-Pad1)"))
    (pad 10 thru_hole oval (at 1.27 29.21 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 101 "Net-(FLUXL101-Pad1)"))
    (pad 11 thru_hole oval (at -1.27 26.67 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 70 "Net-(FLUXL70-Pad1)"))
    (pad 12 thru_hole oval (at 1.27 26.67 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 102 "Net-(FLUXL102-Pad1)"))
    (pad 13 thru_hole oval (at -1.27 24.13 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 71 "Net-(FLUXL71-Pad1)"))
    (pad 14 thru_hole oval (at 1.27 24.13 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 103 "Net-(FLUXL103-Pad1)"))
    (pad 15 thru_hole oval (at -1.27 21.59 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 72 "Net-(FLUXL72-Pad1)"))
    (pad 16 thru_hole oval (at 1.27 21.59 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 104 "Net-(FLUXL104-Pad1)"))
    (pad 17 thru_hole oval (at -1.27 19.05 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 73 "Net-(FLUXL73-Pad1)"))
    (pad 18 thru_hole oval (at 1.27 19.05 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 105 "Net-(FLUXL105-Pad1)"))
    (pad 19 thru_hole oval (at -1.27 16.51 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 74 "Net-(FLUXL74-Pad1)"))
    (pad 20 thru_hole oval (at 1.27 16.51 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 106 "Net-(FLUXL106-Pad1)"))
    (pad 21 thru_hole oval (at -1.27 13.97 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 75 "Net-(FLUXL75-Pad1)"))
    (pad 22 thru_hole oval (at 1.27 13.97 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 107 "Net-(FLUXL107-Pad1)"))
    (pad 23 thru_hole oval (at -1.27 11.43 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 76 "Net-(FLUXL76-Pad1)"))
    (pad 24 thru_hole oval (at 1.27 11.43 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 108 "Net-(FLUXL108-Pad1)"))
    (pad 25 thru_hole oval (at -1.27 8.89 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 77 "Net-(FLUXL77-Pad1)"))
    (pad 26 thru_hole oval (at 1.27 8.89 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 109 "Net-(FLUXL109-Pad1)"))
    (pad 27 thru_hole oval (at -1.27 6.35 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 78 "Net-(FLUXL78-Pad1)"))
    (pad 28 thru_hole oval (at 1.27 6.35 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 110 "Net-(FLUXL110-Pad1)"))
    (pad 29 thru_hole oval (at -1.27 3.81 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 79 "Net-(FLUXL79-Pad1)"))
    (pad 30 thru_hole oval (at 1.27 3.81 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 111 "Net-(FLUXL111-Pad1)"))
    (pad 31 thru_hole oval (at -1.27 1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 80 "Net-(FLUXL80-Pad1)"))
    (pad 32 thru_hole oval (at 1.27 1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 112 "Net-(FLUXL112-Pad1)"))
    (pad 33 thru_hole oval (at -1.27 -1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 81 "Net-(FLUXL81-Pad1)"))
    (pad 34 thru_hole oval (at 1.27 -1.27 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 113 "Net-(FLUXL113-Pad1)"))
    (pad 35 thru_hole oval (at -1.27 -3.81 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 82 "Net-(FLUXL82-Pad1)"))
    (pad 36 thru_hole oval (at 1.27 -3.81 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 114 "Net-(FLUXL114-Pad1)"))
    (pad 37 thru_hole oval (at -1.27 -6.35 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 83 "Net-(FLUXL83-Pad1)"))
    (pad 38 thru_hole oval (at 1.27 -6.35 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 115 "Net-(FLUXL115-Pad1)"))
    (pad 39 thru_hole oval (at -1.27 -8.89 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 84 "Net-(FLUXL84-Pad1)"))
    (pad 40 thru_hole oval (at 1.27 -8.89 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 116 "Net-(FLUXL116-Pad1)"))
    (pad 41 thru_hole oval (at -1.27 -11.43 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 85 "Net-(FLUXL85-Pad1)"))
    (pad 42 thru_hole oval (at 1.27 -11.43 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 117 "Net-(FLUXL117-Pad1)"))
    (pad 43 thru_hole oval (at -1.27 -13.97 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 86 "Net-(FLUXL86-Pad1)"))
    (pad 44 thru_hole oval (at 1.27 -13.97 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 118 "Net-(FLUXL118-Pad1)"))
    (pad 45 thru_hole oval (at -1.27 -16.51 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 87 "Net-(FLUXL87-Pad1)"))
    (pad 46 thru_hole oval (at 1.27 -16.51 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 119 "Net-(FLUXL119-Pad1)"))
    (pad 47 thru_hole oval (at -1.27 -19.05 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 88 "Net-(FLUXL88-Pad1)"))
    (pad 48 thru_hole oval (at 1.27 -19.05 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 120 "Net-(FLUXL120-Pad1)"))
    (pad 49 thru_hole oval (at -1.27 -21.59 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 89 "Net-(FLUXL89-Pad1)"))
    (pad 50 thru_hole oval (at 1.27 -21.59 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 121 "Net-(FLUXL121-Pad1)"))
    (pad 51 thru_hole oval (at -1.27 -24.13 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 90 "Net-(FLUXL90-Pad1)"))
    (pad 52 thru_hole oval (at 1.27 -24.13 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 122 "Net-(FLUXL122-Pad1)"))
    (pad 53 thru_hole oval (at -1.27 -26.67 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 91 "Net-(FLUXL91-Pad1)"))
    (pad 54 thru_hole oval (at 1.27 -26.67 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 123 "Net-(FLUXL123-Pad1)"))
    (pad 55 thru_hole oval (at -1.27 -29.21 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 92 "Net-(FLUXL92-Pad1)"))
    (pad 56 thru_hole oval (at 1.27 -29.21 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 124 "Net-(FLUXL124-Pad1)"))
    (pad 57 thru_hole oval (at -1.27 -31.75 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 93 "Net-(FLUXL93-Pad1)"))
    (pad 58 thru_hole oval (at 1.27 -31.75 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 125 "Net-(FLUXL125-Pad1)"))
    (pad 59 thru_hole oval (at -1.27 -34.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 94 "Net-(FLUXL94-Pad1)"))
    (pad 60 thru_hole oval (at 1.27 -34.29 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 126 "Net-(FLUXL126-Pad1)"))
    (pad 61 thru_hole oval (at -1.27 -36.83 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 95 "Net-(FLUXL95-Pad1)"))
    (pad 62 thru_hole oval (at 1.27 -36.83 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 127 "Net-(FLUXL127-Pad1)"))
    (pad 63 thru_hole oval (at -1.27 -39.37 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 96 "Net-(FLUXL96-Pad1)"))
    (pad 64 thru_hole oval (at 1.27 -39.37 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 128 "Net-(FLUXL128-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x32.wrl
      (at (xyz 0.05 -1.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Malu:Pin_Header_Straight_2x32_TH locked (layer B.Cu) (tedit 0)
    (at 24 70 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at -1.27 44.47 180) (layer B.SilkS))
    (fp_text value CONN_02X32 (at -1.27 42.47 180) (layer B.Fab))
    (pad 1 thru_hole rect (at -1.27 39.37 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 193 "Net-(FLUXL193-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 39.37 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 225 "Net-(FLUXL225-Pad1)"))
    (pad 3 thru_hole oval (at -1.27 36.83 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 194 "Net-(FLUXL194-Pad1)"))
    (pad 4 thru_hole oval (at 1.27 36.83 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 226 "Net-(FLUXL226-Pad1)"))
    (pad 5 thru_hole oval (at -1.27 34.29 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 195 "Net-(FLUXL195-Pad1)"))
    (pad 6 thru_hole oval (at 1.27 34.29 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 227 "Net-(FLUXL227-Pad1)"))
    (pad 7 thru_hole oval (at -1.27 31.75 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 196 "Net-(FLUXL196-Pad1)"))
    (pad 8 thru_hole oval (at 1.27 31.75 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 228 "Net-(FLUXL228-Pad1)"))
    (pad 9 thru_hole oval (at -1.27 29.21 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 197 "Net-(FLUXL197-Pad1)"))
    (pad 10 thru_hole oval (at 1.27 29.21 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 229 "Net-(FLUXL229-Pad1)"))
    (pad 11 thru_hole oval (at -1.27 26.67 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 198 "Net-(FLUXL198-Pad1)"))
    (pad 12 thru_hole oval (at 1.27 26.67 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 230 "Net-(FLUXL230-Pad1)"))
    (pad 13 thru_hole oval (at -1.27 24.13 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 199 "Net-(FLUXL199-Pad1)"))
    (pad 14 thru_hole oval (at 1.27 24.13 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 231 "Net-(FLUXL231-Pad1)"))
    (pad 15 thru_hole oval (at -1.27 21.59 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 200 "Net-(FLUXL200-Pad1)"))
    (pad 16 thru_hole oval (at 1.27 21.59 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 232 "Net-(FLUXL232-Pad1)"))
    (pad 17 thru_hole oval (at -1.27 19.05 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 201 "Net-(FLUXL201-Pad1)"))
    (pad 18 thru_hole oval (at 1.27 19.05 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 233 "Net-(FLUXL233-Pad1)"))
    (pad 19 thru_hole oval (at -1.27 16.51 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 202 "Net-(FLUXL202-Pad1)"))
    (pad 20 thru_hole oval (at 1.27 16.51 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 234 "Net-(FLUXL234-Pad1)"))
    (pad 21 thru_hole oval (at -1.27 13.97 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 203 "Net-(FLUXL203-Pad1)"))
    (pad 22 thru_hole oval (at 1.27 13.97 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 235 "Net-(FLUXL235-Pad1)"))
    (pad 23 thru_hole oval (at -1.27 11.43 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 204 "Net-(FLUXL204-Pad1)"))
    (pad 24 thru_hole oval (at 1.27 11.43 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 236 "Net-(FLUXL236-Pad1)"))
    (pad 25 thru_hole oval (at -1.27 8.89 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 205 "Net-(FLUXL205-Pad1)"))
    (pad 26 thru_hole oval (at 1.27 8.89 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 237 "Net-(FLUXL237-Pad1)"))
    (pad 27 thru_hole oval (at -1.27 6.35 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 206 "Net-(FLUXL206-Pad1)"))
    (pad 28 thru_hole oval (at 1.27 6.35 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 238 "Net-(FLUXL238-Pad1)"))
    (pad 29 thru_hole oval (at -1.27 3.81 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 207 "Net-(FLUXL207-Pad1)"))
    (pad 30 thru_hole oval (at 1.27 3.81 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 239 "Net-(FLUXL239-Pad1)"))
    (pad 31 thru_hole oval (at -1.27 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 208 "Net-(FLUXL208-Pad1)"))
    (pad 32 thru_hole oval (at 1.27 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 240 "Net-(FLUXL240-Pad1)"))
    (pad 33 thru_hole oval (at -1.27 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 209 "Net-(FLUXL209-Pad1)"))
    (pad 34 thru_hole oval (at 1.27 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 241 "Net-(FLUXL241-Pad1)"))
    (pad 35 thru_hole oval (at -1.27 -3.81 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 210 "Net-(FLUXL210-Pad1)"))
    (pad 36 thru_hole oval (at 1.27 -3.81 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 242 "Net-(FLUXL242-Pad1)"))
    (pad 37 thru_hole oval (at -1.27 -6.35 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 211 "Net-(FLUXL211-Pad1)"))
    (pad 38 thru_hole oval (at 1.27 -6.35 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 243 "Net-(FLUXL243-Pad1)"))
    (pad 39 thru_hole oval (at -1.27 -8.89 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 212 "Net-(FLUXL212-Pad1)"))
    (pad 40 thru_hole oval (at 1.27 -8.89 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 244 "Net-(FLUXL244-Pad1)"))
    (pad 41 thru_hole oval (at -1.27 -11.43 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 213 "Net-(FLUXL213-Pad1)"))
    (pad 42 thru_hole oval (at 1.27 -11.43 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 245 "Net-(FLUXL245-Pad1)"))
    (pad 43 thru_hole oval (at -1.27 -13.97 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 214 "Net-(FLUXL214-Pad1)"))
    (pad 44 thru_hole oval (at 1.27 -13.97 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 246 "Net-(FLUXL246-Pad1)"))
    (pad 45 thru_hole oval (at -1.27 -16.51 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 215 "Net-(FLUXL215-Pad1)"))
    (pad 46 thru_hole oval (at 1.27 -16.51 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 247 "Net-(FLUXL247-Pad1)"))
    (pad 47 thru_hole oval (at -1.27 -19.05 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 216 "Net-(FLUXL216-Pad1)"))
    (pad 48 thru_hole oval (at 1.27 -19.05 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 248 "Net-(FLUXL248-Pad1)"))
    (pad 49 thru_hole oval (at -1.27 -21.59 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 217 "Net-(FLUXL217-Pad1)"))
    (pad 50 thru_hole oval (at 1.27 -21.59 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 249 "Net-(FLUXL249-Pad1)"))
    (pad 51 thru_hole oval (at -1.27 -24.13 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 218 "Net-(FLUXL218-Pad1)"))
    (pad 52 thru_hole oval (at 1.27 -24.13 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 250 "Net-(FLUXL250-Pad1)"))
    (pad 53 thru_hole oval (at -1.27 -26.67 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 219 "Net-(FLUXL219-Pad1)"))
    (pad 54 thru_hole oval (at 1.27 -26.67 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 251 "Net-(FLUXL251-Pad1)"))
    (pad 55 thru_hole oval (at -1.27 -29.21 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 220 "Net-(FLUXL220-Pad1)"))
    (pad 56 thru_hole oval (at 1.27 -29.21 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 252 "Net-(FLUXL252-Pad1)"))
    (pad 57 thru_hole oval (at -1.27 -31.75 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 221 "Net-(FLUXL221-Pad1)"))
    (pad 58 thru_hole oval (at 1.27 -31.75 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 253 "Net-(FLUXL253-Pad1)"))
    (pad 59 thru_hole oval (at -1.27 -34.29 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 222 "Net-(FLUXL222-Pad1)"))
    (pad 60 thru_hole oval (at 1.27 -34.29 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 254 "Net-(FLUXL254-Pad1)"))
    (pad 61 thru_hole oval (at -1.27 -36.83 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 223 "Net-(FLUXL223-Pad1)"))
    (pad 62 thru_hole oval (at 1.27 -36.83 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 255 "Net-(FLUXL255-Pad1)"))
    (pad 63 thru_hole oval (at -1.27 -39.37 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 224 "Net-(FLUXL224-Pad1)"))
    (pad 64 thru_hole oval (at 1.27 -39.37 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 256 "Net-(FLUXL256-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x32.wrl
      (at (xyz 0.05 -1.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Malu:Pin_Header_Straight_2x32_TH locked (layer B.Cu) (tedit 0)
    (at 70 24 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -1.27 44.47 90) (layer B.SilkS))
    (fp_text value CONN_02X32 (at -1.27 42.47 90) (layer B.Fab))
    (pad 1 thru_hole rect (at -1.27 39.37 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 129 "Net-(FLUXL129-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 39.37 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 161 "Net-(FLUXL161-Pad1)"))
    (pad 3 thru_hole oval (at -1.27 36.83 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 130 "Net-(FLUXL130-Pad1)"))
    (pad 4 thru_hole oval (at 1.27 36.83 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 162 "Net-(FLUXL162-Pad1)"))
    (pad 5 thru_hole oval (at -1.27 34.29 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 131 "Net-(FLUXL131-Pad1)"))
    (pad 6 thru_hole oval (at 1.27 34.29 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 163 "Net-(FLUXL163-Pad1)"))
    (pad 7 thru_hole oval (at -1.27 31.75 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 132 "Net-(FLUXL132-Pad1)"))
    (pad 8 thru_hole oval (at 1.27 31.75 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 164 "Net-(FLUXL164-Pad1)"))
    (pad 9 thru_hole oval (at -1.27 29.21 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 133 "Net-(FLUXL133-Pad1)"))
    (pad 10 thru_hole oval (at 1.27 29.21 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 165 "Net-(FLUXL165-Pad1)"))
    (pad 11 thru_hole oval (at -1.27 26.67 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 134 "Net-(FLUXL134-Pad1)"))
    (pad 12 thru_hole oval (at 1.27 26.67 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 166 "Net-(FLUXL166-Pad1)"))
    (pad 13 thru_hole oval (at -1.27 24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 135 "Net-(FLUXL135-Pad1)"))
    (pad 14 thru_hole oval (at 1.27 24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 167 "Net-(FLUXL167-Pad1)"))
    (pad 15 thru_hole oval (at -1.27 21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 136 "Net-(FLUXL136-Pad1)"))
    (pad 16 thru_hole oval (at 1.27 21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 168 "Net-(FLUXL168-Pad1)"))
    (pad 17 thru_hole oval (at -1.27 19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 137 "Net-(FLUXL137-Pad1)"))
    (pad 18 thru_hole oval (at 1.27 19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 169 "Net-(FLUXL169-Pad1)"))
    (pad 19 thru_hole oval (at -1.27 16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 138 "Net-(FLUXL138-Pad1)"))
    (pad 20 thru_hole oval (at 1.27 16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 170 "Net-(FLUXL170-Pad1)"))
    (pad 21 thru_hole oval (at -1.27 13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 139 "Net-(FLUXL139-Pad1)"))
    (pad 22 thru_hole oval (at 1.27 13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 171 "Net-(FLUXL171-Pad1)"))
    (pad 23 thru_hole oval (at -1.27 11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 140 "Net-(FLUXL140-Pad1)"))
    (pad 24 thru_hole oval (at 1.27 11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 172 "Net-(FLUXL172-Pad1)"))
    (pad 25 thru_hole oval (at -1.27 8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 141 "Net-(FLUXL141-Pad1)"))
    (pad 26 thru_hole oval (at 1.27 8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 173 "Net-(FLUXL173-Pad1)"))
    (pad 27 thru_hole oval (at -1.27 6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 142 "Net-(FLUXL142-Pad1)"))
    (pad 28 thru_hole oval (at 1.27 6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 174 "Net-(FLUXL174-Pad1)"))
    (pad 29 thru_hole oval (at -1.27 3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 143 "Net-(FLUXL143-Pad1)"))
    (pad 30 thru_hole oval (at 1.27 3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 175 "Net-(FLUXL175-Pad1)"))
    (pad 31 thru_hole oval (at -1.27 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 144 "Net-(FLUXL144-Pad1)"))
    (pad 32 thru_hole oval (at 1.27 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 176 "Net-(FLUXL176-Pad1)"))
    (pad 33 thru_hole oval (at -1.27 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 145 "Net-(FLUXL145-Pad1)"))
    (pad 34 thru_hole oval (at 1.27 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 177 "Net-(FLUXL177-Pad1)"))
    (pad 35 thru_hole oval (at -1.27 -3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 146 "Net-(FLUXL146-Pad1)"))
    (pad 36 thru_hole oval (at 1.27 -3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 178 "Net-(FLUXL178-Pad1)"))
    (pad 37 thru_hole oval (at -1.27 -6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 147 "Net-(FLUXL147-Pad1)"))
    (pad 38 thru_hole oval (at 1.27 -6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 179 "Net-(FLUXL179-Pad1)"))
    (pad 39 thru_hole oval (at -1.27 -8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 148 "Net-(FLUXL148-Pad1)"))
    (pad 40 thru_hole oval (at 1.27 -8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 180 "Net-(FLUXL180-Pad1)"))
    (pad 41 thru_hole oval (at -1.27 -11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 149 "Net-(FLUXL149-Pad1)"))
    (pad 42 thru_hole oval (at 1.27 -11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 181 "Net-(FLUXL181-Pad1)"))
    (pad 43 thru_hole oval (at -1.27 -13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 150 "Net-(FLUXL150-Pad1)"))
    (pad 44 thru_hole oval (at 1.27 -13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 182 "Net-(FLUXL182-Pad1)"))
    (pad 45 thru_hole oval (at -1.27 -16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 151 "Net-(FLUXL151-Pad1)"))
    (pad 46 thru_hole oval (at 1.27 -16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 183 "Net-(FLUXL183-Pad1)"))
    (pad 47 thru_hole oval (at -1.27 -19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 152 "Net-(FLUXL152-Pad1)"))
    (pad 48 thru_hole oval (at 1.27 -19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 184 "Net-(FLUXL184-Pad1)"))
    (pad 49 thru_hole oval (at -1.27 -21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 153 "Net-(FLUXL153-Pad1)"))
    (pad 50 thru_hole oval (at 1.27 -21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 185 "Net-(FLUXL185-Pad1)"))
    (pad 51 thru_hole oval (at -1.27 -24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 154 "Net-(FLUXL154-Pad1)"))
    (pad 52 thru_hole oval (at 1.27 -24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 186 "Net-(FLUXL186-Pad1)"))
    (pad 53 thru_hole oval (at -1.27 -26.67 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 155 "Net-(FLUXL155-Pad1)"))
    (pad 54 thru_hole oval (at 1.27 -26.67 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 187 "Net-(FLUXL187-Pad1)"))
    (pad 55 thru_hole oval (at -1.27 -29.21 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 156 "Net-(FLUXL156-Pad1)"))
    (pad 56 thru_hole oval (at 1.27 -29.21 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 188 "Net-(FLUXL188-Pad1)"))
    (pad 57 thru_hole oval (at -1.27 -31.75 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 157 "Net-(FLUXL157-Pad1)"))
    (pad 58 thru_hole oval (at 1.27 -31.75 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 189 "Net-(FLUXL189-Pad1)"))
    (pad 59 thru_hole oval (at -1.27 -34.29 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 158 "Net-(FLUXL158-Pad1)"))
    (pad 60 thru_hole oval (at 1.27 -34.29 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 190 "Net-(FLUXL190-Pad1)"))
    (pad 61 thru_hole oval (at -1.27 -36.83 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 159 "Net-(FLUXL159-Pad1)"))
    (pad 62 thru_hole oval (at 1.27 -36.83 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 191 "Net-(FLUXL191-Pad1)"))
    (pad 63 thru_hole oval (at -1.27 -39.37 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 160 "Net-(FLUXL160-Pad1)"))
    (pad 64 thru_hole oval (at 1.27 -39.37 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 192 "Net-(FLUXL192-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x32.wrl
      (at (xyz 0.05 -1.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Malu:Pin_Header_Straight_2x32_TH locked (layer B.Cu) (tedit 0)
    (at 116 70)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -1.27 44.47) (layer B.SilkS))
    (fp_text value CONN_02X32 (at -1.27 42.47) (layer B.Fab))
    (pad 1 thru_hole rect (at -1.27 39.37) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 "Net-(FLUXL1-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 39.37) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 33 "Net-(FLUXL33-Pad1)"))
    (pad 3 thru_hole oval (at -1.27 36.83) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 "Net-(FLUXL2-Pad1)"))
    (pad 4 thru_hole oval (at 1.27 36.83) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 34 "Net-(FLUXL34-Pad1)"))
    (pad 5 thru_hole oval (at -1.27 34.29) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 "Net-(FLUXL3-Pad1)"))
    (pad 6 thru_hole oval (at 1.27 34.29) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 35 "Net-(FLUXL35-Pad1)"))
    (pad 7 thru_hole oval (at -1.27 31.75) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 4 "Net-(FLUXL4-Pad1)"))
    (pad 8 thru_hole oval (at 1.27 31.75) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 36 "Net-(FLUXL36-Pad1)"))
    (pad 9 thru_hole oval (at -1.27 29.21) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 "Net-(FLUXL5-Pad1)"))
    (pad 10 thru_hole oval (at 1.27 29.21) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 37 "Net-(FLUXL37-Pad1)"))
    (pad 11 thru_hole oval (at -1.27 26.67) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 6 "Net-(FLUXL6-Pad1)"))
    (pad 12 thru_hole oval (at 1.27 26.67) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 38 "Net-(FLUXL38-Pad1)"))
    (pad 13 thru_hole oval (at -1.27 24.13) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 7 "Net-(FLUXL7-Pad1)"))
    (pad 14 thru_hole oval (at 1.27 24.13) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 39 "Net-(FLUXL39-Pad1)"))
    (pad 15 thru_hole oval (at -1.27 21.59) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(FLUXL8-Pad1)"))
    (pad 16 thru_hole oval (at 1.27 21.59) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 40 "Net-(FLUXL40-Pad1)"))
    (pad 17 thru_hole oval (at -1.27 19.05) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 9 "Net-(FLUXL9-Pad1)"))
    (pad 18 thru_hole oval (at 1.27 19.05) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 41 "Net-(FLUXL41-Pad1)"))
    (pad 19 thru_hole oval (at -1.27 16.51) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 10 "Net-(FLUXL10-Pad1)"))
    (pad 20 thru_hole oval (at 1.27 16.51) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 42 "Net-(FLUXL42-Pad1)"))
    (pad 21 thru_hole oval (at -1.27 13.97) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 11 "Net-(FLUXL11-Pad1)"))
    (pad 22 thru_hole oval (at 1.27 13.97) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 43 "Net-(FLUXL43-Pad1)"))
    (pad 23 thru_hole oval (at -1.27 11.43) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 12 "Net-(FLUXL12-Pad1)"))
    (pad 24 thru_hole oval (at 1.27 11.43) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 44 "Net-(FLUXL44-Pad1)"))
    (pad 25 thru_hole oval (at -1.27 8.89) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 13 "Net-(FLUXL13-Pad1)"))
    (pad 26 thru_hole oval (at 1.27 8.89) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 45 "Net-(FLUXL45-Pad1)"))
    (pad 27 thru_hole oval (at -1.27 6.35) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 14 "Net-(FLUXL14-Pad1)"))
    (pad 28 thru_hole oval (at 1.27 6.35) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 46 "Net-(FLUXL46-Pad1)"))
    (pad 29 thru_hole oval (at -1.27 3.81) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 15 "Net-(FLUXL15-Pad1)"))
    (pad 30 thru_hole oval (at 1.27 3.81) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 47 "Net-(FLUXL47-Pad1)"))
    (pad 31 thru_hole oval (at -1.27 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 16 "Net-(FLUXL16-Pad1)"))
    (pad 32 thru_hole oval (at 1.27 1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 48 "Net-(FLUXL48-Pad1)"))
    (pad 33 thru_hole oval (at -1.27 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 17 "Net-(FLUXL17-Pad1)"))
    (pad 34 thru_hole oval (at 1.27 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 49 "Net-(FLUXL49-Pad1)"))
    (pad 35 thru_hole oval (at -1.27 -3.81) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 18 "Net-(FLUXL18-Pad1)"))
    (pad 36 thru_hole oval (at 1.27 -3.81) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 50 "Net-(FLUXL50-Pad1)"))
    (pad 37 thru_hole oval (at -1.27 -6.35) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 19 "Net-(FLUXL19-Pad1)"))
    (pad 38 thru_hole oval (at 1.27 -6.35) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 51 "Net-(FLUXL51-Pad1)"))
    (pad 39 thru_hole oval (at -1.27 -8.89) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 20 "Net-(FLUXL20-Pad1)"))
    (pad 40 thru_hole oval (at 1.27 -8.89) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 52 "Net-(FLUXL52-Pad1)"))
    (pad 41 thru_hole oval (at -1.27 -11.43) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 21 "Net-(FLUXL21-Pad1)"))
    (pad 42 thru_hole oval (at 1.27 -11.43) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 53 "Net-(FLUXL53-Pad1)"))
    (pad 43 thru_hole oval (at -1.27 -13.97) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 22 "Net-(FLUXL22-Pad1)"))
    (pad 44 thru_hole oval (at 1.27 -13.97) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 54 "Net-(FLUXL54-Pad1)"))
    (pad 45 thru_hole oval (at -1.27 -16.51) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 23 "Net-(FLUXL23-Pad1)"))
    (pad 46 thru_hole oval (at 1.27 -16.51) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 55 "Net-(FLUXL55-Pad1)"))
    (pad 47 thru_hole oval (at -1.27 -19.05) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 24 "Net-(FLUXL24-Pad1)"))
    (pad 48 thru_hole oval (at 1.27 -19.05) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 56 "Net-(FLUXL56-Pad1)"))
    (pad 49 thru_hole oval (at -1.27 -21.59) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 25 "Net-(FLUXL25-Pad1)"))
    (pad 50 thru_hole oval (at 1.27 -21.59) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 57 "Net-(FLUXL57-Pad1)"))
    (pad 51 thru_hole oval (at -1.27 -24.13) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 26 "Net-(FLUXL26-Pad1)"))
    (pad 52 thru_hole oval (at 1.27 -24.13) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 58 "Net-(FLUXL58-Pad1)"))
    (pad 53 thru_hole oval (at -1.27 -26.67) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 27 "Net-(FLUXL27-Pad1)"))
    (pad 54 thru_hole oval (at 1.27 -26.67) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 59 "Net-(FLUXL59-Pad1)"))
    (pad 55 thru_hole oval (at -1.27 -29.21) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 28 "Net-(FLUXL28-Pad1)"))
    (pad 56 thru_hole oval (at 1.27 -29.21) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 60 "Net-(FLUXL60-Pad1)"))
    (pad 57 thru_hole oval (at -1.27 -31.75) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 29 "Net-(FLUXL29-Pad1)"))
    (pad 58 thru_hole oval (at 1.27 -31.75) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 61 "Net-(FLUXL61-Pad1)"))
    (pad 59 thru_hole oval (at -1.27 -34.29) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 30 "Net-(FLUXL30-Pad1)"))
    (pad 60 thru_hole oval (at 1.27 -34.29) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 62 "Net-(FLUXL62-Pad1)"))
    (pad 61 thru_hole oval (at -1.27 -36.83) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 31 "Net-(FLUXL31-Pad1)"))
    (pad 62 thru_hole oval (at 1.27 -36.83) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 63 "Net-(FLUXL63-Pad1)"))
    (pad 63 thru_hole oval (at -1.27 -39.37) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 32 "Net-(FLUXL32-Pad1)"))
    (pad 64 thru_hole oval (at 1.27 -39.37) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 64 "Net-(FLUXL64-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x32.wrl
      (at (xyz 0.05 -1.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (target plus (at 70 70) (size 5) (width 0.15) (layer Edge.Cuts))
  (target plus (at 70 70) (size 5) (width 0.15) (layer Edge.Cuts))
  (target plus (at 70 70) (size 5) (width 0.15) (layer Edge.Cuts))
  (dimension 100 (width 0.3) (layer Eco2.User)
    (gr_text "100.000 mm" (at 70 126.35) (layer Eco2.User))
    (feature1 (pts (xy 120 120) (xy 120 127.7)))
    (feature2 (pts (xy 20 120) (xy 20 127.7)))
    (crossbar (pts (xy 20 125) (xy 120 125)))
    (arrow1a (pts (xy 120 125) (xy 118.873496 125.586421)))
    (arrow1b (pts (xy 120 125) (xy 118.873496 124.413579)))
    (arrow2a (pts (xy 20 125) (xy 21.126504 125.586421)))
    (arrow2b (pts (xy 20 125) (xy 21.126504 124.413579)))
  )
  (dimension 100 (width 0.3) (layer Eco2.User)
    (gr_text "100.000 mm" (at 126.35 70 270) (layer Eco2.User))
    (feature1 (pts (xy 120 120) (xy 127.7 120)))
    (feature2 (pts (xy 120 20) (xy 127.7 20)))
    (crossbar (pts (xy 125 20) (xy 125 120)))
    (arrow1a (pts (xy 125 120) (xy 124.413579 118.873496)))
    (arrow1b (pts (xy 125 120) (xy 125.586421 118.873496)))
    (arrow2a (pts (xy 125 20) (xy 124.413579 21.126504)))
    (arrow2b (pts (xy 125 20) (xy 125.586421 21.126504)))
  )
  (gr_line (start 20 120) (end 20 20) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120 120) (end 20 120) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120 20) (end 120 120) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20 20) (end 120 20) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20 38.5) (end 20 101.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120 101.5) (end 120 38.5) (layer Edge.Cuts) (width 0.15))
)
