<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<text>CAN</text>
<wire x1="0" y1="0" x2="50" y2="0" width="0" layer="20"/>
<wire x1="50" y1="0" x2="50" y2="50" width="0" layer="20"/>
<wire x1="50" y1="50" x2="0" y2="50" width="0" layer="20"/>
<wire x1="0" y1="50" x2="0" y2="0" width="0" layer="20"/>
<text>6 +12V
5 GND
4 CAN-L
3 CAN-H
2 GND
1 +12V</text>
<hole x="3" y="3" drill="3.2"/>
<hole x="47" y="3" drill="3.2"/>
<hole x="47" y="47" drill="3.2"/>
<hole x="3" y="47" drill="3.2"/>
<text>X1</text>
<text>CAN</text>
<text>INTER</text>
<text>12V Select:</text>
<text>INTER</text>
<text>SMPS</text>
<text>3.3V
Select:</text>
<text>+</text>
<text>-</text>
<text>GND</text>
<text>GND</text>
<text>12</text>
<text>3.3</text>
<text>SCL</text>
<text>SDA</text>
<text>SLP</text>
<text>ENU</text>
<text>1</text>
<text>PD4</text>
<text>PC2</text>
<text>PC0</text>
<text>PC1</text>
<text>PC3</text>
<text>PD1</text>
<text>PD0</text>
<text>PD2</text>
<text>INTER</text>
<text>6 +12V
5 GND
4 CAN-L
3 CAN-H
2 GND
1 +12V</text>
<text>CAN2IO v1.0</text>
<text>Joey5337 2015-09</text>
</plain>
<libraries>
<library name="joey_v15">
<description>&lt;h1&gt;HWP-Bibliothek&lt;/h1&gt;
Version 0.08 &lt;br&gt;
Stand 2004-05-06 &lt;br&gt;


Changelog: &lt;br&gt;
&lt;dl&gt;
  &lt;dt&gt;2004-02-15&lt;/dt&gt;
  &lt;dd&gt;Hinzufügen der Tantal-Version des 4.7uF  Elkos &lt;br&gt;
     Prefix "C" für Elkos
  &lt;/dd&gt;
  &lt;dt&gt;2003-03-26  v0.04&lt;/dt&gt;
  &lt;dd&gt;Befestigungsbohrungen (Holes) durch Vias ersetzen.&lt;/dd&gt;

  &lt;dt&gt;2004-04-22&lt;/dt&gt;
  &lt;dd&gt;Pin Assignement am LM317 richtig gestellt, Größe und Nullpunkt des Board auf (0/0), (100,80)mm gesetzt&lt;/dd&gt;

  &lt;dt&gt;2004-04-23&lt;/dt&gt;
  &lt;dd&gt;Hole in package TO220AH (= TO220 liegend) durch Pad/Via ersetzt &lt;br&gt;
  PIC18F258 hinzugefügt. &lt;br&gt;
  Max232 hinzugefügt.
  &lt;/dd&gt;

  &lt;dt&gt;2004-05-04&lt;/dt&gt;
  &lt;dd&gt;Board geringfügig vergrößert, um Fehler beim DRC zu verhindern.&lt;/dd&gt;

  &lt;dt&gt;2004-05-06&lt;/dt&gt;
  &lt;dd&gt;Automatically insert Power supply Gate in schematic for MAX 232&lt;/dd&gt;

  &lt;dt&gt;2004-10-06  v0.09&lt;/dt&gt;
  &lt;dd&gt;Removed wrong pin numbers from the LM317 symbol. (The image you see in the schematic.)&lt;/dd&gt;

  &lt;dt&gt;2005-02-17 v0.10&lt;/dt&gt;
  &lt;dd&gt;Added Round Testpoints in different sizes. (E.g. for In Service Programming)&lt;/dd&gt;

  &lt;dt&gt;2005-03-21  v0.11&lt;/dt&gt;
  &lt;dd&gt;Added IRF7103, Cooler for TO220s.&lt;/dd&gt;

  &lt;dt&gt;2005-10-18 v0.12&lt;/dt&gt;
  &lt;dd&gt;Added new microprocessor: ATmega16 from Atmel, 6-Pin ISP-Connector&lt;/dd&gt;

  &lt;dt&gt;2005-11-10&lt;/dt&gt;
  &lt;dd&gt;Added IRF7104. Better Soldering for TQFP-Package (used in ATmega16)&lt;/dd&gt;

&lt;!--
  &lt;dt&gt;Datum&lt;/dt&gt;
  &lt;dd&gt;TEXT&lt;/dd&gt;
--&gt;
&lt;/dl&gt;</description>
<packages>
<package name="SO8-2">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="con-harting-ml">
<description>&lt;b&gt;Harting  &amp; 3M Connectors&lt;/b&gt;&lt;p&gt;
Low profile connectors, straight&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ML6">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="modular">
<packages>
<package name="JACK6LP">
</package>
</packages>
</library>
<library name="joey_v16">
<description>&lt;h1&gt;HWP-Bibliothek&lt;/h1&gt;
Version 0.08 &lt;br&gt;
Stand 2004-05-06 &lt;br&gt;


Changelog: &lt;br&gt;
&lt;dl&gt;
  &lt;dt&gt;2004-02-15&lt;/dt&gt;
  &lt;dd&gt;Hinzufügen der Tantal-Version des 4.7uF  Elkos &lt;br&gt;
     Prefix "C" für Elkos
  &lt;/dd&gt;
  &lt;dt&gt;2003-03-26  v0.04&lt;/dt&gt;
  &lt;dd&gt;Befestigungsbohrungen (Holes) durch Vias ersetzen.&lt;/dd&gt;

  &lt;dt&gt;2004-04-22&lt;/dt&gt;
  &lt;dd&gt;Pin Assignement am LM317 richtig gestellt, Größe und Nullpunkt des Board auf (0/0), (100,80)mm gesetzt&lt;/dd&gt;

  &lt;dt&gt;2004-04-23&lt;/dt&gt;
  &lt;dd&gt;Hole in package TO220AH (= TO220 liegend) durch Pad/Via ersetzt &lt;br&gt;
  PIC18F258 hinzugefügt. &lt;br&gt;
  Max232 hinzugefügt.
  &lt;/dd&gt;

  &lt;dt&gt;2004-05-04&lt;/dt&gt;
  &lt;dd&gt;Board geringfügig vergrößert, um Fehler beim DRC zu verhindern.&lt;/dd&gt;

  &lt;dt&gt;2004-05-06&lt;/dt&gt;
  &lt;dd&gt;Automatically insert Power supply Gate in schematic for MAX 232&lt;/dd&gt;

  &lt;dt&gt;2004-10-06  v0.09&lt;/dt&gt;
  &lt;dd&gt;Removed wrong pin numbers from the LM317 symbol. (The image you see in the schematic.)&lt;/dd&gt;

  &lt;dt&gt;2005-02-17 v0.10&lt;/dt&gt;
  &lt;dd&gt;Added Round Testpoints in different sizes. (E.g. for In Service Programming)&lt;/dd&gt;

  &lt;dt&gt;2005-03-21  v0.11&lt;/dt&gt;
  &lt;dd&gt;Added IRF7103, Cooler for TO220s.&lt;/dd&gt;

  &lt;dt&gt;2005-10-18 v0.12&lt;/dt&gt;
  &lt;dd&gt;Added new microprocessor: ATmega16 from Atmel, 6-Pin ISP-Connector&lt;/dd&gt;

  &lt;dt&gt;2005-11-10&lt;/dt&gt;
  &lt;dd&gt;Added IRF7104. Better Soldering for TQFP-Package (used in ATmega16)&lt;/dd&gt;

&lt;!--
  &lt;dt&gt;Datum&lt;/dt&gt;
  &lt;dd&gt;TEXT&lt;/dd&gt;
--&gt;
&lt;/dl&gt;</description>
<packages>
<package name="1206">
</package>
<package name="0805">
</package>
<package name="SO18">
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="OSC-5">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="MICROCRYSTAL-MS1V-T1K">
</package>
<package name="SMD-ELLIPSE-70">
</package>
</packages>
</library>
<library name="Inductor-Fastron">
<packages>
<package name="PIS24XX">
</package>
</packages>
</library>
<library name="J5337-Elko-Panasonic">
<description>&lt;h1&gt;SMD-Elkos von Panasonic&lt;/h1&gt;

Gruppenbezeichnung bei Reichelt: &lt;br&gt;
Elkos SMD, Low ESR, 105°C</description>
<packages>
<package name="B">
</package>
</packages>
</library>
<library name="con-phoenix-350">
<description>&lt;b&gt;Phoenix Connectors&lt;/b&gt; Grid 3.50 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1751248">
<description>&lt;b&gt;MKDS 1/ 2-3,5&lt;/b&gt; Printklemme&lt;p&gt;
Nennstrom: 10 A&lt;br&gt;
Bemessungsspannung: 160 V&lt;br&gt;
Raster: 3,5 mm&lt;br&gt;
Polzahl: 2&lt;br&gt;
Montageart: Löten&lt;br&gt;
Anschlussart: Schraubanschluss&lt;br&gt;
Anschlussrichtung vom Leiter zur Platine: 0°&lt;br&gt;
Source: http://eshop.phoenixcontact.com .. 1751248.pdf</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="2X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
</packages>
</library>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="J5337-MCP">
<packages>
<package name="MSOP8">
<description>&lt;b&gt;Micro Small Outline Package&lt;/b&gt; Grid 0.65mm&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/21796H.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC2" library="joey_v15" package="SO8-2" value="SN 65HVD230D"/>
<element name="C7" library="joey_v15" package="0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="joey_v15" package="0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="joey_v15" package="0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISP" library="con-harting-ml" package="ML6" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="joey_v15" package="0805" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CAN1" library="modular" package="JACK6LP" value="JACK6LOW_PROFILE"/>
<element name="CAN2" library="modular" package="JACK6LP" value="JACK6LOW_PROFILE"/>
<element name="R20" library="joey_v16" package="0805" value="(10k)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="joey_v16" package="0805" value="(47n)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-phoenix-350" package="1751248" value="1751248">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="J_BOT" library="pinhead" package="2X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="avr-7" package="TQFP32-08" value="MEGA48/88/168-AU"/>
<element name="JP3" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="IC4" library="joey_v16" package="SO18" value="MCP2510">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="joey_v16" package="0805" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="joey_v16" package="0805" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="J5337-MCP" package="MSOP8" value="MCP16311">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="Inductor-Fastron" package="PIS24XX" value="L-PIS2408 15µ"/>
<element name="C1" library="joey_v16" package="0805" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="joey_v16" package="0805" value="100n"/>
<element name="R1" library="joey_v16" package="0805" value="31k2"/>
<element name="R2" library="joey_v16" package="0805" value="10k"/>
<element name="C6" library="joey_v16" package="1206" value="10u/25V"/>
<element name="C12" library="joey_v16" package="1206" value="10u/25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="J5337-Elko-Panasonic" package="B" value="10u/25V"/>
<element name="JP4" library="pinhead" package="2X02" value="">
<attribute name="VALUE"/>
</element>
<element name="C3" library="joey_v15" package="0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="1" library="joey_v16" package="LED3MM" value="green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="2" library="joey_v16" package="LED3MM" value="red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="joey_v16" package="0805" value="330"/>
<element name="C10" library="J5337-Elko-Panasonic" package="B" value="10u/25V"/>
<element name="R4" library="joey_v16" package="0805" value=""/>
<element name="OSC1" library="joey_v16" package="OSC-5" value="8MHz">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="joey_v16" package="SOT23" value="PESD2CAN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="joey_v16" package="MICROCRYSTAL-MS1V-T1K" value="OSC-SMD-MICROCRYSTAL"/>
<element name="TP1" library="joey_v16" package="SMD-ELLIPSE-70" value="TESTPOINTROUND-70"/>
<element name="TP2" library="joey_v16" package="SMD-ELLIPSE-70" value="TESTPOINTROUND-70"/>
<element name="R5" library="joey_v16" package="0805" value="330"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC2" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="IC2" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="ISP" pad="6"/>
<contactref element="C15" pad="1"/>
<contactref element="CAN2" pad="P$2"/>
<contactref element="CAN1" pad="P$2"/>
<contactref element="CAN1" pad="P$5"/>
<contactref element="CAN2" pad="P$5"/>
<contactref element="J_BOT" pad="1"/>
<contactref element="J_BOT" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="21"/>
<contactref element="X1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U$2" pad="8"/>
<contactref element="U$2" pad="5"/>
<contactref element="R2" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C13" pad="C"/>
<contactref element="C12" pad="1"/>
<contactref element="IC4" pad="9"/>
<contactref element="C3" pad="2"/>
<contactref element="C10" pad="C"/>
<contactref element="U$1" pad="3"/>
<contactref element="R11" pad="1"/>
<contactref element="U$3" pad="P$3"/>
<contactref element="U$3" pad="P$3"/>
<contactref element="TP1" pad="P$1"/>
<contactref element="1" pad="K"/>
<contactref element="2" pad="K"/>
</signal>
<signal name="CANH">
<contactref element="IC2" pad="7"/>
<contactref element="CAN1" pad="P$3"/>
<contactref element="CAN2" pad="P$3"/>
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="CANL">
<contactref element="IC2" pad="6"/>
<contactref element="CAN1" pad="P$4"/>
<contactref element="CAN2" pad="P$4"/>
<contactref element="R4" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="IC2" pad="3"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="ISP" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="18"/>
<contactref element="JP4" pad="4"/>
<contactref element="JP4" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="IC4" pad="18"/>
<contactref element="IC4" pad="17"/>
</signal>
<signal name="N$7">
<contactref element="IC2" pad="4"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="ISP" pad="1"/>
<contactref element="IC1" pad="16"/>
<contactref element="IC4" pad="15"/>
</signal>
<signal name="MOSI">
<contactref element="ISP" pad="4"/>
<contactref element="IC1" pad="15"/>
<contactref element="IC4" pad="14"/>
</signal>
<signal name="SCK">
<contactref element="ISP" pad="3"/>
<contactref element="IC1" pad="17"/>
<contactref element="IC4" pad="13"/>
</signal>
<signal name="N$29">
<contactref element="IC2" pad="8"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$5">
</signal>
<signal name="N$14">
<contactref element="IC2" pad="1"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="R20" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="ISP" pad="5"/>
<contactref element="IC1" pad="29"/>
</signal>
<signal name="SDA">
<contactref element="J_BOT" pad="5"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="SLEEP">
<contactref element="J_BOT" pad="8"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="12VINTERCON">
<contactref element="J_BOT" pad="4"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="+3,3V">
<contactref element="J_BOT" pad="3"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="J_BOT" pad="16"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="ENUM-OUT">
<contactref element="J_BOT" pad="7"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$19">
</signal>
<signal name="N$21">
</signal>
<signal name="N$22">
</signal>
<signal name="N$25">
</signal>
<signal name="N$26">
</signal>
<signal name="N$9">
<contactref element="J_BOT" pad="9"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="N$11">
<contactref element="J_BOT" pad="10"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="J_BOT" pad="6"/>
<contactref element="IC1" pad="28"/>
</signal>
<signal name="12VSMPS">
<contactref element="JP3" pad="1"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP3" pad="5"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$2" pad="4"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="A"/>
</signal>
<signal name="12VCAN">
<contactref element="CAN1" pad="P$1"/>
<contactref element="CAN2" pad="P$1"/>
<contactref element="CAN1" pad="P$6"/>
<contactref element="CAN2" pad="P$6"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="12VTERMINAL">
<contactref element="X1" pad="1"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="IC4" pad="7"/>
<contactref element="C4" pad="1"/>
<contactref element="OSC1" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="IC4" pad="8"/>
<contactref element="C5" pad="1"/>
<contactref element="OSC1" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U$2" pad="6"/>
<contactref element="L2" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="U$2" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="U$2" pad="7"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="R1" pad="2"/>
<contactref element="L2" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="C10" pad="A"/>
</signal>
<signal name="N$32">
</signal>
<signal name="N$15">
<contactref element="IC1" pad="1"/>
<contactref element="IC4" pad="12"/>
</signal>
<signal name="N$37">
<contactref element="IC1" pad="24"/>
<contactref element="J_BOT" pad="15"/>
</signal>
<signal name="N$38">
<contactref element="IC1" pad="25"/>
<contactref element="J_BOT" pad="14"/>
</signal>
<signal name="N$39">
<contactref element="IC1" pad="26"/>
<contactref element="J_BOT" pad="13"/>
</signal>
<signal name="N$27">
<contactref element="IC1" pad="31"/>
<contactref element="J_BOT" pad="12"/>
</signal>
<signal name="N$40">
<contactref element="IC1" pad="30"/>
<contactref element="J_BOT" pad="11"/>
</signal>
<signal name="N$8">
<contactref element="IC4" pad="6"/>
<contactref element="TP2" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="IC4" pad="5"/>
</signal>
<signal name="N$34">
<contactref element="IC4" pad="4"/>
</signal>
<signal name="N$36">
<contactref element="IC4" pad="11"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="14"/>
<contactref element="IC4" pad="16"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="13"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="12"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="R3" pad="1"/>
<contactref element="1" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="22"/>
</signal>
<signal name="N$41">
<contactref element="IC1" pad="8"/>
<contactref element="U$3" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="U$3" pad="P$2"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$28">
<contactref element="IC1" pad="11"/>
</signal>
<signal name="N$42">
<contactref element="R5" pad="1"/>
<contactref element="2" pad="A"/>
</signal>
<signal name="N$43">
<contactref element="IC1" pad="19"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
