<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<packages>
<package name="ARDUINO_DUE_REDUCED">
<description>Footprint for representing an Arduino Due board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
</packages>
<symbols>
<symbol name="ARDUINO_BASIC_IO">
<description>Schematic symbol for representing an Arduino Due board in an EAGLE schematic. Created by Dave Young for Element14. 
More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle
&lt;note: No two pins can be named the same; in  this drawing +5V is the same as +5V. and +5V.. and +5V_ etc...&gt;</description>
<pin name="(N/C)"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="2"/>
<pin name="3"/>
<pin name="3.3V" direction="pas"/>
<pin name="4"/>
<pin name="5"/>
<pin name="5V" direction="pas"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="TX3"/>
<pin name="RX3"/>
<pin name="TX2"/>
<pin name="RX2"/>
<pin name="TX1"/>
<pin name="RX1"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="AREF" direction="pas"/>
<pin name="CANRX"/>
<pin name="CANTX"/>
<pin name="DAC0"/>
<pin name="DAC1"/>
<pin name="GND" direction="pas"/>
<pin name="GND@1" direction="pas"/>
<pin name="GND@0" direction="pas"/>
<pin name="IOREF"/>
<pin name="RESET"/>
<pin name="SCL1"/>
<pin name="SDA1"/>
<pin name="VIN" direction="pas"/>
</symbol>
<symbol name="ADRUINO_SPI">
<pin name="+5V" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="RESET"/>
<pin name="SCK"/>
</symbol>
<symbol name="ARDUINO_EXTRA_IO">
<pin name="+5V@0" direction="pas"/>
<pin name="+5V@1" direction="pas"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="39"/>
<pin name="40"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
<pin name="45"/>
<pin name="46"/>
<pin name="47"/>
<pin name="48"/>
<pin name="49"/>
<pin name="50"/>
<pin name="51"/>
<pin name="52"/>
<pin name="53"/>
<pin name="GND@2" direction="pas"/>
<pin name="GND@1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ARDUINO_DUE" prefix="M">
<description>Device for representing an Arduino Due board with a footprint in an EAGLE design. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
<gates>
<gate name="BASIC" symbol="ARDUINO_BASIC_IO"/>
<gate name="-SPI" symbol="ADRUINO_SPI"/>
<gate name="-XIO" symbol="ARDUINO_EXTRA_IO"/>
</gates>
<devices>
<device name="" package="ARDUINO_DUE_REDUCED">
<connects>
<connect gate="-SPI" pin="+5V" pad=".2"/>
<connect gate="-SPI" pin="GND" pad=".6"/>
<connect gate="-SPI" pin="MISO" pad=".1"/>
<connect gate="-SPI" pin="MOSI" pad=".4"/>
<connect gate="-SPI" pin="RESET" pad=".5"/>
<connect gate="-SPI" pin="SCK" pad=".3"/>
<connect gate="-XIO" pin="+5V@0" pad="5VE1"/>
<connect gate="-XIO" pin="+5V@1" pad="5VE2"/>
<connect gate="-XIO" pin="22" pad="22"/>
<connect gate="-XIO" pin="23" pad="23"/>
<connect gate="-XIO" pin="24" pad="24"/>
<connect gate="-XIO" pin="25" pad="25"/>
<connect gate="-XIO" pin="26" pad="26"/>
<connect gate="-XIO" pin="27" pad="27"/>
<connect gate="-XIO" pin="28" pad="28"/>
<connect gate="-XIO" pin="29" pad="29"/>
<connect gate="-XIO" pin="30" pad="30"/>
<connect gate="-XIO" pin="31" pad="31"/>
<connect gate="-XIO" pin="32" pad="32"/>
<connect gate="-XIO" pin="33" pad="33"/>
<connect gate="-XIO" pin="34" pad="34"/>
<connect gate="-XIO" pin="35" pad="35"/>
<connect gate="-XIO" pin="36" pad="36"/>
<connect gate="-XIO" pin="37" pad="37"/>
<connect gate="-XIO" pin="38" pad="38"/>
<connect gate="-XIO" pin="39" pad="39"/>
<connect gate="-XIO" pin="40" pad="40"/>
<connect gate="-XIO" pin="41" pad="41"/>
<connect gate="-XIO" pin="42" pad="42"/>
<connect gate="-XIO" pin="43" pad="43"/>
<connect gate="-XIO" pin="44" pad="44"/>
<connect gate="-XIO" pin="45" pad="45"/>
<connect gate="-XIO" pin="46" pad="46"/>
<connect gate="-XIO" pin="47" pad="47"/>
<connect gate="-XIO" pin="48" pad="48"/>
<connect gate="-XIO" pin="49" pad="49"/>
<connect gate="-XIO" pin="50" pad="50"/>
<connect gate="-XIO" pin="51" pad="51"/>
<connect gate="-XIO" pin="52" pad="52"/>
<connect gate="-XIO" pin="53" pad="53"/>
<connect gate="-XIO" pin="GND@1" pad="GNDE1"/>
<connect gate="-XIO" pin="GND@2" pad="GNDE2"/>
<connect gate="BASIC" pin="(N/C)" pad="N/C"/>
<connect gate="BASIC" pin="10" pad="10"/>
<connect gate="BASIC" pin="11" pad="11"/>
<connect gate="BASIC" pin="12" pad="12"/>
<connect gate="BASIC" pin="13" pad="13"/>
<connect gate="BASIC" pin="2" pad="2"/>
<connect gate="BASIC" pin="3" pad="3"/>
<connect gate="BASIC" pin="3.3V" pad="3.3V"/>
<connect gate="BASIC" pin="4" pad="4"/>
<connect gate="BASIC" pin="5" pad="5"/>
<connect gate="BASIC" pin="5V" pad="5V"/>
<connect gate="BASIC" pin="6" pad="6"/>
<connect gate="BASIC" pin="7" pad="7"/>
<connect gate="BASIC" pin="8" pad="8"/>
<connect gate="BASIC" pin="9" pad="9"/>
<connect gate="BASIC" pin="A0" pad="A0"/>
<connect gate="BASIC" pin="A1" pad="A1"/>
<connect gate="BASIC" pin="A10" pad="A10"/>
<connect gate="BASIC" pin="A11" pad="A11"/>
<connect gate="BASIC" pin="A2" pad="A2"/>
<connect gate="BASIC" pin="A3" pad="A3"/>
<connect gate="BASIC" pin="A4" pad="A4"/>
<connect gate="BASIC" pin="A5" pad="A5"/>
<connect gate="BASIC" pin="A6" pad="A6"/>
<connect gate="BASIC" pin="A7" pad="A7"/>
<connect gate="BASIC" pin="A8" pad="A8"/>
<connect gate="BASIC" pin="A9" pad="A9"/>
<connect gate="BASIC" pin="AREF" pad="AREF"/>
<connect gate="BASIC" pin="CANRX" pad="CANRX"/>
<connect gate="BASIC" pin="CANTX" pad="CANTX"/>
<connect gate="BASIC" pin="DAC0" pad="DAC0"/>
<connect gate="BASIC" pin="DAC1" pad="DAC1"/>
<connect gate="BASIC" pin="GND" pad="GND3"/>
<connect gate="BASIC" pin="GND@0" pad="GND1"/>
<connect gate="BASIC" pin="GND@1" pad="GND_VIN"/>
<connect gate="BASIC" pin="IOREF" pad="I/OREF"/>
<connect gate="BASIC" pin="RESET" pad="RESET"/>
<connect gate="BASIC" pin="RX" pad="1"/>
<connect gate="BASIC" pin="RX1" pad="19"/>
<connect gate="BASIC" pin="RX2" pad="17"/>
<connect gate="BASIC" pin="RX3" pad="15"/>
<connect gate="BASIC" pin="SCL" pad="21"/>
<connect gate="BASIC" pin="SCL1" pad="SCL1"/>
<connect gate="BASIC" pin="SDA" pad="20"/>
<connect gate="BASIC" pin="SDA1" pad="SDA1"/>
<connect gate="BASIC" pin="TX" pad="0"/>
<connect gate="BASIC" pin="TX1" pad="18"/>
<connect gate="BASIC" pin="TX2" pad="16"/>
<connect gate="BASIC" pin="TX3" pad="14"/>
<connect gate="BASIC" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
