(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 14)
    (no_connects 0)
    (area 19.529999 15.064999 187.905001 100.075001)
    (thickness 1.6)
    (drawings 4)
    (tracks 56)
    (zones 0)
    (modules 9)
    (nets 9)
  )
  (page User 210.007 148.006)
  (title_block
    (title "Relais Modul")
    (date 2001-01-01)
    (company "Paul Brenner")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.9)
    (zone_45_only yes)
    (trace_min 0.4)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF6F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.400000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../../../platine/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(J1-Pad2)")
  (net 5 GND)
  (net 6 "Net-(J2-Pad1)")
  (net 7 "Net-(J2-Pad2)")
  (net 8 "Net-(Q1-Pad2)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(Q1-Pad2)")
  )
  (net_class "Dickere Leiterbahn" ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class "Sehr dick" ""
    (clearance 0.4)
    (trace_width 0.8)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Diodes_THT:D_DO-15_P5.08mm_Vertical_AnodeUp (layer F.Cu) (tedit 5877C982)
    (at 31.645 61.925)
    (descr "D, DO-15 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "D DO-15 series Axial Vertical pin pitch 5.08mm  length 7.6mm diameter 3.6mm")
    (fp_text reference D2 (at 2.54 -2.86) (layer F.SilkS))
    (fp_text value D (at 2.54 2.86) (layer F.Fab))
    (fp_text user K (at -2.56 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (model Diodes_THT.3dshapes/D_DO-15_P5.08mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:bornier3 (layer F.Cu) (tedit 58E390EE)
    (at 34.82 93.04)
    (descr "Bornier d'alimentation 3 pins")
    (tags DEV)
    (fp_text reference J1 (at 5.05 -4.65) (layer F.SilkS))
    (fp_text value Screw_1x03 (at 5.08 3.175) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 5.08 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 10.16 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 5 GND))
    (model Connectors.3dshapes/bornier3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:bornier2 (layer F.Cu) (tedit 58E390E2)
    (at 26 90 270)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference J2 (at 2.54 -5.08 270) (layer F.SilkS))
    (fp_text value Screw_1x02 (at 2 3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad2)"))
    (model Connectors.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Wide (layer F.Cu) (tedit 58E0D40A)
    (at 50.695 71.45)
    (descr "TO-92 leads molded, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference "" (at 2.54 -4.19) (layer F.SilkS) hide)
    (fp_text value 2N3904 (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.19 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 58DCECF5)
    (at 50.695 80.34 270)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 6.35 0 270) (layer F.SilkS))
    (fp_text value 1K (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 58DCECF2)
    (at 55.14 80.34 270)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 0 270) (layer F.SilkS))
    (fp_text value 10k (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 58DD0582)
    (at 44.98 75.26 270)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R3 (at 5.715 0 270) (layer F.SilkS))
    (fp_text value R (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 44.98 71.45 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -3.96 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module KICAD:Relays_Fujitsu-JV-KT-Series_RevE_03Apr2017 (layer F.Cu) (tedit 58E390C4)
    (at 31 76 270)
    (fp_text reference K1 (at 0 -6.5 270) (layer F.SilkS))
    (fp_text value RELAY (at 1 0 360) (layer F.Fab))
    (pad 14 thru_hole oval (at 7.62 3.81 270) (size 5.5 3.5) (drill 1.4) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 -2.54 270) (size 5.5 3.5) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad1)"))
    (pad A2 thru_hole oval (at -7.6 3.8 270) (size 5.5 3.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad A1 thru_hole oval (at -7.6 -3.8 270) (size 5.5 3.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 +5V))
  )
  (gr_line (start 60.855 58.115) (end 19.58 58.115) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.855 100.025) (end 60.855 58.115) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 19.58 58.115) (end 19.58 100.025) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 19.58 100.025) (end 60.855 100.025) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.9))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.65) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 61 100) (xy 20 100) (xy 20 58) (xy 61 58)
      )
    )
  )
)
