(module DEMO_LQFP-100_14x14mm_Pitch0.5mm (layer F.Cu) (tedit 59BC2E3D)
  (descr "LQFP100: plastic low profile quad flat package; 100 leads; body 14 x 14 x 1.4 mm (see NXP sot407-1_po.pdf and sot407-1_fr.pdf)")
  (tags "QFP 0.5")
  (attr smd)
  (fp_text reference REF** (at 0 -9.65) (layer F.SilkS))
  (fp_text value LQFP-100_14x14mm_Pitch0.5mm (at 0 9.65) (layer F.Fab))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (pad 1 thru_hole rect (at -7.9 -6) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 2 thru_hole rect (at -7.9 -5.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 3 thru_hole rect (at -7.9 -5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 4 thru_hole rect (at -7.9 -4.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 5 thru_hole rect (at -7.9 -4) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 6 thru_hole rect (at -7.9 -3.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 7 thru_hole rect (at -7.9 -3) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 8 thru_hole rect (at -7.9 -2.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 9 thru_hole rect (at -7.9 -2) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 10 thru_hole rect (at -7.9 -1.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 11 thru_hole rect (at -7.9 -1) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 12 thru_hole rect (at -7.9 -0.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 13 thru_hole rect (at -7.9 0) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 14 thru_hole rect (at -7.9 0.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 15 thru_hole rect (at -7.9 1) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 16 thru_hole rect (at -7.9 1.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 17 thru_hole rect (at -7.9 2) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 18 thru_hole rect (at -7.9 2.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 19 thru_hole rect (at -7.9 3) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 20 thru_hole rect (at -7.9 3.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 21 thru_hole rect (at -7.9 4) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 22 thru_hole rect (at -7.9 4.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 23 thru_hole rect (at -7.9 5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 24 thru_hole rect (at -7.9 5.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 25 thru_hole rect (at -7.9 6) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 26 thru_hole rect (at -6 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 27 thru_hole rect (at -5.5 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 28 thru_hole rect (at -5 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 29 thru_hole rect (at -4.5 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 30 thru_hole rect (at -4 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 31 thru_hole rect (at -3.5 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 32 thru_hole rect (at -3 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 33 thru_hole rect (at -2.5 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 34 thru_hole rect (at -2 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 35 thru_hole rect (at -1.5 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 36 thru_hole rect (at -1 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 37 thru_hole rect (at -0.5 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 38 thru_hole rect (at 0 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 39 thru_hole rect (at 0.5 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 40 thru_hole rect (at 1 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 41 thru_hole rect (at 1.5 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 42 thru_hole rect (at 2 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 43 thru_hole rect (at 2.5 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 44 thru_hole rect (at 3 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 45 thru_hole rect (at 3.5 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 46 thru_hole rect (at 4 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 47 thru_hole rect (at 4.5 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 48 thru_hole rect (at 5 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 49 thru_hole rect (at 5.5 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 50 thru_hole rect (at 6 7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 51 thru_hole rect (at 7.9 6) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 52 thru_hole rect (at 7.9 5.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 53 thru_hole rect (at 7.9 5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 54 thru_hole rect (at 7.9 4.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 55 thru_hole rect (at 7.9 4) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 56 thru_hole rect (at 7.9 3.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 57 thru_hole rect (at 7.9 3) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 58 thru_hole rect (at 7.9 2.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 59 thru_hole rect (at 7.9 2) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 60 thru_hole rect (at 7.9 1.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 61 thru_hole rect (at 7.9 1) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 62 thru_hole rect (at 7.9 0.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 63 thru_hole rect (at 7.9 0) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 64 thru_hole rect (at 7.9 -0.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 65 thru_hole rect (at 7.9 -1) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 66 thru_hole rect (at 7.9 -1.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 67 thru_hole rect (at 7.9 -2) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 68 thru_hole rect (at 7.9 -2.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 69 thru_hole rect (at 7.9 -3) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 70 thru_hole rect (at 7.9 -3.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 71 thru_hole rect (at 7.9 -4) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 72 thru_hole rect (at 7.9 -4.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 73 thru_hole rect (at 7.9 -5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 74 thru_hole rect (at 7.9 -5.5) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 75 thru_hole rect (at 7.9 -6) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 76 thru_hole rect (at 6 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 77 thru_hole rect (at 5.5 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 78 thru_hole rect (at 5 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 79 thru_hole rect (at 4.5 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 80 thru_hole rect (at 4 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 81 thru_hole rect (at 3.5 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 82 thru_hole rect (at 3 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 83 thru_hole rect (at 2.5 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 84 thru_hole rect (at 2 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 85 thru_hole rect (at 1.5 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 86 thru_hole rect (at 1 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 87 thru_hole rect (at 0.5 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 88 thru_hole rect (at 0 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 89 thru_hole rect (at -0.5 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 90 thru_hole rect (at -1 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 91 thru_hole rect (at -1.5 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 92 thru_hole rect (at -2 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 93 thru_hole rect (at -2.5 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 94 thru_hole rect (at -3 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 95 thru_hole rect (at -3.5 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 96 thru_hole rect (at -4 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 97 thru_hole rect (at -4.5 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 98 thru_hole rect (at -5 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 99 thru_hole rect (at -5.5 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (pad 100 thru_hole rect (at -6 -7.9 90) (size 1.5 0.28) (drill 0.254) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Housings_QFP.3dshapes/LQFP-100_14x14mm_Pitch0.5mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
