(module LED_LT-G6SP_Osram_RevA_07Nov2017 (layer F.Cu) (tedit 5A021A54)
  (fp_text reference H (at 0 5.25) (layer F.SilkS))
  (fp_text value LED_LT-G6SP_Osram_RevB_07Nov2017 (at -0.05 -6) (layer F.Fab) hide)
  (pad 4 smd roundrect (at 0 0) (size 1.6 0.8) (layers F.Adhes)(roundrect_rratio 0.25))
  (pad 1 smd rect (at -2.15 2.2) (size 3 3) (layers F.Cu))
  (pad 1 smd rect (at 2.15 2.2) (size 3 3) (layers F.Cu))
  (pad 1 smd rect (at 2.15 -2.2) (size 3 3) (layers F.Cu))
  (pad 1 smd rect (at -2.15 -2.2) (size 3 3) (layers F.Cu))
  (pad 3 smd rect (at 0 1.525) (size 0.6 1.65) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin -0.001))
  (pad 2 smd rect (at 0 -1.525) (size 0.6 1.65) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin -0.001))
  (pad 1 smd rect (at 1.05 -1.525) (size 0.8 1.65) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin -0.001))
  (pad 1 smd rect (at 1.05 1.525) (size 0.8 1.65) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin -0.001))
  (pad 1 smd rect (at -1.05 -1.525) (size 0.8 1.65) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin -0.001))
  (pad 1 smd rect (at -1.05 1.525) (size 0.8 1.65) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin -0.001))
)
