(module LED_Osram_Adv_TOPLED (layer F.Cu) (tedit 5A0550E3)
  (fp_text reference REF** (at 0 -3) (layer F.SilkS))
  (fp_text value VAL** (at 0 3) (layer F.Fab))
  (pad 2 smd rect (at 2.15 2.2) (size 3 3) (layers F.Cu))
  (pad DNC smd rect (at 0 2.2) (size 0.6 3) (layers F.Cu)
    (zone_connect 0))
  (pad 2 smd rect (at -2.15 2.2) (size 3 3) (layers F.Cu))
  (pad 2 smd rect (at -2.15 -2.2) (size 3 3) (layers F.Cu))
  (pad 2 smd rect (at 2.15 -2.2) (size 3 3) (layers F.Cu))
  (pad 1 smd rect (at 0 -2.2) (size 0.6 3) (layers F.Cu))
  (pad 2 smd rect (at -0.95 -1.425) (size 0.6 1.45) (layers F.Mask))
  (pad 2 smd rect (at 0.95 -1.425) (size 0.6 1.45) (layers F.Mask))
  (pad 2 smd rect (at 0.95 1.425) (size 0.6 1.45) (layers F.Mask))
  (pad 2 smd rect (at -0.95 1.425) (size 0.6 1.45) (layers F.Mask))
  (pad DNC smd rect (at 0 1.425) (size 0.6 1.45) (layers F.Mask))
  (pad 1 smd rect (at 0 -1.425) (size 0.6 1.45) (layers F.Mask))
  (pad 2 smd rect (at -1.05 -1.525) (size 0.8 1.65) (layers F.Paste))
  (pad 2 smd rect (at 1.05 -1.525) (size 0.8 1.65) (layers F.Paste))
  (pad 2 smd rect (at 1.05 1.525) (size 0.8 1.65) (layers F.Paste))
  (pad 2 smd rect (at -1.05 1.525) (size 0.8 1.65) (layers F.Paste))
  (pad 1 smd rect (at 0 -1.525) (size 0.6 1.65) (layers F.Paste))
  (pad DNC smd rect (at 0 1.525) (size 0.6 1.65) (layers F.Paste))
  (model C:/Users/Florian/Documents/Projekte/shared_soft/kicad_libs.pretty/LED_Osram_Adv_TOPLED.wrl
    (at (xyz 0 0 0.06900000000000001))
    (scale (xyz 0.393701 0.393701 0.393701))
    (rotate (xyz 0 0 0))
  )
)
