<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<packages>
<package name="LQFP-144">
<description>LQFP 144-Pin</description>
</package>
</packages>
<symbols>
<symbol name="AT32UC3C-144">
<pin name="PD02"/>
<pin name="PD03"/>
<pin name="PD01"/>
<pin name="PD04"/>
<pin name="PD00"/>
<pin name="PD05"/>
<pin name="PD06"/>
<pin name="PD07"/>
<pin name="PD08"/>
<pin name="PD09"/>
<pin name="PD10"/>
<pin name="VDDIO3" direction="pwr"/>
<pin name="GNDIO3" direction="pwr"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PD16"/>
<pin name="PD17"/>
<pin name="PD18"/>
<pin name="PD19"/>
<pin name="PD20"/>
<pin name="PD21"/>
<pin name="PD22"/>
<pin name="PD23"/>
<pin name="PD24"/>
<pin name="PD25"/>
<pin name="PD26"/>
<pin name="PD27"/>
<pin name="PD28"/>
<pin name="PD29"/>
<pin name="PD30"/>
<pin name="PB00"/>
<pin name="PB01"/>
<pin name="RESET"/>
<pin name="PB02"/>
<pin name="PB03"/>
<pin name="PA00"/>
<pin name="PA01"/>
<pin name="PA02"/>
<pin name="PA03"/>
<pin name="VDDIO1" direction="pwr"/>
<pin name="GNDIO1" direction="pwr"/>
<pin name="PB04"/>
<pin name="PB05"/>
<pin name="PB06"/>
<pin name="PB07"/>
<pin name="PB08"/>
<pin name="PB09"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PB16"/>
<pin name="PB17"/>
<pin name="PA04"/>
<pin name="PA05"/>
<pin name="PA06"/>
<pin name="PA07"/>
<pin name="PA08"/>
<pin name="PA09"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PA16"/>
<pin name="ADCVREFP" direction="pwr"/>
<pin name="ADCVREFN" direction="pwr"/>
<pin name="PA19"/>
<pin name="GNDANA" direction="pwr"/>
<pin name="VDDANA" direction="pwr"/>
<pin name="PA20"/>
<pin name="PA21"/>
<pin name="PA22"/>
<pin name="PA23"/>
<pin name="PA24"/>
<pin name="PA25"/>
<pin name="PA26"/>
<pin name="PA27"/>
<pin name="PA28"/>
<pin name="VBUS" direction="pwr"/>
<pin name="DM"/>
<pin name="DP"/>
<pin name="GNDPLL" direction="pwr"/>
<pin name="VDDIN_5" direction="pwr"/>
<pin name="VDDIN_33" direction="pwr"/>
<pin name="VDDCORE" direction="pwr"/>
<pin name="GNDCORE" direction="pwr"/>
<pin name="PB18"/>
<pin name="PB19"/>
<pin name="PB20"/>
<pin name="PB21"/>
<pin name="PB22"/>
<pin name="PB23"/>
<pin name="PB24"/>
<pin name="PB25"/>
<pin name="PB26"/>
<pin name="PB27"/>
<pin name="PB28"/>
<pin name="PB29"/>
<pin name="PB30"/>
<pin name="PB31"/>
<pin name="PC00"/>
<pin name="PC01"/>
<pin name="PC02"/>
<pin name="PC03"/>
<pin name="GNDIO2" direction="pwr"/>
<pin name="VDDIO2" direction="pwr"/>
<pin name="PC04"/>
<pin name="PC05"/>
<pin name="PC06"/>
<pin name="PC07"/>
<pin name="PC08"/>
<pin name="PC09"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC16"/>
<pin name="PC17"/>
<pin name="PC18"/>
<pin name="PC19"/>
<pin name="PC20"/>
<pin name="PC21"/>
<pin name="PC22"/>
<pin name="PC23"/>
<pin name="PC24"/>
<pin name="PC25"/>
<pin name="PC26"/>
<pin name="PC27"/>
<pin name="PC28"/>
<pin name="PC29"/>
<pin name="VDDIO4" direction="pwr"/>
<pin name="GNDIO4" direction="pwr"/>
<pin name="PC30"/>
<pin name="PC31"/>
<pin name="PA29"/>
</symbol>
<symbol name="MC9S12-144PIN">
<pin name="PP3"/>
<pin name="PP2"/>
<pin name="PP1"/>
<pin name="PP0"/>
<pin name="PK3"/>
<pin name="PK1"/>
<pin name="PK2"/>
<pin name="PK0"/>
<pin name="PT0"/>
<pin name="PT1"/>
<pin name="PT2"/>
<pin name="PT3"/>
<pin name="VDD1" direction="pwr"/>
<pin name="VSS1" direction="pwr"/>
<pin name="PT4"/>
<pin name="PT5"/>
<pin name="PT6"/>
<pin name="PT7"/>
<pin name="PK4"/>
<pin name="PK5"/>
<pin name="PJ1"/>
<pin name="PJ0"/>
<pin name="BKGD"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PH7"/>
<pin name="PH6"/>
<pin name="PH5"/>
<pin name="PH4"/>
<pin name="PE7"/>
<pin name="PE6"/>
<pin name="PE5"/>
<pin name="PE4"/>
<pin name="VSSR1" direction="pwr"/>
<pin name="VDDR1" direction="pwr"/>
<pin name="!RESET"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="XFC"/>
<pin name="VSSPLL" direction="pwr"/>
<pin name="EXTAL" direction="pas"/>
<pin name="XTAL" direction="pas"/>
<pin name="TEST" direction="pas"/>
<pin name="PH1"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE0"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="VSSR2" direction="pwr"/>
<pin name="VDDR2" direction="pwr"/>
<pin name="PAD00"/>
<pin name="PAD01"/>
<pin name="PAD02"/>
<pin name="PAD03"/>
<pin name="PAD04"/>
<pin name="PAD05"/>
<pin name="PAD06"/>
<pin name="PAD07"/>
<pin name="PAD08"/>
<pin name="PAD09"/>
<pin name="PAD10"/>
<pin name="PAD11"/>
<pin name="PAD12"/>
<pin name="PAD13"/>
<pin name="PAD14"/>
<pin name="PAD15"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VRH" direction="pas"/>
<pin name="VRL" direction="pas"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PM7"/>
<pin name="PM6"/>
<pin name="PS0"/>
<pin name="PS1"/>
<pin name="PS2"/>
<pin name="PS3"/>
<pin name="PS4"/>
<pin name="PS5"/>
<pin name="PS6"/>
<pin name="PS7"/>
<pin name="VREGEN" direction="in"/>
<pin name="PJ7"/>
<pin name="PJ6"/>
<pin name="PM1"/>
<pin name="PM2"/>
<pin name="PM3"/>
<pin name="PM4"/>
<pin name="PM5"/>
<pin name="PM0"/>
<pin name="VSSX1" direction="pwr"/>
<pin name="VDDX1" direction="pwr"/>
<pin name="PP4"/>
<pin name="PP5"/>
<pin name="PP6"/>
<pin name="PP7"/>
<pin name="PK7"/>
<pin name="PJ2"/>
<pin name="PK6"/>
<pin name="VDDX2" direction="pwr"/>
<pin name="VSSX2" direction="pwr"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="VDD2" direction="pwr"/>
<pin name="VSS2" direction="pwr"/>
<pin name="PAD16"/>
<pin name="PAD17"/>
<pin name="PAD18"/>
<pin name="PAD19"/>
<pin name="PAD20"/>
<pin name="PAD21"/>
<pin name="PAD22"/>
<pin name="PAD23"/>
<pin name="PJ5"/>
<pin name="PJ4"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AT32UC3C" prefix="VD" uservalue="yes">
<description>Atmel AT32UC3C Mikrocontroller</description>
<gates>
<gate name="VD" symbol="AT32UC3C-144"/>
</gates>
<devices>
<device name="LQFP-144" package="LQFP-144">
<connects>
<connect gate="VD" pin="ADCVREFN" pad="35"/>
<connect gate="VD" pin="ADCVREFP" pad="34"/>
<connect gate="VD" pin="DM" pad="50"/>
<connect gate="VD" pin="DP" pad="51"/>
<connect gate="VD" pin="GNDANA" pad="37"/>
<connect gate="VD" pin="GNDCORE" pad="56"/>
<connect gate="VD" pin="GNDIO1" pad="6"/>
<connect gate="VD" pin="GNDIO2" pad="76"/>
<connect gate="VD" pin="GNDIO3" pad="119"/>
<connect gate="VD" pin="GNDIO4" pad="104"/>
<connect gate="VD" pin="GNDPLL" pad="52"/>
<connect gate="VD" pin="PA00" pad="1"/>
<connect gate="VD" pin="PA01" pad="2"/>
<connect gate="VD" pin="PA02" pad="3"/>
<connect gate="VD" pin="PA03" pad="4"/>
<connect gate="VD" pin="PA04" pad="21"/>
<connect gate="VD" pin="PA05" pad="22"/>
<connect gate="VD" pin="PA06" pad="23"/>
<connect gate="VD" pin="PA07" pad="24"/>
<connect gate="VD" pin="PA08" pad="25"/>
<connect gate="VD" pin="PA09" pad="26"/>
<connect gate="VD" pin="PA10" pad="27"/>
<connect gate="VD" pin="PA11" pad="28"/>
<connect gate="VD" pin="PA12" pad="29"/>
<connect gate="VD" pin="PA13" pad="30"/>
<connect gate="VD" pin="PA14" pad="31"/>
<connect gate="VD" pin="PA15" pad="32"/>
<connect gate="VD" pin="PA16" pad="33"/>
<connect gate="VD" pin="PA19" pad="36"/>
<connect gate="VD" pin="PA20" pad="39"/>
<connect gate="VD" pin="PA21" pad="40"/>
<connect gate="VD" pin="PA22" pad="41"/>
<connect gate="VD" pin="PA23" pad="42"/>
<connect gate="VD" pin="PA24" pad="43"/>
<connect gate="VD" pin="PA25" pad="44"/>
<connect gate="VD" pin="PA26" pad="45"/>
<connect gate="VD" pin="PA27" pad="46"/>
<connect gate="VD" pin="PA28" pad="47"/>
<connect gate="VD" pin="PA29" pad="48"/>
<connect gate="VD" pin="PB00" pad="140"/>
<connect gate="VD" pin="PB01" pad="141"/>
<connect gate="VD" pin="PB02" pad="143"/>
<connect gate="VD" pin="PB03" pad="144"/>
<connect gate="VD" pin="PB04" pad="7"/>
<connect gate="VD" pin="PB05" pad="8"/>
<connect gate="VD" pin="PB06" pad="9"/>
<connect gate="VD" pin="PB07" pad="10"/>
<connect gate="VD" pin="PB08" pad="11"/>
<connect gate="VD" pin="PB09" pad="12"/>
<connect gate="VD" pin="PB10" pad="13"/>
<connect gate="VD" pin="PB11" pad="14"/>
<connect gate="VD" pin="PB12" pad="15"/>
<connect gate="VD" pin="PB13" pad="16"/>
<connect gate="VD" pin="PB14" pad="17"/>
<connect gate="VD" pin="PB15" pad="18"/>
<connect gate="VD" pin="PB16" pad="19"/>
<connect gate="VD" pin="PB17" pad="20"/>
<connect gate="VD" pin="PB18" pad="57"/>
<connect gate="VD" pin="PB19" pad="58"/>
<connect gate="VD" pin="PB20" pad="59"/>
<connect gate="VD" pin="PB21" pad="60"/>
<connect gate="VD" pin="PB22" pad="61"/>
<connect gate="VD" pin="PB23" pad="62"/>
<connect gate="VD" pin="PB24" pad="63"/>
<connect gate="VD" pin="PB25" pad="64"/>
<connect gate="VD" pin="PB26" pad="65"/>
<connect gate="VD" pin="PB27" pad="66"/>
<connect gate="VD" pin="PB28" pad="67"/>
<connect gate="VD" pin="PB29" pad="68"/>
<connect gate="VD" pin="PB30" pad="69"/>
<connect gate="VD" pin="PB31" pad="70"/>
<connect gate="VD" pin="PC00" pad="71"/>
<connect gate="VD" pin="PC01" pad="72"/>
<connect gate="VD" pin="PC02" pad="73"/>
<connect gate="VD" pin="PC03" pad="74"/>
<connect gate="VD" pin="PC04" pad="77"/>
<connect gate="VD" pin="PC05" pad="78"/>
<connect gate="VD" pin="PC06" pad="79"/>
<connect gate="VD" pin="PC07" pad="80"/>
<connect gate="VD" pin="PC08" pad="81"/>
<connect gate="VD" pin="PC09" pad="82"/>
<connect gate="VD" pin="PC10" pad="83"/>
<connect gate="VD" pin="PC11" pad="84"/>
<connect gate="VD" pin="PC12" pad="85"/>
<connect gate="VD" pin="PC13" pad="86"/>
<connect gate="VD" pin="PC14" pad="87"/>
<connect gate="VD" pin="PC15" pad="88"/>
<connect gate="VD" pin="PC16" pad="89"/>
<connect gate="VD" pin="PC17" pad="90"/>
<connect gate="VD" pin="PC18" pad="91"/>
<connect gate="VD" pin="PC19" pad="92"/>
<connect gate="VD" pin="PC20" pad="93"/>
<connect gate="VD" pin="PC21" pad="94"/>
<connect gate="VD" pin="PC22" pad="95"/>
<connect gate="VD" pin="PC23" pad="96"/>
<connect gate="VD" pin="PC24" pad="97"/>
<connect gate="VD" pin="PC25" pad="98"/>
<connect gate="VD" pin="PC26" pad="99"/>
<connect gate="VD" pin="PC27" pad="100"/>
<connect gate="VD" pin="PC28" pad="101"/>
<connect gate="VD" pin="PC29" pad="102"/>
<connect gate="VD" pin="PC30" pad="105"/>
<connect gate="VD" pin="PC31" pad="106"/>
<connect gate="VD" pin="PD00" pad="107"/>
<connect gate="VD" pin="PD01" pad="108"/>
<connect gate="VD" pin="PD02" pad="109"/>
<connect gate="VD" pin="PD03" pad="110"/>
<connect gate="VD" pin="PD04" pad="111"/>
<connect gate="VD" pin="PD05" pad="112"/>
<connect gate="VD" pin="PD06" pad="113"/>
<connect gate="VD" pin="PD07" pad="114"/>
<connect gate="VD" pin="PD08" pad="115"/>
<connect gate="VD" pin="PD09" pad="116"/>
<connect gate="VD" pin="PD10" pad="117"/>
<connect gate="VD" pin="PD11" pad="120"/>
<connect gate="VD" pin="PD12" pad="121"/>
<connect gate="VD" pin="PD13" pad="122"/>
<connect gate="VD" pin="PD14" pad="123"/>
<connect gate="VD" pin="PD15" pad="124"/>
<connect gate="VD" pin="PD16" pad="125"/>
<connect gate="VD" pin="PD17" pad="126"/>
<connect gate="VD" pin="PD18" pad="127"/>
<connect gate="VD" pin="PD19" pad="128"/>
<connect gate="VD" pin="PD20" pad="129"/>
<connect gate="VD" pin="PD21" pad="130"/>
<connect gate="VD" pin="PD22" pad="131"/>
<connect gate="VD" pin="PD23" pad="132"/>
<connect gate="VD" pin="PD24" pad="133"/>
<connect gate="VD" pin="PD25" pad="134"/>
<connect gate="VD" pin="PD26" pad="135"/>
<connect gate="VD" pin="PD27" pad="136"/>
<connect gate="VD" pin="PD28" pad="137"/>
<connect gate="VD" pin="PD29" pad="138"/>
<connect gate="VD" pin="PD30" pad="139"/>
<connect gate="VD" pin="RESET" pad="142"/>
<connect gate="VD" pin="VBUS" pad="49"/>
<connect gate="VD" pin="VDDANA" pad="38"/>
<connect gate="VD" pin="VDDCORE" pad="55"/>
<connect gate="VD" pin="VDDIN_33" pad="54"/>
<connect gate="VD" pin="VDDIN_5" pad="53"/>
<connect gate="VD" pin="VDDIO1" pad="5"/>
<connect gate="VD" pin="VDDIO2" pad="75"/>
<connect gate="VD" pin="VDDIO3" pad="118"/>
<connect gate="VD" pin="VDDIO4" pad="103"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC9S12XD-144" prefix="VD" uservalue="yes">
<description>MC9S12XD-144</description>
<gates>
<gate name="VD" symbol="MC9S12-144PIN"/>
</gates>
<devices>
<device name="LQFP-144" package="LQFP-144">
<connects>
<connect gate="VD" pin="!RESET" pad="54"/>
<connect gate="VD" pin="BKGD" pad="25"/>
<connect gate="VD" pin="EXTAL" pad="58"/>
<connect gate="VD" pin="PA0" pad="73"/>
<connect gate="VD" pin="PA1" pad="74"/>
<connect gate="VD" pin="PA2" pad="75"/>
<connect gate="VD" pin="PA3" pad="76"/>
<connect gate="VD" pin="PA4" pad="77"/>
<connect gate="VD" pin="PA5" pad="78"/>
<connect gate="VD" pin="PA6" pad="79"/>
<connect gate="VD" pin="PA7" pad="80"/>
<connect gate="VD" pin="PAD00" pad="89"/>
<connect gate="VD" pin="PAD01" pad="91"/>
<connect gate="VD" pin="PAD02" pad="93"/>
<connect gate="VD" pin="PAD03" pad="95"/>
<connect gate="VD" pin="PAD04" pad="97"/>
<connect gate="VD" pin="PAD05" pad="99"/>
<connect gate="VD" pin="PAD06" pad="101"/>
<connect gate="VD" pin="PAD07" pad="103"/>
<connect gate="VD" pin="PAD08" pad="90"/>
<connect gate="VD" pin="PAD09" pad="92"/>
<connect gate="VD" pin="PAD10" pad="94"/>
<connect gate="VD" pin="PAD11" pad="96"/>
<connect gate="VD" pin="PAD12" pad="98"/>
<connect gate="VD" pin="PAD13" pad="100"/>
<connect gate="VD" pin="PAD14" pad="102"/>
<connect gate="VD" pin="PAD15" pad="104"/>
<connect gate="VD" pin="PAD16" pad="105"/>
<connect gate="VD" pin="PAD17" pad="106"/>
<connect gate="VD" pin="PAD18" pad="111"/>
<connect gate="VD" pin="PAD19" pad="112"/>
<connect gate="VD" pin="PAD20" pad="113"/>
<connect gate="VD" pin="PAD21" pad="114"/>
<connect gate="VD" pin="PAD22" pad="115"/>
<connect gate="VD" pin="PAD23" pad="116"/>
<connect gate="VD" pin="PB0" pad="32"/>
<connect gate="VD" pin="PB1" pad="33"/>
<connect gate="VD" pin="PB2" pad="34"/>
<connect gate="VD" pin="PB3" pad="35"/>
<connect gate="VD" pin="PB4" pad="36"/>
<connect gate="VD" pin="PB5" pad="37"/>
<connect gate="VD" pin="PB6" pad="38"/>
<connect gate="VD" pin="PB7" pad="39"/>
<connect gate="VD" pin="PC0" pad="28"/>
<connect gate="VD" pin="PC1" pad="29"/>
<connect gate="VD" pin="PC2" pad="30"/>
<connect gate="VD" pin="PC3" pad="31"/>
<connect gate="VD" pin="PC4" pad="40"/>
<connect gate="VD" pin="PC5" pad="41"/>
<connect gate="VD" pin="PC6" pad="42"/>
<connect gate="VD" pin="PC7" pad="43"/>
<connect gate="VD" pin="PD0" pad="65"/>
<connect gate="VD" pin="PD1" pad="66"/>
<connect gate="VD" pin="PD2" pad="67"/>
<connect gate="VD" pin="PD3" pad="68"/>
<connect gate="VD" pin="PD4" pad="83"/>
<connect gate="VD" pin="PD5" pad="84"/>
<connect gate="VD" pin="PD6" pad="85"/>
<connect gate="VD" pin="PD7" pad="86"/>
<connect gate="VD" pin="PE0" pad="72"/>
<connect gate="VD" pin="PE1" pad="71"/>
<connect gate="VD" pin="PE2" pad="70"/>
<connect gate="VD" pin="PE3" pad="69"/>
<connect gate="VD" pin="PE4" pad="51"/>
<connect gate="VD" pin="PE5" pad="50"/>
<connect gate="VD" pin="PE6" pad="49"/>
<connect gate="VD" pin="PE7" pad="48"/>
<connect gate="VD" pin="PH0" pad="64"/>
<connect gate="VD" pin="PH1" pad="63"/>
<connect gate="VD" pin="PH2" pad="62"/>
<connect gate="VD" pin="PH3" pad="61"/>
<connect gate="VD" pin="PH4" pad="47"/>
<connect gate="VD" pin="PH5" pad="46"/>
<connect gate="VD" pin="PH6" pad="45"/>
<connect gate="VD" pin="PH7" pad="44"/>
<connect gate="VD" pin="PJ0" pad="24"/>
<connect gate="VD" pin="PJ1" pad="23"/>
<connect gate="VD" pin="PJ2" pad="5"/>
<connect gate="VD" pin="PJ4" pad="131"/>
<connect gate="VD" pin="PJ5" pad="130"/>
<connect gate="VD" pin="PJ6" pad="129"/>
<connect gate="VD" pin="PJ7" pad="128"/>
<connect gate="VD" pin="PK0" pad="10"/>
<connect gate="VD" pin="PK1" pad="9"/>
<connect gate="VD" pin="PK2" pad="8"/>
<connect gate="VD" pin="PK3" pad="7"/>
<connect gate="VD" pin="PK4" pad="22"/>
<connect gate="VD" pin="PK5" pad="21"/>
<connect gate="VD" pin="PK6" pad="6"/>
<connect gate="VD" pin="PK7" pad="140"/>
<connect gate="VD" pin="PM0" pad="137"/>
<connect gate="VD" pin="PM1" pad="136"/>
<connect gate="VD" pin="PM2" pad="135"/>
<connect gate="VD" pin="PM3" pad="134"/>
<connect gate="VD" pin="PM4" pad="133"/>
<connect gate="VD" pin="PM5" pad="132"/>
<connect gate="VD" pin="PM6" pad="118"/>
<connect gate="VD" pin="PM7" pad="117"/>
<connect gate="VD" pin="PP0" pad="4"/>
<connect gate="VD" pin="PP1" pad="3"/>
<connect gate="VD" pin="PP2" pad="2"/>
<connect gate="VD" pin="PP3" pad="1"/>
<connect gate="VD" pin="PP4" pad="144"/>
<connect gate="VD" pin="PP5" pad="143"/>
<connect gate="VD" pin="PP6" pad="142"/>
<connect gate="VD" pin="PP7" pad="141"/>
<connect gate="VD" pin="PS0" pad="119"/>
<connect gate="VD" pin="PS1" pad="120"/>
<connect gate="VD" pin="PS2" pad="121"/>
<connect gate="VD" pin="PS3" pad="122"/>
<connect gate="VD" pin="PS4" pad="123"/>
<connect gate="VD" pin="PS5" pad="124"/>
<connect gate="VD" pin="PS6" pad="125"/>
<connect gate="VD" pin="PS7" pad="126"/>
<connect gate="VD" pin="PT0" pad="11"/>
<connect gate="VD" pin="PT1" pad="12"/>
<connect gate="VD" pin="PT2" pad="13"/>
<connect gate="VD" pin="PT3" pad="14"/>
<connect gate="VD" pin="PT4" pad="17"/>
<connect gate="VD" pin="PT5" pad="18"/>
<connect gate="VD" pin="PT6" pad="19"/>
<connect gate="VD" pin="PT7" pad="20"/>
<connect gate="VD" pin="TEST" pad="60"/>
<connect gate="VD" pin="VDD1" pad="15"/>
<connect gate="VD" pin="VDD2" pad="87"/>
<connect gate="VD" pin="VDDA" pad="107"/>
<connect gate="VD" pin="VDDPLL" pad="55"/>
<connect gate="VD" pin="VDDR1" pad="53"/>
<connect gate="VD" pin="VDDR2" pad="82"/>
<connect gate="VD" pin="VDDX1" pad="139"/>
<connect gate="VD" pin="VDDX2" pad="26"/>
<connect gate="VD" pin="VREGEN" pad="127"/>
<connect gate="VD" pin="VRH" pad="108"/>
<connect gate="VD" pin="VRL" pad="109"/>
<connect gate="VD" pin="VSS1" pad="16"/>
<connect gate="VD" pin="VSS2" pad="88"/>
<connect gate="VD" pin="VSSA" pad="110"/>
<connect gate="VD" pin="VSSPLL" pad="57"/>
<connect gate="VD" pin="VSSR1" pad="52"/>
<connect gate="VD" pin="VSSR2" pad="81"/>
<connect gate="VD" pin="VSSX1" pad="138"/>
<connect gate="VD" pin="VSSX2" pad="27"/>
<connect gate="VD" pin="XFC" pad="56"/>
<connect gate="VD" pin="XTAL" pad="59"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
