<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components, Power Magnetics, Signal &amp; Communications&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;

&lt;HR&gt;
Eagle Version 6, Library Revision 2017d, 2017-07-04&lt;br&gt;

&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-AMT_750082107">
<description>Analog Modem Transformer WE-AMT</description>
</package>
<package name="WE-AMT_750082111">
<description>Analog Modem Transformer WE-AMT</description>
</package>
<package name="WE-DAA">
<description>Analog Modem Transformer WE-AMT</description>
</package>
<package name="WE-AMT_7500718001">
<description>Analog Modem Transformer WE-AMT</description>
</package>
<package name="WE-AMT_7500718489">
<description>Analog Modem Transformer WE-AMT</description>
</package>
<package name="WE-ASI_L">
<description>SMD-Wire Wound Inductor WE-ASI</description>
</package>
<package name="WE-ASI_M">
<description>SMD-Wire Wound Inductor WE-ASI</description>
</package>
<package name="WE-ASI_SENSOR">
<description>&lt;b&gt;SMD-Wire Wound Inductor&lt;/b&gt;&lt;p&gt;
Especially designed for Automation Standard Interface applications&lt;br&gt;
- Specially constructed for sensors and actuators</description>
</package>
<package name="WE-BAL_0603">
<description>Multilayer Chip Baluns WE-BAL</description>
</package>
<package name="WE-BAL_0805">
<description>Multilayer Chip Baluns WE-BAL</description>
</package>
<package name="WE-BPF_0805_T1">
<description>Multilayer Chip Band -Pass Filter WE-BPF</description>
</package>
<package name="WE-BPF_1008_T5">
<description>Multilayer Chip Band -Pass Filter WE-BPF</description>
</package>
<package name="WE-BPF_1206_748333024">
<description>Multilayer Chip Band -Pass Filter WE-BPF</description>
</package>
<package name="WE-BPF_1206_T3">
<description>Multilayer Chip Band -Pass Filter WE-BPF</description>
</package>
<package name="WE-CAIR_4248">
<description>&lt;B&gt;Air Coil Inductor&lt;/b&gt;&lt;br&gt;
Size 4248&lt;br&gt;
Height 4.2mm Max</description>
</package>
<package name="WE-CBA_0402(W=1.5)">
<description>&lt;b&gt;WE-CBA_0402

&lt;/b&gt;&lt;br&gt;Size: 0402
&lt;b&gt;&lt;br&gt;WIDE BAND / HIGH SPEED: W=1.5</description>
</package>
<package name="WE-CBA_0402(W=2.2)">
<description>&lt;b&gt;WE-CBA_0402

&lt;/b&gt;&lt;br&gt;Size: 0402
&lt;b&gt;&lt;br&gt;HIGH CURRENT: W=2.2</description>
</package>
<package name="WE-CBA_0603(W=2.2)">
<description>&lt;b&gt;WE-CBA_0603

&lt;/b&gt;&lt;br&gt;Size: 0603
&lt;b&gt;&lt;br&gt;WIDE BAND / HIGH SPEED: W=2.2</description>
</package>
<package name="WE-CBA_0603(W=2.6)">
<description>&lt;b&gt;WE-CBA_0603

&lt;/b&gt;&lt;br&gt;Size: 0603
&lt;b&gt;&lt;br&gt;HIGH CURRENT: W=2.6</description>
</package>
<package name="WE-CBA_0805(W=3)">
<description>&lt;b&gt;WE-CBA_0805

&lt;/b&gt;&lt;br&gt;Size: 0805
&lt;b&gt;&lt;br&gt;WIDE BAND / HIGH SPEED: W=3</description>
</package>
<package name="WE-CBA_0805(W=4)">
<description>&lt;b&gt;WE-CBA_0805

&lt;/b&gt;&lt;br&gt;Size: 0805
&lt;b&gt;&lt;br&gt;HIGH CURRENT: W=4</description>
</package>
<package name="WE-CBA_1206(W=4.2)">
<description>&lt;b&gt;WE-CBA_1206

&lt;/b&gt;&lt;br&gt;Size: 1206
&lt;b&gt;&lt;br&gt;WIDE BAND / HIGH SPEED: W=4.2</description>
</package>
<package name="WE-CBA_1206(W=5.2)">
<description>&lt;b&gt;WE-CBA_1206

&lt;/b&gt;&lt;br&gt;Size: 1206
&lt;b&gt;&lt;br&gt;HIGH CURRENT: W=5.2</description>
</package>
<package name="WE-CBA_1806(W=5.5)">
<description>&lt;b&gt;WE-CBA_1806

&lt;/b&gt;&lt;br&gt;Size: 1806
&lt;b&gt;&lt;br&gt;WIDE BAND / HIGH SPEED: W=5.5</description>
</package>
<package name="WE-CBA_1806(W=6.5)">
<description>&lt;b&gt;WE-CBA_1806

&lt;/b&gt;&lt;br&gt;Size: 1806
&lt;b&gt;&lt;br&gt;HIGH CURRENT: W=6.5</description>
</package>
<package name="WE-CBF_HF_0603(W=2.2)">
<description>SMD Multilayer</description>
</package>
<package name="WE-CBF_HF_0402(W=1.5)">
<description>SMD Multilayer</description>
</package>
<package name="0805">
<description>SMD Multilayer</description>
</package>
<package name="1206">
<description>SMD Multilayer</description>
</package>
<package name="1210">
<description>SMD EMI Suppression Ferrite Beads WE-CBF</description>
</package>
<package name="1806">
<description>SMD Multilayer</description>
</package>
<package name="1812">
<description>SMD Multilayer</description>
</package>
<package name="WE-CFWI_1310">
<description>Coupled Flatwire Inductor WE-CFWI</description>
</package>
<package name="WE-CMBH_1.5MM">
<description>Common Mode Power Line Choke WE-CMBH</description>
</package>
<package name="WE-CMBH_1.2MM">
<description>Common Mode Power Line Choke WE-CMBH</description>
</package>
<package name="WE-CMBNC_L(WITHOUT-PINS)_7448040707">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : L Without Pins
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  32.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_L(WITHOUT-PINS)_7448041104">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : L Without Pins
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  32.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_L(WITHOUT-PINS)_7448041502">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : L Without Pins
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  32.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_L(WITHOUT-PINS)_7448041801">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : L Without Pins
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  32.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_L(WITHOUT-PINS)_7448042001">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : L Without Pins
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  32.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_L">
<description>&lt;B&gt;WE-CMBNC
Common Mode Power Line Choke</description>
</package>
<package name="WE-CMBNC_M(WITHOUT-PINS)_7448031002">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : M (Without pins)
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  25.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_M(WITHOUT-PINS)_7448031501">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : M (Without pins)
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  25.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_M">
</package>
<package name="WE-CMBNC_XL(WITHOUT-PINS)_7448050530">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : XL (Without Pins)
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  36.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_XL(WITHOUT-PINS)_7448051012">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : XL (Without Pins)
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  36.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_XL(WITHOUT-PINS)_7448051804">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : XL (Without Pins)
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  36.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_XL(WITHOUT-PINS)_7448052303">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : XL (Without Pins)
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  36.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_XL(WITHOUT-PINS)_7448052502">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : XL (Without Pins)
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  36.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_XL(WITHOUT-PINS)_7448053201">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : XL (Without Pins)
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  36.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_XL">
<description>&lt;B&gt;WE-CMBNC Common Mode Power Line
Choke</description>
</package>
<package name="WE-CMBNC_XS_744801XXXX">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : XS
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  16.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_XXL_7448060535">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : XXL
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  46.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_XXL_7448060620">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : XXL
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  46.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_XXL_7448060814">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : XXL
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  46.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_XXL_7448061309">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : XXL
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  46.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_XXL_7448061507">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : XXL
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  46.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_XXL_7448062105">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : XXL
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  46.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_XXL_7448062603">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : XXL
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  46.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMBNC_XXL_7448063801">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Common Mode Power Line Choke&lt;/B&gt;&lt;/font&gt;
&lt;PRE&gt;  SIZE : XXL
   &lt;/PRE&gt;
&lt;table border="1"&gt;
 
&lt;tr title="You are looking at Row 1" bgcolor="Silver"&gt;
    &lt;td&gt;&lt;font color="#0000FF"&gt;&lt;B&gt; Technical Data &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;td&gt; &lt;font color="#0000FF"&gt;&lt;B&gt; Values &lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
    &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt;Rated Voltage&lt;/td&gt;
    &lt;td&gt; 250VAC &lt;/td&gt;
  &lt;tr title="You are looking at Row 2" bgcolor="white"&gt;
    &lt;td&gt;Frequency&lt;/td&gt;
    &lt;td&gt; 50/60 Hz &lt;/td&gt;
 &lt;tr title="You are looking at Row 1" bgcolor="white"&gt;
    &lt;td&gt; Height &lt;/td&gt;
    &lt;td&gt;  46.0 mm (Max)&lt;/td&gt;
   &lt;/table&gt;</description>
</package>
<package name="WE-CMB_HC_S">
<description>Current Compensated Choke WE-CMB HC</description>
</package>
<package name="WE-CMB_L">
<description>Current Compensated Choke WE-CMB</description>
</package>
<package name="WE-CMB_M_744823601">
<description>Current Compensated Choke WE-CMB</description>
</package>
<package name="WE-CMB_NIZN_XS">
<description>Current Compensated Choke WE-CMB NiZn</description>
</package>
<package name="WE-CMB_NIZN_S">
<description>Current Compensated Choke WE-CMB NiZn</description>
</package>
<package name="WE-CMB_S">
<description>Current Compensated Choke WE-CMB</description>
</package>
<package name="WE-CMB_XL_7448251201">
<description>Current Compensated Choke WE-CMB</description>
</package>
<package name="WE-CMB_XS">
<description>Current Compensated Choke WE-CMB</description>
</package>
<package name="WE-CMB_XXL_7448261418">
<description>Current Compensated Choke WE-CMB</description>
</package>
<package name="WE-CMB_XXL_7448262013">
<description>Current Compensated Choke WE-CMB</description>
</package>
<package name="WE-CMB_XXL_7448262510">
<description>Current Compensated Choke WE-CMB</description>
</package>
<package name="WE-CMB_XXL_7448263505">
<description>Current Compensated Choke WE-CMB</description>
</package>
<package name="WE-CMS_7427520">
<description>&lt;B&gt;WE-CMS Common Mode SMD Bead&lt;/B&gt;&lt;BR&gt;</description>
</package>
<package name="WE-CMS_7427521">
<description>Common Mode SMD Bead WE-CMS</description>
</package>
<package name="WE-CNSW_0805">
<description>SMD Common Mode Noise Suppressor WE-CNSW</description>
</package>
<package name="WE-CNSW_1206">
<description>SMD Common Mode Noise Suppressor WE-CNSW</description>
</package>
<package name="WE-CNSW_0603">
<description>SMD Common Mode Noise Suppressor WE-CNSW</description>
</package>
<package name="WE-CNSW_1812">
<description>SMD Common Mode Noise Suppressor WE-CNSW</description>
</package>
<package name="WE-CNSW_HF_0504">
<description>&lt;b&gt;SMD Common Mode Line Filter&lt;/b&gt;&lt;br&gt;
Size 0504&lt;br&gt;
Height 0.9mm Max</description>
</package>
<package name="WE-CST">
<description>Current Sense Transformer WE-CST</description>
</package>
<package name="WE-DCT">
<description>Toroidal Double Power Choke WE-DCT</description>
</package>
<package name="WE-DD_7332">
<description>SMD-Shielded Coupled Inductor WE-DD</description>
</package>
<package name="WE-DD_1260/1280">
<description>SMD-Shielded Coupled Inductor WE-DD</description>
</package>
<package name="WE_EP7_SMD_8PIN">
<description>Transformer, EP7 SMD 8 Pin</description>
</package>
<package name="WE_EP13_SMD_9PIN">
<description>SMD-xDSL Transformer WE-DSL</description>
</package>
<package name="WE_EP13_THT_9PIN">
<description>SMD-xDSL Transformer WE-DSL</description>
</package>
<package name="WE_EPX9_SMD_8PIN">
<description>Transformer, EPX9 SMD 8 Pin</description>
</package>
<package name="WE_EP13_SMD_12PIN">
<description>Transformer,  EP13 SMD 12 Pin</description>
</package>
<package name="WE-EHPI">
<description>Energy Harvesting Power Inductor WE-EHPI</description>
</package>
<package name="WE-FAMI_8010_744750230150">
</package>
<package name="WE-FAMI_1012_744750340047">
</package>
<package name="WE-FAMI_1012_744750340150">
</package>
<package name="WE-FAMI_1215_744750460100">
</package>
<package name="WE-FAMI_1215_744750460220">
</package>
<package name="WE-FAMI_1280_744750420047">
</package>
<package name="WE-FAMI_1280_744750420068">
</package>
<package name="WE-FAMI_1280_744750420100">
</package>
<package name="WE-FAMI_1280_744750420150">
</package>
<package name="WE-FAMI_1280_744750420220">
</package>
<package name="WE-FAMI_1410_744750530047">
</package>
<package name="WE-FAMI_1410_744750530068">
</package>
<package name="WE-FAMI_1410_744750530100">
</package>
<package name="WE-FAMI_1415_744750560047">
</package>
<package name="WE-FAMI_1415_744750560100">
</package>
<package name="WE-FAMI_1415_744750560220">
</package>
<package name="WE-FAMI_8010_744750230030">
</package>
<package name="WE-FAMI_8010_744750230047">
</package>
<package name="WE-FAMI_8010_744750230068">
</package>
<package name="WE-FAMI_8010_744750230100">
</package>
<package name="WE_EP5_SMD_6PIN">
<description>Transformer, EP5 SMD 6 Pin</description>
</package>
<package name="WE_EP10_SMD_8PIN">
<description>Transformer, EP10 SMD 8 Pin</description>
</package>
<package name="WE_FB_EP7_DIMENSION2">
<description>Transformer, EP7* SMD 8Pin für WE-FB</description>
</package>
<package name="WE_FB_EP7_DIMENSION1">
<description>Transformer, EP7* SMD 8Pin für WE-FB</description>
</package>
<package name="WE_ER9.5_SMD_8PIN">
<description>Transformer, ER9.5 SMD 8 Pin</description>
</package>
<package name="WE_EE35/18/10_THT_HORIZONTAL_14PIN">
<description>Transformer, EE35/18/10 THT Horizontal 14Pin</description>
</package>
<package name="WE_EFD20_SMD_10PIN">
<description>Transformer, EFD20 SMD 10 Pin</description>
</package>
<package name="WE-FC_ET">
<description>Current Compensated Power Line Choke WE-FC</description>
</package>
<package name="WE-FC_UT">
<description>Current Compensated Power Line Choke WE-FC</description>
</package>
<package name="WE_ER11/5_SMD_12PIN">
<description>Transformer, ER11/5 SMD 12Pin</description>
</package>
<package name="WE_ER14.5/6_SMD_12PIN">
<description>Transformer, ER14.5/6 SMD 12Pin</description>
</package>
<package name="WE_EFD15_SMD_12PIN">
<description>Transformer, EFD15 SMD 12 Pin</description>
</package>
<package name="WE_EFD20_SMD_12PIN">
<description>Transformer, EFD20 SMD 12 Pin</description>
</package>
<package name="WE_FLEX+_ETD29">
<description>Transformer, ETD29 THT 14Pin</description>
</package>
<package name="WE_FLEX+_ETD34">
<description>Transformer, ETD34 THT 14Pin</description>
</package>
<package name="WE_FLEX+_ETD39">
<description>Transformer, ETD39 THT 16Pin</description>
</package>
<package name="WE-GDTI_EP7">
<description>&lt;B&gt;SMD Gate Drive Transformer&lt;/b&gt;&lt;br&gt;
Size EP7 &lt;BR&gt;
Height 11.00 mm Max</description>
</package>
<package name="WE-GF_1210">
<description>SMD Wire Wound Inductor WE-GF</description>
</package>
<package name="WE-GF_1812">
<description>SMD Wire Wound Inductor WE-GF</description>
</package>
<package name="WE-HCC_1210">
<description>SMD High Current Cube Inductor WE-HCC</description>
</package>
<package name="WE-HCC_1090">
<description>SMD High Current Cube Inductor WE-HCC</description>
</package>
<package name="WE-HCC_8070">
<description>SMD High Current Cube Inductor WE-HCC</description>
</package>
<package name="WE-HCF_2013">
<description>SMD High Current Inductor WE-HCF</description>
</package>
<package name="WE-HCF_2818">
<description>&lt;b&gt;WE-HCF SMD High Current Inductor</description>
</package>
<package name="WE-HCI_7030/7040/7050">
<description>SMD-Flat Wire High Current Inductor WE-HCI</description>
</package>
<package name="WE-HCI_1335">
<description>SMD-Flat Wire High Current Inductor WE-HCI</description>
</package>
<package name="WE-HCI_1050">
<description>SMD-Flat Wire High Current Inductor WE-HCI</description>
</package>
<package name="WE-HCI_1030">
<description>SMD Flat Wire High Current Inductor WE-HCI</description>
</package>
<package name="WE-HCI_1040">
<description>SMD-Flat Wire High Current Inductor WE-HCI</description>
</package>
<package name="WE-HCI_1350/1365">
<description>SMD-Flat Wire High Current Inductor WE-HCI</description>
</package>
<package name="WE-HCI_1890">
<description>SMD-Flat Wire High Current Inductor WE-HCI</description>
</package>
<package name="WE-HCI_2212">
<description>SMD Flat Wire High Current Inductor WE-HCI</description>
</package>
<package name="WE-HCM_7050">
<description>SMD High Current Flat Wire Power Inductor WE-HCM</description>
</package>
<package name="WE-HCM_1050">
<description>SMD High Current Flat Wire Power Inductor WE-HCM</description>
</package>
<package name="WE-HCM_7070">
<description>SMD High Current Flat Wire Power Inductor WE-HCM</description>
</package>
<package name="WE-HCM_1070">
<description>SMD High Current Flat Wire Power Inductor WE-HCM</description>
</package>
<package name="WE-HCM_1052">
<description>SMD High Current Flat Wire Power Inductor WE-HCM</description>
</package>
<package name="WE-HCM_1350">
<description>SMD High Current Flat Wire Power Inductor WE-HCM</description>
</package>
<package name="WE-HCM_1240">
<description>SMD High Current Flat Wire Power Inductor WE-HCM</description>
</package>
<package name="WE-HCM_1190">
<description>SMD High Current Flat Wire Power Inductor WE-HCM</description>
</package>
<package name="WE-HCM_1390">
<description>SMD High Current Flat Wire Power Inductor WE-HCM</description>
</package>
<package name="749024012">
<description>&lt;B&gt;MAX Height=12.70 mm</description>
</package>
<package name="749014010">
<description>&lt;B&gt;MAX Height=8.40 mm</description>
</package>
<package name="74901401X">
<description>&lt;B&gt;MAX Height=10.85 mm</description>
</package>
<package name="WE-ISDN">
<description>SMD T1/E1 Pri Transformer WE-ISDN</description>
</package>
<package name="WE-KI_0402A">
<description>SMD Wire Wound Ceramic Inductor WE-KI</description>
</package>
<package name="WE-KI_0603A">
<description>SMD Wire Wound Ceramic Inductor WE-KI</description>
</package>
<package name="WE-KI_0603C">
<description>SMD Wire Wound Ceramic Inductor WE-KI</description>
</package>
<package name="WE-KI_0805A">
<description>SMD Wire Wound Ceramic Inductor WE-KI</description>
</package>
<package name="WE-KI_0805C">
<description>SMD Wire Wound Ceramic Inductor WE-KI</description>
</package>
<package name="WE-KI_1008A">
<description>SMD Wire Wound Ceramic Inductor WE-KI</description>
</package>
<package name="7490101120">
<description>MAX Height=2.29mm</description>
</package>
<package name="749020020A">
<description>MAX Height = 7.70mm</description>
</package>
<package name="749020100">
<description>MAX Height = 2.16mm</description>
</package>
<package name="749022015">
<description>MAX Height = 10.26 mm</description>
</package>
<package name="749023010A">
<description>MAX Height = 6.5 mm</description>
</package>
<package name="749023015">
<description>MAX Height = 6.35 mm</description>
</package>
<package name="749023016">
<description>MAX Height = 6.35 mm</description>
</package>
<package name="749050010A">
<description>MAX Height = 6.32 mm</description>
</package>
<package name="WE-LF_612/SV">
<description>Current Compensated Choke WE-LF</description>
</package>
<package name="WE-LF_622/MV">
<description>Current Compensated Choke WE-LF</description>
</package>
<package name="WE-LF_632/LV">
<description>Current Compensated Choke WE-LF</description>
</package>
<package name="WE-LF_642/XV">
<description>Current Compensated Choke WE-LF</description>
</package>
<package name="WE-LF_662/SH">
<description>Current Compensated Choke WE-LF</description>
</package>
<package name="WE-LF_672/MH">
<description>Current Compensated Choke WE-LF</description>
</package>
<package name="WE-LF_682/LH">
<description>Current Compensated Choke WE-LF</description>
</package>
<package name="WE-LF_692/XH">
<description>Current Compensated Choke WE-LF</description>
</package>
<package name="WE-LF_SMD">
<description>Current Compensated Choke WE-LF SMD</description>
</package>
<package name="WE-LHMI_4020">
<description>SMD Power Inductor WE-LHMI</description>
</package>
<package name="WE-LHMI_7030/7050">
<description>SMD Power Inductor WE-LHMI</description>
</package>
<package name="WE-LHMI_1040">
<description>SMD Power Inductor WE-LHMI</description>
</package>
<package name="WE-LHMI_1335">
<description>SMD Power Inductor WE-LHMI</description>
</package>
<package name="WE-LLCR_ETD34">
<description>&lt;PRE&gt;&lt;font face=" Arial"&gt;size: ETD34
Height : 26mm max</description>
</package>
<package name="WE-LLCR_ETD39">
<description>&lt;PRE&gt;&lt;font face=" Arial"&gt;
size: ETD39
Height : 30mm max</description>
</package>
<package name="WE-LLCR_ETD44">
<description>&lt;PRE&gt;&lt;font face=" Arial"&gt;
size: ETD39
Height : 27.5mm max</description>
</package>
<package name="WE-LPF_0603">
<description>Multilayer Chip Low-Pass Filters WE-LPF</description>
</package>
<package name="WE-LPF_0805">
<description>Multilayer Chip Low-Pass Filters WE-LPF</description>
</package>
<package name="WE-LQ_L">
<description>SMD RF Inductor WE-LQ</description>
</package>
<package name="WE-LQ_M">
<description>SMD RF Inductor WE-LQ</description>
</package>
<package name="WE-LQS_3015">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor&lt;/b&gt;&lt;br&gt;
Size:3015&lt;br&gt;
Height :1.5mm Max&lt;/br&gt;</description>
</package>
<package name="WE-LQS_4018">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor&lt;/b&gt;&lt;br&gt;
Size:4018&lt;br&gt;
Height :1.8mm Max&lt;br&gt;</description>
</package>
<package name="WE-LQS_5040">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor&lt;/b&gt;&lt;br&gt;
Size:5040&lt;br&gt;
Height :4.0mm Max&lt;br&gt;</description>
</package>
<package name="WE-LQS_6028">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor&lt;/b&gt;&lt;br&gt;
Size 6028&lt;br&gt;
Height 2.8mm Max</description>
</package>
<package name="WE-LQS_8040">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor&lt;/b&gt;&lt;br&gt;
Size:8040&lt;br&gt;
Height :4.2mm Max&lt;br&gt;</description>
</package>
<package name="WE-MAIA_2506">
<description>WE-MAIA
&lt;br&gt;size: 2506
&lt;br&gt;no vias and traces in restricted area</description>
</package>
<package name="WE-MAIA_2508">
<description>WE-MAIA
&lt;br&gt;size: 2508
&lt;br&gt;no vias and traces in restricted area</description>
</package>
<package name="WE-MAIA_2510">
<description>WE-MAIA
&lt;br&gt;size: 2510
&lt;br&gt;no vias and traces in restricted area</description>
</package>
<package name="WE-MAIA_3010">
<description>WE-MAIA
&lt;br&gt;size: 3010
&lt;br&gt;no vias and traces in restricted area</description>
</package>
<package name="WE-MAIA_3012">
<description>WE-MAIA
&lt;br&gt;size: 3012
&lt;br&gt;no vias and traces in restricted area</description>
</package>
<package name="WE-MAIA_3015">
<description>WE-MAIA
&lt;br&gt;size: 3015
&lt;br&gt;no vias and traces in restricted area</description>
</package>
<package name="WE-MAPI_2506">
<description>&lt;pre&gt;
SMD Multilayer
Size 2506
Height:0.60 mm max</description>
</package>
<package name="WE-MAPI_1610">
<description>&lt;pre&gt;
SMD Multilayer
Size 1610
Height: 	 mm max</description>
</package>
<package name="WE-MAPI_2508">
<description>&lt;pre&gt;
SMD Multilayer
Size 2508
Height:0.80 mm max</description>
</package>
<package name="WE-MAPI_2510/2512">
<description>&lt;pre&gt;
SMD Multilayer
Size 2510
Height:1.00 mm max</description>
</package>
<package name="WE-MAPI_3012_STANDER">
<description>&lt;pre&gt;
SMD Multilayer
Size 3012
Height:1.20 mm max</description>
</package>
<package name="WE-MAPI_3015/3020">
<description>&lt;pre&gt;
SMD Multilayer
Size 3015
Height:1.50 mm max</description>
</package>
<package name="WE-MCA_7488910245">
<description>Multiplayer Chip Antenna WE-MCA</description>
</package>
<package name="WE-MCA_7488105XX/7488940245">
<description>Multiplayer Chip Antenna WE-MCA</description>
</package>
<package name="WE-MCA_7488930245">
<description>Multiplayer Chip Antenna WE-MCA</description>
</package>
<package name="WE-MCA_7488910043">
<description>Multilayer Chip Antenna --
433Mhz---50Ω</description>
</package>
<package name="WE-MCA_7488910092">
<description>Multilayer Chip Antenna WE-MCA</description>
</package>
<package name="WE-MCA_7488912455">
<description>Multilayer Chip Antenna WE-MCA</description>
</package>
<package name="WE-MCA_7488920245">
<description>Multiplayer Chip Antenna WE-MCA</description>
</package>
<package name="0201">
<description>SMD Multilayer</description>
</package>
<package name="0805A">
<description>SMD Multilayer</description>
</package>
<package name="WE-3WAY_74273001">
<description>Multiline EMI Suppression Ferrite WE-MLS</description>
</package>
<package name="WE-4WAY_74273002">
<description>Multiline EMI Suppression Ferrite WE-MLS</description>
</package>
<package name="WE-4WAY_742730021">
<description>Multiline EMI Suppression Ferrite WE-MLS</description>
</package>
<package name="WE-4WAY_742730022">
<description>Multiline EMI Suppression Ferrite WE-MLS</description>
</package>
<package name="WE-4WAY_742730023">
<description>Multiline EMI Suppression Ferrite WE-MLS</description>
</package>
<package name="WE-MPSB_1612">
<description>SMD Multilayer</description>
</package>
<package name="WE-MPSB_1812">
<description>SMD Multilayer</description>
</package>
<package name="WE-MPSB_2220">
<description>SMD Multilayer</description>
</package>
<package name="WE-MPSB_3312">
<description>SMD Multilayer</description>
</package>
<package name="WE-PBF_7427932">
<description>SMD EMI Suppression Ferrite Beads WE-PBF</description>
</package>
<package name="WE-PBF_7427930">
<description>SMD EMI Suppression Ferrite Beads WE-PBF</description>
</package>
<package name="WE-PBF_7427931">
<description>SMD EMI Suppression Ferrite Beads WE-PBF</description>
</package>
<package name="WE-PD_1260/1245/1280/1210">
<description>SMD-Shielded Power Inductor WE-PD</description>
</package>
<package name="WE-PD_7332/7345">
<description>SMD-Shielded Power Inductor WE-PD</description>
</package>
<package name="WE-PD_7332/7345_PLASTIC_BASE">
<description>SMD-Shielded Power Inductor WE-PD</description>
</package>
<package name="WE-PD_6033/6050_PLASTIC_BASE">
<description>SMD-Shielded Power Inductor WE-PD</description>
</package>
<package name="WE-PD_1030/1050">
<description>SMD-Shielded Power Inductors WE-PD</description>
</package>
<package name="WE-PD2_7850">
<description>SMD-Power Inductor WE-PD2</description>
</package>
<package name="WE-PD2_5848/5820">
<description>SMD-Power Inductor WE-PD2</description>
</package>
<package name="WE-PD2_4532">
<description>SMD-Power Inductor WE-PD2</description>
</package>
<package name="WE-PD2_1054">
<description>SMD-Power Inductor WE-PD2</description>
</package>
<package name="WE-PD2A_1054">
<description>WE-PD2A
&lt;BR&gt;size:1054
&lt;br&gt;no vias and rtaces in restricted area</description>
</package>
<package name="WE-PD2A_4532">
<description>WE-PD2A
&lt;BR&gt;size:4532
&lt;br&gt;no vias and rtaces in restricted area</description>
</package>
<package name="WE-PD2A_5848">
<description>WE-PD2A
&lt;BR&gt;size:5848
&lt;br&gt;no vias and rtaces in restricted area</description>
</package>
<package name="WE-PD2A_7850">
<description>WE-PD2A
&lt;BR&gt;size:7850
&lt;br&gt;no vias and rtaces in restricted area</description>
</package>
<package name="WE-PD2SR_7850">
<description>WE-PD2SR Shielded Power Inductor</description>
</package>
<package name="WE-PD3_S">
<description>SMD Power Inductor</description>
</package>
<package name="WE-PD3_X">
<description>SMD Power Inductor</description>
</package>
<package name="WE-PD3_L">
<description>SMD Power Inductor</description>
</package>
<package name="WE-PD3_M">
<description>SMD Power Inductor</description>
</package>
<package name="WE-PD4_XL">
<description>SMD Power Inductor</description>
</package>
<package name="WE-PDA_1210">
<description>&lt;b&gt;WE-PDA_1210
&lt;br&gt;Size 1210;
&lt;br&gt;
&lt;br&gt;no vias and traces in restricted area</description>
</package>
<package name="WE-PDA_1260">
<description>&lt;b&gt;WE-PDA_1260
&lt;br&gt;Size 1260;
&lt;br&gt;
&lt;br&gt;no vias and traces in restricted area</description>
</package>
<package name="WE-PDA_1280">
<description>&lt;b&gt;WE-PDA_1280
&lt;br&gt;Size 1280;
&lt;br&gt;
&lt;br&gt;no vias and traces in restricted area</description>
</package>
<package name="WE-PDA_7332">
<description>&lt;b&gt;WE-PDA_7332
&lt;br&gt;Size 7332;
&lt;br&gt;
&lt;br&gt;no vias and traces in restricted area</description>
</package>
<package name="WE-PDA_7345">
<description>&lt;b&gt;WE-PDA_7345
&lt;br&gt;Size 7345;
&lt;br&gt;
&lt;br&gt;no vias and traces in restricted area</description>
</package>
<package name="WE-PDF">
<description>SMD-Power Inductor WE-PDF</description>
</package>
<package name="WE-PD_HV_1060">
<description>High Voltage SMD Power Inductor WE-PD HV</description>
</package>
<package name="WE-PF_7427929XXX">
<description>SMD EMI Suppression Power Ferrite</description>
</package>
<package name="WE_EER28_THT_HORIZONTAL_9PIN">
<description>Transformer, EER28 THT Horizontal 9 Pins</description>
</package>
<package name="WE_EE20/10/6_THT_HORIZONTAL_10PIN">
<description>Transformer, EE20/10/6 THT Horizontal 10 Pin</description>
</package>
<package name="WE_RM10_THT_12PIN">
<description>WE RM10, 12 Pins</description>
</package>
<package name="WE_RM12_THT_12PIN">
<description>WE RM12, 12 Pins</description>
</package>
<package name="WE_RM14_THT_12PIN">
<description>WE RM14, 12 Pins</description>
</package>
<package name="WE_EFD25_THT_HORIZONTAL_10PIN">
<description>Transformer, EFD25 THT Horizontal 10Pins</description>
</package>
<package name="WE_EFD30_THT_12PIN">
<description>WE EFD30, 12 Pins</description>
</package>
<package name="WE_PQ38/11_6PIN">
<description>WE PQ38/11, 6 Pins</description>
</package>
<package name="WE-PMI_0805">
<description>Power Multilayer Inductor WE-PMI</description>
</package>
<package name="WE-PMI_0806">
<description>Power Multilayer Inductor WE-PMI</description>
</package>
<package name="WE-PMI_1008">
<description>Power Multilayer Inductor WE-PMI</description>
</package>
<package name="WE-PMI_0603">
<description>Power Multilayer Inductor WE-PMI</description>
</package>
<package name="WE_EP13_SMD_10PIN">
<description>Transformer,  EP13 SMD 10 Pin</description>
</package>
<package name="WE-PP_750031160">
<description>&lt;b&gt;WE-PP 750034460&lt;/b&gt;&lt;br&gt;&lt;br&gt;

- L= 500µH&lt;br&gt;
- Turns ration 1:2.7&lt;br&gt;&lt;br&gt;

-- for LTC1535/MAX3535</description>
</package>
<package name="WE-RFH">
<description>Ferrite SMD Inductance WE-RFH</description>
</package>
<package name="WE-RFI_0805A">
<description>Ferite SMD Inductance WE-RFI</description>
</package>
<package name="WE-RFI_1008A">
<description>Ferrite SMD Inductance WE-RFI</description>
</package>
<package name="7499010441">
</package>
<package name="7497110616">
<description>incomplete</description>
</package>
<package name="7497111611A">
<description>&lt;b&gt;MAX HEIGHT=13.50mm
&lt;pre&gt;
PORTS----1X1 + 2XUSB (USB2.0)
LED    -YES</description>
</package>
<package name="7499110122">
<description>&lt;b&gt;MAX HEIGHT=13.50mm
&lt;pre&gt;
PORTS----1X1
LED    -YES</description>
</package>
<package name="7499110123">
<description>&lt;b&gt;MAX HEIGHT=17.10mm
&lt;pre&gt;
PORTS----1X1
LED    -YES</description>
</package>
<package name="7499110124">
<description>&lt;b&gt;MAX HEIGHT=13.50mm
&lt;pre&gt;
PORTS----1X1
LED    --YES</description>
</package>
<package name="7499111000A">
<description>&lt;b&gt;MAX HEIGHT=15.79mm
&lt;pre&gt;
PORTS----1X1
LED    --NO</description>
</package>
<package name="7499111121A">
<description>&lt;b&gt;MAX HEIGHT=13.95mm
&lt;pre&gt;
PORTS----1X1
LED    --YES</description>
</package>
<package name="7499111221A">
<description>&lt;b&gt;MAX HEIGHT=15.79mm
&lt;pre&gt;
PORTS----1X1
LED    --YES</description>
</package>
<package name="7499111446">
<description>&lt;b&gt;MAX HEIGHT=13.95mm
&lt;pre&gt;
PORTS----1X1
LED    --YES</description>
</package>
<package name="7499111447">
<description>&lt;b&gt;MAX HEIGHT=13.55mm
&lt;pre&gt;
PORTS----1X1
LED    -YES</description>
</package>
<package name="7499151120">
<description>&lt;b&gt;MAX HEIGHT=26.0mm
&lt;pre&gt;
PORTS----1X2
LED    -YES</description>
</package>
<package name="7499511440">
<description>&lt;b&gt;MAX HEIGHT=13.87mm
&lt;pre&gt;
PORTS----1X1
LED    -YES</description>
</package>
<package name="7498111001">
<description>&lt;b&gt;MAX HEIGHT=13.55mm
&lt;pre&gt;
PORTS----1X1
LED    -NO</description>
</package>
<package name="7498111120R">
<description>&lt;b&gt;MAX HEIGHT=11.30mm
&lt;pre&gt;
PORTS----1X1
LED    --Yes</description>
</package>
<package name="74990-WITH-LED-TYPE2">
<description>&lt;b&gt;MAX HEIGHT=13.50mm
&lt;pre&gt;
PORTS----1X1
LED    ----YES</description>
</package>
<package name="74990-WITHOUT-LED-(21.84X16.2MM)">
<description>&lt;b&gt;MAX HEIGHT=13.74mm
&lt;pre&gt;
PORTS----1X1
LED    ----NO</description>
</package>
<package name="74990-WITHOUT-LED">
<description>&lt;b&gt;MAX HEIGHT=13.50mm
&lt;pre&gt;
PORTS----1X1
LED    ----NO</description>
</package>
<package name="7499010004A">
<description>&lt;b&gt;MAX HEIGHT=13.74mm
&lt;pre&gt;
PORTS----1X1
LED    --NO</description>
</package>
<package name="74990101210">
<description>&lt;b&gt;MAX HEIGHT=17.50mm
&lt;pre&gt;
VERTICAL MOUNT
PORTS----1X1
LED    --YES</description>
</package>
<package name="74990-WITH-LED">
<description>&lt;b&gt;MAX HEIGHT=13.50mm
&lt;pre&gt;
PORTS----1X1
LED    -YES</description>
</package>
<package name="74990-WITHOUT-LED-(21.84X15.88MM)">
<description>&lt;b&gt;MAX HEIGHT=13.95mm
&lt;pre&gt;
PORTS----1X1
LED    ----NO</description>
</package>
<package name="74990110030">
<description>&lt;b&gt;MAX HEIGHT=13.50mm
&lt;pre&gt;
PORTS----1X1
LED    --NO</description>
</package>
<package name="7499011121A">
<description>&lt;b&gt;MAX HEIGHT=13.90mm
&lt;pre&gt;
PORTS----1X1
LED    --YES</description>
</package>
<package name="7499021125-2PORTS-HORIZONTAL">
<description>&lt;b&gt;MAX HEIGHT=13.50mm
&lt;pre&gt;
PORTS----1X2 HORIZONTAL
LED    --YES</description>
</package>
<package name="7499031120A-4PORTS-HORIZONTAL">
<description>&lt;b&gt;MAX HEIGHT=13.50mm
&lt;pre&gt;
PORTS----1X4 HORIZONTAL
LED    --YES</description>
</package>
<package name="7499051002-1X2-STACKED">
<description>&lt;b&gt;MAX HEIGHT=25.20mm
&lt;pre&gt;
PORTS----1X2 STACKED
LED    --No</description>
</package>
<package name="7499210001A">
<description>&lt;b&gt;MAX HEIGHT=13.74mm
&lt;pre&gt;
PORTS----1X1
LED    --NO</description>
</package>
<package name="7499210121A">
<description>&lt;b&gt;MAX HEIGHT=13.95mm
&lt;pre&gt;
PORTS----1X1
LED    --YES</description>
</package>
<package name="7499210123A">
<description>&lt;b&gt;MAX HEIGHT=16.90mm 
&lt;pre&gt;
PORTS----1X1
LED   ---YES</description>
</package>
<package name="7499210124A">
<description>&lt;b&gt;MAX HEIGHT=13.50mm
&lt;pre&gt;
PORTS----1X1
LED    --YES</description>
</package>
<package name="7499211002A">
<description>&lt;b&gt;MAX HEIGHT=13.74mm
&lt;pre&gt;
PORTS----1X1
LED    ----NO</description>
</package>
<package name="7499211121A">
<description>&lt;b&gt;MAX HEIGHT=13.95mm
&lt;pre&gt;
PORTS----1X1
LED    --YES</description>
</package>
<package name="7499211122A">
<description>&lt;b&gt;MAX HEIGHT=13.74mm
&lt;pre&gt;
PORTS----1X1
LED    --YES</description>
</package>
<package name="749801100X">
<description>&lt;b&gt;MAX HEIGHT=13.60mm
&lt;pre&gt;
PORTS----1X1
LED    --No</description>
</package>
<package name="74980111211">
<description>&lt;b&gt;MAX HEIGHT=13.61mm
&lt;pre&gt;
PORTS----1X1
LED    --Yes</description>
</package>
<package name="7498011122R">
<description>&lt;b&gt;MAX HEIGHT=11.30mm
&lt;pre&gt;
PORTS----1X1
LED    --Yes</description>
</package>
<package name="7498011211">
<description>&lt;b&gt;MAX HEIGHT=13.50mm
&lt;pre&gt;
PORTS----1X1
LED    --Yes</description>
</package>
<package name="7499611421">
<description>&lt;b&gt;MAX HEIGHT=13.87mm
&lt;pre&gt;
PORTS----1X1
LED    -YES</description>
</package>
<package name="74990111215A">
<description>&lt;b&gt;MAX HEIGHT=13.74mm
&lt;pre&gt;
PORTS----1X1
LED    --YES</description>
</package>
<package name="7499411122A">
<description>&lt;b&gt;MAX HEIGHT=13.87mm
&lt;pre&gt;
PORTS----1X1
LED    --YES</description>
</package>
<package name="7499211123A">
<description>&lt;b&gt;MAX HEIGHT=13.95mm
&lt;pre&gt;
PORTS----1X1
LED    --YES</description>
</package>
<package name="7499511611A">
<description>&lt;b&gt;MAX HEIGHT=13.87mm
&lt;pre&gt;
PORTS----1X1
LED    --YES</description>
</package>
<package name="7499111614A">
<description>&lt;b&gt;MAX HEIGHT=13.87mm
&lt;pre&gt;
PORTS----1X1
LED    --YES</description>
</package>
<package name="WE-SCC_1260/1210">
<description>SMD Common Mode Line Filter WE-SCC</description>
</package>
<package name="WE-SCC_7345">
<description>SMD Common Mode Line Filter WE-SCC</description>
</package>
<package name="WE-SD_744710203">
<description>Leaded Wire Wound Rodcore Inductor WE-SD</description>
</package>
<package name="WE-SD_744710205">
<description>Leaded Wire Wound Rodcore Inductor WE-SD</description>
</package>
<package name="WE-SD_744710210">
<description>Leaded Wire Wound Rodcore Inductor WE-SD</description>
</package>
<package name="WE-SD_744710215">
<description>Leaded Wire Wound Rodcore Inductor WE-SD</description>
</package>
<package name="WE-SD_744710603">
<description>Leaded Wire Wound Rodcore Inductor WE-SD</description>
</package>
<package name="WE-SD_744710605">
<description>Leaded Wire Wound Rodcore Inductor WE-SD</description>
</package>
<package name="WE-SD_744710610">
<description>Leaded Wire Wound Rodcore Inductor WE-SD</description>
</package>
<package name="WE-SD_744710615">
<description>Leaded Wire Wound Rodcore Inductor WE-SD</description>
</package>
<package name="WE-SD_744711003">
<description>Leaded Wire Wound Rodcore Inductor WE-SD</description>
</package>
<package name="WE-SD_744711005">
<description>Leaded Wire Wound Rodcore Inductor WE-SD</description>
</package>
<package name="WE-SD_744711010">
<description>Leaded Wire Wound Rodcore Inductor WE-SD</description>
</package>
<package name="WE-SD_744711015">
<description>Leaded Wire Wound Rodcore Inductor WE-SD</description>
</package>
<package name="WE-SECF-0557">
<description>Type 0557</description>
</package>
<package name="WE-SECF-1562">
<description>Type 1562</description>
</package>
<package name="WE-SECF_0148">
<description>331 011 452 048</description>
</package>
<package name="WE-SECF_0315">
<description>331 031 271 520</description>
</package>
<package name="WE-SECF_0320">
<description>Type 0320</description>
</package>
<package name="WE-SECF_0453">
<description>Type 0453</description>
</package>
<package name="WE-SECF_0610">
<description>Type 0610</description>
</package>
<package name="WE-SECF_0825">
<description>Type 0825</description>
</package>
<package name="WE-SECF_1440">
<description>Type 1440</description>
</package>
<package name="WE-SECF_1613">
<description>Type 1613</description>
</package>
<package name="WE-SECF_1670">
<description>Type 1670</description>
</package>
<package name="WE-SECF_1730">
<description>Type 1730</description>
</package>
<package name="WE-SECF_1735">
<description>Type 1735</description>
</package>
<package name="WE-SECF_2140">
<description>Type 2140</description>
</package>
<package name="WE-SECF_2240">
<description>Type 2240</description>
</package>
<package name="WE-SHC_36103205">
<description>Shielding cabinet SMD- Frame WE-SHC&lt;br&gt;
20.0 x 20.0 x 3.0 mm</description>
</package>
<package name="WE-SHC_36103255">
<description>Shielding cabinet SMD- Frame WE-SHC&lt;br&gt;
25.0 x 25.0 x 3.0 mm</description>
</package>
<package name="WE-SHC_36103305">
<description>Shielding cabinet SMD- Frame WE-SHC&lt;br&gt;
30.0 x 30.0 x 3.0 mm</description>
</package>
<package name="WE-SHC_36103505">
<description>Shielding cabinet SMD- Frame WE-SHC&lt;br&gt;
50.0 x 50.0 x 5.0 mm</description>
</package>
<package name="WE-SHC_36103605">
<description>Shielding cabinet SMD- Frame WE-SHC&lt;br&gt;
60.0 x 60.0 x 5.0 mm</description>
</package>
<package name="WE-SHC_36503205">
<description>Shielding cabinet THT- Frame WE-SHC&lt;br&gt;
20.0 x 20.0 x 3.0 mm</description>
</package>
<package name="WE-SHC_36503255">
<description>Shielding cabinet THT- Frame WE-SHC&lt;br&gt;
25.0 x 25.0 x 3.0 mm</description>
</package>
<package name="WE-SHC_36503305">
<description>Shielding cabinet THT- Frame WE-SHC&lt;br&gt;
30.0 x 30.0 x 3.0 mm</description>
</package>
<package name="WE-SHC_36503505">
<description>Shielding cabinet THT- Frame WE-SHC&lt;br&gt;
50.0 x 50.0 x 3.0 mm</description>
</package>
<package name="WE-SHC_36503605">
<description>Shielding cabinet THT- Frame WE-SHC&lt;br&gt;
60.0 x 60.0 x 3.0 mm</description>
</package>
<package name="WE-SI_744101">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744102">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744103">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744104">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744105">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744106">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744107">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744111">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744112">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744113">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744114">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744115">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744116">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744117">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744118">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744119">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744131">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744132">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744133">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744134">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744135">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744136">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744137">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744138">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744139">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744150">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744151">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744152">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744153">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744154">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744155">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_744156">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_7441110">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SI_7441501">
<description>&lt;B&gt;WE-SI&lt;B&gt;&lt;BR&gt;
Leaded Toroidal Storage Choke</description>
</package>
<package name="WE-SL1">
<description>SMD Common-Mode Line Filter WE-SL1</description>
</package>
<package name="WE-SL2">
<description>SMD Common-Mode Line Filter WE-SL2</description>
</package>
<package name="WE-SL3_744252XXX">
<description>SMD Common-Mode Line Filter WE-SL3</description>
</package>
<package name="WE-SL3_744253XXX">
<description>SMD Common-Mode Line Filter WE-SL3</description>
</package>
<package name="WE-SL3_HV">
<description>SMD Common Mode Line Filter WE-SL3 HV</description>
</package>
<package name="WE-SL5">
<description>SMD Common-Mode Line Filter WE-SL5</description>
</package>
<package name="WE-SL5_HC">
<description>SMD Common-Mode WE-SL5 HC</description>
</package>
<package name="WE_LEP28/11.2_6PIN">
<description>Slim-Transformer WE-SLIM</description>
</package>
<package name="WE-SLM">
<description>SMD Common-Mode Line Filter WE-SLM</description>
</package>
<package name="WE-SL_2WINDING">
<description>SMD Common-Mode Line Filter WE-SL</description>
</package>
<package name="WE-SL_4WINDING">
<description>SMD Common-Mode Line Filter WE-SL</description>
</package>
<package name="WE-SPC_48XX">
<description>&lt;b&gt; SMD-Shielded Power Inductor  WE-SPC</description>
</package>
<package name="WE_EPX7_SMD_8PIN">
<description>Transformer, EPX7 SMD 8 Pin</description>
</package>
<package name="WE_EE13/5/6_HORIZONTAL_8PIN">
<description>Transformer, EE13/5/6 Horizontal 8 Pin</description>
</package>
<package name="WE_EE13/7/4_HORIZONTAL_8PIN">
<description>Transformer, EE13/7/5 THT Horizontal 8 Pin</description>
</package>
<package name="WE_EE16/8/5_THT_HORIZONTAL_8PIN">
<description>Transformer, EE16/8/5 THT Horizontal 8 Pin</description>
</package>
<package name="WE_EE25/13/11_THT_VERTICAL_8PIN">
<description>Transformer, EE25/13/11 THT Vertikal 8 Pin</description>
</package>
<package name="WE_E13/7/4_THT_HORIZONTAL_9PIN">
<description>Transformer, E13/7/4 THT Horizontal 9 Pin</description>
</package>
<package name="WE_EE16/8/5_THT_HORIZONTAL_9PIN">
<description>Transformer, EE16/8/5 THT Horizontal 9 Pin</description>
</package>
<package name="WE_EFD15_SMD_10PIN">
<description>Transformer, EFD15 SMD 10 Pin</description>
</package>
<package name="WE_EE16/7/4_THT_HORIZONTAL_10PIN">
<description>Transformer, EE16/7/4 THT Horizontal 10 Pin</description>
</package>
<package name="WE_E16/7/4_THT_VERTIKAL_10PIN">
<description>Transformer, E16/7/4 THT Vertikal 10 Pin</description>
</package>
<package name="WE_EE25/13/7_THT_HORIZONTAL_10PIN">
<description>Transformer, EE25/13/7 THT Horizontal 10 Pin</description>
</package>
<package name="WE_EE25/13/7_THT_VERTICAL_10PIN">
<description>Transformer, EE25/13/7 THT Vertikal 10 Pin</description>
</package>
<package name="WE_ER11.5_SMD_12PIN">
<description>Transformer, ER11.5 SMD 12 Pin</description>
</package>
<package name="WE_ER14.5_SMD_12PIN">
<description>Transformer, ER14.5 SMD 12 Pin</description>
</package>
<package name="WE_EFD25_SMD_12PIN">
<description>Transformer, EFD25 SMD 12 Pin</description>
</package>
<package name="WE_ER28_THT_HORIZONTAL_12PIN">
<description>Transformer, ER28 THT Horizontal 12 Pin</description>
</package>
<package name="WE_EE25/13/7_THT_HORIZONTAL_13PIN">
<description>Transformer, EE25/13/7 THT Horizontal 13 Pin</description>
</package>
<package name="WE_EE20/10/6_THT_HORIZONTAL_14PIN">
<description>Transformer, EE20/10/6 THT Horizontal 14 Pin</description>
</package>
<package name="WE-SUKW_7427511">
<description>EMI Suppression 5-Hole Ferrite Bead WE-SUKW</description>
</package>
<package name="WE-SUKW_7427512">
<description>EMI Suppression 5-Hole Ferrite Bead WE-SUKW</description>
</package>
<package name="WE-TCI_0402">
<description>Thinfilm Chip Inductor</description>
</package>
<package name="WE-TDC_80XX">
<description>SMD Coupled Inductor WE-TDC</description>
</package>
<package name="WE-TFC">
<description>Common Mode Power Line Choke WE-TFC</description>
</package>
<package name="WE-TFCH">
<description>Common Mode Power Line Choke WE-TFCH</description>
</package>
<package name="WE-TI_TIHV_8095">
<description>Radial Leaded Wire Wound Inductor WE-TI</description>
</package>
<package name="WE-TI_1014">
<description>Radial Leaded Wire Wound Inductor WE-TI</description>
</package>
<package name="WE-TI_6065">
<description>Radial Leaded Wire Wound Inductor WE-TI</description>
</package>
<package name="WE-TI_8012B">
<description>Radial Leaded Wire Wound Inductor WE-TI</description>
</package>
<package name="WE-TI_8012">
<description>Radial Leaded Wire Wound Inductor WE-TI</description>
</package>
<package name="WE-TI_5075">
<description>Radial Leaded Wire Wound Inductor WE-TI</description>
</package>
<package name="WE-TI_8075">
<description>Radial Leaded Wire Wound Inductor WE-TI</description>
</package>
<package name="WE-TI_8075_SHRINKTUBE">
<description>Radial Leaded Wire Wound Inductor WE-TI</description>
</package>
<package name="WE-TI/TIHV_SHRINK_8055">
<description>Radial Leaded Wire Wound Inductor WE-TI</description>
</package>
<package name="WE-TIF">
</package>
<package name="WE-TIS_1111">
<description>Shielded Radial Leaded Inductor WE-TIS</description>
</package>
<package name="WE-TIS_8075">
<description>Radial Leaded Wire Wound Inductor WE-TIS</description>
</package>
<package name="WE-TMSB_0201">
<description>Tiny Multilayer Suppression Bead WE-TMSB</description>
</package>
<package name="WE-TPC_4818/4828">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_3816">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_6823">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_1028/1038">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_3510">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_8020/8043">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_5818/5828">
</package>
<package name="WE-TPC_8015/8012">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TPC_2828_OLD">
<description>Shielded Tiny Power Inductor WE-TPC</description>
</package>
<package name="WE-TVS_SOT23-6L">
<description>TVS Diode Array WE-TVS</description>
</package>
<package name="WE-TVS_SOT23-5L">
<description>TVS Diode Array WE-TVS</description>
</package>
<package name="WE-TVS_SOT23-3L">
<description>TVS Diode Array WE-TVS</description>
</package>
<package name="WE-TVS_SOT143-4L">
<description>TVS Diode Array WE-TVS</description>
</package>
<package name="WE-TVS_SOT563">
<description>TVS Diode Array WE-TVS</description>
</package>
<package name="WE-TVS_SC70-6L">
<description>TVS Diode Array WE-TVS</description>
</package>
<package name="WE-TVS_MSOP-10L">
<description>TVS Diode Array WE-TVS</description>
</package>
<package name="WE-TVS_MSOP-8L">
<description>TVS Diode Array WE-TVS</description>
</package>
<package name="WE-TVS_SC70-5L">
<description>TVS Diode Array WE-TVS</description>
</package>
<package name="WE-UCF">
<description>&lt;b&gt;SMD Common Mode Line Filter&lt;/b&gt;&lt;br&gt;
Height 9.3+/-0.2 mm</description>
</package>
<package name="WE-UKW_7427501">
<description>&lt;B&gt;WE-UKW&lt;br&gt;
EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_7427502">
<description>&lt;B&gt;WE-UKW&lt;br&gt;
EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_7427503">
<description>&lt;B&gt;WE-UKW&lt;br&gt;
EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_7427504">
<description>&lt;B&gt;WE-UKW&lt;br&gt;
EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275010">
<description>&lt;B&gt;WE-UKW&lt;br&gt;
EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275011">
<description>&lt;B&gt;WE-UKW&lt;br&gt;
EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275013">
<description>&lt;B&gt;WE-UKW&lt;br&gt;
EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275022">
<description>&lt;B&gt;WE-UKW&lt;br&gt;
EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275023">
<description>&lt;B&gt;WE-UKW&lt;br&gt;
EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275043">
<description>&lt;B&gt;WE-UKW&lt;br&gt;
EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275046">
<description>&lt;B&gt;WE-UKW&lt;br&gt;
EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_742750421">
<description>WE-UKW EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE_E13/7/4_THT_VERTIKAL_6PIN">
<description>Transformer, E13/7/4 THT vertikal 6Pin</description>
</package>
<package name="WE_E16/8/5_THT_HORIZONTAL_9PIN">
<description>Transformer, E16/8/5 THT Horizontal 9 Pin</description>
</package>
<package name="WE_EE13/7/4_THT_HORIZONTAL_9PIN">
<description>Transformer, EE13/7/4 THT Horizontal 9 Pins</description>
</package>
<package name="WE_EE13/6/6_THT_HORIZONTAL_8PIN">
<description>Transformer, EE13/6/6 THT Horizontal 8 Pins</description>
</package>
<package name="WE_EER28/4/11_HORIZONTAL_12PIN">
<description>Transformer, EER 28/4/11 THT Horizontal 12Pin</description>
</package>
<package name="WE_EE16/8/5_THT_HORIZONTAL_6PIN">
<description>Transformer, EE16/8/5 THT Horizontal 6 Pin</description>
</package>
<package name="WE_EE20/10/6_THT_HORIZONTAL_14PIN_1">
<description>Transformer, EE20/10/6 THT Horizontal 14Pin</description>
</package>
<package name="WE_EE20/10/6_THT_HORIZONTAL_8PIN">
<description>Transformer, EE20/10/6 THT Horizontal 8 Pin</description>
</package>
<package name="WE-UOST">
<description>&lt;b&gt;Universal Offline Standard Transformers WE-UOST</description>
</package>
<package name="WE-VD_5MM-DIA">
<description>VARISTOR</description>
</package>
<package name="WE-VD_5MM-1.0">
<description>VARISTOR</description>
</package>
<package name="WE-VD_5MM-1.1">
<description>VARISTOR</description>
</package>
<package name="WE-VD_5MM-1.3">
<description>VARISTOR</description>
</package>
<package name="WE-VD_5MM-1.5">
<description>VARISTOR</description>
</package>
<package name="WE-VD_5MM-1.7">
<description>VARISTOR</description>
</package>
<package name="WE-VD_5MM-1.8">
<description>VARISTOR</description>
</package>
<package name="WE-VD_5MM-2.1">
<description>VARISTOR</description>
</package>
<package name="WE-VD_5MM-2.4">
<description>VARISTOR</description>
</package>
<package name="WE-VD_5MM-2.7">
<description>VARISTOR</description>
</package>
<package name="WE-VD_5MM-3.0">
<description>VARISTOR</description>
</package>
<package name="WE-VD_7MM-DIA">
<description>VARISTOR</description>
</package>
<package name="WE-VD_7MM-1.0">
<description>VARISTOR</description>
</package>
<package name="WE-VD_7MM-1.1">
<description>VARISTOR</description>
</package>
<package name="WE-VD_7MM-1.3">
<description>VARISTOR</description>
</package>
<package name="WE-VD_7MM-1.5">
<description>VARISTOR</description>
</package>
<package name="WE-VD_7MM-1.7">
<description>VARISTOR</description>
</package>
<package name="WE-VD_7MM-1.8">
<description>VARISTOR</description>
</package>
<package name="WE-VD_7MM-2.1">
<description>VARISTOR</description>
</package>
<package name="WE-VD_7MM-2.4">
<description>VARISTOR</description>
</package>
<package name="WE-VD_7MM-2.7">
<description>VARISTOR</description>
</package>
<package name="WE-VD_7MM-3.0">
<description>VARISTOR</description>
</package>
<package name="WE-VD_7MM-3.1">
<description>VARISTOR</description>
</package>
<package name="WE-VD_7MM-3.3">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-DIA">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-0.9">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-1.1">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-1.3">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-1.5">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-1.6">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-1.9">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-2.2">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-2.5">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-2.8">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-2.9">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-3.1">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-3.7">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-4.0">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-4.5">
<description>VARISTOR</description>
</package>
<package name="WE-VD_10MM-9.8">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-DIA">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-0.9">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-1.1">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-1.3">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-1.5">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-1.6">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-1.9">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-10.2">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-2.2">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-2.5">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-2.8">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-2.9">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-3.1">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-3.6">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-4.0">
<description>VARISTOR</description>
</package>
<package name="WE-VD_14MM-4.5">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-DIA">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-0.9">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-1.1">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-1.2">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-1.3">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-1.5">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-1.7">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-10.4">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-2.0">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-2.3">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-2.6">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-2.8">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-2.9">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-3.4">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-3.8">
<description>VARISTOR</description>
</package>
<package name="WE-VD_20MM-4.3">
<description>VARISTOR</description>
</package>
<package name="WESURGE_0201">
<description>WESURGE SMD</description>
</package>
<package name="WESURGE_0402_WAVE">
<description>WESURGE SMD</description>
</package>
<package name="WESURGE_0603_WAVE">
<description>WESURGE SMD</description>
</package>
<package name="WESURGE_0805_WAVE">
<description>WESURGE SMD</description>
</package>
<package name="WE-VEA_0508">
<description>WESURGE ESD Suppressor-Array WE-VEA</description>
</package>
<package name="WE-VEA_0612">
<description>WESURGE ESD Suppressor-Array WE-VEA</description>
</package>
<package name="WESURGE_1206_WAVE">
<description>WESURGE SMD</description>
</package>
<package name="WESURGE_1210_WAVE">
<description>WESURGE SMD</description>
</package>
<package name="WESURGE_1812_WAVE">
<description>WESURGE SMD</description>
</package>
<package name="WESURGE_2220_WAVE">
<description>WESURGE SMD</description>
</package>
<package name="WE-WPCC_3737">
<description>&lt;b&gt;Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Size 3737&lt;br&gt;
The distance between two pins is 5.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_3830">
<description>&lt;b&gt;Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Size 3830&lt;br&gt;
The distance between two pins is 5.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_4832">
<description>&lt;b&gt;Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Size 4832&lt;br&gt;
The distance between two pins is 5.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_5353_DRILL:2MM">
<description>&lt;b&gt;Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Size 5353&lt;br&gt;
The distance between two pins is 5.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_5353_DRILL:4MM">
<description>&lt;b&gt;Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Size 5353&lt;br&gt;
The distance between two pins is 5.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_13055">
<description>&lt;b&gt;Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Size 4832&lt;br&gt;
The distance between two pins of each winding  is 5.0mm min and the ref distance between the pins of two windings is 43.0 mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_Φ50_760308100110">
<description>&lt;b&gt;Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Size Φ50&lt;br&gt;
The distance between two pins is 5.0mm min &lt;br&gt;</description>
</package>
<package name="WE-FB_EP10">
</package>
<package name="WE-FB_EP13_DIMENSION2">
</package>
<package name="WE-FB_EP13_DIMENSION1">
</package>
<package name="WE-FB_ER9.5">
</package>
<package name="WE-FB_EE16/8/5">
</package>
<package name="WE-FB_EE20/10/6">
</package>
<package name="WE-FB_EFD20">
</package>
<package name="WE-FB_EFD25_DIMENSION1">
</package>
<package name="WE-FLEX_ER11/5">
</package>
<package name="WE-FLEX_ER14.5/6">
</package>
<package name="WE-FLEX_EFD15">
</package>
<package name="WE-FLEX_EFD20">
</package>
<package name="WE-MI_0603">
</package>
<package name="WE-MI_0805">
</package>
<package name="WE-MI_1206">
</package>
<package name="WE-MK_0201">
</package>
<package name="WE-MK_0402">
</package>
<package name="WE-MK_0603">
</package>
<package name="749014011">
</package>
<package name="749014012">
</package>
<package name="749014013">
</package>
<package name="WE-FB_EFD20_10PIN">
</package>
<package name="74990111211">
</package>
<package name="WE-CBF_0402(W=1.5)">
</package>
<package name="WE-CBF_0402(W=2.2)">
</package>
<package name="WE-CBF_0603(W=2.2)">
</package>
<package name="WE-CBF_0603(W=2.6)">
</package>
<package name="WE-CBF_0805(W=3.0)">
</package>
<package name="WE-CBF_0805(W=4.0)">
</package>
<package name="WE-CBF_1206(W=4.2)">
</package>
<package name="WE-CBF_1206(W=5.2)">
</package>
<package name="WE-CBF_1806(W=5.5)">
</package>
<package name="WE-CBF_1806(W=6.5)">
</package>
<package name="WE-CBF_1812(W=6.3)">
</package>
<package name="WE-CBF_1812(W=7.3)">
</package>
<package name="WE-CBF_HF_0402(W=2.2)">
</package>
<package name="WE-CBF_HF_0603(W=2.6)">
</package>
<package name="WE-DD_1210/1260/1280_CROSSED">
</package>
<package name="WE-VE_FEMTOF_0603">
</package>
<package name="WE-VE_FEMTOF_0402">
</package>
<package name="WE-VE_ULC_0402">
</package>
<package name="WE-VE_ULC_0603">
</package>
<package name="WE-CAIR_1322">
</package>
<package name="WE-CAIR_1340">
</package>
<package name="WE-CAIR_3136">
</package>
<package name="WE-CAIR_3168">
</package>
<package name="WE-DD_7345">
</package>
<package name="WE-LQS_6045">
</package>
<package name="WE-PD2_HV_1060">
</package>
<package name="WE-TI_1020">
</package>
<package name="WE-SECF_0135">
</package>
<package name="WE-GFH_2520">
</package>
<package name="WE-GFH_3225">
</package>
<package name="WE-GFH_4532">
</package>
<package name="WESURGE_0402_REFLOW">
</package>
<package name="WESURGE_0603_REFLOW">
</package>
<package name="WESURGE_0805_REFLOW">
</package>
<package name="WESURGE_1206_REFLOW">
</package>
<package name="WE-HCM_1078">
</package>
<package name="WE-HCI_5040">
</package>
<package name="WE-MPSB_0603(W=2.6)">
</package>
<package name="WE-MPSB_0805(W=4.0)">
</package>
<package name="WE-MPSB_1206(W=5.2)">
</package>
<package name="WE-FCL_ET35">
</package>
<package name="WE-WAFB_7427602">
</package>
<package name="WE-WAFB_7427603">
</package>
<package name="WE-WAFB_7427604">
</package>
<package name="WE-WAFB_7427605">
</package>
<package name="WE-WAFB_7427606">
</package>
<package name="WE-WAFB_74276031">
</package>
<package name="WE-WAFB_74276032">
</package>
<package name="WE-WAFB_74276041">
</package>
<package name="WE-WAFB_74276051">
</package>
<package name="WE-TCI_0201">
</package>
<package name="WE-LHMI_8030">
</package>
<package name="WE-LHMI_8040">
</package>
<package name="WE-LHMI_4012">
<description>&lt;b&gt; SMD lOW Profile High Current Molded Inductor&lt;/b&gt;&lt;br&gt;
Size 4012&lt;br&gt;</description>
</package>
<package name="WE-LHMI_5020">
<description>&lt;b&gt;SMD Low Profile High Current Molded Inductor&lt;/b&gt;&lt;br&gt;

Size 5020</description>
</package>
<package name="WE-LHMI_5030">
<description>&lt;b&gt;SMD Low Profile High Current Molded Inductor&lt;/b&gt;&lt;br&gt;

size 5030</description>
</package>
<package name="750032052">
</package>
<package name="WE-FAMI_1215_744750460150">
</package>
<package name="WE-XHMI_74439358XXX">
<description>&lt;B&gt;WE-XHMI Xtreme High Current Molded Inductor</description>
</package>
<package name="WE-FI_7447010">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447011">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447012">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447013">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447014">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447015">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447016">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447017">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447018">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447019">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447020">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447021">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447022">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447023">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447024">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447025">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447026">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447027">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447028">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_74470291">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_74470292">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447030">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447031">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447032">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447033">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447034">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447035">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447036">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447037">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447040">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447041">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447042">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447043">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447044">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447045">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447050">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447051">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447052">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447053">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447054">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447055">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447060">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447065">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447070">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447071">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447075">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447076">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447077">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447078">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-FI_7447079">
<description>WE-FI Leaded Toroidal Line Choke</description>
</package>
<package name="WE-LAN10G:0.99MM">
<description>WE-LAN 10G:0.99mm</description>
</package>
<package name="WE-LAN10G1.27MM">
<description>WE-LAN 10G:1.27mm</description>
</package>
<package name="VARTVSP_SMA/DO-214AC">
</package>
<package name="VARTVSP_SMB/DO-214AA">
</package>
<package name="VARTVSP_SMC&amp;SMD/DO-214AB">
</package>
<package name="VARTVSP_SMA/DO-214AC_UNI">
</package>
<package name="VARTVSP_SMB/DO-214AA_UNI">
</package>
<package name="VARTVSP_SMC&amp;SMD/DO-214AB_UNI">
</package>
<package name="WE-PMI_1210">
</package>
<package name="WE-SHC_S11100108">
</package>
<package name="8492121">
</package>
<package name="WE-EXB_744844XXX">
</package>
<package name="WE-EXB_744844102">
</package>
<package name="WE-WPCC_2929">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
type 2929&lt;br&gt;
The distance between two pins is 2.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_Φ19">
<description>WE-WPCC Wireless Power
Charging Receiver Coil,Φ19mm</description>
</package>
<package name="WE-WPCC_Φ20">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
ø 21mm &lt;br&gt;
The distance between two pins is 5.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_2815">
</package>
<package name="WE-WPCC_3426">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
type 3426&lt;br&gt;
The distance between two pins is 2.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_4040">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
type 4040&lt;br&gt;
The distance between two pins is 2.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_4636">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
type 4636&lt;br&gt;
The distance between two pins is 2.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_Φ10">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Φ10mm&lt;br&gt;
The distance between two pins is 2.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_Φ6">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Φ6mm&lt;br&gt;
The distance between two pins is 2.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_Φ15">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Φ15mm&lt;br&gt;
The distance between two pins is 2.0mm min &lt;br&gt;,</description>
</package>
<package name="WE-WPCC_Φ17">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Φ17mm&lt;br&gt;
The distance between two pins is 2.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_Φ26">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Φ26mm&lt;br&gt;
The distance between two pins is 2.0mm min &lt;br&gt;,</description>
</package>
<package name="WE-WPCC_6052">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
Type 6052 &lt;br&gt;
The distance between two pins is 5.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_Φ30">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
ø 30mm &lt;br&gt;
The distance between two pins is 5.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_Φ48">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
ø 47mm &lt;br&gt;
The distance between two pins is 5.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_A19">
<description>&lt;b&gt;WE-WPCC Wireless Power Array&lt;/b&gt;&lt;br&gt;
A19 &lt;br&gt;
The distance between two pins is 5.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_A6">
<description>&lt;b&gt;WE-WPCC Wireless Power Array&lt;/b&gt;&lt;br&gt;
A6 &lt;br&gt;
The distance between two pins is 5.0mm min &lt;br&gt;</description>
</package>
<package name="WE-WPCC_A28">
<description>&lt;b&gt;WE-WPCC Wireless Power Array&lt;/b&gt;&lt;br&gt;
A28 &lt;br&gt;
The distance between two pins is 5.0mm min &lt;br&gt;</description>
</package>
<package name="WE-MAPI_2010">
</package>
<package name="WE-TIF_1016">
</package>
<package name="WE-PMCI_0603_74479262XXX">
</package>
<package name="WE-PMCI_0805_74479275XXX">
</package>
<package name="WE-PMCI_0806_74479276XXX">
</package>
<package name="WE-PMCI_0806_74479276XXXC">
</package>
<package name="WE-PMCI_1008_74479287XXX">
</package>
<package name="WE-PMCI_1008_74479288XXX">
</package>
<package name="WE-PMCI_1210_74479298XXX">
</package>
<package name="WE-PMCI_1210_74479299XXX">
</package>
<package name="WE-UKW_74275143">
<description>&lt;B&gt;WE-UKW&lt;br&gt;
EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275223">
<description>&lt;B&gt;WE-UKW&lt;br&gt;
EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-UKW_74275243">
<description>&lt;B&gt;WE-UKW&lt;br&gt;
EMI Suppression 6-Hole Ferrite Bead</description>
</package>
<package name="WE-LQS_2512">
<description>&lt;b&gt;IndLQS WE-LQS SMD Power Inductor</description>
</package>
<package name="WE-LQS_3012">
<description>&lt;B&gt;WE-LQS SMD Power Inductor</description>
</package>
<package name="WE-LQS_4012">
<description>&lt;b&gt;IndLQS WE-LQS SMD Power Inductor</description>
</package>
<package name="WE-LQS_5020">
<description>&lt;b&gt;IndLQS WE-LQS SMD Power Inductor</description>
</package>
<package name="WE-PMMI_0805">
</package>
<package name="WE-PMMI_0806">
</package>
<package name="WE-CMB_XL_744825XXX">
</package>
<package name="WE-DS_210111003">
</package>
<package name="WE-DS_2101120X3">
</package>
<package name="WE-DS_2106110X3">
</package>
<package name="WE-DS_2106120X3">
</package>
<package name="WE-DS_2121110X3">
</package>
<package name="WE-DS_2121120X3">
</package>
<package name="WE-DS_2126110X3">
</package>
<package name="WE-DS_2126120X3">
</package>
<package name="WE-DS_2141110X3">
</package>
<package name="WE-DS_2141120X3">
</package>
<package name="WE-DS_2146110X3">
</package>
<package name="WE-DS_2146120X3">
</package>
<package name="WE-DS_2161110X3">
</package>
<package name="WE-DS_2161120X3">
</package>
<package name="WE-DS_2166110X3">
</package>
<package name="WE-DS_2166120X3">
</package>
<package name="WE-DS_240117113">
</package>
<package name="WE-DS_240617113">
</package>
<package name="WE-DS_242117113">
</package>
<package name="WE-DS_242617113">
</package>
<package name="WE-DS_244117113">
</package>
<package name="WE-DS_244617113">
</package>
<package name="WE-DS_246117113">
</package>
<package name="WE-DS_246617113">
</package>
<package name="WE-LQS_4025">
</package>
<package name="WE-CBF_1210(W=4.2)">
</package>
<package name="WE-CBF_1210(W=5.2)">
</package>
<package name="WE_EPQ13_SMD_10PIN">
</package>
<package name="WE-MAPI_20XX">
</package>
<package name="WE-MAPI_25XX">
</package>
<package name="WE-VD_7MM-1.4">
</package>
<package name="WE-VD_20MM-4.7">
</package>
<package name="WE-VD_20MM-5.0">
</package>
<package name="7490100111A">
</package>
<package name="7490100161A">
</package>
<package name="7490120110">
</package>
<package name="7490140112">
</package>
<package name="749014018">
</package>
<package name="74902001XA">
</package>
<package name="7490200136">
</package>
<package name="749020111A">
</package>
<package name="749050010U">
</package>
<package name="7499211125">
</package>
<package name="WE-DS_210111023">
</package>
<package name="WE-MAPI_30XX">
</package>
<package name="WE-MAPI_3010">
</package>
<package name="WE-4WAY_742730321">
</package>
<package name="7490100110A/749010012A">
</package>
<package name="749013011A">
</package>
<package name="WE-CMB_M_744823422">
</package>
<package name="WE-CMB_M_744823333">
</package>
<package name="WE-CMB_M_744823305">
</package>
<package name="WE-CMB_M_744823210/20">
</package>
<package name="WE-TI/TIHV_8095_SHRINKING">
</package>
<package name="74990111217">
</package>
<package name="7498111001A">
</package>
<package name="7499011222A">
</package>
<package name="7499111001A">
</package>
<package name="WE-CMBNC_XS_744801XXXX-A">
</package>
<package name="WE-DAA_750082157">
</package>
<package name="WE-EP5_6PIN_2">
</package>
<package name="WE-XHMI_7443934XXXX">
</package>
<package name="WE-XHMI_74439369XXX">
</package>
<package name="WE-XHMI_74439370XXX">
</package>
<package name="WE-CFWI_1312">
<description>&lt;b&gt;Coupled Flatwire Inductor WE-CFWI</description>
</package>
<package name="WE-CFWI_1813">
<description>&lt;b&gt;IndCFWI Coupled Flatwire Inductor</description>
</package>
<package name="WE-POE_EFD15">
</package>
<package name="WE-POE_EP13">
</package>
<package name="WE-POE+_EP13">
</package>
<package name="WE-TPC_2811/2813_OLD">
</package>
<package name="WE-UNIT_750370026">
</package>
<package name="WE-UNIT_750370024">
</package>
<package name="WE-UNIT_750871111">
</package>
<package name="WE-UNIT_760871131">
</package>
<package name="WE-UNIT_STM_750314288">
</package>
<package name="WE-UNIT_PI_750811016">
</package>
<package name="WE-UNIT_EE16/8/5_1">
</package>
<package name="WE-UNIT_PI_75081101XX">
</package>
<package name="WE-UNIT_PT_7508110102">
</package>
<package name="WE-UNIT_PI_NXP_EE20/10/6">
</package>
<package name="WE-UNIT_EFD25">
</package>
<package name="WE-UNIT_NXP_760871038">
</package>
<package name="744830007215">
<description>&lt;B&gt;WE-CMBHV Common Mode Power Line Choke</description>
</package>
<package name="744830010185">
<description>&lt;b&gt;WE-CMBHV Common Mode Power Line Choke</description>
</package>
<package name="744830017132">
<description>&lt;B&gt;WE-CMBHV Common Mode Power Line Choke</description>
</package>
<package name="744830039080">
<description>&lt;B&gt;WE-CMBHV Common Mode Power Line Choke</description>
</package>
<package name="744831010205">
<description>&lt;B&gt;WE-CMBHV Common Mode Power Line Choke</description>
</package>
<package name="744831016164">
<description>&lt;B&gt;WE-CMBHV Common Mode Power Line Choke</description>
</package>
<package name="744831020133">
<description>&lt;B&gt;WE-CMBHV Common Mode Power Line Choke</description>
</package>
<package name="744831034090">
<description>&lt;B&gt;WE-CMBHV Common Mode Power Line Choke</description>
</package>
<package name="744831047068">
<description>&lt;B&gt;WE-CMBHV Common Mode Power Line Choke</description>
</package>
<package name="744830025103">
</package>
<package name="WE-PD2SA_7850">
</package>
<package name="WE-KIHC_0402">
<description>Wire Wound Chip Ceramic Inductor WE-KIHC</description>
</package>
<package name="WE-KIHC_0603">
<description>Wire Wound Chip Ceramic Inductor WE-KIHC</description>
</package>
<package name="WE-LQS_2010">
</package>
<package name="WE-LQS_8065">
</package>
<package name="WE-TPBHV_Φ1.3">
</package>
<package name="WE-TPBHV_Φ1.6">
</package>
<package name="WE-TPBHV_Φ2.0">
</package>
<package name="WE-TPBHV_Φ2.4">
</package>
<package name="WE-TPBHV_Φ2.6">
</package>
<package name="WE-TPBHV_Φ5.5">
</package>
<package name="WE-TPBHV_Φ4.0">
</package>
<package name="WE-TPBHV_Φ4.2">
</package>
<package name="WE-TPBHV_Φ4.5">
</package>
<package name="WE-LQSH_2010">
</package>
<package name="WE-LQSH_2512">
</package>
<package name="WE-LQSH_3012">
</package>
<package name="WE-LQSH_4020">
</package>
<package name="WE-LQFS_3818">
</package>
<package name="WE-LQFS_48X8">
</package>
<package name="WE-MAPI_40XX">
</package>
<package name="WE-MAIA_4020">
</package>
<package name="WE-MAIA_3020">
</package>
<package name="WE-MAIA_2512">
</package>
<package name="749020022A">
</package>
<package name="7490140110">
</package>
<package name="749020100A">
</package>
<package name="7497011611A">
</package>
<package name="7498210002">
</package>
<package name="7498210003">
</package>
<package name="7498210220A">
</package>
<package name="7499010003A">
</package>
<package name="74990101212">
</package>
<package name="74990101241">
</package>
<package name="7499010126A">
</package>
<package name="7499011441A">
</package>
<package name="7499021002A">
</package>
<package name="7499031001A">
</package>
<package name="7499110120A">
</package>
<package name="7499410213">
</package>
<package name="7499410221">
</package>
<package name="7499511002A">
</package>
<package name="WE-WPCC_4027">
</package>
<package name="749022012X">
</package>
<package name="7490220115">
</package>
<package name="WE-WPCC_4444">
</package>
<package name="WE-WPCC_4544">
</package>
<package name="WE-WPCC_4832_760308103215">
</package>
<package name="WE-WPCC_5353_760308141">
</package>
<package name="WE-WPCC_5353_760308102142">
</package>
<package name="WE-WPCC_5353_760308103102">
</package>
<package name="WE-WPCC_Φ50_760308100111">
</package>
<package name="WE-WPCC_Φ50_760308100143">
</package>
<package name="WE-WPCC_Φ50_760308101302">
</package>
<package name="WE-WPCC_Φ50_760308100141">
</package>
<package name="WE-LPCC_7448680100">
</package>
<package name="WE-LPCC_7448680120">
</package>
<package name="WE-LPCC_7448680140">
</package>
<package name="WE-LPCC_7448680180">
</package>
<package name="WE-LPCC_7448680200">
</package>
<package name="WE-LHMI_1365">
</package>
<package name="WE-WPCC_5030">
</package>
<package name="WE-SHC_36103205S">
</package>
<package name="WE-SHC_36105266S">
</package>
<package name="WE-SHC_36105366S">
</package>
<package name="WE-SHC_36106326S">
</package>
<package name="WE-SHC_36107406S">
</package>
<package name="WE-SHC_36903205S">
</package>
<package name="WE-SHC_36903255S">
</package>
<package name="WE-SHC_36903305S">
</package>
<package name="WE-SHC_36905266S">
</package>
<package name="WE-SHC_36906326S">
</package>
<package name="WE-SHC_36907406S">
</package>
<package name="WE-SHC_369010302X">
</package>
<package name="WE-LAN_AQ_749010310">
</package>
<package name="WE-FLEXHV_EFD15">
</package>
<package name="WE-FLEXHV_EFD20">
</package>
<package name="WE-FLEXHV_ER11/5">
</package>
<package name="WE-FLEXHV_ER14.5/6">
</package>
<package name="WE-ACHC_1010">
</package>
<package name="WE-ACHC_1212">
</package>
<package name="WE-DPC_HV_5030">
</package>
<package name="WE-HCF_2815">
</package>
<package name="WE-PD2_3521">
</package>
<package name="WE-DPC_5838">
</package>
</packages>
<symbols>
<symbol name="749050010A">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10G Base-T ,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION---STANDARD

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="D+@1"/>
<pin name="TD@1"/>
<pin name="D-@1"/>
<pin name="TD@2"/>
<pin name="D-@2"/>
<pin name="D+@2"/>
<pin name="X-@2"/>
<pin name="X+@2"/>
<pin name="TX@2"/>
<pin name="X-@1"/>
<pin name="TX@1"/>
<pin name="X+@1"/>
<pin name="D+@3"/>
<pin name="TD@3"/>
<pin name="D-@3"/>
<pin name="TD@4"/>
<pin name="D-@4"/>
<pin name="D+@4"/>
<pin name="X-@4"/>
<pin name="X+@4"/>
<pin name="TX@4"/>
<pin name="X-@3"/>
<pin name="TX@3"/>
<pin name="X+@3"/>
</symbol>
<symbol name="CM2W-V">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="L-1W">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WE-BAL">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="BPF_T1/T5">
<pin name="GND@2" direction="pas"/>
<pin name="OUT" direction="pas"/>
<pin name="GND@1" direction="pas"/>
<pin name="IN" direction="pas"/>
</symbol>
<symbol name="CM2W-H_2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="CM2W-H_1">
<description>&lt;b&gt;WE-CMBH&lt;br&gt;
Common Mode Power Line Choke</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="T_8PIN">
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="T_9PIN">
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="T_12PIN">
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="TRANSFOMER_14PIN">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="T_10PIN">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="L_3W:3W_3">
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="T_3W_1*2">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="T_3W_1/2">
<description>&lt;b&gt;WE-GDT Gate-Drive-Transformer&lt;/b&gt;&lt;br&gt;

Three winding</description>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="749024012">
<description>&lt;PRE&gt;
Typical electrical Values for WE-HV LAN TRANSFORMER 10/100/1000 Base-T,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION----STANDARD

Operating Temperature --- (-40°C up to 85°C)</description>
<pin name="D+"/>
<pin name="TD"/>
<pin name="D-"/>
<pin name="D1+"/>
<pin name="D1-"/>
<pin name="TD1"/>
<pin name="X1-"/>
<pin name="TX1"/>
<pin name="X1+"/>
<pin name="X-"/>
<pin name="TX"/>
<pin name="X+"/>
<pin name="D2+"/>
<pin name="TD2"/>
<pin name="D2-"/>
<pin name="D3+"/>
<pin name="D3-"/>
<pin name="TD3"/>
<pin name="X3-"/>
<pin name="TX3"/>
<pin name="X3+"/>
<pin name="X2-"/>
<pin name="TX2"/>
<pin name="X2+"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="749014010">
<description>&lt;PRE&gt;
Typical electrical Values for WE-HV LAN TRANSFORMER 10/100 Base-T,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION----STANDARD

Operating Temperature ---0°C up to 70°C</description>
<pin name="RD+"/>
<pin name="CRD"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="CTD"/>
<pin name="TX-"/>
<pin name="CTX"/>
<pin name="TX+"/>
<pin name="RX-"/>
<pin name="CRX"/>
<pin name="RX+"/>
</symbol>
<symbol name="749014011">
<description>&lt;PRE&gt;
Typical electrical Values for WE-HV LAN TRANSFORMER 10/100 Base-T,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION----STANDARD

Operating Temperature ---0°C up to 70°C</description>
<pin name="RD+"/>
<pin name="CRD"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="CTD"/>
<pin name="TX-"/>
<pin name="CTX"/>
<pin name="TX+"/>
<pin name="RX-"/>
<pin name="CRX"/>
<pin name="RX+"/>
</symbol>
<symbol name="749014012">
<description>&lt;PRE&gt;
Typical electrical Values for WE-HV LAN TRANSFORMER 10/100 Base-T,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION----STANDARD

Operating Temperature ---0°C up to 70°C</description>
<pin name="RD+"/>
<pin name="CRD"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="CTD"/>
<pin name="TX-"/>
<pin name="CTX"/>
<pin name="TX+"/>
<pin name="RX-"/>
<pin name="CRX"/>
<pin name="RX+"/>
</symbol>
<symbol name="749014013">
<description>&lt;PRE&gt;
Typical electrical Values for WE-HV LAN TRANSFORMER 10/100 Base-T,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION----PoE

Operating Temperature ---0°C up to 70°C</description>
<pin name="RD+"/>
<pin name="CRD"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="CTD"/>
<pin name="TX-"/>
<pin name="CTX"/>
<pin name="TX+"/>
<pin name="RX-"/>
<pin name="CRX"/>
<pin name="RX+"/>
</symbol>
<symbol name="T_3L_2/1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="749010011">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100 Base-T,SMD,

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION----STANDARD

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="RD+"/>
<pin name="RCT"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="TCT"/>
<pin name="TX-"/>
<pin name="TXCT"/>
<pin name="TX+"/>
<pin name="RX-"/>
<pin name="RXCT"/>
<pin name="RX+"/>
</symbol>
<symbol name="749010012">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100 Base-T,SMD,

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION----STANDARD

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="RD+"/>
<pin name="RCT"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="TCT"/>
<pin name="TX-"/>
<pin name="TXCT"/>
<pin name="TX+"/>
<pin name="RX-"/>
<pin name="RXCT"/>
<pin name="RX+"/>
</symbol>
<symbol name="749010014">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100 Base-T,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION----STANDARD

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.	1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="RD+"/>
<pin name="CRX"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="CTX"/>
<pin name="TX-"/>
<pin name="CTD"/>
<pin name="TX+"/>
<pin name="RX-"/>
<pin name="CRD"/>
<pin name="RX+"/>
</symbol>
<symbol name="749010040">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100 Base-T,SMD

&lt;B&gt;NO OF PORT----4

&lt;B&gt;APPLICATION----STANDARD

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="CTVDD4"/>
<pin name="RD4+"/>
<pin name="RD4-"/>
<pin name="TD4-"/>
<pin name="TD4+"/>
<pin name="TX4+"/>
<pin name="TX4-"/>
<pin name="CMGND4"/>
<pin name="RX4+"/>
<pin name="RX4-"/>
<pin name="CTVDD3"/>
<pin name="TD3-"/>
<pin name="TD3+"/>
<pin name="RD3+"/>
<pin name="RD3-"/>
<pin name="RX3-"/>
<pin name="RX3+"/>
<pin name="CMGND3"/>
<pin name="TX3-"/>
<pin name="TX3+"/>
<pin name="CTVDD2"/>
<pin name="RD2+"/>
<pin name="RD2-"/>
<pin name="TD2-"/>
<pin name="TD2+"/>
<pin name="TX2+"/>
<pin name="TX2-"/>
<pin name="CMGND2"/>
<pin name="RX2+"/>
<pin name="RX2-"/>
<pin name="CTVDD1"/>
<pin name="TD1-"/>
<pin name="TD1+"/>
<pin name="RD1+"/>
<pin name="RD1-"/>
<pin name="RX1-"/>
<pin name="RX1+"/>
<pin name="CMGND1"/>
<pin name="TX1-"/>
<pin name="TX1+"/>
</symbol>
<symbol name="7490100111">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100 Base-T,SMD,

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION----STANDARD

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="RD+"/>
<pin name="CRX"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="CTX"/>
<pin name="TX-"/>
<pin name="CTD"/>
<pin name="TX+"/>
<pin name="RX-"/>
<pin name="CRD"/>
<pin name="RX+"/>
</symbol>
<symbol name="7490101120">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100 Base-T,SMD,

&lt;B&gt;NO OF PORT----1 LP

&lt;B&gt;APPLICATION----STANDARD

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="RD+"/>
<pin name="RD-"/>
<pin name="CRD"/>
<pin name="CTD"/>
<pin name="TD-"/>
<pin name="TD+"/>
<pin name="TX-"/>
<pin name="TX+"/>
<pin name="CTX"/>
<pin name="RX-"/>
<pin name="CRX"/>
<pin name="RX+"/>
</symbol>
<symbol name="74901201X">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100 Base-T,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION----PoE+

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="RD+"/>
<pin name="CRD"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="CTD"/>
<pin name="TX-"/>
<pin name="CTX"/>
<pin name="TX+"/>
<pin name="RX-"/>
<pin name="CRX"/>
<pin name="RX+"/>
</symbol>
<symbol name="749013011">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100 Base-T,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION----PoE

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="RD+"/>
<pin name="RXCT"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="TXCT"/>
<pin name="TX-"/>
<pin name="TCT"/>
<pin name="TX+"/>
<pin name="RX-"/>
<pin name="RCT"/>
<pin name="RX+"/>
</symbol>
<symbol name="749013021">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100 Base-T,SMD,

&lt;B&gt;NO OF PORT----2

&lt;B&gt;APPLICATION----PoE

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="RD1+"/>
<pin name="RCT1"/>
<pin name="RD1-"/>
<pin name="TD1+"/>
<pin name="TD1-"/>
<pin name="TCT1"/>
<pin name="TX1-"/>
<pin name="TXCT1"/>
<pin name="TX1+"/>
<pin name="RX1-"/>
<pin name="RXCT1"/>
<pin name="RX1+"/>
<pin name="TD2+"/>
<pin name="RCT2"/>
<pin name="TD2-"/>
<pin name="RD2+"/>
<pin name="RD2-"/>
<pin name="TCT2"/>
<pin name="TX2+"/>
<pin name="TXCT2"/>
<pin name="RX2+"/>
<pin name="TX2-"/>
<pin name="RXCT2"/>
<pin name="RX2-"/>
</symbol>
<symbol name="749013040">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100 Base-T,SMD,

&lt;B&gt;NO OF PORT----4

&lt;B&gt;APPLICATION----PoE

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="RD1+"/>
<pin name="RCT1"/>
<pin name="RD1-"/>
<pin name="TD1+"/>
<pin name="TD1-"/>
<pin name="TCT1"/>
<pin name="TX1-"/>
<pin name="CMT1"/>
<pin name="TX1+"/>
<pin name="RX1-"/>
<pin name="CMR1"/>
<pin name="RX1+"/>
<pin name="RD2+"/>
<pin name="RCT2"/>
<pin name="RD2-"/>
<pin name="TD2+"/>
<pin name="TD2-"/>
<pin name="TCT2"/>
<pin name="TX2-"/>
<pin name="CMT2"/>
<pin name="TX2+"/>
<pin name="RX2-"/>
<pin name="CMR2"/>
<pin name="RX2+"/>
<pin name="RD3+"/>
<pin name="RCT3"/>
<pin name="RD3-"/>
<pin name="TD3+"/>
<pin name="TD3-"/>
<pin name="TCT3"/>
<pin name="TX3-"/>
<pin name="CMT3"/>
<pin name="TX3+"/>
<pin name="RX3-"/>
<pin name="CMR3"/>
<pin name="RX3+"/>
<pin name="RD4+"/>
<pin name="RCT4"/>
<pin name="RD4-"/>
<pin name="TD4+"/>
<pin name="TD4-"/>
<pin name="TCT4"/>
<pin name="TX4-"/>
<pin name="CMT4"/>
<pin name="TX4+"/>
<pin name="RX4-"/>
<pin name="CMR4"/>
<pin name="RX4+"/>
</symbol>
<symbol name="749020010">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100/1000 Base-T,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION---STANDARD

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.	1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="TD1+"/>
<pin name="TCT1"/>
<pin name="TD1-"/>
<pin name="TCT2"/>
<pin name="TD2-"/>
<pin name="TD2+"/>
<pin name="MX2-"/>
<pin name="MX2+"/>
<pin name="MCT2"/>
<pin name="MX1-"/>
<pin name="MCT1"/>
<pin name="MX1+"/>
<pin name="TD3+"/>
<pin name="TCT3"/>
<pin name="TD3-"/>
<pin name="MX3-"/>
<pin name="MCT3"/>
<pin name="MX3+"/>
<pin name="TD4+"/>
<pin name="TCT4"/>
<pin name="TD4-"/>
<pin name="MX4-"/>
<pin name="MCT4"/>
<pin name="MX4+"/>
</symbol>
<symbol name="749020011">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100/1000 Base-T,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION---STANDARD

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="TD1+"/>
<pin name="TCT1"/>
<pin name="TD1-"/>
<pin name="TCT2"/>
<pin name="TD2-"/>
<pin name="TD2+"/>
<pin name="MX2-"/>
<pin name="MX2+"/>
<pin name="MCT2"/>
<pin name="MX1-"/>
<pin name="MCT1"/>
<pin name="MX1+"/>
<pin name="TCT3"/>
<pin name="TD3-"/>
<pin name="TD3+"/>
<pin name="MX3-"/>
<pin name="MX3+"/>
<pin name="MCT3"/>
<pin name="TCT4"/>
<pin name="TD4-"/>
<pin name="TD4+"/>
<pin name="MX4-"/>
<pin name="MX4+"/>
<pin name="MCT4"/>
</symbol>
<symbol name="749020013">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100/1000 Base-T,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION---STANDARD

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="D1+"/>
<pin name="TD1"/>
<pin name="D1-"/>
<pin name="TD2"/>
<pin name="D2-"/>
<pin name="D2+"/>
<pin name="X2-"/>
<pin name="X2+"/>
<pin name="TX2"/>
<pin name="X1-"/>
<pin name="TX1"/>
<pin name="X1+"/>
<pin name="TD3"/>
<pin name="D3-"/>
<pin name="D3+"/>
<pin name="X3-"/>
<pin name="X3+"/>
<pin name="TX3"/>
<pin name="TD4"/>
<pin name="D4-"/>
<pin name="D4+"/>
<pin name="X4-"/>
<pin name="X4+"/>
<pin name="TX4"/>
</symbol>
<symbol name="749020020A">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100/1000 Base-T,SMD

&lt;B&gt;NO OF PORT----2

&lt;B&gt;APPLICATION---STANDARD

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="TD1+"/>
<pin name="TCT1"/>
<pin name="TD1-"/>
<pin name="TCT2"/>
<pin name="TD2-"/>
<pin name="TD2+"/>
<pin name="MX2-"/>
<pin name="MX2+"/>
<pin name="MCT2"/>
<pin name="MX1-"/>
<pin name="MCT1"/>
<pin name="MX1+"/>
<pin name="TCT3"/>
<pin name="TD3-"/>
<pin name="TD3+"/>
<pin name="MX3-"/>
<pin name="MX3+"/>
<pin name="MCT3"/>
<pin name="TCT4"/>
<pin name="TD4-"/>
<pin name="TD4+"/>
<pin name="MX4-"/>
<pin name="MX4+"/>
<pin name="MCT4"/>
</symbol>
<symbol name="749020023">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100/1000 Base-T,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION---STANDARD

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="TD1+"/>
<pin name="TCT1"/>
<pin name="TD1-"/>
<pin name="TCT2"/>
<pin name="TD2-"/>
<pin name="TD2+"/>
<pin name="MX2-"/>
<pin name="MX2+"/>
<pin name="MCT2"/>
<pin name="MX1-"/>
<pin name="MCT1"/>
<pin name="MX1+"/>
<pin name="TCT3"/>
<pin name="TD3-"/>
<pin name="TD3+"/>
<pin name="MX3-"/>
<pin name="MX3+"/>
<pin name="MCT3"/>
<pin name="TCT4"/>
<pin name="TD4-"/>
<pin name="TD4+"/>
<pin name="MX4-"/>
<pin name="MX4+"/>
<pin name="MCT4"/>
</symbol>
<symbol name="749020100">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100/1000 Base-T,SMD

&lt;B&gt;NO OF PORT----0.5 LP

&lt;B&gt;APPLICATION----STANDARD

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="D+"/>
<pin name="TD1"/>
<pin name="D-"/>
<pin name="D1+"/>
<pin name="D1-"/>
<pin name="X1-"/>
<pin name="TX1"/>
<pin name="X1+"/>
<pin name="X-"/>
<pin name="TX"/>
<pin name="X+"/>
<pin name="TD2"/>
</symbol>
<symbol name="749020111">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100/1000 Base-T,SMD

&lt;B&gt;NO OF PORT----1 LP

&lt;B&gt;APPLICATION---STANDARD

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="D1+"/>
<pin name="TD1"/>
<pin name="D1-"/>
<pin name="TD2"/>
<pin name="D2-"/>
<pin name="D2+"/>
<pin name="X2-"/>
<pin name="X2+"/>
<pin name="TX2"/>
<pin name="X1-"/>
<pin name="TX1"/>
<pin name="X1+"/>
<pin name="D3+"/>
<pin name="TD3"/>
<pin name="D3-"/>
<pin name="TD4"/>
<pin name="D4-"/>
<pin name="D4+"/>
<pin name="TX4"/>
<pin name="X4+"/>
<pin name="X4-"/>
<pin name="X3-"/>
<pin name="TX3"/>
<pin name="X3+"/>
</symbol>
<symbol name="749022015">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100/1000 Base-T PoE+,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION---PoE+

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="D1+"/>
<pin name="TD1"/>
<pin name="D1-"/>
<pin name="TD2"/>
<pin name="D2-"/>
<pin name="D2+"/>
<pin name="X2-"/>
<pin name="X2+"/>
<pin name="TX2"/>
<pin name="X1-"/>
<pin name="TX1"/>
<pin name="X1+"/>
<pin name="TD3"/>
<pin name="D3-"/>
<pin name="D3+"/>
<pin name="X3-"/>
<pin name="X3+"/>
<pin name="TX3"/>
<pin name="TD4"/>
<pin name="D4-"/>
<pin name="D4+"/>
<pin name="X4-"/>
<pin name="X4+"/>
<pin name="TX4"/>
</symbol>
<symbol name="749023010">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100/1000 Base-T PoE,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION---PoE

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="TD1+"/>
<pin name="TCT1"/>
<pin name="TD1-"/>
<pin name="MX1-"/>
<pin name="MCT1"/>
<pin name="MX1+"/>
<pin name="TD2+"/>
<pin name="TCT2"/>
<pin name="TD2-"/>
<pin name="MX2-"/>
<pin name="MCT2"/>
<pin name="MX2+"/>
</symbol>
<symbol name="749023015">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100/1000 Base-T PoE,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION---PoE HPLE

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="D1+"/>
<pin name="TD1"/>
<pin name="D1-"/>
<pin name="TD2"/>
<pin name="D2-"/>
<pin name="D2+"/>
<pin name="X2-"/>
<pin name="X2+"/>
<pin name="TX2"/>
<pin name="X1-"/>
<pin name="TX1"/>
<pin name="X1+"/>
<pin name="D3+"/>
<pin name="TD3"/>
<pin name="D3-"/>
<pin name="TD4"/>
<pin name="D4-"/>
<pin name="D4+"/>
<pin name="X4-"/>
<pin name="X4+"/>
<pin name="TX4"/>
<pin name="X3-"/>
<pin name="TX3"/>
<pin name="X3+"/>
</symbol>
<symbol name="749023016">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100/1000 Base-T PoE,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION---PoE HPLE

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.	1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="D1+"/>
<pin name="TD1"/>
<pin name="D1-"/>
<pin name="TD2"/>
<pin name="D2-"/>
<pin name="D2+"/>
<pin name="X2-"/>
<pin name="X2+"/>
<pin name="TX2"/>
<pin name="X1-"/>
<pin name="TX1"/>
<pin name="X1+"/>
<pin name="D3+"/>
<pin name="TD3"/>
<pin name="D3-"/>
<pin name="TD4"/>
<pin name="D4-"/>
<pin name="D4+"/>
<pin name="X4-"/>
<pin name="X4+"/>
<pin name="TX4"/>
<pin name="X3-"/>
<pin name="TX3"/>
<pin name="X3+"/>
</symbol>
<symbol name="749023020">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10/100/1000 Base-T PoE,SMD

&lt;B&gt;NO OF PORT----2

&lt;B&gt;APPLICATION---PoE

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.	1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="TD1+"/>
<pin name="TCT1"/>
<pin name="TD1-"/>
<pin name="MX1-"/>
<pin name="MCT1"/>
<pin name="MX1+"/>
<pin name="TD2+"/>
<pin name="TCT2"/>
<pin name="TD2-"/>
<pin name="MX2-"/>
<pin name="MCT2"/>
<pin name="MX2+"/>
<pin name="TD3+"/>
<pin name="TCT3"/>
<pin name="TD3-"/>
<pin name="MX3-"/>
<pin name="MCT3"/>
<pin name="MX3+"/>
<pin name="TD4+"/>
<pin name="TCT4"/>
<pin name="TD4-"/>
<pin name="MX4-"/>
<pin name="MCT4"/>
<pin name="MX4+"/>
<pin name="TD5+"/>
<pin name="TCT5"/>
<pin name="TD5-"/>
<pin name="MX5-"/>
<pin name="MCT5"/>
<pin name="MX5+"/>
<pin name="TD6+"/>
<pin name="TCT6"/>
<pin name="TD6-"/>
<pin name="MX6-"/>
<pin name="MCT6"/>
<pin name="MX6+"/>
<pin name="TD7+"/>
<pin name="TCT7"/>
<pin name="TD7-"/>
<pin name="MX7-"/>
<pin name="MCT7"/>
<pin name="MX7+"/>
<pin name="TD8+"/>
<pin name="TCT8"/>
<pin name="TD8-"/>
<pin name="MX8-"/>
<pin name="MCT8"/>
<pin name="MX8+"/>
</symbol>
<symbol name="T_4W_2*2">
<pin name="N2_2" direction="pas"/>
<pin name="N1_2" direction="pas"/>
<pin name="N1_1" direction="pas"/>
<pin name="N3_1" direction="pas"/>
<pin name="N3_2" direction="pas"/>
<pin name="N2_1" direction="pas"/>
<pin name="N4_2" direction="pas"/>
<pin name="N4_1" direction="pas"/>
</symbol>
<symbol name="T_8PIN_1">
<pin name="NC5"/>
<pin name="NC1"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="NC4"/>
<pin name="GND2"/>
<pin name="FP"/>
<pin name="GND1"/>
</symbol>
<symbol name="WE-MCA">
<pin name="FP" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="WE-MCA_7488910092">
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
<pin name="NC1" direction="nc"/>
<pin name="FD" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC7" direction="nc"/>
<pin name="NC6" direction="pas"/>
<pin name="NC5" direction="nc"/>
</symbol>
<symbol name="T_4PIN">
<pin name="FD_LB" direction="pas"/>
<pin name="NC2" direction="nc"/>
<pin name="FD_HB" direction="pas"/>
<pin name="NC1" direction="nc"/>
</symbol>
<symbol name="WE-MCA_7488920245">
<pin name="NC1" direction="pwr"/>
<pin name="NC2" direction="pas"/>
<pin name="NC3" direction="pwr"/>
<pin name="GND1" direction="nc"/>
<pin name="FP" direction="nc"/>
<pin name="GND2" direction="nc"/>
</symbol>
<symbol name="L-3W">
<description>&lt;B&gt;WE-MLS mULTILINE emi Suppression Ferrite&lt;/b&gt;&lt;br&gt;
3 WAYS</description>
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="L-4W">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="T_12PIN_1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="T_6PIN">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="7499010441">
<pin name="RD+"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="CTD"/>
<pin name="CRD"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="LED-DUAL-2">
<description>DUAL LED</description>
<pin name="AK2" direction="pas"/>
<pin name="AK1" direction="pas"/>
</symbol>
<symbol name="7497110616">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer &amp; USB 3.0&lt;b&gt;
&lt;pre&gt;

Characteristics:
•RJ45 Connector with integrated transformer &amp; 2x USB 3.0 port &amp; LEDs
•Extended temperature range -40°C to +85°C
•10/100/1000 Base-T

Applications:
•Ethernet, 1 Gigabit Ethernet
•Embedded PC
•Hubs, Router, Switch
•USB 3.0</description>
<pin name="3"/>
<pin name="4"/>
<pin name="1"/>
<pin name="2"/>
<pin name="9"/>
<pin name="10" direction="pwr"/>
<pin name="7"/>
<pin name="8"/>
<pin name="6"/>
<pin name="5"/>
</symbol>
<symbol name="LED-2PIN">
<description>WE-RJ45 LAN HPLE RJ45 LAN Transformer-LED</description>
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
</symbol>
<symbol name="LED-DUAL">
<description>WE-RJ45 LAN HPLE RJ45 LAN Transformer-LED DUAL</description>
<pin name="AK2" direction="pas"/>
<pin name="AK1" direction="pas"/>
</symbol>
<symbol name="USB-3.0">
<pin name="D-"/>
<pin name="D+"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RX-"/>
<pin name="RX+"/>
<pin name="GND_SIG" direction="pwr"/>
<pin name="TX-"/>
<pin name="TX+"/>
</symbol>
<symbol name="GND_PIN">
<description>GND SHIELD PIN</description>
<pin name="1" direction="pwr"/>
</symbol>
<symbol name="7497111611A">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="3"/>
<pin name="4"/>
<pin name="1" direction="pwr"/>
<pin name="2"/>
<pin name="5"/>
<pin name="9"/>
<pin name="10"/>
<pin name="7"/>
<pin name="8"/>
<pin name="6"/>
</symbol>
<symbol name="LED2PIN">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer-LED&lt;b&gt;</description>
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
</symbol>
<symbol name="LED-DUAL1">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer-3-PIN LED</description>
<pin name="A1" direction="pas"/>
<pin name="K1" direction="pas"/>
<pin name="K2" direction="pas"/>
</symbol>
<symbol name="USB2.0">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer USB2.0-4 PIN USB</description>
<pin name="D-"/>
<pin name="D+"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="7499110122">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="2"/>
<pin name="7"/>
<pin name="3"/>
<pin name="9"/>
<pin name="8"/>
<pin name="1"/>
<pin name="6"/>
<pin name="5"/>
<pin name="4"/>
<pin name="10"/>
</symbol>
<symbol name="GNDPIN">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="7499110123">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="3"/>
<pin name="4"/>
<pin name="1"/>
<pin name="2"/>
<pin name="5"/>
<pin name="9"/>
<pin name="10"/>
<pin name="7"/>
<pin name="8"/>
<pin name="6"/>
</symbol>
<symbol name="7499110124">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="3"/>
<pin name="4"/>
<pin name="1"/>
<pin name="2"/>
<pin name="5"/>
<pin name="9"/>
<pin name="10"/>
<pin name="7"/>
<pin name="8"/>
<pin name="6"/>
</symbol>
<symbol name="LED-DUAL-1">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer-DUAL -LED</description>
<pin name="AK2" direction="pas"/>
<pin name="AK1" direction="pas"/>
</symbol>
<symbol name="7499111221A/7499111000A">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="2"/>
<pin name="7"/>
<pin name="3"/>
<pin name="9"/>
<pin name="8"/>
<pin name="1"/>
<pin name="6"/>
<pin name="5"/>
<pin name="4"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
</symbol>
<symbol name="7499111121A">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="3"/>
<pin name="4"/>
<pin name="1"/>
<pin name="2"/>
<pin name="5"/>
<pin name="9" direction="pwr"/>
<pin name="10" direction="pwr"/>
<pin name="7"/>
<pin name="8"/>
<pin name="6"/>
</symbol>
<symbol name="7499111446">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="3"/>
<pin name="4"/>
<pin name="1"/>
<pin name="2"/>
<pin name="5"/>
<pin name="9"/>
<pin name="10" direction="pwr"/>
<pin name="7"/>
<pin name="8"/>
<pin name="6"/>
</symbol>
<symbol name="7499111447">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="3"/>
<pin name="4"/>
<pin name="1"/>
<pin name="2"/>
<pin name="5"/>
<pin name="9"/>
<pin name="10"/>
<pin name="7"/>
<pin name="8"/>
<pin name="6"/>
</symbol>
<symbol name="7499151120">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="3"/>
<pin name="4"/>
<pin name="2"/>
<pin name="5"/>
<pin name="9"/>
<pin name="7"/>
<pin name="8"/>
<pin name="6"/>
<pin name="1"/>
</symbol>
<symbol name="7499511440">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="3"/>
<pin name="4"/>
<pin name="1"/>
<pin name="2"/>
<pin name="5"/>
<pin name="9"/>
<pin name="10"/>
<pin name="7"/>
<pin name="8"/>
<pin name="6"/>
<pin name="11"/>
<pin name="12"/>
<pin name="VC1-1" direction="pwr"/>
<pin name="VC1+1" direction="pwr"/>
<pin name="VC2+1" direction="pwr"/>
<pin name="VC2-1" direction="pwr"/>
</symbol>
<symbol name="7498111001">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="4"/>
<pin name="3"/>
<pin name="2"/>
<pin name="1"/>
<pin name="VCC"/>
<pin name="8"/>
<pin name="7"/>
<pin name="6"/>
<pin name="5"/>
<pin name="GND"/>
</symbol>
<symbol name="7498111120R">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="TRD1+"/>
<pin name="TRD1-"/>
<pin name="TRD0+"/>
<pin name="TRD0-"/>
<pin name="VCC" direction="pwr"/>
<pin name="TRD3+"/>
<pin name="TRD3-"/>
<pin name="TRD2+"/>
<pin name="TRD2-"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="74990X-THT-10/100-T">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="RD+"/>
<pin name="TCT"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="RCT"/>
<pin name="8"/>
</symbol>
<symbol name="74990X-THT-10/100-T-RVS">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="RD+"/>
<pin name="TCT"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="RCT"/>
<pin name="SH"/>
</symbol>
<symbol name="749921-THT-POE-RVS">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="TD+"/>
<pin name="RCT"/>
<pin name="TD-"/>
<pin name="RD+"/>
<pin name="RD-"/>
<pin name="TCT"/>
<pin name="VC1-" direction="pwr"/>
<pin name="VC1+" direction="pwr"/>
</symbol>
<symbol name="749921-TYPE-2-RVS">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="RD+"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="TCT"/>
<pin name="VC1-" direction="pwr"/>
<pin name="VC1+" direction="pwr"/>
<pin name="VC2+" direction="pwr"/>
<pin name="VC2-" direction="pwr"/>
</symbol>
<symbol name="749921-THT-POE">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="RD+"/>
<pin name="TCT"/>
<pin name="RD-" direction="oc"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="RCT"/>
<pin name="VC1-" direction="pwr"/>
<pin name="VC1+" direction="pwr"/>
</symbol>
<symbol name="749921-TYPE-2">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="RD+"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="CTD"/>
<pin name="VC1-" direction="pwr"/>
<pin name="VC1+" direction="pwr"/>
<pin name="VC2+" direction="pwr"/>
<pin name="VC2-" direction="pwr"/>
</symbol>
<symbol name="7498011211">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="RD+"/>
<pin name="TCT"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="RCT"/>
</symbol>
<symbol name="7499611421">
<description>&lt;b&gt;WE-RJ45 LAN RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:

•RJ45 Connector with integrated transformer/
 common mode choke
•Available in SMD, THT and THT with USB
•350µH min. OCL with 8mA bias
•Complies with IEEE 802.3
•Extended temperature range -40°C to +85°C available

Applications:

•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="3"/>
<pin name="4"/>
<pin name="1"/>
<pin name="2"/>
<pin name="9"/>
<pin name="10"/>
<pin name="7"/>
<pin name="8"/>
<pin name="11"/>
<pin name="12"/>
<pin name="6"/>
<pin name="5"/>
</symbol>
<symbol name="74990111215A">
<description>&lt;b&gt;WE-RJ45 LAN HPLE RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:
•HPLE = High Performance &amp; Low EMI 

Würth Elektronik just introduced a new High Performance &amp; Low EMI (HPLE) 
RJ45 Connector series with integrated magnetic filter 
components (Common Mode Choke) for Gigabit Ethernet and Power-over-Ethernet applications.
The main focus of the new high performance RJ45 Connectors is 
to reach a much higher attenuation in the frequency range between 100 MHz and 500 MHz.


Applications:
•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="RD+"/>
<pin name="CTD"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="CRD"/>
<pin name="SH" direction="pwr"/>
</symbol>
<symbol name="7499411122A">
<description>&lt;b&gt;WE-RJ45 LAN HPLE RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:
•HPLE = High Performance &amp; Low EMI 

Würth Elektronik just introduced a new High Performance &amp; Low EMI (HPLE) 
RJ45 Connector series with integrated magnetic filter 
components (Common Mode Choke) for Gigabit Ethernet and Power-over-Ethernet applications.
The main focus of the new high performance RJ45 Connectors is 
to reach a much higher attenuation in the frequency range between 100 MHz and 500 MHz.


Applications:
•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="12"/>
<pin name="4"/>
<pin name="11"/>
<pin name="10"/>
<pin name="5"/>
<pin name="VC1-" direction="pwr"/>
<pin name="VC1+" direction="pwr"/>
<pin name="VC2+" direction="pwr"/>
<pin name="VC2-" direction="pwr"/>
<pin name="6"/>
</symbol>
<symbol name="7499211123A">
<description>&lt;b&gt;WE-RJ45 LAN HPLE RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:
•HPLE = High Performance &amp; Low EMI 

Würth Elektronik just introduced a new High Performance &amp; Low EMI (HPLE) 
RJ45 Connector series with integrated magnetic filter 
components (Common Mode Choke) for Gigabit Ethernet and Power-over-Ethernet applications.
The main focus of the new high performance RJ45 Connectors is 
to reach a much higher attenuation in the frequency range between 100 MHz and 500 MHz.


Applications:
•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="3"/>
<pin name="4"/>
<pin name="1"/>
<pin name="2"/>
<pin name="5"/>
<pin name="VC1-" direction="pwr"/>
<pin name="VC1+" direction="pwr"/>
<pin name="VC2+" direction="pwr"/>
<pin name="VC2-" direction="pwr"/>
</symbol>
<symbol name="7499511611A">
<description>&lt;b&gt;WE-RJ45 LAN HPLE RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:
•HPLE = High Performance &amp; Low EMI 

Würth Elektronik just introduced a new High Performance &amp; Low EMI (HPLE) 
RJ45 Connector series with integrated magnetic filter 
components (Common Mode Choke) for Gigabit Ethernet and Power-over-Ethernet applications.
The main focus of the new high performance RJ45 Connectors is 
to reach a much higher attenuation in the frequency range between 100 MHz and 500 MHz.


Applications:
•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="11"/>
<pin name="4"/>
<pin name="12"/>
<pin name="10"/>
<pin name="5"/>
<pin name="VC1-" direction="pwr"/>
<pin name="VC1+" direction="pwr"/>
<pin name="VC2+" direction="pwr"/>
<pin name="VC2-" direction="pwr"/>
<pin name="6"/>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
</symbol>
<symbol name="7499111614A">
<description>&lt;b&gt;WE-RJ45 LAN HPLE RJ45 LAN Transformer&lt;b&gt;
&lt;pre&gt;
Characteristics:
•HPLE = High Performance &amp; Low EMI 

Würth Elektronik just introduced a new High Performance &amp; Low EMI (HPLE) 
RJ45 Connector series with integrated magnetic filter 
components (Common Mode Choke) for Gigabit Ethernet and Power-over-Ethernet applications.
The main focus of the new high performance RJ45 Connectors is 
to reach a much higher attenuation in the frequency range between 100 MHz and 500 MHz.


Applications:
•ADSL Modems
•Embedded PC
•LAN Applications
•Hub, Router, Switches</description>
<pin name="4"/>
<pin name="3"/>
<pin name="2"/>
<pin name="1"/>
<pin name="8"/>
<pin name="7"/>
<pin name="6"/>
<pin name="5"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
</symbol>
<symbol name="WE-SCC">
<description>&lt;B&gt;WE-SCC SMD Common Mode Line Filter</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WE-SHC">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="3L">
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="TRANSFORMER_11PIN">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="L4">
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="TRANSFORMER_9PIN_1">
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="TRANSFORMER_13PIN">
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="TRANSFORMER_14PIN">
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-TVS_6RTR4">
<pin name="6"/>
<pin name="VDD" direction="pwr"/>
<pin name="4"/>
<pin name="3"/>
<pin name="GND" direction="pwr"/>
<pin name="1"/>
</symbol>
<symbol name="WE-TVS_5RTR2/4RTR2">
<pin name="VDD" direction="pwr"/>
<pin name="2"/>
<pin name="1"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="WE-TVS_6RTR4D">
<pin name="4" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="WE-TVS_3ESD2">
<pin name="I/O2"/>
<pin name="I/O1"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="WE-TVS_3ESB2B">
<pin name="I/O2"/>
<pin name="I/O1"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="WE-TVS_6RTR4FD">
<pin name="VDD" direction="pwr"/>
<pin name="I/O1-1"/>
<pin name="I/O2-1"/>
<pin name="I/O1"/>
<pin name="I/O2"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="WE-TVS_10RTR4D">
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="I/O1"/>
<pin name="I/O2"/>
<pin name="I/O3"/>
<pin name="I/O4"/>
</symbol>
<symbol name="WE-TVS_8RTR6">
<pin name="GND" direction="pwr"/>
<pin name="I/O1"/>
<pin name="I/O2"/>
<pin name="I/O6"/>
<pin name="I/O3"/>
<pin name="I/O4" direction="oc"/>
<pin name="I/O5"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="WE-TVS_6ESD4">
<pin name="2"/>
<pin name="1"/>
<pin name="GND"/>
<pin name="4"/>
<pin name="3"/>
<pin name="GND@1"/>
</symbol>
<symbol name="WE-TVS_6ESD5">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WE-TVS_5ESD4">
<pin name="2"/>
<pin name="1"/>
<pin name="GND"/>
<pin name="4"/>
<pin name="3"/>
</symbol>
<symbol name="L_1W:2W">
<description>&lt;B&gt;Off-line transformer WE-UNIT</description>
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="TRANSFORMER_3L_1">
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="TRANSFORMER_4L">
<description>&lt;b&gt;Universal Offline Standard Transformers WE-UOST</description>
<pin name="1" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="VARISTOR">
<description>&lt;b&gt;Characteristics:&lt;/b&gt;
&lt;pre&gt;
	WE-VD Disk Varistor
•Low clamping voltage
•After a surge impulse the varistor works immediately 
 in normal mode so there is no slip current
•Excellent absorption at surge impulses&lt;/pre&gt;&lt;br&gt;

&lt;b&gt;Applications:&lt;/b&gt;
&lt;pre&gt;
•12–48 VDC distribution
•110–400 V power supply
•Leakage of voltage peaks
•Surge protection in accordance with EN 61000-4-5
&lt;/pre&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WE-VE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WE-VEA">
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="L_2W:1W">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="L_2W:2W">
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="L_2W:2W_2">
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="L_2W:4W">
<pin name="1" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="L_3W:1W">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="WE-FB_EE20/10/6">
<pin name="13" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="L_3W:3W">
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="L_3W:2W">
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="L_3W:3W_2">
<pin name="9" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="L_2W:1W_1">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="L_1W:2W_1">
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="749050010A-1">
<description>&lt;PRE&gt;
Typical electrical Values for WE-LAN 10G Base-T ,SMD

&lt;B&gt;NO OF PORT----1

&lt;B&gt;APPLICATION---STANDARD

Inductance   		350 µH     		100 kHz, 100 mV, 8 mADC
 
Insulation Test Voltage	1500 Vrms		1 Minute
 
Turns Ratio			1:1		± 2%
 
Insertion Loss		-1.1 dB typ.		1 MHz - 100 MHz
 
Return Loss		
	-16 dB min.		1 MHz - 30 MHz

	-14 dB min.		30 MHz - 45 MHz

	-12 dB min.		45 MHz - 60 MHz

	-10 dB min.		60 MHz - 100 MHz
 
Crosstalk		-38 dB typ.		1 MHz - 100 MHz
 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz

 
Differential to Common Mode Rejection	-38 dB typ.		1 MHz - 100 MHz</description>
<pin name="D1+"/>
<pin name="TD1"/>
<pin name="D1-"/>
<pin name="TD2"/>
<pin name="D2-"/>
<pin name="D2+"/>
<pin name="X2-"/>
<pin name="X2+"/>
<pin name="TX2"/>
<pin name="X1-"/>
<pin name="TX1"/>
<pin name="X1+"/>
<pin name="D3+"/>
<pin name="TD3"/>
<pin name="D3-"/>
<pin name="TD4"/>
<pin name="D4-"/>
<pin name="D4+"/>
<pin name="X4-"/>
<pin name="X4+"/>
<pin name="TX4"/>
<pin name="X3-"/>
<pin name="TX3"/>
<pin name="X3+"/>
</symbol>
<symbol name="74990111211">
<pin name="1"/>
<pin name="4"/>
<pin name="2"/>
<pin name="3"/>
<pin name="6"/>
<pin name="5"/>
<pin name="8"/>
</symbol>
<symbol name="L_1W:1W">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-LAN10G:1.27&amp;0.99">
<pin name="TD1-"/>
<pin name="TCT1"/>
<pin name="TD1+"/>
<pin name="MX1+"/>
<pin name="MCT1"/>
<pin name="MX1-"/>
<pin name="TD2+"/>
<pin name="TCT2"/>
<pin name="TD2-"/>
<pin name="TD3+"/>
<pin name="TCT3"/>
<pin name="TD3-"/>
<pin name="TD4+"/>
<pin name="TCT4"/>
<pin name="TD4-"/>
<pin name="MX2+"/>
<pin name="MCT2"/>
<pin name="MX2-"/>
<pin name="MX3+"/>
<pin name="MCT3"/>
<pin name="MX3-"/>
<pin name="MX4+"/>
<pin name="MCT4"/>
<pin name="MX4-"/>
</symbol>
<symbol name="BIDIRECTIONAL">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="UNIDIRECTIONAL">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="8492121">
<pin name="VDD" direction="pas"/>
<pin name="D+" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="D-" direction="pas"/>
</symbol>
<symbol name="WE-EXB">
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="WE-WPCC_2W">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WE-DS_9PIN">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="WE-DS-15PIN">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="WE-DS_25PIN">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="WE-DS-37PIN">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="WE-DS_9PIN_SMD">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="WE-DS_15PIN_SMD">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="WE-DS_25PIN_SMD">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="WE-DS_37PIN_SMD">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="7490120110">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
</symbol>
<symbol name="7490100111A">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="6"/>
<pin name="8"/>
<pin name="7"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
</symbol>
<symbol name="7490100161A">
<pin name="TX+"/>
<pin name="CTX"/>
<pin name="TX-"/>
<pin name="RX+"/>
<pin name="RX-"/>
<pin name="CRX"/>
<pin name="RD-"/>
<pin name="CRD"/>
<pin name="RD+"/>
<pin name="TD-"/>
<pin name="CTD"/>
<pin name="TD+"/>
</symbol>
<symbol name="7490140112">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
</symbol>
<symbol name="749014018">
<pin name="RD+"/>
<pin name="CRD"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="CTD"/>
<pin name="TX-"/>
<pin name="CTX"/>
<pin name="TX+"/>
<pin name="RX-"/>
<pin name="CRX"/>
<pin name="RX+"/>
</symbol>
<symbol name="749020010A">
<pin name="TCT1"/>
<pin name="TD1+"/>
<pin name="TD1-"/>
<pin name="MX1-"/>
<pin name="MX1+"/>
<pin name="MCT1"/>
<pin name="TCT2"/>
<pin name="TD2+"/>
<pin name="TD2-"/>
<pin name="MX2-"/>
<pin name="MX2+"/>
<pin name="MCT2"/>
<pin name="TCT3"/>
<pin name="TD3+"/>
<pin name="TD3-"/>
<pin name="MX3-"/>
<pin name="MX3+"/>
<pin name="MCT3"/>
<pin name="TCT4"/>
<pin name="TD4+"/>
<pin name="TD4-"/>
<pin name="MX4-"/>
<pin name="MX4+"/>
<pin name="MCT4"/>
</symbol>
<symbol name="7490200136">
<pin name="D+"/>
<pin name="TD"/>
<pin name="D-"/>
<pin name="TD1"/>
<pin name="TD2"/>
<pin name="TD3"/>
<pin name="D1+"/>
<pin name="D1-"/>
<pin name="D2+"/>
<pin name="D2-"/>
<pin name="D3+"/>
<pin name="D3-"/>
<pin name="TX"/>
<pin name="TX1"/>
<pin name="TX2"/>
<pin name="TX3"/>
<pin name="X-"/>
<pin name="X+"/>
<pin name="X1+"/>
<pin name="X1-"/>
<pin name="X2+"/>
<pin name="X2-"/>
<pin name="X3+"/>
<pin name="X3-"/>
</symbol>
<symbol name="749020111A">
<pin name="D1+"/>
<pin name="TD1"/>
<pin name="D1-"/>
<pin name="TD2"/>
<pin name="D2-"/>
<pin name="D2+"/>
<pin name="X2-"/>
<pin name="X2+"/>
<pin name="TX2"/>
<pin name="X1-"/>
<pin name="TX1"/>
<pin name="X1+"/>
<pin name="D3+"/>
<pin name="TD3"/>
<pin name="D3-"/>
<pin name="TD4"/>
<pin name="D4-"/>
<pin name="D4+"/>
<pin name="X4-"/>
<pin name="X4+"/>
<pin name="TX4"/>
<pin name="X3-"/>
<pin name="TX3"/>
<pin name="X3+"/>
</symbol>
<symbol name="7499211125">
<pin name="RD+"/>
<pin name="CRD"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="CTD"/>
<pin name="TD-"/>
<pin name="VC1+"/>
<pin name="VC1-"/>
</symbol>
<symbol name="7499410420">
<pin name="6"/>
<pin name="4"/>
<pin name="5"/>
<pin name="2"/>
<pin name="3"/>
<pin name="1"/>
<pin name="V+"/>
<pin name="V-"/>
</symbol>
<symbol name="7490100110A">
<pin name="RX+"/>
<pin name="CRX"/>
<pin name="RX-"/>
<pin name="RD-"/>
<pin name="CRD"/>
<pin name="RD+"/>
<pin name="TX+"/>
<pin name="CTX"/>
<pin name="TX-"/>
<pin name="TD-"/>
<pin name="CTD"/>
<pin name="TD+"/>
</symbol>
<symbol name="749010012A">
<pin name="TD+"/>
<pin name="CTD"/>
<pin name="TD-"/>
<pin name="RD+"/>
<pin name="RD-"/>
<pin name="CRD"/>
<pin name="RX-"/>
<pin name="CRX"/>
<pin name="RX+"/>
<pin name="TX-"/>
<pin name="CTX"/>
<pin name="TX+"/>
</symbol>
<symbol name="749013011A">
<pin name="TD+"/>
<pin name="CTD"/>
<pin name="TD-"/>
<pin name="TX-"/>
<pin name="CTX"/>
<pin name="TX+"/>
<pin name="RD+"/>
<pin name="CRD"/>
<pin name="RD-"/>
<pin name="RX-"/>
<pin name="CRX"/>
<pin name="RX+"/>
</symbol>
<symbol name="749023010A">
<pin name="2"/>
<pin name="1"/>
<pin name="3"/>
<pin name="22"/>
<pin name="24"/>
<pin name="23"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="19"/>
<pin name="21"/>
<pin name="20"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="16"/>
<pin name="18"/>
<pin name="17"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
</symbol>
<symbol name="749022012X">
</symbol>
<symbol name="74990111217">
<pin name="TD+"/>
<pin name="TCT"/>
<pin name="TD-"/>
<pin name="RD+"/>
<pin name="RD-"/>
<pin name="RCT"/>
<pin name="8"/>
</symbol>
<symbol name="74980111211">
<pin name="TD+"/>
<pin name="TCT"/>
<pin name="TD-"/>
<pin name="RD+"/>
<pin name="RD-"/>
<pin name="RCT"/>
<pin name="8"/>
</symbol>
<symbol name="7498111001A">
<pin name="4"/>
<pin name="3"/>
<pin name="2"/>
<pin name="1"/>
<pin name="VCC"/>
<pin name="8"/>
<pin name="7"/>
<pin name="6"/>
<pin name="5"/>
<pin name="GND"/>
</symbol>
<symbol name="74990100011A">
<pin name="RD+"/>
<pin name="TCT"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="RCT"/>
</symbol>
<symbol name="7499011001A">
<pin name="RD+"/>
<pin name="TCT"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="RCT"/>
</symbol>
<symbol name="7499111001A">
<pin name="3"/>
<pin name="4"/>
<pin name="1"/>
<pin name="2"/>
<pin name="VCC"/>
<pin name="7"/>
<pin name="8"/>
<pin name="6"/>
<pin name="5"/>
<pin name="GND"/>
</symbol>
<symbol name="WE-LAN10G:1.27&amp;0.99A">
<pin name="TD1-"/>
<pin name="TCT1"/>
<pin name="TD1+"/>
<pin name="MX1+"/>
<pin name="MCT1"/>
<pin name="MX1-"/>
<pin name="TD2+"/>
<pin name="TCT2"/>
<pin name="TD2-"/>
<pin name="TD3+"/>
<pin name="TCT3"/>
<pin name="TD3-"/>
<pin name="TD4+"/>
<pin name="TCT4"/>
<pin name="TD4-"/>
<pin name="MX2+"/>
<pin name="MCT2"/>
<pin name="MX2-"/>
<pin name="MX3+"/>
<pin name="MCT3"/>
<pin name="MX3-"/>
<pin name="MX4+"/>
<pin name="MCT4"/>
<pin name="MX4-"/>
</symbol>
<symbol name="749050010U">
<pin name="D1+"/>
<pin name="TD1"/>
<pin name="D1-"/>
<pin name="TD2"/>
<pin name="D2-"/>
<pin name="D2+"/>
<pin name="X2-"/>
<pin name="X2+"/>
<pin name="TX2"/>
<pin name="X1-"/>
<pin name="TX1"/>
<pin name="X1+"/>
<pin name="D3+"/>
<pin name="TD3"/>
<pin name="D3-"/>
<pin name="TD4"/>
<pin name="D4-"/>
<pin name="D4+"/>
<pin name="X4-"/>
<pin name="X4+"/>
<pin name="TX4"/>
<pin name="X3-"/>
<pin name="TX3"/>
<pin name="X3+"/>
</symbol>
<symbol name="WE_LPF_0805">
<pin name="OUT" direction="out"/>
<pin name="GND3" direction="pwr"/>
<pin name="NC1" direction="nc"/>
<pin name="GND4" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="GND1" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND2" direction="pwr"/>
</symbol>
<symbol name="WE-POE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="WE-PP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-TVS_824011">
<pin name="I/O2"/>
<pin name="I/O1"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="L_3W:2W-1">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="L_2W:2W_1">
<pin name="1" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="L_3W:1W-1">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="L_3W:1W-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="L_3W:1W-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="L_4W:1W">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="L_4W:1W_1">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="L_3W:2W-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="L_3W:3W_1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="PASTE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="WE-UNIT_NXP_750871830">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="CMBHV">
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="L-1W-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WE-TPB">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="749022012X-1">
<pin name="TD1+"/>
<pin name="TCT1"/>
<pin name="TD1-"/>
<pin name="MX1+"/>
<pin name="MCT1"/>
<pin name="MX1-"/>
<pin name="TD2+"/>
<pin name="TCT2"/>
<pin name="TD2-"/>
<pin name="MX2+"/>
<pin name="MCT2"/>
<pin name="MX2-"/>
<pin name="TD3+"/>
<pin name="TCT3"/>
<pin name="TD3-"/>
<pin name="MX3+"/>
<pin name="MCT3"/>
<pin name="MX3-"/>
<pin name="TD4+"/>
<pin name="TCT4"/>
<pin name="TD4-"/>
<pin name="MX4+"/>
<pin name="MCT4"/>
<pin name="MX4-"/>
</symbol>
<symbol name="749020022A">
<pin name="TCT1"/>
<pin name="TD1+"/>
<pin name="TD1-"/>
<pin name="MX1-"/>
<pin name="MCT1"/>
<pin name="MX1+"/>
<pin name="TCT2"/>
<pin name="TD2+"/>
<pin name="TD2-"/>
<pin name="MX2-"/>
<pin name="MCT2"/>
<pin name="MX2+"/>
<pin name="TCT3"/>
<pin name="TD3+"/>
<pin name="TD3-"/>
<pin name="MX3-"/>
<pin name="MCT3"/>
<pin name="MX3+"/>
<pin name="TCT4"/>
<pin name="TD4+"/>
<pin name="TD4-"/>
<pin name="MX4-"/>
<pin name="MCT4"/>
<pin name="MX4+"/>
<pin name="TCT5"/>
<pin name="TD5+"/>
<pin name="TD5-"/>
<pin name="MX5-"/>
<pin name="MCT5"/>
<pin name="MX5+"/>
<pin name="TCT6"/>
<pin name="TD6+"/>
<pin name="TD6-"/>
<pin name="MX6-"/>
<pin name="MCT6"/>
<pin name="MX6+"/>
<pin name="TCT7"/>
<pin name="TD7+"/>
<pin name="TD7-"/>
<pin name="MX7-"/>
<pin name="MCT7"/>
<pin name="MX7+"/>
<pin name="TCT8"/>
<pin name="TD8+"/>
<pin name="TD8-"/>
<pin name="MX8-"/>
<pin name="MCT8"/>
<pin name="MX8+"/>
</symbol>
<symbol name="7490140110">
<pin name="CRD"/>
<pin name="RD+"/>
<pin name="RD-"/>
<pin name="RX-"/>
<pin name="CRX"/>
<pin name="RX+"/>
<pin name="CTD"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="TX-"/>
<pin name="CTX"/>
<pin name="TX+"/>
</symbol>
<symbol name="749020100A">
<pin name="CT1"/>
<pin name="RD+"/>
<pin name="RD-"/>
<pin name="RX-"/>
<pin name="CT2"/>
<pin name="RX+"/>
<pin name="CT"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="TX-"/>
<pin name="CT3"/>
<pin name="TX+"/>
</symbol>
<symbol name="7497011611A">
<pin name="4"/>
<pin name="1"/>
<pin name="5"/>
<pin name="2"/>
<pin name="3"/>
<pin name="6"/>
</symbol>
<symbol name="LED_2PIN">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
</symbol>
<symbol name="LED_DOUB">
<pin name="AK2" direction="pas"/>
<pin name="AK1" direction="pas"/>
</symbol>
<symbol name="USB2.0-1">
<pin name="D-"/>
<pin name="D+"/>
<pin name="GND" direction="pwr"/>
<pin name="VUSB" direction="pwr"/>
</symbol>
<symbol name="7498210002">
<pin name="4"/>
<pin name="6"/>
<pin name="5"/>
<pin name="VC1-" direction="pwr"/>
<pin name="VC1+" direction="pwr"/>
<pin name="2"/>
<pin name="3"/>
<pin name="1"/>
</symbol>
<symbol name="7498210003">
<pin name="P4"/>
<pin name="P2"/>
<pin name="P6"/>
<pin name="P1"/>
<pin name="P3"/>
<pin name="P5"/>
<pin name="VC1+"/>
<pin name="VC1-"/>
<pin name="VC2+"/>
<pin name="VC2-"/>
</symbol>
<symbol name="7498210220A">
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="V+"/>
<pin name="V1+"/>
<pin name="V-"/>
<pin name="V1-"/>
</symbol>
<symbol name="7499010003A">
<pin name="RD+"/>
<pin name="TCT"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="RCT"/>
<pin name="8"/>
</symbol>
<symbol name="74990101212">
<pin name="RD+"/>
<pin name="TCT"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="RCT"/>
<pin name="8"/>
</symbol>
<symbol name="74990101241">
<pin name="RD+"/>
<pin name="TCT"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="RCT"/>
<pin name="8"/>
</symbol>
<symbol name="7499010126A">
<pin name="RD+"/>
<pin name="TCT"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="RCT"/>
<pin name="8"/>
</symbol>
<symbol name="7499011441A">
<pin name="RD+"/>
<pin name="TCT"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="RCT"/>
<pin name="8"/>
</symbol>
<symbol name="7499021002A">
<pin name="RD+"/>
<pin name="TCT"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="RCT"/>
<pin name="8"/>
</symbol>
<symbol name="SHIELD">
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="7499110120A">
<pin name="4"/>
<pin name="5"/>
<pin name="2"/>
<pin name="3"/>
<pin name="10"/>
<pin name="1"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
</symbol>
<symbol name="7499410213">
<pin name="RD+"/>
<pin name="CTD"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="VC1+"/>
<pin name="VC1-"/>
<pin name="VC2+"/>
<pin name="VC2-"/>
</symbol>
<symbol name="7499410221">
<pin name="P2"/>
<pin name="P1"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="SHIELD"/>
<pin name="P8"/>
<pin name="P7"/>
<pin name="P10"/>
<pin name="P9"/>
</symbol>
<symbol name="7499511002A">
<pin name="P11"/>
<pin name="P12"/>
<pin name="P10"/>
<pin name="P4"/>
<pin name="P6"/>
<pin name="P5"/>
<pin name="P3"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P8"/>
<pin name="P7"/>
<pin name="P9"/>
<pin name="VC1"/>
<pin name="VC2"/>
<pin name="VC3"/>
<pin name="VC4"/>
</symbol>
<symbol name="749022012X-2">
<pin name="TD1+"/>
<pin name="TCT1"/>
<pin name="TD1-"/>
<pin name="MX1+"/>
<pin name="MCT1"/>
<pin name="MX1-"/>
<pin name="TD2+"/>
<pin name="TCT2"/>
<pin name="TD2-"/>
<pin name="MX2+"/>
<pin name="MCT2"/>
<pin name="MX2-"/>
<pin name="TD3+"/>
<pin name="TCT3"/>
<pin name="TD3-"/>
<pin name="MX3+"/>
<pin name="MCT3"/>
<pin name="MX3-"/>
<pin name="TD4+"/>
<pin name="TCT4"/>
<pin name="TD4-"/>
<pin name="MX4+"/>
<pin name="MCT4"/>
<pin name="MX4-"/>
</symbol>
<symbol name="7490220115">
<pin name="TD1"/>
<pin name="D1+"/>
<pin name="D1-"/>
<pin name="X1-"/>
<pin name="TX1"/>
<pin name="X1+"/>
<pin name="TD2"/>
<pin name="D2+"/>
<pin name="D2-"/>
<pin name="X2-"/>
<pin name="TX2"/>
<pin name="X2+"/>
<pin name="TD3"/>
<pin name="D3+"/>
<pin name="D3-"/>
<pin name="X3-"/>
<pin name="TX3"/>
<pin name="X3+"/>
<pin name="TD4"/>
<pin name="D4+"/>
<pin name="D4-"/>
<pin name="X4-"/>
<pin name="TX4"/>
<pin name="X4+"/>
</symbol>
<symbol name="WE-LPCC">
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="LED_DOUB-1">
<pin name="AK2" direction="pas"/>
<pin name="AK1" direction="pas"/>
</symbol>
<symbol name="WE-TIF">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WE-FB_EE16/8/5">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="WE-LAN_AQ_749010310">
<pin name="RD+"/>
<pin name="CRX"/>
<pin name="RD-"/>
<pin name="TD+"/>
<pin name="TD-"/>
<pin name="CTX"/>
<pin name="TX-"/>
<pin name="CTD"/>
<pin name="TX+"/>
<pin name="RX-"/>
<pin name="CRD"/>
<pin name="RX+"/>
</symbol>
<symbol name="WE-FLEXHV_EFD">
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="WE-FLEXHV_ER">
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="WE-DPC_HV">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-DPC">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-AMT" prefix="T" uservalue="yes">
<description>&lt;b&gt;MID-AMT Analog Modem Transformer&lt;/b&gt;&lt;p&gt;

&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;&lt;/b&gt; UL/IEC/EN 60950 compatible
&lt;br&gt; V.29-UL1950
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;/b&gt; Analog Modems
&lt;br&gt; 
&lt;br&gt; 


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/mid-amt_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/ctm/thb_mid-amt_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-AMT/?m"&gt;http://katalog.we-online.de/en/ctm/MID-AMT/?m&lt;/a&gt;&lt;p&gt;


Updated on 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="_750082107" package="WE-AMT_750082107">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_750082111" package="WE-AMT_750082111">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7500718001" package="WE-AMT_7500718001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7500718489" package="WE-AMT_7500718489">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DAA" prefix="L" uservalue="yes">
<description>&lt;b&gt;MID-DAA V.90 Conexant SmartDAA(TM) Signal Transformers&lt;/b&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;/b&gt;&lt;br&gt; Small Size
&lt;br&gt; Flat profile
&lt;br&gt; SMD
&lt;br&gt; V.90 performance
&lt;br&gt; Released for Conexant SmartDAA(TM) solution

&lt;br&gt; 
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;/b&gt; Analog modems
&lt;br&gt; Point of sale
&lt;br&gt;Signal isolation
&lt;br&gt; 
&lt;br&gt; 


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/MID-DAA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/ctm/thb_MID-DAA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-DAA/750082154?m"&gt;http://katalog.we-online.de/en/ctm/MID-DAA/750082154?m&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="_750082154" package="WE-DAA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="750082154/30uH"/>
</technology>
</technologies>
</device>
<device name="_750110007" package="WE-DAA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="750110007/30uH"/>
</technology>
</technologies>
</device>
<device name="_750082157" package="WE-DAA_750082157">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="750082157/450uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-ASI_M" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-ASI SMD Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Specially designed for sensors and actuators

&lt;br&gt; High current and small footprint
&lt;br&gt; High self resonant frequency
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; ASI-applications
&lt;br&gt;Low frequency filter design (kHz range)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndASI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndASI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-ASI"&gt;http://katalog.we-online.de/en/pbs/WE-ASI&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-ASI_M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744776333">
<attribute name="WE-NUMBER" value="744776333/3mH"/>
</technology>
<technology name="_744776347">
<attribute name="WE-NUMBER" value="744776347/4,7mH"/>
</technology>
<technology name="_744776360">
<attribute name="WE-NUMBER" value="744776360/6mH"/>
</technology>
<technology name="_744776381">
<attribute name="WE-NUMBER" value="744776381/8mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-BPF_1008" prefix="BPF" uservalue="yes">
<description>&lt;b&gt;Multilayer Chip Band-Pass Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;  Multilayer Chip Band-Pass Filter with low insertion loss and high attenuation
&lt;br&gt;
&lt;br&gt; SMD component in the sizes 0805 and 1008
&lt;br&gt;
&lt;br&gt; Guaranteed filter characteristics over a wide temperature range
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt;
&lt;br&gt; Wireless communication systems like DECT, PACS, PHS, GSM, WLAN, Bluetooth …

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/RfBPF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_RfBPF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-BPF"&gt;http://katalog.we-online.de/en/pbs/WE-BPF&lt;/a&gt;&lt;p&gt;



Updated by  Dan Xu 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="BPF_T1/T5"/>
</gates>
<devices>
<device name="" package="WE-BPF_1008_T5">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="3"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="_748351024"/>
<technology name="_748351124"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CAIR_4248" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CAIR Air coil
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Inductance values from 1.65nH up to 120 nH
&lt;br&gt; Very high quality factor &gt;100
&lt;br&gt; High self-resonant frequency

&lt;br&gt; High currents up to 3.5 A

&lt;br&gt; 5%(10%) Inductance tolerance
&lt;br&gt; Pick and place process possible
&lt;br&gt; Good solderability (Tinned connector pins)
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;&lt;/b&gt; Especially for RF application
&lt;br&gt; Ideal for high current applications
&lt;br&gt; Broad band filter
&lt;br&gt; RF-Decoupling
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/RfCAIR_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_RfCAIR_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CAIR"&gt;http://katalog.we-online.de/en/pbs/WE-CAIR&lt;/a&gt;&lt;p&gt;

Created on 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CAIR_4248">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744912122">
<attribute name="WE-NUMBER" value="744912122/22nH"/>
</technology>
<technology name="_744912127">
<attribute name="WE-NUMBER" value="744912127/27nH"/>
</technology>
<technology name="_744912133">
<attribute name="WE-NUMBER" value="744912133/33nH"/>
</technology>
<technology name="_744912139">
<attribute name="WE-NUMBER" value="744912139/39nH"/>
</technology>
<technology name="_744912147">
<attribute name="WE-NUMBER" value="744912147/47nH"/>
</technology>
<technology name="_744912156">
<attribute name="WE-NUMBER" value="744912156/56nH"/>
</technology>
<technology name="_744912168">
<attribute name="WE-NUMBER" value="744912168/68nH"/>
</technology>
<technology name="_744912182">
<attribute name="WE-NUMBER" value="744912182/82nH"/>
</technology>
<technology name="_744912210">
<attribute name="WE-NUMBER" value="744912210/100nH"/>
</technology>
<technology name="_744912212">
<attribute name="WE-NUMBER" value="744912212/120nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CBA_1806" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CBA SMD EMI Suppression Ferrite Bead
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;Reliable Ni-Sn electrodes
&lt;br&gt;High rated current up to 5A
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -55°C to +125°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;* Perfect as data line filter and for uncoupling of distribution voltage
&lt;BR&gt;
&lt;br&gt;*This special SMD chip bead ferrites can be put directly on the printed circuit board. They offer excellent anti-EMI properties and low DC-resistance. Placed very close next to the interference source even with smallest size 0402,maximal impedance at 1000 Ω can be reached.&lt;BR&gt;
&lt;br&gt;*High Speed:&lt;BR&gt;"High Speed " SMD ferrites WE-CBF have lower impedance in the lower frequency ranges thus they have only a low attenuation for fast signals. Application e.g. USB 2.0, IEEE 1394,LVDS &lt;BR&gt;
&lt;br&gt;*Wide Band:&lt;BR&gt; "Wide Band" SMD ferrites WE-CBF already show high impedance in low frequency range. Therefore they are wide band through the whole spectrum. Application e.g. control signats, RS232, RS422, DC/DC converter &lt;BR&gt;
&lt;br&gt;*High Current:&lt;BR&gt;"High Current " SMD ferrites WE-CBF are designed for high current (over 1 A). The rated current refers to 40K self-heating. High current SMD ferrites are available in all there types (High Speed, Wide Band and High Frequency). Application e.g. power supply, DC/DC converter&lt;BR&gt;
&lt;br&gt;*Advice:&lt;BR&gt;Pay attention for the use of SMD-Ferrites for high current&gt;1A and ambient temperature over +85°C that the rated current has to be reduced when temperature is above +85°C (Derating).&lt;BR&gt;
&lt;br&gt;*At+100°C environment temperature the maximal rated current has to add up to only 60% of the data sheet value ,without an overload of the component.&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeCBA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeCBA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBA/"&gt;http://katalog.we-online.de/en/pbs/WE-CBA/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-02
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_(HC)" package="WE-CBA_1806(W=6.5)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_782963560"/>
<technology name="_782963820"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CBF_1812" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CBF SMD EMI Suppression Ferrite Bead
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Reliable Ni-Sn electrodes
&lt;br&gt;
&lt;br&gt; High rated current up to 6 A
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfect as data lined filter and for uncoupling of distribution voltage
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeCBF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeCBF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBF"&gt;http://katalog.we-online.de/en/pbs/WE-CBF&lt;/a&gt;&lt;p&gt;

Updated on 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="_WB/HS" package="WE-CBF_1812(W=6.3)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7427925">
<attribute name="WE-NUMBER" value="7427925/120Ω(Z@100MHz)"/>
</technology>
<technology name="_74279250">
<attribute name="WE-NUMBER" value="74279250/70Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
<device name="_HC" package="WE-CBF_1812(W=7.3)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742792510">
<attribute name="WE-NUMBER" value="742792510/70Ω(Z@100MHz)"/>
</technology>
<technology name="_742792511">
<attribute name="WE-NUMBER" value="742792511/120Ω(Z@100MHz)"/>
</technology>
<technology name="_742792514">
<attribute name="WE-NUMBER" value="742792514/600Ω(Z@100MHz)"/>
</technology>
<technology name="_742792515">
<attribute name="WE-NUMBER" value="742792515/785Ω(Z@100MHz)"/>
</technology>
<technology name="_74279252">
<attribute name="WE-NUMBER" value="74279252/880Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CBF_HF_0402" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CBF HF SMD EMI Suppression Ferrite Bead (High Frequency)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Available in 3 types 
&lt;br&gt; Modified internal layout increases the effective suppression range 
&lt;br&gt; The impedance at 1 GHz are at least 3 times higher compared to the WE-CBF product family 
&lt;br&gt; Operating temperature: –55 °C to +125 °C 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;/b&gt; Especially for the suppression of signal lines in the high frequency range 
&lt;br&gt; For fast data lines: CPU, highspeed bus systems, HDD 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/WE-TMSB_74269200x_0201.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/WE-TMSB_74269200x_0201.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBF_HF?"&gt;http://katalog.we-online.de/en/pbs/WE-CBF_HF?&lt;/a&gt;&lt;p&gt;

Updated on 2015-04-24&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="_WB/HS" package="WE-CBF_HF_0402(W=1.5)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742841160">
<attribute name="WE-NUMBER" value="742841160/600Ω(Z@100MHz)"/>
</technology>
<technology name="_742841210">
<attribute name="WE-NUMBER" value="742841210/1000Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
<device name="_HC" package="WE-CBF_HF_0402(W=2.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742843122">
<attribute name="WE-NUMBER" value="742843122/220Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CFWI_1310" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-CFWI Coupled Flatwire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Very low RDC
&lt;BR&gt;
&lt;BR&gt; Low inductance drift over temperature
&lt;BR&gt;
&lt;BR&gt; Operating temperature: –40 °C up to +150 °C
&lt;BR&gt;
&lt;BR&gt; Coupled inductor with two identical windings
&lt;BR&gt;
&lt;BR&gt; More variants due to parallel and serie connection
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt; High power switching regulators
&lt;BR&gt;
&lt;BR&gt; 1:1 flyback converter
&lt;BR&gt;
&lt;BR&gt; Buck, Boost, Sepic and Cuk Converter
&lt;BR&gt;
&lt;BR&gt; Switching regulators with secondary unregulated output voltage
&lt;BR&gt;
&lt;BR&gt;Battery Cell Charging Balancer
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndCFWI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndCFWI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CFWI?"&gt;http://katalog.we-online.de/en/pbs/WE-CFWI?&lt;/a&gt;&lt;p&gt;

updated by  Dan Xu 2014-07-15&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_2"/>
</gates>
<devices>
<device name="" package="WE-CFWI_1310">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_74485540080">
<attribute name="WE-NUMBER" value="74485540080/0,8uH"/>
</technology>
<technology name="_74485540120">
<attribute name="WE-NUMBER" value="74485540120/1,2uH"/>
</technology>
<technology name="_74485540170">
<attribute name="WE-NUMBER" value="74485540170/1,7uH"/>
</technology>
<technology name="_74485540220">
<attribute name="WE-NUMBER" value="74485540220/2,2uH"/>
</technology>
<technology name="_74485540290">
<attribute name="WE-NUMBER" value="74485540290/2,9uH"/>
</technology>
<technology name="_74485540350">
<attribute name="WE-NUMBER" value="74485540350/3,5uH"/>
</technology>
<technology name="_74485540440">
<attribute name="WE-NUMBER" value="74485540440/4,4uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMBH" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-CMBH Common Mode Power Line Choke (Horizontal)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; horizontal design for compact housings 
&lt;br&gt; 
&lt;br&gt; suppression even at low frequency ranges 
&lt;br&gt; 
&lt;br&gt; broadband screening because of low capacitance winding technique 
&lt;br&gt;
&lt;br&gt; highest possible current with small sizes 
&lt;br&gt;
&lt;br&gt; customer specific designs on request 
&lt;br&gt;
&lt;br&gt; operating temperature: -40°C to +125°C 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power electronics 
&lt;br&gt;
&lt;br&gt;Power line in- and output filter 
&lt;br&gt;
&lt;br&gt;Radio interference suppression in motors 
&lt;br&gt;
&lt;br&gt;suppression for common mode noise 
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndCMBH_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndCMBH_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CMBH?"&gt;http://katalog.we-online.de/en/pbs/WE-CMBH?&lt;/a&gt;&lt;p&gt;

Updated by  Dan Xu 2014-07-15&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="_744834101" package="WE-CMBH_1.5MM">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744834101/2X1mH"/>
</technology>
</technologies>
</device>
<device name="_744834622" package="WE-CMBH_1.5MM">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744834622/2X2,2mH"/>
</technology>
</technologies>
</device>
<device name="_744834433" package="WE-CMBH_1.2MM">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744834433/2x3,3mH"/>
</technology>
</technologies>
</device>
<device name="_744834405" package="WE-CMBH_1.2MM">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744834405/2X5mH"/>
</technology>
</technologies>
</device>
<device name="_744834407" package="WE-CMBH_1.2MM">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744834407/2X7mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMBNC" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CMBNC Common Mode Power Line Choke Nanocrystalline
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Very high permeability nanocrystalline core material 
&lt;br&gt;
&lt;br&gt; Improved isolation through plastic case and winding spacer
&lt;br&gt;
&lt;br&gt;  High and stable inductance values at high temperatures 
&lt;br&gt;
&lt;br&gt; High rated currents 
&lt;br&gt;
&lt;br&gt; Broadband suppression
&lt;br&gt;
&lt;br&gt;  Small size
&lt;br&gt;
&lt;br&gt; Frequency range: 1 kHz-300 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: -40°C to +125°C 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power electronics
&lt;br&gt; 
&lt;br&gt;  Power line in- and output filter
&lt;br&gt;
&lt;br&gt;  Radio interference suppression in motors 
&lt;br&gt;
&lt;br&gt; Suppression for common mode noise 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndCMBNC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndCMBNC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CMBNC/"&gt;http://katalog.we-online.de/en/pbs/WE-CMBNC/&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-23&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="_7448040707" package="WE-CMBNC_L(WITHOUT-PINS)_7448040707">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448040707/7mH"/>
</technology>
</technologies>
</device>
<device name="_7448041104" package="WE-CMBNC_L(WITHOUT-PINS)_7448041104">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448041104/4mH"/>
</technology>
</technologies>
</device>
<device name="_7448041502" package="WE-CMBNC_L(WITHOUT-PINS)_7448041502">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448041502/2mH"/>
</technology>
</technologies>
</device>
<device name="_7448041801" package="WE-CMBNC_L(WITHOUT-PINS)_7448041801">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448041801/1,5mH"/>
</technology>
</technologies>
</device>
<device name="_7448042001" package="WE-CMBNC_L(WITHOUT-PINS)_7448042001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448042001/1mH"/>
</technology>
</technologies>
</device>
<device name="_7448040382" package="WE-CMBNC_L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448040382/82mH"/>
</technology>
</technologies>
</device>
<device name="_7448031002" package="WE-CMBNC_M(WITHOUT-PINS)_7448031002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448031002/2mH"/>
</technology>
</technologies>
</device>
<device name="_7448031501" package="WE-CMBNC_M(WITHOUT-PINS)_7448031501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448031501/1mH"/>
</technology>
</technologies>
</device>
<device name="_7448030333" package="WE-CMBNC_M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448030333/33mH"/>
</technology>
</technologies>
</device>
<device name="_7448050530" package="WE-CMBNC_XL(WITHOUT-PINS)_7448050530">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448050530/30mH"/>
</technology>
</technologies>
</device>
<device name="_7448051012" package="WE-CMBNC_XL(WITHOUT-PINS)_7448051012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448051012/12mH"/>
</technology>
</technologies>
</device>
<device name="_7448051804" package="WE-CMBNC_XL(WITHOUT-PINS)_7448051804">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448051804/4,5mH"/>
</technology>
</technologies>
</device>
<device name="_7448052303" package="WE-CMBNC_XL(WITHOUT-PINS)_7448052303">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448052303/2X3mH"/>
</technology>
</technologies>
</device>
<device name="_7448052502" package="WE-CMBNC_XL(WITHOUT-PINS)_7448052502">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448052502/2,5mH"/>
</technology>
</technologies>
</device>
<device name="_7448053201" package="WE-CMBNC_XL(WITHOUT-PINS)_7448053201">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3"/>
<connect gate="G$1" pin="2" pad="10 11 12"/>
<connect gate="G$1" pin="3" pad="7 8 9"/>
<connect gate="G$1" pin="4" pad="4 5 6"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448053201/0,9mH"/>
</technology>
</technologies>
</device>
<device name="_7448050219" package="WE-CMBNC_XL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448050219/190mH"/>
</technology>
</technologies>
</device>
<device name="_7448010911" package="WE-CMBNC_XS_744801XXXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448010911/11mH"/>
</technology>
</technologies>
</device>
<device name="_7448011008" package="WE-CMBNC_XS_744801XXXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448013501/0,5mH"/>
</technology>
</technologies>
</device>
<device name="_7448011305" package="WE-CMBNC_XS_744801XXXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448011305/5mH"/>
</technology>
</technologies>
</device>
<device name="_7448012002" package="WE-CMBNC_XS_744801XXXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448012002/1,6mH"/>
</technology>
</technologies>
</device>
<device name="_7448012501" package="WE-CMBNC_XS_744801XXXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448012501/1mH"/>
</technology>
</technologies>
</device>
<device name="_7448060620" package="WE-CMBNC_XXL_7448060620">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448060620/20mH"/>
</technology>
</technologies>
</device>
<device name="_7448060814" package="WE-CMBNC_XXL_7448060814">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448060814/14mH"/>
</technology>
</technologies>
</device>
<device name="_7448061309" package="WE-CMBNC_XXL_7448061309">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448061309/9mH"/>
</technology>
</technologies>
</device>
<device name="_7448061507" package="WE-CMBNC_XXL_7448061507">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448061507/7mH"/>
</technology>
</technologies>
</device>
<device name="_7448062105" package="WE-CMBNC_XXL_7448062105">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448062105/5mH"/>
</technology>
</technologies>
</device>
<device name="_7448062603" package="WE-CMBNC_XXL_7448062603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448062603/3mH"/>
</technology>
</technologies>
</device>
<device name="_7448063801" package="WE-CMBNC_XXL_7448063801">
<connects>
<connect gate="G$1" pin="1" pad="1 2 3"/>
<connect gate="G$1" pin="2" pad="10 11 12"/>
<connect gate="G$1" pin="3" pad="7 8 9"/>
<connect gate="G$1" pin="4" pad="4 5 6"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448063801/1,5mH"/>
</technology>
</technologies>
</device>
<device name="_7448040435" package="WE-CMBNC_L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448040435/35mH"/>
</technology>
</technologies>
</device>
<device name="_7448040515" package="WE-CMBNC_L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448040515/15mH"/>
</technology>
</technologies>
</device>
<device name="_7448030417" package="WE-CMBNC_M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448030417/17mH"/>
</technology>
</technologies>
</device>
<device name="_7448030509" package="WE-CMBNC_M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448030509/9mH"/>
</technology>
</technologies>
</device>
<device name="_7448050490" package="WE-CMBNC_XL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448050490/90mH"/>
</technology>
</technologies>
</device>
<device name="_7448013501" package="WE-CMBNC_XS_744801XXXX-A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448013501/0,5mH"/>
</technology>
</technologies>
</device>
<device name="_7448060535" package="WE-CMBNC_XXL_7448060535">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448060535/35mH"/>
</technology>
</technologies>
</device>
<device name="_7448014501" package="WE-CMBNC_XS_744801XXXX-A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448014501/0,4mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMB_HC_S" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CMB HC Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; With this product you can achieve high suppression of asymmetric interferences even at low frequency ranges 
&lt;br&gt;
&lt;br&gt;Broadband screening because of anti capacitance winding technique 
&lt;br&gt;
&lt;br&gt; Very compact design 
&lt;br&gt;
&lt;br&gt; Highest possible current with small sizes
&lt;br&gt;
&lt;br&gt;  Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power electronics 
&lt;br&gt; 
&lt;br&gt; Power line in- and output filter 
&lt;br&gt;
&lt;br&gt; For filtering of devices without a stable ground connection 
&lt;br&gt;
&lt;br&gt; Radio interference suppression in motors 
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndCMBHC_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndCMBHC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CMB_HC"&gt;http://katalog.we-online.de/en/pbs/WE-CMB_HC?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-23&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-CMB_HC_S">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_74482210002">
<attribute name="WE-NUMBER" value="74482210002/0,175mH"/>
</technology>
<technology name="_7448225007">
<attribute name="WE-NUMBER" value="7448225007/0,7mH"/>
</technology>
<technology name="_7448227005">
<attribute name="WE-NUMBER" value="7448227005/0,45mH"/>
</technology>
<technology name="_7448229004">
<attribute name="WE-NUMBER" value="7448229004/0,35mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMB" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CMB Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; With this product you can achieve high suppression of asymmetric interferences even at low frequency ranges
&lt;BR&gt;
&lt;BR&gt; Broadband filtering because of low capacitance winding technique
&lt;BR&gt;
&lt;BR&gt; Very compact design
&lt;BR&gt;
&lt;BR&gt; Highest possible current with small sizes
&lt;BR&gt;
&lt;BR&gt; High interference compression asymmetric interference rates also at low frequence range
&lt;BR&gt;
&lt;BR&gt; Custom designs on request
&lt;BR&gt;
&lt;BR&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power electronics
&lt;BR&gt;
&lt;BR&gt; Power line input and output filter
&lt;BR&gt;
&lt;BR&gt; For filtering of devices without a stable ground connection
&lt;BR&gt;
&lt;BR&gt; Radio interference suppression in motors
&lt;BR&gt;
&lt;BR&gt; Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndCMB_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndCMB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CMB"&gt;http://katalog.we-online.de/en/pbs/WE-CMB?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-30&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="_L_744824101" package="WE-CMB_L">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="9"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744824101/1mH"/>
</technology>
</technologies>
</device>
<device name="_M_744823601" package="WE-CMB_M_744823601">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744823601/1mH"/>
</technology>
</technologies>
</device>
<device name="_S_744822301" package="WE-CMB_S">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744822301/1mH"/>
</technology>
</technologies>
</device>
<device name="_XL_7448251201" package="WE-CMB_XL_7448251201">
<connects>
<connect gate="G$1" pin="1" pad="6"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448251201/1mH"/>
</technology>
</technologies>
</device>
<device name="_XS_744821201" package="WE-CMB_XS">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744821201/1mH"/>
</technology>
</technologies>
</device>
<device name="_XXL_7448261418" package="WE-CMB_XXL_7448261418">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448261418/1,8mH"/>
</technology>
</technologies>
</device>
<device name="_XXL_7448262013" package="WE-CMB_XXL_7448262013">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448262013/1,3mH"/>
</technology>
</technologies>
</device>
<device name="_XXL_7448262510" package="WE-CMB_XXL_7448262510">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448262510/1mH"/>
</technology>
</technologies>
</device>
<device name="_XXL_7448263505" package="WE-CMB_XXL_7448263505">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448263505/0,5mH"/>
</technology>
</technologies>
</device>
<device name="_XL_7448258022" package="WE-CMB_XL_744825XXX">
<connects>
<connect gate="G$1" pin="1" pad="6"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448258022/2,2mH"/>
</technology>
</technologies>
</device>
<device name="_M_744823210" package="WE-CMB_M_744823210/20">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744823210/10mH"/>
</technology>
</technologies>
</device>
<device name="_M_744823305" package="WE-CMB_M_744823305">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744823305/5mH"/>
</technology>
</technologies>
</device>
<device name="_M_744823333" package="WE-CMB_M_744823333">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744823333/3,3mH"/>
</technology>
</technologies>
</device>
<device name="_M_744823422" package="WE-CMB_M_744823422">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744823422/2,2mH"/>
</technology>
</technologies>
</device>
<device name="_L_744824622" package="WE-CMB_L">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="9"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744824622/2,2mH"/>
</technology>
</technologies>
</device>
<device name="_L_744824433" package="WE-CMB_L">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="9"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744824433/3,3mH"/>
</technology>
</technologies>
</device>
<device name="_L_744824310" package="WE-CMB_L">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="9"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744824310/10mH"/>
</technology>
</technologies>
</device>
<device name="_L_744824220" package="WE-CMB_L">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="9"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744824220/20mH"/>
</technology>
</technologies>
</device>
<device name="_M_744823220" package="WE-CMB_M_744823210/20">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744823220/20mH"/>
</technology>
</technologies>
</device>
<device name="_S_744822222" package="WE-CMB_S">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744822222/2,2mH"/>
</technology>
</technologies>
</device>
<device name="_S_744822233" package="WE-CMB_S">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744822233/3,3mH"/>
</technology>
</technologies>
</device>
<device name="_S_744822110" package="WE-CMB_S">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744822110/10mH"/>
</technology>
</technologies>
</device>
<device name="_S_744822120" package="WE-CMB_S">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744822120/20mH"/>
</technology>
</technologies>
</device>
<device name="_XL_7448256033" package="WE-CMB_XL_744825XXX">
<connects>
<connect gate="G$1" pin="1" pad="6"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7448256033/3,3mH"/>
</technology>
</technologies>
</device>
<device name="_XL_744825605" package="WE-CMB_XL_744825XXX">
<connects>
<connect gate="G$1" pin="1" pad="6"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744825605/5mH"/>
</technology>
</technologies>
</device>
<device name="_XL_744825510" package="WE-CMB_XL_744825XXX">
<connects>
<connect gate="G$1" pin="1" pad="6"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744825510/10mH"/>
</technology>
</technologies>
</device>
<device name="_XL_744825320" package="WE-CMB_XL_744825XXX">
<connects>
<connect gate="G$1" pin="1" pad="6"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744825320/20mH"/>
</technology>
</technologies>
</device>
<device name="_XL_744825433" package="WE-CMB_XL_744825XXX">
<connects>
<connect gate="G$1" pin="1" pad="6"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744825433/33mH"/>
</technology>
</technologies>
</device>
<device name="_XS_744821240" package="WE-CMB_XS">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744821240/4mH"/>
</technology>
</technologies>
</device>
<device name="_XS_744821150" package="WE-CMB_XS">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744821150/5mH"/>
</technology>
</technologies>
</device>
<device name="_XS_744821110" package="WE-CMB_XS">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744821110/10mH"/>
</technology>
</technologies>
</device>
<device name="_XS_744821039" package="WE-CMB_XS">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744821039/39mH"/>
</technology>
</technologies>
</device>
<device name="_XS_744821120" package="WE-CMB_XS">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744821120/20mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMB_NIZN_S" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CMB NiZn Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Core material: Nickel-Zinc 
&lt;br&gt;
&lt;br&gt; High suppression rates of asymmetric interference at high and medium frequencies 
&lt;br&gt;
&lt;br&gt; Compact size 
&lt;br&gt;
&lt;br&gt; High interference stability against RF interference and burst signals 
&lt;br&gt;
&lt;br&gt; Noise suppression up to 300 MHz
&lt;br&gt;
&lt;br&gt;  Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power electronics 
&lt;br&gt;
&lt;br&gt; Power line in- and output filter 
&lt;br&gt;
&lt;br&gt; Optimized for burst signals
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndCMB_NiZn_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndCMB_NiZn_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CMB_NiZn"&gt;hthttp://katalog.we-online.de/en/pbs/WE-CMB_NiZn&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-30&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-CMB_NIZN_S">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7448421016">
<attribute name="WE-NUMBER" value="7448421016/16uH"/>
</technology>
<technology name="_744842565">
<attribute name="WE-NUMBER" value="744842565/25uH"/>
</technology>
<technology name="_744842742">
<attribute name="WE-NUMBER" value="744842742/42uH"/>
</technology>
<technology name="_744842932">
<attribute name="WE-NUMBER" value="744842932/32uH"/>
</technology>
<technology name="_744942311">
<attribute name="WE-NUMBER" value="744942311/110uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMS" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-CMS Common Mode SMD Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Impedance up to 200 Ω
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power supply systems
&lt;br&gt;
&lt;br&gt; Symmetric data lines
&lt;br&gt;
&lt;br&gt; Common mode interference
&lt;br&gt;
&lt;br&gt; Power electronics
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeCMS_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/FeCMS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CMS/?"&gt;http://katalog.we-online.de/en/pbs/WE-CMS/?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-30&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="_7427520" package="WE-CMS_7427520">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7427520/30Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
<device name="_7427521" package="WE-CMS_7427521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7427521/52Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CNSW_0603" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CNSW SMD Common Mode Line Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High common mode noise suppression at high frequencies
&lt;br&gt;
&lt;br&gt; Small influence on high speed signals through winding symmetry
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC (Size 0805/1206/1812); –40 ºC to +105 ºC (Size 0603)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; USB 2.0 
&lt;br&gt;
&lt;br&gt; IEEE 1394 (Firewire) 
&lt;br&gt;
&lt;br&gt; LVDS 
&lt;br&gt;
&lt;br&gt; High Speed Data Lines 
&lt;br&gt;
&lt;br&gt;LAN 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndCNSW_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndCNSW_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CNSW"&gt;http://katalog.we-online.de/en/pbs/WE-CNSW&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-30&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-CNSW_0603">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_744230121">
<attribute name="WE-NUMBER" value="744230121/120Ω(Z@100MHz)"/>
</technology>
<technology name="_744230181">
<attribute name="WE-NUMBER" value="744230181/180Ω(Z@100MHz)"/>
</technology>
<technology name="_744230220">
<attribute name="WE-NUMBER" value="744230220/22Ω(Z@100MHz)"/>
</technology>
<technology name="_744230251">
<attribute name="WE-NUMBER" value="744230251/250Ω(Z@100MHz)"/>
</technology>
<technology name="_744230450">
<attribute name="WE-NUMBER" value="744230450/45Ω(Z@100MHz)"/>
</technology>
<technology name="_744230900">
<attribute name="WE-NUMBER" value="744230900/90Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CNSW_HF_0805" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-CNSW HF SMD Common Mode Line Filter (High Frequency)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; urrent compensated data line filter
&lt;br&gt;
&lt;br&gt; High common mode noise suppression at high frequencies
&lt;br&gt;
&lt;br&gt; Suitable for high data rates
&lt;br&gt;
&lt;br&gt; Small influence on high speed signals through winding symmetry
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; USB 3.0 
&lt;br&gt;
&lt;br&gt;USB 2.0 
&lt;br&gt; 
&lt;br&gt; HDMI 
&lt;br&gt;
&lt;br&gt; LVDS
&lt;br&gt;
&lt;br&gt; High-Speed data lines 
&lt;br&gt;
&lt;br&gt; IEEE 1394 (Firewire)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndCNSWHF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndCNSWHF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CNSW_HF"&gt;http://katalog.we-online.de/en/pbs/WE-CNSW_HF&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;Created by Dan Xu 2014-6-10&lt;Br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-CNSW_0805">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_744233121">
<attribute name="WE-NUMBER" value="744233121/120Ω(Z@100MHz)"/>
</technology>
<technology name="_744233670">
<attribute name="WE-NUMBER" value="744233670/67Ω(Z@100MHz)"/>
</technology>
<technology name="_744233900">
<attribute name="WE-NUMBER" value="744233900/90Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CST_EE5" prefix="T" uservalue="yes">
<description>&lt;b&gt; WE-CST Current Sense Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Height 5.33 mm max.
&lt;br&gt;
&lt;br&gt; Frequency 50 kHz to 1 MHz 
&lt;br&gt;
&lt;br&gt; Primary current rating up to 10 A 
&lt;br&gt;
&lt;br&gt; Operating temperature: –15 °C to +105 °C 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; AC current detection 
&lt;br&gt;
&lt;br&gt;Switch mode power supply 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtCST_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtCST_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CST"&gt;http://katalog.we-online.de/en/pbs/WE-CST&lt;/a&gt;&lt;p&gt;


&lt;BR&gt;Updated by  Dan Xu 2014-06-10&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="" package="WE-CST">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="7"/>
</connects>
<technologies>
<technology name="_749251020">
<attribute name="WE-NUMBER" value="749251020/80uH"/>
</technology>
<technology name="_749251030">
<attribute name="WE-NUMBER" value="749251030/180uH"/>
</technology>
<technology name="_749251040">
<attribute name="WE-NUMBER" value="749251040/320uH"/>
</technology>
<technology name="_749251050">
<attribute name="WE-NUMBER" value="749251050/500uH"/>
</technology>
<technology name="_749251060">
<attribute name="WE-NUMBER" value="749251060/720uH"/>
</technology>
<technology name="_749251070">
<attribute name="WE-NUMBER" value="749251070/980uH"/>
</technology>
<technology name="_749251100">
<attribute name="WE-NUMBER" value="749251100/2000uH"/>
</technology>
<technology name="_749251125">
<attribute name="WE-NUMBER" value="749251125/3000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DCT_SH" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-DCT Toroidal Double Power Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Very low RDC 
&lt;br&gt;
&lt;br&gt; Very low core losses 
&lt;br&gt;
&lt;br&gt;Saturation current higher up to 120 A 
&lt;br&gt;
&lt;br&gt; Low inductance drift over temperature 
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C up to +125 °C 
&lt;br&gt; 
&lt;br&gt; Coupled inductor with two identical windings 
&lt;br&gt;
&lt;br&gt; More variants due to parallel and series connection 
&lt;br&gt;
&lt;br&gt; Low leakage due to bifilar winding 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; high power switching regulators 
&lt;br&gt;
&lt;br&gt; Solar inverter 
&lt;br&gt;
&lt;br&gt; 1:1 flyback converter 
&lt;br&gt; 
&lt;br&gt; Buck, Boost, Sepic and CUK Converter 
&lt;br&gt; 
&lt;br&gt; Switching regulators with secondary unregulated output voltage 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndDCT_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndDCT_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-DCT"&gt;http://katalog.we-online.de/en/pbs/WE-DCT&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by  Dan Xu 2014-06-10&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-DCT">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7448510091">
<attribute name="WE-NUMBER" value="7448510091/0,091uH"/>
</technology>
<technology name="_744851016">
<attribute name="WE-NUMBER" value="744851016/0,16uH"/>
</technology>
<technology name="_744851027">
<attribute name="WE-NUMBER" value="744851027/0,27uH"/>
</technology>
<technology name="_744851039">
<attribute name="WE-NUMBER" value="744851039/0,39uH"/>
</technology>
<technology name="_744851056">
<attribute name="WE-NUMBER" value="744851056/0,56uH"/>
</technology>
<technology name="_744851100">
<attribute name="WE-NUMBER" value="744851100/1uH"/>
</technology>
<technology name="_744851101">
<attribute name="WE-NUMBER" value="744851101/10uH"/>
</technology>
<technology name="_744851102">
<attribute name="WE-NUMBER" value="744851102/100uH"/>
</technology>
<technology name="_744851220">
<attribute name="WE-NUMBER" value="744851220/2,2uH"/>
</technology>
<technology name="_744851221">
<attribute name="WE-NUMBER" value="744851221/22uH"/>
</technology>
<technology name="_744851330">
<attribute name="WE-NUMBER" value="744851330/3,3uH"/>
</technology>
<technology name="_744851331">
<attribute name="WE-NUMBER" value="744851331/33uH"/>
</technology>
<technology name="_744851470">
<attribute name="WE-NUMBER" value="744851470/4,7uH"/>
</technology>
<technology name="_744851471">
<attribute name="WE-NUMBER" value="744851471/47uH"/>
</technology>
<technology name="_744851561">
<attribute name="WE-NUMBER" value="744851561/56uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DD_7345" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-DD SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; 1:1 transformer 
&lt;br&gt;
&lt;br&gt; Double inductor with two identical windings 
&lt;br&gt;
&lt;br&gt; 4 different sizes available 
&lt;br&gt; 
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Recommended solder profile: Reflow 
&lt;br&gt; 
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; For SEPIC and CUK topologies 
&lt;br&gt;
&lt;br&gt; Flyback applications 
&lt;br&gt;
&lt;br&gt; Switching regulators with second, unregulated output voltages 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndDD_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndDD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-DD"&gt;http://katalog.we-online.de/en/pbs/WE-DD&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by  Dan Xu 2014-06-10&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-DD_7345">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744877001">
<attribute name="WE-NUMBER" value="744877001/1,8uH"/>
</technology>
<technology name="_744877002">
<attribute name="WE-NUMBER" value="744877002/2,4uH"/>
</technology>
<technology name="_744877003">
<attribute name="WE-NUMBER" value="744877003/3,3uH"/>
</technology>
<technology name="_744877004">
<attribute name="WE-NUMBER" value="744877004/4,7uH"/>
</technology>
<technology name="_744877005">
<attribute name="WE-NUMBER" value="744877005/5,6uH"/>
</technology>
<technology name="_744877006">
<attribute name="WE-NUMBER" value="744877006/6,8uH"/>
</technology>
<technology name="_744877008">
<attribute name="WE-NUMBER" value="744877008/8,2uH"/>
</technology>
<technology name="_744877100">
<attribute name="WE-NUMBER" value="744877100/10uH"/>
</technology>
<technology name="_744877101">
<attribute name="WE-NUMBER" value="744877101/100uH"/>
</technology>
<technology name="_744877220">
<attribute name="WE-NUMBER" value="744877220/22uH"/>
</technology>
<technology name="_744877330">
<attribute name="WE-NUMBER" value="744877330/33uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-EHPI_5838" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-EHPI Energy Harvesting Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low profile: 4 mm
&lt;br&gt; Small footprint 6 x 6 mm
&lt;br&gt; Very low secondary RDC
&lt;br&gt; Different turn ratios available
&lt;br&gt; Separated welding/soldering pad for a high reliable component
&lt;br&gt; Optimized, high reliable winding style
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Wireless fire, alarm, gas and metering remote sensors driven by environmental energies based on energy harvesting voltage transformers like LTC3108/LTC3109
&lt;br&gt; Sensors with predictive battery replacements in applications which are difficult to access
&lt;br&gt; Energy self-sufficient supply using subsequent installed sensors for energy harvesting
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndEHP_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndEHP_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-EHPI?"&gt;http://katalog.we-online.de/en/pbs/WE-EHPI?&lt;/a&gt;&lt;p&gt;


Updated on 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-EHPI">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_74488540070">
<attribute name="WE-NUMBER" value="74488540070/7uH/70000uH"/>
</technology>
<technology name="_74488540120">
<attribute name="WE-NUMBER" value="74488540120/13uH/33000uH"/>
</technology>
<technology name="_74488540250">
<attribute name="WE-NUMBER" value="74488540250/25uH/10000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FAMI" prefix="L" uservalue="yes">
<description>&lt;B&gt;WE-FAMI THT Power Inductor&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Optimization of material composition causes high performance &lt;br&gt;
Up to 19.7 A Saturation Current &lt;br&gt;
RDC values starting at 3.8 mΩ&lt;br&gt;
Shielded design &lt;br&gt;
Low stray field &lt;br&gt;
&lt;br&gt;

&lt;b&gt;Application&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
DC/DC converters&lt;br&gt;
 Power supplies and battery chargers&lt;br&gt; 
Home Entertainment Systems &lt;br&gt;
Portable devices like notebooks&lt;br&gt;


&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndFAMI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndFAMI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FAMI"&gt;http://katalog.we-online.de/en/pbs/WE-FAMI&lt;/a&gt;&lt;p&gt;

Updated on 2015-05-21&lt;br&gt;
2015(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_744750230150" package="WE-FAMI_8010_744750230150">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750230150/15uH"/>
</technology>
</technologies>
</device>
<device name="_744750340047" package="WE-FAMI_1012_744750340047">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750340047/4,7uH"/>
</technology>
</technologies>
</device>
<device name="_744750340150" package="WE-FAMI_1012_744750340150">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750340150uH"/>
</technology>
</technologies>
</device>
<device name="_744750460100" package="WE-FAMI_1215_744750460100">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750460100/10uH"/>
</technology>
</technologies>
</device>
<device name="_744750460220" package="WE-FAMI_1215_744750460220">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750460220/22uH"/>
</technology>
</technologies>
</device>
<device name="_744750420047" package="WE-FAMI_1280_744750420047">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750420047/4,7uH"/>
</technology>
</technologies>
</device>
<device name="_744750420068" package="WE-FAMI_1280_744750420068">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750420068/6,8uH"/>
</technology>
</technologies>
</device>
<device name="_744750420100" package="WE-FAMI_1280_744750420100">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750420100/10uH"/>
</technology>
</technologies>
</device>
<device name="_744750420150" package="WE-FAMI_1280_744750420150">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750420150/15uH"/>
</technology>
</technologies>
</device>
<device name="_744750420220" package="WE-FAMI_1280_744750420220">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750420220/22uH"/>
</technology>
</technologies>
</device>
<device name="_744750530047" package="WE-FAMI_1410_744750530047">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750530047/4,7uH"/>
</technology>
</technologies>
</device>
<device name="_744750530068" package="WE-FAMI_1410_744750530068">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750530068/6,8uH"/>
</technology>
</technologies>
</device>
<device name="_744750530100" package="WE-FAMI_1410_744750530100">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750530100/10uH"/>
</technology>
</technologies>
</device>
<device name="_744750560047" package="WE-FAMI_1415_744750560047">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750560047/4,7uH"/>
</technology>
</technologies>
</device>
<device name="_744750560100" package="WE-FAMI_1415_744750560100">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750560100/10uH"/>
</technology>
</technologies>
</device>
<device name="_744750560220" package="WE-FAMI_1415_744750560220">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750560220/22uH"/>
</technology>
</technologies>
</device>
<device name="_744750230030" package="WE-FAMI_8010_744750230030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750230030/3uH"/>
</technology>
</technologies>
</device>
<device name="_744750230047" package="WE-FAMI_8010_744750230047">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750230047/4,7uH"/>
</technology>
</technologies>
</device>
<device name="_744750230068" package="WE-FAMI_8010_744750230068">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750230068/6,8uH"/>
</technology>
</technologies>
</device>
<device name="_744750230100" package="WE-FAMI_8010_744750230100">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750230100/10uH"/>
</technology>
</technologies>
</device>
<device name="_744750460150" package="WE-FAMI_1215_744750460150">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744750460150/15uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP5" prefix="T" uservalue="yes">
<description>&lt;b&gt; WE-FB Flyback Transformer suitable for LT3573/ LT3574/ LT3575/ LT3748
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; easy design in solution 
&lt;br&gt;
&lt;br&gt; less external components needed 
&lt;br&gt;
&lt;br&gt; small board space 
&lt;br&gt; 
&lt;br&gt; low cost 
&lt;br&gt;
&lt;br&gt; no optocoupler needed! 
&lt;br&gt;
&lt;br&gt; long term reliability voltage control 
&lt;br&gt;
&lt;br&gt; no aging 
&lt;br&gt;
&lt;br&gt; same external parts for different output voltages 
&lt;br&gt;
&lt;br&gt; easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop 
&lt;br&gt;
&lt;br&gt; Isolation voltage up to 2.5 kV 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Isolated power design 
&lt;br&gt;
&lt;br&gt; Sensor interfaces 
&lt;br&gt;
&lt;br&gt; Isolated telecom converters 
&lt;br&gt;
&lt;br&gt; Power over Ethernet 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="_750311691" package="WE_EP5_SMD_6PIN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EE35/18/10" prefix="T" uservalue="yes">
<description>&lt;b&gt; WE-FB 3751 Flyback Transformer for LT3751
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Isolation voltage: 1 kVAC 
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC (incl. self-heating) 
&lt;br&gt;
&lt;br&gt; Especially designed for LT3751 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Transformer for capacitor charger or high voltage outputs 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_1W:2W_1"/>
</gates>
<devices>
<device name="" package="WE_EE35/18/10_THT_HORIZONTAL_14PIN">
<connects>
<connect gate="G$1" pin="1" pad="4 5 6 7"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="13"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="8 9 10 11"/>
</connects>
<technologies>
<technology name="_750310349"/>
<technology name="_750310355"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EFD20_750032051" prefix="T" uservalue="yes">
<description>&lt;b&gt; WE-FB 3751 Flyback Transformer for LT3751
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Isolation voltage: 1 kVAC 
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC (incl. self-heating) 
&lt;br&gt;
&lt;br&gt; Especially designed for LT3751 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Transformer for capacitor charger or high voltage outputs 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;



Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-FB_EFD20_10PIN">
<connects>
<connect gate="G$1" pin="1" pad="7" route="any"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="6" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FC_ET20V" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-FC Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Closed rectangular ferrite core
&lt;BR&gt;
&lt;BR&gt; 2-section winding for excellent high frequency performance
&lt;BR&gt;
&lt;BR&gt; 1% stray inductance for symmetrical interference suppression
&lt;BR&gt;
&lt;BR&gt; Operating temperature: –25 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt; 
&lt;br&gt;&lt;/b&gt; Switch mode power supplies
&lt;BR&gt;
&lt;BR&gt; Electronic ballasts for lamps
&lt;BR&gt;
&lt;BR&gt; Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndFC_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndFC_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FC?"&gt;http://katalog.we-online.de/en/pbs/WE-FC?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-FC_ET">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7448640395">
<attribute name="WE-NUMBER" value="7448640395/0,82mH"/>
</technology>
<technology name="_7448640396">
<attribute name="WE-NUMBER" value="7448640396/1,8mH"/>
</technology>
<technology name="_7448640397">
<attribute name="WE-NUMBER" value="7448640397/2,7mH"/>
</technology>
<technology name="_7448640398">
<attribute name="WE-NUMBER" value="7448640398/3,3mH"/>
</technology>
<technology name="_7448640399">
<attribute name="WE-NUMBER" value="7448640399/3,9mH"/>
</technology>
<technology name="_7448640400">
<attribute name="WE-NUMBER" value="7448640400/5,6mH"/>
</technology>
<technology name="_7448640401">
<attribute name="WE-NUMBER" value="7448640401/6,8mH"/>
</technology>
<technology name="_7448640402">
<attribute name="WE-NUMBER" value="7448640402/10mH"/>
</technology>
<technology name="_7448640403">
<attribute name="WE-NUMBER" value="7448640403/18mH"/>
</technology>
<technology name="_7448640404">
<attribute name="WE-NUMBER" value="7448640404/22mH"/>
</technology>
<technology name="_7448640405">
<attribute name="WE-NUMBER" value="7448640405/33mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEX_EFD15" prefix="T" uservalue="yes">
<description>&lt;b&gt; WE-FLEX Flexible Transformer for DC/DC Converter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Transformer with 6 identical windings
&lt;BR&gt;
&lt;BR&gt; 4 sizes with 5 different lengths of air gap each
&lt;BR&gt;
&lt;BR&gt; Insulation test voltage 500 VAC
&lt;BR&gt;
&lt;BR&gt; Low leakage inductance
&lt;BR&gt;
&lt;BR&gt; Operating temperature: –40 ºC to +125 ºC
&lt;BR&gt;
&lt;BR&gt; By using different circuits more than 375 transformer solutions and about 125 choke solutions possible. Consequently, quick prototyping possibilities
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; All kind of switching regulators
&lt;br&gt;
&lt;br&gt;-Flyback converters
&lt;br&gt;-Forward converters
&lt;br&gt;-Push-pull converters
&lt;br&gt;-Step-up/step-down converters
&lt;br&gt;-SEPIC converter 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFlex_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtFlex_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FLEX?"&gt;http://katalog.we-online.de/en/pbs/WE-FLEX?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:3W_3"/>
</gates>
<devices>
<device name="" package="WE-FLEX_EFD15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="11"/>
<connect gate="G$1" pin="11" pad="2"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="9"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="10"/>
<connect gate="G$1" pin="9" pad="3"/>
</connects>
<technologies>
<technology name="_749196301"/>
<technology name="_749196311"/>
<technology name="_749196321"/>
<technology name="_749196331"/>
<technology name="_749196341"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEX+_ETD29" prefix="T" uservalue="yes">
<description>&lt;b&gt; WE-FLEX+ Flexible Transformer for DC/DC Converter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Transformer with 6 identical windings 
&lt;br&gt;
&lt;br&gt; Power up to 300 W possible 
&lt;br&gt;
&lt;br&gt; Isolation voltage 500 VDC 
&lt;br&gt;
&lt;br&gt; Low leakage inductance 
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; All kind of switching regulators
&lt;br&gt; -Flyback converters
&lt;br&gt; -Forward converters
&lt;br&gt; -Push-pull converters
&lt;br&gt; -Step-up/step-down converters
&lt;br&gt; -SEPIC converter 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; 
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFlex_Plus_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtFlex_Plus_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FLEX_Plus?"&gt;http://katalog.we-online.de/en/pbs/WE-FLEX_Plus?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:3W_3"/>
</gates>
<devices>
<device name="" package="WE_FLEX+_ETD29">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="5"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="14"/>
<connect gate="G$1" pin="6" pad="2"/>
<connect gate="G$1" pin="7" pad="13"/>
<connect gate="G$1" pin="8" pad="9"/>
<connect gate="G$1" pin="9" pad="6"/>
</connects>
<technologies>
<technology name="_749197101"/>
<technology name="_749197111"/>
<technology name="_749197121"/>
<technology name="_749197131"/>
<technology name="_749197141"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-GDTI_EP7" prefix="L" uservalue="yes">
<description>&lt;B&gt;SMD Gate Drive Transformer&lt;/b&gt;&lt;br&gt;
-1 or 2 secondary windings&lt;br&gt;
-6 turrns ration&lt;br&gt;
-2500 Vac testing voltage&lt;br&gt;
-Operating voltage up tp 250V&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
--Gate Drive&lt;br&gt;
--Signal&lt;br&gt;
--Power&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtGDTI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtGDTI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-GDTI?"&gt;http://katalog.we-online.de/en/pbs/WE-GDTI?&lt;/a&gt;&lt;p&gt;


Created by  Dan Xu 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-GDTI_EP7">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="7"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="3"/>
</connects>
<technologies>
<technology name="_760301301"/>
<technology name="_760301303"/>
<technology name="_760301304"/>
<technology name="_760301305"/>
<technology name="_760301306"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-GDTI_EP7_760301302" prefix="L" uservalue="yes">
<description>&lt;B&gt;SMD Gate Drive Transformer&lt;/b&gt;&lt;br&gt;
-1 or 2 secondary windings&lt;br&gt;
-6 turrns ration&lt;br&gt;
-2500 Vac testing voltage&lt;br&gt;
-Operating voltage up tp 250V&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
--Gate Drive&lt;br&gt;
--Signal&lt;br&gt;
--Power&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtGDTI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtGDTI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-GDTI/760301302"&gt;http://katalog.we-online.de/en/pbs/WE-GDTI/760301302&lt;/a&gt;&lt;p&gt;

Created by  Dan Xu 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="" package="WE-GDTI_EP7">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-GDT_1SW" prefix="T" uservalue="yes">
<description>&lt;b&gt;SMD Gate Drive Transformer WE-GDT&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics&lt;br&gt;&lt;/b&gt;
- small form factor EP5&lt;br&gt;
- 1 or 2 secondary windings&lt;br&gt;
- 4 different turn rations&lt;br&gt;
- 1500VDC insulation test voltage&lt;br&gt;
- operating voltage up to 80V&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt;
-- Gate Drive&lt;br&gt;
-- Signal&lt;br&gt;
-- Power&lt;br&gt;
-- Synchronous Flyback


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-GDT.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-GDT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-GDT?"&gt;http://katalog.we-online.de/en/pbs/WE-GDT?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="_760301106" package="WE-EP5_6PIN_2">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760301107" package="WE-EP5_6PIN_2">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760301108" package="WE-EP5_6PIN_2">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-GDT_2SW" prefix="T" uservalue="yes">
<description>&lt;b&gt;SMD Gate Drive Transformer WE-GDT&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;&lt;br&gt;
- small form factor EP5&lt;br&gt;
- 1 or 2 secondary windings&lt;br&gt;
- 4 different turn rations&lt;br&gt;
- 1500VDC insulation test voltage&lt;br&gt;
- operating voltage up to 80V&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
-- Gate Drive&lt;br&gt;
-- Signal&lt;br&gt;
-- Power&lt;br&gt;
-- Synchronous Flyback

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-GDT.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-GDT.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-GDT?"&gt;http://katalog.we-online.de/en/pbs/WE-GDT?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_1W:2W"/>
</gates>
<devices>
<device name="_760301105" package="WE-EP5_6PIN_2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760301104" package="WE-EP5_6PIN_2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760301103" package="WE-EP5_6PIN_2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-GF_1812(L)" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Wire wound on ferrite
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +105 °C
&lt;br&gt;
&lt;br&gt; High resistance against dampness
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF circuits like tuner, transponder etc.
&lt;br&gt;
&lt;br&gt; RF amplifier circuits like antennas amplifier
&lt;br&gt;
&lt;br&gt; Oscillator
&lt;br&gt;
&lt;br&gt; Filter circuits
&lt;br&gt;
&lt;br&gt; Amplification circuits

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-GF_SMD-HF.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-GF_SMD-HF.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-GF?"&gt;http://katalog.we-online.de/en/pbs/WE-GF?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-GF_1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744766001">
<attribute name="WE-NUMBER" value="744766001/0,1uH"/>
</technology>
<technology name="_7447660033">
<attribute name="WE-NUMBER" value="7447660033/0,33uH"/>
</technology>
<technology name="_7447660039">
<attribute name="WE-NUMBER" value="7447660039/0,39uH"/>
</technology>
<technology name="_7447660068">
<attribute name="WE-NUMBER" value="7447660068//0,68uH"/>
</technology>
<technology name="_7447660082">
<attribute name="WE-NUMBER" value="7447660082/0,82uH"/>
</technology>
<technology name="_74476601">
<attribute name="WE-NUMBER" value="74476601/1uH"/>
</technology>
<technology name="_744766012">
<attribute name="WE-NUMBER" value="744766012/1,2uH"/>
</technology>
<technology name="_744766015">
<attribute name="WE-NUMBER" value="744764015/1,5uH"/>
</technology>
<technology name="_744766018">
<attribute name="WE-NUMBER" value="744766018/1,8uH"/>
</technology>
<technology name="_74476602">
<attribute name="WE-NUMBER" value="74476602/2,2uH"/>
</technology>
<technology name="_74476603">
<attribute name="WE-NUMBER" value="74476603/3,3uH"/>
</technology>
<technology name="_744766039">
<attribute name="WE-NUMBER" value="744766039/3,9uH"/>
</technology>
<technology name="_74476604">
<attribute name="WE-NUMBER" value="74476604/4,7uH"/>
</technology>
<technology name="_744766056">
<attribute name="WE-NUMBER" value="744766056/5,6uH"/>
</technology>
<technology name="_74476606">
<attribute name="WE-NUMBER" value="74476606/6,8uH"/>
</technology>
<technology name="_744766082">
<attribute name="WE-NUMBER" value="744766082/8,2uH"/>
</technology>
<technology name="_74476610">
<attribute name="WE-NUMBER" value="74476610/10uH"/>
</technology>
<technology name="_744766115">
<attribute name="WE-NUMBER" value="744766115/15uH"/>
</technology>
<technology name="_744766118">
<attribute name="WE-NUMBER" value="744766118/18uH"/>
</technology>
<technology name="_744766122">
<attribute name="WE-NUMBER" value="744766122/22uH"/>
</technology>
<technology name="_744766133">
<attribute name="WE-NUMBER" value="744766133/33uH"/>
</technology>
<technology name="_744766147">
<attribute name="WE-NUMBER" value="744766147/47uH"/>
</technology>
<technology name="_744766156">
<attribute name="WE-NUMBER" value="744766156/56uH"/>
</technology>
<technology name="_744766168">
<attribute name="WE-NUMBER" value="744766168/68uH"/>
</technology>
<technology name="_74476620">
<attribute name="WE-NUMBER" value="74476620/100uH"/>
</technology>
<technology name="_744766215">
<attribute name="WE-NUMBER" value="744766215/150uH"/>
</technology>
<technology name="_744766218">
<attribute name="WE-NUMBER" value="744766218/180uH"/>
</technology>
<technology name="_744766220">
<attribute name="WE-NUMBER" value="744766220/220uH"/>
</technology>
<technology name="_744766233">
<attribute name="WE-NUMBER" value="744766233/330uH"/>
</technology>
<technology name="_744766239">
<attribute name="WE-NUMBER" value="744766239/390uH"/>
</technology>
<technology name="_74476624">
<attribute name="WE-NUMBER" value="74476624/470uH"/>
</technology>
<technology name="_74476625">
<attribute name="WE-NUMBER" value="74476625/560uH"/>
</technology>
<technology name="_74476626">
<attribute name="WE-NUMBER" value="74476626/680uH"/>
</technology>
<technology name="_74476628">
<attribute name="WE-NUMBER" value="74476628/820uH"/>
</technology>
<technology name="_74476630">
<attribute name="WE-NUMBER" value="74476630/1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-GFH_4532" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD RF Choke WE-GFH&lt;/b&gt;&lt;p&gt;

- Wire wound ferrite&lt;br&gt;
- For higher currents&lt;p&gt;

-- HF-circuits like tuner, transponder etc.
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-GFH.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-GFH.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-GFH"&gt;http://katalog.we-online.de/en/pbs/WE-GFH&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-GFH_4532">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744766901">
<attribute name="WE-NUMBER" value="744766901/1uH"/>
</technology>
<technology name="_7447669012">
<attribute name="WE-NUMBER" value="7447669012/1,2uH"/>
</technology>
<technology name="_744766902">
<attribute name="WE-NUMBER" value="744766902/2uH"/>
</technology>
<technology name="_744766903">
<attribute name="WE-NUMBER" value="744766903/3uH"/>
</technology>
<technology name="_7447669039">
<attribute name="WE-NUMBER" value="7447669039/3,9uH"/>
</technology>
<technology name="_744766904">
<attribute name="WE-NUMBER" value="744766904/4uH"/>
</technology>
<technology name="_744766906">
<attribute name="WE-NUMBER" value="744766906/6,8uH"/>
</technology>
<technology name="_744766910">
<attribute name="WE-NUMBER" value="744766910/10uH"/>
</technology>
<technology name="_7447669112">
<attribute name="WE-NUMBER" value="7447669112/12uH"/>
</technology>
<technology name="_7447669115">
<attribute name="WE-NUMBER" value="7447669115/15uH"/>
</technology>
<technology name="_7447669118">
<attribute name="WE-NUMBER" value="7447669118/18uH"/>
</technology>
<technology name="_7447669122">
<attribute name="WE-NUMBER" value="7447669122/22uH"/>
</technology>
<technology name="_7447669127">
<attribute name="WE-NUMBER" value="7447669127/27uH"/>
</technology>
<technology name="_7447669133">
<attribute name="WE-NUMBER" value="7447669133/33uH"/>
</technology>
<technology name="_7447669139">
<attribute name="WE-NUMBER" value="7447669139/39uH"/>
</technology>
<technology name="_7447669147">
<attribute name="WE-NUMBER" value="7447669147/47uH"/>
</technology>
<technology name="_7447669156">
<attribute name="WE-NUMBER" value="7447669156/56uH"/>
</technology>
<technology name="_7447669168">
<attribute name="WE-NUMBER" value="7447669168/68uH"/>
</technology>
<technology name="_7447669182">
<attribute name="WE-NUMBER" value="7447669182/82uH"/>
</technology>
<technology name="_744766920">
<attribute name="WE-NUMBER" value="744766920/100uH"/>
</technology>
<technology name="_7447669212">
<attribute name="WE-NUMBER" value="7447669212/120uH"/>
</technology>
<technology name="_7447669218">
<attribute name="WE-NUMBER" value="7447669218/180uH"/>
</technology>
<technology name="_7447669220">
<attribute name="WE-NUMBER" value="7447669220/220uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCC_8070" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Cube Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Current capability up to 27 A
&lt;br&gt;
&lt;br&gt; Excellent saturation characteristics
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter choke for DC/DC converter
&lt;br&gt;
&lt;br&gt; Single and polyphase buck converter
&lt;br&gt;
&lt;br&gt; Filter choke for motor electronics
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCC.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCC?"&gt;http://katalog.we-online.de/en/pbs/WE-HCC?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCC_8070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443340030">
<attribute name="WE-NUMBER" value="7443340030/0,3uH"/>
</technology>
<technology name="_7443340047">
<attribute name="WE-NUMBER" value="7443340047/0,47uH"/>
</technology>
<technology name="_7443340068">
<attribute name="WE-NUMBER" value="7443340068/0,68uH"/>
</technology>
<technology name="_7443340100">
<attribute name="WE-NUMBER" value="7443440100/1uH"/>
</technology>
<technology name="_7443340150">
<attribute name="WE-NUMBER" value="7443340150/1,5uH"/>
</technology>
<technology name="_7443340220">
<attribute name="WE-NUMBER" value="7443340220/2,2uH"/>
</technology>
<technology name="_7443340330">
<attribute name="WE-NUMBER" value="7443340330/3,3uH"/>
</technology>
<technology name="_7443340470">
<attribute name="WE-NUMBER" value="7443340470/4,7uH"/>
</technology>
<technology name="_7443340680">
<attribute name="WE-NUMBER" value="7443340680/6,8uH"/>
</technology>
<technology name="_7443341000">
<attribute name="WE-NUMBER" value="7443341000/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCF_2818" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Saturation current up to 75 A
&lt;br&gt;
&lt;br&gt; Very low core losses (MnZn)
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Current capability up to 32 A
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Storage inductor for high efficiency DC/DC converters
&lt;br&gt;
&lt;br&gt; Single and polyphase buck converters
&lt;br&gt;
&lt;br&gt; Filter for audio applications
&lt;br&gt;
&lt;br&gt; Optimized for high current boost applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-hcf_smd_hochstrominduktivitaet_11.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-hcf_smd_hochstrominduktivitaet_11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCF#vs_ct:1"&gt;http://katalog.we-online.de/en/pbs/WE-HCF#vs_ct:1&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCF_2818">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443640330">
<attribute name="WE-NUMBER" value="7443640330/3,3uH"/>
</technology>
<technology name="_7443640470">
<attribute name="WE-NUMBER" value="7443640470/4,7uH"/>
</technology>
<technology name="_7443640680">
<attribute name="WE-NUMBER" value="7443640680/6,8uH"/>
</technology>
<technology name="_7443641000">
<attribute name="WE-NUMBER" value="7443641000/10uH"/>
</technology>
<technology name="_7443641500">
<attribute name="WE-NUMBER" value="7443641500/15uH"/>
</technology>
<technology name="_7443642200">
<attribute name="WE-NUMBER" value="7443642200/22uH"/>
</technology>
<technology name="_7443643300">
<attribute name="WE-NUMBER" value="7443643300/33uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_7050" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Flat wire coil for low losses at high frequency
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +150/155 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; Industrial computers
&lt;br&gt;
&lt;br&gt; Motherboards
&lt;br&gt;
&lt;br&gt; High current switching regulators
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Polyphase-switching regulators
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCI?"&gt;http://katalog.we-online.de/en/pbs/WE-HCI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_7030/7040/7050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744314024">
<attribute name="WE-NUMBER" value="744314024/0,24uH"/>
</technology>
<technology name="_744314047">
<attribute name="WE-NUMBER" value="744314047/0,47uH"/>
</technology>
<technology name="_744314076">
<attribute name="WE-NUMBER" value="744314076/0,76uH"/>
</technology>
<technology name="_744314101">
<attribute name="WE-NUMBER" value="744314101/10uH"/>
</technology>
<technology name="_744314110">
<attribute name="WE-NUMBER" value="744314110/1,1uH"/>
</technology>
<technology name="_744314150">
<attribute name="WE-NUMBER" value="744314150/1,5uH"/>
</technology>
<technology name="_744314200">
<attribute name="WE-NUMBER" value="744314200/2uH"/>
</technology>
<technology name="_744314330">
<attribute name="WE-NUMBER" value="744314330/3,3uH"/>
</technology>
<technology name="_744314490">
<attribute name="WE-NUMBER" value="744314490/4,9uH"/>
</technology>
<technology name="_744314650">
<attribute name="WE-NUMBER" value="744314650/6,5uH"/>
</technology>
<technology name="_744314760">
<attribute name="WE-NUMBER" value="744314760/7,6uH"/>
</technology>
<technology name="_744314850">
<attribute name="WE-NUMBER" value="744314850/8,5uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_7070" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;
&lt;br&gt; High saturation current up to 81 A
&lt;br&gt;
&lt;br&gt; Extremly low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; RDC tolerance ± 7%
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;
&lt;br&gt; CPU/RAM power supply
&lt;br&gt;
&lt;br&gt; Power PC
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCM?"&gt;http://katalog.we-online.de/en/pbs/WE-HCM?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCM_7070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744307012">
<attribute name="WE-NUMBER" value="744307012/120nH"/>
</technology>
<technology name="_744307016">
<attribute name="WE-NUMBER" value="744307016/160nH"/>
</technology>
<technology name="_744307022">
<attribute name="WE-NUMBER" value="744307022/220nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-ISDN" prefix="T" uservalue="yes">
<description>&lt;b&gt;SMD T1/E1 Pri Transformer WE-ISDN&lt;/b&gt;&lt;p&gt;

- Small surface mount package&lt;br&gt;
- Separate transit and receive devices for layout flexibility&lt;br&gt;
- Low cross talk: excellent layout density&lt;br&gt;
- Meets ITU G. 703 ISDN-Primary rate recommendations&lt;br&gt;
- 1500 VAC dielectric strength&lt;br&gt;
- 100 Ohm line&lt;br&gt;&lt;br&gt;

-- ISDN&lt;br&gt;
-- Matched to IC manufacturers transceivers


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_MID-ISDN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_MID-ISDN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-ISDN?"&gt;http://katalog.we-online.de/en/ctm/MID-ISDN?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="T_3L_2/1"/>
</gates>
<devices>
<device name="_750050480" package="WE-ISDN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-KI_0402A" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Wire Wound Ceramic Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; WE-KI series offers you an excellent Q factor and highest possible self resonant frequencies up to 12.5 GHz
&lt;br&gt;
&lt;br&gt; Inductance tolerances: 5% (2% on request)
&lt;br&gt;
&lt;br&gt; High thermal stability
&lt;br&gt;
&lt;br&gt; Operating temperature: –40°C to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Especially developed for high frequency applications
&lt;br&gt;
&lt;br&gt; RF transceiver/communications
&lt;br&gt;
&lt;br&gt; Bluetooth
&lt;br&gt;
&lt;br&gt; Wireless LAN
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-KI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-KI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-KI"&gt;http://katalog.we-online.de/en/pbs/WE-KI&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="" package="WE-KI_0402A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744765010A">
<attribute name="WE-NUMBER" value="744765010A/1nH"/>
</technology>
<technology name="_744765019A">
<attribute name="WE-NUMBER" value="744765019A/1,9nH"/>
</technology>
<technology name="_744765020A">
<attribute name="WE-NUMBER" value="744765020A/2nH"/>
</technology>
<technology name="_744765022A">
<attribute name="WE-NUMBER" value="744765022A/2,2nH"/>
</technology>
<technology name="_744765024A">
<attribute name="WE-NUMBER" value="744765024A/2,4nH"/>
</technology>
<technology name="_744765027A">
<attribute name="WE-NUMBER" value="744765027A/2,7nH"/>
</technology>
<technology name="_744765033A">
<attribute name="WE-NUMBER" value="744765033A/3,3nH"/>
</technology>
<technology name="_744765036A">
<attribute name="WE-NUMBER" value="744765036A/3,6nH"/>
</technology>
<technology name="_744765039A">
<attribute name="WE-NUMBER" value="744765039A/3,9nH"/>
</technology>
<technology name="_744765043A">
<attribute name="WE-NUMBER" value="744765043A/4,3nH"/>
</technology>
<technology name="_744765047A">
<attribute name="WE-NUMBER" value="744765047A/4,7nH"/>
</technology>
<technology name="_744765051A">
<attribute name="WE-NUMBER" value="744765051a/5,1nH"/>
</technology>
<technology name="_744765056A">
<attribute name="WE-NUMBER" value="744765056A/5,6nH"/>
</technology>
<technology name="_744765062A">
<attribute name="WE-NUMBER" value="744765062A/6,2nH"/>
</technology>
<technology name="_744765068A">
<attribute name="WE-NUMBER" value="744765068A/6,8nH"/>
</technology>
<technology name="_744765075A">
<attribute name="WE-NUMBER" value="744765075A/7,5nH"/>
</technology>
<technology name="_744765082A">
<attribute name="WE-NUMBER" value="744765082A/8,2nH"/>
</technology>
<technology name="_744765087A">
<attribute name="WE-NUMBER" value="744795087A/8,7nH"/>
</technology>
<technology name="_744765090A">
<attribute name="WE-NUMBER" value="744765090A/9nH"/>
</technology>
<technology name="_744765095A">
<attribute name="WE-NUMBER" value="744765095A/9,5nH"/>
</technology>
<technology name="_744765110A">
<attribute name="WE-NUMBER" value="744765110A/10nH"/>
</technology>
<technology name="_744765111A">
<attribute name="WE-NUMBER" value="744765111A/11nH"/>
</technology>
<technology name="_744765112A">
<attribute name="WE-NUMBER" value="744765112A/12nH"/>
</technology>
<technology name="_744765113A">
<attribute name="WE-NUMBER" value="744765113A/13nH"/>
</technology>
<technology name="_744765115A">
<attribute name="WE-NUMBER" value="744765115A/15nH"/>
</technology>
<technology name="_744765116A">
<attribute name="WE-NUMBER" value="744765116A/16nH"/>
</technology>
<technology name="_744765118A">
<attribute name="WE-NUMBER" value="744765118A/18nH"/>
</technology>
<technology name="_744765119A">
<attribute name="WE-NUMBER" value="744765119A/19nH"/>
</technology>
<technology name="_744765120A">
<attribute name="WE-NUMBER" value="744765120A/20nH"/>
</technology>
<technology name="_744765122A">
<attribute name="WE-NUMBER" value="744765122A/22nH"/>
</technology>
<technology name="_744765123A">
<attribute name="WE-NUMBER" value="744765123A/23nH"/>
</technology>
<technology name="_744765124A">
<attribute name="WE-NUMBER" value="744765124A/24nH"/>
</technology>
<technology name="_744765127A">
<attribute name="WE-NUMBER" value="744765127A/27nH"/>
</technology>
<technology name="_744765130A">
<attribute name="WE-NUMBER" value="744765130A/30nH"/>
</technology>
<technology name="_744765133A">
<attribute name="WE-NUMBER" value="744795133A/33nH"/>
</technology>
<technology name="_744765136A">
<attribute name="WE-NUMBER" value="744765136A/36nH"/>
</technology>
<technology name="_744765139A">
<attribute name="WE-NUMBER" value="744765139A/39nH"/>
</technology>
<technology name="_744765140A">
<attribute name="WE-NUMBER" value="744765140A/40nH"/>
</technology>
<technology name="_744765143A">
<attribute name="WE-NUMBER" value="744765143A/43nH"/>
</technology>
<technology name="_744765147A">
<attribute name="WE-NUMBER" value="744765147A/47nH"/>
</technology>
<technology name="_744765151A">
<attribute name="WE-NUMBER" value="744765151A/51nH"/>
</technology>
<technology name="_744765156A">
<attribute name="WE-NUMBER" value="744765156A/56nH"/>
</technology>
<technology name="_744765168A">
<attribute name="WE-NUMBER" value="744765168A/68nH"/>
</technology>
<technology name="_744765210A">
<attribute name="WE-NUMBER" value="744765210A/100nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_SV" prefix="L" uservalue="yes">
<description>&lt;b&gt;Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Easy assembly due to 4 pole housing
&lt;br&gt;
&lt;br&gt; Compact, small size
&lt;br&gt;
&lt;br&gt; 4 soldering pins for perfect mechanical decoupling
&lt;br&gt;
&lt;br&gt; Toroidal core choke with sector winding
&lt;br&gt;
&lt;br&gt; High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Custom designs on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;
&lt;br&gt; Power electronics
&lt;br&gt;
&lt;br&gt; SMPS
&lt;br&gt;
&lt;br&gt; Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LF?"&gt;http://katalog.we-online.de/en/pbs/WE-LF?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-LF_612/SV">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7446120027">
<attribute name="WE-NUMBER" value="7446120027/27mH"/>
</technology>
<technology name="_7446120039">
<attribute name="WE-NUMBER" value="7446120039/39mH"/>
</technology>
<technology name="_7446120047">
<attribute name="WE-NUMBER" value="7446120047.47mH"/>
</technology>
<technology name="_7446121007">
<attribute name="WE-NUMBER" value="7446121007/6,8mH"/>
</technology>
<technology name="_7446121010">
<attribute name="WE-NUMBER" value="7446121010/10mH"/>
</technology>
<technology name="_7446121018">
<attribute name="WE-NUMBER" value="7446121018/18mH"/>
</technology>
<technology name="_7446122001">
<attribute name="WE-NUMBER" value="7446122001/1mH"/>
</technology>
<technology name="_7446122003">
<attribute name="WE-NUMBER" value="7446122003/3,3mH"/>
</technology>
<technology name="_74461240004">
<attribute name="WE-NUMBER" value="74461240004/0,4mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_SMD" prefix="L" uservalue="yes">
<description>&lt;b&gt;Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; SMD power line choke
&lt;br&gt;
&lt;br&gt; Compact size
&lt;br&gt;
&lt;br&gt; Toroidal core with sector winding
&lt;br&gt;
&lt;br&gt; High attenuation of common mode interferences in low and middle frequency range
&lt;br&gt;
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Mains filter
&lt;br&gt;
&lt;br&gt; Power electronics
&lt;br&gt;
&lt;br&gt; SMPS
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LF_SMD.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LF_SMD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LF_SMD?"&gt;http://katalog.we-online.de/en/pbs/WE-LF_SMD?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-LF_SMD">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7446630027">
<attribute name="WE-NUMBER" value="7446630027/27mH"/>
</technology>
<technology name="_7446630039">
<attribute name="WE-NUMBER" value="7446630039/39mH"/>
</technology>
<technology name="_7446630047">
<attribute name="WE-NUMBER" value="7446630047/47mH"/>
</technology>
<technology name="_7446631007">
<attribute name="WE-NUMBER" value="7446631007/6,8mH"/>
</technology>
<technology name="_7446631010">
<attribute name="WE-NUMBER" value="7446631010/10mH"/>
</technology>
<technology name="_7446632001">
<attribute name="WE-NUMBER" value="7446632001/1mH"/>
</technology>
<technology name="_7446632002">
<attribute name="WE-NUMBER" value="7446632002/2,2mH"/>
</technology>
<technology name="_7446632003">
<attribute name="WE-NUMBER" value="7446632003/3,3mH"/>
</technology>
<technology name="_74466340007">
<attribute name="WE-NUMBER" value="74466340007/0,7mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_1040" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Low Profile High Current Molded Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Handles high transient current spikes
&lt;br&gt;
&lt;br&gt; No acoustic noise and no leakage field
&lt;br&gt;
&lt;br&gt; Frequency range up to 5 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;Br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC converters for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital cameras
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LHMI?"&gt;http://katalog.we-online.de/en/pbs/WE-LHMI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LHMI_1040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373680022">
<attribute name="WE-NUMBER" value="744373680022/2,2uH"/>
</technology>
<technology name="_744373680036">
<attribute name="WE-NUMBER" value="744373680036/0,36uH"/>
</technology>
<technology name="_744373680039">
<attribute name="WE-NUMBER" value="744373680039/0,39uH"/>
</technology>
<technology name="_744373680045">
<attribute name="WE-NUMBER" value="744373680045/0,45uH"/>
</technology>
<technology name="_744373680056">
<attribute name="WE-NUMBER" value="744373680056/0,56uH"/>
</technology>
<technology name="_744373680068">
<attribute name="WE-NUMBER" value="744373680068/0,68uH"/>
</technology>
<technology name="_74437368010">
<attribute name="WE-NUMBER" value="74437368010/1uH"/>
</technology>
<technology name="_74437368022">
<attribute name="WE-NUMBER" value="74437368022/0,22uH"/>
</technology>
<technology name="_74437368033">
<attribute name="WE-NUMBER" value="74437368033/3,3uH"/>
</technology>
<technology name="_74437368039">
<attribute name="WE-NUMBER" value="74437368039/3,9uH"/>
</technology>
<technology name="_74437368047">
<attribute name="WE-NUMBER" value="74437368047/4,7uH"/>
</technology>
<technology name="_74437368068">
<attribute name="WE-NUMBER" value="74437368068/6,8uH"/>
</technology>
<technology name="_74437368100">
<attribute name="WE-NUMBER" value="744737368100/10uH"/>
</technology>
<technology name="_74437368150">
<attribute name="WE-NUMBER" value="74437368150/15uH"/>
</technology>
<technology name="_74437368220">
<attribute name="WE-NUMBER" value="74437368220/22uH"/>
</technology>
<technology name="_74437368330">
<attribute name="WE-NUMBER" value="744373680330/33uH"/>
</technology>
<technology name="_74437368470">
<attribute name="WE-NUMBER" value="74437368470/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LLCR_ETD39" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LLCR Resonant Converter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Transformer for high efficiency power supply
&lt;br&gt;
&lt;br&gt; Input voltage 360–400 VDC
&lt;br&gt;
&lt;br&gt; Switching frequency 70–120 kHz
&lt;br&gt;
&lt;br&gt; Output power 150 W–250 W
&lt;br&gt;
&lt;br&gt; Testing voltage 4 kVAC
&lt;br&gt;
&lt;br&gt; Litz wire for low eddy current losses
&lt;br&gt;
&lt;br&gt; Defined leakage inductance for use without additional resonant inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power supplies for PC, netbook, LED lighting and other power supplies
&lt;br&gt;
&lt;br&gt; High efficient resonant converters
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtLLCR_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtLLCR_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LLCR?"&gt;http://katalog.we-online.de/en/pbs/WE-LLCR?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:2W"/>
</gates>
<devices>
<device name="_760895631" package="WE-LLCR_ETD39">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="8 9"/>
<connect gate="G$1" pin="3" pad="11 12"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="13 14"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="5"/>
<connect gate="G$1" pin="8" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760895641" package="WE-LLCR_ETD39">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="8"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="14"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="5"/>
<connect gate="G$1" pin="8" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760895651" package="WE-LLCR_ETD39">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="8"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="14"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="5"/>
<connect gate="G$1" pin="8" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LPF_0603" prefix="LPF" uservalue="yes">
<description>&lt;b&gt;Multilayer Chip Low-Pass Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Operating temperature: –40 °C to +85 °C
&lt;br&gt;
&lt;br&gt; Power capacity up to 3 W
&lt;br&gt;
&lt;br&gt; Low insertion loss and high attenuation in the stop-band
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt;
&lt;br&gt; Wireless communication systems like DECT, PACS, PHS, GSM, WLAN, Bluetooth …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/RfLPF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/RfLPF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LPF?"&gt;http://katalog.we-online.de/en/pbs/WE-LPF?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="T_6PIN"/>
</gates>
<devices>
<device name="_748112024" package="WE-LPF_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LPF_0805" prefix="LPF" uservalue="yes">
<description>&lt;b&gt;Multilayer Chip Low-Pass Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Operating temperature: –40 °C to +85 °C
&lt;br&gt;
&lt;br&gt; Power capacity up to 3 W
&lt;br&gt;
&lt;br&gt; Low insertion loss and high attenuation in the stop-band
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt;
&lt;br&gt; Wireless communication systems like DECT, PACS, PHS, GSM, WLAN, Bluetooth …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/RfLPF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/RfLPF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LPF?"&gt;http://katalog.we-online.de/en/pbs/WE-LPF?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE_LPF_0805"/>
</gates>
<devices>
<device name="" package="WE-LPF_0805">
<connects>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="3"/>
<connect gate="G$1" pin="GND3" pad="5"/>
<connect gate="G$1" pin="GND4" pad="7"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="OUT" pad="4"/>
</connects>
<technologies>
<technology name="_748111009"/>
<technology name="_748121055"/>
<technology name="_748125024"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQ_1812" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Miniature chip inductor wound on a special ferrite core
&lt;br&gt;
&lt;br&gt; Small inductances for compact circuits
&lt;br&gt;
&lt;br&gt; High Q at high frequencies
&lt;br&gt;
&lt;br&gt; Low DC-resistance
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;  Low power DC/DC-converters from Linear Technology, National Semiconductor, Texas Instruments, Fairchild Semiconductor, ON Semiconductor, STMicroelectronics, Maxim, MPS, Semtech, Exar, Analogic Tech, Diodes and Cologne Chip
&lt;br&gt;
&lt;br&gt; EMI-Filtering
&lt;br&gt;
&lt;br&gt; RF-circuits
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndLQ_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndLQ_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQ?"&gt;http://katalog.we-online.de/en/pbs/WE-LQ?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQ_L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744045001">
<attribute name="WE-NUMBER" value="744045001/1uH"/>
</technology>
<technology name="_7440450015">
<attribute name="WE-NUMBER" value="7440450015/1,5uH"/>
</technology>
<technology name="_7440450018">
<attribute name="WE-NUMBER" value="7440450018/1,8uH"/>
</technology>
<technology name="_744045002">
<attribute name="WE-NUMBER" value="744045002/2,2uH"/>
</technology>
<technology name="_7440450027">
<attribute name="WE-NUMBER" value="7440450027/2,7uH"/>
</technology>
<technology name="_744045003">
<attribute name="WE-NUMBER" value="744045003/3,3uH"/>
</technology>
<technology name="_7440450039">
<attribute name="WE-NUMBER" value="7440450039/3,9uH"/>
</technology>
<technology name="_744045004">
<attribute name="WE-NUMBER" value="744045004/4,7uH"/>
</technology>
<technology name="_7440450056">
<attribute name="WE-NUMBER" value="7440450056/5,6uH"/>
</technology>
<technology name="_744045006">
<attribute name="WE-NUMBER" value="744045006/6,8uH"/>
</technology>
<technology name="_744045008">
<attribute name="WE-NUMBER" value="744045008/8,2uH"/>
</technology>
<technology name="_744045100">
<attribute name="WE-NUMBER" value="744045100/10uH"/>
</technology>
<technology name="_744045102">
<attribute name="WE-NUMBER" value="744045102/1000uH"/>
</technology>
<technology name="_744045120">
<attribute name="WE-NUMBER" value="744045120/12uH"/>
</technology>
<technology name="_744045150">
<attribute name="WE-NUMBER" value="744045150/15uH"/>
</technology>
<technology name="_744045152">
<attribute name="WE-NUMBER" value="744042152/1500uH"/>
</technology>
<technology name="_744045180">
<attribute name="WE-NUMBER" value="744045180/18uH"/>
</technology>
<technology name="_744045210">
<attribute name="WE-NUMBER" value="744045210/100uH"/>
</technology>
<technology name="_744045215">
<attribute name="WE-NUMBER" value="744045215/150uH"/>
</technology>
<technology name="_744045220">
<attribute name="WE-NUMBER" value="744045220/22uH"/>
</technology>
<technology name="_744045222">
<attribute name="WE-NUMBER" value="744045222/2200uH"/>
</technology>
<technology name="_744045330">
<attribute name="WE-NUMBER" value="744045330/33uH"/>
</technology>
<technology name="_744045391">
<attribute name="WE-NUMBER" value="744045391/390uH"/>
</technology>
<technology name="_744045470">
<attribute name="WE-NUMBER" value="744045470/47uH"/>
</technology>
<technology name="_744045471">
<attribute name="WE-NUMBER" value="744045471/470uH"/>
</technology>
<technology name="_744045680">
<attribute name="WE-NUMBER" value="744045680/68uH"/>
</technology>
<technology name="_744045681">
<attribute name="WE-NUMBER" value="744045681/680uH"/>
</technology>
<technology name="_744045820">
<attribute name="WE-NUMBER" value="744045820/82uH"/>
</technology>
<technology name="_744045821">
<attribute name="WE-NUMBER" value="744045821/820uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQS_8065" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Tiny Power Inductor design
&lt;br&gt;
&lt;br&gt; 1.7 times more current in comparison with unshielded versions
&lt;br&gt;
&lt;br&gt; Robust design &amp; high durability
&lt;br&gt;
&lt;br&gt; Low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded with magnetic glue reducing buzz noise in ultra-low levels
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC Converters
&lt;br&gt;
&lt;br&gt; Switching controllers which required high efficiency
&lt;br&gt;
&lt;br&gt; Portable power (Smartphones, digital cameras, Tablets, etc.)
&lt;br&gt;
&lt;br&gt; Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt; Big sizes (5040, 60xx, 8040) used for shock-proof circuits
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndLQS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndLQS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQS"&gt;http://katalog.we-online.de/en/pbs/WE-LQS&lt;/a&gt;&lt;p&gt;


Created  by  Dan Xu 2014-05-21&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQS_8065">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74404086102">
<attribute name="WE-NUMBER" value="74404086102/1000uH"/>
</technology>
<technology name="_74404086103">
<attribute name="WE-NUMBER" value="74404086103/10000uH"/>
</technology>
<technology name="_74404086152">
<attribute name="WE-NUMBER" value="74404086152/1500uH"/>
</technology>
<technology name="_74404086222">
<attribute name="WE-NUMBER" value="74404086222/2200uH"/>
</technology>
<technology name="_74404086332">
<attribute name="WE-NUMBER" value="74404086332/3300uH"/>
</technology>
<technology name="_74404086472">
<attribute name="WE-NUMBER" value="74404086472/4700uH"/>
</technology>
<technology name="_74404086682">
<attribute name="WE-NUMBER" value="74404086682/6800uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_2506" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-MAIA SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;

&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;Hight current capability and handles hight transient current spikes
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range:-40°C up to 125°C
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;DC/DC-converter for high current power supplies  
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices 
&lt;br&gt;Wireless communication devices
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAIA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndMAIA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAIA/"&gt;http://katalog.we-online.de/en/pbs/WE-MAIA/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-04
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="" package="WE-MAIA_2506">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383210047">
<attribute name="WE-NUMBER" value="784383210047/0,47uH"/>
</technology>
<technology name="_78438321010">
<attribute name="WE-NUMBER" value="78438321010/1uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_4030" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD Metal Alloy Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;
&lt;br&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt;
&lt;br&gt; Low acoustic noise and low leakage flux noise
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC-converter for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL-converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital camera
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt; Wireless communication devices
&lt;br&gt;
&lt;br&gt; Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAPI?"&gt;http://katalog.we-online.de/en/pbs/WE-MAPI?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAPI_40XX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74438357010">
<attribute name="WE-NUMBER" value="74438357010/1uH"/>
</technology>
<technology name="_74438357012">
<attribute name="WE-NUMBER" value="74438357012/1,2uH"/>
</technology>
<technology name="_74438357015">
<attribute name="WE-NUMBER" value="74438357015/1,5uH"/>
</technology>
<technology name="_74438357018">
<attribute name="WE-NUMBER" value="74438357018/1,8uH"/>
</technology>
<technology name="_74438357022">
<attribute name="WE-NUMBER" value="74438357022/2,2uH"/>
</technology>
<technology name="_74438357047">
<attribute name="WE-NUMBER" value="74438357047/4,7uH"/>
</technology>
<technology name="_74438357056">
<attribute name="WE-NUMBER" value="74438357056/5,6uH"/>
</technology>
<technology name="_74438357068">
<attribute name="WE-NUMBER" value="74438357068/6,8uH"/>
</technology>
<technology name="_74438357082">
<attribute name="WE-NUMBER" value="74438357082/8,2uH"/>
</technology>
<technology name="_74438357100">
<attribute name="WE-NUMBER" value="744383570100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_2PIN" prefix="ANT" uservalue="yes">
<description>&lt;b&gt;Multilayer Chip Antenna
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; SMD Multilayer Chip Antenna
&lt;br&gt;
&lt;br&gt; Extremely low profile
&lt;br&gt;
&lt;br&gt; Very light component
&lt;br&gt;
&lt;br&gt; Power capacity: 5 W max.
&lt;br&gt;
&lt;br&gt; Omni-directional
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +85 °C
&lt;br&gt;
&lt;br&gt; High gain
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; applications
&lt;br&gt;
&lt;br&gt; WLAN
&lt;br&gt;
&lt;br&gt; Home RF (868 MHz)
&lt;br&gt;
&lt;br&gt; Bluetooth applications
&lt;br&gt;
&lt;br&gt; GSM 900
&lt;br&gt;
&lt;br&gt; ISM 868/2400
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MCA.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MCA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MCA?"&gt;http://katalog.we-online.de/en/pbs/WE-MCA?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA"/>
</gates>
<devices>
<device name="_7488910245" package="WE-MCA_7488910245">
<connects>
<connect gate="G$1" pin="FP" pad="2"/>
<connect gate="G$1" pin="NC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7488930245" package="WE-MCA_7488930245">
<connects>
<connect gate="G$1" pin="FP" pad="1"/>
<connect gate="G$1" pin="NC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7488910043" package="WE-MCA_7488910043">
<connects>
<connect gate="G$1" pin="FP" pad="1"/>
<connect gate="G$1" pin="NC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7488940245" package="WE-MCA_7488105XX/7488940245">
<connects>
<connect gate="G$1" pin="FP" pad="1"/>
<connect gate="G$1" pin="NC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_7488910092" prefix="ANT" uservalue="yes">
<description>&lt;b&gt;Multilayer Chip Antenna
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; SMD Multilayer Chip Antenna
&lt;br&gt;
&lt;br&gt; Extremely low profile
&lt;br&gt;
&lt;br&gt; Very light component
&lt;br&gt;
&lt;br&gt; Power capacity: 5 W max.
&lt;br&gt;
&lt;br&gt; Omni-directional
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +85 °C
&lt;br&gt;
&lt;br&gt; High gain
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; applications
&lt;br&gt;
&lt;br&gt; WLAN
&lt;br&gt;
&lt;br&gt; Home RF (868 MHz)
&lt;br&gt;
&lt;br&gt; Bluetooth applications
&lt;br&gt;
&lt;br&gt; GSM 900
&lt;br&gt;
&lt;br&gt; ISM 868/2400
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MCA.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MCA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MCA?"&gt;http://katalog.we-online.de/en/pbs/WE-MCA?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA_7488910092"/>
</gates>
<devices>
<device name="" package="WE-MCA_7488910092">
<connects>
<connect gate="G$1" pin="FD" pad="2"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="3"/>
<connect gate="G$1" pin="NC3" pad="4"/>
<connect gate="G$1" pin="NC4" pad="5"/>
<connect gate="G$1" pin="NC5" pad="6"/>
<connect gate="G$1" pin="NC6" pad="7"/>
<connect gate="G$1" pin="NC7" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_7488912455" prefix="ANT" uservalue="yes">
<description>&lt;b&gt;Multilayer Chip Antenna
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; SMD Multilayer Chip Antenna
&lt;br&gt;
&lt;br&gt; Extremely low profile
&lt;br&gt;
&lt;br&gt; Very light component
&lt;br&gt;
&lt;br&gt; Power capacity: 5 W max.
&lt;br&gt;
&lt;br&gt; Omni-directional
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +85 °C
&lt;br&gt;
&lt;br&gt; High gain
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; applications
&lt;br&gt;
&lt;br&gt; WLAN
&lt;br&gt;
&lt;br&gt; Home RF (868 MHz)
&lt;br&gt;
&lt;br&gt; Bluetooth applications
&lt;br&gt;
&lt;br&gt; GSM 900
&lt;br&gt;
&lt;br&gt; ISM 868/2400
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MCA.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MCA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MCA?"&gt;http://katalog.we-online.de/en/pbs/WE-MCA?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="T_4PIN"/>
</gates>
<devices>
<device name="" package="WE-MCA_7488912455">
<connects>
<connect gate="G$1" pin="FD_HB" pad="4"/>
<connect gate="G$1" pin="FD_LB" pad="3"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_7488920245" prefix="ANT" uservalue="yes">
<description>&lt;b&gt;Multilayer Chip Antenna
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; SMD Multilayer Chip Antenna
&lt;br&gt;
&lt;br&gt; Extremely low profile
&lt;br&gt;
&lt;br&gt; Very light component
&lt;br&gt;
&lt;br&gt; Power capacity: 5 W max.
&lt;br&gt;
&lt;br&gt; Omni-directional
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +85 °C
&lt;br&gt;
&lt;br&gt; High gain
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; applications
&lt;br&gt;
&lt;br&gt; WLAN
&lt;br&gt;
&lt;br&gt; Home RF (868 MHz)
&lt;br&gt;
&lt;br&gt; Bluetooth applications
&lt;br&gt;
&lt;br&gt; GSM 900
&lt;br&gt;
&lt;br&gt; ISM 868/2400
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MCA.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MCA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MCA?"&gt;http://katalog.we-online.de/en/pbs/WE-MCA?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA_7488920245"/>
</gates>
<devices>
<device name="" package="WE-MCA_7488920245">
<connects>
<connect gate="G$1" pin="FP" pad="1"/>
<connect gate="G$1" pin="GND1" pad="2"/>
<connect gate="G$1" pin="GND2" pad="3"/>
<connect gate="G$1" pin="NC1" pad="4"/>
<connect gate="G$1" pin="NC2" pad="5"/>
<connect gate="G$1" pin="NC3" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MI_0603" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Multilayer Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Smallest inductor possible for less space needed on the printed circuit board and therefore perfect suitable for high density mounting
&lt;br&gt;
&lt;br&gt; No cross coupling because of closed magnetic circuits
&lt;br&gt;
&lt;br&gt; No crosstalk
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter circuits
&lt;br&gt;
&lt;br&gt; Oscillators
&lt;br&gt;
&lt;br&gt; Adjustment networks
&lt;br&gt;
&lt;br&gt; Discretely built T- or π-Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MI?"&gt;http://katalog.we-online.de/en/pbs/WE-MI?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="" package="WE-MI_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479614">
<attribute name="WE-NUMBER" value="74479614/0,047uH"/>
</technology>
<technology name="_74479616">
<attribute name="WE-NUMBER" value="74479616/0,068uH"/>
</technology>
<technology name="_7447962">
<attribute name="WE-NUMBER" value="7447962/0,1uH"/>
</technology>
<technology name="_744796215">
<attribute name="WE-NUMBER" value="744796215/1,5uH"/>
</technology>
<technology name="_74479623">
<attribute name="WE-NUMBER" value="74479623/0,22uH"/>
</technology>
<technology name="_744796233">
<attribute name="WE-NUMBER" value="744796233/0,33uH"/>
</technology>
<technology name="_74479628">
<attribute name="WE-NUMBER" value="74479628/0,82uH"/>
</technology>
<technology name="_74479632">
<attribute name="WE-NUMBER" value="74479632/0,47uH"/>
</technology>
<technology name="_7447964">
<attribute name="WE-NUMBER" value="7447964/0,68uH"/>
</technology>
<technology name="_74479645">
<attribute name="WE-NUMBER" value="74479645/0,56uH"/>
</technology>
<technology name="_7447965">
<attribute name="WE-NUMBER" value="7447965/1uH"/>
</technology>
<technology name="_74479651">
<attribute name="WE-NUMBER" value="74479651/1,8uH"/>
</technology>
<technology name="_74479652">
<attribute name="WE-NUMBER" value="74479652/2,2uH"/>
</technology>
<technology name="_74479653">
<attribute name="WE-NUMBER" value="74479653/3,3uH"/>
</technology>
<technology name="_7447966">
<attribute name="WE-NUMBER" value="7447966/4,7uH"/>
</technology>
<technology name="_74479668">
<attribute name="WE-NUMBER" value="74479668/6,8uH"/>
</technology>
<technology name="_7447967">
<attribute name="WE-NUMBER" value="7447967/8,2uH"/>
</technology>
<technology name="_7447968">
<attribute name="WE-NUMBER" value="7447968/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MK_0201" prefix="L" uservalue="yes">
<description>&lt;b&gt;Multilayer Ceramic SMD Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Windings printed on ceramic substrate
&lt;br&gt;
&lt;br&gt; Extremely high self resonant frequency &gt; 17 GHz
&lt;br&gt;
&lt;br&gt; Inductive tolerances of 5%; ± 0.3 nH
&lt;br&gt;
&lt;br&gt; Operating temperature: –40°C to +120°C
&lt;br&gt;
&lt;br&gt; Inductance is stable over temperature
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; High frequency circuits
&lt;br&gt;
&lt;br&gt; Bluetooth
&lt;br&gt;
&lt;br&gt; Wireless LAN
&lt;br&gt;
&lt;br&gt; Filter circuits
&lt;br&gt;
&lt;br&gt; Oscillators
&lt;br&gt;
&lt;br&gt; Pagers
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; PCMCIA-cards
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-mk_multilayer_keramik_smd_induktivitaet.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-mk_multilayer_keramik_smd_induktivitaet.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MK?"&gt;http://katalog.we-online.de/en/pbs/WE-MK?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="" package="WE-MK_0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74478201">
<attribute name="WE-NUMBER" value="74478201/1nH"/>
</technology>
<technology name="_744782012">
<attribute name="WE-NUMBER" value="744782012/1,2nH"/>
</technology>
<technology name="_744782015">
<attribute name="WE-NUMBER" value="744782015/1,5nH"/>
</technology>
<technology name="_744782018">
<attribute name="WE-NUMBER" value="744782018/1,8nH"/>
</technology>
<technology name="_744782022">
<attribute name="WE-NUMBER" value="744782022/2,2nH"/>
</technology>
<technology name="_744782027">
<attribute name="WE-NUMBER" value="744782027/2,7nH"/>
</technology>
<technology name="_744782033">
<attribute name="WE-NUMBER" value="744782033/3,3nH"/>
</technology>
<technology name="_744782039">
<attribute name="WE-NUMBER" value="744782039/3,9nH"/>
</technology>
<technology name="_744782047">
<attribute name="WE-NUMBER" value="744782047/4,7nH"/>
</technology>
<technology name="_744782056">
<attribute name="WE-NUMBER" value="744782056/5,6nH"/>
</technology>
<technology name="_744782068">
<attribute name="WE-NUMBER" value="744782068/6,8nH"/>
</technology>
<technology name="_744782082">
<attribute name="WE-NUMBER" value="744782082/8,2nH"/>
</technology>
<technology name="_74478210">
<attribute name="WE-NUMBER" value="74478210/10nH"/>
</technology>
<technology name="_74478212">
<attribute name="WE-NUMBER" value="74478212/1,2nH"/>
</technology>
<technology name="_74478215">
<attribute name="WE-NUMBER" value="74478215/1,5nH"/>
</technology>
<technology name="_74478218">
<attribute name="WE-NUMBER" value="74478218/1,8nH"/>
</technology>
<technology name="_74478222">
<attribute name="WE-NUMBER" value="74478222/22nH"/>
</technology>
<technology name="_74478227">
<attribute name="WE-NUMBER" value="74478227/27nH"/>
</technology>
<technology name="_74478233">
<attribute name="WE-NUMBER" value="74478233/3,3nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MLS-3WAY" prefix="L" uservalue="yes">
<description>&lt;b&gt;Multiline EMI Suppression Ferrite
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High impedance common mode inductor with 2x2 windings made by PCB line connection
&lt;br&gt;
&lt;br&gt; High rated current with typ. 4 A
&lt;br&gt;
&lt;br&gt; Broadband filtering because of the NiZn-ferrite core
&lt;br&gt;
&lt;br&gt; RF common mode inductor for 2, 3 or 4 lines in one component
&lt;br&gt;
&lt;br&gt; Compact size
&lt;br&gt;
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Custom designs on request
&lt;br&gt;
&lt;br&gt; With the appropriate layout (see below) the impedance (i.e. 4 windings) respectively the current (parallel circuit) could be increased
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfect suitable for absorption of common or differential mode interferences in the field of EMC
&lt;br&gt;
&lt;br&gt; High-current DC output filters of power supplies e.g. battery chargers, industrial power supplies
&lt;br&gt;
&lt;br&gt; With one turn the component performes like a 3 or 4 times common mode choke for the signal
&lt;br&gt;
&lt;br&gt; 4-line sensor application


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MLS.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MLS.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MLS?"&gt;http://katalog.we-online.de/en/pbs/WE-MLS?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-3W"/>
</gates>
<devices>
<device name="_74273001" package="WE-3WAY_74273001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MLS-4WAY" prefix="L" uservalue="yes">
<description>&lt;b&gt;Multiline EMI Suppression Ferrite
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High impedance common mode inductor with 2x2 windings made by PCB line connection
&lt;br&gt;
&lt;br&gt; High rated current with typ. 4 A
&lt;br&gt;
&lt;br&gt; Broadband filtering because of the NiZn-ferrite core
&lt;br&gt;
&lt;br&gt; RF common mode inductor for 2, 3 or 4 lines in one component
&lt;br&gt;
&lt;br&gt; Compact size
&lt;br&gt;
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Custom designs on request
&lt;br&gt;
&lt;br&gt; With the appropriate layout (see below) the impedance (i.e. 4 windings) respectively the current (parallel circuit) could be increased
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfect suitable for absorption of common or differential mode interferences in the field of EMC
&lt;br&gt;
&lt;br&gt; High-current DC output filters of power supplies e.g. battery chargers, industrial power supplies
&lt;br&gt;
&lt;br&gt; With one turn the component performes like a 3 or 4 times common mode choke for the signal
&lt;br&gt;
&lt;br&gt; 4-line sensor application


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MLS.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MLS.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MLS?"&gt;http://katalog.we-online.de/en/pbs/WE-MLS?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-4W"/>
</gates>
<devices>
<device name="_74273002" package="WE-4WAY_74273002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_742730021" package="WE-4WAY_742730021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_742730022" package="WE-4WAY_742730022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_742730023" package="WE-4WAY_742730023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_742730321" package="WE-4WAY_742730321">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PBF" prefix="L" uservalue="yes">
<description>&lt;b&gt;Flat Wire High Current SMD Ferrite Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Flat wire
&lt;br&gt;
&lt;br&gt; Suitable for applications with high currents up to 6 A
&lt;br&gt;
&lt;br&gt; Glued version: High mechanical stability
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Voltage supply for high load current
&lt;br&gt;
&lt;br&gt; Glued version: Especially for applications with permanent vibrations
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PBF.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PBF.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PBF?"&gt;http://katalog.we-online.de/en/pbs/WE-PBF?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="_7427932" package="WE-PBF_7427932">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7427930" package="WE-PBF_7427930">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7427931" package="WE-PBF_7427931">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74279390" package="WE-PBF_7427930">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74279391" package="WE-PBF_7427931">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74279392" package="WE-PBF_7427932">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_1030" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; High Saturation currents up to 25 A
&lt;br&gt;
&lt;br&gt; Very low self-losses at high switching frequency‘s
&lt;br&gt;
&lt;br&gt; Wide inductances spectrum available at all sizes
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt; Integrated DC/DC- converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD?"&gt;http://katalog.we-online.de/en/pbs/WE-PD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD_1030/1050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447713015">
<attribute name="WE-NUMBER" value="7447713015/1,5uH"/>
</technology>
<technology name="_7447713022">
<attribute name="WE-NUMBER" value="7447713022/2,2uH"/>
</technology>
<technology name="_7447713033">
<attribute name="WE-NUMBER" value="7447713033/3,3uH"/>
</technology>
<technology name="_7447713047">
<attribute name="WE-NUMBER" value="7447713047/4,7uH"/>
</technology>
<technology name="_7447713082">
<attribute name="WE-NUMBER" value="7447713082/8,2uH"/>
</technology>
<technology name="_7447713100">
<attribute name="WE-NUMBER" value="7447713100/10uH"/>
</technology>
<technology name="_7447713101">
<attribute name="WE-NUMBER" value="7447713101/100uH"/>
</technology>
<technology name="_7447713102">
<attribute name="WE-NUMBER" value="7447713102/1000uH"/>
</technology>
<technology name="_7447713121">
<attribute name="WE-NUMBER" value="7447713121/120uH"/>
</technology>
<technology name="_7447713150">
<attribute name="WE-NUMBER" value="7447713150/15uH"/>
</technology>
<technology name="_7447713151">
<attribute name="WE-NUMBER" value="7447713151/150uH"/>
</technology>
<technology name="_7447713220">
<attribute name="WE-NUMBER" value="7447713220/22uH"/>
</technology>
<technology name="_7447713330">
<attribute name="WE-NUMBER" value="7447713330/33uH"/>
</technology>
<technology name="_7447713331">
<attribute name="WE-NUMBER" value="7447713331/330uH"/>
</technology>
<technology name="_7447713470">
<attribute name="WE-NUMBER" value="7447713470/47uH"/>
</technology>
<technology name="_7447713471">
<attribute name="WE-NUMBER" value="7447713471/470uH"/>
</technology>
<technology name="_7447713680">
<attribute name="WE-NUMBER" value="7447713680/68uH"/>
</technology>
<technology name="_7447713820">
<attribute name="WE-NUMBER" value="7447713820/82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2_1054" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Open size
&lt;br&gt;
&lt;br&gt; Saturation currents up to 14 A
&lt;br&gt;
&lt;br&gt; Low tolerances at high inductance values
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC-converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Optimal attenuation in MHz frequency range
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD2"&gt;http://katalog.we-online.de/en/pbs/WE-PD2&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2_1054">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744776012">
<attribute name="WE-NUMBER" value="744776012/1,2uHuH"/>
</technology>
<technology name="_744776022">
<attribute name="WE-NUMBER" value="744776022/2,2uH"/>
</technology>
<technology name="_744776033">
<attribute name="WE-NUMBER" value="744776033/3,3uH"/>
</technology>
<technology name="_744776047">
<attribute name="WE-NUMBER" value="744776047/4,7uH"/>
</technology>
<technology name="_744776056">
<attribute name="WE-NUMBER" value="744776056/5,6uH"/>
</technology>
<technology name="_744776068">
<attribute name="WE-NUMBER" value="744776068/6,8uH"/>
</technology>
<technology name="_744776082">
<attribute name="WE-NUMBER" value="744776082/8,2uH"/>
</technology>
<technology name="_74477610">
<attribute name="WE-NUMBER" value="74477610/10uH"/>
</technology>
<technology name="_744776112">
<attribute name="WE-NUMBER" value="744776112/12uH"/>
</technology>
<technology name="_744776115">
<attribute name="WE-NUMBER" value="744776115/15uH"/>
</technology>
<technology name="_744776118">
<attribute name="WE-NUMBER" value="744776118/18uH"/>
</technology>
<technology name="_744776122">
<attribute name="WE-NUMBER" value="744776122/22uH"/>
</technology>
<technology name="_744776127">
<attribute name="WE-NUMBER" value="744776127/27uH"/>
</technology>
<technology name="_744776133">
<attribute name="WE-NUMBER" value="744776133/33uH"/>
</technology>
<technology name="_744776139">
<attribute name="WE-NUMBER" value="744776139/39uH"/>
</technology>
<technology name="_744776147">
<attribute name="WE-NUMBER" value="744776147/47uH"/>
</technology>
<technology name="_744776156">
<attribute name="WE-NUMBER" value="744776156/56uH"/>
</technology>
<technology name="_744776168">
<attribute name="WE-NUMBER" value="744776168/68uH"/>
</technology>
<technology name="_744776182">
<attribute name="WE-NUMBER" value="744776182/82uH"/>
</technology>
<technology name="_74477620">
<attribute name="WE-NUMBER" value="74477620/100uH"/>
</technology>
<technology name="_744776212">
<attribute name="WE-NUMBER" value="744776212/120uH"/>
</technology>
<technology name="_744776215">
<attribute name="WE-NUMBER" value="744776215/150uH"/>
</technology>
<technology name="_744776218">
<attribute name="WE-NUMBER" value="744776218/180uH"/>
</technology>
<technology name="_744776222">
<attribute name="WE-NUMBER" value="744776222/220uH"/>
</technology>
<technology name="_744776227">
<attribute name="WE-NUMBER" value="744776227/270uH"/>
</technology>
<technology name="_744776233">
<attribute name="WE-NUMBER" value="744776233/330uH"/>
</technology>
<technology name="_744776239">
<attribute name="WE-NUMBER" value="744776239/390uH"/>
</technology>
<technology name="_744776247">
<attribute name="WE-NUMBER" value="744776247/470uH"/>
</technology>
<technology name="_744776256">
<attribute name="WE-NUMBER" value="744776256/560uH"/>
</technology>
<technology name="_744776268">
<attribute name="WE-NUMBER" value="744776268/680uH"/>
</technology>
<technology name="_744776282">
<attribute name="WE-NUMBER" value="744776282/820uH"/>
</technology>
<technology name="_74477630">
<attribute name="WE-NUMBER" value="74477630/1000uH"/>
</technology>
<technology name="_744776312">
<attribute name="WE-NUMBER" value="744776312/1200uH"/>
</technology>
<technology name="_744776322">
<attribute name="WE-NUMBER" value="744776322/2200uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2A_1054" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-PD2A SMD Power Inductor
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;
&lt;/b&gt;&lt;br&gt;Open size
&lt;br&gt;Current capability up to 14A
&lt;br&gt;Operating temperature:-40°C  to 125°C
&lt;br&gt;Recommended soder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;switching regulators with low operating voltage (navigation system, air conditioning, entertainment, park assistance control)
&lt;br&gt;Integrated DC/DC-converter 
&lt;br&gt;Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD2A/"&gt;http://katalog.we-online.de/en/pbs/WE-PD2A/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-04
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="" package="WE-PD2A_1054">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784776012">
<attribute name="WE-NUMBER" value="784776012/1,2uH"/>
</technology>
<technology name="_784776022">
<attribute name="WE-NUMBER" value="784776022/2,2uH"/>
</technology>
<technology name="_784776033">
<attribute name="WE-NUMBER" value="784776033/3,3uH"/>
</technology>
<technology name="_784776047">
<attribute name="WE-NUMBER" value="784776047/4,7uH"/>
</technology>
<technology name="_784776056">
<attribute name="WE-NUMBER" value="784776056/5,6uH"/>
</technology>
<technology name="_784776068">
<attribute name="WE-NUMBER" value="784776068/6,8uH"/>
</technology>
<technology name="_784776082">
<attribute name="WE-NUMBER" value="784776082/8,2uH"/>
</technology>
<technology name="_78477610">
<attribute name="WE-NUMBER" value="78477610/10uH"/>
</technology>
<technology name="_784776112">
<attribute name="WE-NUMBER" value="784776112/12uH"/>
</technology>
<technology name="_784776115">
<attribute name="WE-NUMBER" value="784776115/15uH"/>
</technology>
<technology name="_784776118">
<attribute name="WE-NUMBER" value="784776118/18uH"/>
</technology>
<technology name="_784776122">
<attribute name="WE-NUMBER" value="784776122/22uH"/>
</technology>
<technology name="_784776127">
<attribute name="WE-NUMBER" value="784776127/27uH"/>
</technology>
<technology name="_784776133">
<attribute name="WE-NUMBER" value="784776133/33uH"/>
</technology>
<technology name="_784776139">
<attribute name="WE-NUMBER" value="784776139/39uH"/>
</technology>
<technology name="_784776147">
<attribute name="WE-NUMBER" value="784776147/47uH"/>
</technology>
<technology name="_784776156">
<attribute name="WE-NUMBER" value="784776156/56uH"/>
</technology>
<technology name="_784776168">
<attribute name="WE-NUMBER" value="784776168/68uH"/>
</technology>
<technology name="_784776182">
<attribute name="WE-NUMBER" value="784776182/82uH"/>
</technology>
<technology name="_78477620">
<attribute name="WE-NUMBER" value="78477620/100uH"/>
</technology>
<technology name="_784776212">
<attribute name="WE-NUMBER" value="784776212/120uH"/>
</technology>
<technology name="_784776215">
<attribute name="WE-NUMBER" value="784776215/150uH"/>
</technology>
<technology name="_784776218">
<attribute name="WE-NUMBER" value="784776218/180uH"/>
</technology>
<technology name="_784776222">
<attribute name="WE-NUMBER" value="784776222/220uH"/>
</technology>
<technology name="_784776227">
<attribute name="WE-NUMBER" value="784776227/270uH"/>
</technology>
<technology name="_784776233">
<attribute name="WE-NUMBER" value="784776233/330uH"/>
</technology>
<technology name="_784776239">
<attribute name="WE-NUMBER" value="784776239/390uH"/>
</technology>
<technology name="_784776247">
<attribute name="WE-NUMBER" value="784776247/470uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2SR_7850" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic shielded version from the WE-PD2, which results in a low leakage field
&lt;br&gt;
&lt;br&gt; High saturation current due the self-centering shielding ring construction
&lt;br&gt;
&lt;br&gt; Pin compatible with the PD2 size 7850
&lt;br&gt;
&lt;br&gt; Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C up to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switching regulators with low operation voltage like in portable devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD2SR.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD2SR.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD2SR?"&gt;http://katalog.we-online.de/en/pbs/WE-PD2SR?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2SR_7850">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744787012">
<attribute name="WE-NUMBER" value="744787012/1,2uH"/>
</technology>
<technology name="_744787027">
<attribute name="WE-NUMBER" value="744787027/2,7uH"/>
</technology>
<technology name="_744787039">
<attribute name="WE-NUMBER" value="744787039/3,9uH"/>
</technology>
<technology name="_744787047">
<attribute name="WE-NUMBER" value="744787047/4,7uH"/>
</technology>
<technology name="_744787068">
<attribute name="WE-NUMBER" value="744787068/6,8uH"/>
</technology>
<technology name="_744787082">
<attribute name="WE-NUMBER" value="744787082/8,2uH"/>
</technology>
<technology name="_744787100">
<attribute name="WE-NUMBER" value="744787100/10uH"/>
</technology>
<technology name="_744787101">
<attribute name="WE-NUMBER" value="744787101/100uH"/>
</technology>
<technology name="_744787120">
<attribute name="WE-NUMBER" value="744787120/12uH"/>
</technology>
<technology name="_744787121">
<attribute name="WE-NUMBER" value="744787121/120uH"/>
</technology>
<technology name="_744787150">
<attribute name="WE-NUMBER" value="744787150/15uH"/>
</technology>
<technology name="_744787151">
<attribute name="WE-NUMBER" value="744787151/150uH"/>
</technology>
<technology name="_744787180">
<attribute name="WE-NUMBER" value="744787180/18uH"/>
</technology>
<technology name="_744787181">
<attribute name="WE-NUMBER" value="744787181/180uH"/>
</technology>
<technology name="_744787220">
<attribute name="WE-NUMBER" value="744787220/22uH"/>
</technology>
<technology name="_744787221">
<attribute name="WE-NUMBER" value="744787221/220uH"/>
</technology>
<technology name="_744787330">
<attribute name="WE-NUMBER" value="744787330/33uH"/>
</technology>
<technology name="_744787470">
<attribute name="WE-NUMBER" value="744787470/47uH"/>
</technology>
<technology name="_744787680">
<attribute name="WE-NUMBER" value="744787680/68uH"/>
</technology>
<technology name="_744787820">
<attribute name="WE-NUMBER" value="744787820/82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2_HV_1054" prefix="L" uservalue="yes">
<description>&lt;b&gt;High Voltage SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Unshielded construction
&lt;br&gt;
&lt;br&gt; Designed for 400 VDC
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Non-isolated buck or buck-boost converter like Power Integrations LinkSwitch-TN
&lt;br&gt;
&lt;br&gt; Constant current LED driver
&lt;br&gt;
&lt;br&gt; Utility metering
&lt;br&gt;
&lt;br&gt; Filter for power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD2_HV?"&gt;http://katalog.we-online.de/en/pbs/WE-PD2_HV?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2_1054">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_76877630">
<attribute name="WE-NUMBER" value="76877630/1000uH"/>
</technology>
<technology name="_768776312">
<attribute name="WE-NUMBER" value="768776312/1200uH"/>
</technology>
<technology name="_768776322">
<attribute name="WE-NUMBER" value="768776332/2200uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD3_X" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; Working frequency up to 10 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; EMI-filter
&lt;br&gt;
&lt;br&gt; Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Texas Instruments, Maxim, Semtech, ON Semiconductor, Cologne Chip, STMicroelectronics, Maxim, MPS, Diodes, Analogic Tech and Exar
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-pd3_smd_speicherdrossel.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-pd3_smd_speicherdrossel.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD3?"&gt;http://katalog.we-online.de/en/pbs/WE-PD3?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD3_X">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74459010">
<attribute name="WE-NUMBER" value="74459010/10uH"/>
</technology>
<technology name="_74459115">
<attribute name="WE-NUMBER" value="74459115/15uH"/>
</technology>
<technology name="_74459122">
<attribute name="WE-NUMBER" value="74459122/22uH"/>
</technology>
<technology name="_74459133">
<attribute name="WE-NUMBER" value="74459133/33uH"/>
</technology>
<technology name="_74459147">
<attribute name="WE-NUMBER" value="74459147/47uH"/>
</technology>
<technology name="_74459168">
<attribute name="WE-NUMBER" value="74459168/68uH"/>
</technology>
<technology name="_7445920">
<attribute name="WE-NUMBER" value="7445920/100uH"/>
</technology>
<technology name="_74459215">
<attribute name="WE-NUMBER" value="74459215/150uH"/>
</technology>
<technology name="_74459222">
<attribute name="WE-NUMBER" value="74459222/220uH"/>
</technology>
<technology name="_74459233">
<attribute name="WE-NUMBER" value="74459233/330uH"/>
</technology>
<technology name="_74459247">
<attribute name="WE-NUMBER" value="74459247/470uH"/>
</technology>
<technology name="_74459268">
<attribute name="WE-NUMBER" value="74459268/680uH"/>
</technology>
<technology name="_7445930">
<attribute name="WE-NUMBER" value="7445930/1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD4_L" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Current loading up to 38 A
&lt;br&gt;
&lt;br&gt; Compact size
&lt;br&gt;
&lt;br&gt; Low-loss ferrite core
&lt;br&gt;
&lt;br&gt; Application frequency range up to 10 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Noise suppression
&lt;br&gt;
&lt;br&gt; Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Maxim, Semtech, Texas Instruments, Fairchild Semiconductor, Cologne Chip, ON Semiconductor, STMicroelectronics, MPS, Exar, Analogic Tech and Diodes
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="hhttp://katalog.we-online.de/media/images/v2/Family_WE-PD4.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD4.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD4?"&gt;http://katalog.we-online.de/en/pbs/WE-PD4?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD3_L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7445601">
<attribute name="WE-NUMBER" value="7445601/1uH"/>
</technology>
<technology name="_74456015">
<attribute name="WE-NUMBER" value="74456015/1,5uH"/>
</technology>
<technology name="_74456022">
<attribute name="WE-NUMBER" value="74456022/2,2uH"/>
</technology>
<technology name="_74456025">
<attribute name="WE-NUMBER" value="74456025/2,5uH"/>
</technology>
<technology name="_74456033">
<attribute name="WE-NUMBER" value="74456033/3,3uH"/>
</technology>
<technology name="_74456047">
<attribute name="WE-NUMBER" value="74456047/4,7uH"/>
</technology>
<technology name="_74456056">
<attribute name="WE-NUMBER" value="74456056/5,6uH"/>
</technology>
<technology name="_74456068">
<attribute name="WE-NUMBER" value="74456068/6,8uH"/>
</technology>
<technology name="_74456082">
<attribute name="WE-NUMBER" value="74456082/8,2uH"/>
</technology>
<technology name="_7445610">
<attribute name="WE-NUMBER" value="7445610/10uH"/>
</technology>
<technology name="_74456115">
<attribute name="WE-NUMBER" value="74456115/15uH"/>
</technology>
<technology name="_74456122">
<attribute name="WE-NUMBER" value="74456122/22uH"/>
</technology>
<technology name="_74456133">
<attribute name="WE-NUMBER" value="74456133/33uH"/>
</technology>
<technology name="_74456147">
<attribute name="WE-NUMBER" value="74456147/47uH"/>
</technology>
<technology name="_74456168">
<attribute name="WE-NUMBER" value="74456168/68uH"/>
</technology>
<technology name="_7445620">
<attribute name="WE-NUMBER" value="7445620/100uH"/>
</technology>
<technology name="_74456215">
<attribute name="WE-NUMBER" value="74456215/150uH"/>
</technology>
<technology name="_74456222">
<attribute name="WE-NUMBER" value="74456222/220uH"/>
</technology>
<technology name="_74456233">
<attribute name="WE-NUMBER" value="74456233/330uH"/>
</technology>
<technology name="_74456247">
<attribute name="WE-NUMBER" value="74456247/470uH"/>
</technology>
<technology name="_74456268">
<attribute name="WE-NUMBER" value="74456268/680uH"/>
</technology>
<technology name="_7445630">
<attribute name="WE-NUMBER" value="7445630/1000uH"/>
</technology>
<technology name="_74456322">
<attribute name="WE-NUMBER" value="74456322/2200uH"/>
</technology>
<technology name="_74456347">
<attribute name="WE-NUMBER" value="74456347/4700uH"/>
</technology>
<technology name="_74456382">
<attribute name="WE-NUMBER" value="74456382/8200uH"/>
</technology>
<technology name="_7445640">
<attribute name="WE-NUMBER" value="7445640/10000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDA_1210" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-PDA SMD Shielded Power Inductor
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;Wire connection:welding technology
&lt;br&gt;Operating temperature:-40°C up to 125°C
&lt;br&gt;Highest possible current loading for SMD Inductors
&lt;br&gt;Magnetically shielded version which results in a low leakage field High storage capacity
&lt;br&gt;Low self-losses
&lt;br&gt;Core Material:NiZn
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;Multimedia applications
&lt;br&gt;Switching regulators with low operating voltages (Computer, Notebook, smart phones)
&lt;br&gt;Integrated DC/DC-converter
&lt;br&gt;Perfect suitable for switching regulators with exrtemely high efficiency (&gt;86%)
&lt;br&gt;

&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-pda.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-pda.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PDA/"&gt;http://katalog.we-online.de/en/pbs/WE-PDA/
&lt;/a&gt;&lt;p&gt;Created: 2015-01-30
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="" package="WE-PDA_1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7847709010">
<attribute name="WE-NUMBER" value="7847709010/1uH"/>
</technology>
<technology name="_7847709022">
<attribute name="WE-NUMBER" value="7847709022/2,2uH"/>
</technology>
<technology name="_7847709033">
<attribute name="WE-NUMBER" value="7847709033/3,3uH"/>
</technology>
<technology name="_7847709047">
<attribute name="WE-NUMBER" value="7847709047/4,7uH"/>
</technology>
<technology name="_7847709068">
<attribute name="WE-NUMBER" value="7847709068/6,8uH"/>
</technology>
<technology name="_7847709100">
<attribute name="WE-NUMBER" value="7847709100/10uH"/>
</technology>
<technology name="_7847709101">
<attribute name="WE-NUMBER" value="7847709101/100uH"/>
</technology>
<technology name="_7847709102">
<attribute name="WE-NUMBER" value="7847709102/1000uH"/>
</technology>
<technology name="_7847709220">
<attribute name="WE-NUMBER" value="7847709220/22uH"/>
</technology>
<technology name="_7847709221">
<attribute name="WE-NUMBER" value="7847709221/220uH"/>
</technology>
<technology name="_7847709330">
<attribute name="WE-NUMBER" value="7847709330/33uH"/>
</technology>
<technology name="_7847709331">
<attribute name="WE-NUMBER" value="7847709331/330uH"/>
</technology>
<technology name="_7847709470">
<attribute name="WE-NUMBER" value="7847709470/47uH"/>
</technology>
<technology name="_7847709471">
<attribute name="WE-NUMBER" value="7847709471/470uH"/>
</technology>
<technology name="_7847709680">
<attribute name="WE-NUMBER" value="7847709680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDF_1045" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Flatwire Power Inductor
&lt;br&gt; 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Core material: NiZn
&lt;br&gt;
&lt;br&gt; Flat wire power inductor
&lt;br&gt;
&lt;br&gt; Advanced operating temperature: –40 °C up to +150 °C
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;br&gt; Low self-losses
&lt;br&gt;
&lt;br&gt; High saturation current
&lt;br&gt;
&lt;br&gt; Flat wire coil for lower losses at high frequency ranges
&lt;br&gt;
&lt;br&gt; High Self Resonance Frequency
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Suitable for high frequency switching regulators
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PDF%20Gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PDF%20Gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PDF?"&gt;http://katalog.we-online.de/en/pbs/WE-PDF?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PDF">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447797022">
<attribute name="WE-NUMBER" value="7447797022/0,22uH"/>
</technology>
<technology name="_7447797050">
<attribute name="WE-NUMBER" value="7447797050/0,5uH"/>
</technology>
<technology name="_7447797110">
<attribute name="WE-NUMBER" value="7447797110/1,1uH"/>
</technology>
<technology name="_7447797180">
<attribute name="WE-NUMBER" value="7447797180/1,8uH"/>
</technology>
<technology name="_7447797250">
<attribute name="WE-NUMBER" value="7447797250/2,5uH"/>
</technology>
<technology name="_7447797360">
<attribute name="WE-NUMBER" value="7447797360/3,6uH"/>
</technology>
<technology name="_7447797470">
<attribute name="WE-NUMBER" value="7447797470/4,7uH"/>
</technology>
<technology name="_7447797620">
<attribute name="WE-NUMBER" value="7447797620/6,2uH"/>
</technology>
<technology name="_7447797820">
<attribute name="WE-NUMBER" value="7447797820/8,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_HV_1210" prefix="L" uservalue="yes">
<description>&lt;b&gt;High Voltage SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Shielded part for ideal wire protection
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Magnetically schielded
&lt;br&gt;
&lt;br&gt; Designed for 400 VDC Applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Non-isolated buck or buck-boost converter like Power Integrations LinkSwitch-TN
&lt;br&gt;
&lt;br&gt; Constant current LED driver
&lt;br&gt;
&lt;br&gt; Utility metering
&lt;br&gt;
&lt;br&gt; Filter for power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD_HV.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD_HV.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD_HV?"&gt;http://katalog.we-online.de/en/pbs/WE-PD_HV?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD_1260/1245/1280/1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7687709102">
<attribute name="WE-NUMBER" value="7687709102/1000uH"/>
</technology>
<technology name="_7687709152">
<attribute name="WE-NUMBER" value="7687709152/1500uH"/>
</technology>
<technology name="_7687709221">
<attribute name="WE-NUMBER" value="7687709221/220uH"/>
</technology>
<technology name="_7687709222">
<attribute name="WE-NUMBER" value="7687709222/2200uH"/>
</technology>
<technology name="_7687709332">
<attribute name="WE-NUMBER" value="7687709332/3300uH"/>
</technology>
<technology name="_7687709471">
<attribute name="WE-NUMBER" value="7687709471/470uH"/>
</technology>
<technology name="_7687709681">
<attribute name="WE-NUMBER" value="7687709681/680uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PF_1280" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD EMI Suppression Power Ferrite
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Suitable for applications with high currents up to 10 A
&lt;br&gt;
&lt;br&gt; Magnetically shielded version
&lt;br&gt;
&lt;br&gt; Core material NiZn for the use in a wide frequency range
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Interference suppression in motors
&lt;br&gt;
&lt;br&gt; Switch mode power supply
&lt;br&gt;
&lt;br&gt; Power electronics
&lt;br&gt;
&lt;br&gt; PWM controller
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PF.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PF.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PF?"&gt;http://katalog.we-online.de/en/pbs/WE-PF?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="" package="WE-PF_7427929XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742792901"/>
<technology name="_742792902"/>
<technology name="_742792903"/>
<technology name="_742792904"/>
<technology name="_742792906"/>
<technology name="_742792907"/>
<technology name="_742792910"/>
<technology name="_7427929112"/>
<technology name="_7427929115"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PFC" prefix="T" uservalue="yes">
<description>&lt;b&gt;PFC Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; PFC choke for power up to 250 W
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; PQ 38/11 construction height &lt;10 mm above PCB
&lt;br&gt;
&lt;br&gt; Auxiliary winding
&lt;br&gt;
&lt;br&gt; RF strand for low losses due to skin and proximity effects
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Active Power Factor correction
&lt;br&gt;
&lt;br&gt; For all ICs CPU PFC ON Semiconductor
&lt;br&gt;
&lt;br&gt; Lighting applications
&lt;br&gt;
&lt;br&gt; Switchmode power supplies
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PFC.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PFC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PFC?"&gt;http://katalog.we-online.de/en/pbs/WE-PFC?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="_760803200" package="WE_EER28_THT_HORIZONTAL_9PIN">
<connects>
<connect gate="G$1" pin="1" pad="9"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760800080" package="WE_EE20/10/6_THT_HORIZONTAL_10PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="10"/>
<connect gate="G$1" pin="3" pad="9"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760801130" package="WE_RM10_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760801030" package="WE_RM10_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760801020" package="WE_RM10_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760802112" package="WE_RM10_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760804110" package="WE_RM10_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760802122" package="WE_RM12_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760804310" package="WE_RM12_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760805210" package="WE_RM12_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760806200" package="WE_RM12_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760805410" package="WE_RM14_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760806400" package="WE_RM14_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760801031" package="WE_EFD25_THT_HORIZONTAL_10PIN">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="9"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760801131" package="WE_EFD30_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="11"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760801021" package="WE_EFD30_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="11"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760802113" package="WE_EFD30_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="11"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760804111" package="WE_EFD30_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="11"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760805211" package="WE_EFD30_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="11"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760806201" package="WE_EFD30_THT_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="11"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760806302" package="WE_PQ38/11_6PIN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMI_1210" prefix="L" uservalue="yes">
<description>&lt;b&gt;Power Multilayer Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact multilayer type
&lt;br&gt;
&lt;br&gt; Suitable for applications with high currents up to 2.7 A
&lt;br&gt;
&lt;br&gt; Smallest RDC-Values starting at 40 mΩ
&lt;br&gt;
&lt;br&gt; Magnetically shielded construction: No crosstalk
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Available in four sizes and three different types (Low Profile, Low RDC &amp; High Saturation Current)
&lt;br&gt;
&lt;br&gt; Recommended soldering profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;
&lt;br&gt; Electronic devices with very low profile
&lt;br&gt;
&lt;br&gt; Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMI?"&gt;http://katalog.we-online.de/en/pbs/WE-PMI?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMI_1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479897122">
<attribute name="WE-NUMBER" value="74479897122/0,22uH"/>
</technology>
<technology name="_74479897150">
<attribute name="WE-NUMBER" value="74479897150/0,5uH"/>
</technology>
<technology name="_74479899111">
<attribute name="WE-NUMBER" value="74479899111/0,11uH"/>
</technology>
<technology name="_74479899130">
<attribute name="WE-NUMBER" value="74479899130/0,3uH"/>
</technology>
<technology name="_74479899150">
<attribute name="WE-NUMBER" value="74479899150/0,5uH"/>
</technology>
<technology name="_74479899210">
<attribute name="WE-NUMBER" value="74479899210/1uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-POE_EFD15" prefix="T" uservalue="yes">
<description>&lt;b&gt;Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Flyback transformer designed for PoE PDs
&lt;br&gt;
&lt;br&gt; Input voltage: 36 V to 57 V
&lt;br&gt;
&lt;br&gt; Switching frequencies: 200–500 kHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Insulation test voltage: 1.5 kVAC/1 min
&lt;br&gt;
&lt;br&gt; Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Suitable for PoE IC’s like LTC4267, TPS 23750, TPS 23770, LM5070, LM 5071, LM 5072
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-poe_uebertrager_power_over_ethernet.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-poe_uebertrager_power_over_ethernet.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PoE?"&gt;http://katalog.we-online.de/en/pbs/WE-PoE?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE"/>
</gates>
<devices>
<device name="" package="WE_EFD15_SMD_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="9"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="5" pad="12"/>
<connect gate="G$1" pin="6" pad="7"/>
<connect gate="G$1" pin="7" pad="11"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="10"/>
</connects>
<technologies>
<technology name="_749119318"/>
<technology name="_749119333"/>
<technology name="_749119350"/>
<technology name="_7491193912"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-POE+_EFD20" prefix="T" uservalue="yes">
<description>&lt;b&gt;Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 25 W PoE+ requirements of IEEE802.3at
&lt;br&gt;
&lt;br&gt; Frequency range: 250–400 kHz
&lt;br&gt;
&lt;br&gt; Input voltage range: 36–72 V
&lt;br&gt;
&lt;br&gt; 1.5 kV Hipot test between primary and secondary
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE+ powered devices
&lt;br&gt;
&lt;br&gt; IP phones
&lt;br&gt;
&lt;br&gt; WLAN-Access points
&lt;br&gt;
&lt;br&gt; Security cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-POE+.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-POE+.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-POE-PLUS?m"&gt;http://katalog.we-online.de/en/pbs/WE-POE-PLUS?m&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE_EFD20_SMD_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="2" pad="10 11 12"/>
<connect gate="G$1" pin="3" pad="7 8 9"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="3 4"/>
</connects>
<technologies>
<technology name="_749119433"/>
<technology name="_749119450"/>
<technology name="_7491194501"/>
<technology name="_7491194912"/>
<technology name="_750310925"/>
<technology name="_750310926"/>
<technology name="_750310927"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-POE+_EP13" prefix="T" uservalue="yes">
<description>&lt;b&gt;Power over Ethernet Plus Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Designed to meet 25 W PoE+ requirements of IEEE802.3at
&lt;br&gt;
&lt;br&gt; Frequency range: 250–400 kHz
&lt;br&gt;
&lt;br&gt; Input voltage range: 36–72 V
&lt;br&gt;
&lt;br&gt; 1.5 kV Hipot test between primary and secondary
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE+ powered devices
&lt;br&gt;
&lt;br&gt; IP phones
&lt;br&gt;
&lt;br&gt; WLAN-Access points
&lt;br&gt;
&lt;br&gt; Security cameras
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-POE+.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-POE+.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-POE-PLUS?m"&gt;http://katalog.we-online.de/en/pbs/WE-POE-PLUS?m&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-POE+_EP13">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6 7"/>
<connect gate="G$1" pin="3" pad="9 10"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="3"/>
</connects>
<technologies>
<technology name="_750310742"/>
<technology name="_750310743"/>
<technology name="_750310744"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-POE_EP10" prefix="T" uservalue="yes">
<description>&lt;b&gt;Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Flyback transformer designed for PoE PDs
&lt;br&gt;
&lt;br&gt; Input voltage: 36 V to 57 V
&lt;br&gt;
&lt;br&gt; Switching frequencies: 200–500 kHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Insulation test voltage: 1.5 kVAC/1 min
&lt;br&gt;
&lt;br&gt; Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Suitable for PoE IC’s like LTC4267, TPS 23750, TPS 23770, LM5070, LM 5071, LM 5072
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-poe_uebertrager_power_over_ethernet.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-poe_uebertrager_power_over_ethernet.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PoE?"&gt;http://katalog.we-online.de/en/pbs/WE-PoE?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_1W:1W"/>
</gates>
<devices>
<device name="" package="WE_EP10_SMD_8PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="5 6"/>
<connect gate="G$1" pin="3" pad="7 8"/>
<connect gate="G$1" pin="6" pad="4"/>
</connects>
<technologies>
<technology name="_750310062"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-POE_EP13" prefix="T" uservalue="yes">
<description>&lt;b&gt;Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Flyback transformer designed for PoE PDs
&lt;br&gt;
&lt;br&gt; Input voltage: 36 V to 57 V
&lt;br&gt;
&lt;br&gt; Switching frequencies: 200–500 kHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Insulation test voltage: 1.5 kVAC/1 min
&lt;br&gt;
&lt;br&gt; Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Suitable for PoE IC’s like LTC4267, TPS 23750, TPS 23770, LM5070, LM 5071, LM 5072
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-poe_uebertrager_power_over_ethernet.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-poe_uebertrager_power_over_ethernet.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PoE?"&gt;http://katalog.we-online.de/en/pbs/WE-PoE?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-POE_EP13">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="4" pad="8"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="1"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="4"/>
</connects>
<technologies>
<technology name="_7491199112"/>
<technology name="_7491199212"/>
<technology name="_7491199312"/>
<technology name="_749119933"/>
<technology name="_7491199331"/>
<technology name="_7491199332"/>
<technology name="_749119950"/>
<technology name="_7491199501"/>
<technology name="_750310013"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RFH_1008A" prefix="L" uservalue="yes">
<description>&lt;b&gt; Ferrite SMD Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High thermal stability
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;
&lt;br&gt; High inductances
&lt;br&gt;
&lt;br&gt; High currents
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Developed especially for RF applications
&lt;br&gt;
&lt;br&gt; Perfect for telecommunication applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RFH.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RFH.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-RFH?"&gt;http://katalog.we-online.de/en/pbs/WE-RFH?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="" package="WE-RFH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744758256A">
<attribute name="WE-NUMBER" value="744758256A/0,56uH"/>
</technology>
<technology name="_744758282A">
<attribute name="WE-NUMBER" value="744758282A/0,82uH"/>
</technology>
<technology name="_744758310A">
<attribute name="WE-NUMBER" value="744728310A/1uH"/>
</technology>
<technology name="_744758312A">
<attribute name="WE-NUMBER" value="744758312A/1,2uH"/>
</technology>
<technology name="_744758315A">
<attribute name="WE-NUMBER" value="744758315A/1,5uH"/>
</technology>
<technology name="_744758318A">
<attribute name="WE-NUMBER" value="744758318A/1,8uH"/>
</technology>
<technology name="_744758322A">
<attribute name="WE-NUMBER" value="744758322A/2,2uH"/>
</technology>
<technology name="_744758327A">
<attribute name="WE-NUMBER" value="744758327A/2,7uH"/>
</technology>
<technology name="_744758333A">
<attribute name="WE-NUMBER" value="744728333A/3,3uH"/>
</technology>
<technology name="_744758339A">
<attribute name="WE-NUMBER" value="744758339A/3,9uH"/>
</technology>
<technology name="_744758347A">
<attribute name="WE-NUMBER" value="744758347A/4,7uH"/>
</technology>
<technology name="_744758356A">
<attribute name="WE-NUMBER" value="744758356A/5,6uH"/>
</technology>
<technology name="_744758368A">
<attribute name="WE-NUMBER" value="744758368A/6,8uH"/>
</technology>
<technology name="_744758382A">
<attribute name="WE-NUMBER" value="744758382A/8,2uH"/>
</technology>
<technology name="_744758410A">
<attribute name="WE-NUMBER" value="744728410A/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RFI_0805A" prefix="L" uservalue="yes">
<description>&lt;b&gt;Ferrite SMD Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High thermal stability
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +85 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Especially developed for RF applications
&lt;br&gt;
&lt;br&gt; RFID
&lt;br&gt;
&lt;br&gt; Low frequency radio applications (Keyless)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RFI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RFI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-RFI?"&gt;http://katalog.we-online.de/en/pbs/WE-RFI?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="" package="WE-RFI_0805A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744760247A">
<attribute name="WE-NUMBER" value="744760247A/0,47uH"/>
</technology>
<technology name="_744760256A">
<attribute name="WE-NUMBER" value="744760256A/0,56uH"/>
</technology>
<technology name="_744760268A">
<attribute name="WE-NUMBER" value="744760268A/0,68uH"/>
</technology>
<technology name="_744760282A">
<attribute name="WE-NUMBER" value="744760282A/0,82uH"/>
</technology>
<technology name="_744760310A">
<attribute name="WE-NUMBER" value="744760310A/1uH"/>
</technology>
<technology name="_744760312A">
<attribute name="WE-NUMBER" value="744760312A/1,2uH"/>
</technology>
<technology name="_744760315A">
<attribute name="WE-NUMBER" value="744760315A/1,5uH"/>
</technology>
<technology name="_744760318A">
<attribute name="WE-NUMBER" value="744760318A/1,8uH"/>
</technology>
<technology name="_744760322A">
<attribute name="WE-NUMBER" value="744760322A/2,2uH"/>
</technology>
<technology name="_744760327A">
<attribute name="WE-NUMBER" value="744760327A/2,7uH"/>
</technology>
<technology name="_744760333A">
<attribute name="WE-NUMBER" value="744760333A/3,3uH"/>
</technology>
<technology name="_744760339A">
<attribute name="WE-NUMBER" value="744760339A/3,9uH"/>
</technology>
<technology name="_744760347A">
<attribute name="WE-NUMBER" value="744760347A/4,7uH"/>
</technology>
<technology name="_744760356A">
<attribute name="WE-NUMBER" value="744760356A/5,6uH"/>
</technology>
<technology name="_744760382A">
<attribute name="WE-NUMBER" value="744760382A/8,2uH"/>
</technology>
<technology name="_744760410A">
<attribute name="WE-NUMBER" value="744760410A/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499111121A" prefix="T" uservalue="yes">
<description>&lt;b&gt; RJ45 LAN Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; RJ45 connector with integrated transformer common mode choke
&lt;br&gt;
&lt;br&gt; Available in SMD, THT and THT with USB
&lt;br&gt;
&lt;br&gt; 350 μH min. OCL with 8 mA bias
&lt;br&gt;
&lt;br&gt; Complies with IEEE 802.3
&lt;br&gt;
&lt;br&gt; Extended temperature range from –40 °C to +85 °C available
&lt;br&gt;
&lt;br&gt; PoE/PoE+
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; XDSL Modems
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; LAN network applications
&lt;br&gt;
&lt;br&gt; Hub, Router, Switches
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499010441?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499010441?&lt;/a&gt;&lt;p&gt;



&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7499111121A"/>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
</gates>
<devices>
<device name="" package="7499111121A">
<connects>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="13"/>
<connect gate="LED-GREEN" pin="K" pad="14"/>
<connect gate="LED-YELLOW" pin="A" pad="11"/>
<connect gate="LED-YELLOW" pin="K" pad="12"/>
<connect gate="RJ45LAN" pin="1" pad="1"/>
<connect gate="RJ45LAN" pin="10" pad="10"/>
<connect gate="RJ45LAN" pin="2" pad="2"/>
<connect gate="RJ45LAN" pin="3" pad="3"/>
<connect gate="RJ45LAN" pin="4" pad="4"/>
<connect gate="RJ45LAN" pin="5" pad="5"/>
<connect gate="RJ45LAN" pin="6" pad="6"/>
<connect gate="RJ45LAN" pin="7" pad="7"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499111121A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SCC_1260" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Common Mode Line Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Enormous common mode impedance Z
&lt;br&gt;
&lt;br&gt; Small dimensions
&lt;br&gt;
&lt;br&gt; High current ratings
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Attenuation of common mode noise
&lt;br&gt;
&lt;br&gt; Power supplies
&lt;br&gt;
&lt;br&gt; Data lines
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;&lt;a href=&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSCC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndSCC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SCC?"&gt;http://katalog.we-online.de/en/pbs/WE-SCC?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SCC"/>
</gates>
<devices>
<device name="" package="WE-SCC_1260/1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744282010"/>
<technology name="_744282100"/>
<technology name="_744282101"/>
<technology name="_744282102"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SD" prefix="L" uservalue="yes">
<description>&lt;b&gt;Rod Core Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Rated current up to 15 A
&lt;br&gt;
&lt;br&gt; Inductance is independent from rated DC current
&lt;br&gt;
&lt;br&gt; High mechanical stability
&lt;br&gt;
&lt;br&gt; High saturation currents
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +150 ºC
&lt;br&gt;
&lt;br&gt; Custom designs on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switching regulators
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; Motors
&lt;br&gt;
&lt;br&gt; Power amplifiers
&lt;br&gt;
&lt;br&gt; Power supplies
&lt;br&gt;
&lt;br&gt; Broadband filtering
&lt;br&gt;
&lt;br&gt; Typical in VHF
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;&lt;a href=&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSD_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndSD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SD?"&gt;http://katalog.we-online.de/en/pbs/WE-SD?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="_744710203" package="WE-SD_744710203">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744710203/2uH"/>
</technology>
</technologies>
</device>
<device name="_744710205" package="WE-SD_744710205">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744710205/2uH"/>
</technology>
</technologies>
</device>
<device name="_744710210" package="WE-SD_744710210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744710210/2uH"/>
</technology>
</technologies>
</device>
<device name="_744710215" package="WE-SD_744710215">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744710215/2uH"/>
</technology>
</technologies>
</device>
<device name="_744710603" package="WE-SD_744710603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744710603/6uH"/>
</technology>
</technologies>
</device>
<device name="_744710605" package="WE-SD_744710605">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744710605/6uH"/>
</technology>
</technologies>
</device>
<device name="_744710610" package="WE-SD_744710610">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744710610/6uH"/>
</technology>
</technologies>
</device>
<device name="_744710615" package="WE-SD_744710615">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744710615/6uH"/>
</technology>
</technologies>
</device>
<device name="_744711003" package="WE-SD_744711003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744711003/10uH"/>
</technology>
</technologies>
</device>
<device name="_744711005" package="WE-SD_744711005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744711005/10uH"/>
</technology>
</technologies>
</device>
<device name="_744711010" package="WE-SD_744711010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744711010/10uH"/>
</technology>
</technologies>
</device>
<device name="_744711015" package="WE-SD_744711015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744711015/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SECF" prefix="SECF" uservalue="yes">
<description>&lt;b&gt; SMD EMI Contact Finger
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Material: Copper Beryllium (CuBe) gold-plated (AU)
&lt;br&gt;
&lt;br&gt; Corrosion resistant
&lt;br&gt;
&lt;br&gt; Wear resistant
&lt;br&gt;
&lt;br&gt; High temperatures and mechanical weight have no influence on the excellent connection properties
&lt;br&gt;
&lt;br&gt; Reliable solderability
&lt;br&gt;
&lt;br&gt; Tape &amp; reel packaging
&lt;br&gt;
&lt;br&gt; Perfectly suited for automated placement
&lt;br&gt;
&lt;br&gt; Different types and sizes available
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Contact between PCB's ground and housing
&lt;br&gt;
&lt;br&gt; Low impedance RF connection between PCBs and/or PCB and metal case
&lt;br&gt;
&lt;br&gt;

&lt;/b&gt;&lt;br&gt;&lt;a href=&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-SECF.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-SECF.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SECF?"&gt;http://katalog.we-online.de/en/pbs/WE-SECF?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-15&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="GNDPIN"/>
</gates>
<devices>
<device name="_331051472057" package="WE-SECF-0557">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_331151702562" package="WE-SECF-1562">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_331011452048" package="WE-SECF_0148">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_331031321515" package="WE-SECF_0315">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_331031271520" package="WE-SECF_0320">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_331041402053" package="WE-SECF_0453">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_331061603010" package="WE-SECF_0610">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Otto"/>
<attribute name="CREATED-DATE" value="MAR 2013"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/pbs/datasheet/331061603010.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name="_331081302025" package="WE-SECF_0825">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_331141352540" package="WE-SECF_1440">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_331161702513" package="WE-SECF_1613">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_331161452070" package="WE-SECF_1670">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_331171302030" package="WE-SECF_1730">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_331171302035" package="WE-SECF_1735">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_331211503040" package="WE-SECF_2140">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_331221602040" package="WE-SECF_2240">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_331011452535" package="WE-SECF_0135">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SHC" prefix="SHC" uservalue="yes">
<description>&lt;b&gt; Shielding Cabinet
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Tin plate in accordance with DIN EN 10202/10203
&lt;br&gt;
&lt;br&gt; Shielding effectiveness up to 55 dB
&lt;br&gt;
&lt;br&gt; Two-part case consisting of a solderable grid frame (SMD/THT) and a removable cover
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; To prevent EMI radiation from PCB and to keep sensitivity low of:  
&lt;br&gt; - RF output stages
&lt;br&gt; - RF input and amplifier stages;
&lt;br&gt; - Oscillators
&lt;br&gt; - EMC sensitive parts in plastic cases
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;&lt;a href=&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_SHC_S1610002x.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_SHC_S1610002x.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SHC?m"&gt;http://katalog.we-online.de/en/pbs/WE-SHC?m&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SHC"/>
</gates>
<devices>
<device name="_36103205" package="WE-SHC_36103205">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36103255" package="WE-SHC_36103255">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36103305" package="WE-SHC_36103305">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36103505" package="WE-SHC_36103505">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36103605" package="WE-SHC_36103605">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 49"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36503205" package="WE-SHC_36503205">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 9 10 11 12 13 14 15 16 17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36503255" package="WE-SHC_36503255">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36503305" package="WE-SHC_36503305">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36503505" package="WE-SHC_36503505">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 40 41 42 43 44 45 47 48 49 50 56"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36503605" package="WE-SHC_36503605">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36103205S" package="WE-SHC_36103205S">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36105266S" package="WE-SHC_36105266S">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36105366S" package="WE-SHC_36105366S">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36106326S" package="WE-SHC_36106326S">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36107406S" package="WE-SHC_36107406S">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36903205S" package="WE-SHC_36903205S">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36903255S" package="WE-SHC_36903255S">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36903305S" package="WE-SHC_36903305S">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36905266S" package="WE-SHC_36905266S">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36906326S" package="WE-SHC_36906326S">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_36907406S" package="WE-SHC_36907406S">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_3690103020" package="WE-SHC_369010302X">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_3690103021" package="WE-SHC_369010302X">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_3690103022" package="WE-SHC_369010302X">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_3690103023" package="WE-SHC_369010302X">
<connects>
<connect gate="G$1" pin="GND" pad="1 2 3 4 5 6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SI" prefix="L" uservalue="yes">
<description>&lt;br&gt; Leaded Toroidal Storage Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low magnetic stray field
&lt;br&gt;
&lt;br&gt; Low leakage and minimal noise because of the toroidal core made of iron powder
&lt;br&gt;
&lt;br&gt; Available for rated currents 0.5 A, 1 A, 3 A and 5 A
&lt;br&gt;
&lt;br&gt; Custom designs on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfectly suitable for switching regulators from
&lt;br&gt; – Texas Instruments (LM)
&lt;br&gt; – Linear Technology (LT)
&lt;br&gt;– Maxim
&lt;br&gt;
&lt;br&gt; Used for example in switching power supplies and voltage transformers
&lt;br&gt;
&lt;br&gt; Switching regulators up to 100 kHz
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndSI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SI/744101"&gt;http://katalog.we-online.de/en/pbs/WE-SI/744101&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-06-10&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="_744101" package="WE-SI_744101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744101/50uH"/>
</technology>
</technologies>
</device>
<device name="_744102" package="WE-SI_744102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744102/73uH"/>
</technology>
</technologies>
</device>
<device name="_744103" package="WE-SI_744103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744103/109uH"/>
</technology>
</technologies>
</device>
<device name="_744104" package="WE-SI_744104">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744104/167uH"/>
</technology>
</technologies>
</device>
<device name="_744105" package="WE-SI_744105">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744105/258uH"/>
</technology>
</technologies>
</device>
<device name="_744106" package="WE-SI_744106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744106/393uH"/>
</technology>
</technologies>
</device>
<device name="_744107" package="WE-SI_744107">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744107/557uH"/>
</technology>
</technologies>
</device>
<device name="_744111" package="WE-SI_744111">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744111/37uH"/>
</technology>
</technologies>
</device>
<device name="_7441110" package="WE-SI_7441110">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7441110/1619uH"/>
</technology>
</technologies>
</device>
<device name="_744112" package="WE-SI_744112">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744112/53uH"/>
</technology>
</technologies>
</device>
<device name="_744113" package="WE-SI_744113">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744113/80uH"/>
</technology>
</technologies>
</device>
<device name="_744114" package="WE-SI_744114">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744114/127uH"/>
</technology>
</technologies>
</device>
<device name="_744115" package="WE-SI_744115">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744115/200uH"/>
</technology>
</technologies>
</device>
<device name="_744116" package="WE-SI_744116">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744116/345uH"/>
</technology>
</technologies>
</device>
<device name="_744117" package="WE-SI_744117">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744117/390uH"/>
</technology>
</technologies>
</device>
<device name="_744118" package="WE-SI_744118">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744118/600uH"/>
</technology>
</technologies>
</device>
<device name="_744119" package="WE-SI_744119">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744119/890uH"/>
</technology>
</technologies>
</device>
<device name="_744131" package="WE-SI_744131">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744131/34uH"/>
</technology>
</technologies>
</device>
<device name="_744132" package="WE-SI_744132">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744132/49uH"/>
</technology>
</technologies>
</device>
<device name="_744133" package="WE-SI_744133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744133/75uH"/>
</technology>
</technologies>
</device>
<device name="_744134" package="WE-SI_744134">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744134/92uH"/>
</technology>
</technologies>
</device>
<device name="_744135" package="WE-SI_744135">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744135/157uH"/>
</technology>
</technologies>
</device>
<device name="_744136" package="WE-SI_744136">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744136/346uH"/>
</technology>
</technologies>
</device>
<device name="_744137" package="WE-SI_744137">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744137/630uH"/>
</technology>
</technologies>
</device>
<device name="_744138" package="WE-SI_744138">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744138/727uH"/>
</technology>
</technologies>
</device>
<device name="_744139" package="WE-SI_744139">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744139/1124uH"/>
</technology>
</technologies>
</device>
<device name="_744150" package="WE-SI_744150">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744150/26uH"/>
</technology>
</technologies>
</device>
<device name="_7441501" package="WE-SI_7441501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7441510/12uH"/>
</technology>
</technologies>
</device>
<device name="_744151" package="WE-SI_744151">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744151/48uH"/>
</technology>
</technologies>
</device>
<device name="_744152" package="WE-SI_744152">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744152/82uH"/>
</technology>
</technologies>
</device>
<device name="_744153" package="WE-SI_744153">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744153/137uH"/>
</technology>
</technologies>
</device>
<device name="_744154" package="WE-SI_744154">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744154/172uH"/>
</technology>
</technologies>
</device>
<device name="_744155" package="WE-SI_744155">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744155/220uH"/>
</technology>
</technologies>
</device>
<device name="_744156" package="WE-SI_744156">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744156/380uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SL1" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Common Mode Line Filter WE-SL1&lt;/b&gt;&lt;p&gt;
- Small size&lt;br&gt; 
- Low Profile, only 1,65 mm&lt;br&gt;
- High Impedance up to 2000 ohm&lt;br&gt;
- High Current up to 300mA &lt;br&gt;
- Low leakage inductance&lt;br&gt;&lt;br&gt;

-- USB&lt;br&gt;
-- CAN&lt;br&gt;
-- Firewire&lt;br&gt;
-- Data Lines&lt;br&gt;
-- Power Lines&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSL1_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndSL1_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SL1?"&gt;http://katalog.we-online.de/en/pbs/WE-SL1?1&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-SL1">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_744212100">
<attribute name="WE-NUMBER" value="744212100/10uH"/>
</technology>
<technology name="_744212101">
<attribute name="WE-NUMBER" value="744212101/100uH"/>
</technology>
<technology name="_744212181">
<attribute name="WE-NUMBER" value="744212181/180uH"/>
</technology>
<technology name="_744212221">
<attribute name="WE-NUMBER" value="744212221/220uH"/>
</technology>
<technology name="_744212331">
<attribute name="WE-NUMBER" value="744212331/330uH"/>
</technology>
<technology name="_744212470">
<attribute name="WE-NUMBER" value="744212470/47uH"/>
</technology>
<technology name="_744212510">
<attribute name="WE-NUMBER" value="744212510/51uH"/>
</technology>
<technology name="_744212820">
<attribute name="WE-NUMBER" value="744212820/82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SL2" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Common-Mode Line Filter WE-SL2&lt;/b&gt;&lt;p&gt;

For distortion-free removal of noise from transmitted 
electrical signals&lt;br&gt;
- Double current-compensated choke&lt;br&gt;
- Offering a wide band width with the core materials NiZn/MnZn&lt;br&gt;&lt;br&gt;

-- Current compensated choke for data and signal lines&lt;br&gt;
-- Power supply systems&lt;br&gt;
-- Filter for measurement signals&lt;br&gt;
-- CAN


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSL2_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndSL2_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SL2?"&gt;http://katalog.we-online.de/en/pbs/WE-SL2?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-SL2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_744220">
<attribute name="WE-NUMBER" value="744220/4700uH"/>
</technology>
<technology name="_744220103">
<attribute name="WE-NUMBER" value="744220103/10000uH"/>
</technology>
<technology name="_744220203">
<attribute name="WE-NUMBER" value="744220203/20000uH"/>
</technology>
<technology name="_744221">
<attribute name="WE-NUMBER" value="744221/2000uH"/>
</technology>
<technology name="_744222">
<attribute name="WE-NUMBER" value="744222/1000uH"/>
</technology>
<technology name="_744223">
<attribute name="WE-NUMBER" value="744223/500uH"/>
</technology>
<technology name="_744224">
<attribute name="WE-NUMBER" value="744224/250uH"/>
</technology>
<technology name="_744225">
<attribute name="WE-NUMBER" value="744225/40uH"/>
</technology>
<technology name="_744225S">
<attribute name="WE-NUMBER" value="744225S/40uH"/>
</technology>
<technology name="_744226">
<attribute name="WE-NUMBER" value="744226/10uH"/>
</technology>
<technology name="_744226S">
<attribute name="WE-NUMBER" value="744226S/10uH"/>
</technology>
<technology name="_744227">
<attribute name="WE-NUMBER" value="744227/51uH"/>
</technology>
<technology name="_744227S">
<attribute name="WE-NUMBER" value="744227S/51uH"/>
</technology>
<technology name="_744228">
<attribute name="WE-NUMBER" value="744228/25uH"/>
</technology>
<technology name="_744228S">
<attribute name="WE-NUMBER" value="744228S/25uH"/>
</technology>
<technology name="_744229">
<attribute name="WE-NUMBER" value="744229/6500uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SL3_744252XXX" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Common Mode Line Filter WE-SL3&lt;/b&gt;&lt;p&gt;
- Small size&lt;br&gt; - Low Profile, only 2.5 mm&lt;br&gt;- High Impedance tp to 5000 ohm&lt;br&gt;- High Current up to 700mA &lt;br&gt;
- Low leakage inductance&lt;p&gt;
- USB&lt;br&gt;
- CAN&lt;br&gt;
-  Firewire&lt;br&gt;
- Data Lines&lt;br&gt;
- Power Lines&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSL3_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndSL3_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SL3?"&gt;http://katalog.we-online.de/en/pbs/WE-SL3?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-SL3_744252XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="3"/>
</connects>
<technologies>
<technology name="_744252101">
<attribute name="WE-NUMBER" value="744252101/100uH"/>
</technology>
<technology name="_744252220">
<attribute name="WE-NUMBER" value="744252220/22uH"/>
</technology>
<technology name="_744252510">
<attribute name="WE-NUMBER" value="744252510/51uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SL3_744253XXX" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Common Mode Line Filter WE-SL3&lt;/b&gt;&lt;p&gt;
- Small size&lt;br&gt; - Low Profile, only 2.5 mm&lt;br&gt;- High Impedance tp to 5000 ohm&lt;br&gt;- High Current up to 700mA &lt;br&gt;
- Low leakage inductance&lt;p&gt;
- USB&lt;br&gt;
- CAN&lt;br&gt;
-  Firewire&lt;br&gt;
- Data Lines&lt;br&gt;
- Power Lines&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSL3_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndSL3_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SL3?"&gt;http://katalog.we-online.de/en/pbs/WE-SL3?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="3L"/>
</gates>
<devices>
<device name="" package="WE-SL3_744253XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="_744253101">
<attribute name="WE-NUMBER" value="744253101/100uH"/>
</technology>
<technology name="_744253200">
<attribute name="WE-NUMBER" value="744253200/20uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SL5" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Common Mode Line Filter WE-SL5&lt;/b&gt;&lt;p&gt;
- Small size&lt;br&gt;
- Low Profile&lt;br&gt;
- High Impedance up to 13000 ohm&lt;br&gt;
- High Current up to 2500mA &lt;P&gt;

-- Data Lines&lt;br&gt;
-- Power Lines



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSL5_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndSL5_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SL5?"&gt;http://katalog.we-online.de/en/pbs/WE-SL5?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-SL5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744272102">
<attribute name="WE-NUMBER" value="744272102/1000uH"/>
</technology>
<technology name="_744272121">
<attribute name="WE-NUMBER" value="744272121/120uH"/>
</technology>
<technology name="_744272221">
<attribute name="WE-NUMBER" value="744272221/220uH"/>
</technology>
<technology name="_744272222">
<attribute name="WE-NUMBER" value="744272222/2200uH"/>
</technology>
<technology name="_744272251">
<attribute name="WE-NUMBER" value="744272251/250uH"/>
</technology>
<technology name="_744272332">
<attribute name="WE-NUMBER" value="744272332/3300uH"/>
</technology>
<technology name="_744272392">
<attribute name="WE-NUMBER" value="744272392/3900uH"/>
</technology>
<technology name="_744272471">
<attribute name="WE-NUMBER" value="744272471/470uH"/>
</technology>
<technology name="_744272472">
<attribute name="WE-NUMBER" value="744272472/4700uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SL5_HC" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Common Mode WE-SL5&lt;/b&gt;&lt;p&gt;
- Small size&lt;br&gt;
- Low Profile&lt;br&gt;
- High Impedance up to 1000 ohm&lt;br&gt;
- High Current up to 5000mA &lt;P&gt;

-- Data Lines&lt;br&gt;
-- Power Lines



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSL5HC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndSL5_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SL5_HC?"&gt;http://katalog.we-online.de/en/pbs/WE-SL5_HC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-SL5_HC">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_744273102">
<attribute name="WE-NUMBER" value="744273102/11uH"/>
</technology>
<technology name="_744273222">
<attribute name="WE-NUMBER" value="744273222/30uH"/>
</technology>
<technology name="_744273501">
<attribute name="WE-NUMBER" value="744273501/5uH"/>
</technology>
<technology name="_744273801">
<attribute name="WE-NUMBER" value="744273801/9uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SLIM_LEP28" prefix="T" uservalue="yes">
<description>&lt;b&gt;Slim-Transformer WE-SLIM&lt;/b&gt;&lt;br&gt;&lt;br&gt;

- total hight 12.0 mm max.&lt;br&gt;
- height 8.0 mm above PCB&lt;br&gt;
- output power 65W&lt;br&gt;&lt;br&gt;

-- offline switch mode power supplies&lt;br&gt;
-- TV&lt;br&gt;
-- devices with heigh issues

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtSLIM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtSLIM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-SLIM?"&gt;http://katalog.we-online.de/en/ctm/MID-SLIM?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="TRANSFORMER_11PIN"/>
</gates>
<devices>
<device name="" package="WE_LEP28/11.2_6PIN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_760871333"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SLM" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Common Mode Line Filter WE-SLM&lt;/b&gt;&lt;p&gt;
- Small size&lt;br&gt;
 - Low Profile&lt;br&gt;
- High Impedance&lt;br&gt; 
- High current capability up to 300 mA&lt;p&gt;

-- USB&lt;br&gt;
-- CAN&lt;br&gt;
-- Firewire&lt;br&gt;
-- Data Lines&lt;br&gt;
-- Power supply systems&lt;br&gt;
-- Signal Lines


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSLM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndSLM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SLM??"&gt;http://katalog.we-online.de/en/pbs/WE-SLM??&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-SLM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_744242101">
<attribute name="WE-NUMBER" value="744242101/100uH"/>
</technology>
<technology name="_744242110">
<attribute name="WE-NUMBER" value="744242110/11uH"/>
</technology>
<technology name="_744242220">
<attribute name="WE-NUMBER" value="744242220/22uH"/>
</technology>
<technology name="_744242330">
<attribute name="WE-NUMBER" value="744242330/33uH"/>
</technology>
<technology name="_744242471">
<attribute name="WE-NUMBER" value="744242471/470uH"/>
</technology>
<technology name="_744242510">
<attribute name="WE-NUMBER" value="744242510/51uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SL_2WINDING" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Common-Mode Choke Line Filter WE-SL&lt;/b&gt;&lt;p&gt;

For distortion-free removal of noise from transmitted 
electrical signals&lt;br&gt;
- 2 or 4 winding configuration&lt;br&gt;
- Offering a wide band width with the core materials of NiZn and MnZn&lt;br&gt;&lt;br&gt;

-- Current compensated choke for data and signal lines&lt;br&gt;
-- USB/CAN/ISDN-Bus&lt;br&gt;
-- Power supply systems&lt;br&gt;
-- Control lines&lt;br&gt;
-- LAN, PBX, cable TV, CD-ROM, 8mm video, etc.


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSL_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndSL_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SL?"&gt;http://katalog.we-online.de/en/pbs/WE-SL?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-SL_2WINDING">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_744206"/>
<technology name="_744207"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SL_4WINDING" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Common-Mode Choke Line Filter WE-SL&lt;/b&gt;&lt;p&gt;

For distortion-free removal of noise from transmitted 
electrical signals&lt;br&gt;
- 2 or 4 winding configuration&lt;br&gt;
- Offering a wide band width with the core materials of NiZn and MnZn&lt;br&gt;&lt;br&gt;

-- Current compensated choke for data and signal lines&lt;br&gt;
-- USB/CAN/ISDN-Bus&lt;br&gt;
-- Power supply systems&lt;br&gt;
-- Control lines&lt;br&gt;
-- LAN, PBX, cable TV, CD-ROM, 8mm video, etc.

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSL_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndSL_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SL?"&gt;http://katalog.we-online.de/en/pbs/WE-SL?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L4"/>
</gates>
<devices>
<device name="" package="WE-SL_4WINDING">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="7"/>
<connect gate="G$1" pin="7" pad="6"/>
<connect gate="G$1" pin="8" pad="5"/>
</connects>
<technologies>
<technology name="_744201"/>
<technology name="_744202"/>
<technology name="_744203"/>
<technology name="_744204"/>
<technology name="_744205"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPC_4838" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD-Shielded Power Inductor  WE-SPC

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndSPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SPC?"&gt;http://katalog.we-online.de/en/pbs/WE-SPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="" package="WE-SPC_48XX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744089430022">
<attribute name="WE-NUMBER" value="74408943002/0,22uH"/>
</technology>
<technology name="_744089430039">
<attribute name="WE-NUMBER" value="744089430039/0,39uH"/>
</technology>
<technology name="_744089430056">
<attribute name="WE-NUMBER" value="744089430056/5,6uH"/>
</technology>
<technology name="_744089430082">
<attribute name="WE-NUMBER" value="744089430082/0,82uH"/>
</technology>
<technology name="_74408943010">
<attribute name="WE-NUMBER" value="74408943010/1uH"/>
</technology>
<technology name="_74408943022">
<attribute name="WE-NUMBER" value="74408943022/2,2uH"/>
</technology>
<technology name="_74408943033">
<attribute name="WE-NUMBER" value="74408943033/3,3uH"/>
</technology>
<technology name="_74408943047">
<attribute name="WE-NUMBER" value="74408943047/4,7uH"/>
</technology>
<technology name="_74408943068">
<attribute name="WE-NUMBER" value="74408943068/6,8uH"/>
</technology>
<technology name="_74408943082">
<attribute name="WE-NUMBER" value="74408943082/8,2uH"/>
</technology>
<technology name="_74408943100">
<attribute name="WE-NUMBER" value="74408943100/10uH"/>
</technology>
<technology name="_74408943101">
<attribute name="WE-NUMBER" value="74408943101/100uH"/>
</technology>
<technology name="_74408943150">
<attribute name="WE-NUMBER" value="74408943150/15uH"/>
</technology>
<technology name="_74408943220">
<attribute name="WE-NUMBER" value="74408943220/22uH"/>
</technology>
<technology name="_74408943330">
<attribute name="WE-NUMBER" value="74408943330/33uH"/>
</technology>
<technology name="_74408943470">
<attribute name="WE-NUMBER" value="74408943470/47uH"/>
</technology>
<technology name="_74408943560">
<attribute name="WE-NUMBER" value="74408943560/56uH"/>
</technology>
<technology name="_74408943680">
<attribute name="WE-NUMBER" value="74408943680/68uH"/>
</technology>
<technology name="_74408943820">
<attribute name="WE-NUMBER" value="74408943820/82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SUKW" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD EMI Suppression 5-Hole Ferrite Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Impedance up to 580 Ω
&lt;br&gt;
&lt;br&gt; SMD version for an easy installation on the PCB
&lt;br&gt;
&lt;br&gt; Special NiSn pad for improved soldering results
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection against radio frequency interferences of components on PCB’s of PC’s, text processing and other digital devices
&lt;br&gt;
&lt;br&gt; Typical in power supply
&lt;br&gt;
&lt;br&gt; Power electronics
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/FeSUKW_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SUKW?"&gt;http://katalog.we-online.de/en/pbs/WE-SUKW?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="_7427511" package="WE-SUKW_7427511">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7427512" package="WE-SUKW_7427512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TCI_0201" prefix="L" uservalue="yes">
<description>&lt;b&gt;Thinfilm Chip Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High self resonant frequency
&lt;br&gt;
&lt;br&gt; Tight tolerances of 2% (1% on request) or ± 0.1 nH and small inductance values
&lt;br&gt;
&lt;br&gt; Outstanding temperature stability
&lt;br&gt;
&lt;br&gt; In high frequency circuit the inductance is very stable
&lt;br&gt;
&lt;br&gt; Small inductance values
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Mobile phone
&lt;br&gt;
&lt;br&gt; Pagers
&lt;br&gt;
&lt;br&gt; GPS products
&lt;br&gt;
&lt;br&gt; Wireless LAN
&lt;br&gt;
&lt;br&gt; Communication appliances
&lt;br&gt;
&lt;br&gt; RF Transceiver Module
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/RfTCI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/RfTCI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TCI?"&gt;http://katalog.we-online.de/en/pbs/WE-TCI?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="" package="WE-TCI_0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744900010">
<attribute name="WE-NUMBER" value="744900010/1nH"/>
</technology>
<technology name="_744900012">
<attribute name="WE-NUMBER" value="744900012/1,2nH"/>
</technology>
<technology name="_744900013">
<attribute name="WE-NUMBER" value="744900013/1,3nH"/>
</technology>
<technology name="_744900014">
<attribute name="WE-NUMBER" value="744900014/1,4nH"/>
</technology>
<technology name="_744900015">
<attribute name="WE-NUMBER" value="744900015/1,5nH"/>
</technology>
<technology name="_744900018">
<attribute name="WE-NUMBER" value="744900018/1,8nH"/>
</technology>
<technology name="_744900019">
<attribute name="WE-NUMBER" value="744900019/1,9nH"/>
</technology>
<technology name="_744900020">
<attribute name="WE-NUMBER" value="744900020/2nH"/>
</technology>
<technology name="_744900022">
<attribute name="WE-NUMBER" value="744900022/2,2nH"/>
</technology>
<technology name="_744900027">
<attribute name="WE-NUMBER" value="744900027/2,7nH"/>
</technology>
<technology name="_744900033">
<attribute name="WE-NUMBER" value="744900033/3,3nH"/>
</technology>
<technology name="_744900039">
<attribute name="WE-NUMBER" value="744900039/3,9nH"/>
</technology>
<technology name="_744900047">
<attribute name="WE-NUMBER" value="744900047/4,7nH"/>
</technology>
<technology name="_744900056">
<attribute name="WE-NUMBER" value="744900056/5,6nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TDC_8018" prefix="L" uservalue="yes">
<description>&lt;b&gt;SEPIC SMD Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Core material: NiZn
&lt;br&gt;
&lt;br&gt; Low profile
&lt;br&gt;
&lt;br&gt; Magnetical shielded which results in a low leakage field
&lt;br&gt;
&lt;br&gt; 8x8 mm case
&lt;br&gt;
&lt;br&gt; 1:1 transformer
&lt;br&gt;
&lt;br&gt; Low self-losses
&lt;br&gt;
&lt;br&gt; High self resonance frequency
&lt;br&gt;
&lt;br&gt; Coupled inductor with two identical windings
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C up to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Non-isolated flyback converter
&lt;br&gt;
&lt;br&gt; Buck or Boost with AUX winding
&lt;br&gt;
&lt;br&gt; BUCK-BOOST, SEPIC, ZETA &amp; CUK Converter
&lt;br&gt;
&lt;br&gt; Switching regulators with secondary unregulated output voltages
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTDC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTDC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TDC?"&gt;http://katalog.we-online.de/en/pbs/WE-TDC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-TDC_80XX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="3"/>
</connects>
<technologies>
<technology name="_744894300033">
<attribute name="WE-NUMBER" value="744894300033/0,33uH"/>
</technology>
<technology name="_744894300068">
<attribute name="WE-NUMBER" value="744894300068/0,68uH"/>
</technology>
<technology name="_74489430010">
<attribute name="WE-NUMBER" value="74489430010/1uH"/>
</technology>
<technology name="_74489430022">
<attribute name="WE-NUMBER" value="74489430022/2,2uH"/>
</technology>
<technology name="_74489430027">
<attribute name="WE-NUMBER" value="74489430027/2,7uH"/>
</technology>
<technology name="_74489430039">
<attribute name="WE-NUMBER" value="74489430039/3,9uH"/>
</technology>
<technology name="_74489430056">
<attribute name="WE-NUMBER" value="74489430056/5,6uH"/>
</technology>
<technology name="_74489430068">
<attribute name="WE-NUMBER" value="74489430068/6,8uH"/>
</technology>
<technology name="_74489430100">
<attribute name="WE-NUMBER" value="74489430100/10uH"/>
</technology>
<technology name="_74489430120">
<attribute name="WE-NUMBER" value="74489430120/12uH"/>
</technology>
<technology name="_74489430150">
<attribute name="WE-NUMBER" value="74489430150/15uH"/>
</technology>
<technology name="_74489430180">
<attribute name="WE-NUMBER" value="74489430180/18uH"/>
</technology>
<technology name="_74489430220">
<attribute name="WE-NUMBER" value="74489430220/22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TFC_UT" prefix="L" uservalue="yes">
<description>&lt;b&gt;Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Approximate 1% stray inductance for symmetrical interference suppression
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Mains filter
&lt;br&gt;
&lt;br&gt; Suppression of common mode noise
&lt;br&gt;
&lt;br&gt; Compact switch mode power supplies
&lt;br&gt;
&lt;br&gt; Electronic ballast applications (LED bulb)
&lt;br&gt;
&lt;br&gt; Lighting
&lt;br&gt;
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTFC_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTFC_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TFC?"&gt;http://katalog.we-online.de/en/pbs/WE-TFC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-TFC">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_744862018">
<attribute name="WE-NUMBER" value="744862018/1,8mH"/>
</technology>
<technology name="_744862033">
<attribute name="WE-NUMBER" value="744862033/3,3mH"/>
</technology>
<technology name="_744862056">
<attribute name="WE-NUMBER" value="744862056/5,6mH"/>
</technology>
<technology name="_744862082">
<attribute name="WE-NUMBER" value="744862082/8,2mH"/>
</technology>
<technology name="_744862100">
<attribute name="WE-NUMBER" value="744862100/10mH"/>
</technology>
<technology name="_744862120">
<attribute name="WE-NUMBER" value="744862120/12mH"/>
</technology>
<technology name="_744862180">
<attribute name="WE-NUMBER" value="744862180/18mH"/>
</technology>
<technology name="_744862250">
<attribute name="WE-NUMBER" value="744862250/25mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TFCH_UT" prefix="L" uservalue="yes">
<description>&lt;b&gt;Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Approximate 1% stray inductance for symmetrical interference suppression
&lt;br&gt;
&lt;br&gt; Optimized frequency range: 10 kHz to 100 MHz
&lt;br&gt;
&lt;br&gt; Attenuation up to 65 dB
&lt;br&gt;
&lt;br&gt; Inductance tolerance: +50%/–30%
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Mains filter
&lt;br&gt;
&lt;br&gt; Suppression of common mode noise
&lt;br&gt;
&lt;br&gt; Compact switch mode power supplies
&lt;br&gt;
&lt;br&gt; Electronic ballast applications (LED bulb)
&lt;br&gt;
&lt;br&gt; Lighting
&lt;br&gt;
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTFCH_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTFCH_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TFCH?"&gt;http://katalog.we-online.de/en/pbs/WE-TFCH?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-TFCH">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="3"/>
</connects>
<technologies>
<technology name="_744861018">
<attribute name="WE-NUMBER" value="744861018/1,8mH"/>
</technology>
<technology name="_744861033">
<attribute name="WE-NUMBER" value="744861033/3,3mH"/>
</technology>
<technology name="_744861056">
<attribute name="WE-NUMBER" value="744861056/5,6mH"/>
</technology>
<technology name="_744861082">
<attribute name="WE-NUMBER" value="744861082/8,2mH"/>
</technology>
<technology name="_744861100">
<attribute name="WE-NUMBER" value="744861100/10mH"/>
</technology>
<technology name="_744861120">
<attribute name="WE-NUMBER" value="744861120/12mH"/>
</technology>
<technology name="_744861180">
<attribute name="WE-NUMBER" value="744861180/18mH"/>
</technology>
<technology name="_744861250">
<attribute name="WE-NUMBER" value="744861250/25mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TI_8095" prefix="L" uservalue="yes">
<description>&lt;b&gt;Radial Leaded Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Radial through-hole inductor
&lt;br&gt;
&lt;br&gt; High saturation core material
&lt;br&gt;
&lt;br&gt; Small size
&lt;br&gt;
&lt;br&gt; Maximum current up to 8.5 A
&lt;br&gt;
&lt;br&gt; Custom design on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Signal filtering
&lt;br&gt;
&lt;br&gt; Switches, switching power supply for small and medium voltage
&lt;br&gt;
&lt;br&gt; Power supply filter
&lt;br&gt;
&lt;br&gt; EMI filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TI?"&gt;http://katalog.we-online.de/en/pbs/WE-TI?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="" package="WE-TI_TIHV_8095">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744772010">
<attribute name="WE-NUMBER" value="744772010/1uH"/>
</technology>
<technology name="_7447720122">
<attribute name="WE-NUMBER" value="7447720122/1200uH"/>
</technology>
<technology name="_7447720150">
<attribute name="WE-NUMBER" value="7447720150/15uH"/>
</technology>
<technology name="_7447720151">
<attribute name="WE-NUMBER" value="7447720151/150uH"/>
</technology>
<technology name="_7447720180">
<attribute name="WE-NUMBER" value="7447720180/18uH"/>
</technology>
<technology name="_7447720181">
<attribute name="WE-NUMBER" value="7447720181/180uH"/>
</technology>
<technology name="_744772022">
<attribute name="WE-NUMBER" value="744772022/2,2uH"/>
</technology>
<technology name="_7447720222">
<attribute name="WE-NUMBER" value="7447720222/2200uH"/>
</technology>
<technology name="_744772033">
<attribute name="WE-NUMBER" value="744772033/3,3uH"/>
</technology>
<technology name="_7447720392">
<attribute name="WE-NUMBER" value="7447720392/3900uH"/>
</technology>
<technology name="_744772047">
<attribute name="WE-NUMBER" value="744772047/4,7uH"/>
</technology>
<technology name="_744772068">
<attribute name="WE-NUMBER" value="744772068/6,8uH"/>
</technology>
<technology name="_744772100">
<attribute name="WE-NUMBER" value="744772100/10uH"/>
</technology>
<technology name="_744772101">
<attribute name="WE-NUMBER" value="744772101/100uH"/>
</technology>
<technology name="_744772102">
<attribute name="WE-NUMBER" value="744772102/1000uH"/>
</technology>
<technology name="_744772103">
<attribute name="WE-NUMBER" value="744772103/10000uH"/>
</technology>
<technology name="_744772121">
<attribute name="WE-NUMBER" value="744772121/120uH"/>
</technology>
<technology name="_744772152">
<attribute name="WE-NUMBER" value="744772152/1500uH"/>
</technology>
<technology name="_744772182">
<attribute name="WE-NUMBER" value="744772182/1800uH"/>
</technology>
<technology name="_744772200">
<attribute name="WE-NUMBER" value="744772200/20uH"/>
</technology>
<technology name="_744772220">
<attribute name="WE-NUMBER" value="744772220/22uH"/>
</technology>
<technology name="_744772221">
<attribute name="WE-NUMBER" value="744772221/220uH"/>
</technology>
<technology name="_744772330">
<attribute name="WE-NUMBER" value="744772330/33uH"/>
</technology>
<technology name="_744772331">
<attribute name="WE-NUMBER" value="744772331/330uH"/>
</technology>
<technology name="_744772332">
<attribute name="WE-NUMBER" value="744772332/3300uH"/>
</technology>
<technology name="_744772390">
<attribute name="WE-NUMBER" value="744772390/39uH"/>
</technology>
<technology name="_744772470">
<attribute name="WE-NUMBER" value="744772470/47uH"/>
</technology>
<technology name="_744772471">
<attribute name="WE-NUMBER" value="744772471/470uH"/>
</technology>
<technology name="_744772472">
<attribute name="WE-NUMBER" value="744772472/4700uH"/>
</technology>
<technology name="_744772560">
<attribute name="WE-NUMBER" value="744772560/56uH"/>
</technology>
<technology name="_744772561">
<attribute name="WE-NUMBER" value="744772561/560uH"/>
</technology>
<technology name="_744772680">
<attribute name="WE-NUMBER" value="744772680/68uH"/>
</technology>
<technology name="_744772681">
<attribute name="WE-NUMBER" value="744772681/680uH"/>
</technology>
<technology name="_744772702">
<attribute name="WE-NUMBER" value="744772702/7000uH"/>
</technology>
<technology name="_744772820">
<attribute name="WE-NUMBER" value="744772820/82uH"/>
</technology>
<technology name="_7447728215">
<attribute name="WE-NUMBER" value="7447728215/820uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TIF_1014" prefix="L" uservalue="yes">
<description>&lt;B&gt;WE-TIF Radial Leaded Wire Wound Inductor with 4 Pins&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Radial through-hole inductor &lt;br&gt;
High saturation core material&lt;br&gt;
 Maximum current up to 3.1 A &lt;br&gt;
2 additional pins for high mechanical stability&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Application&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Signal filtering &lt;br&gt;
EMI and power supply filter&lt;br&gt;
 DC/DC converters &lt;br&gt;
Switching power&lt;br&gt;
 Supplies for small and medium voltage&lt;br&gt; 
Power supply for LED &lt;br&gt;
Nearfield applications &lt;br&gt;



&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTIF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTIF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TIF"&gt;http://katalog.we-online.de/en/pbs/WE-TIF&lt;/a&gt;&lt;p&gt;

Updated on 2015-05-21&lt;br&gt;
2015(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TIF"/>
</gates>
<devices>
<device name="" package="WE-TIF">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447211101">
<attribute name="WE-NUMBER" value="7447211101/100uH"/>
</technology>
<technology name="_7447211102">
<attribute name="WE-NUMBER" value="7447211102/1000uH"/>
</technology>
<technology name="_7447211103">
<attribute name="WE-NUMBER" value="7447211103/10000uH"/>
</technology>
<technology name="_7447211221">
<attribute name="WE-NUMBER" value="7447211221/220uH"/>
</technology>
<technology name="_7447211222">
<attribute name="WE-NUMBER" value="7447211222/2200uH"/>
</technology>
<technology name="_7447211331">
<attribute name="WE-NUMBER" value="7447211331/330uH"/>
</technology>
<technology name="_7447211332">
<attribute name="WE-NUMBER" value="7447211332/3300uH"/>
</technology>
<technology name="_7447211471">
<attribute name="WE-NUMBER" value="7447211471/470uH"/>
</technology>
<technology name="_7447211472">
<attribute name="WE-NUMBER" value="7447211472/4700uH"/>
</technology>
<technology name="_7447211681">
<attribute name="WE-NUMBER" value="7447211681/680uH"/>
</technology>
<technology name="_7447211682">
<attribute name="WE-NUMBER" value="7447211682/6800uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TIS_8075" prefix="L" uservalue="yes">
<description>&lt;b&gt;Shielded Radial Leaded Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Shielded radial through-hole inductor
&lt;br&gt;
&lt;br&gt; High rated and saturation current
&lt;br&gt;
&lt;br&gt; High inductance values
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter choke
&lt;br&gt;
&lt;br&gt; Storage choke
&lt;br&gt;
&lt;br&gt; Class D amplifiers
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTIS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTIS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TIS?"&gt;http://katalog.we-online.de/en/pbs/WE-TIS?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="" package="WE-TIS_8075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744731102">
<attribute name="WE-NUMBER" value="744731102/1000uH"/>
</technology>
<technology name="_744731152">
<attribute name="WE-NUMBER" value="744731152/1500uH"/>
</technology>
<technology name="_744731222">
<attribute name="WE-NUMBER" value="744731222/2200uH"/>
</technology>
<technology name="_744731331">
<attribute name="WE-NUMBER" value="744731331/330uH"/>
</technology>
<technology name="_744731332">
<attribute name="WE-NUMBER" value="744731332/3300uH"/>
</technology>
<technology name="_744731471">
<attribute name="WE-NUMBER" value="744731471/470uH"/>
</technology>
<technology name="_744731472">
<attribute name="WE-NUMBER" value="744731472/4700uH"/>
</technology>
<technology name="_744731562">
<attribute name="WE-NUMBER" value="744731562/5600uH"/>
</technology>
<technology name="_744731680">
<attribute name="WE-NUMBER" value="744731680/68uH"/>
</technology>
<technology name="_744731681">
<attribute name="WE-NUMBER" value="744731681/680uH"/>
</technology>
<technology name="_744731822">
<attribute name="WE-NUMBER" value="744731822/8200uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TIHV" prefix="L" uservalue="yes">
<description>&lt;b&gt;Radial Leaded Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Radial through-hole inductor
&lt;br&gt;
&lt;br&gt; High saturation core material
&lt;br&gt;
&lt;br&gt; Unshielded construction
&lt;br&gt;
&lt;br&gt; Designed for 400 VDC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Non-isolated buck or buck-boost converter like Power Integrations LinkSwitch-TN
&lt;br&gt;
&lt;br&gt; Constant current LED driver
&lt;br&gt;
&lt;br&gt; Utility metering
&lt;br&gt;
&lt;br&gt; Filter for power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTIHV_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTIHV_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TI_HV?"&gt;http://katalog.we-online.de/en/pbs/WE-TI_HV?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="" package="WE-TI_TIHV_8095">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_768772102">
<attribute name="WE-NUMBER" value="768772102/1000uH"/>
</technology>
<technology name="_768772122">
<attribute name="WE-NUMBER" value="768772122/1200uH"/>
</technology>
<technology name="_768772152">
<attribute name="WE-NUMBER" value="768772152/1500uH"/>
</technology>
<technology name="_768772182">
<attribute name="WE-NUMBER" value="768772182/1800uH"/>
</technology>
<technology name="_768772221">
<attribute name="WE-NUMBER" value="768772221/220uH"/>
</technology>
<technology name="_768772222">
<attribute name="WE-NUMBER" value="768772222/2200uH"/>
</technology>
<technology name="_768772331">
<attribute name="WE-NUMBER" value="768772331/330uH"/>
</technology>
<technology name="_768772332">
<attribute name="WE-NUMBER" value="768772332/3300uH"/>
</technology>
<technology name="_768772471">
<attribute name="WE-NUMBER" value="768772471/470uH"/>
</technology>
<technology name="_768772681">
<attribute name="WE-NUMBER" value="768772681/680uH"/>
</technology>
<technology name="_768772821">
<attribute name="WE-NUMBER" value="768772821/820uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TMSB" prefix="L" uservalue="yes">
<description>&lt;b&gt;Tiny Multilayer Suppression Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Perfect for Miniaturization of EMI solutions
&lt;br&gt;
&lt;br&gt; Wide Impedance range from 10 up to 300 Ω
&lt;br&gt;
&lt;br&gt; Operating Temperature: –55 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; General signal and low power lines
&lt;br&gt;
&lt;br&gt; Audio-, video-, clocklines
&lt;br&gt;
&lt;br&gt; Small handheld
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeTMSB_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/FeTMSB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TMSB?"&gt;http://katalog.we-online.de/en/pbs/WE-TMSB?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="" package="WE-TMSB_0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742692001"/>
<technology name="_742692002"/>
<technology name="_742692003"/>
<technology name="_742692004"/>
<technology name="_742692005"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_824001" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode High Speed Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Sturdy design
&lt;br&gt;
&lt;br&gt; Very low capacitance
&lt;br&gt;
&lt;br&gt; Flow Thru Design for a simple layout
&lt;br&gt;
&lt;br&gt; Rail to Rail protection
&lt;br&gt;
&lt;br&gt; Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Very fast data lines
&lt;br&gt;
&lt;br&gt; USB 2.0
&lt;br&gt;
&lt;br&gt; Ethernet
&lt;br&gt;
&lt;br&gt; PoE
&lt;br&gt;
&lt;br&gt; VGA
&lt;br&gt;
&lt;br&gt; Sim Cards
&lt;br&gt;
&lt;br&gt; Keypads
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2,
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?"&gt;http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6RTR4"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_824011" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode High Speed Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Sturdy design
&lt;br&gt;
&lt;br&gt; Very low capacitance
&lt;br&gt;
&lt;br&gt; Flow Thru Design for a simple layout
&lt;br&gt;
&lt;br&gt; Rail to Rail protection
&lt;br&gt;
&lt;br&gt; Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Very fast data lines
&lt;br&gt;
&lt;br&gt; USB 2.0
&lt;br&gt;
&lt;br&gt; Ethernet
&lt;br&gt;
&lt;br&gt; PoE
&lt;br&gt;
&lt;br&gt; VGA
&lt;br&gt;
&lt;br&gt; Sim Cards
&lt;br&gt;
&lt;br&gt; Keypads
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2,
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?"&gt;http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_824011"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-5L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I/O1" pad="3"/>
<connect gate="G$1" pin="I/O2" pad="4"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_824013" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode High Speed Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Sturdy design
&lt;br&gt;
&lt;br&gt; Very low capacitance
&lt;br&gt;
&lt;br&gt; Flow Thru Design for a simple layout
&lt;br&gt;
&lt;br&gt; Rail to Rail protection
&lt;br&gt;
&lt;br&gt; Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Very fast data lines
&lt;br&gt;
&lt;br&gt; USB 2.0
&lt;br&gt;
&lt;br&gt; Ethernet
&lt;br&gt;
&lt;br&gt; PoE
&lt;br&gt;
&lt;br&gt; VGA
&lt;br&gt;
&lt;br&gt; Sim Cards
&lt;br&gt;
&lt;br&gt; Keypads
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2,
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?"&gt;http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6RTR4"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_824014" prefix="D">
<description>&lt;b&gt;TVS Diode Super Speed Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Operating temperature: –55 ºC to +85 °C for 824 014 x; –40 ºC to +85 °C for 824 016 46
&lt;br&gt;
&lt;br&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Very low capacitance
&lt;br&gt;
&lt;br&gt; Rail to Rail protection
&lt;br&gt;
&lt;br&gt; Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Super Speed data lines
&lt;br&gt;
&lt;br&gt; HDMI 1.3/1.4, DVI
&lt;br&gt;
&lt;brr&gt; DisplayPort
&lt;br&gt;
&lt;br&gt; USB 3.0 SuperSpeed
&lt;br&gt;
&lt;brr&gt; SATA
&lt;br&gt;
&lt;br&gt; GBit LAN
&lt;br&gt;
&lt;brr&gt; ESD protection in accordance with EN 61000-4-2
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/24014?"&gt;http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/24014?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6RTR4D"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_824015" prefix="D">
<description>&lt;b&gt;TVS Diode High Speed Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Sturdy design
&lt;br&gt;
&lt;br&gt; Very low capacitance
&lt;br&gt;
&lt;br&gt; Flow Thru Design for a simple layout
&lt;br&gt;
&lt;br&gt; Rail to Rail protection
&lt;br&gt;
&lt;br&gt; Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Very fast data lines
&lt;br&gt;
&lt;br&gt; USB 2.0
&lt;br&gt;
&lt;br&gt; Ethernet
&lt;br&gt;
&lt;br&gt; PoE
&lt;br&gt;
&lt;br&gt; VGA
&lt;br&gt;
&lt;br&gt; Sim Cards
&lt;br&gt;
&lt;br&gt; Keypads
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2,
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?"&gt;http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6RTR4"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_824021" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode Standard Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Operating temperature: –55 ºC to +85 °C for 824 023 x; –55 ºC to +125 °C for 824 021/824 022
&lt;br&gt;
&lt;br&gt; Very low clamping voltage
&lt;br&gt;
&lt;br&gt; High ESD withstand voltage
&lt;br&gt;
&lt;br&gt; Unidirectional or bidirectional protection
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC power supply
&lt;br&gt;
&lt;br&gt; Headsets and accessories
&lt;br&gt;
&lt;br&gt; PDAs
&lt;br&gt;
&lt;br&gt; Digital cameras
&lt;br&gt;
&lt;br&gt; MP3-Player
&lt;br&gt;
&lt;br&gt; Touch Panels
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_3ESD2"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-3L">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I/O1" pad="1"/>
<connect gate="G$1" pin="I/O2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_824022" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode Standard Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Operating temperature: –55 ºC to +85 °C for 824 023 x; –55 ºC to +125 °C for 824 021/824 022
&lt;br&gt;
&lt;br&gt; Very low clamping voltage
&lt;br&gt;
&lt;br&gt; High ESD withstand voltage
&lt;br&gt;
&lt;br&gt; Unidirectional or bidirectional protection
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC power supply
&lt;br&gt;
&lt;br&gt; Headsets and accessories
&lt;br&gt;
&lt;br&gt; PDAs
&lt;br&gt;
&lt;br&gt; Digital cameras
&lt;br&gt;
&lt;br&gt; MP3-Player
&lt;br&gt;
&lt;br&gt; Touch Panels
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_3ESB2B"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-3L">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I/O1" pad="1"/>
<connect gate="G$1" pin="I/O2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_8240026" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode High Speed Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Sturdy design
&lt;br&gt;
&lt;br&gt; Very low capacitance
&lt;br&gt;
&lt;br&gt; Flow Thru Design for a simple layout
&lt;br&gt;
&lt;br&gt; Rail to Rail protection
&lt;br&gt;
&lt;br&gt; Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Very fast data lines
&lt;br&gt;
&lt;br&gt; USB 2.0
&lt;br&gt;
&lt;br&gt; Ethernet
&lt;br&gt;
&lt;br&gt; PoE
&lt;br&gt;
&lt;br&gt; VGA
&lt;br&gt;
&lt;br&gt; Sim Cards
&lt;br&gt;
&lt;br&gt; Keypads
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2,
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?"&gt;http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_5RTR2/4RTR2"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT143-4L">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_8240116" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode High Speed Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Sturdy design
&lt;br&gt;
&lt;br&gt; Very low capacitance
&lt;br&gt;
&lt;br&gt; Flow Thru Design for a simple layout
&lt;br&gt;
&lt;br&gt; Rail to Rail protection
&lt;br&gt;
&lt;br&gt; Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Very fast data lines
&lt;br&gt;
&lt;br&gt; USB 2.0
&lt;br&gt;
&lt;br&gt; Ethernet
&lt;br&gt;
&lt;br&gt; PoE
&lt;br&gt;
&lt;br&gt; VGA
&lt;br&gt;
&lt;br&gt; Sim Cards
&lt;br&gt;
&lt;br&gt; Keypads
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2,
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?"&gt;http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_5RTR2/4RTR2"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT143-4L">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_8240136" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode High Speed Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Sturdy design
&lt;br&gt;
&lt;br&gt; Very low capacitance
&lt;br&gt;
&lt;br&gt; Flow Thru Design for a simple layout
&lt;br&gt;
&lt;br&gt; Rail to Rail protection
&lt;br&gt;
&lt;br&gt; Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Very fast data lines
&lt;br&gt;
&lt;br&gt; USB 2.0
&lt;br&gt;
&lt;br&gt; Ethernet
&lt;br&gt;
&lt;br&gt; PoE
&lt;br&gt;
&lt;br&gt; VGA
&lt;br&gt;
&lt;br&gt; Sim Cards
&lt;br&gt;
&lt;br&gt; Keypads
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2,
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?"&gt;http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_5RTR2/4RTR2"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT143-4L">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_82400102" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode High Speed Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Sturdy design
&lt;br&gt;
&lt;br&gt; Very low capacitance
&lt;br&gt;
&lt;br&gt; Flow Thru Design for a simple layout
&lt;br&gt;
&lt;br&gt; Rail to Rail protection
&lt;br&gt;
&lt;br&gt; Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Very fast data lines
&lt;br&gt;
&lt;br&gt; USB 2.0
&lt;br&gt;
&lt;br&gt; Ethernet
&lt;br&gt;
&lt;br&gt; PoE
&lt;br&gt;
&lt;br&gt; VGA
&lt;br&gt;
&lt;br&gt; Sim Cards
&lt;br&gt;
&lt;br&gt; Keypads
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2,
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?"&gt;http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6RTR4FD"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-6L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I/O1" pad="1"/>
<connect gate="G$1" pin="I/O1-1" pad="6"/>
<connect gate="G$1" pin="I/O2" pad="3"/>
<connect gate="G$1" pin="I/O2-1" pad="4"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_82400152" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode High Speed Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Sturdy design
&lt;br&gt;
&lt;br&gt; Very low capacitance
&lt;br&gt;
&lt;br&gt; Flow Thru Design for a simple layout
&lt;br&gt;
&lt;br&gt; Rail to Rail protection
&lt;br&gt;
&lt;br&gt; Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Very fast data lines
&lt;br&gt;
&lt;br&gt; USB 2.0
&lt;br&gt;
&lt;br&gt; Ethernet
&lt;br&gt;
&lt;br&gt; PoE
&lt;br&gt;
&lt;br&gt; VGA
&lt;br&gt;
&lt;br&gt; Sim Cards
&lt;br&gt;
&lt;br&gt; Keypads
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2,
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?"&gt;http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6RTR4FD"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT563">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I/O1" pad="1"/>
<connect gate="G$1" pin="I/O1-1" pad="6"/>
<connect gate="G$1" pin="I/O2" pad="3"/>
<connect gate="G$1" pin="I/O2-1" pad="4"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_82400274" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode High Speed Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Sturdy design
&lt;br&gt;
&lt;br&gt; Very low capacitance
&lt;br&gt;
&lt;br&gt; Flow Thru Design for a simple layout
&lt;br&gt;
&lt;br&gt; Rail to Rail protection
&lt;br&gt;
&lt;br&gt; Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Very fast data lines
&lt;br&gt;
&lt;br&gt; USB 2.0
&lt;br&gt;
&lt;br&gt; Ethernet
&lt;br&gt;
&lt;br&gt; PoE
&lt;br&gt;
&lt;br&gt; VGA
&lt;br&gt;
&lt;br&gt; Sim Cards
&lt;br&gt;
&lt;br&gt; Keypads
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2,
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?"&gt;http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824001?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6RTR4"/>
</gates>
<devices>
<device name="" package="WE-TVS_SC70-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_82401444" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode Super Speed Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Operating temperature: –55 ºC to +85 °C for 824 014 x; –40 ºC to +85 °C for 824 016 46
&lt;br&gt;
&lt;br&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Very low capacitance
&lt;br&gt;
&lt;br&gt; Rail to Rail protection
&lt;br&gt;
&lt;br&gt; Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Super Speed data lines
&lt;br&gt;
&lt;br&gt; HDMI 1.3/1.4, DVI
&lt;br&gt;
&lt;brr&gt; DisplayPort
&lt;br&gt;
&lt;br&gt; USB 3.0 SuperSpeed
&lt;br&gt;
&lt;brr&gt; SATA
&lt;br&gt;
&lt;br&gt; GBit LAN
&lt;br&gt;
&lt;brr&gt; ESD protection in accordance with EN 61000-4-2
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_10RTR4D"/>
</gates>
<devices>
<device name="" package="WE-TVS_MSOP-10L">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="I/O1" pad="1"/>
<connect gate="G$1" pin="I/O2" pad="2"/>
<connect gate="G$1" pin="I/O3" pad="4"/>
<connect gate="G$1" pin="I/O4" pad="5"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_82401646" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode Super Speed Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Operating temperature: –55 ºC to +85 °C for 824 014 x; –40 ºC to +85 °C for 824 016 46
&lt;br&gt;
&lt;br&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Very low capacitance
&lt;br&gt;
&lt;br&gt; Rail to Rail protection
&lt;br&gt;
&lt;br&gt; Epoxy flame resistant UL94 V-0
&lt;br&gt;
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Super Speed data lines
&lt;br&gt;
&lt;br&gt; HDMI 1.3/1.4, DVI
&lt;br&gt;
&lt;brr&gt; DisplayPort
&lt;br&gt;
&lt;br&gt; USB 3.0 SuperSpeed
&lt;br&gt;
&lt;brr&gt; SATA
&lt;br&gt;
&lt;br&gt; GBit LAN
&lt;br&gt;
&lt;brr&gt; ESD protection in accordance with EN 61000-4-2
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_8RTR6"/>
</gates>
<devices>
<device name="" package="WE-TVS_MSOP-8L">
<connects>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="I/O1" pad="1"/>
<connect gate="G$1" pin="I/O2" pad="2"/>
<connect gate="G$1" pin="I/O3" pad="3"/>
<connect gate="G$1" pin="I/O4" pad="4"/>
<connect gate="G$1" pin="I/O5" pad="5"/>
<connect gate="G$1" pin="I/O6" pad="6"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_82402304" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode Standard Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Operating temperature: –55 ºC to +85 °C for 824 023 x; –55 ºC to +125 °C for 824 021/824 022
&lt;br&gt;
&lt;br&gt; Very low clamping voltage
&lt;br&gt;
&lt;br&gt; High ESD withstand voltage
&lt;br&gt;
&lt;br&gt; Unidirectional or bidirectional protection
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC power supply
&lt;br&gt;
&lt;br&gt; Headsets and accessories
&lt;br&gt;
&lt;br&gt; PDAs
&lt;br&gt;
&lt;br&gt; Digital cameras
&lt;br&gt;
&lt;br&gt; MP3-Player
&lt;br&gt;
&lt;br&gt; Touch Panels
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6ESD4"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_82402305" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode Standard Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Operating temperature: –55 ºC to +85 °C for 824 023 x; –55 ºC to +125 °C for 824 021/824 022
&lt;br&gt;
&lt;br&gt; Very low clamping voltage
&lt;br&gt;
&lt;br&gt; High ESD withstand voltage
&lt;br&gt;
&lt;br&gt; Unidirectional or bidirectional protection
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC power supply
&lt;br&gt;
&lt;br&gt; Headsets and accessories
&lt;br&gt;
&lt;br&gt; PDAs
&lt;br&gt;
&lt;br&gt; Digital cameras
&lt;br&gt;
&lt;br&gt; MP3-Player
&lt;br&gt;
&lt;br&gt; Touch Panels
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVS_HIGHSPEED.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824021?"&gt;http://katalog.we-online.de/en/pbs/WE-TVS_High_Speed/824021?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6ESD5"/>
</gates>
<devices>
<device name="" package="WE-TVS_SOT23-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_82402374" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode Standard Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Operating temperature: –55 ºC to +85 °C for 824 023 x; –55 ºC to +125 °C for 824 021/824 022
&lt;br&gt;
&lt;br&gt; Very low clamping voltage
&lt;br&gt;
&lt;br&gt; High ESD withstand voltage
&lt;br&gt;
&lt;br&gt; Unidirectional or bidirectional protection
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC power supply
&lt;br&gt;
&lt;br&gt; Headsets and accessories
&lt;br&gt;
&lt;br&gt; PDAs
&lt;br&gt;
&lt;br&gt; Digital cameras
&lt;br&gt;
&lt;br&gt; MP3-Player
&lt;br&gt;
&lt;br&gt; Touch Panels
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_5ESD4"/>
</gates>
<devices>
<device name="" package="WE-TVS_SC70-5L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVS_82402375" prefix="D" uservalue="yes">
<description>&lt;b&gt;TVS Diode Standard Series
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Operating temperature: –55 ºC to +85 °C for 824 023 x; –55 ºC to +125 °C for 824 021/824 022
&lt;br&gt;
&lt;br&gt; Very low clamping voltage
&lt;br&gt;
&lt;br&gt; High ESD withstand voltage
&lt;br&gt;
&lt;br&gt; Unidirectional or bidirectional protection
&lt;br&gt; RoHS, REACH and free of halogens
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC power supply
&lt;br&gt;
&lt;br&gt; Headsets and accessories
&lt;br&gt;
&lt;br&gt; PDAs
&lt;br&gt;
&lt;br&gt; Digital cameras
&lt;br&gt;
&lt;br&gt; MP3-Player
&lt;br&gt;
&lt;br&gt; Touch Panels
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2
&lt;br&gt;– 8 kV contact discharge
&lt;br&gt;– 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TVS_6ESD5"/>
</gates>
<devices>
<device name="" package="WE-TVS_SC70-6L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UCF_2TURNS" prefix="L" uservalue="yes">
<description>&lt;B&gt;WE-UCF SMD Common Mode Line Filter
&lt;Br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High inductance range
&lt;br&gt;
&lt;br&gt; High current range
&lt;br&gt;
&lt;br&gt; Small package
&lt;br&gt;
&lt;br&gt; Low profile
&lt;br&gt;
&lt;br&gt; Surface mount technology
&lt;br&gt; Wide range of filtering spectrum
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;Br&gt;&lt;/b&gt; Filtering
&lt;br&gt;
&lt;br&gt; DC power lines
&lt;br&gt;
&lt;br&gt; Buck-/Boost Converter filtering
&lt;br&gt;
&lt;br&gt; Data lines with low bitrate
&lt;br&gt;
&lt;br&gt; Heavily influenced lines
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndUCF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndUCF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-UCF?"&gt;http://katalog.we-online.de/en/pbs/WE-UCF?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-UCF">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="10"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
</connects>
<technologies>
<technology name="_744290103">
<attribute name="WE-NUMBER" value="744290103/2x10mH"/>
</technology>
<technology name="_744290104">
<attribute name="WE-NUMBER" value="744290104/2X100mH"/>
</technology>
<technology name="_744290152">
<attribute name="WE-NUMBER" value="744290152/2X1,5mH"/>
</technology>
<technology name="_744290283">
<attribute name="WE-NUMBER" value="744290283/2X28mH"/>
</technology>
<technology name="_744290321">
<attribute name="WE-NUMBER" value="744290321/2X0,32mH"/>
</technology>
<technology name="_744290472">
<attribute name="WE-NUMBER" value="744290472/2X4,7mH"/>
</technology>
<technology name="_744290473">
<attribute name="WE-NUMBER" value="744290473/2X47mH"/>
</technology>
<technology name="_744290683">
<attribute name="WE-NUMBER" value="744290683/2X68mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UKW_1SW" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Impedance will increase with more turns, available in 1 to 3 turns
&lt;br&gt;
&lt;br&gt; 4 different materials available for perfect interference suppression
&lt;Br&gt;
&lt;br&gt; Also available ready-bent or in individual length
&lt;br&gt;
&lt;br&gt; Maximum current capability is 3 A / 5 A (short-time)
&lt;br&gt;
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection against radio frequency interferences of components on PCB’s of PC’s, text processing and other digital devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeUKW_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeUKW_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-UKW/S/"&gt;http://katalog.we-online.de/en/pbs/WE-UKW/S/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created  by  Dan Xu 2014-06-10&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="_7427501" package="WE-UKW_7427501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7427502" package="WE-UKW_7427502">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7427503" package="WE-UKW_7427503">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7427504" package="WE-UKW_7427504">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74275010" package="WE-UKW_74275010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74275011" package="WE-UKW_74275011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74275013" package="WE-UKW_74275013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74275023" package="WE-UKW_74275023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74275043" package="WE-UKW_74275043">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74275046" package="WE-UKW_74275046">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74275143" package="WE-UKW_74275143">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74275223" package="WE-UKW_74275223">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74275243" package="WE-UKW_74275243">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_E13/7/4VERTICAL" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-UNIT Off-Line Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Nominal input voltage: 125–375 VDC (85–265 VAC)
&lt;br&gt;
&lt;br&gt; Output power 3 W and 9 W
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Clearance and creepage distance 6 mm min.
&lt;br&gt;
&lt;br&gt; Insulation test voltage: 4 kVAC, 1 Minute
&lt;br&gt;
&lt;br&gt; Design compliant to EN 61558-2-16: reinforced insulation; except 749 118 10 xx: Basic insulation
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Designed for Tiny Switch ICs from Power Integration and NCP101x or 105x of ON Semiconductor
&lt;br&gt;
&lt;br&gt; For SMPS with universal input from 85 VAC up to 265 VAC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtUNIT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtUNIT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-UNIT?m"&gt;http://katalog.we-online.de/en/pbs/WE-UNIT?m&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="" package="WE_E13/7/4_THT_VERTIKAL_6PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7491181012"/>
<technology name="_7491181024"/>
<technology name="_749118105"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_E13/7/4HORIZONTAL" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-UNIT Off-Line Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Nominal input voltage: 125–375 VDC (85–265 VAC)
&lt;br&gt;
&lt;br&gt; Output power 3 W and 9 W
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Clearance and creepage distance 6 mm min.
&lt;br&gt;
&lt;br&gt; Insulation test voltage: 4 kVAC, 1 Minute
&lt;br&gt;
&lt;br&gt; Design compliant to EN 61558-2-16: reinforced insulation; except 749 118 10 xx: Basic insulation
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Designed for Tiny Switch ICs from Power Integration and NCP101x or 105x of ON Semiconductor
&lt;br&gt;
&lt;br&gt; For SMPS with universal input from 85 VAC up to 265 VAC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtUNIT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtUNIT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-UNIT?m"&gt;http://katalog.we-online.de/en/pbs/WE-UNIT?m&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-V"/>
</gates>
<devices>
<device name="" package="WE_E13/7/4_THT_HORIZONTAL_9PIN">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="9"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7491181112"/>
<technology name="_7491181124"/>
<technology name="_749118115"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_E16/7/4" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-UNIT Off-Line Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Nominal input voltage: 125–375 VDC (85–265 VAC)
&lt;br&gt;
&lt;br&gt; Output power 3 W and 9 W
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Clearance and creepage distance 6 mm min.
&lt;br&gt;
&lt;br&gt; Insulation test voltage: 4 kVAC, 1 Minute
&lt;br&gt;
&lt;br&gt; Design compliant to EN 61558-2-16: reinforced insulation; except 749 118 10 xx: Basic insulation
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Designed for Tiny Switch ICs from Power Integration and NCP101x or 105x of ON Semiconductor
&lt;br&gt;
&lt;br&gt; For SMPS with universal input from 85 VAC up to 265 VAC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtUNIT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtUNIT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-UNIT?m"&gt;http://katalog.we-online.de/en/pbs/WE-UNIT?m&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_1W:2W"/>
</gates>
<devices>
<device name="" package="WE_E16/7/4_THT_VERTIKAL_10PIN">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="6" pad="9"/>
</connects>
<technologies>
<technology name="_7491182012"/>
<technology name="_7491182024"/>
<technology name="_749118205"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_E16/8/5" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-UNIT Off-Line Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Nominal input voltage: 125–375 VDC (85–265 VAC)
&lt;br&gt;
&lt;br&gt; Output power 3 W and 9 W
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Clearance and creepage distance 6 mm min.
&lt;br&gt;
&lt;br&gt; Insulation test voltage: 4 kVAC, 1 Minute
&lt;br&gt;
&lt;br&gt; Design compliant to EN 61558-2-16: reinforced insulation; except 749 118 10 xx: Basic insulation
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Designed for Tiny Switch ICs from Power Integration and NCP101x or 105x of ON Semiconductor
&lt;br&gt;
&lt;br&gt; For SMPS with universal input from 85 VAC up to 265 VAC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtUNIT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtUNIT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-UNIT?m"&gt;http://katalog.we-online.de/en/pbs/WE-UNIT?m&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_1W:2W"/>
</gates>
<devices>
<device name="" package="WE_E16/8/5_THT_HORIZONTAL_9PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="8"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="1"/>
</connects>
<technologies>
<technology name="_7491182112"/>
<technology name="_7491182124"/>
<technology name="_749118215"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_NXP_750340505" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit NXP&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750340505?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750340505?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:1W"/>
</gates>
<devices>
<device name="" package="WE-UNIT_EFD25">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="9"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="1"/>
<connect gate="G$1" pin="7" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_NXP_750871013" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit NXP&lt;/b&gt;&lt;br&gt;&lt;br&gt;

- Nominal input voltage: 85-265 VAC&lt;br&gt;
- Operating temperature: -40°C to +125 °C&lt;br&gt;
- Isolation voltage 4 kVAC&lt;br&gt;&lt;br&gt;

-- Especially designed for several ICs from NXP TEA1521T&lt;br&gt;
-- Universal input&lt;br&gt;
-- Smart meters&lt;br&gt;
-- Dimmable 12 V LED driver&lt;br&gt;
-- Offline-switch mode power supplies

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750871013?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750871013?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE_EE13/7/4_THT_HORIZONTAL_9PIN">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="9"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_NXP_750871035" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit NXP&lt;/b&gt;&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750871035?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750871035?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE_EE13/6/6_THT_HORIZONTAL_8PIN">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="3"/>
<connect gate="G$1" pin="6" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_NXP_750871530" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit NXP&lt;/b&gt;&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750871530?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750871530?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-UNIT_EE16/8/5_1">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="8"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="5"/>
<connect gate="G$1" pin="7" pad="4"/>
<connect gate="G$1" pin="8" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_NXP_750871630" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit NXP&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750871630?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750871630?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:2W-2"/>
</gates>
<devices>
<device name="" package="WE-UNIT_PI_NXP_EE20/10/6">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="6" pad="13 14"/>
<connect gate="G$1" pin="7" pad="10 11"/>
<connect gate="G$1" pin="8" pad="7 8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_NXP_750871830" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit NXP&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750871830?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750871830?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-UNIT_NXP_750871830"/>
</gates>
<devices>
<device name="" package="WE-UNIT_EE16/8/5_1">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="8"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_NXP_750871831" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit NXP&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750871831?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750871831?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:3W_1"/>
</gates>
<devices>
<device name="" package="WE_EE25/13/7_THT_HORIZONTAL_13PIN">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="5" pad="7"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="10"/>
<connect gate="G$1" pin="8" pad="11"/>
<connect gate="G$1" pin="9" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_PI_750871032" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit PI&lt;/b&gt;&lt;br&gt;&lt;br&gt;

- Nominal input voltage: 85-265 VAC&lt;br&gt;
- Output power 4.2 W &lt;br&gt;
- Operating temperature: -40°C to +125 °C&lt;br&gt;
- Clearance and creepage distance 6 mm min.&lt;br&gt;
- Isolation voltage 4 kVAC&lt;br&gt;&lt;br&gt;

-- Especially designed for several ICs from Power Integrations LNK605&lt;br&gt;
-- Universal input&lt;br&gt;
-- Offline-switch mode power supplies

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_PI?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_PI?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:1W-1"/>
</gates>
<devices>
<device name="" package="WE_EE16/7/4_THT_HORIZONTAL_10PIN">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="10"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="5" pad="3"/>
<connect gate="G$1" pin="7" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_STM_750370026" prefix="T" uservalue="yes">
<description>&lt;b&gt;MID-UNIT STM Offline Transformers for STMicroelectronicsI&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_STM?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_STM?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:2W-1"/>
</gates>
<devices>
<device name="" package="WE-UNIT_750370026">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_STM_750370228" prefix="T" uservalue="yes">
<description>&lt;b&gt;MID-UNIT STM Offline Transformers for STMicroelectronics&lt;/b&gt;&lt;br&gt;&lt;br&gt;



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_STM?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_STM?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:1W"/>
</gates>
<devices>
<device name="" package="WE_EE20/10/6_THT_HORIZONTAL_14PIN">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="8"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_PI_750811630" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit PI&lt;/b&gt;&lt;br&gt;&lt;br&gt;

- Nominal input voltage: 85-265 VAC&lt;br&gt;
- Output power 34.4 W &lt;br&gt;
- Operating temperature: -40°C to +125 °C&lt;br&gt;
- Clearance and creepage distance 6 mm min.&lt;br&gt;
- Isolation voltage 4 kVAC&lt;br&gt;&lt;br&gt;

-- Especially designed for several ICs from Power Integrations TOP258&lt;br&gt;
-- Universal input&lt;br&gt;
-- Offline-switch mode power supplies

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_PI?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_PI?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:2W-2"/>
</gates>
<devices>
<device name="" package="WE_EER28/4/11_HORIZONTAL_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="9 10"/>
<connect gate="G$1" pin="7" pad="11 12"/>
<connect gate="G$1" pin="8" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_STM_750310660" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit STM&lt;/b&gt;&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_STM/750310660?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_STM/750310660?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="TRANSFORMER_3L_1"/>
</gates>
<devices>
<device name="" package="WE_EE16/8/5_THT_HORIZONTAL_6PIN">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="7"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_STM_750370024" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit STM&lt;/b&gt;&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_STM/750370024?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_STM/750370024?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="TRANSFORMER_3L_1"/>
</gates>
<devices>
<device name="" package="WE-UNIT_750370024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="6" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_STM_750871110" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit STM&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_STM/750871110?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_STM/750871110?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE_EE20/10/6_THT_HORIZONTAL_14PIN_1">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="7 9"/>
<connect gate="G$1" pin="3" pad="12 14"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_STM_750871111" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit STM&lt;/b&gt;&lt;br&gt;&lt;br&gt;



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_STM/750871111?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_STM/750871111?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-UNIT_750871111">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="12 14"/>
<connect gate="G$1" pin="3" pad="7 9"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_STM_750871010" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit STM&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_STM?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_STM?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:2W_2"/>
</gates>
<devices>
<device name="" package="WE_EE16/8/5_THT_HORIZONTAL_9PIN">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="9"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="2"/>
<connect gate="G$1" pin="7" pad="1"/>
<connect gate="G$1" pin="8" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UOST" prefix="T" uservalue="yes">
<description>&lt;b&gt; WE-UOST Universal Offline Standard Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt; Input voltage range 85–265 VAC (125–375 VDC)
&lt;br&gt;
&lt;br&gt; Output power 12–16 W
&lt;br&gt;
&lt;br&gt; Designed to comply with EN61558-2-16: Reinforced insulation
&lt;br&gt;
&lt;br&gt; Creepage and clearance distance &gt;6.5 mm
&lt;br&gt;
&lt;br&gt; Insulation test voltage 4 kVAC
&lt;br&gt;
&lt;br&gt; For SMD assembly
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; SMPS with power up to 16 W
&lt;br&gt;
&lt;br&gt; Auxiliary power supplies
&lt;br&gt;
&lt;br&gt; Usable with all low power AC/DC ICs like LT3798/99, UCC28610, ViPER &amp; Tiny/Link Switch
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtUOST_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtUOST_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-UOST?"&gt;http://katalog.we-online.de/en/pbs/WE-UOST?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="TRANSFORMER_4L"/>
</gates>
<devices>
<device name="" package="WE-UOST">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_760871113"/>
<technology name="_760871135"/>
<technology name="_760871142"/>
<technology name="_760875112"/>
<technology name="_760875131"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VD_5MM" prefix="RV" uservalue="yes">
<description>&lt;b&gt;WE-VD Disk Varistor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; After a surge impulse the varistor works immediately in normal mode so there is no slip current
&lt;br&gt;
&lt;br&gt; Excellent absorption at surge impulses
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC for types up to 95 VRMS –40 ºC to +125 ºC for types from 115 VRMS
&lt;br&gt;
&lt;br&gt; Response time &lt; 25 ns
&lt;br&gt;
&lt;br&gt; UL1449 3rd Edition, CSA and VDE approved UL: File E332875 CSA: File 224856 VDE: File 40016986 and 40016998 IEC: 60950-1: 2005 Annex Q from ∅ 10 mm
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; 12–48 VDC distribution
&lt;br&gt;
&lt;br&gt; 110–400 V power supply
&lt;br&gt;
&lt;br&gt; Leakage of voltage peaks
&lt;br&gt;
&lt;br&gt; Surge protection in accordance with EN 61000-4-5
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVD_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VD?"&gt;http://katalog.we-online.de/en/pbs/WE-VD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="VARISTOR"/>
</gates>
<devices>
<device name=",820451111" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820451311" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820451411" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820451511" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820451701" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820451711" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820451911" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820452001" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820452001.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820452501" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820453001" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820453001.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820455001" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820456001" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820457501" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820459501" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820550607" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820551102" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820551111" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820551311" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820551311.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820551406" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820551406.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820551411" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820551511" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820551701" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820551711" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820551911" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820552001" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820552501" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820552501.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820553001" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820555001" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820556001" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820556001.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820557501" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820559501" package="WE-VD_5MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820452111" package="WE-VD_5MM-1.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820552111" package="WE-VD_5MM-1.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820452311" package="WE-VD_5MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820453501" package="WE-VD_5MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820552311" package="WE-VD_5MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820553501" package="WE-VD_5MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820452511" package="WE-VD_5MM-1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820552511" package="WE-VD_5MM-1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820452711" package="WE-VD_5MM-1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820454001" package="WE-VD_5MM-1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820552711" package="WE-VD_5MM-1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820552711.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820554001" package="WE-VD_5MM-1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820554001.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820453011" package="WE-VD_5MM-1.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820553011" package="WE-VD_5MM-1.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820453211" package="WE-VD_5MM-1.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820553211" package="WE-VD_5MM-1.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820453511" package="WE-VD_5MM-2.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820553511" package="WE-VD_5MM-2.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820453811" package="WE-VD_5MM-2.4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820453811.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820553811" package="WE-VD_5MM-2.4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820553811.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820454211" package="WE-VD_5MM-2.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820554211" package="WE-VD_5MM-2.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820454611" package="WE-VD_5MM-3.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820554611" package="WE-VD_5MM-3.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820554611.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VD_7MM" prefix="RV" uservalue="yes">
<description>&lt;b&gt;WE-VD Disk Varistor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; After a surge impulse the varistor works immediately in normal mode so there is no slip current
&lt;br&gt;
&lt;br&gt; Excellent absorption at surge impulses
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC for types up to 95 VRMS –40 ºC to +125 ºC for types from 115 VRMS
&lt;br&gt;
&lt;br&gt; Response time &lt; 25 ns
&lt;br&gt;
&lt;br&gt; UL1449 3rd Edition, CSA and VDE approved UL: File E332875 CSA: File 224856 VDE: File 40016986 and 40016998 IEC: 60950-1: 2005 Annex Q from ∅ 10 mm
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; 12–48 VDC distribution
&lt;br&gt;
&lt;br&gt; 110–400 V power supply
&lt;br&gt;
&lt;br&gt; Leakage of voltage peaks
&lt;br&gt;
&lt;br&gt; Surge protection in accordance with EN 61000-4-5
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVD_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VD?"&gt;http://katalog.we-online.de/en/pbs/WE-VD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="VARISTOR"/>
</gates>
<devices>
<device name=",820476001" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820477501" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820479501" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820571102" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820571111" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820571111.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820571311" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820571311.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820571401" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820571406" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820571406.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820571411" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820571511" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820471511.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820571701" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820571711" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820571911" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820572001" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820572501" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820572501.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820573001" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820573001.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820575001" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820475001.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820576001" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820576001.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820577501" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820579501" package="WE-VD_7MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820472111" package="WE-VD_7MM-1.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820572111" package="WE-VD_7MM-1.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820472311" package="WE-VD_7MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820473501" package="WE-VD_7MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820572311" package="WE-VD_7MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820573501" package="WE-VD_7MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820472511" package="WE-VD_7MM-1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820572511" package="WE-VD_7MM-1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820572511.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820472711" package="WE-VD_7MM-1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820474001" package="WE-VD_7MM-1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820572711" package="WE-VD_7MM-1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820572711.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820574001" package="WE-VD_7MM-1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820574001.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820473011" package="WE-VD_7MM-1.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820573011" package="WE-VD_7MM-1.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820573011.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820473211" package="WE-VD_7MM-1.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820573211" package="WE-VD_7MM-1.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820473511" package="WE-VD_7MM-2.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820573511" package="WE-VD_7MM-2.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820473811" package="WE-VD_7MM-2.4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820573811" package="WE-VD_7MM-2.4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820474211" package="WE-VD_7MM-2.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820474211.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820574211" package="WE-VD_7MM-2.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820574211.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820474611" package="WE-VD_7MM-3.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820474611.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820574611" package="WE-VD_7MM-3.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820574611.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820474811" package="WE-VD_7MM-3.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820574811" package="WE-VD_7MM-3.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820475111" package="WE-VD_7MM-3.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820575111" package="WE-VD_7MM-3.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820471511" package="WE-VD_7MM-1.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=",820475001" package="WE-VD_7MM-1.4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VD_10MM" prefix="RV" uservalue="yes">
<description>&lt;b&gt;WE-VD Disk Varistor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; After a surge impulse the varistor works immediately in normal mode so there is no slip current
&lt;br&gt;
&lt;br&gt; Excellent absorption at surge impulses
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC for types up to 95 VRMS –40 ºC to +125 ºC for types from 115 VRMS
&lt;br&gt;
&lt;br&gt; Response time &lt; 25 ns
&lt;br&gt;
&lt;br&gt; UL1449 3rd Edition, CSA and VDE approved UL: File E332875 CSA: File 224856 VDE: File 40016986 and 40016998 IEC: 60950-1: 2005 Annex Q from ∅ 10 mm
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; 12–48 VDC distribution
&lt;br&gt;
&lt;br&gt; 110–400 V power supply
&lt;br&gt;
&lt;br&gt; Leakage of voltage peaks
&lt;br&gt;
&lt;br&gt; Surge protection in accordance with EN 61000-4-5
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVD_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VD?"&gt;http://katalog.we-online.de/en/pbs/WE-VD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="VARISTOR"/>
</gates>
<devices>
<device name=",820510407" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820511102" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820511111" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820416001" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820417501" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820419501" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820511311" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820511311.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820511401" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820511406" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820511411" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820511511" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820511701" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820511711" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820511911" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820512001" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820512001.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820512111" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820512501" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820512501.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820513001" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820513001.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820515001" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820516001" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820517501" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820519501" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820411102" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820411111" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820411311" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820411311.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820411406" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820411411" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820411511" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820411701" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820411711" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820411911" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820412001" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820412001.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820412111" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820412501" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820413001" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820415001" package="WE-VD_10MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820412311" package="WE-VD_10MM-0.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820413501" package="WE-VD_10MM-0.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820512311" package="WE-VD_10MM-0.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820512311.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820513501" package="WE-VD_10MM-0.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820412511" package="WE-VD_10MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820412511.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820512511" package="WE-VD_10MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820512511.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820412711" package="WE-VD_10MM-1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820412711.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820514001" package="WE-VD_10MM-1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820414001" package="WE-VD_10MM-1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820512711" package="WE-VD_10MM-1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820512711.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820413011" package="WE-VD_10MM-1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820513011" package="WE-VD_10MM-1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820513011.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820413211" package="WE-VD_10MM-1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820513211" package="WE-VD_10MM-1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820413511" package="WE-VD_10MM-1.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820513511" package="WE-VD_10MM-1.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820413811" package="WE-VD_10MM-2.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820513811" package="WE-VD_10MM-2.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820414211" package="WE-VD_10MM-2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820514211" package="WE-VD_10MM-2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820414611" package="WE-VD_10MM-2.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820514611" package="WE-VD_10MM-2.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820514611.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820414811" package="WE-VD_10MM-2.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820514811" package="WE-VD_10MM-2.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820415111" package="WE-VD_10MM-3.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820515111" package="WE-VD_10MM-3.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820415511" package="WE-VD_10MM-3.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820415511B.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820515511" package="WE-VD_10MM-3.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820416211" package="WE-VD_10MM-4.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820516211" package="WE-VD_10MM-4.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820416811" package="WE-VD_10MM-4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820516811" package="WE-VD_10MM-4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820511021" package="WE-VD_10MM-9.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820415511B" package="WE-VD_10MM-3.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VD_14MM" prefix="RV" uservalue="yes">
<description>&lt;b&gt;WE-VD Disk Varistor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; After a surge impulse the varistor works immediately in normal mode so there is no slip current
&lt;br&gt;
&lt;br&gt; Excellent absorption at surge impulses
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC for types up to 95 VRMS –40 ºC to +125 ºC for types from 115 VRMS
&lt;br&gt;
&lt;br&gt; Response time &lt; 25 ns
&lt;br&gt;
&lt;br&gt; UL1449 3rd Edition, CSA and VDE approved UL: File E332875 CSA: File 224856 VDE: File 40016986 and 40016998 IEC: 60950-1: 2005 Annex Q from ∅ 10 mm
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; 12–48 VDC distribution
&lt;br&gt;
&lt;br&gt; 110–400 V power supply
&lt;br&gt;
&lt;br&gt; Leakage of voltage peaks
&lt;br&gt;
&lt;br&gt; Surge protection in accordance with EN 61000-4-5
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVD_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VD?"&gt;http://katalog.we-online.de/en/pbs/WE-VD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="VARISTOR"/>
</gates>
<devices>
<device name=",820441111E" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820441311E" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820441311E.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820441411E" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820441511E" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820441711E" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820442111E" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820445001E" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820446001E" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820447501E" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820449501E" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820441911E" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820541102" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820541311" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820541311.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820541406" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820541406.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820541111" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820541411" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820541511" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820541701" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820541711" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820541911" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820542001" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820542111" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820545001" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820546001" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820547501" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820549501" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820543001" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820543001.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820542501" package="WE-VD_14MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820542501.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820442311E" package="WE-VD_14MM-0.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820443501" package="WE-VD_14MM-0.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820542311" package="WE-VD_14MM-0.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820543501" package="WE-VD_14MM-0.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820442511E" package="WE-VD_14MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820542511" package="WE-VD_14MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820542511.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820442711E" package="WE-VD_14MM-1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820442711E.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820444001" package="WE-VD_14MM-1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820542711" package="WE-VD_14MM-1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820542711.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820544001" package="WE-VD_14MM-1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820443011E" package="WE-VD_14MM-1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820543011" package="WE-VD_14MM-1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820543011.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820443211E" package="WE-VD_14MM-1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820443211E.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820543211" package="WE-VD_14MM-1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820443511E" package="WE-VD_14MM-1.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820543511" package="WE-VD_14MM-1.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820441021E" package="WE-VD_14MM-10.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820541021" package="WE-VD_14MM-10.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820541021.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820443811E" package="WE-VD_14MM-2.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820543811" package="WE-VD_14MM-2.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820444211E" package="WE-VD_14MM-2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820444211E.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820544211" package="WE-VD_14MM-2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820544211.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820444611E" package="WE-VD_14MM-2.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820444611E.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820544611" package="WE-VD_14MM-2.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820544611.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820444811E" package="WE-VD_14MM-2.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820544811" package="WE-VD_14MM-2.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820445111E" package="WE-VD_14MM-3.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820545111" package="WE-VD_14MM-3.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820545111.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820445511E" package="WE-VD_14MM-3.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820445511E.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820545511" package="WE-VD_14MM-3.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820446211E" package="WE-VD_14MM-4.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820446211E.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820546211" package="WE-VD_14MM-4.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820446811E" package="WE-VD_14MM-4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820546811" package="WE-VD_14MM-4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820546811.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VD_20MM" prefix="RV" uservalue="yes">
<description>&lt;b&gt;WE-VD Disk Varistor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; After a surge impulse the varistor works immediately in normal mode so there is no slip current
&lt;br&gt;
&lt;br&gt; Excellent absorption at surge impulses
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC for types up to 95 VRMS –40 ºC to +125 ºC for types from 115 VRMS
&lt;br&gt;
&lt;br&gt; Response time &lt; 25 ns
&lt;br&gt;
&lt;br&gt; UL1449 3rd Edition, CSA and VDE approved UL: File E332875 CSA: File 224856 VDE: File 40016986 and 40016998 IEC: 60950-1: 2005 Annex Q from ∅ 10 mm
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; 12–48 VDC distribution
&lt;br&gt;
&lt;br&gt; 110–400 V power supply
&lt;br&gt;
&lt;br&gt; Leakage of voltage peaks
&lt;br&gt;
&lt;br&gt; Surge protection in accordance with EN 61000-4-5
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVD_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VD?"&gt;http://katalog.we-online.de/en/pbs/WE-VD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="VARISTOR"/>
</gates>
<devices>
<device name=",820421102" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820421111" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820421311" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820421402" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820421411" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820421511" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820421702" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820421711" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820421911" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820422002" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820422111" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820422311" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820422501" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820422506" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820423006" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820423506" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820426001" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820427501" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820429501" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820521102" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820521111" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820521311" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820521311.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820521402" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820521411" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820521511" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820521702" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820521711" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820521911" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820522002" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820522111" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820522311" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820522501" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820522506" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820523006" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820523006.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820523506" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820526001" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820527501" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820527501.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820529501" package="WE-VD_20MM-DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820422511" package="WE-VD_20MM-0.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820522511" package="WE-VD_20MM-0.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820522511.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820422711" package="WE-VD_20MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820422711.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820424001" package="WE-VD_20MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820424006" package="WE-VD_20MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820522711" package="WE-VD_20MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820522711.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820524001" package="WE-VD_20MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820524006" package="WE-VD_20MM-1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820425001" package="WE-VD_20MM-1.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820525001" package="WE-VD_20MM-1.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820423011" package="WE-VD_20MM-1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820523011" package="WE-VD_20MM-1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820423211" package="WE-VD_20MM-1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820423211.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820523211" package="WE-VD_20MM-1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820523211.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820423511" package="WE-VD_20MM-1.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820523511" package="WE-VD_20MM-1.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820521021" package="WE-VD_20MM-10.4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820423811" package="WE-VD_20MM-2.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820523811" package="WE-VD_20MM-2.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820424211" package="WE-VD_20MM-2.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820524211" package="WE-VD_20MM-2.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820424611" package="WE-VD_20MM-2.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820524611" package="WE-VD_20MM-2.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820524611.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820424811" package="WE-VD_20MM-2.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820524811" package="WE-VD_20MM-2.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820425111" package="WE-VD_20MM-2.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820525111" package="WE-VD_20MM-2.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820425511" package="WE-VD_20MM-3.4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820425511.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820525511" package="WE-VD_20MM-3.4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820525511.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820426211" package="WE-VD_20MM-3.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820526211" package="WE-VD_20MM-3.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/index.php?language=en&amp;pf=WE-VD"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820426811" package="WE-VD_20MM-4.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820426811.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820526811" package="WE-VD_20MM-4.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="May 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/820526811.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
<device name=",820523811B" package="WE-VD_20MM-4.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=",820524211B" package="WE-VD_20MM-5.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VE_0402" prefix="RV" uservalue="yes">
<description>&lt;b&gt;WE-VE ESD Suppressor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast response time
&lt;br&gt;
&lt;br&gt; No leakage current
&lt;br&gt;
&lt;br&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Almost no energy consumption in stand-by mode
&lt;br&gt;
&lt;br&gt; Excellent absorption for ESD-impulses
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;
&lt;br&gt; Nickel barrier
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection of data lines
&lt;br&gt;
&lt;br&gt; Protection of bus systems
&lt;br&gt;
&lt;br&gt; Protection of semiconductors
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2 – 8 kV contact discharge – 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVE_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVE_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VE?"&gt;http://katalog.we-online.de/en/pbs/WE-VE?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-VE"/>
</gates>
<devices>
<device name="" package="WESURGE_0402_REFLOW">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_82357050100"/>
<technology name="_82357050220"/>
<technology name="_82357050330"/>
<technology name="_82357050560"/>
<technology name="_82357120050"/>
<technology name="_82357120100"/>
<technology name="_82357120220"/>
<technology name="_82357240010"/>
<technology name="_82357240030"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VEA_0508" prefix="RV" uservalue="yes">
<description>&lt;b&gt;WE-VEA ESD Suppressor-Array
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; &lt;br&gt;Fast response time (1 ns)
&lt;br&gt;
&lt;br&gt; Low signal insertion loss
&lt;br&gt;
&lt;br&gt; No leakage current
&lt;br&gt;
&lt;br&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Almost no energy consumption in stand-by mode
&lt;br&gt;
&lt;br&gt; Excellent absorption for ESD-impulses
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection of data lines
&lt;br&gt;
&lt;br&gt; Protection of bus systems
&lt;br&gt;
&lt;br&gt; Protection of video transmission lines
&lt;br&gt;
&lt;br&gt; Protection of semiconductors
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVEA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVEA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VEA?"&gt;http://katalog.we-online.de/en/pbs/WE-VEA?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-VEA"/>
</gates>
<devices>
<device name="_82380050100" package="WE-VEA_0508">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="7"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="4"/>
<connect gate="G$1" pin="8" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VE_ULC_0402" prefix="D" uservalue="yes">
<description>&lt;b&gt; WE-VE ULC ESD Suppressor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast response time
&lt;br&gt;
&lt;br&gt; No leakage current
&lt;br&gt;
&lt;br&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Almost no energy consumption in stand-by mode
&lt;br&gt;
&lt;br&gt; Excellent absorption for ESD-impulses
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;
&lt;br&gt; Nickel barrier
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection of data lines
&lt;br&gt;
&lt;br&gt; Protection of bus systems
&lt;br&gt;
&lt;br&gt; Protection of semiconductors
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2 – 8 kV contact discharge – 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVE_ULC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVE_ULC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VE_ULC?"&gt;http://katalog.we-online.de/en/pbs/WE-VE_ULC?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-VE"/>
</gates>
<devices>
<device name="_82307050029" package="WE-VE_ULC_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VS_0402" prefix="RV" uservalue="yes">
<description>&lt;b&gt;WE-VS SMD Varistor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast response time
&lt;br&gt;
&lt;br&gt; Low leakage current
&lt;br&gt;
&lt;br&gt; Nickel barrier for leadfree soldering
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection of DC distribution
&lt;br&gt;
&lt;br&gt; Protection of power supply
&lt;br&gt;
&lt;br&gt; Protection of bus systems and communication lines
&lt;br&gt;
&lt;br&gt; Limiting of overvoltages
&lt;br&gt;
&lt;br&gt; Protection of semiconductors
&lt;br&gt;
&lt;br&gt; Surge protection in accordance with EN 61000-4-5
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2
&lt;br&gt;
&lt;br&gt; Burst protection in accordance with EN 61000-4-4
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VS?"&gt;http://katalog.we-online.de/en/pbs/WE-VS?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="VARISTOR"/>
</gates>
<devices>
<device name="_WAVE" package="WESURGE_0402_WAVE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_82537040"/>
<technology name="_82537070"/>
<technology name="_82537110"/>
<technology name="_82557060"/>
<technology name="_82557140"/>
</technologies>
</device>
<device name="_REFLOW" package="WESURGE_0402_REFLOW">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_82537040"/>
<technology name="_82537070"/>
<technology name="_82537110"/>
<technology name="_82557060"/>
<technology name="_82557140"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-WPCC_1W(RX)" prefix="L" uservalue="yes">
<description>&lt;b&gt;Wireless Power Charging Coil&lt;/b&gt;&lt;br&gt;
-Qi standard compliant&lt;br&gt;
-Thinnest on the market&lt;br&gt;
-Easiness of assembly&lt;br&gt;
-Evaluated and approved by very major semiconductor manufacturer&lt;br&gt;
-Litz wire-highest Q-value on the market&lt;br&gt;
-Applicable for up to 5W&lt;br&gt;
-High permeability shielding&lt;br&gt;
-Cancels charging flux to be not coupled into sensitive components or batteries&lt;br&gt;
-High reliable construction&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
-- Portable devices used in a clean area .where connectors pose a risk of polluting e.g. medical facilities,(industrial )clean rooms,mining industry&lt;br&gt;
--Devices with a large number of mating cycles to avoid connector damage:eg.Smart watches,fittness tracker...&lt;br&gt;
--Consumer products:eg. Digital cameras,baby phone,walkie talky remote control,smartphone sleeves,watertight products&lt;br&gt;
--Explosion sensitive area where the use of a physical connection is hazardous&lt;br&gt;
--Smart sensors&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtWPCC_Receiver_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtWPCC_Receiver_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-WPCC_Receiver"&gt;http://katalog.we-online.de/en/pbs/WE-WPCC_Receiver&lt;/a&gt;&lt;p&gt;


Created by  Dan Xu 2014-05-21&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="_760308102210" package="WE-WPCC_3737">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308103204" package="WE-WPCC_3830">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308103202" package="WE-WPCC_4832">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308102213" package="WE-WPCC_2929">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308101214" package="WE-WPCC_Φ19">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308103206" package="WE-WPCC_2815">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308103205" package="WE-WPCC_3426">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308102207" package="WE-WPCC_4040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308103211" package="WE-WPCC_4636">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308101208" package="WE-WPCC_Φ10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308101216" package="WE-WPCC_Φ6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308101219" package="WE-WPCC_Φ15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308101220" package="WE-WPCC_Φ17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308101303" package="WE-WPCC_Φ26">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308103215" package="WE-WPCC_4832_760308103215">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308103203" package="WE-WPCC_4832">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308101208A" package="WE-WPCC_Φ10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308101217" package="WE-WPCC_Φ10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-WPCC_3W" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Coil
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Qi-standard compliant
&lt;br&gt;
&lt;br&gt; Evaluated and approved by every major semiconductor manufacturer
&lt;br&gt;
&lt;br&gt; Litzwire used – highest Q-value available on market
&lt;br&gt;
&lt;br&gt; Applicable for up to 20 W
&lt;br&gt;
&lt;br&gt; High permeability shielding
&lt;br&gt;
&lt;br&gt; Cancels charging flux to be not coupled into sensitive components or batteries
&lt;br&gt;
&lt;br&gt; High reliable construction
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable devices used in a clean area, where connectors pose a risk of polluting e.g. medical facilities, (industrial) clean rooms, mining industry
&lt;br&gt;
&lt;br&gt; Devices with a large number of mating cycles to avoid connector damage: eg. Smart watches, fitness tracker …
&lt;br&gt;
&lt;br&gt; Consumer products: eg. Digital cameras, baby phone, walkie talky, remote control, smartphone sleeves, watertight products
&lt;br&gt;
&lt;br&gt; Explosion sensitive area where the use of a physical connection is hazardous
&lt;br&gt;
&lt;br&gt; Smart sensors
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/WE-WPCC_Array_106_104119_104120.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/WE-WPCC_Array_106_104119_104120.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-WPCC-ARRAY"&gt;http://katalog.we-online.de/en/pbs/WE-WPCC-ARRAY&lt;/a&gt;&lt;p&gt;


Created by  Dan Xu 2014-05-21&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-3W"/>
</gates>
<devices>
<device name="_760308104120" package="WE-WPCC_A28">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308106" package="WE-WPCC_A6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP7_750310799" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE_FB_EP7_DIMENSION1">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="5 6"/>
<connect gate="G$1" pin="3" pad="7 8"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP7_750370040" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE_FB_EP7_DIMENSION1">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="5 6"/>
<connect gate="G$1" pin="3" pad="7 8"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP7_750370041" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE_FB_EP7_DIMENSION1">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="5 6"/>
<connect gate="G$1" pin="3" pad="7 8"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP7_750370047" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE_FB_EP7_DIMENSION2">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="5 6"/>
<connect gate="G$1" pin="3" pad="7 8"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP7_750370058" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE_FB_EP7_DIMENSION2">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="5 6"/>
<connect gate="G$1" pin="3" pad="7 8"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP7_750370059" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE_FB_EP7_DIMENSION2">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="5 6"/>
<connect gate="G$1" pin="3" pad="7 8"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP7_750311692" prefix="T">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_1W:2W"/>
</gates>
<devices>
<device name="" package="WE_FB_EP7_DIMENSION1">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="8"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="7"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP10" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-FB_EP10">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="5 6"/>
<connect gate="G$1" pin="3" pad="7 8"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="4"/>
</connects>
<technologies>
<technology name="_750310471"/>
<technology name="_750310559"/>
<technology name="_750310562"/>
<technology name="_750310563"/>
<technology name="_750311303"/>
<technology name="_750311304"/>
<technology name="_750311305"/>
<technology name="_750311306"/>
<technology name="_750311307"/>
<technology name="_750311308"/>
<technology name="_750311567"/>
<technology name="_750311675"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP10_750310564">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-FB_EP10">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="8"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="7"/>
<connect gate="G$1" pin="6" pad="1"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP10_750311342" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:2W_2"/>
</gates>
<devices>
<device name="" package="WE-FB_EP10">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="8"/>
<connect gate="G$1" pin="5" pad="7"/>
<connect gate="G$1" pin="6" pad="1"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP13_750311486" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-FB_EP13_DIMENSION1">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="10"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="9"/>
<connect gate="G$1" pin="5" pad="7"/>
<connect gate="G$1" pin="6" pad="1"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP13_750311681">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-FB_EP13_DIMENSION1">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="10"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="9"/>
<connect gate="G$1" pin="5" pad="7"/>
<connect gate="G$1" pin="6" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP13" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-FB_EP13_DIMENSION1">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="6 7"/>
<connect gate="G$1" pin="3" pad="9 10"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="5"/>
</connects>
<technologies>
<technology name="_750311422"/>
<technology name="_750311423"/>
<technology name="_750311424"/>
<technology name="_750311456"/>
<technology name="_750311457"/>
<technology name="_750311458"/>
<technology name="_750311564"/>
<technology name="_750311624"/>
<technology name="_750311625"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP13_750311856" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:4W"/>
</gates>
<devices>
<device name="" package="WE-FB_EP13_DIMENSION2">
<connects>
<connect gate="G$1" pin="1" pad="14"/>
<connect gate="G$1" pin="10" pad="9"/>
<connect gate="G$1" pin="11" pad="16"/>
<connect gate="G$1" pin="12" pad="11"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="5"/>
<connect gate="G$1" pin="7" pad="6"/>
<connect gate="G$1" pin="8" pad="7"/>
<connect gate="G$1" pin="9" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP13_750311439" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-FB_EP13_DIMENSION1">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP13_750311688" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-FB_EP13_DIMENSION1">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6 7"/>
<connect gate="G$1" pin="3" pad="9 10"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EP13_750311689" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-FB_EP13_DIMENSION1">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="6 7"/>
<connect gate="G$1" pin="3" pad="9 10"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="2"/>
<connect gate="G$1" pin="6" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_ER9.5" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:2W"/>
</gates>
<devices>
<device name="_750370042" package="WE-FB_ER9.5">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="1"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EE16/8/5" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="WE-FB_EE16/8/5"/>
</gates>
<devices>
<device name="_750811048" package="WE-FB_EE16/8/5">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="8"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="1"/>
<connect gate="G$1" pin="7" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EE20/10/6" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="WE-FB_EE20/10/6"/>
</gates>
<devices>
<device name="_750311911" package="WE-FB_EE20/10/6">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="10" pad="6"/>
<connect gate="G$1" pin="11" pad="5"/>
<connect gate="G$1" pin="12" pad="3"/>
<connect gate="G$1" pin="13" pad="1"/>
<connect gate="G$1" pin="14" pad="4"/>
<connect gate="G$1" pin="2" pad="14"/>
<connect gate="G$1" pin="3" pad="13"/>
<connect gate="G$1" pin="4" pad="12"/>
<connect gate="G$1" pin="5" pad="11"/>
<connect gate="G$1" pin="6" pad="10"/>
<connect gate="G$1" pin="7" pad="9"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EFD20" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_3W:3W"/>
</gates>
<devices>
<device name="" package="WE-FB_EFD20">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="10" pad="5"/>
<connect gate="G$1" pin="11" pad="3"/>
<connect gate="G$1" pin="12" pad="4"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="11"/>
<connect gate="G$1" pin="5" pad="10"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="8"/>
<connect gate="G$1" pin="8" pad="7"/>
<connect gate="G$1" pin="9" pad="6"/>
</connects>
<technologies>
<technology name="_750310617"/>
<technology name="_750311385"/>
<technology name="_750311597"/>
<technology name="_750311598"/>
<technology name="_750311605"/>
<technology name="_750311607"/>
<technology name="_750311797"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EFD20_750311599" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_3W:2W"/>
</gates>
<devices>
<device name="" package="WE-FB_EFD20">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="10" pad="4"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="11"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="6"/>
<connect gate="G$1" pin="8" pad="5"/>
<connect gate="G$1" pin="9" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EFD20_750311600" prefix="T">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_3W:2W"/>
</gates>
<devices>
<device name="" package="WE-FB_EFD20">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="10" pad="4"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="11"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="6"/>
<connect gate="G$1" pin="8" pad="5"/>
<connect gate="G$1" pin="9" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EFD20_750311604">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_3W:2W"/>
</gates>
<devices>
<device name="" package="WE-FB_EFD20">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="10" pad="4"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="11"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="6"/>
<connect gate="G$1" pin="8" pad="5"/>
<connect gate="G$1" pin="9" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EFD20_750311608" prefix="L" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_3W:2W"/>
</gates>
<devices>
<device name="" package="WE-FB_EFD20">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="10" pad="4"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="11"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="6"/>
<connect gate="G$1" pin="8" pad="5"/>
<connect gate="G$1" pin="9" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EFD25_750311889" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-FB_EFD25_DIMENSION1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="4" pad="9"/>
<connect gate="G$1" pin="5" pad="7"/>
<connect gate="G$1" pin="6" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EFD25" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_3W:3W"/>
</gates>
<devices>
<device name="" package="WE-FB_EFD25_DIMENSION1">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="10" pad="5"/>
<connect gate="G$1" pin="11" pad="3"/>
<connect gate="G$1" pin="12" pad="4"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="11"/>
<connect gate="G$1" pin="5" pad="10"/>
<connect gate="G$1" pin="6" pad="7"/>
<connect gate="G$1" pin="7" pad="8"/>
<connect gate="G$1" pin="8" pad="9"/>
<connect gate="G$1" pin="9" pad="6"/>
</connects>
<technologies>
<technology name="_750311589"/>
<technology name="_750311590"/>
<technology name="_750311591"/>
<technology name="_750311592"/>
<technology name="_750311593"/>
<technology name="_750311594"/>
<technology name="_750311595"/>
<technology name="_750311596"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EFD25_750311771" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_3W:3W_2"/>
</gates>
<devices>
<device name="" package="WE-FB_EFD25_DIMENSION1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="4"/>
<connect gate="G$1" pin="11" pad="2"/>
<connect gate="G$1" pin="12" pad="3"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="3" pad="11"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="7"/>
<connect gate="G$1" pin="6" pad="8"/>
<connect gate="G$1" pin="7" pad="9"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="9" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EFD25_750310988" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_2W:1W_1"/>
</gates>
<devices>
<device name="" package="WE-FB_EFD25_DIMENSION1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EFD25_750311783" prefix="T" uservalue="yes">
<description>&lt;b&gt; &lt;b&gt; WE-FB Flyback Transformer LT35xx / LT3748&lt;/B&gt;
&lt;br&gt;
&lt;BR&gt;
Characteristics
&lt;br&gt; &lt;/B&gt;Standard transformers for various output voltages currents available&lt;BR&gt;&lt;/B&gt;
 Easy design of custom power supply due to standard circuit and change of transformers and two components for feedback loop&lt;BR&gt;
Isolation voltage up to 2.5 kV
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications &lt;BR&gt;
&lt;/B&gt; Isolated power design&lt;BR&gt;
Sensor interfaces&lt;BR&gt;
Isolated telecom converters&lt;BR&gt;
 Power over Ethernet&lt;BR&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFB_LT_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtFB_LT_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FB_Linear?"&gt;http://katalog.we-online.de/en/pbs/WE-FB_Linear?&lt;/a&gt;&lt;p&gt;


Updated 2015-04-03&lt;br&gt;
2015 (C) Wurth Elektronik
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L_3W:3W"/>
</gates>
<devices>
<device name="" package="WE-FB_EFD25_DIMENSION1">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="10" pad="5"/>
<connect gate="G$1" pin="11" pad="3"/>
<connect gate="G$1" pin="12" pad="4"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="11"/>
<connect gate="G$1" pin="5" pad="10"/>
<connect gate="G$1" pin="6" pad="7"/>
<connect gate="G$1" pin="7" pad="8"/>
<connect gate="G$1" pin="8" pad="9"/>
<connect gate="G$1" pin="9" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HV-LAN_749024012" prefix="T" uservalue="yes">
<description>&lt;B&gt;WE-LAN HV LAN-Transformer&lt;p&gt;

Characteristics:&lt;pRE&gt;
•Compliant with IEEE802.3 and 802.3af standards
•Operating temperature: 0 °C to +70 °C
•SMD
•4 kV Hipot test&lt;PRE&gt;

&lt;B&gt;Applications:&lt;PRE&gt;&lt;/B&gt;
•Ethernet
•Compliant with most IC's for Ethernet applications 
like Intel, AMD, Conexant, Realtek, etc.
•Hub, Router, Switches, medical applications

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/749024012?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/749024012?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="LAN1" symbol="749024012"/>
</gates>
<devices>
<device name="" package="749024012">
<connects>
<connect gate="LAN1" pin="D+" pad="1"/>
<connect gate="LAN1" pin="D-" pad="3"/>
<connect gate="LAN1" pin="D1+" pad="6"/>
<connect gate="LAN1" pin="D1-" pad="8"/>
<connect gate="LAN1" pin="D2+" pad="11"/>
<connect gate="LAN1" pin="D2-" pad="13"/>
<connect gate="LAN1" pin="D3+" pad="16"/>
<connect gate="LAN1" pin="D3-" pad="18"/>
<connect gate="LAN1" pin="TD" pad="2"/>
<connect gate="LAN1" pin="TD1" pad="7"/>
<connect gate="LAN1" pin="TD2" pad="12"/>
<connect gate="LAN1" pin="TD3" pad="17"/>
<connect gate="LAN1" pin="TX" pad="39"/>
<connect gate="LAN1" pin="TX1" pad="34"/>
<connect gate="LAN1" pin="TX2" pad="29"/>
<connect gate="LAN1" pin="TX3" pad="24"/>
<connect gate="LAN1" pin="X+" pad="40"/>
<connect gate="LAN1" pin="X-" pad="38"/>
<connect gate="LAN1" pin="X1+" pad="35"/>
<connect gate="LAN1" pin="X1-" pad="33"/>
<connect gate="LAN1" pin="X2+" pad="30"/>
<connect gate="LAN1" pin="X2-" pad="28"/>
<connect gate="LAN1" pin="X3+" pad="25"/>
<connect gate="LAN1" pin="X3-" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HV-LAN_749014010" prefix="T" uservalue="yes">
<description>&lt;B&gt;WE-LAN HV LAN-Transformer&lt;p&gt;

Characteristics:&lt;pRE&gt;
•Compliant with IEEE802.3 and 802.3af standards
•Operating temperature: 0 °C to +70 °C
•SMD
•4 kV Hipot test&lt;PRE&gt;

&lt;B&gt;Applications:&lt;PRE&gt;&lt;/B&gt;
•Ethernet
•Compliant with most IC's for Ethernet applications 
like Intel, AMD, Conexant, Realtek, etc.
•Hub, Router, Switches, medical applications


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/749014010"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/749014010?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="LAN" symbol="749014010"/>
</gates>
<devices>
<device name="" package="749014010">
<connects>
<connect gate="LAN" pin="CRD" pad="2"/>
<connect gate="LAN" pin="CRX" pad="11"/>
<connect gate="LAN" pin="CTD" pad="5"/>
<connect gate="LAN" pin="CTX" pad="8"/>
<connect gate="LAN" pin="RD+" pad="1"/>
<connect gate="LAN" pin="RD-" pad="3"/>
<connect gate="LAN" pin="RX+" pad="12"/>
<connect gate="LAN" pin="RX-" pad="10"/>
<connect gate="LAN" pin="TD+" pad="4"/>
<connect gate="LAN" pin="TD-" pad="6"/>
<connect gate="LAN" pin="TX+" pad="9"/>
<connect gate="LAN" pin="TX-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HV-LAN_749014011" prefix="T" uservalue="yes">
<description>&lt;B&gt;WE-LAN HV LAN-Transformer&lt;p&gt;

Characteristics:&lt;pRE&gt;
•Compliant with IEEE802.3 and 802.3af standards
•Operating temperature: 0 °C to +70 °C
•SMD
•4 kV Hipot test&lt;PRE&gt;

&lt;B&gt;Applications:&lt;PRE&gt;&lt;/B&gt;
•Ethernet
•Compliant with most IC's for Ethernet applications 
like Intel, AMD, Conexant, Realtek, etc.
•Hub, Router, Switches, medical applications


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN"&gt;http://katalog.we-online.de/en/pbs/WE-LAN&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="LAN" symbol="749014011"/>
</gates>
<devices>
<device name="" package="74901401X">
<connects>
<connect gate="LAN" pin="CRD" pad="2"/>
<connect gate="LAN" pin="CRX" pad="15"/>
<connect gate="LAN" pin="CTD" pad="7"/>
<connect gate="LAN" pin="CTX" pad="10"/>
<connect gate="LAN" pin="RD+" pad="1"/>
<connect gate="LAN" pin="RD-" pad="3"/>
<connect gate="LAN" pin="RX+" pad="16"/>
<connect gate="LAN" pin="RX-" pad="14"/>
<connect gate="LAN" pin="TD+" pad="6"/>
<connect gate="LAN" pin="TD-" pad="8"/>
<connect gate="LAN" pin="TX+" pad="11"/>
<connect gate="LAN" pin="TX-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HV-LAN_749014012" prefix="T">
<description>&lt;B&gt;WE-LAN HV LAN-Transformer&lt;p&gt;

Characteristics:&lt;pRE&gt;
•Compliant with IEEE802.3 and 802.3af standards
•Operating temperature: 0 °C to +70 °C
•SMD
•4 kV Hipot test&lt;PRE&gt;

&lt;B&gt;Applications:&lt;PRE&gt;&lt;/B&gt;
•Ethernet
•Compliant with most IC's for Ethernet applications 
like Intel, AMD, Conexant, Realtek, etc.
•Hub, Router, Switches, medical applications


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN"&gt;http://katalog.we-online.de/en/pbs/WE-LAN&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="LAN" symbol="749014012"/>
</gates>
<devices>
<device name="" package="74901401X">
<connects>
<connect gate="LAN" pin="CRD" pad="2"/>
<connect gate="LAN" pin="CRX" pad="15"/>
<connect gate="LAN" pin="CTD" pad="7"/>
<connect gate="LAN" pin="CTX" pad="10"/>
<connect gate="LAN" pin="RD+" pad="1"/>
<connect gate="LAN" pin="RD-" pad="3"/>
<connect gate="LAN" pin="RX+" pad="16"/>
<connect gate="LAN" pin="RX-" pad="14"/>
<connect gate="LAN" pin="TD+" pad="6"/>
<connect gate="LAN" pin="TD-" pad="8"/>
<connect gate="LAN" pin="TX+" pad="11"/>
<connect gate="LAN" pin="TX-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HV-LAN_749014013" prefix="T">
<description>&lt;B&gt;WE-LAN HV LAN-Transformer&lt;p&gt;

Characteristics:&lt;pRE&gt;
•Compliant with IEEE802.3 and 802.3af standards
•Operating temperature: 0 °C to +70 °C
•SMD
•4 kV Hipot test&lt;PRE&gt;

&lt;B&gt;Applications:&lt;PRE&gt;&lt;/B&gt;
•Ethernet
•Compliant with most IC's for Ethernet applications 
like Intel, AMD, Conexant, Realtek, etc.
•Hub, Router, Switches, medical applications

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/749014013"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/749014013&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="LAN" symbol="749014013"/>
</gates>
<devices>
<device name="" package="74901401X">
<connects>
<connect gate="LAN" pin="CRD" pad="2"/>
<connect gate="LAN" pin="CRX" pad="15"/>
<connect gate="LAN" pin="CTD" pad="7"/>
<connect gate="LAN" pin="CTX" pad="10"/>
<connect gate="LAN" pin="RD+" pad="1"/>
<connect gate="LAN" pin="RD-" pad="3"/>
<connect gate="LAN" pin="RX+" pad="16"/>
<connect gate="LAN" pin="RX-" pad="14"/>
<connect gate="LAN" pin="TD+" pad="6"/>
<connect gate="LAN" pin="TD-" pad="8"/>
<connect gate="LAN" pin="TX+" pad="11"/>
<connect gate="LAN" pin="TX-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_749020020A" prefix="T" uservalue="yes">
<description>&lt;b&gt;LAN-Transformer WE-LAN 10/100/1000 Base Tx&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3 standards&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/S/749020020A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/S/749020020A?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="LAN1" symbol="749020020A"/>
<gate name="LAN2" symbol="749020020A"/>
</gates>
<devices>
<device name="" package="749020020A">
<connects>
<connect gate="LAN1" pin="MCT1" pad="48"/>
<connect gate="LAN1" pin="MCT2" pad="45"/>
<connect gate="LAN1" pin="MCT3" pad="42"/>
<connect gate="LAN1" pin="MCT4" pad="39"/>
<connect gate="LAN1" pin="MX1+" pad="47"/>
<connect gate="LAN1" pin="MX1-" pad="46"/>
<connect gate="LAN1" pin="MX2+" pad="44"/>
<connect gate="LAN1" pin="MX2-" pad="43"/>
<connect gate="LAN1" pin="MX3+" pad="41"/>
<connect gate="LAN1" pin="MX3-" pad="40"/>
<connect gate="LAN1" pin="MX4+" pad="38"/>
<connect gate="LAN1" pin="MX4-" pad="37"/>
<connect gate="LAN1" pin="TCT1" pad="1"/>
<connect gate="LAN1" pin="TCT2" pad="4"/>
<connect gate="LAN1" pin="TCT3" pad="7"/>
<connect gate="LAN1" pin="TCT4" pad="10"/>
<connect gate="LAN1" pin="TD1+" pad="2"/>
<connect gate="LAN1" pin="TD1-" pad="3"/>
<connect gate="LAN1" pin="TD2+" pad="5"/>
<connect gate="LAN1" pin="TD2-" pad="6"/>
<connect gate="LAN1" pin="TD3+" pad="8"/>
<connect gate="LAN1" pin="TD3-" pad="9"/>
<connect gate="LAN1" pin="TD4+" pad="11"/>
<connect gate="LAN1" pin="TD4-" pad="12"/>
<connect gate="LAN2" pin="MCT1" pad="36"/>
<connect gate="LAN2" pin="MCT2" pad="33"/>
<connect gate="LAN2" pin="MCT3" pad="30"/>
<connect gate="LAN2" pin="MCT4" pad="27"/>
<connect gate="LAN2" pin="MX1+" pad="35"/>
<connect gate="LAN2" pin="MX1-" pad="34"/>
<connect gate="LAN2" pin="MX2+" pad="32"/>
<connect gate="LAN2" pin="MX2-" pad="31"/>
<connect gate="LAN2" pin="MX3+" pad="29"/>
<connect gate="LAN2" pin="MX3-" pad="28"/>
<connect gate="LAN2" pin="MX4+" pad="26"/>
<connect gate="LAN2" pin="MX4-" pad="25"/>
<connect gate="LAN2" pin="TCT1" pad="13"/>
<connect gate="LAN2" pin="TCT2" pad="16"/>
<connect gate="LAN2" pin="TCT3" pad="19"/>
<connect gate="LAN2" pin="TCT4" pad="22"/>
<connect gate="LAN2" pin="TD1+" pad="14"/>
<connect gate="LAN2" pin="TD1-" pad="15"/>
<connect gate="LAN2" pin="TD2+" pad="17"/>
<connect gate="LAN2" pin="TD2-" pad="18"/>
<connect gate="LAN2" pin="TD3+" pad="20"/>
<connect gate="LAN2" pin="TD3-" pad="21"/>
<connect gate="LAN2" pin="TD4+" pad="23"/>
<connect gate="LAN2" pin="TD4-" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_749020100" prefix="T" uservalue="yes">
<description>&lt;b&gt;LAN-Transformer WE-LAN 10/10/1000 Base Tx&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3 standards&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/S/749020100?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/S/749020100?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="749020100"/>
</gates>
<devices>
<device name="" package="749020100">
<connects>
<connect gate="G$1" pin="D+" pad="1"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="D1+" pad="7"/>
<connect gate="G$1" pin="D1-" pad="8"/>
<connect gate="G$1" pin="TD1" pad="3"/>
<connect gate="G$1" pin="TD2" pad="6"/>
<connect gate="G$1" pin="TX" pad="14"/>
<connect gate="G$1" pin="TX1" pad="11"/>
<connect gate="G$1" pin="X+" pad="16"/>
<connect gate="G$1" pin="X-" pad="15"/>
<connect gate="G$1" pin="X1+" pad="10"/>
<connect gate="G$1" pin="X1-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_749022015" prefix="T" uservalue="yes">
<description>&lt;b&gt;LAN-Transformer WE-LAN 10/10/1000 Base Tx&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3 standards&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/S/749022015?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/S/749022015?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="LAN1" symbol="749022015"/>
</gates>
<devices>
<device name="" package="749022015">
<connects>
<connect gate="LAN1" pin="D1+" pad="2"/>
<connect gate="LAN1" pin="D1-" pad="3"/>
<connect gate="LAN1" pin="D2+" pad="5"/>
<connect gate="LAN1" pin="D2-" pad="6"/>
<connect gate="LAN1" pin="D3+" pad="8"/>
<connect gate="LAN1" pin="D3-" pad="9"/>
<connect gate="LAN1" pin="D4+" pad="11"/>
<connect gate="LAN1" pin="D4-" pad="12"/>
<connect gate="LAN1" pin="TD1" pad="1"/>
<connect gate="LAN1" pin="TD2" pad="4"/>
<connect gate="LAN1" pin="TD3" pad="7"/>
<connect gate="LAN1" pin="TD4" pad="10"/>
<connect gate="LAN1" pin="TX1" pad="24"/>
<connect gate="LAN1" pin="TX2" pad="21"/>
<connect gate="LAN1" pin="TX3" pad="18"/>
<connect gate="LAN1" pin="TX4" pad="15"/>
<connect gate="LAN1" pin="X1+" pad="23"/>
<connect gate="LAN1" pin="X1-" pad="22"/>
<connect gate="LAN1" pin="X2+" pad="20"/>
<connect gate="LAN1" pin="X2-" pad="19"/>
<connect gate="LAN1" pin="X3+" pad="17"/>
<connect gate="LAN1" pin="X3-" pad="16"/>
<connect gate="LAN1" pin="X4+" pad="14"/>
<connect gate="LAN1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_749023010A" prefix="T" uservalue="yes">
<description>&lt;b&gt;LAN-Transformer WE-LAN 10/10/1000 Base Tx&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3 standards&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch




&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/S/749023010A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/S/749023010A?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="749023010A"/>
</gates>
<devices>
<device name="" package="749023010A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_749023015" prefix="T" uservalue="yes">
<description>&lt;b&gt;LAN-Transformer WE-LAN 10/10/1000 Base Tx&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3 standards&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/S/749023015?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/S/749023015?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="LAN1" symbol="749023015"/>
</gates>
<devices>
<device name="" package="749023015">
<connects>
<connect gate="LAN1" pin="D1+" pad="2"/>
<connect gate="LAN1" pin="D1-" pad="3"/>
<connect gate="LAN1" pin="D2+" pad="5"/>
<connect gate="LAN1" pin="D2-" pad="6"/>
<connect gate="LAN1" pin="D3+" pad="8"/>
<connect gate="LAN1" pin="D3-" pad="9"/>
<connect gate="LAN1" pin="D4+" pad="11"/>
<connect gate="LAN1" pin="D4-" pad="12"/>
<connect gate="LAN1" pin="TD1" pad="1"/>
<connect gate="LAN1" pin="TD2" pad="4"/>
<connect gate="LAN1" pin="TD3" pad="7"/>
<connect gate="LAN1" pin="TD4" pad="10"/>
<connect gate="LAN1" pin="TX1" pad="24"/>
<connect gate="LAN1" pin="TX2" pad="21"/>
<connect gate="LAN1" pin="TX3" pad="18"/>
<connect gate="LAN1" pin="TX4" pad="15"/>
<connect gate="LAN1" pin="X1+" pad="23"/>
<connect gate="LAN1" pin="X1-" pad="22"/>
<connect gate="LAN1" pin="X2+" pad="20"/>
<connect gate="LAN1" pin="X2-" pad="19"/>
<connect gate="LAN1" pin="X3+" pad="17"/>
<connect gate="LAN1" pin="X3-" pad="16"/>
<connect gate="LAN1" pin="X4+" pad="14"/>
<connect gate="LAN1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_749023016" prefix="T" uservalue="yes">
<description>&lt;b&gt;LAN-Transformer WE-LAN 10/10/1000 Base Tx&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3 standards&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/S/749023016?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/S/749023016?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="LAN1" symbol="749023016"/>
</gates>
<devices>
<device name="" package="749023016">
<connects>
<connect gate="LAN1" pin="D1+" pad="2"/>
<connect gate="LAN1" pin="D1-" pad="3"/>
<connect gate="LAN1" pin="D2+" pad="5"/>
<connect gate="LAN1" pin="D2-" pad="6"/>
<connect gate="LAN1" pin="D3+" pad="8"/>
<connect gate="LAN1" pin="D3-" pad="9"/>
<connect gate="LAN1" pin="D4+" pad="11"/>
<connect gate="LAN1" pin="D4-" pad="12"/>
<connect gate="LAN1" pin="TD1" pad="1"/>
<connect gate="LAN1" pin="TD2" pad="4"/>
<connect gate="LAN1" pin="TD3" pad="7"/>
<connect gate="LAN1" pin="TD4" pad="10"/>
<connect gate="LAN1" pin="TX1" pad="24"/>
<connect gate="LAN1" pin="TX2" pad="21"/>
<connect gate="LAN1" pin="TX3" pad="18"/>
<connect gate="LAN1" pin="TX4" pad="15"/>
<connect gate="LAN1" pin="X1+" pad="23"/>
<connect gate="LAN1" pin="X1-" pad="22"/>
<connect gate="LAN1" pin="X2+" pad="20"/>
<connect gate="LAN1" pin="X2-" pad="19"/>
<connect gate="LAN1" pin="X3+" pad="17"/>
<connect gate="LAN1" pin="X3-" pad="16"/>
<connect gate="LAN1" pin="X4+" pad="14"/>
<connect gate="LAN1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN-10G_749050010A" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;/b&gt;&lt;p&gt;
- Compliant with standards: IEEE 802.3an and upcoming IEEE 802.3bt&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Ethernet speed up to 10Gbit/s&lt;br&gt;
--Power over Ethernet PoE and PoE+&lt;br&gt;
--10Gbit with ETR and PoE up to 150 W (for industrial applications)&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-10G"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-10G&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="LAN1" symbol="749050010A-1"/>
</gates>
<devices>
<device name="" package="749050010A">
<connects>
<connect gate="LAN1" pin="D1+" pad="2"/>
<connect gate="LAN1" pin="D1-" pad="3"/>
<connect gate="LAN1" pin="D2+" pad="5"/>
<connect gate="LAN1" pin="D2-" pad="6"/>
<connect gate="LAN1" pin="D3+" pad="8"/>
<connect gate="LAN1" pin="D3-" pad="9"/>
<connect gate="LAN1" pin="D4+" pad="11"/>
<connect gate="LAN1" pin="D4-" pad="12"/>
<connect gate="LAN1" pin="TD1" pad="1"/>
<connect gate="LAN1" pin="TD2" pad="4"/>
<connect gate="LAN1" pin="TD3" pad="7"/>
<connect gate="LAN1" pin="TD4" pad="10"/>
<connect gate="LAN1" pin="TX1" pad="24"/>
<connect gate="LAN1" pin="TX2" pad="21"/>
<connect gate="LAN1" pin="TX3" pad="18"/>
<connect gate="LAN1" pin="TX4" pad="15"/>
<connect gate="LAN1" pin="X1+" pad="23"/>
<connect gate="LAN1" pin="X1-" pad="22"/>
<connect gate="LAN1" pin="X2+" pad="20"/>
<connect gate="LAN1" pin="X2-" pad="19"/>
<connect gate="LAN1" pin="X3+" pad="17"/>
<connect gate="LAN1" pin="X3-" pad="16"/>
<connect gate="LAN1" pin="X4+" pad="14"/>
<connect gate="LAN1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499010441" prefix="T" uservalue="yes">
<description>&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;WE-RJ45 LAN
 THT Surge Protection&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
&lt;PRE&gt;
 &lt;/PRE&gt;&lt;font color="#0000FF"&gt;&lt;B&gt;Characteristics:&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
&lt;PRE&gt;
 With two integrated gas discharge tubes
 High surge withstand voltage
 Small capacitance of surge device
&lt;PRE&gt;
&lt;font color="#0000FF"&gt;&lt;B&gt;Application:&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;
&lt;PRE&gt;
 Telecom devices
 Bridges, hubs, router, power line adapter
 LAN networks in rough environments
&lt;/PRE&gt;


&lt;/b&gt;&lt;br&gt;&lt;a href="&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtLAN_RJ45_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtLAN_RJ45_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499010441?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499010441?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-26&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499010441"/>
<gate name="G$4" symbol="GNDPIN"/>
<gate name="GREEN-YELLOW" symbol="LED-DUAL-1"/>
<gate name="GREEN-YELLOW-1" symbol="LED_DOUB-1"/>
</gates>
<devices>
<device name="" package="7499010441">
<connects>
<connect gate="G$1" pin="CRD" pad="5"/>
<connect gate="G$1" pin="CTD" pad="4"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="8"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="G$4" pin="GND" pad="Z1 Z2"/>
<connect gate="GREEN-YELLOW" pin="AK1" pad="9"/>
<connect gate="GREEN-YELLOW" pin="AK2" pad="10"/>
<connect gate="GREEN-YELLOW-1" pin="AK1" pad="11"/>
<connect gate="GREEN-YELLOW-1" pin="AK2" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7497110616" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7497110616

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1 +2USB 

&lt;b&gt;Application	Standard USB3.0

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN/OANGE

&lt;b&gt;EMI Fingers	NO


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7497110616?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7497110616?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-23&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7497110616"/>
<gate name="USB-1" symbol="USB-3.0"/>
<gate name="USB-2" symbol="USB-3.0"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
<gate name="YELLOW" symbol="LED-2PIN"/>
<gate name="GREEN-ORANGE" symbol="LED-DUAL"/>
</gates>
<devices>
<device name="" package="7497110616">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2 Z3 Z4 Z5 Z6 Z7 Z8"/>
<connect gate="GREEN-ORANGE" pin="AK1" pad="13"/>
<connect gate="GREEN-ORANGE" pin="AK2" pad="14"/>
<connect gate="RJ45LAN" pin="1" pad="1"/>
<connect gate="RJ45LAN" pin="10" pad="10"/>
<connect gate="RJ45LAN" pin="2" pad="2"/>
<connect gate="RJ45LAN" pin="3" pad="3"/>
<connect gate="RJ45LAN" pin="4" pad="4"/>
<connect gate="RJ45LAN" pin="5" pad="5"/>
<connect gate="RJ45LAN" pin="6" pad="6"/>
<connect gate="RJ45LAN" pin="7" pad="7"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="9" pad="9"/>
<connect gate="USB-1" pin="D+" pad="U3"/>
<connect gate="USB-1" pin="D-" pad="U2"/>
<connect gate="USB-1" pin="GND" pad="U4"/>
<connect gate="USB-1" pin="GND_SIG" pad="U7"/>
<connect gate="USB-1" pin="RX+" pad="U6"/>
<connect gate="USB-1" pin="RX-" pad="U5"/>
<connect gate="USB-1" pin="TX+" pad="U9"/>
<connect gate="USB-1" pin="TX-" pad="U8"/>
<connect gate="USB-1" pin="VCC" pad="U1"/>
<connect gate="USB-2" pin="D+" pad="U12"/>
<connect gate="USB-2" pin="D-" pad="U11"/>
<connect gate="USB-2" pin="GND" pad="U13"/>
<connect gate="USB-2" pin="GND_SIG" pad="U16"/>
<connect gate="USB-2" pin="RX+" pad="U15"/>
<connect gate="USB-2" pin="RX-" pad="U14"/>
<connect gate="USB-2" pin="TX+" pad="U18"/>
<connect gate="USB-2" pin="TX-" pad="U17"/>
<connect gate="USB-2" pin="VCC" pad="U10"/>
<connect gate="YELLOW" pin="A" pad="12"/>
<connect gate="YELLOW" pin="K" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7497110616.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7497111611A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7497111611A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1 + 2xUSB

&lt;b&gt;Application	Standard USB2.0

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	GREEN/ORANGE-YELLOW

&lt;b&gt;EMI Fingers	YES&lt;/b&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7497111611A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7497111611A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-23&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7497111611A"/>
<gate name="USB-1" symbol="USB2.0"/>
<gate name="USB-2" symbol="USB2.0"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
<gate name="YELLOW" symbol="LED-2PIN"/>
<gate name="GREEN-ORANGE" symbol="LED-DUAL1"/>
</gates>
<devices>
<device name="" package="7497111611A">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2 Z3 Z4 Z5 Z6 Z7 Z8"/>
<connect gate="GREEN-ORANGE" pin="A1" pad="15"/>
<connect gate="GREEN-ORANGE" pin="K1" pad="14"/>
<connect gate="GREEN-ORANGE" pin="K2" pad="16"/>
<connect gate="RJ45LAN" pin="1" pad="1"/>
<connect gate="RJ45LAN" pin="10" pad="10"/>
<connect gate="RJ45LAN" pin="2" pad="2"/>
<connect gate="RJ45LAN" pin="3" pad="3"/>
<connect gate="RJ45LAN" pin="4" pad="4"/>
<connect gate="RJ45LAN" pin="5" pad="5"/>
<connect gate="RJ45LAN" pin="6" pad="6"/>
<connect gate="RJ45LAN" pin="7" pad="7"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="9" pad="9"/>
<connect gate="USB-1" pin="D+" pad="U3"/>
<connect gate="USB-1" pin="D-" pad="U2"/>
<connect gate="USB-1" pin="GND" pad="USB1-4"/>
<connect gate="USB-1" pin="VCC" pad="US1"/>
<connect gate="USB-2" pin="D+" pad="U7"/>
<connect gate="USB-2" pin="D-" pad="U6"/>
<connect gate="USB-2" pin="GND" pad="U8"/>
<connect gate="USB-2" pin="VCC" pad="U5"/>
<connect gate="YELLOW" pin="A" pad="12"/>
<connect gate="YELLOW" pin="K" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7497111611A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499110122" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499110122

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	Down

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	No



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499110122?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499110122?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;


&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7499110122"/>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
</gates>
<devices>
<device name="" package="7499110122">
<connects>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="13"/>
<connect gate="LED-GREEN" pin="K" pad="14"/>
<connect gate="LED-YELLOW" pin="A" pad="11"/>
<connect gate="LED-YELLOW" pin="K" pad="12"/>
<connect gate="RJ45LAN" pin="1" pad="1"/>
<connect gate="RJ45LAN" pin="10" pad="10"/>
<connect gate="RJ45LAN" pin="2" pad="2"/>
<connect gate="RJ45LAN" pin="3" pad="3"/>
<connect gate="RJ45LAN" pin="4" pad="4"/>
<connect gate="RJ45LAN" pin="5" pad="5"/>
<connect gate="RJ45LAN" pin="6" pad="6"/>
<connect gate="RJ45LAN" pin="7" pad="7"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499110122.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499110123" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499110123

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	VERTICAL

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	No

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499110123?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499110123?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;


&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7499110123"/>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
<gate name="GREEN" symbol="LED-DUAL"/>
<gate name="YELLOW" symbol="LED-DUAL"/>
</gates>
<devices>
<device name="" package="7499110123">
<connects>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
<connect gate="GREEN" pin="AK1" pad="11"/>
<connect gate="GREEN" pin="AK2" pad="12"/>
<connect gate="RJ45LAN" pin="1" pad="1"/>
<connect gate="RJ45LAN" pin="10" pad="10"/>
<connect gate="RJ45LAN" pin="2" pad="9"/>
<connect gate="RJ45LAN" pin="3" pad="8"/>
<connect gate="RJ45LAN" pin="4" pad="7"/>
<connect gate="RJ45LAN" pin="5" pad="6"/>
<connect gate="RJ45LAN" pin="6" pad="5"/>
<connect gate="RJ45LAN" pin="7" pad="4"/>
<connect gate="RJ45LAN" pin="8" pad="3"/>
<connect gate="RJ45LAN" pin="9" pad="2"/>
<connect gate="YELLOW" pin="AK1" pad="13"/>
<connect gate="YELLOW" pin="AK2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499110123.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499110124" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499110124

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	GREEN/YELLOW-GREEN

&lt;b&gt;EMI Fingers	No

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499110124?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499110124?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;


&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7499110124"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="LED-GREEN&amp;YELLOW" symbol="LED-DUAL-1"/>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
</gates>
<devices>
<device name="" package="7499110124">
<connects>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="11"/>
<connect gate="LED-GREEN" pin="K" pad="12"/>
<connect gate="LED-GREEN&amp;YELLOW" pin="AK1" pad="13"/>
<connect gate="LED-GREEN&amp;YELLOW" pin="AK2" pad="14"/>
<connect gate="RJ45LAN" pin="1" pad="1"/>
<connect gate="RJ45LAN" pin="10" pad="10"/>
<connect gate="RJ45LAN" pin="2" pad="2"/>
<connect gate="RJ45LAN" pin="3" pad="3"/>
<connect gate="RJ45LAN" pin="4" pad="4"/>
<connect gate="RJ45LAN" pin="5" pad="5"/>
<connect gate="RJ45LAN" pin="6" pad="6"/>
<connect gate="RJ45LAN" pin="7" pad="7"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499110124.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499111000A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499111000A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	NONE

&lt;b&gt;EMI Fingers	Yes


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499111000A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499111000A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;


&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7499111221A/7499111000A"/>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
</gates>
<devices>
<device name="" package="7499111000A">
<connects>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
<connect gate="RJ45LAN" pin="1" pad="1"/>
<connect gate="RJ45LAN" pin="10" pad="10"/>
<connect gate="RJ45LAN" pin="11" pad="11"/>
<connect gate="RJ45LAN" pin="12" pad="12"/>
<connect gate="RJ45LAN" pin="2" pad="2"/>
<connect gate="RJ45LAN" pin="3" pad="3"/>
<connect gate="RJ45LAN" pin="4" pad="4"/>
<connect gate="RJ45LAN" pin="5" pad="5"/>
<connect gate="RJ45LAN" pin="6" pad="6"/>
<connect gate="RJ45LAN" pin="7" pad="7"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499111000A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499111221A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499111221A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	GREEN-GREEN

&lt;b&gt;EMI Fingers	Yes

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499111221A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499111221A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;


&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7499111221A/7499111000A"/>
<gate name="LEDGREEN" symbol="LED2PIN"/>
<gate name="LED-GREEN1" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
</gates>
<devices>
<device name="" package="7499111221A">
<connects>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
<connect gate="LED-GREEN1" pin="A" pad="16"/>
<connect gate="LED-GREEN1" pin="K" pad="15"/>
<connect gate="LEDGREEN" pin="A" pad="14"/>
<connect gate="LEDGREEN" pin="K" pad="13"/>
<connect gate="RJ45LAN" pin="1" pad="1"/>
<connect gate="RJ45LAN" pin="10" pad="10"/>
<connect gate="RJ45LAN" pin="11" pad="11"/>
<connect gate="RJ45LAN" pin="12" pad="12"/>
<connect gate="RJ45LAN" pin="2" pad="2"/>
<connect gate="RJ45LAN" pin="3" pad="3"/>
<connect gate="RJ45LAN" pin="4" pad="4"/>
<connect gate="RJ45LAN" pin="5" pad="5"/>
<connect gate="RJ45LAN" pin="6" pad="6"/>
<connect gate="RJ45LAN" pin="7" pad="7"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499111221A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499111446" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499111446

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	DOWN

&lt;b&gt;LED (Left-Right)	GREEN/YELLOW-GREEN/YELLOW

&lt;b&gt;EMI Fingers	yes


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499111446?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499111446?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;


&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45" symbol="7499111446"/>
<gate name="LED-YELLOW-GREEN" symbol="LED-DUAL-1"/>
<gate name="LED-YELLOW-GREEN1" symbol="LED-DUAL-1"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="7499111446">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-YELLOW-GREEN" pin="AK1" pad="11"/>
<connect gate="LED-YELLOW-GREEN" pin="AK2" pad="12"/>
<connect gate="LED-YELLOW-GREEN1" pin="AK1" pad="13"/>
<connect gate="LED-YELLOW-GREEN1" pin="AK2" pad="14"/>
<connect gate="RJ45" pin="1" pad="1"/>
<connect gate="RJ45" pin="10" pad="10"/>
<connect gate="RJ45" pin="2" pad="2"/>
<connect gate="RJ45" pin="3" pad="3"/>
<connect gate="RJ45" pin="4" pad="4"/>
<connect gate="RJ45" pin="5" pad="5"/>
<connect gate="RJ45" pin="6" pad="6"/>
<connect gate="RJ45" pin="7" pad="7"/>
<connect gate="RJ45" pin="8" pad="8"/>
<connect gate="RJ45" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499111446.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499111447" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499111447

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	Up

&lt;b&gt;LED (Left-Right)	GREEN/YELLOW-GREEN/YELLOW

&lt;b&gt;EMI Fingers	yes
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499111447?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499111447?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7499111447"/>
<gate name="LED-GREEN/YELLOW" symbol="LED-DUAL-1"/>
<gate name="LED-GREEN/YELLOW1" symbol="LED-DUAL-1"/>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
</gates>
<devices>
<device name="" package="7499111447">
<connects>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
<connect gate="LED-GREEN/YELLOW" pin="AK1" pad="11"/>
<connect gate="LED-GREEN/YELLOW" pin="AK2" pad="12"/>
<connect gate="LED-GREEN/YELLOW1" pin="AK1" pad="13"/>
<connect gate="LED-GREEN/YELLOW1" pin="AK2" pad="14"/>
<connect gate="RJ45LAN" pin="1" pad="1"/>
<connect gate="RJ45LAN" pin="10" pad="10"/>
<connect gate="RJ45LAN" pin="2" pad="2"/>
<connect gate="RJ45LAN" pin="3" pad="3"/>
<connect gate="RJ45LAN" pin="4" pad="4"/>
<connect gate="RJ45LAN" pin="5" pad="5"/>
<connect gate="RJ45LAN" pin="6" pad="6"/>
<connect gate="RJ45LAN" pin="7" pad="7"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499111447.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499151120" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499151120

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x2 Stacked

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP &amp; DOWN

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	Yes

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499151120?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499151120?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN-DOWN" symbol="7499151120"/>
<gate name="RJ45LAN-UP" symbol="7499151120"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="LED-GREEN1" symbol="LED2PIN"/>
<gate name="LED-YELLOW1" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="7499151120">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2 Z3 Z4"/>
<connect gate="LED-GREEN" pin="A" pad="11"/>
<connect gate="LED-GREEN" pin="K" pad="12"/>
<connect gate="LED-GREEN1" pin="A" pad="A11"/>
<connect gate="LED-GREEN1" pin="K" pad="A12"/>
<connect gate="LED-YELLOW" pin="A" pad="14"/>
<connect gate="LED-YELLOW" pin="K" pad="13"/>
<connect gate="LED-YELLOW1" pin="A" pad="A14"/>
<connect gate="LED-YELLOW1" pin="K" pad="A13"/>
<connect gate="RJ45LAN-DOWN" pin="1" pad="1"/>
<connect gate="RJ45LAN-DOWN" pin="2" pad="2"/>
<connect gate="RJ45LAN-DOWN" pin="3" pad="3"/>
<connect gate="RJ45LAN-DOWN" pin="4" pad="4"/>
<connect gate="RJ45LAN-DOWN" pin="5" pad="5"/>
<connect gate="RJ45LAN-DOWN" pin="6" pad="6"/>
<connect gate="RJ45LAN-DOWN" pin="7" pad="7"/>
<connect gate="RJ45LAN-DOWN" pin="8" pad="8"/>
<connect gate="RJ45LAN-DOWN" pin="9" pad="9"/>
<connect gate="RJ45LAN-UP" pin="1" pad="A1"/>
<connect gate="RJ45LAN-UP" pin="2" pad="A2"/>
<connect gate="RJ45LAN-UP" pin="3" pad="A3"/>
<connect gate="RJ45LAN-UP" pin="4" pad="A4"/>
<connect gate="RJ45LAN-UP" pin="5" pad="A5"/>
<connect gate="RJ45LAN-UP" pin="6" pad="A6"/>
<connect gate="RJ45LAN-UP" pin="7" pad="A7"/>
<connect gate="RJ45LAN-UP" pin="8" pad="A8"/>
<connect gate="RJ45LAN-UP" pin="9" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499151120.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499511440" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499511440

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	PoE

&lt;b&gt;Tab Position	UP 

&lt;b&gt;LED (Left-Right)	GREEN/YELLOW-GREEN/YELLOW

&lt;b&gt;EMI Fingers	Yes

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499511440?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499511440?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-30&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7499511440"/>
<gate name="LED-GREEN/YELLOW" symbol="LED-DUAL-1"/>
<gate name="LED-GREEN/YELLOW1" symbol="LED-DUAL-1"/>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
</gates>
<devices>
<device name="" package="7499511440">
<connects>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
<connect gate="LED-GREEN/YELLOW" pin="AK1" pad="17"/>
<connect gate="LED-GREEN/YELLOW" pin="AK2" pad="18"/>
<connect gate="LED-GREEN/YELLOW1" pin="AK1" pad="19"/>
<connect gate="LED-GREEN/YELLOW1" pin="AK2" pad="20"/>
<connect gate="RJ45LAN" pin="1" pad="1"/>
<connect gate="RJ45LAN" pin="10" pad="10"/>
<connect gate="RJ45LAN" pin="11" pad="11"/>
<connect gate="RJ45LAN" pin="12" pad="12"/>
<connect gate="RJ45LAN" pin="2" pad="2"/>
<connect gate="RJ45LAN" pin="3" pad="3"/>
<connect gate="RJ45LAN" pin="4" pad="4"/>
<connect gate="RJ45LAN" pin="5" pad="5"/>
<connect gate="RJ45LAN" pin="6" pad="6"/>
<connect gate="RJ45LAN" pin="7" pad="7"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="9" pad="9"/>
<connect gate="RJ45LAN" pin="VC1+1" pad="13"/>
<connect gate="RJ45LAN" pin="VC1-1" pad="14"/>
<connect gate="RJ45LAN" pin="VC2+1" pad="15"/>
<connect gate="RJ45LAN" pin="VC2-1" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499511440.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498111001" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7498111001

&lt;b&gt;Design		SMD

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP 

&lt;b&gt;LED (Left-Right)	NONE

&lt;b&gt;EMI Fingers	Yes

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7498111001?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7498111001?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-23&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7498111001"/>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
</gates>
<devices>
<device name="" package="7498111001">
<connects>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
<connect gate="RJ45LAN" pin="1" pad="1"/>
<connect gate="RJ45LAN" pin="2" pad="2"/>
<connect gate="RJ45LAN" pin="3" pad="3"/>
<connect gate="RJ45LAN" pin="4" pad="4"/>
<connect gate="RJ45LAN" pin="5" pad="5"/>
<connect gate="RJ45LAN" pin="6" pad="6"/>
<connect gate="RJ45LAN" pin="7" pad="7"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="GND" pad="10"/>
<connect gate="RJ45LAN" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7498111001.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498111120R" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7498111120R

&lt;b&gt;Design		SMD

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	Yes
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7498111120R"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7498111120R?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-23&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7498111120R"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="GND.SHIELD" symbol="GNDPIN"/>
</gates>
<devices>
<device name="" package="7498111120R">
<connects>
<connect gate="GND.SHIELD" pin="GND" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="2"/>
<connect gate="LED-GREEN" pin="K" pad="1"/>
<connect gate="LED-YELLOW" pin="A" pad="14"/>
<connect gate="LED-YELLOW" pin="K" pad="13"/>
<connect gate="RJ45LAN" pin="GND" pad="12"/>
<connect gate="RJ45LAN" pin="TRD0+" pad="3"/>
<connect gate="RJ45LAN" pin="TRD0-" pad="4"/>
<connect gate="RJ45LAN" pin="TRD1+" pad="5"/>
<connect gate="RJ45LAN" pin="TRD1-" pad="6"/>
<connect gate="RJ45LAN" pin="TRD2+" pad="7"/>
<connect gate="RJ45LAN" pin="TRD2-" pad="8"/>
<connect gate="RJ45LAN" pin="TRD3+" pad="9"/>
<connect gate="RJ45LAN" pin="TRD3-" pad="10"/>
<connect gate="RJ45LAN" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7498111120R.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990100011A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	74990100011A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	NONE

&lt;b&gt;EMI Fingers	No

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/74990100011A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/74990100011A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-23&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
<gate name="G$1" symbol="74990100011A"/>
</gates>
<devices>
<device name="" package="74990-WITHOUT-LED-(21.84X16.2MM)">
<connects>
<connect gate="G$1" pin="RCT" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="TCT" pad="4"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/74990100011A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499010001A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499010001A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	NONE

&lt;b&gt;EMI Fingers	No



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499010001A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499010001A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;
&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-26&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
<gate name="G$1" symbol="74990X-THT-10/100-T"/>
</gates>
<devices>
<device name="" package="74990-WITHOUT-LED">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="RCT" pad="5"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="TCT" pad="2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499010001A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499010004A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499010004A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	Down

&lt;b&gt;LED (Left-Right)	NONE

&lt;b&gt;EMI Fingers	No


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499010004A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499010004A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;
&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-26&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
<gate name="G$1" symbol="74990X-THT-10/100-T"/>
</gates>
<devices>
<device name="" package="7499010004A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="RCT" pad="5"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="TCT" pad="4"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499010004A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990101210" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	74990101210

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1 Vertical

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position 	Vertical

&lt;b&gt;LED (Left-Right)	Yellow-Green

&lt;b&gt;EMI Fingers	No





&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/74990101210?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/74990101210?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-26&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="74990X-THT-10/100-T"/>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="74990101210">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="11"/>
<connect gate="LED-GREEN" pin="K" pad="12"/>
<connect gate="LED-YELLOW" pin="A" pad="9"/>
<connect gate="LED-YELLOW" pin="K" pad="10"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="RCT" pad="5"/>
<connect gate="RJ45LAN" pin="RD+" pad="3"/>
<connect gate="RJ45LAN" pin="RD-" pad="6"/>
<connect gate="RJ45LAN" pin="TCT" pad="4"/>
<connect gate="RJ45LAN" pin="TD+" pad="1"/>
<connect gate="RJ45LAN" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/74990101210.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499010121A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499010121A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	Yellow-Green

&lt;b&gt;EMI Fingers	No



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499010121A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499010001A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-26&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="74990X-THT-10/100-T"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="74990-WITH-LED">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="10"/>
<connect gate="LED-GREEN" pin="K" pad="9"/>
<connect gate="LED-YELLOW" pin="A" pad="12"/>
<connect gate="LED-YELLOW" pin="K" pad="11"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="RCT" pad="5"/>
<connect gate="RJ45LAN" pin="RD+" pad="4"/>
<connect gate="RJ45LAN" pin="RD-" pad="6"/>
<connect gate="RJ45LAN" pin="TCT" pad="2"/>
<connect gate="RJ45LAN" pin="TD+" pad="1"/>
<connect gate="RJ45LAN" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499010121A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499010211A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499010211A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	DOWN

&lt;b&gt;LED (Left-Right)	Green-Yellow

&lt;b&gt;EMI Fingers	No



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499010211A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499010211A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-26&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="74990X-THT-10/100-T"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="74990-WITH-LED-TYPE2">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="9"/>
<connect gate="LED-GREEN" pin="K" pad="10"/>
<connect gate="LED-YELLOW" pin="A" pad="12"/>
<connect gate="LED-YELLOW" pin="K" pad="11"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="RCT" pad="5"/>
<connect gate="RJ45LAN" pin="RD+" pad="3"/>
<connect gate="RJ45LAN" pin="RD-" pad="6"/>
<connect gate="RJ45LAN" pin="TCT" pad="4"/>
<connect gate="RJ45LAN" pin="TD+" pad="1"/>
<connect gate="RJ45LAN" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499010211A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499011001A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499011001A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	Down

&lt;b&gt;LED (Left-Right)	NONE

&lt;b&gt;EMI Fingers	Yes






&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499011001A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499011001A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
<gate name="G$1" symbol="7499011001A"/>
</gates>
<devices>
<device name="" package="74990-WITHOUT-LED-(21.84X15.88MM)">
<connects>
<connect gate="G$1" pin="RCT" pad="7"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="TCT" pad="4"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499011001A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499011002A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499011002A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	Down

&lt;b&gt;LED (Left-Right)	NONE

&lt;b&gt;EMI Fingers	Yes





&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499010001A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499010001A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;


&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="74990X-THT-10/100-T"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="74990-WITHOUT-LED-(21.84X15.88MM)">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="RCT" pad="5"/>
<connect gate="RJ45LAN" pin="RD+" pad="4"/>
<connect gate="RJ45LAN" pin="RD-" pad="6"/>
<connect gate="RJ45LAN" pin="TCT" pad="2"/>
<connect gate="RJ45LAN" pin="TD+" pad="1"/>
<connect gate="RJ45LAN" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499011002A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990110030" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	74990110030

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	NONE

&lt;b&gt;EMI Fingers	Yes



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/74990110030?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/74990110030?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;


&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="74990X-THT-10/100-T"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="74990110030">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="RCT" pad="5"/>
<connect gate="RJ45LAN" pin="RD+" pad="4"/>
<connect gate="RJ45LAN" pin="RD-" pad="6"/>
<connect gate="RJ45LAN" pin="TCT" pad="2"/>
<connect gate="RJ45LAN" pin="TD+" pad="1"/>
<connect gate="RJ45LAN" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/74990110030.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499011121A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499011121A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	DOWN

&lt;b&gt;LED (Left-Right)	Yellow-Green

&lt;b&gt;EMI Fingers	Yes




&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499011121A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499011121A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;


&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="74990X-THT-10/100-T"/>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="7499011121A">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="11"/>
<connect gate="LED-GREEN" pin="K" pad="12"/>
<connect gate="LED-YELLOW" pin="A" pad="9"/>
<connect gate="LED-YELLOW" pin="K" pad="10"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="RCT" pad="5"/>
<connect gate="RJ45LAN" pin="RD+" pad="4"/>
<connect gate="RJ45LAN" pin="RD-" pad="6"/>
<connect gate="RJ45LAN" pin="TCT" pad="2"/>
<connect gate="RJ45LAN" pin="TD+" pad="1"/>
<connect gate="RJ45LAN" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499011121A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990112116A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	74990112116A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	Green-Yellow

&lt;b&gt;EMI Fingers	Yes




&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/74990112116A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/74990112116A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;


&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="74990X-THT-10/100-T"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="74990-WITH-LED">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="12"/>
<connect gate="LED-GREEN" pin="K" pad="11"/>
<connect gate="LED-YELLOW" pin="A" pad="10"/>
<connect gate="LED-YELLOW" pin="K" pad="9"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="RCT" pad="5"/>
<connect gate="RJ45LAN" pin="RD+" pad="4"/>
<connect gate="RJ45LAN" pin="RD-" pad="6"/>
<connect gate="RJ45LAN" pin="TCT" pad="2"/>
<connect gate="RJ45LAN" pin="TD+" pad="1"/>
<connect gate="RJ45LAN" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/74990112116A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499011222A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499011222A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	DOWN

&lt;b&gt;LED (Left-Right)	Green-Green

&lt;b&gt;EMI Fingers	Yes



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499011222A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499011222A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="LED-GREEN1" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
<gate name="G$1" symbol="74990X-THT-10/100-T"/>
</gates>
<devices>
<device name="" package="7499011222A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="RCT" pad="5"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="TCT" pad="4"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="9"/>
<connect gate="LED-GREEN" pin="K" pad="10"/>
<connect gate="LED-GREEN1" pin="A" pad="11"/>
<connect gate="LED-GREEN1" pin="K" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499021125" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499021125

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x2 HORIZONTAL

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	DOWN

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	Yes



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499021125?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499021125?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;


&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="LED-YELLOW1" symbol="LED2PIN"/>
<gate name="LED-GREEN1" symbol="LED2PIN"/>
<gate name="LED-YELLOW2" symbol="LED2PIN"/>
<gate name="LED-GREEN2" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
<gate name="G$1" symbol="74990X-THT-10/100-T"/>
<gate name="G$2" symbol="74990X-THT-10/100-T"/>
</gates>
<devices>
<device name="" package="7499021125-2PORTS-HORIZONTAL">
<connects>
<connect gate="G$1" pin="8" pad="A8"/>
<connect gate="G$1" pin="RCT" pad="A5"/>
<connect gate="G$1" pin="RD+" pad="A3"/>
<connect gate="G$1" pin="RD-" pad="A6"/>
<connect gate="G$1" pin="TCT" pad="A4"/>
<connect gate="G$1" pin="TD+" pad="A1"/>
<connect gate="G$1" pin="TD-" pad="A2"/>
<connect gate="G$2" pin="8" pad="B8"/>
<connect gate="G$2" pin="RCT" pad="B5"/>
<connect gate="G$2" pin="RD+" pad="B3"/>
<connect gate="G$2" pin="RD-" pad="B6"/>
<connect gate="G$2" pin="TCT" pad="B4"/>
<connect gate="G$2" pin="TD+" pad="B1"/>
<connect gate="G$2" pin="TD-" pad="B2"/>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2 Z3"/>
<connect gate="LED-GREEN1" pin="A" pad="A11"/>
<connect gate="LED-GREEN1" pin="K" pad="A12"/>
<connect gate="LED-GREEN2" pin="A" pad="B11"/>
<connect gate="LED-GREEN2" pin="K" pad="B12"/>
<connect gate="LED-YELLOW1" pin="A" pad="A9"/>
<connect gate="LED-YELLOW1" pin="K" pad="A10"/>
<connect gate="LED-YELLOW2" pin="A" pad="B9"/>
<connect gate="LED-YELLOW2" pin="K" pad="B10"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499021125.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499031120A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499031120A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x4 HORIZONTAL

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	DOWN

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	Yes

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499031120A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499031120A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;


&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="LED-YELLOW2" symbol="LED2PIN"/>
<gate name="LED-GREEN1" symbol="LED2PIN"/>
<gate name="LED-GREEN2" symbol="LED2PIN"/>
<gate name="LED-YELLOW1" symbol="LED2PIN"/>
<gate name="LED-YELLOW3" symbol="LED2PIN"/>
<gate name="LED-GREEN3" symbol="LED2PIN"/>
<gate name="LED-YELLOW4" symbol="LED2PIN"/>
<gate name="LED-GREEN4" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
<gate name="G$1" symbol="74990X-THT-10/100-T"/>
<gate name="G$2" symbol="74990X-THT-10/100-T"/>
<gate name="G$3" symbol="74990X-THT-10/100-T"/>
<gate name="G$4" symbol="74990X-THT-10/100-T"/>
</gates>
<devices>
<device name="" package="7499031120A-4PORTS-HORIZONTAL">
<connects>
<connect gate="G$1" pin="8" pad="A8"/>
<connect gate="G$1" pin="RCT" pad="A5"/>
<connect gate="G$1" pin="RD+" pad="A4"/>
<connect gate="G$1" pin="RD-" pad="A6"/>
<connect gate="G$1" pin="TCT" pad="A2"/>
<connect gate="G$1" pin="TD+" pad="A1"/>
<connect gate="G$1" pin="TD-" pad="A3"/>
<connect gate="G$2" pin="8" pad="B8"/>
<connect gate="G$2" pin="RCT" pad="B5"/>
<connect gate="G$2" pin="RD+" pad="B4"/>
<connect gate="G$2" pin="RD-" pad="B6"/>
<connect gate="G$2" pin="TCT" pad="B2"/>
<connect gate="G$2" pin="TD+" pad="B1"/>
<connect gate="G$2" pin="TD-" pad="B3"/>
<connect gate="G$3" pin="8" pad="C8"/>
<connect gate="G$3" pin="RCT" pad="C5"/>
<connect gate="G$3" pin="RD+" pad="C4"/>
<connect gate="G$3" pin="RD-" pad="C6"/>
<connect gate="G$3" pin="TCT" pad="C2"/>
<connect gate="G$3" pin="TD+" pad="C1"/>
<connect gate="G$3" pin="TD-" pad="C3"/>
<connect gate="G$4" pin="8" pad="D8"/>
<connect gate="G$4" pin="RCT" pad="D5"/>
<connect gate="G$4" pin="RD+" pad="D4"/>
<connect gate="G$4" pin="RD-" pad="D6"/>
<connect gate="G$4" pin="TCT" pad="D2"/>
<connect gate="G$4" pin="TD+" pad="D1"/>
<connect gate="G$4" pin="TD-" pad="D3"/>
<connect gate="GND_SHIELD" pin="1" pad="Z3 Z4 Z5 Z6 Z7"/>
<connect gate="LED-GREEN1" pin="A" pad="A11"/>
<connect gate="LED-GREEN1" pin="K" pad="A12"/>
<connect gate="LED-GREEN2" pin="A" pad="B9"/>
<connect gate="LED-GREEN2" pin="K" pad="B10"/>
<connect gate="LED-GREEN3" pin="A" pad="C11"/>
<connect gate="LED-GREEN3" pin="K" pad="C12"/>
<connect gate="LED-GREEN4" pin="A" pad="D11"/>
<connect gate="LED-GREEN4" pin="K" pad="D12"/>
<connect gate="LED-YELLOW1" pin="A" pad="A9"/>
<connect gate="LED-YELLOW1" pin="K" pad="A10"/>
<connect gate="LED-YELLOW2" pin="A" pad="B11"/>
<connect gate="LED-YELLOW2" pin="K" pad="B12"/>
<connect gate="LED-YELLOW3" pin="A" pad="C9"/>
<connect gate="LED-YELLOW3" pin="K" pad="C10"/>
<connect gate="LED-YELLOW4" pin="A" pad="D9"/>
<connect gate="LED-YELLOW4" pin="K" pad="D10"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499031120A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499051002" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499051002

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x2 STACKED

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP &amp; DOWN

&lt;b&gt;LED (Left-Right)	NONE

&lt;b&gt;EMI Fingers	Yes


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499051002?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499051002?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN1" symbol="74990X-THT-10/100-T"/>
<gate name="RJ45LAN2" symbol="74990X-THT-10/100-T"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="7499051002-1X2-STACKED">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2 Z3 Z4"/>
<connect gate="RJ45LAN1" pin="8" pad="A8"/>
<connect gate="RJ45LAN1" pin="RCT" pad="A5"/>
<connect gate="RJ45LAN1" pin="RD+" pad="A4"/>
<connect gate="RJ45LAN1" pin="RD-" pad="A6"/>
<connect gate="RJ45LAN1" pin="TCT" pad="A2"/>
<connect gate="RJ45LAN1" pin="TD+" pad="A1"/>
<connect gate="RJ45LAN1" pin="TD-" pad="A3"/>
<connect gate="RJ45LAN2" pin="8" pad="B8"/>
<connect gate="RJ45LAN2" pin="RCT" pad="B5"/>
<connect gate="RJ45LAN2" pin="RD+" pad="B4"/>
<connect gate="RJ45LAN2" pin="RD-" pad="B6"/>
<connect gate="RJ45LAN2" pin="TCT" pad="B2"/>
<connect gate="RJ45LAN2" pin="TD+" pad="B1"/>
<connect gate="RJ45LAN2" pin="TD-" pad="B3"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499051002.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499210001A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499210001A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T PoE

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	PoE

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	NONE

&lt;b&gt;EMI Fingers	No



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499210001A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499210001A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-30&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="749921-THT-POE-RVS"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="7499210001A">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="RJ45LAN" pin="RCT" pad="5"/>
<connect gate="RJ45LAN" pin="RD+" pad="4"/>
<connect gate="RJ45LAN" pin="RD-" pad="6"/>
<connect gate="RJ45LAN" pin="TCT" pad="2"/>
<connect gate="RJ45LAN" pin="TD+" pad="1"/>
<connect gate="RJ45LAN" pin="TD-" pad="3"/>
<connect gate="RJ45LAN" pin="VC1+" pad="9"/>
<connect gate="RJ45LAN" pin="VC1-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499210001A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499210121A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499210121A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T PoE

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	PoE

&lt;b&gt;Tab Position	DOWN

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	No





&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499210121A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499210121A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-30&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="749921-THT-POE-RVS"/>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="7499210121A">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="13"/>
<connect gate="LED-GREEN" pin="K" pad="14"/>
<connect gate="LED-YELLOW" pin="A" pad="11"/>
<connect gate="LED-YELLOW" pin="K" pad="12"/>
<connect gate="RJ45LAN" pin="RCT" pad="3"/>
<connect gate="RJ45LAN" pin="RD+" pad="1"/>
<connect gate="RJ45LAN" pin="RD-" pad="2"/>
<connect gate="RJ45LAN" pin="TCT" pad="4"/>
<connect gate="RJ45LAN" pin="TD+" pad="5"/>
<connect gate="RJ45LAN" pin="TD-" pad="6"/>
<connect gate="RJ45LAN" pin="VC1+" pad="9"/>
<connect gate="RJ45LAN" pin="VC1-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499210121A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499210123A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499210123A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T PoE

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	PoE

&lt;b&gt;Tab Position	VERTICAL

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	No



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499210123?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499210123?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-30&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="RJ45LAN" symbol="749921-THT-POE-RVS"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="7499210123A">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="13"/>
<connect gate="LED-GREEN" pin="K" pad="14"/>
<connect gate="LED-YELLOW" pin="A" pad="11"/>
<connect gate="LED-YELLOW" pin="K" pad="12"/>
<connect gate="RJ45LAN" pin="RCT" pad="3"/>
<connect gate="RJ45LAN" pin="RD+" pad="1"/>
<connect gate="RJ45LAN" pin="RD-" pad="2"/>
<connect gate="RJ45LAN" pin="TCT" pad="4"/>
<connect gate="RJ45LAN" pin="TD+" pad="5"/>
<connect gate="RJ45LAN" pin="TD-" pad="6"/>
<connect gate="RJ45LAN" pin="VC1+" pad="9"/>
<connect gate="RJ45LAN" pin="VC1-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499210123.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499210124A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499210124A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T PoE

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	PoE

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	No



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499210124A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499210124A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-30&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="749921-THT-POE-RVS"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="7499210124A">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="12"/>
<connect gate="LED-GREEN" pin="K" pad="11"/>
<connect gate="LED-YELLOW" pin="A" pad="14"/>
<connect gate="LED-YELLOW" pin="K" pad="13"/>
<connect gate="RJ45LAN" pin="RCT" pad="3"/>
<connect gate="RJ45LAN" pin="RD+" pad="1"/>
<connect gate="RJ45LAN" pin="RD-" pad="2"/>
<connect gate="RJ45LAN" pin="TCT" pad="4"/>
<connect gate="RJ45LAN" pin="TD+" pad="5"/>
<connect gate="RJ45LAN" pin="TD-" pad="6"/>
<connect gate="RJ45LAN" pin="VC1+" pad="9"/>
<connect gate="RJ45LAN" pin="VC1-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499210124A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499211002A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499211002A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T PoE

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	PoE

&lt;b&gt;Tab Position	DOWN

&lt;b&gt;LED (Left-Right)	NONE

&lt;b&gt;EMI Fingers	Yes


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499211002A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499211002A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-30&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="749921-TYPE-2-RVS"/>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
</gates>
<devices>
<device name="" package="7499211002A">
<connects>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
<connect gate="RJ45LAN" pin="RD+" pad="4"/>
<connect gate="RJ45LAN" pin="RD-" pad="5"/>
<connect gate="RJ45LAN" pin="TCT" pad="3"/>
<connect gate="RJ45LAN" pin="TD+" pad="1"/>
<connect gate="RJ45LAN" pin="TD-" pad="2"/>
<connect gate="RJ45LAN" pin="VC1+" pad="7"/>
<connect gate="RJ45LAN" pin="VC1-" pad="8"/>
<connect gate="RJ45LAN" pin="VC2+" pad="9"/>
<connect gate="RJ45LAN" pin="VC2-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499211002A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499211121A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499211121A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T PoE

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	PoE

&lt;b&gt;Tab Position	DOWN

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	Yes



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499211121A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499211121A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-30&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="RJ45LAN" symbol="749921-THT-POE"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
<gate name="NC" symbol="NC"/>
</gates>
<devices>
<device name="" package="7499211121A">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="13"/>
<connect gate="LED-GREEN" pin="K" pad="14"/>
<connect gate="LED-YELLOW" pin="A" pad="11"/>
<connect gate="LED-YELLOW" pin="K" pad="12"/>
<connect gate="NC" pin="NC" pad="7 8"/>
<connect gate="RJ45LAN" pin="RCT" pad="3"/>
<connect gate="RJ45LAN" pin="RD+" pad="1"/>
<connect gate="RJ45LAN" pin="RD-" pad="2"/>
<connect gate="RJ45LAN" pin="TCT" pad="4"/>
<connect gate="RJ45LAN" pin="TD+" pad="5"/>
<connect gate="RJ45LAN" pin="TD-" pad="6"/>
<connect gate="RJ45LAN" pin="VC1+" pad="9"/>
<connect gate="RJ45LAN" pin="VC1-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499211121A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499211122A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499211122A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T PoE

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	PoE

&lt;b&gt;Tab Position	DOWN

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	Yes
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499211122A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499211122A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-30&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="749921-TYPE-2"/>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
</gates>
<devices>
<device name="" package="7499211122A">
<connects>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="13"/>
<connect gate="LED-GREEN" pin="K" pad="14"/>
<connect gate="LED-YELLOW" pin="A" pad="11"/>
<connect gate="LED-YELLOW" pin="K" pad="12"/>
<connect gate="RJ45LAN" pin="CTD" pad="3"/>
<connect gate="RJ45LAN" pin="RD+" pad="4"/>
<connect gate="RJ45LAN" pin="RD-" pad="5"/>
<connect gate="RJ45LAN" pin="TD+" pad="1"/>
<connect gate="RJ45LAN" pin="TD-" pad="2"/>
<connect gate="RJ45LAN" pin="VC1+" pad="7"/>
<connect gate="RJ45LAN" pin="VC1-" pad="8"/>
<connect gate="RJ45LAN" pin="VC2+" pad="9"/>
<connect gate="RJ45LAN" pin="VC2-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499211122A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498011001A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7498011001A

&lt;b&gt;Design		SMD

&lt;b&gt;xBase-T		10/100 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	Down

&lt;b&gt;LED (Left-Right)	None

&lt;b&gt;EMI Fingers	Yes



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7498011001A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7498011001A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-23&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="74990X-THT-10/100-T"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="749801100X">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="RCT" pad="5"/>
<connect gate="RJ45LAN" pin="RD+" pad="4"/>
<connect gate="RJ45LAN" pin="RD-" pad="6"/>
<connect gate="RJ45LAN" pin="TCT" pad="2"/>
<connect gate="RJ45LAN" pin="TD+" pad="1"/>
<connect gate="RJ45LAN" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7498011001A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498011008" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7498011008

&lt;b&gt;Design		SMD

&lt;b&gt;xBase-T		10/100 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	Down

&lt;b&gt;LED (Left-Right)	None

&lt;b&gt;EMI Fingers	Yes




&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7498011008?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7498011008?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;
&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-23&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
<gate name="G$1" symbol="74990X-THT-10/100-T"/>
</gates>
<devices>
<device name="" package="749801100X">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="RCT" pad="5"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="TCT" pad="4"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7498011008.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74980111211" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	74980111211

&lt;b&gt;Design		SMD

&lt;b&gt;xBase-T		10/100 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	Up

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	Yes


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/74980111211?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/74980111211?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-23&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74980111211"/>
<gate name="GND" symbol="GNDPIN"/>
<gate name="GREEN" symbol="LED-2PIN"/>
<gate name="YELLOW" symbol="LED-2PIN"/>
</gates>
<devices>
<device name="" package="74980111211">
<connects>
<connect gate="G$1" pin="8" pad="10"/>
<connect gate="G$1" pin="RCT" pad="7"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="TCT" pad="4"/>
<connect gate="G$1" pin="TD+" pad="3"/>
<connect gate="G$1" pin="TD-" pad="5"/>
<connect gate="GND" pin="GND" pad="Z1 Z2"/>
<connect gate="GREEN" pin="A" pad="1"/>
<connect gate="GREEN" pin="K" pad="2"/>
<connect gate="YELLOW" pin="A" pad="12"/>
<connect gate="YELLOW" pin="K" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/74980111211.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498011122R" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7498011122R

&lt;b&gt;Design		SMD

&lt;b&gt;xBase-T		10/100 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	Up

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	Yes


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7498011122R?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7498011122R?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-23&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="74990X-THT-10/100-T"/>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="7498011122R">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="P11"/>
<connect gate="LED-GREEN" pin="K" pad="P12"/>
<connect gate="LED-YELLOW" pin="A" pad="P9"/>
<connect gate="LED-YELLOW" pin="K" pad="P10"/>
<connect gate="RJ45LAN" pin="8" pad="P8"/>
<connect gate="RJ45LAN" pin="RCT" pad="P5"/>
<connect gate="RJ45LAN" pin="RD+" pad="P4"/>
<connect gate="RJ45LAN" pin="RD-" pad="P6"/>
<connect gate="RJ45LAN" pin="TCT" pad="P2"/>
<connect gate="RJ45LAN" pin="TD+" pad="P1"/>
<connect gate="RJ45LAN" pin="TD-" pad="P3"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7498011122R.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498011211" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7498011211

&lt;b&gt;Design		SMD

&lt;b&gt;xBase-T		10/100 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	DOWN

&lt;b&gt;LED (Left-Right)	GREEN-YELLOW

&lt;b&gt;EMI Fingers	Yes


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7498011211?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7498011211?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-23&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7498011211"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="LED-YELLOW" symbol="LED2PIN"/>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
</gates>
<devices>
<device name="" package="7498011211">
<connects>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="1"/>
<connect gate="LED-GREEN" pin="K" pad="2"/>
<connect gate="LED-YELLOW" pin="A" pad="9"/>
<connect gate="LED-YELLOW" pin="K" pad="10"/>
<connect gate="RJ45LAN" pin="RCT" pad="7"/>
<connect gate="RJ45LAN" pin="RD+" pad="6"/>
<connect gate="RJ45LAN" pin="RD-" pad="8"/>
<connect gate="RJ45LAN" pin="TCT" pad="4"/>
<connect gate="RJ45LAN" pin="TD+" pad="3"/>
<connect gate="RJ45LAN" pin="TD-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7498011211.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499611421" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499611421

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10G Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	GREEN/YELLOW-GREEN

&lt;b&gt;EMI Fingers	Yes



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499611421?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499611421?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-30&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7499611421"/>
<gate name="LED-GREEN" symbol="LED2PIN"/>
<gate name="LED-YELLOW/GREEN" symbol="LED-DUAL-1"/>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
</gates>
<devices>
<device name="" package="7499611421">
<connects>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="14"/>
<connect gate="LED-GREEN" pin="K" pad="13"/>
<connect gate="LED-YELLOW/GREEN" pin="AK1" pad="16"/>
<connect gate="LED-YELLOW/GREEN" pin="AK2" pad="15"/>
<connect gate="RJ45LAN" pin="1" pad="1"/>
<connect gate="RJ45LAN" pin="10" pad="10"/>
<connect gate="RJ45LAN" pin="11" pad="11"/>
<connect gate="RJ45LAN" pin="12" pad="12"/>
<connect gate="RJ45LAN" pin="2" pad="2"/>
<connect gate="RJ45LAN" pin="3" pad="3"/>
<connect gate="RJ45LAN" pin="4" pad="4"/>
<connect gate="RJ45LAN" pin="5" pad="5"/>
<connect gate="RJ45LAN" pin="6" pad="6"/>
<connect gate="RJ45LAN" pin="7" pad="7"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499611421.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990111215A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	74990111215A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T 

&lt;b&gt;Ports		1x1 

&lt;b&gt;Application	Standard HPLE

&lt;b&gt;Tab Position	Down

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	YES


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/74990111215A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/74990111215A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;


&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="74990111215A"/>
<gate name="LED-YELLOW" symbol="LED-2PIN"/>
<gate name="LED-GREEN" symbol="LED-2PIN"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="74990111215A">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="11"/>
<connect gate="LED-GREEN" pin="K" pad="12"/>
<connect gate="LED-YELLOW" pin="A" pad="9"/>
<connect gate="LED-YELLOW" pin="K" pad="10"/>
<connect gate="RJ45LAN" pin="CRD" pad="5"/>
<connect gate="RJ45LAN" pin="CTD" pad="2"/>
<connect gate="RJ45LAN" pin="RD+" pad="4"/>
<connect gate="RJ45LAN" pin="RD-" pad="6"/>
<connect gate="RJ45LAN" pin="SH" pad="8"/>
<connect gate="RJ45LAN" pin="TD+" pad="1"/>
<connect gate="RJ45LAN" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/74990111215A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499411122A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499411122A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	PoE+ HPLE

&lt;b&gt;Tab Position	Up

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	YES



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499411122A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499411122A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-30&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7499411122A"/>
<gate name="LED-GREEN" symbol="LED-2PIN"/>
<gate name="LED-YELLOW" symbol="LED-2PIN"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="7499411122A">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="18"/>
<connect gate="LED-GREEN" pin="K" pad="17"/>
<connect gate="LED-YELLOW" pin="A" pad="20"/>
<connect gate="LED-YELLOW" pin="K" pad="19"/>
<connect gate="RJ45LAN" pin="10" pad="10"/>
<connect gate="RJ45LAN" pin="11" pad="11"/>
<connect gate="RJ45LAN" pin="12" pad="12"/>
<connect gate="RJ45LAN" pin="4" pad="4"/>
<connect gate="RJ45LAN" pin="5" pad="5"/>
<connect gate="RJ45LAN" pin="6" pad="6"/>
<connect gate="RJ45LAN" pin="VC1+" pad="13"/>
<connect gate="RJ45LAN" pin="VC1-" pad="14"/>
<connect gate="RJ45LAN" pin="VC2+" pad="15"/>
<connect gate="RJ45LAN" pin="VC2-" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499411122A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499211123A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499211123A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	PoE HPLE

&lt;b&gt;Tab Position	Down

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	YES



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499211123A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499211123A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-30&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7499211123A"/>
<gate name="LED-YELLOW" symbol="LED-2PIN"/>
<gate name="LED-GREEN" symbol="LED-2PIN"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="7499211123A">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-GREEN" pin="A" pad="13"/>
<connect gate="LED-GREEN" pin="K" pad="14"/>
<connect gate="LED-YELLOW" pin="A" pad="11"/>
<connect gate="LED-YELLOW" pin="K" pad="12"/>
<connect gate="RJ45LAN" pin="1" pad="1"/>
<connect gate="RJ45LAN" pin="2" pad="2"/>
<connect gate="RJ45LAN" pin="3" pad="3"/>
<connect gate="RJ45LAN" pin="4" pad="4"/>
<connect gate="RJ45LAN" pin="5" pad="5"/>
<connect gate="RJ45LAN" pin="VC1+" pad="7"/>
<connect gate="RJ45LAN" pin="VC1-" pad="8"/>
<connect gate="RJ45LAN" pin="VC2+" pad="9"/>
<connect gate="RJ45LAN" pin="VC2-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/pbs/datasheet/7499211123A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499511611A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499511611A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	PoE+ HPLE

&lt;b&gt;Tab Position	Up

&lt;b&gt;LED (Left-Right)	GREEN/ORANGE-YELLOW

&lt;b&gt;EMI Fingers	YES


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499511611A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499511611A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-30&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7499511611A"/>
<gate name="LED-YELLOW" symbol="LED-2PIN"/>
<gate name="LED-ORANGE/GREEN" symbol="LED-DUAL"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="7499511611A">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-ORANGE/GREEN" pin="AK1" pad="19"/>
<connect gate="LED-ORANGE/GREEN" pin="AK2" pad="20"/>
<connect gate="LED-YELLOW" pin="A" pad="18"/>
<connect gate="LED-YELLOW" pin="K" pad="17"/>
<connect gate="RJ45LAN" pin="1" pad="1"/>
<connect gate="RJ45LAN" pin="10" pad="10"/>
<connect gate="RJ45LAN" pin="11" pad="11"/>
<connect gate="RJ45LAN" pin="12" pad="12"/>
<connect gate="RJ45LAN" pin="2" pad="2"/>
<connect gate="RJ45LAN" pin="3" pad="3"/>
<connect gate="RJ45LAN" pin="4" pad="4"/>
<connect gate="RJ45LAN" pin="5" pad="5"/>
<connect gate="RJ45LAN" pin="6" pad="6"/>
<connect gate="RJ45LAN" pin="7" pad="7"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="9" pad="9"/>
<connect gate="RJ45LAN" pin="VC1+" pad="13"/>
<connect gate="RJ45LAN" pin="VC1-" pad="14"/>
<connect gate="RJ45LAN" pin="VC2+" pad="15"/>
<connect gate="RJ45LAN" pin="VC2-" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499511611A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499111614A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499111614A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard HPLE

&lt;b&gt;Tab Position	Up

&lt;b&gt;LED (Left-Right)	GREEN/ORANGE-YELLOW

&lt;b&gt;EMI Fingers	YES


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499111614A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499111614A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;


&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="RJ45LAN" symbol="7499111614A"/>
<gate name="LED-YELLOW" symbol="LED-2PIN"/>
<gate name="LED-ORANGE/GREEN" symbol="LED-DUAL"/>
<gate name="GND_SHIELD" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="7499111614A">
<connects>
<connect gate="GND_SHIELD" pin="1" pad="Z1 Z2"/>
<connect gate="LED-ORANGE/GREEN" pin="AK1" pad="16"/>
<connect gate="LED-ORANGE/GREEN" pin="AK2" pad="15"/>
<connect gate="LED-YELLOW" pin="A" pad="14"/>
<connect gate="LED-YELLOW" pin="K" pad="13"/>
<connect gate="RJ45LAN" pin="1" pad="1"/>
<connect gate="RJ45LAN" pin="10" pad="10"/>
<connect gate="RJ45LAN" pin="11" pad="12"/>
<connect gate="RJ45LAN" pin="12" pad="11"/>
<connect gate="RJ45LAN" pin="2" pad="2"/>
<connect gate="RJ45LAN" pin="3" pad="3"/>
<connect gate="RJ45LAN" pin="4" pad="4"/>
<connect gate="RJ45LAN" pin="5" pad="5"/>
<connect gate="RJ45LAN" pin="6" pad="6"/>
<connect gate="RJ45LAN" pin="7" pad="7"/>
<connect gate="RJ45LAN" pin="8" pad="8"/>
<connect gate="RJ45LAN" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPANY-URL" value="http://www.we-online.de"/>
<attribute name="CREATED-BY" value="Christin Zierenner"/>
<attribute name="CREATED-DATE" value="AUG 2012"/>
<attribute name="DATASHEET-URL" value="http://katalog.we-online.de/kataloge/eisos/media/pdf/7499111614A.pdf"/>
<attribute name="MANUFACTURER" value="Würth Elektronik eiSos GmbH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990111211" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	74990111211

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	L-R yellow-green

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/74990110030?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/74990110030?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="74990111211"/>
<gate name="YELLOW" symbol="LED-2PIN"/>
<gate name="GREEN" symbol="LED-2PIN"/>
<gate name="G$4" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="74990111211">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$4" pin="SHIELD" pad="Z1 Z2"/>
<connect gate="GREEN" pin="A" pad="11"/>
<connect gate="GREEN" pin="K" pad="12"/>
<connect gate="YELLOW" pin="A" pad="9"/>
<connect gate="YELLOW" pin="K" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UKW_2SW" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-UKW EMI Suppression 6-Hole Ferrite Bead
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Impedance will increase with more turns, available in 1 to 3 turns
&lt;br&gt;
&lt;br&gt; 4 different materials available for perfect interference suppression
&lt;Br&gt;
&lt;br&gt; Also available ready-bent or in individual length
&lt;br&gt;
&lt;br&gt; Maximum current capability is 3 A / 5 A (short-time)
&lt;br&gt;
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection against radio frequency interferences of components on PCB’s of PC’s, text processing and other digital devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeUKW_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeUKW_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-UKW/S/"&gt;http://katalog.we-online.de/en/pbs/WE-UKW/S/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created  by  Dan Xu 2014-06-10&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="_742750421" package="WE-UKW_742750421">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74275022" package="WE-UKW_74275022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FCL_ET35" prefix="L" uservalue="yes">
<description>&lt;B&gt;WE-FCL Common Mode Power Line Choke&lt;/B&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;br&gt;&lt;/b&gt;
Approximate 1% stray inductance for symmetrical interference suppression&lt;br&gt;
Closed rectangular ferrite core&lt;br&gt;
Attenuation up to 75 dB with high rated current&lt;br&gt;
Inductance tolerance: +50 %/-30%&lt;br&gt;
Operating temperature: -40°C up to +125°C&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Application&lt;br&gt;&lt;/b&gt;
Mains filter&lt;br&gt;
Suppression of common mode noise&lt;br&gt;
Switch mode power supplies&lt;br&gt;
Electronic ballast applications&lt;br&gt;
Lighting&lt;br&gt;
White goods&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndFCL_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndFCL_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FCL"&gt;http://katalog.we-online.de/en/pbs/WE-FCL?&lt;/a&gt;&lt;p&gt;


Updated on 2014-08-05&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-FCL_ET35">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_744866103"/>
<technology name="_744866104"/>
<technology name="_744866223"/>
<technology name="_744866392"/>
<technology name="_744866563"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-WAFB" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-WAFB Sleeve Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Ferrite cores for easy PCB assembly
&lt;br&gt;
&lt;br&gt; Three different materials available
&lt;br&gt;(3 W 300/ 3 W 800/ 4 W 1500 C)
&lt;br&gt;
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; THT components
&lt;br&gt;
&lt;br&gt; Sensors
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeWAFB_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeWAFB_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-WAFB"&gt;
http://katalog.we-online.de/en/pbs/WE-WAFB &lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="_7427602" package="WE-WAFB_7427602">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7427603" package="WE-WAFB_7427603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74276031" package="WE-WAFB_74276031">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74276032" package="WE-WAFB_74276032">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7427604" package="WE-WAFB_7427604">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74276041" package="WE-WAFB_74276041">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7427605" package="WE-WAFB_7427605">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74276051" package="WE-WAFB_74276051">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7427606" package="WE-WAFB_7427606">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FB_EFD20_750032052" prefix="T" uservalue="yes">
<description>&lt;b&gt; WE-FB 3751 Flyback Transformer for LT3751
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Isolation voltage: 1 kVAC 
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC (incl. self-heating) 
&lt;br&gt;
&lt;br&gt; Especially designed for LT3751 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Transformer for capacitor charger or high voltage outputs 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;





Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_1W:1W"/>
</gates>
<devices>
<device name="" package="750032052">
<connects>
<connect gate="G$1" pin="1" pad="6 7"/>
<connect gate="G$1" pin="2" pad="1"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="6" pad="4 5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_1510" prefix="L" uservalue="yes">
<description>&lt;B&gt;WE-XHMI Xtreme High Current Molded Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;br&gt;&lt;/b&gt;

Flat wire coil for low copper losses&lt;br&gt;
Composite core material allows high saturation currents&lt;br&gt;
Compact design&lt;br&gt;
Magnetically shielded&lt;br&gt;
High current capability and handles high transient current spikes&lt;br&gt;
Low leakage flux noise&lt;br&gt;
Operating temperature: -40°C up to +125°C&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;

DC/DC-converter for high current power supplies&lt;br&gt;
DC/DC-converter for Field Programmable Gate Array (FPGA)&lt;br&gt;
Power supplies for mobile devices&lt;br&gt;
POL-converters&lt;br&gt;
Mainboards/ graphic cards&lt;br&gt;
Battery powered devices&lt;br&gt;
Wireless communication devices&lt;br&gt;
Filter&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndXHMI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndXHMI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-XHMI"&gt;http://katalog.we-online.de/en/pbs/WE-XHMI&lt;/a&gt;&lt;p&gt;
Created 2015-08-05&lt;br&gt;
2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-XHMI_74439370XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439370047">
<attribute name="WE-NUMBER" value="74439370047/4,7uH"/>
</technology>
<technology name="_74439370068">
<attribute name="WE-NUMBER" value="74439370068/6,8uH"/>
</technology>
<technology name="_74439370082">
<attribute name="WE-NUMBER" value="74439370082/8,2uH"/>
</technology>
<technology name="_74439370100">
<attribute name="WE-NUMBER" value="74439370100/10uH"/>
</technology>
<technology name="_74439370150">
<attribute name="WE-NUMBER" value="74439370150/15uH"/>
</technology>
<technology name="_74439370220">
<attribute name="WE-NUMBER" value="74439370220/22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FI" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-FI&lt;BR&gt;
Leaded Toroidal Line Choke&lt;/B&gt;
&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;
Current loading up to 5 A&lt;BR&gt;
Iron powder cores with low losses&lt;BR&gt;
Low magnetically leakage field&lt;BR&gt;
Operating temperature: -25 C to +125 C&lt;BR&gt;
Custom designs on reques&lt;BR&gt;
&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;
Application in voltage transformers and power supplies&lt;BR&gt;
For interference frequencies up to 10 MHz; for switching frequencies up to 100 kHz&lt;BR&gt;
Perfect for filtering of symmetric interferences&lt;BR&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndFI_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndFI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/pbs/datasheet/7447010.pdf"&gt;http://katalog.we-online.de/pbs/datasheet/7447010.pdf&lt;/a&gt;&lt;p&gt;
Updated on 2015-06-16&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="_7447010" package="WE-FI_7447010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447011" package="WE-FI_7447011">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447012" package="WE-FI_7447012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447013" package="WE-FI_7447013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447014" package="WE-FI_7447014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447015" package="WE-FI_7447015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447016" package="WE-FI_7447016">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447017" package="WE-FI_7447017">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447018" package="WE-FI_7447018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447019" package="WE-FI_7447019">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447020" package="WE-FI_7447020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447021" package="WE-FI_7447021">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447022" package="WE-FI_7447022">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447023" package="WE-FI_7447023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447024" package="WE-FI_7447024">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447025" package="WE-FI_7447025">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447026" package="WE-FI_7447026">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447027" package="WE-FI_7447027">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447028" package="WE-FI_7447028">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74470291" package="WE-FI_74470291">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_74470292" package="WE-FI_74470292">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447030" package="WE-FI_7447030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447031" package="WE-FI_7447031">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447032" package="WE-FI_7447032">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447033" package="WE-FI_7447033">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447034" package="WE-FI_7447034">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447035" package="WE-FI_7447035">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447036" package="WE-FI_7447036">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447037" package="WE-FI_7447037">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447040" package="WE-FI_7447040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447041" package="WE-FI_7447041">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447042" package="WE-FI_7447042">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447043" package="WE-FI_7447043">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447044" package="WE-FI_7447044">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447045" package="WE-FI_7447045">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447050" package="WE-FI_7447050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447051" package="WE-FI_7447051">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447052" package="WE-FI_7447052">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447053" package="WE-FI_7447053">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447054" package="WE-FI_7447054">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447055" package="WE-FI_7447055">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447060" package="WE-FI_7447060">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447065" package="WE-FI_7447065">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447070" package="WE-FI_7447070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447071" package="WE-FI_7447071">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447075" package="WE-FI_7447075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447076" package="WE-FI_7447076">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447077" package="WE-FI_7447077">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447078" package="WE-FI_7447078">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7447079" package="WE-FI_7447079">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN-10G_749050017" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;/b&gt;&lt;p&gt;
- Compliant with standards: IEEE 802.3an and upcoming IEEE 802.3bt&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Ethernet speed up to 10Gbit/s&lt;br&gt;
--Power over Ethernet PoE and PoE+&lt;br&gt;
--10Gbit with ETR and PoE up to 150 W (for industrial applications)&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-10G"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-10G&lt;/a&gt;&lt;p&gt;
2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LAN10G:1.27&amp;0.99"/>
</gates>
<devices>
<device name="" package="WE-LAN10G:0.99MM">
<connects>
<connect gate="G$1" pin="MCT1" pad="24"/>
<connect gate="G$1" pin="MCT2" pad="21"/>
<connect gate="G$1" pin="MCT3" pad="18"/>
<connect gate="G$1" pin="MCT4" pad="15"/>
<connect gate="G$1" pin="MX1+" pad="23"/>
<connect gate="G$1" pin="MX1-" pad="22"/>
<connect gate="G$1" pin="MX2+" pad="20"/>
<connect gate="G$1" pin="MX2-" pad="19"/>
<connect gate="G$1" pin="MX3+" pad="17"/>
<connect gate="G$1" pin="MX3-" pad="16"/>
<connect gate="G$1" pin="MX4+" pad="14"/>
<connect gate="G$1" pin="MX4-" pad="13"/>
<connect gate="G$1" pin="TCT1" pad="1"/>
<connect gate="G$1" pin="TCT2" pad="4"/>
<connect gate="G$1" pin="TCT3" pad="7"/>
<connect gate="G$1" pin="TCT4" pad="10"/>
<connect gate="G$1" pin="TD1+" pad="2"/>
<connect gate="G$1" pin="TD1-" pad="3"/>
<connect gate="G$1" pin="TD2+" pad="5"/>
<connect gate="G$1" pin="TD2-" pad="6"/>
<connect gate="G$1" pin="TD3+" pad="8"/>
<connect gate="G$1" pin="TD3-" pad="9"/>
<connect gate="G$1" pin="TD4+" pad="11"/>
<connect gate="G$1" pin="TD4-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN-10G_749050018" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;/b&gt;&lt;p&gt;
- Compliant with standards: IEEE 802.3an and upcoming IEEE 802.3bt&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Ethernet speed up to 10Gbit/s&lt;br&gt;
--Power over Ethernet PoE and PoE+&lt;br&gt;
--10Gbit with ETR and PoE up to 150 W (for industrial applications)&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-10G"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-10G&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LAN10G:1.27&amp;0.99A"/>
</gates>
<devices>
<device name="" package="WE-LAN10G:0.99MM">
<connects>
<connect gate="G$1" pin="MCT1" pad="24"/>
<connect gate="G$1" pin="MCT2" pad="21"/>
<connect gate="G$1" pin="MCT3" pad="18"/>
<connect gate="G$1" pin="MCT4" pad="15"/>
<connect gate="G$1" pin="MX1+" pad="23"/>
<connect gate="G$1" pin="MX1-" pad="22"/>
<connect gate="G$1" pin="MX2+" pad="20"/>
<connect gate="G$1" pin="MX2-" pad="19"/>
<connect gate="G$1" pin="MX3+" pad="17"/>
<connect gate="G$1" pin="MX3-" pad="16"/>
<connect gate="G$1" pin="MX4+" pad="14"/>
<connect gate="G$1" pin="MX4-" pad="13"/>
<connect gate="G$1" pin="TCT1" pad="1"/>
<connect gate="G$1" pin="TCT2" pad="4"/>
<connect gate="G$1" pin="TCT3" pad="7"/>
<connect gate="G$1" pin="TCT4" pad="10"/>
<connect gate="G$1" pin="TD1+" pad="2"/>
<connect gate="G$1" pin="TD1-" pad="3"/>
<connect gate="G$1" pin="TD2+" pad="5"/>
<connect gate="G$1" pin="TD2-" pad="6"/>
<connect gate="G$1" pin="TD3+" pad="8"/>
<connect gate="G$1" pin="TD3-" pad="9"/>
<connect gate="G$1" pin="TD4+" pad="11"/>
<connect gate="G$1" pin="TD4-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN-10G_749052011" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;/b&gt;&lt;p&gt;
- Compliant with standards: IEEE 802.3an and upcoming IEEE 802.3bt&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Ethernet speed up to 10Gbit/s&lt;br&gt;
--Power over Ethernet PoE and PoE+&lt;br&gt;
--10Gbit with ETR and PoE up to 150 W (for industrial applications)&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-10G"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-10G&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LAN10G:1.27&amp;0.99"/>
</gates>
<devices>
<device name="" package="WE-LAN10G1.27MM">
<connects>
<connect gate="G$1" pin="MCT1" pad="24"/>
<connect gate="G$1" pin="MCT2" pad="21"/>
<connect gate="G$1" pin="MCT3" pad="18"/>
<connect gate="G$1" pin="MCT4" pad="15"/>
<connect gate="G$1" pin="MX1+" pad="23"/>
<connect gate="G$1" pin="MX1-" pad="22"/>
<connect gate="G$1" pin="MX2+" pad="20"/>
<connect gate="G$1" pin="MX2-" pad="19"/>
<connect gate="G$1" pin="MX3+" pad="17"/>
<connect gate="G$1" pin="MX3-" pad="16"/>
<connect gate="G$1" pin="MX4+" pad="14"/>
<connect gate="G$1" pin="MX4-" pad="13"/>
<connect gate="G$1" pin="TCT1" pad="1"/>
<connect gate="G$1" pin="TCT2" pad="4"/>
<connect gate="G$1" pin="TCT3" pad="7"/>
<connect gate="G$1" pin="TCT4" pad="10"/>
<connect gate="G$1" pin="TD1+" pad="2"/>
<connect gate="G$1" pin="TD1-" pad="3"/>
<connect gate="G$1" pin="TD2+" pad="5"/>
<connect gate="G$1" pin="TD2-" pad="6"/>
<connect gate="G$1" pin="TD3+" pad="8"/>
<connect gate="G$1" pin="TD3-" pad="9"/>
<connect gate="G$1" pin="TD4+" pad="11"/>
<connect gate="G$1" pin="TD4-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN-10G_749052012" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;/b&gt;&lt;p&gt;
- Compliant with standards: IEEE 802.3an and upcoming IEEE 802.3bt&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Ethernet speed up to 10Gbit/s&lt;br&gt;
--Power over Ethernet PoE and PoE+&lt;br&gt;
--10Gbit with ETR and PoE up to 150 W (for industrial applications)&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-10G"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-10G&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LAN10G:1.27&amp;0.99"/>
</gates>
<devices>
<device name="" package="WE-LAN10G:0.99MM">
<connects>
<connect gate="G$1" pin="MCT1" pad="24"/>
<connect gate="G$1" pin="MCT2" pad="21"/>
<connect gate="G$1" pin="MCT3" pad="18"/>
<connect gate="G$1" pin="MCT4" pad="15"/>
<connect gate="G$1" pin="MX1+" pad="23"/>
<connect gate="G$1" pin="MX1-" pad="22"/>
<connect gate="G$1" pin="MX2+" pad="20"/>
<connect gate="G$1" pin="MX2-" pad="19"/>
<connect gate="G$1" pin="MX3+" pad="17"/>
<connect gate="G$1" pin="MX3-" pad="16"/>
<connect gate="G$1" pin="MX4+" pad="14"/>
<connect gate="G$1" pin="MX4-" pad="13"/>
<connect gate="G$1" pin="TCT1" pad="1"/>
<connect gate="G$1" pin="TCT2" pad="4"/>
<connect gate="G$1" pin="TCT3" pad="7"/>
<connect gate="G$1" pin="TCT4" pad="10"/>
<connect gate="G$1" pin="TD1+" pad="2"/>
<connect gate="G$1" pin="TD1-" pad="3"/>
<connect gate="G$1" pin="TD2+" pad="5"/>
<connect gate="G$1" pin="TD2-" pad="6"/>
<connect gate="G$1" pin="TD3+" pad="8"/>
<connect gate="G$1" pin="TD3-" pad="9"/>
<connect gate="G$1" pin="TD4+" pad="11"/>
<connect gate="G$1" pin="TD4-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN-10G_749052050" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;/b&gt;&lt;p&gt;
- Compliant with standards: IEEE 802.3an and upcoming IEEE 802.3bt&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Ethernet speed up to 10Gbit/s&lt;br&gt;
--Power over Ethernet PoE and PoE+&lt;br&gt;
--10Gbit with ETR and PoE up to 150 W (for industrial applications)&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-10G"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-10G&lt;/a&gt;&lt;p&gt;
2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LAN10G:1.27&amp;0.99"/>
</gates>
<devices>
<device name="" package="WE-LAN10G1.27MM">
<connects>
<connect gate="G$1" pin="MCT1" pad="24"/>
<connect gate="G$1" pin="MCT2" pad="21"/>
<connect gate="G$1" pin="MCT3" pad="18"/>
<connect gate="G$1" pin="MCT4" pad="15"/>
<connect gate="G$1" pin="MX1+" pad="23"/>
<connect gate="G$1" pin="MX1-" pad="22"/>
<connect gate="G$1" pin="MX2+" pad="20"/>
<connect gate="G$1" pin="MX2-" pad="19"/>
<connect gate="G$1" pin="MX3+" pad="17"/>
<connect gate="G$1" pin="MX3-" pad="16"/>
<connect gate="G$1" pin="MX4+" pad="14"/>
<connect gate="G$1" pin="MX4-" pad="13"/>
<connect gate="G$1" pin="TCT1" pad="1"/>
<connect gate="G$1" pin="TCT2" pad="4"/>
<connect gate="G$1" pin="TCT3" pad="7"/>
<connect gate="G$1" pin="TCT4" pad="10"/>
<connect gate="G$1" pin="TD1+" pad="2"/>
<connect gate="G$1" pin="TD1-" pad="3"/>
<connect gate="G$1" pin="TD2+" pad="5"/>
<connect gate="G$1" pin="TD2-" pad="6"/>
<connect gate="G$1" pin="TD3+" pad="8"/>
<connect gate="G$1" pin="TD3-" pad="9"/>
<connect gate="G$1" pin="TD4+" pad="11"/>
<connect gate="G$1" pin="TD4-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN-10G_749053010" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;/b&gt;&lt;p&gt;
- Compliant with standards: IEEE 802.3an and upcoming IEEE 802.3bt&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Ethernet speed up to 10Gbit/s&lt;br&gt;
--Power over Ethernet PoE and PoE+&lt;br&gt;
--10Gbit with ETR and PoE up to 150 W (for industrial applications)&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-10G"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-10G&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LAN10G:1.27&amp;0.99"/>
</gates>
<devices>
<device name="" package="WE-LAN10G:0.99MM">
<connects>
<connect gate="G$1" pin="MCT1" pad="24"/>
<connect gate="G$1" pin="MCT2" pad="21"/>
<connect gate="G$1" pin="MCT3" pad="18"/>
<connect gate="G$1" pin="MCT4" pad="15"/>
<connect gate="G$1" pin="MX1+" pad="23"/>
<connect gate="G$1" pin="MX1-" pad="22"/>
<connect gate="G$1" pin="MX2+" pad="20"/>
<connect gate="G$1" pin="MX2-" pad="19"/>
<connect gate="G$1" pin="MX3+" pad="17"/>
<connect gate="G$1" pin="MX3-" pad="16"/>
<connect gate="G$1" pin="MX4+" pad="14"/>
<connect gate="G$1" pin="MX4-" pad="13"/>
<connect gate="G$1" pin="TCT1" pad="1"/>
<connect gate="G$1" pin="TCT2" pad="4"/>
<connect gate="G$1" pin="TCT3" pad="7"/>
<connect gate="G$1" pin="TCT4" pad="10"/>
<connect gate="G$1" pin="TD1+" pad="2"/>
<connect gate="G$1" pin="TD1-" pad="3"/>
<connect gate="G$1" pin="TD2+" pad="5"/>
<connect gate="G$1" pin="TD2-" pad="6"/>
<connect gate="G$1" pin="TD3+" pad="8"/>
<connect gate="G$1" pin="TD3-" pad="9"/>
<connect gate="G$1" pin="TD4+" pad="11"/>
<connect gate="G$1" pin="TD4-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN-10G_749053011" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;/b&gt;&lt;p&gt;
- Compliant with standards: IEEE 802.3an and upcoming IEEE 802.3bt&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Ethernet speed up to 10Gbit/s&lt;br&gt;
--Power over Ethernet PoE and PoE+&lt;br&gt;
--10Gbit with ETR and PoE up to 150 W (for industrial applications)&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-10G"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-10G&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LAN10G:1.27&amp;0.99"/>
</gates>
<devices>
<device name="" package="WE-LAN10G:0.99MM">
<connects>
<connect gate="G$1" pin="MCT1" pad="24"/>
<connect gate="G$1" pin="MCT2" pad="21"/>
<connect gate="G$1" pin="MCT3" pad="18"/>
<connect gate="G$1" pin="MCT4" pad="15"/>
<connect gate="G$1" pin="MX1+" pad="23"/>
<connect gate="G$1" pin="MX1-" pad="22"/>
<connect gate="G$1" pin="MX2+" pad="20"/>
<connect gate="G$1" pin="MX2-" pad="19"/>
<connect gate="G$1" pin="MX3+" pad="17"/>
<connect gate="G$1" pin="MX3-" pad="16"/>
<connect gate="G$1" pin="MX4+" pad="14"/>
<connect gate="G$1" pin="MX4-" pad="13"/>
<connect gate="G$1" pin="TCT1" pad="1"/>
<connect gate="G$1" pin="TCT2" pad="4"/>
<connect gate="G$1" pin="TCT3" pad="7"/>
<connect gate="G$1" pin="TCT4" pad="10"/>
<connect gate="G$1" pin="TD1+" pad="2"/>
<connect gate="G$1" pin="TD1-" pad="3"/>
<connect gate="G$1" pin="TD2+" pad="5"/>
<connect gate="G$1" pin="TD2-" pad="6"/>
<connect gate="G$1" pin="TD3+" pad="8"/>
<connect gate="G$1" pin="TD3-" pad="9"/>
<connect gate="G$1" pin="TD4+" pad="11"/>
<connect gate="G$1" pin="TD4-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN-10G_749053012" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;/b&gt;&lt;p&gt;
- Compliant with standards: IEEE 802.3an and upcoming IEEE 802.3bt&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Ethernet speed up to 10Gbit/s&lt;br&gt;
--Power over Ethernet PoE and PoE+&lt;br&gt;
--10Gbit with ETR and PoE up to 150 W (for industrial applications)&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-10G"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-10G&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LAN10G:1.27&amp;0.99"/>
</gates>
<devices>
<device name="" package="WE-LAN10G:0.99MM">
<connects>
<connect gate="G$1" pin="MCT1" pad="24"/>
<connect gate="G$1" pin="MCT2" pad="21"/>
<connect gate="G$1" pin="MCT3" pad="18"/>
<connect gate="G$1" pin="MCT4" pad="15"/>
<connect gate="G$1" pin="MX1+" pad="23"/>
<connect gate="G$1" pin="MX1-" pad="22"/>
<connect gate="G$1" pin="MX2+" pad="20"/>
<connect gate="G$1" pin="MX2-" pad="19"/>
<connect gate="G$1" pin="MX3+" pad="17"/>
<connect gate="G$1" pin="MX3-" pad="16"/>
<connect gate="G$1" pin="MX4+" pad="14"/>
<connect gate="G$1" pin="MX4-" pad="13"/>
<connect gate="G$1" pin="TCT1" pad="1"/>
<connect gate="G$1" pin="TCT2" pad="4"/>
<connect gate="G$1" pin="TCT3" pad="7"/>
<connect gate="G$1" pin="TCT4" pad="10"/>
<connect gate="G$1" pin="TD1+" pad="2"/>
<connect gate="G$1" pin="TD1-" pad="3"/>
<connect gate="G$1" pin="TD2+" pad="5"/>
<connect gate="G$1" pin="TD2-" pad="6"/>
<connect gate="G$1" pin="TD3+" pad="8"/>
<connect gate="G$1" pin="TD3-" pad="9"/>
<connect gate="G$1" pin="TD4+" pad="11"/>
<connect gate="G$1" pin="TD4-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN-10G_749053013" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;/b&gt;&lt;p&gt;
- Compliant with standards: IEEE 802.3an and upcoming IEEE 802.3bt&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Ethernet speed up to 10Gbit/s&lt;br&gt;
--Power over Ethernet PoE and PoE+&lt;br&gt;
--10Gbit with ETR and PoE up to 150 W (for industrial applications)&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-10G"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-10G&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LAN10G:1.27&amp;0.99A"/>
</gates>
<devices>
<device name="" package="WE-LAN10G:0.99MM">
<connects>
<connect gate="G$1" pin="MCT1" pad="24"/>
<connect gate="G$1" pin="MCT2" pad="21"/>
<connect gate="G$1" pin="MCT3" pad="18"/>
<connect gate="G$1" pin="MCT4" pad="15"/>
<connect gate="G$1" pin="MX1+" pad="23"/>
<connect gate="G$1" pin="MX1-" pad="22"/>
<connect gate="G$1" pin="MX2+" pad="20"/>
<connect gate="G$1" pin="MX2-" pad="19"/>
<connect gate="G$1" pin="MX3+" pad="17"/>
<connect gate="G$1" pin="MX3-" pad="16"/>
<connect gate="G$1" pin="MX4+" pad="14"/>
<connect gate="G$1" pin="MX4-" pad="13"/>
<connect gate="G$1" pin="TCT1" pad="1"/>
<connect gate="G$1" pin="TCT2" pad="4"/>
<connect gate="G$1" pin="TCT3" pad="7"/>
<connect gate="G$1" pin="TCT4" pad="10"/>
<connect gate="G$1" pin="TD1+" pad="2"/>
<connect gate="G$1" pin="TD1-" pad="3"/>
<connect gate="G$1" pin="TD2+" pad="5"/>
<connect gate="G$1" pin="TD2-" pad="6"/>
<connect gate="G$1" pin="TD3+" pad="8"/>
<connect gate="G$1" pin="TD3-" pad="9"/>
<connect gate="G$1" pin="TD4+" pad="11"/>
<connect gate="G$1" pin="TD4-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVSP_BI_400W" prefix="D" uservalue="yes">
<description>&lt;b&gt; WE-TVSP Power TVS Diode&lt;/b&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVSP/824500101"&gt;http://katalog.we-online.de/en/pbs/WE-TVSP/824500101&lt;/a&gt;&lt;p&gt;

2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="BIDIRECTIONAL"/>
</gates>
<devices>
<device name="" package="VARTVSP_SMA/DO-214AC">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_824501101"/>
<technology name="_824501102"/>
<technology name="_824501111"/>
<technology name="_824501121"/>
<technology name="_824501131"/>
<technology name="_824501141"/>
<technology name="_824501151"/>
<technology name="_824501161"/>
<technology name="_824501171"/>
<technology name="_824501181"/>
<technology name="_824501201"/>
<technology name="_824501221"/>
<technology name="_824501241"/>
<technology name="_824501261"/>
<technology name="_824501281"/>
<technology name="_824501301"/>
<technology name="_824501331"/>
<technology name="_824501361"/>
<technology name="_824501401"/>
<technology name="_824501431"/>
<technology name="_824501451"/>
<technology name="_824501481"/>
<technology name="_824501500"/>
<technology name="_824501511"/>
<technology name="_824501541"/>
<technology name="_824501581"/>
<technology name="_824501600"/>
<technology name="_824501601"/>
<technology name="_824501641"/>
<technology name="_824501650"/>
<technology name="_824501700"/>
<technology name="_824501701"/>
<technology name="_824501750"/>
<technology name="_824501751"/>
<technology name="_824501781"/>
<technology name="_824501800"/>
<technology name="_824501850"/>
<technology name="_824501851"/>
<technology name="_824501900"/>
<technology name="_824501901"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVSP_UNI_400W" prefix="D" uservalue="yes">
<description>&lt;b&gt; WE-TVSP Power TVS Diode&lt;/b&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVSP/824500101"&gt;http://katalog.we-online.de/en/pbs/WE-TVSP/824500101&lt;/a&gt;&lt;p&gt;

2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="UNIDIRECTIONAL"/>
</gates>
<devices>
<device name="" package="VARTVSP_SMA/DO-214AC_UNI">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="_824500101"/>
<technology name="_824500102"/>
<technology name="_824500111"/>
<technology name="_824500121"/>
<technology name="_824500131"/>
<technology name="_824500141"/>
<technology name="_824500151"/>
<technology name="_824500161"/>
<technology name="_824500171"/>
<technology name="_824500181"/>
<technology name="_824500201"/>
<technology name="_824500221"/>
<technology name="_824500241"/>
<technology name="_824500261"/>
<technology name="_824500281"/>
<technology name="_824500301"/>
<technology name="_824500331"/>
<technology name="_824500361"/>
<technology name="_824500401"/>
<technology name="_824500431"/>
<technology name="_824500451"/>
<technology name="_824500481"/>
<technology name="_824500500"/>
<technology name="_824500511"/>
<technology name="_824500541"/>
<technology name="_824500581"/>
<technology name="_824500600"/>
<technology name="_824500601"/>
<technology name="_824500641"/>
<technology name="_824500650"/>
<technology name="_824500700"/>
<technology name="_824500701"/>
<technology name="_824500750"/>
<technology name="_824500751"/>
<technology name="_824500781"/>
<technology name="_824500800"/>
<technology name="_824500850"/>
<technology name="_824500851"/>
<technology name="_824500900"/>
<technology name="_824500901"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-EPLE" prefix="J" uservalue="yes">
<description>&lt;b&gt; WE-EPLE USB 2.0 A Connector
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; It is recommended that the temperature of the part does
not exceed +125°C under worst case conditions.
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Storage Temperature: -20°C to +60°C
&lt;br&gt;
&lt;br&gt; Operating Temperature: -40°C to +85°C
&lt;br&gt;
&lt;br&gt; Test conditions of Electrical Properties: 20°C, 33% RH
if not specified differently
&lt;br&gt;
&lt;br&gt;Flamability rating: UL94-V0
&lt;br&gt;
&lt;br&gt;Quality class: 1500 mating cycles

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;&lt;a href="&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-EPLE_USB2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-EPLE_USB2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-EPLE/8492121"&gt;http://katalog.we-online.de/en/pbs/WE-EPLE/8492121&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="8492121"/>
</gates>
<devices>
<device name="_8492121" package="8492121">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="8492121"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-EXB" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-ExB Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; It is recommended that the temperature of the part does
not exceed +125°C under worst case conditions..
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Storage Temperature: -20°C to +60°C
&lt;br&gt;
&lt;br&gt; Operating Temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt; Temperature Rise: &lt; 55K
&lt;br&gt;
&lt;br&gt;Test conditions of Electrical Properties: 20°C, 33% RH
&lt;br&gt;if not specified differently
&lt;br&gt;

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-ExB.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-ExB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-EXB"&gt;http://katalog.we-online.de/en/pbs/WE-EXB&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-EXB"/>
</gates>
<devices>
<device name="_744844470" package="WE-EXB_744844XXX">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744844470/47uH"/>
</technology>
</technologies>
</device>
<device name="_744844102" package="WE-EXB_744844102">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744844102/1000uH"/>
</technology>
</technologies>
</device>
<device name="_744844101" package="WE-EXB_744844XXX">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744844101/100uH"/>
</technology>
</technologies>
</device>
<device name="_744844221" package="WE-EXB_744844XXX">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744844221/220uH"/>
</technology>
</technologies>
</device>
<device name="_744844471" package="WE-EXB_744844XXX">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744844471/470uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-WPCC_1W(TX)" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-WPCC Wireless Power
Charging Transmitter Coil
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Qi standard compliant
&lt;br&gt;Litzwire used - highest Q-value available on market
&lt;br&gt;Applicable for up to 20 W (up to 200 W outside the standards)
&lt;br&gt;High permeability shielding
&lt;br&gt;Cancels charging flux to be not coupled into sensitive components or batteries
&lt;br&gt;High reliable construction
&lt;br&gt;Pot core construction limits the stray field in the design

&lt;br&gt; &lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Portable devices used in a clean area, where connectors pose a risk of polluting e.g. medical facilities, (industrial) clean rooms, mining industry
&lt;br&gt;Devices with a large number of mating cycles to avoid connector damage: e.g. Smart watches, fitness tracker...
&lt;br&gt;Consumer products: e.g. Digital cameras, baby phone, walkie talkie, remote control, smartphone sleeves, watertight products
&lt;br&gt;Explosion sensitive area where the use of a physical connection is hazardous
Smart sensors

&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-WPCC%20Transmitter.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-WPCC%20Transmitter.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-WPCC-TRANSMITTER"&gt;http://katalog.we-online.de/en/pbs/WE-WPCC-TRANSMITTER&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="_760308101104" package="WE-WPCC_Φ20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308100110" package="WE-WPCC_Φ50_760308100110">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308101" package="WE-WPCC_5353_DRILL:2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308111" package="WE-WPCC_5353_DRILL:4MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308104113" package="WE-WPCC_6052">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308101103" package="WE-WPCC_Φ30">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308101304" package="WE-WPCC_Φ48">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308141" package="WE-WPCC_5353_760308141">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308102142" package="WE-WPCC_5353_760308102142">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308103102" package="WE-WPCC_5353_760308103102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308100111" package="WE-WPCC_Φ50_760308100111">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308100143" package="WE-WPCC_Φ50_760308100143">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308100141" package="WE-WPCC_Φ50_760308100141">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308101302" package="WE-WPCC_Φ50_760308101302">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308110" package="WE-WPCC_5353_DRILL:2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308105" package="WE-WPCC_5353_DRILL:4MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308102144" package="WE-WPCC_5353_DRILL:2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308102308" package="WE-WPCC_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308101105" package="WE-WPCC_Φ20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-WPCC_2W(TX)" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-WPCC Wireless Power Array
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Qi-standard compliant
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; Litzwire used – highest Q-value available on market
&lt;br&gt;
&lt;br&gt; Applicable for up to 20 W (up to 200 W outside the standards)
&lt;br&gt;
&lt;br&gt; High permeability shielding
&lt;br&gt;
&lt;br&gt; Cancels charging flux to be not coupled into sensitive components or batteries
&lt;br&gt;
&lt;br&gt; High reliable construction
&lt;br&gt;
&lt;br&gt;Pot core construction limits the stray field in the design
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable devices used in a clean area, where connectors pose a risk of polluting e.g. medical facilities, (industrial) clean rooms, mining industry
&lt;br&gt;
&lt;br&gt; Devices with a large number of mating cycles to avoid connector damage: eg. Smart watches, fitness tracker …
&lt;br&gt;
&lt;br&gt; Consumer products: eg. Digital cameras, baby phone, walkie talky, remote control, smartphone sleeves, watertight products
&lt;br&gt;
&lt;br&gt; Explosion sensitive area where the use of a physical connection is hazardous
&lt;br&gt;
&lt;br&gt; Smart sensors
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/WE-WPCC_Array_106_104119_104120.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/WE-WPCC_Array_106_104119_104120.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-WPCC-ARRAY"&gt;http://katalog.we-online.de/en/pbs/WE-WPCC-ARRAY&lt;/a&gt;&lt;p&gt;


2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-WPCC_2W"/>
</gates>
<devices>
<device name="_760308104119" package="WE-WPCC_A19">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMCI_1210HS" prefix="L" uservalue="yes">
<description>&lt;br&gt;&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PMCI Power Molded Chip
Inductor&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;
&lt;br&gt;Compact inductor chip type
&lt;br&gt;High effciency
&lt;br&gt;Suitable for applications with high currents up to 3.6 A. Very high DC-Bias current
&lt;br&gt;Very small electrical resistance, smallest RDC-Values starting at 19 mΩ
&lt;br&gt;Magnetically shielded construction: No crosstalk
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Available in five sizes and three different types (Low Profile, Standard and High Saturation Current)
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMCI"&gt;http://katalog.we-online.de/en/pbs/WE-PMCI&lt;/a&gt;&lt;p&gt;

&lt;br&gt;&lt;/b&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_1210_74479299XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479290125">
<attribute name="WE-NUMBER" value="74479290125/0,25uH"/>
</technology>
<technology name="_74479299147">
<attribute name="WE-NUMBER" value="74479299147/0,47uH"/>
</technology>
<technology name="_74479299210">
<attribute name="WE-NUMBER" value="74479299210/1uH"/>
</technology>
<technology name="_74479299222">
<attribute name="WE-NUMBER" value="7447929222/2,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMMI_0805LP" prefix="L" uservalue="yes">
<description>&lt;br&gt; &lt;B&gt;WE-PMMI Power Molded
Multilayer Inductor&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics

&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact multilayer type&lt;br&gt;
Suitable for applications with high currents up to 3.5A. Very high DC-bias current up to 4A. &lt;br&gt;
Smallest RDC-Values starting at 15 mΩ&lt;br&gt;
Magnetically shielded construction: No crosstalk&lt;br&gt;
Operating temperature: –40 °C to +125 °C&lt;br&gt;
Available in two sizes and two different types (Low Profile, Standard)&lt;br&gt;
Recommended soldering profile: Reflow&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications

&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Applications

&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;Electronic portable devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks, Digital Cameras, HDD's

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMMI_0805-0806_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMMI_0805-0806_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMMI"&gt;http://katalog.we-online.de/en/pbs/WE-PMMI&lt;/a&gt;&lt;p&gt;


&lt;br&gt;&lt;/b&gt;2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMMI_0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479974111">
<attribute name="WE-NUMBER" value="74479974111/0,11uH"/>
</technology>
<technology name="_74479974133">
<attribute name="WE-NUMBER" value="74479974133/0,33uH"/>
</technology>
<technology name="_74479974147">
<attribute name="WE-NUMBER" value="74479974147/0,47uH"/>
</technology>
<technology name="_74479974156">
<attribute name="WE-NUMBER" value="74479974156/0,56uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_210111003" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter, Solder Pin Straight
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_gerade"&gt;
http://katalog.we-online.de/en/pbs/Filter_gerade&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_9PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_210111003">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="210111003/9pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_210112043" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_abgewinkelt"&gt;
http://katalog.we-online.de/en/pbs/Filter_abgewinkelt&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_9PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2101120X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="210112043/9pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_210611003" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter, Solder Pin Straight
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_gerade"&gt;
http://katalog.we-online.de/en/pbs/Filter_gerade&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_9PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2106110X3">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="8"/>
<connect gate="G$1" pin="8" pad="7"/>
<connect gate="G$1" pin="9" pad="6"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="210611003/9pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_210612043" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_abgewinkelt"&gt;
http://katalog.we-online.de/en/pbs/Filter_abgewinkelt&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_9PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2106120X3">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="8"/>
<connect gate="G$1" pin="8" pad="7"/>
<connect gate="G$1" pin="9" pad="6"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="210612043/9pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_212111003" prefix="D-SUB">
<description>&lt;b&gt; WE-DS D-SUB-Filter, Solder Pin Straight
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_gerade"&gt;
http://katalog.we-online.de/en/pbs/Filter_gerade&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-15PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2121110X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="212111003/15pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_212112043" prefix="D-SUB">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_abgewinkelt"&gt;
http://katalog.we-online.de/en/pbs/Filter_abgewinkelt&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-15PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2121120X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="212112043/15pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_212611003" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter, Solder Pin Straight
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_gerade"&gt;
http://katalog.we-online.de/en/pbs/Filter_gerade&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-15PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2126110X3">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="10" pad="14"/>
<connect gate="G$1" pin="11" pad="13"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="11"/>
<connect gate="G$1" pin="14" pad="10"/>
<connect gate="G$1" pin="15" pad="9"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="9" pad="15"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="212611003/15pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_212612043" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_abgewinkelt"&gt;
http://katalog.we-online.de/en/pbs/Filter_abgewinkelt&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-15PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2126120X3">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="10" pad="14"/>
<connect gate="G$1" pin="11" pad="13"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="11"/>
<connect gate="G$1" pin="14" pad="10"/>
<connect gate="G$1" pin="15" pad="9"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="9" pad="15"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="212612043/15pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_214111003" prefix="D-SUB">
<description>&lt;b&gt; WE-DS D-SUB-Filter, Solder Pin Straight
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_gerade"&gt;
http://katalog.we-online.de/en/pbs/Filter_gerade&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_25PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2141110X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="214111003/25pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_214112043" prefix="D-SUB">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_abgewinkelt"&gt;
http://katalog.we-online.de/en/pbs/Filter_abgewinkelt&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_25PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2141120X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="214112043/25Pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_214611003" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter, Solder Pin Straight
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_gerade"&gt;
http://katalog.we-online.de/en/pbs/Filter_gerade&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_25PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2146110X3">
<connects>
<connect gate="G$1" pin="1" pad="13"/>
<connect gate="G$1" pin="10" pad="4"/>
<connect gate="G$1" pin="11" pad="3"/>
<connect gate="G$1" pin="12" pad="2"/>
<connect gate="G$1" pin="13" pad="1"/>
<connect gate="G$1" pin="14" pad="25"/>
<connect gate="G$1" pin="15" pad="24"/>
<connect gate="G$1" pin="16" pad="23"/>
<connect gate="G$1" pin="17" pad="22"/>
<connect gate="G$1" pin="18" pad="21"/>
<connect gate="G$1" pin="19" pad="20"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="20" pad="19"/>
<connect gate="G$1" pin="21" pad="18"/>
<connect gate="G$1" pin="22" pad="17"/>
<connect gate="G$1" pin="23" pad="16"/>
<connect gate="G$1" pin="24" pad="15"/>
<connect gate="G$1" pin="25" pad="14"/>
<connect gate="G$1" pin="3" pad="11"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="8"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="9" pad="5"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="214611003/25 pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_214612043" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_abgewinkelt"&gt;
http://katalog.we-online.de/en/pbs/Filter_abgewinkelt&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_25PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2146120X3">
<connects>
<connect gate="G$1" pin="1" pad="13"/>
<connect gate="G$1" pin="10" pad="4"/>
<connect gate="G$1" pin="11" pad="3"/>
<connect gate="G$1" pin="12" pad="2"/>
<connect gate="G$1" pin="13" pad="1"/>
<connect gate="G$1" pin="14" pad="25"/>
<connect gate="G$1" pin="15" pad="24"/>
<connect gate="G$1" pin="16" pad="23"/>
<connect gate="G$1" pin="17" pad="22"/>
<connect gate="G$1" pin="18" pad="21"/>
<connect gate="G$1" pin="19" pad="20"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="20" pad="19"/>
<connect gate="G$1" pin="21" pad="18"/>
<connect gate="G$1" pin="22" pad="17"/>
<connect gate="G$1" pin="23" pad="16"/>
<connect gate="G$1" pin="24" pad="15"/>
<connect gate="G$1" pin="25" pad="14"/>
<connect gate="G$1" pin="3" pad="11"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="8"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="9" pad="5"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="514612043/25Pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_216111003" prefix="D-SUB">
<description>&lt;b&gt; WE-DS D-SUB-Filter, Solder Pin Straight
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_gerade"&gt;
http://katalog.we-online.de/en/pbs/Filter_gerade&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-37PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2161110X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="216111003/37pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_216112043" prefix="D-SUB">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_abgewinkelt"&gt;
http://katalog.we-online.de/en/pbs/Filter_abgewinkelt&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-37PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2161120X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="216112043/37Pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_216611003" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter, Solder Pin Straight
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_gerader_Loetstift_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_gerade"&gt;
http://katalog.we-online.de/en/pbs/Filter_gerade&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-37PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2166110X3">
<connects>
<connect gate="G$1" pin="1" pad="19"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="9"/>
<connect gate="G$1" pin="12" pad="8"/>
<connect gate="G$1" pin="13" pad="7"/>
<connect gate="G$1" pin="14" pad="6"/>
<connect gate="G$1" pin="15" pad="5"/>
<connect gate="G$1" pin="16" pad="4"/>
<connect gate="G$1" pin="17" pad="3"/>
<connect gate="G$1" pin="18" pad="2"/>
<connect gate="G$1" pin="19" pad="1"/>
<connect gate="G$1" pin="2" pad="18"/>
<connect gate="G$1" pin="20" pad="37"/>
<connect gate="G$1" pin="21" pad="36"/>
<connect gate="G$1" pin="22" pad="35"/>
<connect gate="G$1" pin="23" pad="34"/>
<connect gate="G$1" pin="24" pad="33"/>
<connect gate="G$1" pin="25" pad="32"/>
<connect gate="G$1" pin="26" pad="31"/>
<connect gate="G$1" pin="27" pad="30"/>
<connect gate="G$1" pin="28" pad="29"/>
<connect gate="G$1" pin="29" pad="28"/>
<connect gate="G$1" pin="3" pad="17"/>
<connect gate="G$1" pin="30" pad="27"/>
<connect gate="G$1" pin="31" pad="26"/>
<connect gate="G$1" pin="32" pad="25"/>
<connect gate="G$1" pin="33" pad="24"/>
<connect gate="G$1" pin="34" pad="23"/>
<connect gate="G$1" pin="35" pad="22"/>
<connect gate="G$1" pin="36" pad="21"/>
<connect gate="G$1" pin="37" pad="20"/>
<connect gate="G$1" pin="4" pad="16"/>
<connect gate="G$1" pin="5" pad="15"/>
<connect gate="G$1" pin="6" pad="14"/>
<connect gate="G$1" pin="7" pad="13"/>
<connect gate="G$1" pin="8" pad="12"/>
<connect gate="G$1" pin="9" pad="11"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="216611003/37Pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_216612043" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_abgewinkelt_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_abgewinkelt"&gt;
http://katalog.we-online.de/en/pbs/Filter_abgewinkelt&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-37PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2166120X3">
<connects>
<connect gate="G$1" pin="1" pad="19"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="9"/>
<connect gate="G$1" pin="12" pad="8"/>
<connect gate="G$1" pin="13" pad="7"/>
<connect gate="G$1" pin="14" pad="6"/>
<connect gate="G$1" pin="15" pad="5"/>
<connect gate="G$1" pin="16" pad="4"/>
<connect gate="G$1" pin="17" pad="3"/>
<connect gate="G$1" pin="18" pad="2"/>
<connect gate="G$1" pin="19" pad="1"/>
<connect gate="G$1" pin="2" pad="18"/>
<connect gate="G$1" pin="20" pad="37"/>
<connect gate="G$1" pin="21" pad="36"/>
<connect gate="G$1" pin="22" pad="35"/>
<connect gate="G$1" pin="23" pad="34"/>
<connect gate="G$1" pin="24" pad="33"/>
<connect gate="G$1" pin="25" pad="32"/>
<connect gate="G$1" pin="26" pad="31"/>
<connect gate="G$1" pin="27" pad="30"/>
<connect gate="G$1" pin="28" pad="29"/>
<connect gate="G$1" pin="29" pad="28"/>
<connect gate="G$1" pin="3" pad="17"/>
<connect gate="G$1" pin="30" pad="27"/>
<connect gate="G$1" pin="31" pad="26"/>
<connect gate="G$1" pin="32" pad="25"/>
<connect gate="G$1" pin="33" pad="24"/>
<connect gate="G$1" pin="34" pad="23"/>
<connect gate="G$1" pin="35" pad="22"/>
<connect gate="G$1" pin="36" pad="21"/>
<connect gate="G$1" pin="37" pad="20"/>
<connect gate="G$1" pin="4" pad="16"/>
<connect gate="G$1" pin="5" pad="15"/>
<connect gate="G$1" pin="6" pad="14"/>
<connect gate="G$1" pin="7" pad="13"/>
<connect gate="G$1" pin="8" pad="12"/>
<connect gate="G$1" pin="9" pad="11"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="216612043/37pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_240117113" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Low size: 6.3 mm
&lt;br&gt;
&lt;br&gt; Rated voltage: 125 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_SMD?sid=29b915c42a"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-Filter Bent 90°&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_9PIN_SMD"/>
</gates>
<devices>
<device name="" package="WE-DS_240117113">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="10 11 12 13 GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="240117113/9pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_240617113" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Low size: 6.3 mm
&lt;br&gt;
&lt;br&gt; Rated voltage: 125 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_SMD?sid=29b915c42a"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-Filter Bent 90°&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_9PIN_SMD"/>
</gates>
<devices>
<device name="" package="WE-DS_240617113">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="8"/>
<connect gate="G$1" pin="8" pad="7"/>
<connect gate="G$1" pin="9" pad="6"/>
<connect gate="G$1" pin="GND" pad="10 11 12 13 GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="240617113/9pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_242117113" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Low size: 6.3 mm
&lt;br&gt;
&lt;br&gt; Rated voltage: 125 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_SMD?sid=29b915c42a"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-Filter Bent 90°&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_15PIN_SMD"/>
</gates>
<devices>
<device name="" package="WE-DS_242117113">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2 L1 L2 R1 R2" route="any"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="242117113/15pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_242617113" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Low size: 6.3 mm
&lt;br&gt;
&lt;br&gt; Rated voltage: 125 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_SMD?sid=29b915c42a"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-Filter Bent 90°&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_15PIN_SMD"/>
</gates>
<devices>
<device name="" package="WE-DS_242617113">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="10" pad="14"/>
<connect gate="G$1" pin="11" pad="13"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="11"/>
<connect gate="G$1" pin="14" pad="10"/>
<connect gate="G$1" pin="15" pad="9"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="9" pad="15"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2 L1 L2 R1 R2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="242617113/15pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_244117113" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Low size: 6.3 mm
&lt;br&gt;
&lt;br&gt; Rated voltage: 125 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_SMD?sid=29b915c42a"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-Filter Bent 90°&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_25PIN_SMD"/>
</gates>
<devices>
<device name="" package="WE-DS_244117113">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2 L1 L2 R1 R2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="244117113/25pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_244617113" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Low size: 6.3 mm
&lt;br&gt;
&lt;br&gt; Rated voltage: 125 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_SMD?sid=29b915c42a"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-Filter Bent 90°&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_25PIN_SMD"/>
</gates>
<devices>
<device name="" package="WE-DS_244617113">
<connects>
<connect gate="G$1" pin="1" pad="13"/>
<connect gate="G$1" pin="10" pad="4"/>
<connect gate="G$1" pin="11" pad="3"/>
<connect gate="G$1" pin="12" pad="2"/>
<connect gate="G$1" pin="13" pad="1"/>
<connect gate="G$1" pin="14" pad="25"/>
<connect gate="G$1" pin="15" pad="24"/>
<connect gate="G$1" pin="16" pad="23"/>
<connect gate="G$1" pin="17" pad="22"/>
<connect gate="G$1" pin="18" pad="21"/>
<connect gate="G$1" pin="19" pad="20"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="20" pad="19"/>
<connect gate="G$1" pin="21" pad="18"/>
<connect gate="G$1" pin="22" pad="17"/>
<connect gate="G$1" pin="23" pad="16"/>
<connect gate="G$1" pin="24" pad="15"/>
<connect gate="G$1" pin="25" pad="14"/>
<connect gate="G$1" pin="3" pad="11"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="8"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="9" pad="5"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2 L1 L2 R1 R2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="244617113/25pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_246117113" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Low size: 6.3 mm
&lt;br&gt;
&lt;br&gt; Rated voltage: 125 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_SMD?sid=29b915c42a"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-Filter Bent 90°&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_37PIN_SMD"/>
</gates>
<devices>
<device name="" package="WE-DS_246117113">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2 L1 L2 R1 R2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="246117113/37Pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_246617113" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Low size: 6.3 mm
&lt;br&gt;
&lt;br&gt; Rated voltage: 125 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_AbsDSubFilter_SMD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/Filter_SMD?sid=29b915c42a"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-Filter Bent 90°&lt;/a&gt;&lt;p&gt;


Created on 2015-05-04&lt;br&gt;
2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_37PIN_SMD"/>
</gates>
<devices>
<device name="" package="WE-DS_246617113">
<connects>
<connect gate="G$1" pin="1" pad="19"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="9"/>
<connect gate="G$1" pin="12" pad="8"/>
<connect gate="G$1" pin="13" pad="7"/>
<connect gate="G$1" pin="14" pad="6"/>
<connect gate="G$1" pin="15" pad="5"/>
<connect gate="G$1" pin="16" pad="4"/>
<connect gate="G$1" pin="17" pad="3"/>
<connect gate="G$1" pin="18" pad="2"/>
<connect gate="G$1" pin="19" pad="1"/>
<connect gate="G$1" pin="2" pad="18"/>
<connect gate="G$1" pin="20" pad="37"/>
<connect gate="G$1" pin="21" pad="36"/>
<connect gate="G$1" pin="22" pad="35"/>
<connect gate="G$1" pin="23" pad="34"/>
<connect gate="G$1" pin="24" pad="33"/>
<connect gate="G$1" pin="25" pad="32"/>
<connect gate="G$1" pin="26" pad="31"/>
<connect gate="G$1" pin="27" pad="30"/>
<connect gate="G$1" pin="28" pad="29"/>
<connect gate="G$1" pin="29" pad="28"/>
<connect gate="G$1" pin="3" pad="17"/>
<connect gate="G$1" pin="30" pad="27"/>
<connect gate="G$1" pin="31" pad="26"/>
<connect gate="G$1" pin="32" pad="25"/>
<connect gate="G$1" pin="33" pad="24"/>
<connect gate="G$1" pin="34" pad="23"/>
<connect gate="G$1" pin="35" pad="22"/>
<connect gate="G$1" pin="36" pad="21"/>
<connect gate="G$1" pin="37" pad="20"/>
<connect gate="G$1" pin="4" pad="16"/>
<connect gate="G$1" pin="5" pad="15"/>
<connect gate="G$1" pin="6" pad="14"/>
<connect gate="G$1" pin="7" pad="13"/>
<connect gate="G$1" pin="8" pad="12"/>
<connect gate="G$1" pin="9" pad="11"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2 L1 L2 R1 R2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="246617113/37Pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-POEH_EPQ13" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-PoEH Power over Ethernet High Power Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; DFlyback or Forward Transformer
&lt;br&gt;Input voltage: 9 V or 33 V to 57 V
&lt;br&gt;Switching frequencies: 200-400 kHz
&lt;br&gt;Operating temperature: -40°C up to +125°C
&lt;br&gt;Insulation test voltage: 1.5 kVAC
&lt;br&gt;Different output voltages available
&lt;br&gt;Optimized core and bobbin design for 30% more power handling
&lt;br&gt;Standard footprint to EP13

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE and PoE+ powered devices
&lt;br&gt;Telecom
&lt;br&gt;Industrial applications
&lt;br&gt;WLAN acess point
&lt;br&gt;Safety cameras

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PoEH.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PoEH.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-POEH?"&gt;http://katalog.we-online.de/en/pbs/WE-POEH&lt;/a&gt;&lt;p&gt;



20146 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:2W"/>
</gates>
<devices>
<device name="" package="WE_EPQ13_SMD_10PIN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="9"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="7"/>
<connect gate="G$1" pin="6" pad="5"/>
<connect gate="G$1" pin="7" pad="4"/>
<connect gate="G$1" pin="8" pad="3"/>
</connects>
<technologies>
<technology name="_7491195112"/>
<technology name="_7491195212"/>
<technology name="_7491195224"/>
<technology name="_749119533"/>
<technology name="_7491195331"/>
<technology name="_749119550"/>
<technology name="_7491195501"/>
<technology name="_7491196112"/>
<technology name="_7491196212"/>
<technology name="_749119633"/>
<technology name="_7491196331"/>
<technology name="_749119650"/>
<technology name="_7491196501"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_7490100111A" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN LAN Transformer 10/100 Base T&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3, IEEE 802.3af and IEEE 802.3at standards&lt;br&gt;
- SMT&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/7490100111A"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/7490100111A&lt;/a&gt;&lt;p&gt;

2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7490100111A"/>
</gates>
<devices>
<device name="" package="7490100111A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_7490100161A" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN LAN Transformer 10/100 Base T&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3, IEEE 802.3af and IEEE 802.3at standards&lt;br&gt;
- SMT&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/7490100161A"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/7490100161A&lt;/a&gt;&lt;p&gt;

2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7490100161A"/>
</gates>
<devices>
<device name="" package="7490100161A">
<connects>
<connect gate="G$1" pin="CRD" pad="10"/>
<connect gate="G$1" pin="CRX" pad="7"/>
<connect gate="G$1" pin="CTD" pad="15"/>
<connect gate="G$1" pin="CTX" pad="2"/>
<connect gate="G$1" pin="RD+" pad="11"/>
<connect gate="G$1" pin="RD-" pad="9"/>
<connect gate="G$1" pin="RX+" pad="6"/>
<connect gate="G$1" pin="RX-" pad="8"/>
<connect gate="G$1" pin="TD+" pad="16"/>
<connect gate="G$1" pin="TD-" pad="14"/>
<connect gate="G$1" pin="TX+" pad="1"/>
<connect gate="G$1" pin="TX-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_7490120110" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN LAN Transformer 10/100 Base T&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3, IEEE 802.3af and IEEE 802.3at standards&lt;br&gt;
- SMT&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/S"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/S&lt;/a&gt;&lt;p&gt;

2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7490120110"/>
</gates>
<devices>
<device name="" package="7490120110">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_7490140112" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN LAN Transformer 10/100 Base T&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3, IEEE 802.3af and IEEE 802.3at standards&lt;br&gt;
- SMT&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/7490140112"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/7490140112&lt;/a&gt;&lt;p&gt;

2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7490140112"/>
</gates>
<devices>
<device name="" package="7490140112">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_749014018" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN LAN Transformer 10/100 Base T&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3, IEEE 802.3af and IEEE 802.3at standards&lt;br&gt;
- SMT&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/7490100111A"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/749014018&lt;/a&gt;&lt;p&gt;

2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="749014018"/>
</gates>
<devices>
<device name="" package="749014018">
<connects>
<connect gate="G$1" pin="CRD" pad="2"/>
<connect gate="G$1" pin="CRX" pad="11"/>
<connect gate="G$1" pin="CTD" pad="5"/>
<connect gate="G$1" pin="CTX" pad="8"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="3"/>
<connect gate="G$1" pin="RX+" pad="12"/>
<connect gate="G$1" pin="RX-" pad="10"/>
<connect gate="G$1" pin="TD+" pad="4"/>
<connect gate="G$1" pin="TD-" pad="6"/>
<connect gate="G$1" pin="TX+" pad="9"/>
<connect gate="G$1" pin="TX-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_749020010A" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN LAN Transformer 10/100 Base T&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3, IEEE 802.3af and IEEE 802.3at standards&lt;br&gt;
- SMT&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/749020010A"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/749020010A&lt;/a&gt;&lt;p&gt;

2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="749020010A"/>
</gates>
<devices>
<device name="" package="74902001XA">
<connects>
<connect gate="G$1" pin="MCT1" pad="24"/>
<connect gate="G$1" pin="MCT2" pad="21"/>
<connect gate="G$1" pin="MCT3" pad="18"/>
<connect gate="G$1" pin="MCT4" pad="15"/>
<connect gate="G$1" pin="MX1+" pad="23"/>
<connect gate="G$1" pin="MX1-" pad="22"/>
<connect gate="G$1" pin="MX2+" pad="20"/>
<connect gate="G$1" pin="MX2-" pad="19"/>
<connect gate="G$1" pin="MX3+" pad="17"/>
<connect gate="G$1" pin="MX3-" pad="16"/>
<connect gate="G$1" pin="MX4+" pad="14"/>
<connect gate="G$1" pin="MX4-" pad="13"/>
<connect gate="G$1" pin="TCT1" pad="1"/>
<connect gate="G$1" pin="TCT2" pad="4"/>
<connect gate="G$1" pin="TCT3" pad="7"/>
<connect gate="G$1" pin="TCT4" pad="10"/>
<connect gate="G$1" pin="TD1+" pad="2"/>
<connect gate="G$1" pin="TD1-" pad="3"/>
<connect gate="G$1" pin="TD2+" pad="5"/>
<connect gate="G$1" pin="TD2-" pad="6"/>
<connect gate="G$1" pin="TD3+" pad="8"/>
<connect gate="G$1" pin="TD3-" pad="9"/>
<connect gate="G$1" pin="TD4+" pad="11"/>
<connect gate="G$1" pin="TD4-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_7490200136" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN LAN Transformer 10/100 Base T&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3, IEEE 802.3af and IEEE 802.3at standards&lt;br&gt;
- SMT&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/7490200136"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/7490200136&lt;/a&gt;&lt;p&gt;

2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7490200136"/>
</gates>
<devices>
<device name="" package="7490200136">
<connects>
<connect gate="G$1" pin="D+" pad="2"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="D1+" pad="5"/>
<connect gate="G$1" pin="D1-" pad="6"/>
<connect gate="G$1" pin="D2+" pad="8"/>
<connect gate="G$1" pin="D2-" pad="9"/>
<connect gate="G$1" pin="D3+" pad="11"/>
<connect gate="G$1" pin="D3-" pad="12"/>
<connect gate="G$1" pin="TD" pad="1"/>
<connect gate="G$1" pin="TD1" pad="4"/>
<connect gate="G$1" pin="TD2" pad="7"/>
<connect gate="G$1" pin="TD3" pad="10"/>
<connect gate="G$1" pin="TX" pad="15"/>
<connect gate="G$1" pin="TX1" pad="18"/>
<connect gate="G$1" pin="TX2" pad="21"/>
<connect gate="G$1" pin="TX3" pad="24"/>
<connect gate="G$1" pin="X+" pad="14"/>
<connect gate="G$1" pin="X-" pad="13"/>
<connect gate="G$1" pin="X1+" pad="17"/>
<connect gate="G$1" pin="X1-" pad="16"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="23"/>
<connect gate="G$1" pin="X3-" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_749020111A" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN LAN Transformer 10/100 Base T&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3, IEEE 802.3af and IEEE 802.3at standards&lt;br&gt;
- SMT&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/7490100111A"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/7490100111A&lt;/a&gt;&lt;p&gt;

2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="749020111A"/>
</gates>
<devices>
<device name="" package="749020111A">
<connects>
<connect gate="G$1" pin="D1+" pad="1"/>
<connect gate="G$1" pin="D1-" pad="2"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="7"/>
<connect gate="G$1" pin="D3-" pad="8"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="TD1" pad="3"/>
<connect gate="G$1" pin="TD2" pad="4"/>
<connect gate="G$1" pin="TD3" pad="9"/>
<connect gate="G$1" pin="TD4" pad="10"/>
<connect gate="G$1" pin="TX1" pad="22"/>
<connect gate="G$1" pin="TX2" pad="21"/>
<connect gate="G$1" pin="TX3" pad="16"/>
<connect gate="G$1" pin="TX4" pad="15"/>
<connect gate="G$1" pin="X1+" pad="24"/>
<connect gate="G$1" pin="X1-" pad="23"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="18"/>
<connect gate="G$1" pin="X3-" pad="17"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN-10G_749050010U" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;/b&gt;&lt;p&gt;
- Compliant with standards: IEEE 802.3an and upcoming IEEE 802.3bt&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Ethernet speed up to 10Gbit/s&lt;br&gt;
--Power over Ethernet PoE and PoE+&lt;br&gt;
--10Gbit with ETR and PoE up to 150 W (for industrial applications)&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-10G"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-10G&lt;/a&gt;&lt;p&gt;
2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="749050010U"/>
</gates>
<devices>
<device name="" package="749050010U">
<connects>
<connect gate="G$1" pin="D1+" pad="23"/>
<connect gate="G$1" pin="D1-" pad="22"/>
<connect gate="G$1" pin="D2+" pad="20"/>
<connect gate="G$1" pin="D2-" pad="19"/>
<connect gate="G$1" pin="D3+" pad="17"/>
<connect gate="G$1" pin="D3-" pad="16"/>
<connect gate="G$1" pin="D4+" pad="14"/>
<connect gate="G$1" pin="D4-" pad="13"/>
<connect gate="G$1" pin="TD1" pad="24"/>
<connect gate="G$1" pin="TD2" pad="21"/>
<connect gate="G$1" pin="TD3" pad="18"/>
<connect gate="G$1" pin="TD4" pad="15"/>
<connect gate="G$1" pin="TX1" pad="1"/>
<connect gate="G$1" pin="TX2" pad="4"/>
<connect gate="G$1" pin="TX3" pad="7"/>
<connect gate="G$1" pin="TX4" pad="10"/>
<connect gate="G$1" pin="X1+" pad="2"/>
<connect gate="G$1" pin="X1-" pad="3"/>
<connect gate="G$1" pin="X2+" pad="5"/>
<connect gate="G$1" pin="X2-" pad="6"/>
<connect gate="G$1" pin="X3+" pad="8"/>
<connect gate="G$1" pin="X3-" pad="9"/>
<connect gate="G$1" pin="X4+" pad="11"/>
<connect gate="G$1" pin="X4-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499211125" prefix="T" uservalue="yes">
<description>&lt;b&gt; WE-RJ45 LAN Transformer &lt;/b&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics&lt;/b&gt;&lt;br&gt;
&lt;br&gt;RJ45 Connector with integrated transformer/ common mode choke
&lt;br&gt;Available in SMD, THT and THT with USB
&lt;br&gt;350µH min. OCL with 8mA bias
&lt;br&gt;Complies with IEEE 802.3
&lt;br&gt;Extended temperature range -40°C to +85°C available
&lt;br&gt;PoE/ PoE+
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt;xDSL Modems
&lt;br&gt;Embedded PC
&lt;br&gt;LAN Applications
&lt;br&gt;Hub, Router, Switches
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45/7499211125"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45/7499211125&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Yingchun Shan 2016-08-30&lt;br&gt;
&lt;/b&gt;2016(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499211125"/>
<gate name="G$2" symbol="GND_PIN"/>
<gate name="GREEN" symbol="LED-2PIN"/>
<gate name="YELLOW" symbol="LED-2PIN"/>
</gates>
<devices>
<device name="" package="7499211125">
<connects>
<connect gate="G$1" pin="CRD" pad="3"/>
<connect gate="G$1" pin="CTD" pad="5"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="2"/>
<connect gate="G$1" pin="TD+" pad="4"/>
<connect gate="G$1" pin="TD-" pad="6"/>
<connect gate="G$1" pin="VC1+" pad="9"/>
<connect gate="G$1" pin="VC1-" pad="10"/>
<connect gate="G$2" pin="1" pad="Z3 Z4"/>
<connect gate="GREEN" pin="A" pad="12"/>
<connect gate="GREEN" pin="K" pad="11"/>
<connect gate="YELLOW" pin="A" pad="13"/>
<connect gate="YELLOW" pin="K" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_210111023" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter, Solder Pin Straight
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_D-SUB-Filter_mit_geradem_Ltstift.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_D-SUB-Filter_mit_geradem_Ltstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT/210111023"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT/210111023&lt;/a&gt;&lt;p&gt;



2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_9PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_210111023">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="210111023/9pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_210112013" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;



2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_9PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2101120X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="210112013/9pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_210611023" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter, Solder Pin Straight
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_D-SUB-Filter_mit_geradem_Ltstift.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_D-SUB-Filter_mit_geradem_Ltstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT/210111023"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT/210111023&lt;/a&gt;&lt;p&gt;



2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_9PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2106110X3">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="8"/>
<connect gate="G$1" pin="8" pad="7"/>
<connect gate="G$1" pin="9" pad="6"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="210611023/9pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_210612013" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;


2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_9PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2106120X3">
<connects>
<connect gate="G$1" pin="1" pad="5"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="8"/>
<connect gate="G$1" pin="8" pad="7"/>
<connect gate="G$1" pin="9" pad="6"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="210612013/9pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_212111023" prefix="D-SUB">
<description>&lt;b&gt; WE-DS D-SUB-Filter, Solder Pin Straight
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_D-SUB-Filter_mit_geradem_Ltstift.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_D-SUB-Filter_mit_geradem_Ltstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT/212111023"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT/212111023&lt;/a&gt;&lt;p&gt;



2016(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-15PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2121110X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="212111023/15pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_212112013" prefix="D-SUB">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;



2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-15PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2121120X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="212112013/15pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_212611023" prefix="D-SUB">
<description>&lt;b&gt; WE-DS D-SUB-Filter, Solder Pin Straight
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_D-SUB-Filter_mit_geradem_Ltstift.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_D-SUB-Filter_mit_geradem_Ltstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT/212611023"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT/212611023&lt;/a&gt;&lt;p&gt;


2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-15PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2126110X3">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="10" pad="14"/>
<connect gate="G$1" pin="11" pad="13"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="11"/>
<connect gate="G$1" pin="14" pad="10"/>
<connect gate="G$1" pin="15" pad="9"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="9" pad="15"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="212611023/15pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_212612013" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;


2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-15PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2126120X3">
<connects>
<connect gate="G$1" pin="1" pad="8"/>
<connect gate="G$1" pin="10" pad="14"/>
<connect gate="G$1" pin="11" pad="13"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="11"/>
<connect gate="G$1" pin="14" pad="10"/>
<connect gate="G$1" pin="15" pad="9"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="4"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
<connect gate="G$1" pin="9" pad="15"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="212612013/15pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_214111023" prefix="D-SUB">
<description>&lt;b&gt; WE-DS D-SUB-Filter Solder Cup
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Easy soldering, even for small strand cross sections
&lt;br&gt;
&lt;br&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt;  Rated current @ 20 ºC: 5 A 
&lt;br&gt;
&lt;br&gt; Withstand voltage: 250 VRMS
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt;Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_mit_loetkelch.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_mit_loetkelch.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-SOLDER-CUP/210613023"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-SOLDER-CUP/210613023&lt;/a&gt;&lt;p&gt;

2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_25PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2141110X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="214111023/25pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_214112013" prefix="D-SUB">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;


2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_25PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2141120X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="214112013/25pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_214611023" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter, Solder Pin Straight
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_D-SUB-Filter_mit_geradem_Ltstift.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_D-SUB-Filter_mit_geradem_Ltstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;


2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_25PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2146110X3">
<connects>
<connect gate="G$1" pin="1" pad="13"/>
<connect gate="G$1" pin="10" pad="4"/>
<connect gate="G$1" pin="11" pad="3"/>
<connect gate="G$1" pin="12" pad="2"/>
<connect gate="G$1" pin="13" pad="1"/>
<connect gate="G$1" pin="14" pad="25"/>
<connect gate="G$1" pin="15" pad="24"/>
<connect gate="G$1" pin="16" pad="23"/>
<connect gate="G$1" pin="17" pad="22"/>
<connect gate="G$1" pin="18" pad="21"/>
<connect gate="G$1" pin="19" pad="20"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="20" pad="19"/>
<connect gate="G$1" pin="21" pad="18"/>
<connect gate="G$1" pin="22" pad="17"/>
<connect gate="G$1" pin="23" pad="16"/>
<connect gate="G$1" pin="24" pad="15"/>
<connect gate="G$1" pin="25" pad="14"/>
<connect gate="G$1" pin="3" pad="11"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="8"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="9" pad="5"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="214611023/25Pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_214612013" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;


2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS_25PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2146120X3">
<connects>
<connect gate="G$1" pin="1" pad="13"/>
<connect gate="G$1" pin="10" pad="4"/>
<connect gate="G$1" pin="11" pad="3"/>
<connect gate="G$1" pin="12" pad="2"/>
<connect gate="G$1" pin="13" pad="1"/>
<connect gate="G$1" pin="14" pad="25"/>
<connect gate="G$1" pin="15" pad="24"/>
<connect gate="G$1" pin="16" pad="23"/>
<connect gate="G$1" pin="17" pad="22"/>
<connect gate="G$1" pin="18" pad="21"/>
<connect gate="G$1" pin="19" pad="20"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="20" pad="19"/>
<connect gate="G$1" pin="21" pad="18"/>
<connect gate="G$1" pin="22" pad="17"/>
<connect gate="G$1" pin="23" pad="16"/>
<connect gate="G$1" pin="24" pad="15"/>
<connect gate="G$1" pin="25" pad="14"/>
<connect gate="G$1" pin="3" pad="11"/>
<connect gate="G$1" pin="4" pad="10"/>
<connect gate="G$1" pin="5" pad="9"/>
<connect gate="G$1" pin="6" pad="8"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="9" pad="5"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="214612043/25pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_216111023" prefix="D-SUB">
<description>&lt;b&gt; WE-DS D-SUB-Filter, Solder Pin Straight
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_D-SUB-Filter_mit_geradem_Ltstift.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_D-SUB-Filter_mit_geradem_Ltstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;



2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-37PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2161110X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="216111023/37Pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_216112013" prefix="D-SUB">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;


2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-37PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2161120X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="216112013/37Pins_male"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_216611023" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter, Solder Pin Straight
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation: max. ≥ 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of UNC 4/40 or through hole
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_D-SUB-Filter_mit_geradem_Ltstift.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_D-SUB-Filter_mit_geradem_Ltstift.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-STRAIGHT&lt;/a&gt;&lt;p&gt;



2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-37PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2166110X3">
<connects>
<connect gate="G$1" pin="1" pad="19"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="9"/>
<connect gate="G$1" pin="12" pad="8"/>
<connect gate="G$1" pin="13" pad="7"/>
<connect gate="G$1" pin="14" pad="6"/>
<connect gate="G$1" pin="15" pad="5"/>
<connect gate="G$1" pin="16" pad="4"/>
<connect gate="G$1" pin="17" pad="3"/>
<connect gate="G$1" pin="18" pad="2"/>
<connect gate="G$1" pin="19" pad="1"/>
<connect gate="G$1" pin="2" pad="18"/>
<connect gate="G$1" pin="20" pad="37"/>
<connect gate="G$1" pin="21" pad="36"/>
<connect gate="G$1" pin="22" pad="35"/>
<connect gate="G$1" pin="23" pad="34"/>
<connect gate="G$1" pin="24" pad="33"/>
<connect gate="G$1" pin="25" pad="32"/>
<connect gate="G$1" pin="26" pad="31"/>
<connect gate="G$1" pin="27" pad="30"/>
<connect gate="G$1" pin="28" pad="29"/>
<connect gate="G$1" pin="29" pad="28"/>
<connect gate="G$1" pin="3" pad="17"/>
<connect gate="G$1" pin="30" pad="27"/>
<connect gate="G$1" pin="31" pad="26"/>
<connect gate="G$1" pin="32" pad="25"/>
<connect gate="G$1" pin="33" pad="24"/>
<connect gate="G$1" pin="34" pad="23"/>
<connect gate="G$1" pin="35" pad="22"/>
<connect gate="G$1" pin="36" pad="21"/>
<connect gate="G$1" pin="37" pad="20"/>
<connect gate="G$1" pin="4" pad="16"/>
<connect gate="G$1" pin="5" pad="15"/>
<connect gate="G$1" pin="6" pad="14"/>
<connect gate="G$1" pin="7" pad="13"/>
<connect gate="G$1" pin="8" pad="12"/>
<connect gate="G$1" pin="9" pad="11"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="216611023/37pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DS_216612013" prefix="D-SUB" uservalue="yes">
<description>&lt;b&gt; WE-DS D-SUB-Filter Connectors Bent 90°
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Standard type filtered with 1000 pF
&lt;br&gt;
&lt;br&gt; High attenuation of more than 40 dB @ 180 MHz
&lt;br&gt;
&lt;br&gt; Choice of earthing metal sheet or high speed
earthing clip
&lt;br&gt;
&lt;br&gt; Rated voltage: 100 VDC
&lt;br&gt;
&lt;br&gt; Rated current @ 20 ºC: 5 A
&lt;br&gt;
&lt;br&gt;  Withstand voltage: 250 VRMS 
&lt;br&gt;
&lt;br&gt; Insulation resistance: min. 1000 MΩ
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filtering of interfaces 
&lt;br&gt;
&lt;br&gt; External connection to 
&lt;br&gt;  -printer
&lt;br&gt;  -sensor
&lt;br&gt;  -display
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_d-sub_filter_90_abgewinkelt.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90"&gt;
http://katalog.we-online.de/en/pbs/D-SUB-FILTER-BENT90&lt;/a&gt;&lt;p&gt;



2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DS-37PIN"/>
</gates>
<devices>
<device name="" package="WE-DS_2166120X3">
<connects>
<connect gate="G$1" pin="1" pad="19"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="9"/>
<connect gate="G$1" pin="12" pad="8"/>
<connect gate="G$1" pin="13" pad="7"/>
<connect gate="G$1" pin="14" pad="6"/>
<connect gate="G$1" pin="15" pad="5"/>
<connect gate="G$1" pin="16" pad="4"/>
<connect gate="G$1" pin="17" pad="3"/>
<connect gate="G$1" pin="18" pad="2"/>
<connect gate="G$1" pin="19" pad="1"/>
<connect gate="G$1" pin="2" pad="18"/>
<connect gate="G$1" pin="20" pad="37"/>
<connect gate="G$1" pin="21" pad="36"/>
<connect gate="G$1" pin="22" pad="35"/>
<connect gate="G$1" pin="23" pad="34"/>
<connect gate="G$1" pin="24" pad="33"/>
<connect gate="G$1" pin="25" pad="32"/>
<connect gate="G$1" pin="26" pad="31"/>
<connect gate="G$1" pin="27" pad="30"/>
<connect gate="G$1" pin="28" pad="29"/>
<connect gate="G$1" pin="29" pad="28"/>
<connect gate="G$1" pin="3" pad="17"/>
<connect gate="G$1" pin="30" pad="27"/>
<connect gate="G$1" pin="31" pad="26"/>
<connect gate="G$1" pin="32" pad="25"/>
<connect gate="G$1" pin="33" pad="24"/>
<connect gate="G$1" pin="34" pad="23"/>
<connect gate="G$1" pin="35" pad="22"/>
<connect gate="G$1" pin="36" pad="21"/>
<connect gate="G$1" pin="37" pad="20"/>
<connect gate="G$1" pin="4" pad="16"/>
<connect gate="G$1" pin="5" pad="15"/>
<connect gate="G$1" pin="6" pad="14"/>
<connect gate="G$1" pin="7" pad="13"/>
<connect gate="G$1" pin="8" pad="12"/>
<connect gate="G$1" pin="9" pad="11"/>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="216612013/37pins_female"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_7490100110A" prefix="T" uservalue="yes">
<description>&lt;b&gt;LAN-Transformer WE-LAN 10/100 Base T&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3 standards&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/S/7490100110A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/S/7490100110A?&lt;/a&gt;&lt;p&gt;



2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7490100110A"/>
</gates>
<devices>
<device name="" package="7490100110A/749010012A">
<connects>
<connect gate="G$1" pin="CRD" pad="15"/>
<connect gate="G$1" pin="CRX" pad="2"/>
<connect gate="G$1" pin="CTD" pad="10"/>
<connect gate="G$1" pin="CTX" pad="7"/>
<connect gate="G$1" pin="RD+" pad="16"/>
<connect gate="G$1" pin="RD-" pad="14"/>
<connect gate="G$1" pin="RX+" pad="1"/>
<connect gate="G$1" pin="RX-" pad="3"/>
<connect gate="G$1" pin="TD+" pad="11"/>
<connect gate="G$1" pin="TD-" pad="9"/>
<connect gate="G$1" pin="TX+" pad="6"/>
<connect gate="G$1" pin="TX-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_749010012A" prefix="T" uservalue="yes">
<description>&lt;b&gt;LAN-Transformer WE-LAN 10/100 Base T&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3 standards&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/S/749010011?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/S/749010012A?&lt;/a&gt;&lt;p&gt;



2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="749010012A"/>
</gates>
<devices>
<device name="" package="7490100110A/749010012A">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CRX" pad="10"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="15"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="11"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_749013011A" prefix="T" uservalue="yes">
<description>&lt;b&gt;UtLAN
10/100 Base-T SMD Transformer 1 Port WE-LAN&lt;/b&gt;&lt;p&gt;

- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/S/749010011?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/S/749010011A?&lt;/a&gt;&lt;p&gt;



2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="749013011A"/>
</gates>
<devices>
<device name="" package="749013011A">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CRX" pad="10"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="15"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="11"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990111217" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	74990111217

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard HPLE

&lt;b&gt;Tab Position	Up

&lt;b&gt;LED (Left-Right)	yellow-green 

&lt;b&gt;EMI Fingers	YES



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45/74990111217?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45/74990111217&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Created by Yingchun Shan 2014-07-10&lt;br&gt;
&lt;/b&gt;2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="74990111217"/>
<gate name="GND" symbol="GNDPIN"/>
<gate name="YELLOW" symbol="LED-2PIN"/>
<gate name="GREEN" symbol="LED-2PIN"/>
</gates>
<devices>
<device name="" package="74990111217">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="RCT" pad="5"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="TCT" pad="4"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="GND" pin="GND" pad="Z1 Z2"/>
<connect gate="GREEN" pin="A" pad="11"/>
<connect gate="GREEN" pin="K" pad="12"/>
<connect gate="YELLOW" pin="A" pad="9"/>
<connect gate="YELLOW" pin="K" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498111001A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7498111001A

&lt;b&gt;Design		SMD

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP 

&lt;b&gt;LED (Left-Right)	NONE

&lt;b&gt;EMI Fingers	Yes

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7498111001?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Created  by  Yingchun Shan 2016-08-23&lt;br&gt;
&lt;/b&gt;2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498111001A"/>
<gate name="GND_SHIELD" symbol="GNDPIN"/>
</gates>
<devices>
<device name="" package="7498111001A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="GND_SHIELD" pin="GND" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499111001A" prefix="T" uservalue="yes">
<description>&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499111001A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T 

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	NONE

&lt;b&gt;EMI Fingers	Yes


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_RJ45_drei(2).jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499111000A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN_RJ45/7499111000A?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Created  by Yingchun Shan 2016-08-29&lt;br&gt;
&lt;/b&gt;2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499111001A"/>
<gate name="GND_SHILED" symbol="GND_PIN"/>
</gates>
<devices>
<device name="" package="7499111001A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="GND_SHILED" pin="1" pad="Z1 Z2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_STM_760871131" prefix="T" uservalue="yes">
<description>&lt;b&gt;MID-UNIT STM Offline Transformers for STMicroelectronics&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_STM?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_STM?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-UNIT_760871131">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="7 8"/>
<connect gate="G$1" pin="3" pad="11 12"/>
<connect gate="G$1" pin="4" pad="9 10"/>
<connect gate="G$1" pin="5" pad="13 14"/>
<connect gate="G$1" pin="6" pad="5"/>
<connect gate="G$1" pin="7" pad="6"/>
<connect gate="G$1" pin="8" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_STM_750314288" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit STM&lt;/b&gt;&lt;br&gt;&lt;br&gt;



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_STM?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_STM?&lt;/a&gt;&lt;p&gt;

Created  by  Yingchun 2016-09-21&lt;br&gt;
2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:2W_1"/>
</gates>
<devices>
<device name="" package="WE-UNIT_STM_750314288">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="9"/>
<connect gate="G$1" pin="5" pad="10"/>
<connect gate="G$1" pin="6" pad="7"/>
<connect gate="G$1" pin="7" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_PI_750811019" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit PI&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_PI?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_PI?&lt;/a&gt;&lt;p&gt;


Created  by  Yingchun 2016-09-22&lt;br&gt;
2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:1W-2"/>
</gates>
<devices>
<device name="" package="WE-UNIT_EE16/8/5_1">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_PI_7508110100" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit PI&lt;/b&gt;&lt;br&gt;&lt;br&gt;



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_PI?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_PI?&lt;/a&gt;&lt;p&gt;


Created  by  Yingchun 2016-09-22&lt;br&gt;
2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:1W-3"/>
</gates>
<devices>
<device name="" package="WE-UNIT_PI_75081101XX">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="7"/>
<connect gate="G$1" pin="6" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_PI_7508110101" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit PI&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_PI?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_PI?&lt;/a&gt;&lt;p&gt;


Created  by  Yingchun 2016-09-22&lt;br&gt;
2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_4W:1W"/>
</gates>
<devices>
<device name="" package="WE-UNIT_PI_75081101XX">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="1"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="5" pad="3"/>
<connect gate="G$1" pin="6" pad="7"/>
<connect gate="G$1" pin="7" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_PI_750310849" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit PI&lt;/b&gt;&lt;br&gt;&lt;br&gt;



&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_PI?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_PI?&lt;/a&gt;&lt;p&gt;


Created  by  Yingchun 2016-09-22&lt;br&gt;
2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_4W:1W_1"/>
</gates>
<devices>
<device name="" package="WE-UNIT_PI_NXP_EE20/10/6">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_NXP_760871038" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit NXP&lt;/b&gt;&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_NXP_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750871035?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_NXP/750871035?&lt;/a&gt;&lt;p&gt;


Created  by Yingchun 2016-09-221&lt;br&gt;
2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:1W"/>
</gates>
<devices>
<device name="" package="WE-UNIT_NXP_760871038">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMBHV" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-CMBHV&lt;BR&gt;
Common Mode Power Line Choke&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-CMBHV_XL-XXL.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-CMBHV_XL-XXL.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/de/pbs/WE-CMBHV"&gt;http://katalog.we-online.de/de/pbs/WE-CMBHV&lt;/a&gt;&lt;p&gt;


Created by Yingchun on 2016&lt;br&gt;

2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CMBHV"/>
</gates>
<devices>
<device name="_XL_744830007215" package="744830007215">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744830007215/0,7mH"/>
</technology>
</technologies>
</device>
<device name="_XL_744830010185" package="744830010185">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744830010185/1mH"/>
</technology>
</technologies>
</device>
<device name="_XL_744830017132" package="744830017132">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744830017132/1,7mH"/>
</technology>
</technologies>
</device>
<device name="_XL_744830039080" package="744830039080">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744830039080/3,9mH"/>
</technology>
</technologies>
</device>
<device name="_XXL_744831010205" package="744831010205">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744831010205/1mH"/>
</technology>
</technologies>
</device>
<device name="_XXL_744831016164" package="744831016164">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744831016164/1,6mH"/>
</technology>
</technologies>
</device>
<device name="_XXL_744831020133" package="744831020133">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744831020133/2mH"/>
</technology>
</technologies>
</device>
<device name="_XXL_744831034090" package="744831034090">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744831034090/3,4mH"/>
</technology>
</technologies>
</device>
<device name="_XXL_744831047068" package="744831047068">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744831047068/4,7mH"/>
</technology>
</technologies>
</device>
<device name="_XL_744830025103" package="744830025103">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="744830025103/2,5mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2SA_7850" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-PD2SA SMD Power Inductor&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD2SA.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD2SA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD2SA"&gt;http://katalog.we-online.de/en/pbs/WE-PD2SA&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2SA_7850">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784787012">
<attribute name="WE-NUMBER" value="784787012/1,2uH"/>
</technology>
<technology name="_784787027">
<attribute name="WE-NUMBER" value="784787027/2,7uH"/>
</technology>
<technology name="_784787039">
<attribute name="WE-NUMBER" value="784787039/3,9uH"/>
</technology>
<technology name="_784787047">
<attribute name="WE-NUMBER" value="784787047/4,7uH"/>
</technology>
<technology name="_784787068">
<attribute name="WE-NUMBER" value="784787068/6,8uH"/>
</technology>
<technology name="_784787082">
<attribute name="WE-NUMBER" value="784787082/8,2uH"/>
</technology>
<technology name="_784787100">
<attribute name="WE-NUMBER" value="784787100/10uH"/>
</technology>
<technology name="_784787101">
<attribute name="WE-NUMBER" value="784787101/100uH"/>
</technology>
<technology name="_784787120">
<attribute name="WE-NUMBER" value="784787120/12uH"/>
</technology>
<technology name="_784787121">
<attribute name="WE-NUMBER" value="784787121/120uH"/>
</technology>
<technology name="_784787150">
<attribute name="WE-NUMBER" value="784787150/15uH"/>
</technology>
<technology name="_784787151">
<attribute name="WE-NUMBER" value="784787151/150uH"/>
</technology>
<technology name="_784787180">
<attribute name="WE-NUMBER" value="784787180/18uH"/>
</technology>
<technology name="_784787181">
<attribute name="WE-NUMBER" value="784787181/180uH"/>
</technology>
<technology name="_784787220">
<attribute name="WE-NUMBER" value="784787220/22uH"/>
</technology>
<technology name="_784787221">
<attribute name="WE-NUMBER" value="784787221/220uH"/>
</technology>
<technology name="_784787330">
<attribute name="WE-NUMBER" value="784787330/33uH"/>
</technology>
<technology name="_784787470">
<attribute name="WE-NUMBER" value="784787470/47uH"/>
</technology>
<technology name="_784787680">
<attribute name="WE-NUMBER" value="784787680/68uH"/>
</technology>
<technology name="_784787820">
<attribute name="WE-NUMBER" value="784787820/82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-KIHC_0402" prefix="L" uservalue="yes">
<description>&lt;b&gt;Wire Wound Chip Ceramic Inductor WE-KIHC&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt; Inductance values ​​from 1 nH up to 51 nH
&lt;br&gt;High quality factor Q
&lt;br&gt;High self-resonant frequency
&lt;br&gt;High currents up to 2.3 A
&lt;br&gt;2% Inductance tolerance
&lt;br&gt;Operating temperature: -40 ° C to +125 ° C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt; 
&lt;br&gt;Especially for RF application
&lt;br&gt;Ideal for high current applications
&lt;br&gt;Wideband filter
&lt;br&gt;Decoupling
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-ki%20hc_keramik_smd_induktivitaet.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-ki%20hc_keramik_smd_induktivitaet.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-KIHC"&gt;http://katalog.we-online.de/en/pbs/WE-KIHC&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-KIHC_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744916010">
<attribute name="WE-NUMBER" value="744916010/1nH"/>
</technology>
<technology name="_744916020">
<attribute name="WE-NUMBER" value="744916020/2nH"/>
</technology>
<technology name="_744916022">
<attribute name="WE-NUMBER" value="744916022/2,2nH"/>
</technology>
<technology name="_744916027">
<attribute name="WE-NUMBER" value="744916027/2,7nH"/>
</technology>
<technology name="_744916033">
<attribute name="WE-NUMBER" value="744916033/3,3nH"/>
</technology>
<technology name="_744916036">
<attribute name="WE-NUMBER" value="744916036/3,6nH"/>
</technology>
<technology name="_744916039">
<attribute name="WE-NUMBER" value="744916039/3,9nH"/>
</technology>
<technology name="_744916043">
<attribute name="WE-NUMBER" value="744916043/4,3nH"/>
</technology>
<technology name="_744916047">
<attribute name="WE-NUMBER" value="744916047/4,7nH"/>
</technology>
<technology name="_744916051">
<attribute name="WE-NUMBER" value="7446051/5,1nH"/>
</technology>
<technology name="_744916056">
<attribute name="WE-NUMBER" value="744916056/5,6nH"/>
</technology>
<technology name="_744916062">
<attribute name="WE-NUMBER" value="744916062/6,2nH"/>
</technology>
<technology name="_744916068">
<attribute name="WE-NUMBER" value="744916068/6,8nH"/>
</technology>
<technology name="_744916082">
<attribute name="WE-NUMBER" value="744916082/8,2nH"/>
</technology>
<technology name="_744916087">
<attribute name="WE-NUMBER" value="744916082/8,7nH"/>
</technology>
<technology name="_744916090">
<attribute name="WE-NUMBER" value="744916090/9nH"/>
</technology>
<technology name="_744916095">
<attribute name="WE-NUMBER" value="744916095/9,5nH"/>
</technology>
<technology name="_744916110">
<attribute name="WE-NUMBER" value="744916110/10nH"/>
</technology>
<technology name="_744916111">
<attribute name="WE-NUMBER" value="744916111/11nH"/>
</technology>
<technology name="_744916112">
<attribute name="WE-NUMBER" value="744916112/12nH"/>
</technology>
<technology name="_744916113">
<attribute name="WE-NUMBER" value="744916113/13nH"/>
</technology>
<technology name="_744916115">
<attribute name="WE-NUMBER" value="744916115/15nH"/>
</technology>
<technology name="_744916116">
<attribute name="WE-NUMBER" value="744916116/16nH"/>
</technology>
<technology name="_744916118">
<attribute name="WE-NUMBER" value="744916118/18nH"/>
</technology>
<technology name="_744916119">
<attribute name="WE-NUMBER" value="744916119/19nH"/>
</technology>
<technology name="_744916121">
<attribute name="WE-NUMBER" value="744916121/21nH"/>
</technology>
<technology name="_744916122">
<attribute name="WE-NUMBER" value="744916122/22nH"/>
</technology>
<technology name="_744916123">
<attribute name="WE-NUMBER" value="744916123/23nH"/>
</technology>
<technology name="_744916124">
<attribute name="WE-NUMBER" value="744916124/24nH"/>
</technology>
<technology name="_744916125">
<attribute name="WE-NUMBER" value="744916125/25nH"/>
</technology>
<technology name="_744916126">
<attribute name="WE-NUMBER" value="744916126/26nH"/>
</technology>
<technology name="_744916127">
<attribute name="WE-NUMBER" value="744916127/27nH"/>
</technology>
<technology name="_744916130">
<attribute name="WE-NUMBER" value="744916130/30nH"/>
</technology>
<technology name="_744916133">
<attribute name="WE-NUMBER" value="744916133/33nH"/>
</technology>
<technology name="_744916136">
<attribute name="WE-NUMBER" value="744916136/36nH"/>
</technology>
<technology name="_744916137">
<attribute name="WE-NUMBER" value="744916137/37nH"/>
</technology>
<technology name="_744916139">
<attribute name="WE-NUMBER" value=""/>
</technology>
<technology name="_744916140">
<attribute name="WE-NUMBER" value="744916140/40nH"/>
</technology>
<technology name="_744916143">
<attribute name="WE-NUMBER" value="744916143/43nH"/>
</technology>
<technology name="_744916147">
<attribute name="WE-NUMBER" value="744916147/47nH"/>
</technology>
<technology name="_744916151">
<attribute name="WE-NUMBER" value="744916151/51nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPBHV" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-TPB HV Three-Phase Common Mode Power Line Choke&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TPBHV_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TPBHV_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPBHV"&gt;http://katalog.we-online.de/en/pbs/WE-TPBHV&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TPB"/>
</gates>
<devices>
<device name="_744835150072" package="WE-TPBHV_Φ1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744839208072" package="WE-TPBHV_Φ1.3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744835090095" package="WE-TPBHV_Φ1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744838480095" package="WE-TPBHV_Φ1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744839125095" package="WE-TPBHV_Φ1.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744835050135" package="WE-TPBHV_Φ2.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744835034160" package="WE-TPBHV_Φ2.4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744838180160" package="WE-TPBHV_Φ2.4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744839047160" package="WE-TPBHV_Φ2.4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744835021220" package="WE-TPBHV_Φ2.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744837018220" package="WE-TPBHV_Φ2.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744839029220" package="WE-TPBHV_Φ2.6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744837002460" package="WE-TPBHV_Φ5.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744838040400" package="WE-TPBHV_Φ4.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744839010400" package="WE-TPBHV_Φ4.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744839003460" package="WE-TPBHV_Φ4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744837010290" package="WE-TPBHV_Φ4.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_744837006400" package="WE-TPBHV_Φ4.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQSH_4020" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-LQSH SMD Semi-Shielded High Saturation Power Inductor&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LQSH_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LQSH_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQSH"&gt;http://katalog.we-online.de/en/pbs/WE-LQSH&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQSH_4020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744050420047">
<attribute name="WE-NUMBER" value="744050420047/0,47uH"/>
</technology>
<technology name="_74405042010">
<attribute name="WE-NUMBER" value="74405042010/1uH"/>
</technology>
<technology name="_74405042022">
<attribute name="WE-NUMBER" value="74405042022/2,2uH"/>
</technology>
<technology name="_74405042033">
<attribute name="WE-NUMBER" value="74405042033/3,3uH"/>
</technology>
<technology name="_74405042047">
<attribute name="WE-NUMBER" value="74405042047/4,7uH"/>
</technology>
<technology name="_74405042068">
<attribute name="WE-NUMBER" value="74405042068/6,8uH"/>
</technology>
<technology name="_74405042100">
<attribute name="WE-NUMBER" value="74405042100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQFS_4828" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-LQFS SMD Semishielded Tiny Power Inductor&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LQFS_3818-4828.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LQFS_3818-4828.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQFS"&gt;http://katalog.we-online.de/en/pbs/WE-LQFS&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQFS_48X8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74406043012">
<attribute name="WE-NUMBER" value="74406043012/1,2uH"/>
</technology>
<technology name="_74406043027">
<attribute name="WE-NUMBER" value="74406043027/2,7uH"/>
</technology>
<technology name="_74406043047">
<attribute name="WE-NUMBER" value="74406043047/4,7uH"/>
</technology>
<technology name="_74406043068">
<attribute name="WE-NUMBER" value="74406043068/6,8uH"/>
</technology>
<technology name="_74406043100">
<attribute name="WE-NUMBER" value="74406043100/10uH"/>
</technology>
<technology name="_74406043101">
<attribute name="WE-NUMBER" value="74406043101/100uH"/>
</technology>
<technology name="_74406043220">
<attribute name="WE-NUMBER" value="74406043220/22uH"/>
</technology>
<technology name="_74406043221">
<attribute name="WE-NUMBER" value="74406043221/220uH"/>
</technology>
<technology name="_74406043330">
<attribute name="WE-NUMBER" value="74406043330/33uH"/>
</technology>
<technology name="_74406043331">
<attribute name="WE-NUMBER" value="74406043331/330uH"/>
</technology>
<technology name="_74406043470">
<attribute name="WE-NUMBER" value="74406043470/47uH"/>
</technology>
<technology name="_74406043471">
<attribute name="WE-NUMBER" value="74406043471/470uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_749020022A" prefix="T" uservalue="yes">
<description>&lt;B&gt;WE-LAN LAN Transformer&lt;br&gt;&lt;/b&gt;

&lt;br&gt;&lt;B&gt;Characteristics&lt;/B&gt;
&lt;br&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt
SMD
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;Ethernet speed up to 10 Gbit/s
&lt;br&gt;Power over Ethernet PoE and PoE+
&lt;br&gt;Compliant with most IC’s for Ethernet applications such as Intel, AMD, Microchip and Realtek
&lt;br&gt;Hub, Router, Switches, IPcameras, IoT
&lt;br&gt;
&lt;br&gt;

&lt;/b&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;&lt;br&gt;            
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/749020022A?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/749020022A?&lt;/a&gt;&lt;p&gt;
&lt;b&gt;&lt;br&gt;
&lt;br&gt;
2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="749020022A"/>
</gates>
<devices>
<device name="" package="749020022A">
<connects>
<connect gate="G$1" pin="MCT1" pad="49"/>
<connect gate="G$1" pin="MCT2" pad="46"/>
<connect gate="G$1" pin="MCT3" pad="43"/>
<connect gate="G$1" pin="MCT4" pad="40"/>
<connect gate="G$1" pin="MCT5" pad="36"/>
<connect gate="G$1" pin="MCT6" pad="33"/>
<connect gate="G$1" pin="MCT7" pad="30"/>
<connect gate="G$1" pin="MCT8" pad="27"/>
<connect gate="G$1" pin="MX1+" pad="50"/>
<connect gate="G$1" pin="MX1-" pad="48"/>
<connect gate="G$1" pin="MX2+" pad="47"/>
<connect gate="G$1" pin="MX2-" pad="45"/>
<connect gate="G$1" pin="MX3+" pad="44"/>
<connect gate="G$1" pin="MX3-" pad="42"/>
<connect gate="G$1" pin="MX4+" pad="41"/>
<connect gate="G$1" pin="MX4-" pad="39"/>
<connect gate="G$1" pin="MX5+" pad="37"/>
<connect gate="G$1" pin="MX5-" pad="35"/>
<connect gate="G$1" pin="MX6+" pad="34"/>
<connect gate="G$1" pin="MX6-" pad="32"/>
<connect gate="G$1" pin="MX7+" pad="31"/>
<connect gate="G$1" pin="MX7-" pad="29"/>
<connect gate="G$1" pin="MX8+" pad="28"/>
<connect gate="G$1" pin="MX8-" pad="26"/>
<connect gate="G$1" pin="TCT1" pad="2"/>
<connect gate="G$1" pin="TCT2" pad="5"/>
<connect gate="G$1" pin="TCT3" pad="8"/>
<connect gate="G$1" pin="TCT4" pad="11"/>
<connect gate="G$1" pin="TCT5" pad="15"/>
<connect gate="G$1" pin="TCT6" pad="18"/>
<connect gate="G$1" pin="TCT7" pad="21"/>
<connect gate="G$1" pin="TCT8" pad="24"/>
<connect gate="G$1" pin="TD1+" pad="1"/>
<connect gate="G$1" pin="TD1-" pad="3"/>
<connect gate="G$1" pin="TD2+" pad="4"/>
<connect gate="G$1" pin="TD2-" pad="6"/>
<connect gate="G$1" pin="TD3+" pad="7"/>
<connect gate="G$1" pin="TD3-" pad="9"/>
<connect gate="G$1" pin="TD4+" pad="10"/>
<connect gate="G$1" pin="TD4-" pad="12"/>
<connect gate="G$1" pin="TD5+" pad="14"/>
<connect gate="G$1" pin="TD5-" pad="16"/>
<connect gate="G$1" pin="TD6+" pad="17"/>
<connect gate="G$1" pin="TD6-" pad="19"/>
<connect gate="G$1" pin="TD7+" pad="20"/>
<connect gate="G$1" pin="TD7-" pad="22"/>
<connect gate="G$1" pin="TD8+" pad="23"/>
<connect gate="G$1" pin="TD8-" pad="25"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_7490140110" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Characteristics &lt;/B&gt;
&lt;br&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt
SMD
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;Ethernet speed up to 10 Gbit/s
&lt;br&gt;Power over Ethernet PoE and PoE+
&lt;br&gt;Compliant with most IC’s for Ethernet applications such as Intel, AMD, Microchip and Realtek
&lt;br&gt;Hub, Router, Switches, IPcameras, IoT
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/7490140110?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/7490140110?&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7490140110"/>
</gates>
<devices>
<device name="" package="7490140110">
<connects>
<connect gate="G$1" pin="CRD" pad="2"/>
<connect gate="G$1" pin="CRX" pad="15"/>
<connect gate="G$1" pin="CTD" pad="7"/>
<connect gate="G$1" pin="CTX" pad="10"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="3"/>
<connect gate="G$1" pin="RX+" pad="16"/>
<connect gate="G$1" pin="RX-" pad="14"/>
<connect gate="G$1" pin="TD+" pad="6"/>
<connect gate="G$1" pin="TD-" pad="8"/>
<connect gate="G$1" pin="TX+" pad="11"/>
<connect gate="G$1" pin="TX-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_749020100A" prefix="T" uservalue="yes">
<description>&lt;B&gt;WE-LAN LAN Transformer&lt;br&gt;&lt;/b&gt;

&lt;br&gt;&lt;B&gt;Characteristics&lt;/B&gt;
&lt;br&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt
SMD
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;Ethernet speed up to 10 Gbit/s
&lt;br&gt;Power over Ethernet PoE and PoE+
&lt;br&gt;Compliant with most IC’s for Ethernet applications such as Intel, AMD, Microchip and Realtek
&lt;br&gt;Hub, Router, Switches, IPcameras, IoT
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN"&gt;http://katalog.we-online.de/en/pbs/WE-LAN&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="749020100A"/>
</gates>
<devices>
<device name="" package="749020100A">
<connects>
<connect gate="G$1" pin="CT" pad="3"/>
<connect gate="G$1" pin="CT1" pad="6"/>
<connect gate="G$1" pin="CT2" pad="11"/>
<connect gate="G$1" pin="CT3" pad="14"/>
<connect gate="G$1" pin="RD+" pad="7"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="10"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7497011611A" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-RJ45 LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	749701611A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	Yellow-Green-ORANGE

&lt;b&gt;EMI Fingers	No
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7497011611A"/>
<gate name="YELLOW" symbol="LED_2PIN"/>
<gate name="GREEN-ORANGE" symbol="LED_DOUB"/>
<gate name="G$2" symbol="USB2.0-1"/>
<gate name="GND" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="7497011611A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$2" pin="D+" pad="U3"/>
<connect gate="G$2" pin="D-" pad="U2"/>
<connect gate="G$2" pin="GND" pad="U4"/>
<connect gate="G$2" pin="VUSB" pad="U1"/>
<connect gate="GND" pin="SHIELD" pad="Z1 Z2 Z3 Z4 Z5 Z6"/>
<connect gate="GREEN-ORANGE" pin="AK1" pad="15"/>
<connect gate="GREEN-ORANGE" pin="AK2" pad="16"/>
<connect gate="YELLOW" pin="A" pad="14"/>
<connect gate="YELLOW" pin="K" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498210002" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-RJ45 LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7498210002

&lt;b&gt;Design		SMD

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	DOWN

&lt;b&gt;LED (Left-Right)	NO

&lt;b&gt;EMI Fingers	No
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498210002"/>
<gate name="GND" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="7498210002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="VC1+" pad="9"/>
<connect gate="G$1" pin="VC1-" pad="10"/>
<connect gate="GND" pin="SHIELD" pad="SHELL SHELL1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498210003" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-RJ45 LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7498210003

&lt;b&gt;Design		SMD

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	NO

&lt;b&gt;EMI Fingers	No
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498210003"/>
<gate name="GND" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="7498210003">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="P6" pad="P6"/>
<connect gate="G$1" pin="VC1+" pad="P10"/>
<connect gate="G$1" pin="VC1-" pad="P9"/>
<connect gate="G$1" pin="VC2+" pad="P11"/>
<connect gate="G$1" pin="VC2-" pad="P12"/>
<connect gate="GND" pin="SHIELD" pad="SHELL SHELL1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7498210220A" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-RJ45 LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7498210220A

&lt;b&gt;Design		SMD

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	Vertical

&lt;b&gt;LED (Left-Right)	GREEN-GREEN

&lt;b&gt;EMI Fingers	No
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7498210220A"/>
<gate name="GREEN" symbol="LED_2PIN"/>
<gate name="GREEN1" symbol="LED_2PIN"/>
<gate name="G$2" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="7498210220A">
<connects>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="P6" pad="P6"/>
<connect gate="G$1" pin="P7" pad="P7"/>
<connect gate="G$1" pin="V+" pad="P9"/>
<connect gate="G$1" pin="V-" pad="P11"/>
<connect gate="G$1" pin="V1+" pad="P10"/>
<connect gate="G$1" pin="V1-" pad="P12"/>
<connect gate="G$2" pin="SHIELD" pad="SHELL SHELL1"/>
<connect gate="GREEN" pin="A" pad="P1"/>
<connect gate="GREEN" pin="K" pad="P2"/>
<connect gate="GREEN1" pin="A" pad="P13"/>
<connect gate="GREEN1" pin="K" pad="P14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499010003A" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-RJ45 LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499010003A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	NO

&lt;b&gt;EMI Fingers	No
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499010003A"/>
<gate name="GND" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="7499010003A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="RCT" pad="5"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="TCT" pad="2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="GND" pin="SHIELD" pad="SHELL SHELL1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990101212" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-RJ45 LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	74990101212

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP

&lt;b&gt;LED (Left-Right)	GREEN-YELLOW

&lt;b&gt;EMI Fingers	No
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="74990101212"/>
<gate name="GREEN" symbol="LED_2PIN"/>
<gate name="YELLOW" symbol="LED_2PIN"/>
<gate name="G$2" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="74990101212">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="RCT" pad="5"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="TCT" pad="2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$2" pin="SHIELD" pad="SHELL SHELL1"/>
<connect gate="GREEN" pin="A" pad="10"/>
<connect gate="GREEN" pin="K" pad="9"/>
<connect gate="YELLOW" pin="A" pad="12"/>
<connect gate="YELLOW" pin="K" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_74990101241" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-RJ45 LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	74990101241

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	Vertical 

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	No
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="74990101241"/>
<gate name="YELLOW" symbol="LED_2PIN"/>
<gate name="GREEN" symbol="LED_2PIN"/>
<gate name="G$2" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="74990101241">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="RCT" pad="5"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="TCT" pad="2"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$2" pin="SHIELD" pad="SHELL SHELL1"/>
<connect gate="GREEN" pin="A" pad="11"/>
<connect gate="GREEN" pin="K" pad="12"/>
<connect gate="YELLOW" pin="A" pad="9"/>
<connect gate="YELLOW" pin="K" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499010126A" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-RJ45 LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499010126A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	Vertical 

&lt;b&gt;LED (Left-Right)    Yellow-Green	

&lt;b&gt;EMI Fingers	No
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499010126A"/>
<gate name="YELLOW" symbol="LED_2PIN"/>
<gate name="GREEN" symbol="LED_2PIN"/>
<gate name="GND" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="7499010126A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="RCT" pad="5"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="TCT" pad="4"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="GND" pin="SHIELD" pad="SHELL SHELL1"/>
<connect gate="GREEN" pin="A" pad="11"/>
<connect gate="GREEN" pin="K" pad="12"/>
<connect gate="YELLOW" pin="A" pad="9"/>
<connect gate="YELLOW" pin="K" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499011441A" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-RJ45 LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499011441A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP
&lt;b&gt;LED (Left-Right)	Yellow_Green-Yellow_Green

&lt;b&gt;EMI Fingers	No
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499011441A"/>
<gate name="GREEN-YELLOW" symbol="LED_DOUB"/>
<gate name="GREEN1-YELLOW1" symbol="LED_DOUB"/>
<gate name="GND" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="7499011441A">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="RCT" pad="5"/>
<connect gate="G$1" pin="RD+" pad="3"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="TCT" pad="4"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
<connect gate="GND" pin="SHIELD" pad="SHELL SHELL1"/>
<connect gate="GREEN-YELLOW" pin="AK1" pad="9"/>
<connect gate="GREEN-YELLOW" pin="AK2" pad="10"/>
<connect gate="GREEN1-YELLOW1" pin="AK1" pad="11"/>
<connect gate="GREEN1-YELLOW1" pin="AK2" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499021002A" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-RJ45 LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499021002A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x2

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	DOWN

&lt;b&gt;LED (Left-Right)	NO

&lt;b&gt;EMI Fingers	No
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="A" symbol="7499021002A"/>
<gate name="B" symbol="7499021002A"/>
<gate name="GND" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="7499021002A">
<connects>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="RCT" pad="A5"/>
<connect gate="A" pin="RD+" pad="A4"/>
<connect gate="A" pin="RD-" pad="A6"/>
<connect gate="A" pin="TCT" pad="A2"/>
<connect gate="A" pin="TD+" pad="A1"/>
<connect gate="A" pin="TD-" pad="A3"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="RCT" pad="B5"/>
<connect gate="B" pin="RD+" pad="B4"/>
<connect gate="B" pin="RD-" pad="B6"/>
<connect gate="B" pin="TCT" pad="B2"/>
<connect gate="B" pin="TD+" pad="B1"/>
<connect gate="B" pin="TD-" pad="B3"/>
<connect gate="GND" pin="SHIELD" pad="SHELL SHELL1 SHELL2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499031001A" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-RJ45 LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;

&lt;br&gt;
&lt;br&gt;&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499031001A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x4

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	DOWN

&lt;b&gt;LED (Left-Right)	NO

&lt;b&gt;EMI Fingers	No
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="A" symbol="7499021002A"/>
<gate name="B" symbol="7499021002A"/>
<gate name="C" symbol="7499021002A"/>
<gate name="D" symbol="7499021002A"/>
<gate name="GND" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="7499031001A">
<connects>
<connect gate="A" pin="8" pad="A8"/>
<connect gate="A" pin="RCT" pad="A5"/>
<connect gate="A" pin="RD+" pad="A4"/>
<connect gate="A" pin="RD-" pad="A6"/>
<connect gate="A" pin="TCT" pad="A2"/>
<connect gate="A" pin="TD+" pad="A1"/>
<connect gate="A" pin="TD-" pad="A3"/>
<connect gate="B" pin="8" pad="B8"/>
<connect gate="B" pin="RCT" pad="B5"/>
<connect gate="B" pin="RD+" pad="B4"/>
<connect gate="B" pin="RD-" pad="B6"/>
<connect gate="B" pin="TCT" pad="B2"/>
<connect gate="B" pin="TD+" pad="B1"/>
<connect gate="B" pin="TD-" pad="B3"/>
<connect gate="C" pin="8" pad="C8"/>
<connect gate="C" pin="RCT" pad="C5"/>
<connect gate="C" pin="RD+" pad="C4"/>
<connect gate="C" pin="RD-" pad="C6"/>
<connect gate="C" pin="TCT" pad="C2"/>
<connect gate="C" pin="TD+" pad="C1"/>
<connect gate="C" pin="TD-" pad="C3"/>
<connect gate="D" pin="8" pad="D8"/>
<connect gate="D" pin="RCT" pad="D5"/>
<connect gate="D" pin="RD+" pad="D4"/>
<connect gate="D" pin="RD-" pad="D6"/>
<connect gate="D" pin="TCT" pad="D2"/>
<connect gate="D" pin="TD+" pad="D1"/>
<connect gate="D" pin="TD-" pad="D3"/>
<connect gate="GND" pin="SHIELD" pad="SHELL SHELL1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499110120A" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-RJ45 LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;

&lt;br&gt;
&lt;br&gt;&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499110120A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	Vertical 

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	No
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499110120A"/>
<gate name="YELLOW" symbol="LED_2PIN"/>
<gate name="GREEN" symbol="LED_2PIN"/>
<gate name="G$4" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="7499110120A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$4" pin="SHIELD" pad="SHELL SHELL1"/>
<connect gate="GREEN" pin="A" pad="13"/>
<connect gate="GREEN" pin="K" pad="14"/>
<connect gate="YELLOW" pin="A" pad="11"/>
<connect gate="YELLOW" pin="K" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499410213" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-RJ45 LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;



&lt;br&gt;
&lt;br&gt;&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499410213

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	DOWN

&lt;b&gt;LED (Left-Right)	YELLOW-GREEN

&lt;b&gt;EMI Fingers	No
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499410213"/>
<gate name="GREEN" symbol="LED_2PIN"/>
<gate name="YELLOW" symbol="LED_2PIN"/>
<gate name="G$2" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="7499410213">
<connects>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="5"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="VC1+" pad="7"/>
<connect gate="G$1" pin="VC1-" pad="8"/>
<connect gate="G$1" pin="VC2+" pad="9"/>
<connect gate="G$1" pin="VC2-" pad="10"/>
<connect gate="G$2" pin="SHIELD" pad="SHELL SHELL1"/>
<connect gate="GREEN" pin="A" pad="11"/>
<connect gate="GREEN" pin="K" pad="12"/>
<connect gate="YELLOW" pin="A" pad="13"/>
<connect gate="YELLOW" pin="K" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499410221" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-RJ45 LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;




&lt;br&gt;
&lt;br&gt;&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499410221

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	Vertical 

&lt;b&gt;LED (Left-Right)	GREEN-GREEN

&lt;b&gt;EMI Fingers	No
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499410221"/>
<gate name="GREEN" symbol="LED_2PIN"/>
<gate name="GREEN1" symbol="LED_2PIN"/>
</gates>
<devices>
<device name="" package="7499410221">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P10" pad="10"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
<connect gate="G$1" pin="P5" pad="5"/>
<connect gate="G$1" pin="P7" pad="7"/>
<connect gate="G$1" pin="P8" pad="8"/>
<connect gate="G$1" pin="P9" pad="9"/>
<connect gate="G$1" pin="SHIELD" pad="SHELL SHELL1"/>
<connect gate="GREEN" pin="A" pad="12"/>
<connect gate="GREEN" pin="K" pad="11"/>
<connect gate="GREEN1" pin="A" pad="14"/>
<connect gate="GREEN1" pin="K" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RJ45_7499511002A" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-RJ45 LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;

&lt;br&gt;&lt;pre&gt;&lt;big&gt;
&lt;b&gt;Order Code	7499511002A

&lt;b&gt;Design		THT

&lt;b&gt;xBase-T		10/100/1000 Base-T

&lt;b&gt;Ports		1x1

&lt;b&gt;Application	Standard

&lt;b&gt;Tab Position	UP/DOWN

&lt;b&gt;LED (Left-Right)	No

&lt;b&gt;EMI Fingers	No
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RJ45-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-RJ45"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-RJ45&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7499511002A"/>
<gate name="G$2" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="7499511002A">
<connects>
<connect gate="G$1" pin="P1" pad="1"/>
<connect gate="G$1" pin="P10" pad="10"/>
<connect gate="G$1" pin="P11" pad="11"/>
<connect gate="G$1" pin="P12" pad="12"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P4" pad="4"/>
<connect gate="G$1" pin="P5" pad="5"/>
<connect gate="G$1" pin="P6" pad="6"/>
<connect gate="G$1" pin="P7" pad="7"/>
<connect gate="G$1" pin="P8" pad="8"/>
<connect gate="G$1" pin="P9" pad="9"/>
<connect gate="G$1" pin="VC1" pad="13"/>
<connect gate="G$1" pin="VC2" pad="14"/>
<connect gate="G$1" pin="VC3" pad="15"/>
<connect gate="G$1" pin="VC4" pad="16"/>
<connect gate="G$2" pin="SHIELD" pad="SHELL SHELL1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_749022012X" prefix="T" uservalue="yes">
<description>&lt;B&gt;WE-LAN LAN Transformer&lt;br&gt;&lt;/b&gt;

&lt;br&gt;&lt;B&gt;Characteristics&lt;/B&gt;
&lt;br&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt
SMD
&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications&lt;/B&gt;
&lt;br&gt;Ethernet speed up to 10 Gbit/s
&lt;br&gt;Power over Ethernet PoE and PoE+
&lt;br&gt;Compliant with most IC’s for Ethernet applications such as Intel, AMD, Microchip and Realtek
&lt;br&gt;Hub, Router, Switches, IPcameras, IoT
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN"&gt;http://katalog.we-online.de/en/pbs/WE-LAN&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="749022012X-2"/>
</gates>
<devices>
<device name="" package="749022012X">
<connects>
<connect gate="G$1" pin="MCT1" pad="24"/>
<connect gate="G$1" pin="MCT2" pad="21"/>
<connect gate="G$1" pin="MCT3" pad="18"/>
<connect gate="G$1" pin="MCT4" pad="15"/>
<connect gate="G$1" pin="MX1+" pad="23"/>
<connect gate="G$1" pin="MX1-" pad="22"/>
<connect gate="G$1" pin="MX2+" pad="20"/>
<connect gate="G$1" pin="MX2-" pad="19"/>
<connect gate="G$1" pin="MX3+" pad="17"/>
<connect gate="G$1" pin="MX3-" pad="16"/>
<connect gate="G$1" pin="MX4+" pad="14"/>
<connect gate="G$1" pin="MX4-" pad="13"/>
<connect gate="G$1" pin="TCT1" pad="1"/>
<connect gate="G$1" pin="TCT2" pad="4"/>
<connect gate="G$1" pin="TCT3" pad="7"/>
<connect gate="G$1" pin="TCT4" pad="10"/>
<connect gate="G$1" pin="TD1+" pad="2"/>
<connect gate="G$1" pin="TD1-" pad="3"/>
<connect gate="G$1" pin="TD2+" pad="5"/>
<connect gate="G$1" pin="TD2-" pad="6"/>
<connect gate="G$1" pin="TD3+" pad="8"/>
<connect gate="G$1" pin="TD3-" pad="9"/>
<connect gate="G$1" pin="TD4+" pad="11"/>
<connect gate="G$1" pin="TD4-" pad="12"/>
</connects>
<technologies>
<technology name="_7490220120"/>
<technology name="_7490220121"/>
<technology name="_7490220122"/>
<technology name="_7490220123"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_7490220115" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN LAN Transformer&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;Compliant with standards: IEEE 802.3u, IEEE 802.3ab, IEEE 802.3af, IEEE 802.3at and upcoming IEE 802.3bt
SMD

&lt;br&gt;&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;Ethernet speed up to 10 Gbit/s
&lt;br&gt;Power over Ethernet PoE and PoE+
&lt;br&gt;Compliant with most IC’s for Ethernet applications such as Intel, AMD, Microchip and Realtek
&lt;br&gt;Hub, Router, Switches, IPcameras, IoT
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/7490220115?"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/7490220115?&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7490220115"/>
</gates>
<devices>
<device name="" package="7490220115">
<connects>
<connect gate="G$1" pin="D1+" pad="2"/>
<connect gate="G$1" pin="D1-" pad="3"/>
<connect gate="G$1" pin="D2+" pad="5"/>
<connect gate="G$1" pin="D2-" pad="6"/>
<connect gate="G$1" pin="D3+" pad="8"/>
<connect gate="G$1" pin="D3-" pad="9"/>
<connect gate="G$1" pin="D4+" pad="11"/>
<connect gate="G$1" pin="D4-" pad="12"/>
<connect gate="G$1" pin="TD1" pad="1"/>
<connect gate="G$1" pin="TD2" pad="4"/>
<connect gate="G$1" pin="TD3" pad="7"/>
<connect gate="G$1" pin="TD4" pad="10"/>
<connect gate="G$1" pin="TX1" pad="24"/>
<connect gate="G$1" pin="TX2" pad="21"/>
<connect gate="G$1" pin="TX3" pad="18"/>
<connect gate="G$1" pin="TX4" pad="15"/>
<connect gate="G$1" pin="X1+" pad="23"/>
<connect gate="G$1" pin="X1-" pad="22"/>
<connect gate="G$1" pin="X2+" pad="20"/>
<connect gate="G$1" pin="X2-" pad="19"/>
<connect gate="G$1" pin="X3+" pad="17"/>
<connect gate="G$1" pin="X3-" pad="16"/>
<connect gate="G$1" pin="X4+" pad="14"/>
<connect gate="G$1" pin="X4-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN-10G_749052051" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN 10G Transformer 10Gbit Base-T&lt;/b&gt;&lt;p&gt;
- Compliant with standards: IEEE 802.3an and upcoming IEEE 802.3bt&lt;br&gt;
- SMD&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Ethernet speed up to 10Gbit/s&lt;br&gt;
--Power over Ethernet PoE and PoE+&lt;br&gt;
--10Gbit with ETR and PoE up to 150 W (for industrial applications)&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN10GBit" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN-10G"&gt;http://katalog.we-online.de/en/pbs/WE-LAN-10G&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Created By Yingchun,Shan
(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LAN10G:1.27&amp;0.99"/>
</gates>
<devices>
<device name="" package="WE-LAN10G1.27MM">
<connects>
<connect gate="G$1" pin="MCT1" pad="24"/>
<connect gate="G$1" pin="MCT2" pad="21"/>
<connect gate="G$1" pin="MCT3" pad="18"/>
<connect gate="G$1" pin="MCT4" pad="15"/>
<connect gate="G$1" pin="MX1+" pad="23"/>
<connect gate="G$1" pin="MX1-" pad="22"/>
<connect gate="G$1" pin="MX2+" pad="20"/>
<connect gate="G$1" pin="MX2-" pad="19"/>
<connect gate="G$1" pin="MX3+" pad="17"/>
<connect gate="G$1" pin="MX3-" pad="16"/>
<connect gate="G$1" pin="MX4+" pad="14"/>
<connect gate="G$1" pin="MX4-" pad="13"/>
<connect gate="G$1" pin="TCT1" pad="1"/>
<connect gate="G$1" pin="TCT2" pad="4"/>
<connect gate="G$1" pin="TCT3" pad="7"/>
<connect gate="G$1" pin="TCT4" pad="10"/>
<connect gate="G$1" pin="TD1+" pad="2"/>
<connect gate="G$1" pin="TD1-" pad="3"/>
<connect gate="G$1" pin="TD2+" pad="5"/>
<connect gate="G$1" pin="TD2-" pad="6"/>
<connect gate="G$1" pin="TD3+" pad="8"/>
<connect gate="G$1" pin="TD3-" pad="9"/>
<connect gate="G$1" pin="TD4+" pad="11"/>
<connect gate="G$1" pin="TD4-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-WPCC_2W(RX)" prefix="L" uservalue="yes">
<description>&lt;b&gt;Wireless Power Charging Coil&lt;/b&gt;&lt;br&gt;
-Qi standard compliant&lt;br&gt;
-Thinnest on the market&lt;br&gt;
-Easiness of assembly&lt;br&gt;
-Evaluated and approved by very major semiconductor manufacturer&lt;br&gt;
-Litz wire-highest Q-value on the market&lt;br&gt;
-Applicable for up to 5W&lt;br&gt;
-High permeability shielding&lt;br&gt;
-Cancels charging flux to be not coupled into sensitive components or batteries&lt;br&gt;
-High reliable construction&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
-- Portable devices used in a clean area .where connectors pose a risk of polluting e.g. medical facilities,(industrial )clean rooms,mining industry&lt;br&gt;
--Devices with a large number of mating cycles to avoid connector damage:eg.Smart watches,fittness tracker...&lt;br&gt;
--Consumer products:eg. Digital cameras,baby phone,walkie talky remote control,smartphone sleeves,watertight products&lt;br&gt;
--Explosion sensitive area where the use of a physical connection is hazardous&lt;br&gt;
--Smart sensors&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtWPCC_Receiver_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_UtWPCC_Receiver_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-WPCC_Receiver"&gt;http://katalog.we-online.de/en/pbs/WE-WPCC_Receiver&lt;/a&gt;&lt;p&gt;


Created by  Yingchun,Shan&lt;br&gt;

2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-WPCC_2W"/>
</gates>
<devices>
<device name="_760308103307" package="WE-WPCC_4027">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308102306" package="WE-WPCC_4444">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_760308103305" package="WE-WPCC_4544">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LPCC" prefix="L" uservalue="yes">
<description>&lt;b&gt;&lt;br&gt;WE-LPCC Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Stable leakage inductance for differential mode filtering
&lt;br&gt;High current capabilities
&lt;br&gt;Low profile
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; AC/DC converter
&lt;br&gt;High frequency DC/DC converter
&lt;br&gt;Mains LED Drivers
&lt;br&gt;Switch Mode Power Supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LPCC_7448680xxx_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LPCC_7448680xxx_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LPCC/"&gt;http://katalog.we-online.de/en/pbs/WE-LPCC/&lt;/a&gt;&lt;p&gt;
Created  by  Yingchun,Shan 2017-05-11&lt;br&gt;
2017(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LPCC"/>
</gates>
<devices>
<device name="_7448680100" package="WE-LPCC_7448680100">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7448680120" package="WE-LPCC_7448680120">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7448680140" package="WE-LPCC_7448680140">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7448680180" package="WE-LPCC_7448680180">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_7448680200" package="WE-LPCC_7448680200">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_6030" prefix="L" uservalue="yes">
<description>&lt;B&gt;WE-XHMI Xtreme High Current Molded Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;br&gt;&lt;/b&gt;

Flat wire coil for low copper losses&lt;br&gt;
Composite core material allows high saturation currents&lt;br&gt;
Compact design&lt;br&gt;
Magnetically shielded&lt;br&gt;
High current capability and handles high transient current spikes&lt;br&gt;
Low leakage flux noise&lt;br&gt;
Operating temperature: -40°C up to +125°C&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;

DC/DC-converter for high current power supplies&lt;br&gt;
DC/DC-converter for Field Programmable Gate Array (FPGA)&lt;br&gt;
Power supplies for mobile devices&lt;br&gt;
POL-converters&lt;br&gt;
Mainboards/ graphic cards&lt;br&gt;
Battery powered devices&lt;br&gt;
Wireless communication devices&lt;br&gt;
Filter&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndXHMI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndXHMI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-XHMI"&gt;http://katalog.we-online.de/en/pbs/WE-XHMI&lt;/a&gt;&lt;p&gt;
Created 2015-08-05&lt;br&gt;
2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-XHMI_7443934XXXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744393440018">
<attribute name="WE-NUMBER" value="744393440018/0,18uH"/>
</technology>
<technology name="_744393440033">
<attribute name="WE-NUMBER" value="744393440033/0,33uH"/>
</technology>
<technology name="_744393440056">
<attribute name="WE-NUMBER" value="744393440056/0,56uH"/>
</technology>
<technology name="_74439344010">
<attribute name="WE-NUMBER" value="74439344010/1uH"/>
</technology>
<technology name="_74439344012">
<attribute name="WE-NUMBER" value="74439344012/1,2uH"/>
</technology>
<technology name="_74439344022">
<attribute name="WE-NUMBER" value="74439344022/2,2uH"/>
</technology>
<technology name="_74439344033">
<attribute name="WE-NUMBER" value="74439344033/3,3uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_6060" prefix="L" uservalue="yes">
<description>&lt;B&gt;WE-XHMI Xtreme High Current Molded Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;br&gt;&lt;/b&gt;

Flat wire coil for low copper losses&lt;br&gt;
Composite core material allows high saturation currents&lt;br&gt;
Compact design&lt;br&gt;
Magnetically shielded&lt;br&gt;
High current capability and handles high transient current spikes&lt;br&gt;
Low leakage flux noise&lt;br&gt;
Operating temperature: -40°C up to +125°C&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;

DC/DC-converter for high current power supplies&lt;br&gt;
DC/DC-converter for Field Programmable Gate Array (FPGA)&lt;br&gt;
Power supplies for mobile devices&lt;br&gt;
POL-converters&lt;br&gt;
Mainboards/ graphic cards&lt;br&gt;
Battery powered devices&lt;br&gt;
Wireless communication devices&lt;br&gt;
Filter&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndXHMI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndXHMI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-XHMI"&gt;http://katalog.we-online.de/en/pbs/WE-XHMI&lt;/a&gt;&lt;p&gt;
Created 2015-08-05&lt;br&gt;
2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-XHMI_7443934XXXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439346047">
<attribute name="WE-NUMBER" value="74439346047/4,7uH"/>
</technology>
<technology name="_74439346056">
<attribute name="WE-NUMBER" value="74439346056/5,6uH"/>
</technology>
<technology name="_74439346068">
<attribute name="WE-NUMBER" value="74439346068/6,8uH"/>
</technology>
<technology name="_74439346082">
<attribute name="WE-NUMBER" value="74439346082/8,2uH"/>
</technology>
<technology name="_74439346100">
<attribute name="WE-NUMBER" value="74439346100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_8080" prefix="L" uservalue="yes">
<description>&lt;B&gt;WE-XHMI Xtreme High Current Molded Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;br&gt;&lt;/b&gt;

Flat wire coil for low copper losses&lt;br&gt;
Composite core material allows high saturation currents&lt;br&gt;
Compact design&lt;br&gt;
Magnetically shielded&lt;br&gt;
High current capability and handles high transient current spikes&lt;br&gt;
Low leakage flux noise&lt;br&gt;
Operating temperature: -40°C up to +125°C&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;

DC/DC-converter for high current power supplies&lt;br&gt;
DC/DC-converter for Field Programmable Gate Array (FPGA)&lt;br&gt;
Power supplies for mobile devices&lt;br&gt;
POL-converters&lt;br&gt;
Mainboards/ graphic cards&lt;br&gt;
Battery powered devices&lt;br&gt;
Wireless communication devices&lt;br&gt;
Filter&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndXHMI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndXHMI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-XHMI"&gt;http://katalog.we-online.de/en/pbs/WE-XHMI&lt;/a&gt;&lt;p&gt;
Created 2015-08-05&lt;br&gt;
2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-XHMI_74439358XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439358010">
<attribute name="WE-NUMBER" value="74439358010/1uH"/>
</technology>
<technology name="_74439358022">
<attribute name="WE-NUMBER" value="74439358022/2,2uH"/>
</technology>
<technology name="_74439358047">
<attribute name="WE-NUMBER" value="74439358047/4,7uH"/>
</technology>
<technology name="_74439358068">
<attribute name="WE-NUMBER" value="74439358068/6,2uH"/>
</technology>
<technology name="_74439358100">
<attribute name="WE-NUMBER" value="74439358100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-XHMI_1090" prefix="L" uservalue="yes">
<description>&lt;B&gt;WE-XHMI Xtreme High Current Molded Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
&lt;b&gt;Characteristicscs&lt;br&gt;&lt;/b&gt;

Flat wire coil for low copper losses&lt;br&gt;
Composite core material allows high saturation currents&lt;br&gt;
Compact design&lt;br&gt;
Magnetically shielded&lt;br&gt;
High current capability and handles high transient current spikes&lt;br&gt;
Low leakage flux noise&lt;br&gt;
Operating temperature: -40°C up to +125°C&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;

DC/DC-converter for high current power supplies&lt;br&gt;
DC/DC-converter for Field Programmable Gate Array (FPGA)&lt;br&gt;
Power supplies for mobile devices&lt;br&gt;
POL-converters&lt;br&gt;
Mainboards/ graphic cards&lt;br&gt;
Battery powered devices&lt;br&gt;
Wireless communication devices&lt;br&gt;
Filter&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndXHMI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndXHMI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-XHMI"&gt;http://katalog.we-online.de/en/pbs/WE-XHMI&lt;/a&gt;&lt;p&gt;
Created 2015-08-05&lt;br&gt;
2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-XHMI_74439369XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74439369022">
<attribute name="WE-NUMBER" value="74439369022/2,2uH"/>
</technology>
<technology name="_74439369033">
<attribute name="WE-NUMBER" value="74439369033/3,3uH"/>
</technology>
<technology name="_74439369047">
<attribute name="WE-NUMBER" value="74439369047/4,7uH"/>
</technology>
<technology name="_74439369056">
<attribute name="WE-NUMBER" value="74439369056/5,6uH"/>
</technology>
<technology name="_74439369068">
<attribute name="WE-NUMBER" value="74439369068/6,8uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-ASI_SENSOR" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-ASI SMD Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Specially designed for sensors and actuators

&lt;br&gt; High current and small footprint
&lt;br&gt; High self resonant frequency
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; ASI-applications
&lt;br&gt;Low frequency filter design (kHz range)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndASI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndASI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-ASI"&gt;http://katalog.we-online.de/en/pbs/WE-ASI&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-ASI_SENSOR">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744775318">
<attribute name="WE-NUMBER" value="744775318/18mH"/>
</technology>
<technology name="_744775330">
<attribute name="WE-NUMBER" value="744775330/3mH"/>
</technology>
<technology name="_744775347">
<attribute name="WE-NUMBER" value="744775347/4,7mH"/>
</technology>
<technology name="_744775360">
<attribute name="WE-NUMBER" value="744775360/6mH"/>
</technology>
<technology name="_744775380">
<attribute name="WE-NUMBER" value="744775380/8mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-ASI_L" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-ASI SMD Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Specially designed for sensors and actuators

&lt;br&gt; High current and small footprint
&lt;br&gt; High self resonant frequency
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; ASI-applications
&lt;br&gt;Low frequency filter design (kHz range)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndASI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndASI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-ASI"&gt;http://katalog.we-online.de/en/pbs/WE-ASI&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-ASI_L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74458303">
<attribute name="WE-NUMBER" value="74458303/3mH"/>
</technology>
<technology name="_74458304">
<attribute name="WE-NUMBER" value="74458304/4,7mH"/>
</technology>
<technology name="_74458306">
<attribute name="WE-NUMBER" value="74458306/6mH"/>
</technology>
<technology name="_74458308">
<attribute name="WE-NUMBER" value="74458308/8mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-BAL_0603" prefix="BAL" uservalue="yes">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt; Operating temperature: –40 °C to +85 °C
&lt;br&gt; Power Capacity: 2 W max.
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/RfBAL_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_RfBAL_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-BAL"&gt;http://katalog.we-online.de/en/pbs/WE-BAL&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL"/>
</gates>
<devices>
<device name="" package="WE-BAL_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="_748411245"/>
<technology name="_748412245"/>
<technology name="_748415245"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-BAL_0805" prefix="BAL" uservalue="yes">
<description>&lt;b&gt;WE-BAL Multilayer Chip Balun
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low loss SMD Balun with balanced impedance of 50 to 200 Ω
&lt;br&gt; Operating temperature: –40 °C to +85 °C
&lt;br&gt; Power Capacity: 2 W max.
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt; Wireless communication systems like Home RF, DECT, WLAN, Bluetooth, ZigBee …
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/RfBAL_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_RfBAL_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-BAL"&gt;http://katalog.we-online.de/en/pbs/WE-BAL&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-BAL"/>
</gates>
<devices>
<device name="" package="WE-BAL_0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="_748421245"/>
<technology name="_748421551"/>
<technology name="_748422245"/>
<technology name="_748425245"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-BPF_0805" prefix="BPF" uservalue="yes">
<description>&lt;b&gt;Multilayer Chip Band-Pass Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;  Multilayer Chip Band-Pass Filter with low insertion loss and high attenuation
&lt;br&gt;
&lt;br&gt; SMD component in the sizes 0805 and 1008
&lt;br&gt;
&lt;br&gt; Guaranteed filter characteristics over a wide temperature range
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF applications
&lt;br&gt;
&lt;br&gt; Wireless communication systems like DECT, PACS, PHS, GSM, WLAN, Bluetooth …

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/RfBPF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_RfBPF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-BPF"&gt;http://katalog.we-online.de/en/pbs/WE-BPF&lt;/a&gt;&lt;p&gt;



Updated by  Dan Xu 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="BPF_T1/T5"/>
</gates>
<devices>
<device name="" package="WE-BPF_0805_T1">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="3"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="_748323024"/>
<technology name="_748323056"/>
<technology name="_748323155"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CAIR_1322" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CAIR Air coil
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Inductance values from 1.65nH up to 120 nH
&lt;br&gt; Very high quality factor &gt;100
&lt;br&gt; High self-resonant frequency

&lt;br&gt; High currents up to 3.5 A

&lt;br&gt; 5%(10%) Inductance tolerance
&lt;br&gt; Pick and place process possible
&lt;br&gt; Good solderability (Tinned connector pins)
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;&lt;/b&gt; Especially for RF application
&lt;br&gt; Ideal for high current applications
&lt;br&gt; Broad band filter
&lt;br&gt; RF-Decoupling
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/RfCAIR_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_RfCAIR_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CAIR"&gt;http://katalog.we-online.de/en/pbs/WE-CAIR&lt;/a&gt;&lt;p&gt;

Created on 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CAIR_1322">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744910016">
<attribute name="WE-NUMBER" value="744910016/1,65nH"/>
</technology>
<technology name="_744910025">
<attribute name="WE-NUMBER" value="744910025/2,55nH"/>
</technology>
<technology name="_744910038">
<attribute name="WE-NUMBER" value="744910038/3,85nH"/>
</technology>
<technology name="_744910054">
<attribute name="WE-NUMBER" value="744910054/5,45nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CAIR_3136" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CAIR Air coil
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Inductance values from 1.65nH up to 120 nH
&lt;br&gt; Very high quality factor &gt;100
&lt;br&gt; High self-resonant frequency

&lt;br&gt; High currents up to 3.5 A

&lt;br&gt; 5%(10%) Inductance tolerance
&lt;br&gt; Pick and place process possible
&lt;br&gt; Good solderability (Tinned connector pins)
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;&lt;/b&gt; Especially for RF application
&lt;br&gt; Ideal for high current applications
&lt;br&gt; Broad band filter
&lt;br&gt; RF-Decoupling
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/RfCAIR_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_RfCAIR_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CAIR"&gt;http://katalog.we-online.de/en/pbs/WE-CAIR&lt;/a&gt;&lt;p&gt;

Created on 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CAIR_3136">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744913025">
<attribute name="WE-NUMBER" value="744913025/2,5nH"/>
</technology>
<technology name="_744913050">
<attribute name="WE-NUMBER" value="744913050/5nH"/>
</technology>
<technology name="_744913080">
<attribute name="WE-NUMBER" value="744913080/8nH"/>
</technology>
<technology name="_744913112">
<attribute name="WE-NUMBER" value="744913112/12,5nH"/>
</technology>
<technology name="_744913118">
<attribute name="WE-NUMBER" value="744913118/18,5nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CAIR_1340" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CAIR Air coil
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Inductance values from 1.65nH up to 120 nH
&lt;br&gt; Very high quality factor &gt;100
&lt;br&gt; High self-resonant frequency

&lt;br&gt; High currents up to 3.5 A

&lt;br&gt; 5%(10%) Inductance tolerance
&lt;br&gt; Pick and place process possible
&lt;br&gt; Good solderability (Tinned connector pins)
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;&lt;/b&gt; Especially for RF application
&lt;br&gt; Ideal for high current applications
&lt;br&gt; Broad band filter
&lt;br&gt; RF-Decoupling
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/RfCAIR_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_RfCAIR_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CAIR"&gt;http://katalog.we-online.de/en/pbs/WE-CAIR&lt;/a&gt;&lt;p&gt;

Created on 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CAIR_1340">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744911056">
<attribute name="WE-NUMBER" value="744911056/5,6nH"/>
</technology>
<technology name="_744911071">
<attribute name="WE-NUMBER" value="744911071/7,15nH"/>
</technology>
<technology name="_744911088">
<attribute name="WE-NUMBER" value="744911088/8,8nH"/>
</technology>
<technology name="_744911098">
<attribute name="WE-NUMBER" value="744911098/9,85nH"/>
</technology>
<technology name="_744911112">
<attribute name="WE-NUMBER" value="744911112/12,55nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CAIR_3168" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CAIR Air coil
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Inductance values from 1.65nH up to 120 nH
&lt;br&gt; Very high quality factor &gt;100
&lt;br&gt; High self-resonant frequency

&lt;br&gt; High currents up to 3.5 A

&lt;br&gt; 5%(10%) Inductance tolerance
&lt;br&gt; Pick and place process possible
&lt;br&gt; Good solderability (Tinned connector pins)
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;&lt;/b&gt; Especially for RF application
&lt;br&gt; Ideal for high current applications
&lt;br&gt; Broad band filter
&lt;br&gt; RF-Decoupling
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/RfCAIR_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_RfCAIR_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CAIR"&gt;http://katalog.we-online.de/en/pbs/WE-CAIR&lt;/a&gt;&lt;p&gt;

Created on 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-CAIR_3168">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744914117">
<attribute name="WE-NUMBER" value="744914117/17,5nH"/>
</technology>
<technology name="_744914122">
<attribute name="WE-NUMBER" value="744914122/22nH"/>
</technology>
<technology name="_744914128">
<attribute name="WE-NUMBER" value="744914128/28nH"/>
</technology>
<technology name="_744914135">
<attribute name="WE-NUMBER" value="744914135/35,5nH"/>
</technology>
<technology name="_744914143">
<attribute name="WE-NUMBER" value="744914143/43nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CBA_0402" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CBA SMD EMI Suppression Ferrite Bead
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;Reliable Ni-Sn electrodes
&lt;br&gt;High rated current up to 5A
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -55°C to +125°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;* Perfect as data line filter and for uncoupling of distribution voltage
&lt;BR&gt;
&lt;br&gt;*This special SMD chip bead ferrites can be put directly on the printed circuit board. They offer excellent anti-EMI properties and low DC-resistance. Placed very close next to the interference source even with smallest size 0402,maximal impedance at 1000 Ω can be reached.&lt;BR&gt;
&lt;br&gt;*High Speed:&lt;BR&gt;"High Speed " SMD ferrites WE-CBF have lower impedance in the lower frequency ranges thus they have only a low attenuation for fast signals. Application e.g. USB 2.0, IEEE 1394,LVDS &lt;BR&gt;
&lt;br&gt;*Wide Band:&lt;BR&gt; "Wide Band" SMD ferrites WE-CBF already show high impedance in low frequency range. Therefore they are wide band through the whole spectrum. Application e.g. control signats, RS232, RS422, DC/DC converter &lt;BR&gt;
&lt;br&gt;*High Current:&lt;BR&gt;"High Current " SMD ferrites WE-CBF are designed for high current (over 1 A). The rated current refers to 40K self-heating. High current SMD ferrites are available in all there types (High Speed, Wide Band and High Frequency). Application e.g. power supply, DC/DC converter&lt;BR&gt;
&lt;br&gt;*Advice:&lt;BR&gt;Pay attention for the use of SMD-Ferrites for high current&gt;1A and ambient temperature over +85°C that the rated current has to be reduced when temperature is above +85°C (Derating).&lt;BR&gt;
&lt;br&gt;*At+100°C environment temperature the maximal rated current has to add up to only 60% of the data sheet value ,without an overload of the component.&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeCBA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeCBA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBA/"&gt;http://katalog.we-online.de/en/pbs/WE-CBA/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-02
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_WB/HS" package="WE-CBA_0402(W=1.5)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_782422101"/>
<technology name="_782422102"/>
<technology name="_782422221"/>
<technology name="_782422331"/>
<technology name="_782422511"/>
<technology name="_782422601"/>
</technologies>
</device>
<device name="_HC" package="WE-CBA_0402(W=2.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_782423100"/>
<technology name="_782423700"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CBA_0603" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CBA SMD EMI Suppression Ferrite Bead
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;Reliable Ni-Sn electrodes
&lt;br&gt;High rated current up to 5A
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -55°C to +125°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;* Perfect as data line filter and for uncoupling of distribution voltage
&lt;BR&gt;
&lt;br&gt;*This special SMD chip bead ferrites can be put directly on the printed circuit board. They offer excellent anti-EMI properties and low DC-resistance. Placed very close next to the interference source even with smallest size 0402,maximal impedance at 1000 Ω can be reached.&lt;BR&gt;
&lt;br&gt;*High Speed:&lt;BR&gt;"High Speed " SMD ferrites WE-CBF have lower impedance in the lower frequency ranges thus they have only a low attenuation for fast signals. Application e.g. USB 2.0, IEEE 1394,LVDS &lt;BR&gt;
&lt;br&gt;*Wide Band:&lt;BR&gt; "Wide Band" SMD ferrites WE-CBF already show high impedance in low frequency range. Therefore they are wide band through the whole spectrum. Application e.g. control signats, RS232, RS422, DC/DC converter &lt;BR&gt;
&lt;br&gt;*High Current:&lt;BR&gt;"High Current " SMD ferrites WE-CBF are designed for high current (over 1 A). The rated current refers to 40K self-heating. High current SMD ferrites are available in all there types (High Speed, Wide Band and High Frequency). Application e.g. power supply, DC/DC converter&lt;BR&gt;
&lt;br&gt;*Advice:&lt;BR&gt;Pay attention for the use of SMD-Ferrites for high current&gt;1A and ambient temperature over +85°C that the rated current has to be reduced when temperature is above +85°C (Derating).&lt;BR&gt;
&lt;br&gt;*At+100°C environment temperature the maximal rated current has to add up to only 60% of the data sheet value ,without an overload of the component.&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeCBA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeCBA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBA/"&gt;http://katalog.we-online.de/en/pbs/WE-CBA/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-02
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_WB/HS" package="WE-CBA_0603(W=2.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_782631101"/>
<technology name="_782631182"/>
<technology name="_782631222"/>
<technology name="_782631331"/>
<technology name="_782632102"/>
<technology name="_782632121"/>
<technology name="_782632181"/>
<technology name="_782632511"/>
<technology name="_782632620"/>
</technologies>
</device>
<device name="_HC" package="WE-CBA_0603(W=2.6)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_782633601"/>
<technology name="_782633620"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CBA_0805" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CBA SMD EMI Suppression Ferrite Bead
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;Reliable Ni-Sn electrodes
&lt;br&gt;High rated current up to 5A
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -55°C to +125°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;* Perfect as data line filter and for uncoupling of distribution voltage
&lt;BR&gt;
&lt;br&gt;*This special SMD chip bead ferrites can be put directly on the printed circuit board. They offer excellent anti-EMI properties and low DC-resistance. Placed very close next to the interference source even with smallest size 0402,maximal impedance at 1000 Ω can be reached.&lt;BR&gt;
&lt;br&gt;*High Speed:&lt;BR&gt;"High Speed " SMD ferrites WE-CBF have lower impedance in the lower frequency ranges thus they have only a low attenuation for fast signals. Application e.g. USB 2.0, IEEE 1394,LVDS &lt;BR&gt;
&lt;br&gt;*Wide Band:&lt;BR&gt; "Wide Band" SMD ferrites WE-CBF already show high impedance in low frequency range. Therefore they are wide band through the whole spectrum. Application e.g. control signats, RS232, RS422, DC/DC converter &lt;BR&gt;
&lt;br&gt;*High Current:&lt;BR&gt;"High Current " SMD ferrites WE-CBF are designed for high current (over 1 A). The rated current refers to 40K self-heating. High current SMD ferrites are available in all there types (High Speed, Wide Band and High Frequency). Application e.g. power supply, DC/DC converter&lt;BR&gt;
&lt;br&gt;*Advice:&lt;BR&gt;Pay attention for the use of SMD-Ferrites for high current&gt;1A and ambient temperature over +85°C that the rated current has to be reduced when temperature is above +85°C (Derating).&lt;BR&gt;
&lt;br&gt;*At+100°C environment temperature the maximal rated current has to add up to only 60% of the data sheet value ,without an overload of the component.&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeCBA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeCBA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBA/"&gt;http://katalog.we-online.de/en/pbs/WE-CBA/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-02
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_WB/HS" package="WE-CBA_0805(W=3)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_782851102"/>
<technology name="_782851202"/>
</technologies>
</device>
<device name="_HC" package="WE-CBA_0805(W=4)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_782853112"/>
<technology name="_782853121"/>
<technology name="_782853152"/>
<technology name="_782853200"/>
<technology name="_782853221"/>
<technology name="_782853270"/>
<technology name="_782853561"/>
<technology name="_782853680"/>
<technology name="_782853910"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CBA_1206" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CBA SMD EMI Suppression Ferrite Bead
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;Reliable Ni-Sn electrodes
&lt;br&gt;High rated current up to 5A
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Operating temperature: -55°C to +125°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;* Perfect as data line filter and for uncoupling of distribution voltage
&lt;BR&gt;
&lt;br&gt;*This special SMD chip bead ferrites can be put directly on the printed circuit board. They offer excellent anti-EMI properties and low DC-resistance. Placed very close next to the interference source even with smallest size 0402,maximal impedance at 1000 Ω can be reached.&lt;BR&gt;
&lt;br&gt;*High Speed:&lt;BR&gt;"High Speed " SMD ferrites WE-CBF have lower impedance in the lower frequency ranges thus they have only a low attenuation for fast signals. Application e.g. USB 2.0, IEEE 1394,LVDS &lt;BR&gt;
&lt;br&gt;*Wide Band:&lt;BR&gt; "Wide Band" SMD ferrites WE-CBF already show high impedance in low frequency range. Therefore they are wide band through the whole spectrum. Application e.g. control signats, RS232, RS422, DC/DC converter &lt;BR&gt;
&lt;br&gt;*High Current:&lt;BR&gt;"High Current " SMD ferrites WE-CBF are designed for high current (over 1 A). The rated current refers to 40K self-heating. High current SMD ferrites are available in all there types (High Speed, Wide Band and High Frequency). Application e.g. power supply, DC/DC converter&lt;BR&gt;
&lt;br&gt;*Advice:&lt;BR&gt;Pay attention for the use of SMD-Ferrites for high current&gt;1A and ambient temperature over +85°C that the rated current has to be reduced when temperature is above +85°C (Derating).&lt;BR&gt;
&lt;br&gt;*At+100°C environment temperature the maximal rated current has to add up to only 60% of the data sheet value ,without an overload of the component.&lt;BR&gt;
&lt;br&gt;
&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeCBA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeCBA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBA/"&gt;http://katalog.we-online.de/en/pbs/WE-CBA/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-02
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_HC" package="WE-CBA_1206(W=5.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_782763102"/>
<technology name="_782763621"/>
<technology name="_782763820"/>
</technologies>
</device>
<device name="_WB/HS" package="WE-CBA_1206(W=4.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_782762301"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CFWI_1312" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-CFWI Coupled Flatwire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Very low RDC
&lt;BR&gt;
&lt;BR&gt; Low inductance drift over temperature
&lt;BR&gt;
&lt;BR&gt; Operating temperature: –40 °C up to +150 °C
&lt;BR&gt;
&lt;BR&gt; Coupled inductor with two identical windings
&lt;BR&gt;
&lt;BR&gt; More variants due to parallel and serie connection
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt; High power switching regulators
&lt;BR&gt;
&lt;BR&gt; 1:1 flyback converter
&lt;BR&gt;
&lt;BR&gt; Buck, Boost, Sepic and Cuk Converter
&lt;BR&gt;
&lt;BR&gt; Switching regulators with secondary unregulated output voltage
&lt;BR&gt;
&lt;BR&gt;Battery Cell Charging Balancer
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndCFWI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndCFWI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CFWI?"&gt;http://katalog.we-online.de/en/pbs/WE-CFWI?&lt;/a&gt;&lt;p&gt;

updated by  Dan Xu 2014-07-15&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_2"/>
</gates>
<devices>
<device name="" package="WE-CFWI_1312">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_74485540101">
<attribute name="WE-NUMBER" value="74485540101/10uH"/>
</technology>
<technology name="_74485540680">
<attribute name="WE-NUMBER" value="74485540680/6,8uH"/>
</technology>
<technology name="_74485540820">
<attribute name="WE-NUMBER" value="74485540820/8,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CFWI_1813" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-CFWI Coupled Flatwire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Very low RDC
&lt;BR&gt;
&lt;BR&gt; Low inductance drift over temperature
&lt;BR&gt;
&lt;BR&gt; Operating temperature: –40 °C up to +150 °C
&lt;BR&gt;
&lt;BR&gt; Coupled inductor with two identical windings
&lt;BR&gt;
&lt;BR&gt; More variants due to parallel and serie connection
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt; High power switching regulators
&lt;BR&gt;
&lt;BR&gt; 1:1 flyback converter
&lt;BR&gt;
&lt;BR&gt; Buck, Boost, Sepic and Cuk Converter
&lt;BR&gt;
&lt;BR&gt; Switching regulators with secondary unregulated output voltage
&lt;BR&gt;
&lt;BR&gt;Battery Cell Charging Balancer
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndCFWI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndCFWI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CFWI?"&gt;http://katalog.we-online.de/en/pbs/WE-CFWI?&lt;/a&gt;&lt;p&gt;

updated by  Dan Xu 2014-07-15&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_2"/>
</gates>
<devices>
<device name="" package="WE-CFWI_1813">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_74485542101">
<attribute name="WE-NUMBER" value="74485542101/10uH"/>
</technology>
<technology name="_74485542680">
<attribute name="WE-NUMBER" value="74485542680/6,8uH"/>
</technology>
<technology name="_74485542820">
<attribute name="WE-NUMBER" value="74485542820/8,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DD_7332" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-DD SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; 1:1 transformer 
&lt;br&gt;
&lt;br&gt; Double inductor with two identical windings 
&lt;br&gt;
&lt;br&gt; 4 different sizes available 
&lt;br&gt; 
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Recommended solder profile: Reflow 
&lt;br&gt; 
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; For SEPIC and CUK topologies 
&lt;br&gt;
&lt;br&gt; Flyback applications 
&lt;br&gt;
&lt;br&gt; Switching regulators with second, unregulated output voltages 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndDD_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndDD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-DD"&gt;http://katalog.we-online.de/en/pbs/WE-DD&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by  Dan Xu 2014-06-10&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-DD_7332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744878001">
<attribute name="WE-NUMBER" value="744878001/1,3uH"/>
</technology>
<technology name="_744878002">
<attribute name="WE-NUMBER" value="744878002/2,4uH"/>
</technology>
<technology name="_744878003">
<attribute name="WE-NUMBER" value="744878003/3,3uH"/>
</technology>
<technology name="_744878004">
<attribute name="WE-NUMBER" value="744878004/4,7uH"/>
</technology>
<technology name="_744878005">
<attribute name="WE-NUMBER" value="744878005/5,6uH"/>
</technology>
<technology name="_744878006">
<attribute name="WE-NUMBER" value="744878006/6,8uH"/>
</technology>
<technology name="_744878008">
<attribute name="WE-NUMBER" value="744878008/8,2uH"/>
</technology>
<technology name="_744878100">
<attribute name="WE-NUMBER" value="744878100/10uH"/>
</technology>
<technology name="_744878101">
<attribute name="WE-NUMBER" value="744878101/100uH"/>
</technology>
<technology name="_744878220">
<attribute name="WE-NUMBER" value="744878220/22uH"/>
</technology>
<technology name="_744878470">
<attribute name="WE-NUMBER" value="744878470/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DD_1210" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-DD SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; 1:1 transformer 
&lt;br&gt;
&lt;br&gt; Double inductor with two identical windings 
&lt;br&gt;
&lt;br&gt; 4 different sizes available 
&lt;br&gt; 
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Recommended solder profile: Reflow 
&lt;br&gt; 
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; For SEPIC and CUK topologies 
&lt;br&gt;
&lt;br&gt; Flyback applications 
&lt;br&gt;
&lt;br&gt; Switching regulators with second, unregulated output voltages 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndDD_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndDD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-DD"&gt;http://katalog.we-online.de/en/pbs/WE-DD&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by  Dan Xu 2014-06-10&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-DD_1210/1260/1280_CROSSED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_7448709022">
<attribute name="WE-NUMBER" value="7448709022/2,2uH"/>
</technology>
<technology name="_7448709033">
<attribute name="WE-NUMBER" value="7448709033/3,3uH"/>
</technology>
<technology name="_7448709047">
<attribute name="WE-NUMBER" value="7448709047/4,7uH"/>
</technology>
<technology name="_7448709068">
<attribute name="WE-NUMBER" value="7448709068/6,8uH"/>
</technology>
<technology name="_7448709100">
<attribute name="WE-NUMBER" value="7448709100/10uH"/>
</technology>
<technology name="_7448709220">
<attribute name="WE-NUMBER" value="7448709220/22uH"/>
</technology>
<technology name="_7448709330">
<attribute name="WE-NUMBER" value="7448709330/3,3uH"/>
</technology>
<technology name="_7448709470">
<attribute name="WE-NUMBER" value="7448709470/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DD_1260" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-DD SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; 1:1 transformer 
&lt;br&gt;
&lt;br&gt; Double inductor with two identical windings 
&lt;br&gt;
&lt;br&gt; 4 different sizes available 
&lt;br&gt; 
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Recommended solder profile: Reflow 
&lt;br&gt; 
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; For SEPIC and CUK topologies 
&lt;br&gt;
&lt;br&gt; Flyback applications 
&lt;br&gt;
&lt;br&gt; Switching regulators with second, unregulated output voltages 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndDD_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndDD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-DD"&gt;http://katalog.we-online.de/en/pbs/WE-DD&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by  Dan Xu 2014-06-10&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-DD_1260/1280">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_744874001">
<attribute name="WE-NUMBER" value="744874001/1,5uH"/>
</technology>
<technology name="_744874002">
<attribute name="WE-NUMBER" value="744874002/2,4uH"/>
</technology>
<technology name="_744874003">
<attribute name="WE-NUMBER" value="744874003/3,3uH"/>
</technology>
<technology name="_744874004">
<attribute name="WE-NUMBER" value="744874004/4,7uH"/>
</technology>
<technology name="_744874006">
<attribute name="WE-NUMBER" value="744874006/6,8uH"/>
</technology>
<technology name="_744874100">
<attribute name="WE-NUMBER" value="744874100/10uH"/>
</technology>
<technology name="_744874101">
<attribute name="WE-NUMBER" value="744874101/100uH"/>
</technology>
<technology name="_744874220">
<attribute name="WE-NUMBER" value="744874220/22uH"/>
</technology>
<technology name="_744874470">
<attribute name="WE-NUMBER" value="744874470/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DD_1280" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-DD SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; 1:1 transformer 
&lt;br&gt;
&lt;br&gt; Double inductor with two identical windings 
&lt;br&gt;
&lt;br&gt; 4 different sizes available 
&lt;br&gt; 
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Recommended solder profile: Reflow 
&lt;br&gt; 
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; For SEPIC and CUK topologies 
&lt;br&gt;
&lt;br&gt; Flyback applications 
&lt;br&gt;
&lt;br&gt; Switching regulators with second, unregulated output voltages 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndDD_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndDD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-DD"&gt;http://katalog.we-online.de/en/pbs/WE-DD&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by  Dan Xu 2014-06-10&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-DD_1260/1280">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_744873001">
<attribute name="WE-NUMBER" value="744873001/1,5uH"/>
</technology>
<technology name="_744873002">
<attribute name="WE-NUMBER" value="744873002/2,4uH"/>
</technology>
<technology name="_744873003">
<attribute name="WE-NUMBER" value="744873003/3,3uH"/>
</technology>
<technology name="_744873004">
<attribute name="WE-NUMBER" value="744873004/4,7uH"/>
</technology>
<technology name="_744873100">
<attribute name="WE-NUMBER" value="744873100/10uH"/>
</technology>
<technology name="_744873101">
<attribute name="WE-NUMBER" value="744873101/100uH"/>
</technology>
<technology name="_744873150">
<attribute name="WE-NUMBER" value="744873150/15uH"/>
</technology>
<technology name="_744873220">
<attribute name="WE-NUMBER" value="744873220/22uH"/>
</technology>
<technology name="_744873221">
<attribute name="WE-NUMBER" value="744873221/220uH"/>
</technology>
<technology name="_744873330">
<attribute name="WE-NUMBER" value="744873330/33uH"/>
</technology>
<technology name="_744873470">
<attribute name="WE-NUMBER" value="744873470/47uH"/>
</technology>
<technology name="_744873680">
<attribute name="WE-NUMBER" value="744873680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DD_1260_CROSSED" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-DD SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; 1:1 transformer 
&lt;br&gt;
&lt;br&gt; Double inductor with two identical windings 
&lt;br&gt;
&lt;br&gt; 4 different sizes available 
&lt;br&gt; 
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Recommended solder profile: Reflow 
&lt;br&gt; 
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; For SEPIC and CUK topologies 
&lt;br&gt;
&lt;br&gt; Flyback applications 
&lt;br&gt;
&lt;br&gt; Switching regulators with second, unregulated output voltages 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndDD_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndDD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-DD"&gt;http://katalog.we-online.de/en/pbs/WE-DD&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by  Dan Xu 2014-06-10&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-DD_1210/1260/1280_CROSSED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_744871004">
<attribute name="WE-NUMBER" value="744971004/4,7uH"/>
</technology>
<technology name="_744871006">
<attribute name="WE-NUMBER" value="744871006/6,8uH"/>
</technology>
<technology name="_744871100">
<attribute name="WE-NUMBER" value="744871100/10uH"/>
</technology>
<technology name="_744871101">
<attribute name="WE-NUMBER" value="744871101/100uH"/>
</technology>
<technology name="_744871220">
<attribute name="WE-NUMBER" value="744871220/22uH"/>
</technology>
<technology name="_744871330">
<attribute name="WE-NUMBER" value="744871330/33uH"/>
</technology>
<technology name="_744871470">
<attribute name="WE-NUMBER" value="744871470/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DD_1280_CROSSED" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-DD SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; 1:1 transformer 
&lt;br&gt;
&lt;br&gt; Double inductor with two identical windings 
&lt;br&gt;
&lt;br&gt; 4 different sizes available 
&lt;br&gt; 
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Recommended solder profile: Reflow 
&lt;br&gt; 
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; For SEPIC and CUK topologies 
&lt;br&gt;
&lt;br&gt; Flyback applications 
&lt;br&gt;
&lt;br&gt; Switching regulators with second, unregulated output voltages 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndDD_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndDD_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-DD"&gt;http://katalog.we-online.de/en/pbs/WE-DD&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Updated by  Dan Xu 2014-06-10&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-DD_1210/1260/1280_CROSSED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_7448700015">
<attribute name="WE-NUMBER" value="7448700015/1,5uH"/>
</technology>
<technology name="_744870002">
<attribute name="WE-NUMBER" value="744870002/2,4uH"/>
</technology>
<technology name="_744870003">
<attribute name="WE-NUMBER" value="744870003/3,3uH"/>
</technology>
<technology name="_744870004">
<attribute name="WE-NUMBER" value="744870004/4,7uH"/>
</technology>
<technology name="_744870006">
<attribute name="WE-NUMBER" value="744870006//6,8uH"/>
</technology>
<technology name="_744870100">
<attribute name="WE-NUMBER" value="744870100/10uH"/>
</technology>
<technology name="_744870101">
<attribute name="WE-NUMBER" value="744870101/100uH"/>
</technology>
<technology name="_744870151">
<attribute name="WE-NUMBER" value="744870151/150uH"/>
</technology>
<technology name="_744870220">
<attribute name="WE-NUMBER" value="744870220/22uH"/>
</technology>
<technology name="_744870221">
<attribute name="WE-NUMBER" value="744870221/220uH"/>
</technology>
<technology name="_744870470">
<attribute name="WE-NUMBER" value="744870470/47uH"/>
</technology>
<technology name="_744870471">
<attribute name="WE-NUMBER" value="7448770471/470uH"/>
</technology>
<technology name="_744870680">
<attribute name="WE-NUMBER" value="744870680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-GF_1210(M)" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Wire wound on ferrite
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +105 °C
&lt;br&gt;
&lt;br&gt; High resistance against dampness
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; RF circuits like tuner, transponder etc.
&lt;br&gt;
&lt;br&gt; RF amplifier circuits like antennas amplifier
&lt;br&gt;
&lt;br&gt; Oscillator
&lt;br&gt;
&lt;br&gt; Filter circuits
&lt;br&gt;
&lt;br&gt; Amplification circuits

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-GF_SMD-HF.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-GF_SMD-HF.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-GF?"&gt;http://katalog.we-online.de/en/pbs/WE-GF?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-GF_1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744764002">
<attribute name="WE-NUMBER" value="744764002/0,22uH"/>
</technology>
<technology name="_7447640027">
<attribute name="WE-NUMBER" value="7447640027/0,27uH"/>
</technology>
<technology name="_744764003">
<attribute name="WE-NUMBER" value="744764003/0,39uH"/>
</technology>
<technology name="_7447640033">
<attribute name="WE-NUMBER" value="7447640033/0,33uH"/>
</technology>
<technology name="_744764004">
<attribute name="WE-NUMBER" value="744764004/0,47uH"/>
</technology>
<technology name="_744764005">
<attribute name="WE-NUMBER" value="744764005/0,56uH"/>
</technology>
<technology name="_744764006">
<attribute name="WE-NUMBER" value="744764006/0,68uH"/>
</technology>
<technology name="_7447640082">
<attribute name="WE-NUMBER" value="7447640082/0,82uH"/>
</technology>
<technology name="_74476401">
<attribute name="WE-NUMBER" value="74476401/1uH"/>
</technology>
<technology name="_744764012">
<attribute name="WE-NUMBER" value="744764012/1,2uH"/>
</technology>
<technology name="_744764015">
<attribute name="WE-NUMBER" value="744764015/1,5uH"/>
</technology>
<technology name="_744764018">
<attribute name="WE-NUMBER" value="744764018/1,8uH"/>
</technology>
<technology name="_74476402">
<attribute name="WE-NUMBER" value="74476402/2,2uH"/>
</technology>
<technology name="_744764027">
<attribute name="WE-NUMBER" value="744764027/2,7uH"/>
</technology>
<technology name="_74476403">
<attribute name="WE-NUMBER" value="74476403/3,3uH"/>
</technology>
<technology name="_744764039">
<attribute name="WE-NUMBER" value="744764039/3,9uH"/>
</technology>
<technology name="_74476404">
<attribute name="WE-NUMBER" value="74476404/4,7uH"/>
</technology>
<technology name="_74476406">
<attribute name="WE-NUMBER" value="74476406/6,8uH"/>
</technology>
<technology name="_74476410">
<attribute name="WE-NUMBER" value="74476410/10uH"/>
</technology>
<technology name="_744764112">
<attribute name="WE-NUMBER" value="744764112/12uH"/>
</technology>
<technology name="_744764115">
<attribute name="WE-NUMBER" value="744764115/15uH"/>
</technology>
<technology name="_744764118">
<attribute name="WE-NUMBER" value="744764118/18uH"/>
</technology>
<technology name="_744764122">
<attribute name="WE-NUMBER" value="744764122/22uH"/>
</technology>
<technology name="_744764133">
<attribute name="WE-NUMBER" value="744764133/33uH"/>
</technology>
<technology name="_744764139">
<attribute name="WE-NUMBER" value="744764139/39uH"/>
</technology>
<technology name="_744764147">
<attribute name="WE-NUMBER" value="744764147/47uH"/>
</technology>
<technology name="_744764156">
<attribute name="WE-NUMBER" value="744764156/56uH"/>
</technology>
<technology name="_744764168">
<attribute name="WE-NUMBER" value="744764168/68uH"/>
</technology>
<technology name="_74476420">
<attribute name="WE-NUMBER" value="74476420/100uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-GFH_2520" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD RF Choke WE-GFH&lt;/b&gt;&lt;p&gt;

- Wire wound ferrite&lt;br&gt;
- For higher currents&lt;p&gt;

-- HF-circuits like tuner, transponder etc.
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-GFH.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-GFH.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-GFH"&gt;http://katalog.we-online.de/en/pbs/WE-GFH&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-GFH_2520">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447629010">
<attribute name="WE-NUMBER" value="7447629010/1uH"/>
</technology>
<technology name="_7447629015">
<attribute name="WE-NUMBER" value="7447629015/1,5uH"/>
</technology>
<technology name="_7447629022">
<attribute name="WE-NUMBER" value="7447629022/2,2uH"/>
</technology>
<technology name="_7447629033">
<attribute name="WE-NUMBER" value="7447629033/3,3uH"/>
</technology>
<technology name="_7447629047">
<attribute name="WE-NUMBER" value="7447629047/4,7uH"/>
</technology>
<technology name="_7447629068">
<attribute name="WE-NUMBER" value="7447629068/6,8uH"/>
</technology>
<technology name="_7447629100">
<attribute name="WE-NUMBER" value="7447629100/10uH"/>
</technology>
<technology name="_7447629150">
<attribute name="WE-NUMBER" value="7447629150/15uH"/>
</technology>
<technology name="_7447629220">
<attribute name="WE-NUMBER" value="7447629220/22uH"/>
</technology>
<technology name="_7447629330">
<attribute name="WE-NUMBER" value="7447629330/33uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-GFH_3225" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD RF Choke WE-GFH&lt;/b&gt;&lt;p&gt;

- Wire wound ferrite&lt;br&gt;
- For higher currents&lt;p&gt;

-- HF-circuits like tuner, transponder etc.
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-GFH.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-GFH.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-GFH"&gt;http://katalog.we-online.de/en/pbs/WE-GFH&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-GFH_3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744764901">
<attribute name="WE-NUMBER" value="744764901/1uH"/>
</technology>
<technology name="_7447649015">
<attribute name="WE-NUMBER" value="7447649015/1,5uH"/>
</technology>
<technology name="_744764902">
<attribute name="WE-NUMBER" value="744764902/2,2uH"/>
</technology>
<technology name="_744764903">
<attribute name="WE-NUMBER" value="744764903//3,3uH"/>
</technology>
<technology name="_744764904">
<attribute name="WE-NUMBER" value="744764904/4,7uH"/>
</technology>
<technology name="_744764910">
<attribute name="WE-NUMBER" value="744764910/10uH"/>
</technology>
<technology name="_7447649115">
<attribute name="WE-NUMBER" value="7447649115/15uH"/>
</technology>
<technology name="_7447649122">
<attribute name="WE-NUMBER" value="7447649122/22uH"/>
</technology>
<technology name="_7447649133">
<attribute name="WE-NUMBER" value="7447649133/33uH"/>
</technology>
<technology name="_7447649147">
<attribute name="WE-NUMBER" value="7447649147/47uH"/>
</technology>
<technology name="_7447649168">
<attribute name="WE-NUMBER" value="7447649168/68uH"/>
</technology>
<technology name="_744764920">
<attribute name="WE-NUMBER" value="744764920/100uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCC_1090" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Cube Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Current capability up to 27 A
&lt;br&gt;
&lt;br&gt; Excellent saturation characteristics
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter choke for DC/DC converter
&lt;br&gt;
&lt;br&gt; Single and polyphase buck converter
&lt;br&gt;
&lt;br&gt; Filter choke for motor electronics
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCC.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCC?"&gt;http://katalog.we-online.de/en/pbs/WE-HCC?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCC_1090">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744330470">
<attribute name="WE-NUMBER" value="744330470/4,7uH"/>
</technology>
<technology name="_744330680">
<attribute name="WE-NUMBER" value="744330680/6,8uH"/>
</technology>
<technology name="_744330820">
<attribute name="WE-NUMBER" value="744330820/8,2uH"/>
</technology>
<technology name="_7443330022">
<attribute name="WE-NUMBER" value="7443330022/0,22uH"/>
</technology>
<technology name="_7443330033">
<attribute name="WE-NUMBER" value="7443330033/0,33uH"/>
</technology>
<technology name="_7443330047">
<attribute name="WE-NUMBER" value="7443330047/0,47uH"/>
</technology>
<technology name="_7443330068">
<attribute name="WE-NUMBER" value="7443330068/0,68uH"/>
</technology>
<technology name="_7443330082">
<attribute name="WE-NUMBER" value="7443330082/0,82uH"/>
</technology>
<technology name="_7443330100">
<attribute name="WE-NUMBER" value="7443330100/1uH"/>
</technology>
<technology name="_7443330150">
<attribute name="WE-NUMBER" value="7443330150/1,5uH"/>
</technology>
<technology name="_7443330220">
<attribute name="WE-NUMBER" value="7443330220/2,2uH"/>
</technology>
<technology name="_7443330330">
<attribute name="WE-NUMBER" value="7443330330/3,3uH"/>
</technology>
<technology name="_7443331000">
<attribute name="WE-NUMBER" value="7443331000/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCC_1210" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Cube Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Current capability up to 27 A
&lt;br&gt;
&lt;br&gt; Excellent saturation characteristics
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter choke for DC/DC converter
&lt;br&gt;
&lt;br&gt; Single and polyphase buck converter
&lt;br&gt;
&lt;br&gt; Filter choke for motor electronics
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCC.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCC?"&gt;http://katalog.we-online.de/en/pbs/WE-HCC?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-05-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCC_1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443310022">
<attribute name="WE-NUMBER" value="7443310022/0,22uH"/>
</technology>
<technology name="_7443310033">
<attribute name="WE-NUMBER" value="7443310033/0,33uH"/>
</technology>
<technology name="_7443310047">
<attribute name="WE-NUMBER" value="7443310047/0,47uH"/>
</technology>
<technology name="_7443310068">
<attribute name="WE-NUMBER" value="7443310068/0,68uH"/>
</technology>
<technology name="_7443310082">
<attribute name="WE-NUMBER" value="7443310082/0,82uH"/>
</technology>
<technology name="_7443310100">
<attribute name="WE-NUMBER" value="7443310100/1uH"/>
</technology>
<technology name="_7443310150">
<attribute name="WE-NUMBER" value="7443310150/1,5uH"/>
</technology>
<technology name="_7443310220">
<attribute name="WE-NUMBER" value="7443310220/2,2uH"/>
</technology>
<technology name="_7443310330">
<attribute name="WE-NUMBER" value="7443310330/3,3uH"/>
</technology>
<technology name="_7443310390">
<attribute name="WE-NUMBER" value="7443310390/3,9uH"/>
</technology>
<technology name="_7443310470">
<attribute name="WE-NUMBER" value="7443310470/4,7uH"/>
</technology>
<technology name="_7443320022">
<attribute name="WE-NUMBER" value="7443320022,0,22uH"/>
</technology>
<technology name="_7443320033">
<attribute name="WE-NUMBER" value="7443320033/0,33uH"/>
</technology>
<technology name="_7443320047">
<attribute name="WE-NUMBER" value="7443320047/0,47uH"/>
</technology>
<technology name="_7443320068">
<attribute name="WE-NUMBER" value="7443320068/0,68uH"/>
</technology>
<technology name="_7443320082">
<attribute name="WE-NUMBER" value="7443320082/8,2uH"/>
</technology>
<technology name="_7443320100">
<attribute name="WE-NUMBER" value="744332100/1uH"/>
</technology>
<technology name="_7443320150">
<attribute name="WE-NUMBER" value="7443320150/1,5uH"/>
</technology>
<technology name="_7443320220">
<attribute name="WE-NUMBER" value="7443320220/2,2uH"/>
</technology>
<technology name="_7443320330">
<attribute name="WE-NUMBER" value="7443320330/3,3uH"/>
</technology>
<technology name="_7443320470">
<attribute name="WE-NUMBER" value="7443320470/4,7uH"/>
</technology>
<technology name="_7443320680">
<attribute name="WE-NUMBER" value="7443320680/6,8uH"/>
</technology>
<technology name="_7443320820">
<attribute name="WE-NUMBER" value="7443320820/8,2uH"/>
</technology>
<technology name="_7443321000">
<attribute name="WE-NUMBER" value="7443321000/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCF_2013" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Saturation current up to 75 A
&lt;br&gt;
&lt;br&gt; Very low core losses (MnZn)
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Current capability up to 32 A
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Storage inductor for high efficiency DC/DC converters
&lt;br&gt;
&lt;br&gt; Single and polyphase buck converters
&lt;br&gt;
&lt;br&gt; Filter for audio applications
&lt;br&gt;
&lt;br&gt; Optimized for high current boost applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-hcf_smd_hochstrominduktivitaet_11.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-hcf_smd_hochstrominduktivitaet_11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCF#vs_ct:1"&gt;http://katalog.we-online.de/en/pbs/WE-HCF#vs_ct:1&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCF_2013">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443630070">
<attribute name="WE-NUMBER" value="7443630070/0,7uH"/>
</technology>
<technology name="_7443630140">
<attribute name="WE-NUMBER" value="7443630140/1,4uH"/>
</technology>
<technology name="_7443630220">
<attribute name="WE-NUMBER" value="7443630220/2,2uH"/>
</technology>
<technology name="_7443630310">
<attribute name="WE-NUMBER" value="7443630310/3,1uH"/>
</technology>
<technology name="_7443630420">
<attribute name="WE-NUMBER" value="7443630420/4,2uH"/>
</technology>
<technology name="_7443630550">
<attribute name="WE-NUMBER" value="7443630550/5,5uH"/>
</technology>
<technology name="_7443630700">
<attribute name="WE-NUMBER" value="7443630700/7uH"/>
</technology>
<technology name="_7443630860">
<attribute name="WE-NUMBER" value="7443630860/8,6uH"/>
</technology>
<technology name="_7443631000">
<attribute name="WE-NUMBER" value="7443631000/10uH"/>
</technology>
<technology name="_7443631500">
<attribute name="WE-NUMBER" value="7443631500/15uH"/>
</technology>
<technology name="_7443632200">
<attribute name="WE-NUMBER" value="7443632200/22uH"/>
</technology>
<technology name="_7443633300">
<attribute name="WE-NUMBER" value="7443633300/33uH"/>
</technology>
<technology name="_7443634700">
<attribute name="WE-NUMBER" value="7443634700/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1030" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Flat wire coil for low losses at high frequency
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +150/155 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; Industrial computers
&lt;br&gt;
&lt;br&gt; Motherboards
&lt;br&gt;
&lt;br&gt; High current switching regulators
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Polyphase-switching regulators
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCI?"&gt;http://katalog.we-online.de/en/pbs/WE-HCI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744323020">
<attribute name="WE-NUMBER" value="744323020/0,2uH"/>
</technology>
<technology name="_744323033">
<attribute name="WE-NUMBER" value="744323033/0,33uH"/>
</technology>
<technology name="_744323056">
<attribute name="WE-NUMBER" value="744323056/0,56uH"/>
</technology>
<technology name="_744323068">
<attribute name="WE-NUMBER" value="744323068/0,68uH"/>
</technology>
<technology name="_744323100">
<attribute name="WE-NUMBER" value="744323100/1uH"/>
</technology>
<technology name="_744323120">
<attribute name="WE-NUMBER" value="744323120/1,2uH"/>
</technology>
<technology name="_744323150">
<attribute name="WE-NUMBER" value="744323150/1,5uH"/>
</technology>
<technology name="_744323220">
<attribute name="WE-NUMBER" value="744323220/0,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1040" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Flat wire coil for low losses at high frequency
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +150/155 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; Industrial computers
&lt;br&gt;
&lt;br&gt; Motherboards
&lt;br&gt;
&lt;br&gt; High current switching regulators
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Polyphase-switching regulators
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCI?"&gt;http://katalog.we-online.de/en/pbs/WE-HCI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443552100">
<attribute name="WE-NUMBER" value="7443552100/1uH"/>
</technology>
<technology name="_744355215">
<attribute name="WE-NUMBER" value="744355215/0,15uH"/>
</technology>
<technology name="_7443552150">
<attribute name="WE-NUMBER" value="7443552150/1,5uH"/>
</technology>
<technology name="_7443552200">
<attribute name="WE-NUMBER" value="7443552200/2uH"/>
</technology>
<technology name="_7443552280">
<attribute name="WE-NUMBER" value="7443552280/2,8uH"/>
</technology>
<technology name="_744355230">
<attribute name="WE-NUMBER" value="744355230/0,3uH"/>
</technology>
<technology name="_7443552430">
<attribute name="WE-NUMBER" value="7443552430/4,3uH"/>
</technology>
<technology name="_744355256">
<attribute name="WE-NUMBER" value="744355256/0,56uH"/>
</technology>
<technology name="_7443552560">
<attribute name="WE-NUMBER" value="7443552560/5,6uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1050" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Flat wire coil for low losses at high frequency
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +150/155 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; Industrial computers
&lt;br&gt;
&lt;br&gt; Motherboards
&lt;br&gt;
&lt;br&gt; High current switching regulators
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Polyphase-switching regulators
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCI?"&gt;http://katalog.we-online.de/en/pbs/WE-HCI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744325016">
<attribute name="WE-NUMBER" value="744325016/0,16uH"/>
</technology>
<technology name="_744325040">
<attribute name="WE-NUMBER" value="744325040/0,4uH"/>
</technology>
<technology name="_744325072">
<attribute name="WE-NUMBER" value="744325072/0,72uH"/>
</technology>
<technology name="_7443251000">
<attribute name="WE-NUMBER" value="7443251000/10uH"/>
</technology>
<technology name="_744325120">
<attribute name="WE-NUMBER" value="744325120/1,2uH"/>
</technology>
<technology name="_7443251600">
<attribute name="WE-NUMBER" value="7443251600/16uH"/>
</technology>
<technology name="_744325180">
<attribute name="WE-NUMBER" value="744325180/1,8uH"/>
</technology>
<technology name="_744325240">
<attribute name="WE-NUMBER" value="744325240/2,4uH"/>
</technology>
<technology name="_744325330">
<attribute name="WE-NUMBER" value="744325330/3,3uH"/>
</technology>
<technology name="_744325420">
<attribute name="WE-NUMBER" value="744325420/4,2uH"/>
</technology>
<technology name="_744325550">
<attribute name="WE-NUMBER" value="744325550/5,5uH"/>
</technology>
<technology name="_744325650">
<attribute name="WE-NUMBER" value="744325650/6,5uH"/>
</technology>
<technology name="_744325780">
<attribute name="WE-NUMBER" value="744325780/7,8uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1335" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Flat wire coil for low losses at high frequency
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +150/155 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; Industrial computers
&lt;br&gt;
&lt;br&gt; Motherboards
&lt;br&gt;
&lt;br&gt; High current switching regulators
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Polyphase-switching regulators
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCI?"&gt;http://katalog.we-online.de/en/pbs/WE-HCI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1335">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744313025">
<attribute name="WE-NUMBER" value="744313025/0,25uH"/>
</technology>
<technology name="_744313068">
<attribute name="WE-NUMBER" value="744313068/0,68uH"/>
</technology>
<technology name="_744313120">
<attribute name="WE-NUMBER" value="744313120/1,2uH"/>
</technology>
<technology name="_744313180">
<attribute name="WE-NUMBER" value="744313180/1,8uH"/>
</technology>
<technology name="_744313220">
<attribute name="WE-NUMBER" value="744313220/2,2uH"/>
</technology>
<technology name="_744313330">
<attribute name="WE-NUMBER" value="7443133330/3,3uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1350" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Flat wire coil for low losses at high frequency
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +150/155 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; Industrial computers
&lt;br&gt;
&lt;br&gt; Motherboards
&lt;br&gt;
&lt;br&gt; High current switching regulators
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Polyphase-switching regulators
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCI?"&gt;http://katalog.we-online.de/en/pbs/WE-HCI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1350/1365">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443550101">
<attribute name="WE-NUMBER" value="7443550101/10uH"/>
</technology>
<technology name="_7443550140">
<attribute name="WE-NUMBER" value="7443550140/1,4uH"/>
</technology>
<technology name="_744355019">
<attribute name="WE-NUMBER" value="744355019/0,19uH"/>
</technology>
<technology name="_7443550230">
<attribute name="WE-NUMBER" value="7443550230/2,3uH"/>
</technology>
<technology name="_7443550320">
<attribute name="WE-NUMBER" value="7443550320/3,2uH"/>
</technology>
<technology name="_744355047">
<attribute name="WE-NUMBER" value="744355047/0,47uH"/>
</technology>
<technology name="_7443550480">
<attribute name="WE-NUMBER" value="7443550480/4,8uH"/>
</technology>
<technology name="_7443550600">
<attribute name="WE-NUMBER" value="7443550600/6uH"/>
</technology>
<technology name="_7443550820">
<attribute name="WE-NUMBER" value="7443550820/8,2uH"/>
</technology>
<technology name="_744355090">
<attribute name="WE-NUMBER" value="744355090/0,9uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1365" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Flat wire coil for low losses at high frequency
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +150/155 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; Industrial computers
&lt;br&gt;
&lt;br&gt; Motherboards
&lt;br&gt;
&lt;br&gt; High current switching regulators
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Polyphase-switching regulators
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCI?"&gt;http://katalog.we-online.de/en/pbs/WE-HCI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1350/1365">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443551111">
<attribute name="WE-NUMBER" value="7443551111/11,3uH"/>
</technology>
<technology name="_7443551130">
<attribute name="WE-NUMBER" value="7443551130/1,3uH"/>
</technology>
<technology name="_7443551131">
<attribute name="WE-NUMBER" value="7443551131/13uH"/>
</technology>
<technology name="_7443551151">
<attribute name="WE-NUMBER" value="7443551151/15,4uH"/>
</technology>
<technology name="_7443551181">
<attribute name="WE-NUMBER" value="7443551181/18uH"/>
</technology>
<technology name="_7443551200">
<attribute name="WE-NUMBER" value="7443551200/2uH"/>
</technology>
<technology name="_744355122">
<attribute name="WE-NUMBER" value="744355122/0,2uH"/>
</technology>
<technology name="_7443551221">
<attribute name="WE-NUMBER" value="7443551221/22uH"/>
</technology>
<technology name="_7443551280">
<attribute name="WE-NUMBER" value="7443551280/2,8uH"/>
</technology>
<technology name="_7443551331">
<attribute name="WE-NUMBER" value="7443551331/33uH"/>
</technology>
<technology name="_7443551370">
<attribute name="WE-NUMBER" value="7443551370/3,7uH"/>
</technology>
<technology name="_744355147">
<attribute name="WE-NUMBER" value="744355147/0,41uH"/>
</technology>
<technology name="_7443551470">
<attribute name="WE-NUMBER" value="7443551470/4,7uH"/>
</technology>
<technology name="_7443551600">
<attribute name="WE-NUMBER" value="7443551600/6uH"/>
</technology>
<technology name="_7443551730">
<attribute name="WE-NUMBER" value="7443551730/7,3uH"/>
</technology>
<technology name="_744355182">
<attribute name="WE-NUMBER" value="744355182/0,82uH"/>
</technology>
<technology name="_7443551920">
<attribute name="WE-NUMBER" value="7443551920/9,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_2212" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Flat wire coil for low losses at high frequency
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +150/155 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; Industrial computers
&lt;br&gt;
&lt;br&gt; Motherboards
&lt;br&gt;
&lt;br&gt; High current switching regulators
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Polyphase-switching regulators
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCI?"&gt;http://katalog.we-online.de/en/pbs/WE-HCI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_2212">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74435580330">
<attribute name="WE-NUMBER" value="74435580330/3,3uH"/>
</technology>
<technology name="_74435580680">
<attribute name="WE-NUMBER" value="74435580680/6,8uH"/>
</technology>
<technology name="_74435580820">
<attribute name="WE-NUMBER" value="74435580820/8,2uH"/>
</technology>
<technology name="_74435581000">
<attribute name="WE-NUMBER" value="74435581000/10uH"/>
</technology>
<technology name="_74435581200">
<attribute name="WE-NUMBER" value="74435581200/12uH"/>
</technology>
<technology name="_74435582200">
<attribute name="WE-NUMBER" value="74435582200/22uH"/>
</technology>
<technology name="_74435583300">
<attribute name="WE-NUMBER" value="74435583300/33uH"/>
</technology>
<technology name="_74435584700">
<attribute name="WE-NUMBER" value="74435584700/47uH"/>
</technology>
<technology name="_74435586800">
<attribute name="WE-NUMBER" value="74435586800/68uH"/>
</technology>
<technology name="_74435588200">
<attribute name="WE-NUMBER" value="74435588200/82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1890" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Flat wire coil for low losses at high frequency
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +150/155 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; Industrial computers
&lt;br&gt;
&lt;br&gt; Motherboards
&lt;br&gt;
&lt;br&gt; High current switching regulators
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Polyphase-switching regulators
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCI?"&gt;http://katalog.we-online.de/en/pbs/WE-HCI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1890">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443556082">
<attribute name="WE-NUMBER" value="7443556082/0,82uH"/>
</technology>
<technology name="_74435561100">
<attribute name="WE-NUMBER" value="74435561100/10uH"/>
</technology>
<technology name="_7443556130">
<attribute name="WE-NUMBER" value="7443556130/1,3uH"/>
</technology>
<technology name="_7443556190">
<attribute name="WE-NUMBER" value="7443556190/1,9uH"/>
</technology>
<technology name="_7443556260">
<attribute name="WE-NUMBER" value="7443556260/2,6uH"/>
</technology>
<technology name="_7443556350">
<attribute name="WE-NUMBER" value="7443556350/3,5uH"/>
</technology>
<technology name="_7443556450">
<attribute name="WE-NUMBER" value="7443556450/4,5uH"/>
</technology>
<technology name="_7443556560">
<attribute name="WE-NUMBER" value="7443556560/5,6uH"/>
</technology>
<technology name="_7443556680">
<attribute name="WE-NUMBER" value="7443556680/6,8uH"/>
</technology>
<technology name="_74435571100">
<attribute name="WE-NUMBER" value="74435571100/10uH"/>
</technology>
<technology name="_74435571500">
<attribute name="WE-NUMBER" value="74435571500/15uH"/>
</technology>
<technology name="_74435572200">
<attribute name="WE-NUMBER" value="74435572200/22uH"/>
</technology>
<technology name="_74435573300">
<attribute name="WE-NUMBER" value="74435573300/33uH"/>
</technology>
<technology name="_74435574700">
<attribute name="WE-NUMBER" value="74435574700/47uH"/>
</technology>
<technology name="_7443557560">
<attribute name="WE-NUMBER" value="7443557560/5,6uH"/>
</technology>
<technology name="_7443557760">
<attribute name="WE-NUMBER" value="7443557760/7,6uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_5040" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Flat wire coil for low losses at high frequency
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +150/155 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; Industrial computers
&lt;br&gt;
&lt;br&gt; Motherboards
&lt;br&gt;
&lt;br&gt; High current switching regulators
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Polyphase-switching regulators
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCI?"&gt;http://katalog.we-online.de/en/pbs/WE-HCI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_5040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744316022">
<attribute name="WE-NUMBER" value="744316022/0,22uH"/>
</technology>
<technology name="_744316033">
<attribute name="WE-NUMBER" value="744316033/0,33uH"/>
</technology>
<technology name="_744316047">
<attribute name="WE-NUMBER" value="744316047/0,47uH"/>
</technology>
<technology name="_744316068">
<attribute name="WE-NUMBER" value="744316068/0,68uH"/>
</technology>
<technology name="_744316100">
<attribute name="WE-NUMBER" value="744316100/1uH"/>
</technology>
<technology name="_744316150">
<attribute name="WE-NUMBER" value="744316150/1,5uH"/>
</technology>
<technology name="_744316220">
<attribute name="WE-NUMBER" value="744316220/2,2uH"/>
</technology>
<technology name="_744316330">
<attribute name="WE-NUMBER" value="744316330/3,3uH"/>
</technology>
<technology name="_744316470">
<attribute name="WE-NUMBER" value="744316470/4,7uH"/>
</technology>
<technology name="_744316560">
<attribute name="WE-NUMBER" value="7443166560/5,6uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_7030" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Flat wire coil for low losses at high frequency
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +150/155 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; Industrial computers
&lt;br&gt;
&lt;br&gt; Motherboards
&lt;br&gt;
&lt;br&gt; High current switching regulators
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Polyphase-switching regulators
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCI?"&gt;http://katalog.we-online.de/en/pbs/WE-HCI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_7030/7040/7050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744310013">
<attribute name="WE-NUMBER" value="744310013/0,13uH"/>
</technology>
<technology name="_744310024">
<attribute name="WE-NUMBER" value="744310024/0,24uH"/>
</technology>
<technology name="_744310055">
<attribute name="WE-NUMBER" value="744310055/0,52uH"/>
</technology>
<technology name="_744310095">
<attribute name="WE-NUMBER" value="744310095/0,95uH"/>
</technology>
<technology name="_744310115">
<attribute name="WE-NUMBER" value="744310115/1,15uH"/>
</technology>
<technology name="_744310150">
<attribute name="WE-NUMBER" value="744310150/1,5uH"/>
</technology>
<technology name="_744310200">
<attribute name="WE-NUMBER" value="744310200/2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_7040" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Flat Wire High Current Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Flat wire coil for low losses at high frequency
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +150/155 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; Industrial computers
&lt;br&gt;
&lt;br&gt; Motherboards
&lt;br&gt;
&lt;br&gt; High current switching regulators
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Polyphase-switching regulators
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCI?"&gt;http://katalog.we-online.de/en/pbs/WE-HCI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_7030/7040/7050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744311022">
<attribute name="WE-NUMBER" value="744311022/0,22uH"/>
</technology>
<technology name="_744311047">
<attribute name="WE-NUMBER" value="744311047/0,4uH"/>
</technology>
<technology name="_744311068">
<attribute name="WE-NUMBER" value="744311068/0,68uH"/>
</technology>
<technology name="_744311100">
<attribute name="WE-NUMBER" value="744311100/1uH"/>
</technology>
<technology name="_744311150">
<attribute name="WE-NUMBER" value="744311150/1,5uH"/>
</technology>
<technology name="_744311220">
<attribute name="WE-NUMBER" value="744311220/2,2uH"/>
</technology>
<technology name="_744311330">
<attribute name="WE-NUMBER" value="744311330/3,3uH"/>
</technology>
<technology name="_744311470">
<attribute name="WE-NUMBER" value="744311470/4,7uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_7050" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;
&lt;br&gt; High saturation current up to 81 A
&lt;br&gt;
&lt;br&gt; Extremly low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; RDC tolerance ± 7%
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;
&lt;br&gt; CPU/RAM power supply
&lt;br&gt;
&lt;br&gt; Power PC
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCM?"&gt;http://katalog.we-online.de/en/pbs/WE-HCM?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCM_7050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744302007">
<attribute name="WE-NUMBER" value="744302007/72nH"/>
</technology>
<technology name="_744302010">
<attribute name="WE-NUMBER" value="744302010/105nH"/>
</technology>
<technology name="_744302015">
<attribute name="WE-NUMBER" value="744302015/150nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1050" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;
&lt;br&gt; High saturation current up to 81 A
&lt;br&gt;
&lt;br&gt; Extremly low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; RDC tolerance ± 7%
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;
&lt;br&gt; CPU/RAM power supply
&lt;br&gt;
&lt;br&gt; Power PC
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCM?"&gt;http://katalog.we-online.de/en/pbs/WE-HCM?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCM_1050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744303012">
<attribute name="WE-NUMBER" value="744303012/120nH"/>
</technology>
<technology name="_744303015">
<attribute name="WE-NUMBER" value="744303015/155nH"/>
</technology>
<technology name="_744303022">
<attribute name="WE-NUMBER" value="744303022/220nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1052" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;
&lt;br&gt; High saturation current up to 81 A
&lt;br&gt;
&lt;br&gt; Extremly low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; RDC tolerance ± 7%
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;
&lt;br&gt; CPU/RAM power supply
&lt;br&gt;
&lt;br&gt; Power PC
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCM?"&gt;http://katalog.we-online.de/en/pbs/WE-HCM?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCM_1052">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744306020">
<attribute name="WE-NUMBER" value="744306020/200nH"/>
</technology>
<technology name="_744306025">
<attribute name="WE-NUMBER" value="744306025/250nH"/>
</technology>
<technology name="_744306030">
<attribute name="WE-NUMBER" value="744306030/300nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1070" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;
&lt;br&gt; High saturation current up to 81 A
&lt;br&gt;
&lt;br&gt; Extremly low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; RDC tolerance ± 7%
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;
&lt;br&gt; CPU/RAM power supply
&lt;br&gt;
&lt;br&gt; Power PC
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCM?"&gt;http://katalog.we-online.de/en/pbs/WE-HCM?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCM_1070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744308015">
<attribute name="WE-NUMBER" value="744308015/150nH"/>
</technology>
<technology name="_744308020">
<attribute name="WE-NUMBER" value="744308020/200nH"/>
</technology>
<technology name="_744308025">
<attribute name="WE-NUMBER" value="744308025/250nH"/>
</technology>
<technology name="_744308033">
<attribute name="WE-NUMBER" value="744308033/330nH"/>
</technology>
<technology name="_744308040">
<attribute name="WE-NUMBER" value="744308040/400nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1078" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;
&lt;br&gt; High saturation current up to 81 A
&lt;br&gt;
&lt;br&gt; Extremly low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; RDC tolerance ± 7%
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;
&lt;br&gt; CPU/RAM power supply
&lt;br&gt;
&lt;br&gt; Power PC
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCM?"&gt;http://katalog.we-online.de/en/pbs/WE-HCM?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCM_1078">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443081010">
<attribute name="WE-NUMBER" value="7443081010/100nH"/>
</technology>
<technology name="_7443081012">
<attribute name="WE-NUMBER" value="7443081012/120nH"/>
</technology>
<technology name="_7443081015">
<attribute name="WE-NUMBER" value="7443081015/150nH"/>
</technology>
<technology name="_7443081018">
<attribute name="WE-NUMBER" value="7443081018/180nH"/>
</technology>
<technology name="_7443081022">
<attribute name="WE-NUMBER" value="7443081022/220nH"/>
</technology>
<technology name="_7443081030">
<attribute name="WE-NUMBER" value="7443081030/300nH"/>
</technology>
<technology name="_7443081040">
<attribute name="WE-NUMBER" value="7443081040/400nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1190" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;
&lt;br&gt; High saturation current up to 81 A
&lt;br&gt;
&lt;br&gt; Extremly low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; RDC tolerance ± 7%
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;
&lt;br&gt; CPU/RAM power supply
&lt;br&gt;
&lt;br&gt; Power PC
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCM?"&gt;http://katalog.we-online.de/en/pbs/WE-HCM?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCM_1190">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744301025">
<attribute name="WE-NUMBER" value="744301025/250nH"/>
</technology>
<technology name="_744301033">
<attribute name="WE-NUMBER" value="744301033/330nH"/>
</technology>
<technology name="_744301047">
<attribute name="WE-NUMBER" value="744301047/470nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1240" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;
&lt;br&gt; High saturation current up to 81 A
&lt;br&gt;
&lt;br&gt; Extremly low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; RDC tolerance ± 7%
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;
&lt;br&gt; CPU/RAM power supply
&lt;br&gt;
&lt;br&gt; Power PC
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCM?"&gt;http://katalog.we-online.de/en/pbs/WE-HCM?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCM_1240">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744304010">
<attribute name="WE-NUMBER" value="744304010/100nH"/>
</technology>
<technology name="_744304016">
<attribute name="WE-NUMBER" value="744304016/160nH"/>
</technology>
<technology name="_744304022">
<attribute name="WE-NUMBER" value="744304022/220nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1350" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;
&lt;br&gt; High saturation current up to 81 A
&lt;br&gt;
&lt;br&gt; Extremly low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; RDC tolerance ± 7%
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;
&lt;br&gt; CPU/RAM power supply
&lt;br&gt;
&lt;br&gt; Power PC
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCM?"&gt;http://katalog.we-online.de/en/pbs/WE-HCM?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCM_1350">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744305022">
<attribute name="WE-NUMBER" value="744305022/220nH"/>
</technology>
<technology name="_744305033">
<attribute name="WE-NUMBER" value="744305033/330nH"/>
</technology>
<technology name="_744305040">
<attribute name="WE-NUMBER" value="744305040/400nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCM_1390" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Flat Wire Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Lowest core losses (MnZn)
&lt;br&gt;
&lt;br&gt; High saturation current up to 81 A
&lt;br&gt;
&lt;br&gt; Extremly low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; RDC tolerance ± 7%
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Multiphase switching regulator
&lt;br&gt;
&lt;br&gt; CPU/RAM power supply
&lt;br&gt;
&lt;br&gt; Power PC
&lt;br&gt;
&lt;br&gt; Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-HCM.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCM?"&gt;http://katalog.we-online.de/en/pbs/WE-HCM?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCM_1390">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744309012">
<attribute name="WE-NUMBER" value="744309012/120nH"/>
</technology>
<technology name="_744309025">
<attribute name="WE-NUMBER" value="744309025/250nH"/>
</technology>
<technology name="_744309033">
<attribute name="WE-NUMBER" value="744309033/330nH"/>
</technology>
<technology name="_744309047">
<attribute name="WE-NUMBER" value="744309047/470nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_1335" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Low Profile High Current Molded Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Handles high transient current spikes
&lt;br&gt;
&lt;br&gt; No acoustic noise and no leakage field
&lt;br&gt;
&lt;br&gt; Frequency range up to 5 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;Br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC converters for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital cameras
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LHMI?"&gt;http://katalog.we-online.de/en/pbs/WE-LHMI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LHMI_1335">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373770022">
<attribute name="WE-NUMBER" value="744373770022/0,22uH"/>
</technology>
<technology name="_744373770033">
<attribute name="WE-NUMBER" value="744373770033/0,33uH"/>
</technology>
<technology name="_744373770047">
<attribute name="WE-NUMBER" value="744373770047/0,47uH"/>
</technology>
<technology name="_744373770056">
<attribute name="WE-NUMBER" value="744373770056/0,56uH"/>
</technology>
<technology name="_744373770068">
<attribute name="WE-NUMBER" value="744373770068/0,68uH"/>
</technology>
<technology name="_74437377010">
<attribute name="WE-NUMBER" value="74437377010/1uH"/>
</technology>
<technology name="_74437377015">
<attribute name="WE-NUMBER" value="74437377015/1,5uH"/>
</technology>
<technology name="_74437377022">
<attribute name="WE-NUMBER" value="74437377022/2,2uH"/>
</technology>
<technology name="_74437377033">
<attribute name="WE-NUMBER" value="74437377033/3,3uH"/>
</technology>
<technology name="_74437377047">
<attribute name="WE-NUMBER" value="74437377047/0,47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_1365" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Low Profile High Current Molded Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Handles high transient current spikes
&lt;br&gt;
&lt;br&gt; No acoustic noise and no leakage field
&lt;br&gt;
&lt;br&gt; Frequency range up to 5 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;Br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC converters for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital cameras
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LHMI?"&gt;http://katalog.we-online.de/en/pbs/WE-LHMI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LHMI_1365">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443739650022">
<attribute name="WE-NUMBER" value="7443739650022/0,22uH"/>
</technology>
<technology name="_7443739650033">
<attribute name="WE-NUMBER" value="7443739650033/0,33uH"/>
</technology>
<technology name="_7443739650047">
<attribute name="WE-NUMBER" value="7443739650047/0,47uH"/>
</technology>
<technology name="_7443739650056">
<attribute name="WE-NUMBER" value="7443739650056/0,56uH"/>
</technology>
<technology name="_7443739650068">
<attribute name="WE-NUMBER" value="7443739650068/0,68uH"/>
</technology>
<technology name="_744373965010">
<attribute name="WE-NUMBER" value="744373965010/1uH"/>
</technology>
<technology name="_744373965015">
<attribute name="WE-NUMBER" value="744373965015/1,5uH"/>
</technology>
<technology name="_744373965022">
<attribute name="WE-NUMBER" value="744373965022/2,2uH"/>
</technology>
<technology name="_744373965033">
<attribute name="WE-NUMBER" value="744373965033/3,3uH"/>
</technology>
<technology name="_744373965047">
<attribute name="WE-NUMBER" value="744373965047/4,7uH"/>
</technology>
<technology name="_744373965068">
<attribute name="WE-NUMBER" value="744373965068/6,8uH"/>
</technology>
<technology name="_744373965100">
<attribute name="WE-NUMBER" value="744373965100/10uH"/>
</technology>
<technology name="_744373965101">
<attribute name="WE-NUMBER" value="744373965101/100uH"/>
</technology>
<technology name="_744373965120">
<attribute name="WE-NUMBER" value="744373965120/12uH"/>
</technology>
<technology name="_744373965150">
<attribute name="WE-NUMBER" value="744373965150/15uH"/>
</technology>
<technology name="_744373965220">
<attribute name="WE-NUMBER" value="744373965220/22uH"/>
</technology>
<technology name="_744373965330">
<attribute name="WE-NUMBER" value="744373965330/33uH"/>
</technology>
<technology name="_744373965470">
<attribute name="WE-NUMBER" value="744373965470/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_4012" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Low Profile High Current Molded Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Handles high transient current spikes
&lt;br&gt;
&lt;br&gt; No acoustic noise and no leakage field
&lt;br&gt;
&lt;br&gt; Frequency range up to 5 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;Br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC converters for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital cameras
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LHMI?"&gt;http://katalog.we-online.de/en/pbs/WE-LHMI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LHMI_4012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373210010">
<attribute name="WE-NUMBER" value="744373210010/1uH"/>
</technology>
<technology name="_744373210022">
<attribute name="WE-NUMBER" value="744373210022/0,22uH"/>
</technology>
<technology name="_744373210047">
<attribute name="WE-NUMBER" value="744373210047/0,47uH"/>
</technology>
<technology name="_74437321010">
<attribute name="WE-NUMBER" value="74437321010/0,1uH"/>
</technology>
<technology name="_74437321015">
<attribute name="WE-NUMBER" value="74437321015/1,5uH"/>
</technology>
<technology name="_74437321022">
<attribute name="WE-NUMBER" value="74437321022/2,2uH"/>
</technology>
<technology name="_74437321033">
<attribute name="WE-NUMBER" value="74437321033/3,3uH"/>
</technology>
<technology name="_74437321047">
<attribute name="WE-NUMBER" value="74437321047/4,7uH"/>
</technology>
<technology name="_74437321056">
<attribute name="WE-NUMBER" value="74437321056/5,6uH"/>
</technology>
<technology name="_74437321068">
<attribute name="WE-NUMBER" value="74437321068/6,8uH"/>
</technology>
<technology name="_74437321082">
<attribute name="WE-NUMBER" value="74437321082/8,2uH"/>
</technology>
<technology name="_74437321100">
<attribute name="WE-NUMBER" value="74437321100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_4020" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Low Profile High Current Molded Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Handles high transient current spikes
&lt;br&gt;
&lt;br&gt; No acoustic noise and no leakage field
&lt;br&gt;
&lt;br&gt; Frequency range up to 5 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;Br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC converters for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital cameras
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LHMI?"&gt;http://katalog.we-online.de/en/pbs/WE-LHMI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LHMI_4020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373240010">
<attribute name="WE-NUMBER" value="744373240010/0,1uH"/>
</technology>
<technology name="_744373240022">
<attribute name="WE-NUMBER" value="744373240022/0,22uH"/>
</technology>
<technology name="_744373240033">
<attribute name="WE-NUMBER" value="744373240033/0,33uH"/>
</technology>
<technology name="_744373240047">
<attribute name="WE-NUMBER" value="744373240047/0,47uH"/>
</technology>
<technology name="_744373240056">
<attribute name="WE-NUMBER" value="744373240056/0,56uH"/>
</technology>
<technology name="_744373240068">
<attribute name="WE-NUMBER" value="744373240068/0,68uH"/>
</technology>
<technology name="_74437324010">
<attribute name="WE-NUMBER" value="74437324010/1uH"/>
</technology>
<technology name="_74437324012">
<attribute name="WE-NUMBER" value="74437324012/1,2uH"/>
</technology>
<technology name="_74437324015">
<attribute name="WE-NUMBER" value="74437324015/1,5uH"/>
</technology>
<technology name="_74437324022">
<attribute name="WE-NUMBER" value="74437324022/2,2uH"/>
</technology>
<technology name="_74437324033">
<attribute name="WE-NUMBER" value="74437324033/3,3uH"/>
</technology>
<technology name="_74437324047">
<attribute name="WE-NUMBER" value="74437324047/4,7uH"/>
</technology>
<technology name="_74437324056">
<attribute name="WE-NUMBER" value="74437324056/5,6uH"/>
</technology>
<technology name="_74437324068">
<attribute name="WE-NUMBER" value="74437324068/6,8uH"/>
</technology>
<technology name="_74437324082">
<attribute name="WE-NUMBER" value="74437324082/8,2uH"/>
</technology>
<technology name="_74437324100">
<attribute name="WE-NUMBER" value="74437324100/10uH"/>
</technology>
<technology name="_74437324150">
<attribute name="WE-NUMBER" value="74437324150/15uH"/>
</technology>
<technology name="_74437324220">
<attribute name="WE-NUMBER" value="74437324220/22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_5020" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Low Profile High Current Molded Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Handles high transient current spikes
&lt;br&gt;
&lt;br&gt; No acoustic noise and no leakage field
&lt;br&gt;
&lt;br&gt; Frequency range up to 5 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;Br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC converters for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital cameras
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LHMI?"&gt;http://katalog.we-online.de/en/pbs/WE-LHMI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LHMI_5020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373340033">
<attribute name="WE-NUMBER" value="744373340033/0,33uH"/>
</technology>
<technology name="_744373340047">
<attribute name="WE-NUMBER" value="744373340047/0,47uH"/>
</technology>
<technology name="_744373340068">
<attribute name="WE-NUMBER" value="744373340068/0,68uH"/>
</technology>
<technology name="_74437334010">
<attribute name="WE-NUMBER" value="74437334010/1uH"/>
</technology>
<technology name="_74437334012">
<attribute name="WE-NUMBER" value="74437334012/1,2uH"/>
</technology>
<technology name="_74437334015">
<attribute name="WE-NUMBER" value="74437334015/1,5uH"/>
</technology>
<technology name="_74437334022">
<attribute name="WE-NUMBER" value="74437334022/2,2uH"/>
</technology>
<technology name="_74437334033">
<attribute name="WE-NUMBER" value="74437334033/3,3uH"/>
</technology>
<technology name="_74437334047">
<attribute name="WE-NUMBER" value="74437334047/4,7uH"/>
</technology>
<technology name="_74437334056">
<attribute name="WE-NUMBER" value="74437334056/5,6uH"/>
</technology>
<technology name="_74437334068">
<attribute name="WE-NUMBER" value="74437334068/6,8uH"/>
</technology>
<technology name="_74437334082">
<attribute name="WE-NUMBER" value="74437334082/8,2uH"/>
</technology>
<technology name="_74437334100">
<attribute name="WE-NUMBER" value="74437334100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_5030" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Low Profile High Current Molded Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Handles high transient current spikes
&lt;br&gt;
&lt;br&gt; No acoustic noise and no leakage field
&lt;br&gt;
&lt;br&gt; Frequency range up to 5 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;Br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC converters for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital cameras
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LHMI?"&gt;http://katalog.we-online.de/en/pbs/WE-LHMI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LHMI_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373360033">
<attribute name="WE-NUMBER" value="744373360033/0,33uH"/>
</technology>
<technology name="_744373360047">
<attribute name="WE-NUMBER" value="744373360047/0,47uH"/>
</technology>
<technology name="_744373360068">
<attribute name="WE-NUMBER" value="744373360068/0,68uH"/>
</technology>
<technology name="_74437336010">
<attribute name="WE-NUMBER" value="74437336010/1uH"/>
</technology>
<technology name="_74437336012">
<attribute name="WE-NUMBER" value="74437336012/1,2uH"/>
</technology>
<technology name="_74437336015">
<attribute name="WE-NUMBER" value="74437336015/1,5uH"/>
</technology>
<technology name="_74437336022">
<attribute name="WE-NUMBER" value="74437336022/2,2uH"/>
</technology>
<technology name="_74437336033">
<attribute name="WE-NUMBER" value="74437336033/3,3uH"/>
</technology>
<technology name="_74437336047">
<attribute name="WE-NUMBER" value="74437336047/4,7uH"/>
</technology>
<technology name="_74437336056">
<attribute name="WE-NUMBER" value="74437336056/5,6uH"/>
</technology>
<technology name="_74437336068">
<attribute name="WE-NUMBER" value="74437336068/6,8uH"/>
</technology>
<technology name="_74437336100">
<attribute name="WE-NUMBER" value="74437336100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_7030" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Low Profile High Current Molded Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Handles high transient current spikes
&lt;br&gt;
&lt;br&gt; No acoustic noise and no leakage field
&lt;br&gt;
&lt;br&gt; Frequency range up to 5 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;Br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC converters for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital cameras
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LHMI?"&gt;http://katalog.we-online.de/en/pbs/WE-LHMI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LHMI_7030/7050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373460022">
<attribute name="WE-NUMBER" value="744373460022/0,22uH"/>
</technology>
<technology name="_744373460033">
<attribute name="WE-NUMBER" value="744373460033/0,33uH"/>
</technology>
<technology name="_744373460047">
<attribute name="WE-NUMBER" value="744373460047/0,47uH"/>
</technology>
<technology name="_744373460068">
<attribute name="WE-NUMBER" value="744373460068/0,68uH"/>
</technology>
<technology name="_744373460082">
<attribute name="WE-NUMBER" value="744373460082/0,82uH"/>
</technology>
<technology name="_74437346010">
<attribute name="WE-NUMBER" value="74437346010/1uH"/>
</technology>
<technology name="_74437346015">
<attribute name="WE-NUMBER" value="74437346015/1,5uH"/>
</technology>
<technology name="_74437346018">
<attribute name="WE-NUMBER" value="74437346018/1,8uH"/>
</technology>
<technology name="_74437346022">
<attribute name="WE-NUMBER" value="74437346022/2,2uH"/>
</technology>
<technology name="_74437346025">
<attribute name="WE-NUMBER" value="74437346025/2,5uH"/>
</technology>
<technology name="_74437346033">
<attribute name="WE-NUMBER" value="74437346033/3,3uH"/>
</technology>
<technology name="_74437346047">
<attribute name="WE-NUMBER" value="74437346047/4,7uH"/>
</technology>
<technology name="_74437346056">
<attribute name="WE-NUMBER" value="74437346056/5,6uH"/>
</technology>
<technology name="_74437346068">
<attribute name="WE-NUMBER" value="74437346068/6,8uH"/>
</technology>
<technology name="_74437346082">
<attribute name="WE-NUMBER" value="74437346082/8,2uH"/>
</technology>
<technology name="_74437346100">
<attribute name="WE-NUMBER" value="74437346100/10uH"/>
</technology>
<technology name="_74437346220">
<attribute name="WE-NUMBER" value="74437346220/22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_7050" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Low Profile High Current Molded Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Handles high transient current spikes
&lt;br&gt;
&lt;br&gt; No acoustic noise and no leakage field
&lt;br&gt;
&lt;br&gt; Frequency range up to 5 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;Br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC converters for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital cameras
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LHMI?"&gt;http://katalog.we-online.de/en/pbs/WE-LHMI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LHMI_7030/7050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373490047">
<attribute name="WE-NUMBER" value="744373490047/0,47uH"/>
</technology>
<technology name="_744373490056">
<attribute name="WE-NUMBER" value="744373490056/0,56uH"/>
</technology>
<technology name="_744373490068">
<attribute name="WE-NUMBER" value="744373490068/6,8uH"/>
</technology>
<technology name="_744373490082">
<attribute name="WE-NUMBER" value="744373490082/0,82uH"/>
</technology>
<technology name="_74437349010">
<attribute name="WE-NUMBER" value="74437349010/1uH"/>
</technology>
<technology name="_74437349012">
<attribute name="WE-NUMBER" value="74437349012/1,2uH"/>
</technology>
<technology name="_74437349015">
<attribute name="WE-NUMBER" value="74437349015/1,5uH"/>
</technology>
<technology name="_74437349022">
<attribute name="WE-NUMBER" value="74437349022/2,2uH"/>
</technology>
<technology name="_74437349033">
<attribute name="WE-NUMBER" value="74437349033/3,3uH"/>
</technology>
<technology name="_74437349047">
<attribute name="WE-NUMBER" value="74437349047/4,7uH"/>
</technology>
<technology name="_74437349056">
<attribute name="WE-NUMBER" value="74437349056/5,6uH"/>
</technology>
<technology name="_74437349068">
<attribute name="WE-NUMBER" value="74437349068/6,8uH"/>
</technology>
<technology name="_74437349082">
<attribute name="WE-NUMBER" value="74437349082/8,2uH"/>
</technology>
<technology name="_74437349100">
<attribute name="WE-NUMBER" value="74437349100/10uH"/>
</technology>
<technology name="_74437349150">
<attribute name="WE-NUMBER" value="74437349150/15uH"/>
</technology>
<technology name="_74437349220">
<attribute name="WE-NUMBER" value="74437349220/22uH"/>
</technology>
<technology name="_74437349330">
<attribute name="WE-NUMBER" value="74437349330/33uH"/>
</technology>
<technology name="_74437349470">
<attribute name="WE-NUMBER" value="74437349470/47uH"/>
</technology>
<technology name="_74437349560">
<attribute name="WE-NUMBER" value="74437349560/56uH"/>
</technology>
<technology name="_74437349680">
<attribute name="WE-NUMBER" value="74437349680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_8030" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Low Profile High Current Molded Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Handles high transient current spikes
&lt;br&gt;
&lt;br&gt; No acoustic noise and no leakage field
&lt;br&gt;
&lt;br&gt; Frequency range up to 5 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;Br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC converters for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital cameras
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LHMI?"&gt;http://katalog.we-online.de/en/pbs/WE-LHMI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LHMI_8030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373560022">
<attribute name="WE-NUMBER" value="744373560022/0,22uH"/>
</technology>
<technology name="_744373560033">
<attribute name="WE-NUMBER" value="744373560033/0,33uH"/>
</technology>
<technology name="_744373560047">
<attribute name="WE-NUMBER" value="744373560047/0,47uH"/>
</technology>
<technology name="_744373560068">
<attribute name="WE-NUMBER" value="744373560068/0,68uH"/>
</technology>
<technology name="_744373560082">
<attribute name="WE-NUMBER" value="744373560082/0,82uH"/>
</technology>
<technology name="_74437356010">
<attribute name="WE-NUMBER" value="74437356010/1uH"/>
</technology>
<technology name="_74437356015">
<attribute name="WE-NUMBER" value="74437356015/1,5uH"/>
</technology>
<technology name="_74437356022">
<attribute name="WE-NUMBER" value="74437356022/2,2uH"/>
</technology>
<technology name="_74437356033">
<attribute name="WE-NUMBER" value="74437356033/3,3uH"/>
</technology>
<technology name="_74437356047">
<attribute name="WE-NUMBER" value="74437356047/4,7uH"/>
</technology>
<technology name="_74437356068">
<attribute name="WE-NUMBER" value="74437356068/6,8uH"/>
</technology>
<technology name="_74437356082">
<attribute name="WE-NUMBER" value="74437356082/8,2uH"/>
</technology>
<technology name="_74437356100">
<attribute name="WE-NUMBER" value="74437356100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LHMI_8040" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Low Profile High Current Molded Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Handles high transient current spikes
&lt;br&gt;
&lt;br&gt; No acoustic noise and no leakage field
&lt;br&gt;
&lt;br&gt; Frequency range up to 5 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;Br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC converters for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital cameras
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LHMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LHMI?"&gt;http://katalog.we-online.de/en/pbs/WE-LHMI?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LHMI_8040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744373580022">
<attribute name="WE-NUMBER" value="744373580022/0,22uH"/>
</technology>
<technology name="_744373580033">
<attribute name="WE-NUMBER" value="744373580033/0,33uH"/>
</technology>
<technology name="_744373580047">
<attribute name="WE-NUMBER" value="744373580047/0,47uH"/>
</technology>
<technology name="_744373580068">
<attribute name="WE-NUMBER" value="744373580068/0,68uH"/>
</technology>
<technology name="_744373580082">
<attribute name="WE-NUMBER" value="744373580082/0,82uH"/>
</technology>
<technology name="_74437358010">
<attribute name="WE-NUMBER" value="74437358010/1uH"/>
</technology>
<technology name="_74437358022">
<attribute name="WE-NUMBER" value="74437358022/2,2uH"/>
</technology>
<technology name="_74437358033">
<attribute name="WE-NUMBER" value="74437358033/3,3uH"/>
</technology>
<technology name="_74437358047">
<attribute name="WE-NUMBER" value="74437358047/4,7uH"/>
</technology>
<technology name="_74437358068">
<attribute name="WE-NUMBER" value="74437358068/6,8uH"/>
</technology>
<technology name="_74437358082">
<attribute name="WE-NUMBER" value="74437358082/8,2uH"/>
</technology>
<technology name="_74437358100">
<attribute name="WE-NUMBER" value="74437358100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQ_1210" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Miniature chip inductor wound on a special ferrite core
&lt;br&gt;
&lt;br&gt; Small inductances for compact circuits
&lt;br&gt;
&lt;br&gt; High Q at high frequencies
&lt;br&gt;
&lt;br&gt; Low DC-resistance
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;  Low power DC/DC-converters from Linear Technology, National Semiconductor, Texas Instruments, Fairchild Semiconductor, ON Semiconductor, STMicroelectronics, Maxim, MPS, Semtech, Exar, Analogic Tech, Diodes and Cologne Chip
&lt;br&gt;
&lt;br&gt; EMI-Filtering
&lt;br&gt;
&lt;br&gt; RF-circuits
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndLQ_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndLQ_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQ?"&gt;http://katalog.we-online.de/en/pbs/WE-LQ?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQ_M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744032001">
<attribute name="WE-NUMBER" value="744032001/1uH"/>
</technology>
<technology name="_7440320015">
<attribute name="WE-NUMBER" value="7440320015/1,5uH"/>
</technology>
<technology name="_7440320018">
<attribute name="WE-NUMBER" value="7440320018/1,8uH"/>
</technology>
<technology name="_744032002">
<attribute name="WE-NUMBER" value="744032002/2,2uH"/>
</technology>
<technology name="_7440320027">
<attribute name="WE-NUMBER" value="7440320027/2,7uH"/>
</technology>
<technology name="_744032003">
<attribute name="WE-NUMBER" value="744032003/3,3uH"/>
</technology>
<technology name="_7440320039">
<attribute name="WE-NUMBER" value="7440320039/3,9uH"/>
</technology>
<technology name="_744032004">
<attribute name="WE-NUMBER" value="744032004/4,7uH"/>
</technology>
<technology name="_7440320056">
<attribute name="WE-NUMBER" value="7440320056/5,6uH"/>
</technology>
<technology name="_744032006">
<attribute name="WE-NUMBER" value="744032006/6,8uH"/>
</technology>
<technology name="_744032008">
<attribute name="WE-NUMBER" value="744032008/8,2uH"/>
</technology>
<technology name="_744032100">
<attribute name="WE-NUMBER" value="744032100/10uH"/>
</technology>
<technology name="_744032101">
<attribute name="WE-NUMBER" value="744032101/100uH"/>
</technology>
<technology name="_744032120">
<attribute name="WE-NUMBER" value="744032120/12uH"/>
</technology>
<technology name="_744032121">
<attribute name="WE-NUMBER" value="744032121/120uH"/>
</technology>
<technology name="_744032150">
<attribute name="WE-NUMBER" value="744032150/15uH"/>
</technology>
<technology name="_744032180">
<attribute name="WE-NUMBER" value="744032180/18uH"/>
</technology>
<technology name="_744032220">
<attribute name="WE-NUMBER" value="744032220/22uH"/>
</technology>
<technology name="_744032221">
<attribute name="WE-NUMBER" value="744032221/220uH"/>
</technology>
<technology name="_744032331">
<attribute name="WE-NUMBER" value="744032331/330uH"/>
</technology>
<technology name="_744032471">
<attribute name="WE-NUMBER" value="744032471/470uH"/>
</technology>
<technology name="_744032680">
<attribute name="WE-NUMBER" value="744032680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQFS_3818" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-LQFS SMD Semishielded Tiny Power Inductor&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LQFS_3818-4828.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LQFS_3818-4828.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQFS"&gt;http://katalog.we-online.de/en/pbs/WE-LQFS&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQFS_3818">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74406032010">
<attribute name="WE-NUMBER" value="74406032010/1uH"/>
</technology>
<technology name="_74406032015">
<attribute name="WE-NUMBER" value="74406032015/1,5uH"/>
</technology>
<technology name="_74406032033">
<attribute name="WE-NUMBER" value="74406032033/3,3uH"/>
</technology>
<technology name="_74406032047">
<attribute name="WE-NUMBER" value="74406032047/4,7uH"/>
</technology>
<technology name="_74406032068">
<attribute name="WE-NUMBER" value="744060032068/6,8uH"/>
</technology>
<technology name="_74406032100">
<attribute name="WE-NUMBER" value="74406032100/10uH"/>
</technology>
<technology name="_74406032101">
<attribute name="WE-NUMBER" value="74406032101/100uH"/>
</technology>
<technology name="_74406032220">
<attribute name="WE-NUMBER" value="74406032220/22uH"/>
</technology>
<technology name="_74406032330">
<attribute name="WE-NUMBER" value="74406032330/33uH"/>
</technology>
<technology name="_74406032470">
<attribute name="WE-NUMBER" value="74406032470/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQFS_4818" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-LQFS SMD Semishielded Tiny Power Inductor&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LQFS_3818-4828.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LQFS_3818-4828.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQFS"&gt;http://katalog.we-online.de/en/pbs/WE-LQFS&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQFS_48X8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74406042010">
<attribute name="WE-NUMBER" value="74406042010/1uH"/>
</technology>
<technology name="_74406042015">
<attribute name="WE-NUMBER" value="74406042015/1,5uH"/>
</technology>
<technology name="_74406042022">
<attribute name="WE-NUMBER" value="74406042022/2,2uH"/>
</technology>
<technology name="_74406042033">
<attribute name="WE-NUMBER" value="74406042033/3,3uH"/>
</technology>
<technology name="_74406042047">
<attribute name="WE-NUMBER" value="74406042047/4,7uH"/>
</technology>
<technology name="_74406042068">
<attribute name="WE-NUMBER" value="74406042068/6,8uH"/>
</technology>
<technology name="_74406042100">
<attribute name="WE-NUMBER" value="74406042100/10uH"/>
</technology>
<technology name="_74406042101">
<attribute name="WE-NUMBER" value="74406042101/100uH"/>
</technology>
<technology name="_74406042220">
<attribute name="WE-NUMBER" value="74406042220/22uH"/>
</technology>
<technology name="_74406042330">
<attribute name="WE-NUMBER" value="74406042330/33uH"/>
</technology>
<technology name="_74406042470">
<attribute name="WE-NUMBER" value="74406042470/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQS_2010" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Tiny Power Inductor design
&lt;br&gt;
&lt;br&gt; 1.7 times more current in comparison with unshielded versions
&lt;br&gt;
&lt;br&gt; Robust design &amp; high durability
&lt;br&gt;
&lt;br&gt; Low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded with magnetic glue reducing buzz noise in ultra-low levels
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC Converters
&lt;br&gt;
&lt;br&gt; Switching controllers which required high efficiency
&lt;br&gt;
&lt;br&gt; Portable power (Smartphones, digital cameras, Tablets, etc.)
&lt;br&gt;
&lt;br&gt; Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt; Big sizes (5040, 60xx, 8040) used for shock-proof circuits
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndLQS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndLQS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQS"&gt;http://katalog.we-online.de/en/pbs/WE-LQS&lt;/a&gt;&lt;p&gt;


Created  by  Dan Xu 2014-05-21&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQS_2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744040200016">
<attribute name="WE-NUMBER" value="744040200016/0,16uH"/>
</technology>
<technology name="_744040200033">
<attribute name="WE-NUMBER" value="744040200033/0,33uH"/>
</technology>
<technology name="_744040200047">
<attribute name="WE-NUMBER" value="744040200047/0,47uH"/>
</technology>
<technology name="_744040200068">
<attribute name="WE-NUMBER" value="744040200068/0,68uH"/>
</technology>
<technology name="_74404020010">
<attribute name="WE-NUMBER" value="74404020010/1uH"/>
</technology>
<technology name="_74404020015">
<attribute name="WE-NUMBER" value="74404020015/1,5uH"/>
</technology>
<technology name="_74404020022">
<attribute name="WE-NUMBER" value="74404020022/2,2uH"/>
</technology>
<technology name="_74404020033">
<attribute name="WE-NUMBER" value="744040200033/0,33uH"/>
</technology>
<technology name="_74404020047">
<attribute name="WE-NUMBER" value="74404020047/0,47uH"/>
</technology>
<technology name="_74404020068">
<attribute name="WE-NUMBER" value="74404020068/6,8uH"/>
</technology>
<technology name="_74404020100">
<attribute name="WE-NUMBER" value="74404020100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQS_2512" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Tiny Power Inductor design
&lt;br&gt;
&lt;br&gt; 1.7 times more current in comparison with unshielded versions
&lt;br&gt;
&lt;br&gt; Robust design &amp; high durability
&lt;br&gt;
&lt;br&gt; Low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded with magnetic glue reducing buzz noise in ultra-low levels
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC Converters
&lt;br&gt;
&lt;br&gt; Switching controllers which required high efficiency
&lt;br&gt;
&lt;br&gt; Portable power (Smartphones, digital cameras, Tablets, etc.)
&lt;br&gt;
&lt;br&gt; Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt; Big sizes (5040, 60xx, 8040) used for shock-proof circuits
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndLQS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndLQS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQS"&gt;http://katalog.we-online.de/en/pbs/WE-LQS&lt;/a&gt;&lt;p&gt;


Created  by  Dan Xu 2014-05-21&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQS_2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744040240016">
<attribute name="WE-NUMBER" value="744040240016/0,16uH"/>
</technology>
<technology name="_744040240047">
<attribute name="WE-NUMBER" value="744040240047/0,47uH"/>
</technology>
<technology name="_744040240068">
<attribute name="WE-NUMBER" value="744040240068/0,68uH"/>
</technology>
<technology name="_74404024010">
<attribute name="WE-NUMBER" value="74404024010/1uH"/>
</technology>
<technology name="_74404024015">
<attribute name="WE-NUMBER" value="74404024015/1,5uH"/>
</technology>
<technology name="_74404024022">
<attribute name="WE-NUMBER" value="74404024022/2,2uH"/>
</technology>
<technology name="_74404024033">
<attribute name="WE-NUMBER" value="74404024033/3,3uH"/>
</technology>
<technology name="_74404024047">
<attribute name="WE-NUMBER" value="74404024047/4,7uH"/>
</technology>
<technology name="_74404024068">
<attribute name="WE-NUMBER" value="74404024068/6,8uH"/>
</technology>
<technology name="_74404024100">
<attribute name="WE-NUMBER" value="74404024100/10uH"/>
</technology>
<technology name="_74404024150">
<attribute name="WE-NUMBER" value="74404024150/15uH"/>
</technology>
<technology name="_74404024180">
<attribute name="WE-NUMBER" value="74404024180/18uH"/>
</technology>
<technology name="_74404024220">
<attribute name="WE-NUMBER" value="74404024220/22uH"/>
</technology>
<technology name="_74404024330">
<attribute name="WE-NUMBER" value="74404024330/33uH"/>
</technology>
<technology name="_74404024470">
<attribute name="WE-NUMBER" value="74404024470/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQS_3012" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Tiny Power Inductor design
&lt;br&gt;
&lt;br&gt; 1.7 times more current in comparison with unshielded versions
&lt;br&gt;
&lt;br&gt; Robust design &amp; high durability
&lt;br&gt;
&lt;br&gt; Low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded with magnetic glue reducing buzz noise in ultra-low levels
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC Converters
&lt;br&gt;
&lt;br&gt; Switching controllers which required high efficiency
&lt;br&gt;
&lt;br&gt; Portable power (Smartphones, digital cameras, Tablets, etc.)
&lt;br&gt;
&lt;br&gt; Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt; Big sizes (5040, 60xx, 8040) used for shock-proof circuits
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndLQS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndLQS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQS"&gt;http://katalog.we-online.de/en/pbs/WE-LQS&lt;/a&gt;&lt;p&gt;


Created  by  Dan Xu 2014-05-21&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQS_3012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74404031010A">
<attribute name="WE-NUMBER" value="74404031010A"/>
</technology>
<technology name="_74404031027A">
<attribute name="WE-NUMBER" value="74404031027A/2,7uH"/>
</technology>
<technology name="_74404031047A">
<attribute name="WE-NUMBER" value="74404031047A/4,7uH"/>
</technology>
<technology name="_74404031068A">
<attribute name="WE-NUMBER" value="74404031068A/6,8uH"/>
</technology>
<technology name="_74404031100A">
<attribute name="WE-NUMBER" value="74404031100A/10uH"/>
</technology>
<technology name="_74404031150A">
<attribute name="WE-NUMBER" value="74404031150A/15uH"/>
</technology>
<technology name="_74404031220A">
<attribute name="WE-NUMBER" value="74404031220A/22uH"/>
</technology>
<technology name="_74404031330A">
<attribute name="WE-NUMBER" value="74404031330A/33uH"/>
</technology>
<technology name="_74404031470A">
<attribute name="WE-NUMBER" value="74404031470A/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQS_3015" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Tiny Power Inductor design
&lt;br&gt;
&lt;br&gt; 1.7 times more current in comparison with unshielded versions
&lt;br&gt;
&lt;br&gt; Robust design &amp; high durability
&lt;br&gt;
&lt;br&gt; Low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded with magnetic glue reducing buzz noise in ultra-low levels
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC Converters
&lt;br&gt;
&lt;br&gt; Switching controllers which required high efficiency
&lt;br&gt;
&lt;br&gt; Portable power (Smartphones, digital cameras, Tablets, etc.)
&lt;br&gt;
&lt;br&gt; Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt; Big sizes (5040, 60xx, 8040) used for shock-proof circuits
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndLQS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndLQS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQS"&gt;http://katalog.we-online.de/en/pbs/WE-LQS&lt;/a&gt;&lt;p&gt;


Created  by  Dan Xu 2014-05-21&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQS_3015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744040320047">
<attribute name="WE-NUMBER" value="744040320047/0,47uH"/>
</technology>
<technology name="_74404032010">
<attribute name="WE-NUMBER" value="74404032010/1uH"/>
</technology>
<technology name="_74404032015">
<attribute name="WE-NUMBER" value="74404032015/1,5uH"/>
</technology>
<technology name="_74404032022">
<attribute name="WE-NUMBER" value="74404032022/2,2uH"/>
</technology>
<technology name="_74404032033">
<attribute name="WE-NUMBER" value="74404032033/3,3uH"/>
</technology>
<technology name="_74404032047">
<attribute name="WE-NUMBER" value="74404032047/4,7uH"/>
</technology>
<technology name="_74404032068">
<attribute name="WE-NUMBER" value="74404032068/6,8uH"/>
</technology>
<technology name="_74404032100">
<attribute name="WE-NUMBER" value="74404032100/10uH"/>
</technology>
<technology name="_74404032150">
<attribute name="WE-NUMBER" value="74404032150/15uH"/>
</technology>
<technology name="_74404032220">
<attribute name="WE-NUMBER" value="74404032220/22uH"/>
</technology>
<technology name="_74404032330">
<attribute name="WE-NUMBER" value="74404032330/33uH"/>
</technology>
<technology name="_74404032470">
<attribute name="WE-NUMBER" value="74404032470/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQS_4012" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Tiny Power Inductor design
&lt;br&gt;
&lt;br&gt; 1.7 times more current in comparison with unshielded versions
&lt;br&gt;
&lt;br&gt; Robust design &amp; high durability
&lt;br&gt;
&lt;br&gt; Low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded with magnetic glue reducing buzz noise in ultra-low levels
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC Converters
&lt;br&gt;
&lt;br&gt; Switching controllers which required high efficiency
&lt;br&gt;
&lt;br&gt; Portable power (Smartphones, digital cameras, Tablets, etc.)
&lt;br&gt;
&lt;br&gt; Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt; Big sizes (5040, 60xx, 8040) used for shock-proof circuits
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndLQS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndLQS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQS"&gt;http://katalog.we-online.de/en/pbs/WE-LQS&lt;/a&gt;&lt;p&gt;


Created  by  Dan Xu 2014-05-21&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQS_4012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744040410047">
<attribute name="WE-NUMBER" value="744040410047/0,47uH"/>
</technology>
<technology name="_74404041010">
<attribute name="WE-NUMBER" value="74404041010/1uH"/>
</technology>
<technology name="_74404041033">
<attribute name="WE-NUMBER" value="74404041033/3,3uH"/>
</technology>
<technology name="_74404041047">
<attribute name="WE-NUMBER" value="74404041047/0,47uH"/>
</technology>
<technology name="_74404041100">
<attribute name="WE-NUMBER" value="74401041100/10uH"/>
</technology>
<technology name="_74404041101">
<attribute name="WE-NUMBER" value="74404041101/100uH"/>
</technology>
<technology name="_74404041330">
<attribute name="WE-NUMBER" value="74404041330/33uH"/>
</technology>
<technology name="_74404041470">
<attribute name="WE-NUMBER" value="74404041470/47uH"/>
</technology>
<technology name="_74404041680">
<attribute name="WE-NUMBER" value="74404041680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQS_4018" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Tiny Power Inductor design
&lt;br&gt;
&lt;br&gt; 1.7 times more current in comparison with unshielded versions
&lt;br&gt;
&lt;br&gt; Robust design &amp; high durability
&lt;br&gt;
&lt;br&gt; Low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded with magnetic glue reducing buzz noise in ultra-low levels
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC Converters
&lt;br&gt;
&lt;br&gt; Switching controllers which required high efficiency
&lt;br&gt;
&lt;br&gt; Portable power (Smartphones, digital cameras, Tablets, etc.)
&lt;br&gt;
&lt;br&gt; Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt; Big sizes (5040, 60xx, 8040) used for shock-proof circuits
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndLQS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndLQS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQS"&gt;http://katalog.we-online.de/en/pbs/WE-LQS&lt;/a&gt;&lt;p&gt;


Created  by  Dan Xu 2014-05-21&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQS_4018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744040420033">
<attribute name="WE-NUMBER" value="744040420033/0,33uH"/>
</technology>
<technology name="_74404042010">
<attribute name="WE-NUMBER" value="74404042010/1uH"/>
</technology>
<technology name="_74404042015">
<attribute name="WE-NUMBER" value="74404042015/1,5uH"/>
</technology>
<technology name="_74404042022">
<attribute name="WE-NUMBER" value="74404042022/2,2uH"/>
</technology>
<technology name="_74404042033">
<attribute name="WE-NUMBER" value="74404042033/3,3uH"/>
</technology>
<technology name="_74404042047">
<attribute name="WE-NUMBER" value="74404042047/4,7uH"/>
</technology>
<technology name="_74404042068">
<attribute name="WE-NUMBER" value="74404042068/6,8uH"/>
</technology>
<technology name="_74404042100">
<attribute name="WE-NUMBER" value="74404042100/10uH"/>
</technology>
<technology name="_74404042101">
<attribute name="WE-NUMBER" value="74404042101/100uH"/>
</technology>
<technology name="_74404042150">
<attribute name="WE-NUMBER" value="74404042150/1,5uH"/>
</technology>
<technology name="_74404042151">
<attribute name="WE-NUMBER" value="74404042151/150uH"/>
</technology>
<technology name="_74404042220">
<attribute name="WE-NUMBER" value="74404042220/22uH"/>
</technology>
<technology name="_74404042221">
<attribute name="WE-NUMBER" value="74404042221/220uH"/>
</technology>
<technology name="_74404042330">
<attribute name="WE-NUMBER" value="74404042330/33uH"/>
</technology>
<technology name="_74404042331">
<attribute name="WE-NUMBER" value="7440404233/330uH"/>
</technology>
<technology name="_74404042470">
<attribute name="WE-NUMBER" value="74404042470/47uH"/>
</technology>
<technology name="_74404042680">
<attribute name="WE-NUMBER" value="74404042680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQS_4025" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Tiny Power Inductor design
&lt;br&gt;
&lt;br&gt; 1.7 times more current in comparison with unshielded versions
&lt;br&gt;
&lt;br&gt; Robust design &amp; high durability
&lt;br&gt;
&lt;br&gt; Low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded with magnetic glue reducing buzz noise in ultra-low levels
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC Converters
&lt;br&gt;
&lt;br&gt; Switching controllers which required high efficiency
&lt;br&gt;
&lt;br&gt; Portable power (Smartphones, digital cameras, Tablets, etc.)
&lt;br&gt;
&lt;br&gt; Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt; Big sizes (5040, 60xx, 8040) used for shock-proof circuits
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndLQS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndLQS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQS"&gt;http://katalog.we-online.de/en/pbs/WE-LQS&lt;/a&gt;&lt;p&gt;


Created  by  Dan Xu 2014-05-21&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQS_4025">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74404043010A">
<attribute name="WE-NUMBER" value="74404043010A/1uH"/>
</technology>
<technology name="_74404043022A">
<attribute name="WE-NUMBER" value="74404043022A/2,2uH"/>
</technology>
<technology name="_74404043033A">
<attribute name="WE-NUMBER" value="74404043033A/3,3uH"/>
</technology>
<technology name="_74404043047A">
<attribute name="WE-NUMBER" value="74404043047/4,7uH"/>
</technology>
<technology name="_74404043100A">
<attribute name="WE-NUMBER" value="74404043100A/10uH"/>
</technology>
<technology name="_74404043101A">
<attribute name="WE-NUMBER" value="74404043101A/100uH"/>
</technology>
<technology name="_74404043102A">
<attribute name="WE-NUMBER" value="74404043102A/1000uH"/>
</technology>
<technology name="_74404043150A">
<attribute name="WE-NUMBER" value="74404043150A/15uH"/>
</technology>
<technology name="_74404043151A">
<attribute name="WE-NUMBER" value="74404043151A/150uH"/>
</technology>
<technology name="_74404043220A">
<attribute name="WE-NUMBER" value="74404043220A/22uH"/>
</technology>
<technology name="_74404043221A">
<attribute name="WE-NUMBER" value="74404043221A/220uH"/>
</technology>
<technology name="_74404043330A">
<attribute name="WE-NUMBER" value="74404043330A/33uH"/>
</technology>
<technology name="_74404043470A">
<attribute name="WE-NUMBER" value="74404043470A/47uH"/>
</technology>
<technology name="_74404043471A">
<attribute name="WE-NUMBER" value="74404043471A/470uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQS_5020" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Tiny Power Inductor design
&lt;br&gt;
&lt;br&gt; 1.7 times more current in comparison with unshielded versions
&lt;br&gt;
&lt;br&gt; Robust design &amp; high durability
&lt;br&gt;
&lt;br&gt; Low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded with magnetic glue reducing buzz noise in ultra-low levels
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC Converters
&lt;br&gt;
&lt;br&gt; Switching controllers which required high efficiency
&lt;br&gt;
&lt;br&gt; Portable power (Smartphones, digital cameras, Tablets, etc.)
&lt;br&gt;
&lt;br&gt; Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt; Big sizes (5040, 60xx, 8040) used for shock-proof circuits
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndLQS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndLQS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQS"&gt;http://katalog.we-online.de/en/pbs/WE-LQS&lt;/a&gt;&lt;p&gt;


Created  by  Dan Xu 2014-05-21&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQS_5020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744040520047">
<attribute name="WE-NUMBER" value="744040520047/0,47uH"/>
</technology>
<technology name="_74404052010">
<attribute name="WE-NUMBER" value="74404052010/1uH"/>
</technology>
<technology name="_74404052012">
<attribute name="WE-NUMBER" value="74404052012/1,2uH"/>
</technology>
<technology name="_74404052015">
<attribute name="WE-NUMBER" value="74404052015/1,5uH"/>
</technology>
<technology name="_74404052022">
<attribute name="WE-NUMBER" value="74404052022/2,2uH"/>
</technology>
<technology name="_74404052033">
<attribute name="WE-NUMBER" value="74404052033/3,3uH"/>
</technology>
<technology name="_74404052039">
<attribute name="WE-NUMBER" value="74404052039/3,9uH"/>
</technology>
<technology name="_74404052047">
<attribute name="WE-NUMBER" value="74404052047/4,7uH"/>
</technology>
<technology name="_74404052056">
<attribute name="WE-NUMBER" value="74404052056/5,6uH"/>
</technology>
<technology name="_74404052068">
<attribute name="WE-NUMBER" value="74404052068/6,8uH"/>
</technology>
<technology name="_74404052075">
<attribute name="WE-NUMBER" value="74404042075/7,5uH"/>
</technology>
<technology name="_74404052100">
<attribute name="WE-NUMBER" value="74404052100/10uH"/>
</technology>
<technology name="_74404052101">
<attribute name="WE-NUMBER" value="74404052101/100uH"/>
</technology>
<technology name="_74404052220">
<attribute name="WE-NUMBER" value="74404052220/22uH"/>
</technology>
<technology name="_74404052330">
<attribute name="WE-NUMBER" value="74404052330/33uH"/>
</technology>
<technology name="_74404052470">
<attribute name="WE-NUMBER" value="74404052470/47uH"/>
</technology>
<technology name="_74404052680">
<attribute name="WE-NUMBER" value="74404052680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQS_5040" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Tiny Power Inductor design
&lt;br&gt;
&lt;br&gt; 1.7 times more current in comparison with unshielded versions
&lt;br&gt;
&lt;br&gt; Robust design &amp; high durability
&lt;br&gt;
&lt;br&gt; Low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded with magnetic glue reducing buzz noise in ultra-low levels
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC Converters
&lt;br&gt;
&lt;br&gt; Switching controllers which required high efficiency
&lt;br&gt;
&lt;br&gt; Portable power (Smartphones, digital cameras, Tablets, etc.)
&lt;br&gt;
&lt;br&gt; Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt; Big sizes (5040, 60xx, 8040) used for shock-proof circuits
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndLQS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndLQS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQS"&gt;http://katalog.we-online.de/en/pbs/WE-LQS&lt;/a&gt;&lt;p&gt;


Created  by  Dan Xu 2014-05-21&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQS_5040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74404054010">
<attribute name="WE-NUMBER" value="74404054010/1uH"/>
</technology>
<technology name="_74404054015">
<attribute name="WE-NUMBER" value="74404054015/1,5uH"/>
</technology>
<technology name="_74404054022">
<attribute name="WE-NUMBER" value="74404054022/2,2uH"/>
</technology>
<technology name="_74404054033">
<attribute name="WE-NUMBER" value="74404054033/3,3uH"/>
</technology>
<technology name="_74404054047">
<attribute name="WE-NUMBER" value="74404054047/4,7uH"/>
</technology>
<technology name="_74404054068">
<attribute name="WE-NUMBER" value="74404054068/6,8uH"/>
</technology>
<technology name="_74404054100">
<attribute name="WE-NUMBER" value="74404054100/10uH"/>
</technology>
<technology name="_74404054101">
<attribute name="WE-NUMBER" value="74404054101/100uH"/>
</technology>
<technology name="_74404054102">
<attribute name="WE-NUMBER" value="74404054102/1000uH"/>
</technology>
<technology name="_74404054150">
<attribute name="WE-NUMBER" value="74404054150/15uH"/>
</technology>
<technology name="_74404054220">
<attribute name="WE-NUMBER" value="74404054220/22uH"/>
</technology>
<technology name="_74404054330">
<attribute name="WE-NUMBER" value="74404054330/33uH"/>
</technology>
<technology name="_74404054470">
<attribute name="WE-NUMBER" value="74404054470/47uH"/>
</technology>
<technology name="_74404054680">
<attribute name="WE-NUMBER" value="74404054680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQS_6028" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Tiny Power Inductor design
&lt;br&gt;
&lt;br&gt; 1.7 times more current in comparison with unshielded versions
&lt;br&gt;
&lt;br&gt; Robust design &amp; high durability
&lt;br&gt;
&lt;br&gt; Low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded with magnetic glue reducing buzz noise in ultra-low levels
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC Converters
&lt;br&gt;
&lt;br&gt; Switching controllers which required high efficiency
&lt;br&gt;
&lt;br&gt; Portable power (Smartphones, digital cameras, Tablets, etc.)
&lt;br&gt;
&lt;br&gt; Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt; Big sizes (5040, 60xx, 8040) used for shock-proof circuits
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndLQS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndLQS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQS"&gt;http://katalog.we-online.de/en/pbs/WE-LQS&lt;/a&gt;&lt;p&gt;


Created  by  Dan Xu 2014-05-21&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQS_6028">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744040630082">
<attribute name="WE-NUMBER" value="744040630082/0,82uH"/>
</technology>
<technology name="_74404063010">
<attribute name="WE-NUMBER" value="74404063010/1uH"/>
</technology>
<technology name="_74404063012">
<attribute name="WE-NUMBER" value="74404063012/1,2uH"/>
</technology>
<technology name="_74404063015">
<attribute name="WE-NUMBER" value="74404063015uH"/>
</technology>
<technology name="_74404063022">
<attribute name="WE-NUMBER" value="74404063022/2,2uH"/>
</technology>
<technology name="_74404063033">
<attribute name="WE-NUMBER" value="74404063033/3,3uH"/>
</technology>
<technology name="_74404063047">
<attribute name="WE-NUMBER" value="74404063047/4,7uH"/>
</technology>
<technology name="_74404063068">
<attribute name="WE-NUMBER" value="74404063068/6,8uH"/>
</technology>
<technology name="_74404063082">
<attribute name="WE-NUMBER" value="74404063082/8,2uH"/>
</technology>
<technology name="_74404063100">
<attribute name="WE-NUMBER" value="74404063100/10uH"/>
</technology>
<technology name="_74404063101">
<attribute name="WE-NUMBER" value="74404063101/100uH"/>
</technology>
<technology name="_74404063102">
<attribute name="WE-NUMBER" value="74404063102/1000uH"/>
</technology>
<technology name="_74404063150">
<attribute name="WE-NUMBER" value="74404063150/15uH"/>
</technology>
<technology name="_74404063220">
<attribute name="WE-NUMBER" value="74404063220/22uH"/>
</technology>
<technology name="_74404063330">
<attribute name="WE-NUMBER" value="74404063330/33uH"/>
</technology>
<technology name="_74404063470">
<attribute name="WE-NUMBER" value="74404063470/47uH"/>
</technology>
<technology name="_74404063680">
<attribute name="WE-NUMBER" value="74404063680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQS_6045" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Tiny Power Inductor design
&lt;br&gt;
&lt;br&gt; 1.7 times more current in comparison with unshielded versions
&lt;br&gt;
&lt;br&gt; Robust design &amp; high durability
&lt;br&gt;
&lt;br&gt; Low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded with magnetic glue reducing buzz noise in ultra-low levels
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC Converters
&lt;br&gt;
&lt;br&gt; Switching controllers which required high efficiency
&lt;br&gt;
&lt;br&gt; Portable power (Smartphones, digital cameras, Tablets, etc.)
&lt;br&gt;
&lt;br&gt; Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt; Big sizes (5040, 60xx, 8040) used for shock-proof circuits
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndLQS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndLQS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQS"&gt;http://katalog.we-online.de/en/pbs/WE-LQS&lt;/a&gt;&lt;p&gt;


Created  by  Dan Xu 2014-05-21&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQS_6045">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744040640047">
<attribute name="WE-NUMBER" value="744040640047/0,47uH"/>
</technology>
<technology name="_744040640068">
<attribute name="WE-NUMBER" value="744040640068/0,68uH"/>
</technology>
<technology name="_74404064010">
<attribute name="WE-NUMBER" value="74404064010/1uH"/>
</technology>
<technology name="_74404064012">
<attribute name="WE-NUMBER" value="74404064012/1,2uH"/>
</technology>
<technology name="_74404064015">
<attribute name="WE-NUMBER" value="74404064015/1,5uH"/>
</technology>
<technology name="_74404064018">
<attribute name="WE-NUMBER" value="74404064018/1,8uH"/>
</technology>
<technology name="_74404064022">
<attribute name="WE-NUMBER" value="74404064022/2,2uH"/>
</technology>
<technology name="_74404064033">
<attribute name="WE-NUMBER" value="74404064033/3,3uH"/>
</technology>
<technology name="_74404064047">
<attribute name="WE-NUMBER" value="74404064047/4,7uH"/>
</technology>
<technology name="_74404064068">
<attribute name="WE-NUMBER" value="74404064068/6,8uH"/>
</technology>
<technology name="_74404064082">
<attribute name="WE-NUMBER" value="74404064082/8,2uH"/>
</technology>
<technology name="_74404064100">
<attribute name="WE-NUMBER" value="74404064100/10uH"/>
</technology>
<technology name="_74404064101">
<attribute name="WE-NUMBER" value="74404064101/100uH"/>
</technology>
<technology name="_74404064102">
<attribute name="WE-NUMBER" value="74404064102/1000uH"/>
</technology>
<technology name="_74404064120">
<attribute name="WE-NUMBER" value="74404064120/12uH"/>
</technology>
<technology name="_74404064121">
<attribute name="WE-NUMBER" value="74404064121/120uH"/>
</technology>
<technology name="_74404064150">
<attribute name="WE-NUMBER" value="74404064150/15uH"/>
</technology>
<technology name="_74404064151">
<attribute name="WE-NUMBER" value="74404064151/150uH"/>
</technology>
<technology name="_74404064152">
<attribute name="WE-NUMBER" value="74404064152/1500uH"/>
</technology>
<technology name="_74404064180">
<attribute name="WE-NUMBER" value="74404064180/18uH"/>
</technology>
<technology name="_74404064220">
<attribute name="WE-NUMBER" value="74404064220/22uH"/>
</technology>
<technology name="_74404064221">
<attribute name="WE-NUMBER" value="74404064221/220uH"/>
</technology>
<technology name="_74404064330">
<attribute name="WE-NUMBER" value="74404064330/33uH"/>
</technology>
<technology name="_74404064331">
<attribute name="WE-NUMBER" value="74404064331/330uH"/>
</technology>
<technology name="_74404064470">
<attribute name="WE-NUMBER" value="74404064470/47uH"/>
</technology>
<technology name="_74404064680">
<attribute name="WE-NUMBER" value="74404064680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQS_8040" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Tiny Power Inductor design
&lt;br&gt;
&lt;br&gt; 1.7 times more current in comparison with unshielded versions
&lt;br&gt;
&lt;br&gt; Robust design &amp; high durability
&lt;br&gt;
&lt;br&gt; Low RDC
&lt;br&gt;
&lt;br&gt; Magnetically shielded with magnetic glue reducing buzz noise in ultra-low levels
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC Converters
&lt;br&gt;
&lt;br&gt; Switching controllers which required high efficiency
&lt;br&gt;
&lt;br&gt; Portable power (Smartphones, digital cameras, Tablets, etc.)
&lt;br&gt;
&lt;br&gt; Embedded laptops and PCs
&lt;br&gt;
&lt;br&gt; Big sizes (5040, 60xx, 8040) used for shock-proof circuits
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndLQS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndLQS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQS"&gt;http://katalog.we-online.de/en/pbs/WE-LQS&lt;/a&gt;&lt;p&gt;


Created  by  Dan Xu 2014-05-21&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQS_8040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74404084010">
<attribute name="WE-NUMBER" value="74401084010/1uH"/>
</technology>
<technology name="_74404084015">
<attribute name="WE-NUMBER" value="74404084015/1,5uH"/>
</technology>
<technology name="_74404084022">
<attribute name="WE-NUMBER" value="74404084022/2,2uH"/>
</technology>
<technology name="_74404084033">
<attribute name="WE-NUMBER" value="74404084033/3,3uH"/>
</technology>
<technology name="_74404084047">
<attribute name="WE-NUMBER" value="74404084047/4,7uH"/>
</technology>
<technology name="_74404084068">
<attribute name="WE-NUMBER" value="74404084068/6,8uH"/>
</technology>
<technology name="_74404084082">
<attribute name="WE-NUMBER" value="74404084082/8,2uH"/>
</technology>
<technology name="_74404084100">
<attribute name="WE-NUMBER" value="74404084100/10uH"/>
</technology>
<technology name="_74404084101">
<attribute name="WE-NUMBER" value="74404084101/100uH"/>
</technology>
<technology name="_74404084102">
<attribute name="WE-NUMBER" value="74404084102/1000uH"/>
</technology>
<technology name="_74404084120">
<attribute name="WE-NUMBER" value="74404084120/12uH"/>
</technology>
<technology name="_74404084121">
<attribute name="WE-NUMBER" value="74404084121/120uH"/>
</technology>
<technology name="_74404084150">
<attribute name="WE-NUMBER" value="74407084150/15uH"/>
</technology>
<technology name="_74404084151">
<attribute name="WE-NUMBER" value="74404084151/150uH"/>
</technology>
<technology name="_74404084180">
<attribute name="WE-NUMBER" value="74404084180/18uH"/>
</technology>
<technology name="_74404084220">
<attribute name="WE-NUMBER" value="74404084220/22uH"/>
</technology>
<technology name="_74404084221">
<attribute name="WE-NUMBER" value="74404084221/220uH"/>
</technology>
<technology name="_74404084330">
<attribute name="WE-NUMBER" value="74404084330/33uH"/>
</technology>
<technology name="_74404084331">
<attribute name="WE-NUMBER" value="74404084331/330uH"/>
</technology>
<technology name="_74404084470">
<attribute name="WE-NUMBER" value="74404084470/47uH"/>
</technology>
<technology name="_74404084680">
<attribute name="WE-NUMBER" value="74404084680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQSH_2010" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-LQSH SMD Semi-Shielded High Saturation Power Inductor&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LQSH_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LQSH_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQSH"&gt;http://katalog.we-online.de/en/pbs/WE-LQSH&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQS_2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744050200047">
<attribute name="WE-NUMBER" value="744050200047/0,47uH"/>
</technology>
<technology name="_74405020010">
<attribute name="WE-NUMBER" value="74405020010/1uH"/>
</technology>
<technology name="_74405020015">
<attribute name="WE-NUMBER" value="74404020015/1,5uH"/>
</technology>
<technology name="_74405020022">
<attribute name="WE-NUMBER" value="74405020022/2,5uH"/>
</technology>
<technology name="_74405020047">
<attribute name="WE-NUMBER" value="74404020047/4,7uH"/>
</technology>
<technology name="_74405020100">
<attribute name="WE-NUMBER" value="74405020100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQSH_2512" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-LQSH SMD Semi-Shielded High Saturation Power Inductor&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LQSH_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LQSH_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQSH"&gt;http://katalog.we-online.de/en/pbs/WE-LQSH&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQSH_2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744050240047">
<attribute name="WE-NUMBER" value="744050240047/0,47uH"/>
</technology>
<technology name="_74405024010">
<attribute name="WE-NUMBER" value="74405024010/1uH"/>
</technology>
<technology name="_74405024015">
<attribute name="WE-NUMBER" value="74405024015/1,5uH"/>
</technology>
<technology name="_74405024022">
<attribute name="WE-NUMBER" value="74405024022/2,2uH"/>
</technology>
<technology name="_74405024033">
<attribute name="WE-NUMBER" value="74405024033/3,3uH"/>
</technology>
<technology name="_74405024047">
<attribute name="WE-NUMBER" value="74405024047/4,7uH"/>
</technology>
<technology name="_74405024100">
<attribute name="WE-NUMBER" value="74405024100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQSH_3012" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-LQSH SMD Semi-Shielded High Saturation Power Inductor&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LQSH_2016.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LQSH_2016.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LQSH"&gt;http://katalog.we-online.de/en/pbs/WE-LQSH&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-LQSH_3012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744050310047">
<attribute name="WE-NUMBER" value="744050310047/0,47uH"/>
</technology>
<technology name="_74405031010">
<attribute name="WE-NUMBER" value="74405031010/1uH"/>
</technology>
<technology name="_74405031015">
<attribute name="WE-NUMBER" value="74405031015/1,5uH"/>
</technology>
<technology name="_74405031022">
<attribute name="WE-NUMBER" value="74405031022/2,2uH"/>
</technology>
<technology name="_74405031033">
<attribute name="WE-NUMBER" value="74405031033/3,3uH"/>
</technology>
<technology name="_74405031047">
<attribute name="WE-NUMBER" value="74405031047/4,7uH"/>
</technology>
<technology name="_74405031100">
<attribute name="WE-NUMBER" value="74405031100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_4020" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD Metal Alloy Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;
&lt;br&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt;
&lt;br&gt; Low acoustic noise and low leakage flux noise
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC-converter for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL-converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital camera
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt; Wireless communication devices
&lt;br&gt;
&lt;br&gt; Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAPI?"&gt;http://katalog.we-online.de/en/pbs/WE-MAPI?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAPI_40XX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383560033">
<attribute name="WE-NUMBER" value="744383560033/0,33uH"/>
</technology>
<technology name="_744383560056">
<attribute name="WE-NUMBER" value="744383560056/0,56uH"/>
</technology>
<technology name="_744383560068">
<attribute name="WE-NUMBER" value="744383560068/0,68uH"/>
</technology>
<technology name="_74438356010">
<attribute name="WE-NUMBER" value="74438356010/1uH"/>
</technology>
<technology name="_74438356012">
<attribute name="WE-NUMBER" value="74438356012/1,2uH"/>
</technology>
<technology name="_74438356015">
<attribute name="WE-NUMBER" value="74438356015/1,5uH"/>
</technology>
<technology name="_74438356018">
<attribute name="WE-NUMBER" value="74438356018/1,8uH"/>
</technology>
<technology name="_74438356022">
<attribute name="WE-NUMBER" value="74438356022/2,2uH"/>
</technology>
<technology name="_74438356033">
<attribute name="WE-NUMBER" value="74438356033/3,3uH"/>
</technology>
<technology name="_74438356047">
<attribute name="WE-NUMBER" value="74438356047/4,7uH"/>
</technology>
<technology name="_74438356056">
<attribute name="WE-NUMBER" value="74438356056/5,6uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_1610" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD Metal Alloy Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;
&lt;br&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt;
&lt;br&gt; Low acoustic noise and low leakage flux noise
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC-converter for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL-converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital camera
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt; Wireless communication devices
&lt;br&gt;
&lt;br&gt; Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAPI?"&gt;http://katalog.we-online.de/en/pbs/WE-MAPI?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAPI_1610">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383130033">
<attribute name="WE-NUMBER" value="744383130033/0,33uH"/>
</technology>
<technology name="_744383130047">
<attribute name="WE-NUMBER" value="744383130047/0,47uH"/>
</technology>
<technology name="_744383130056">
<attribute name="WE-NUMBER" value="744383130056/0,56uH"/>
</technology>
<technology name="_744383130068">
<attribute name="WE-NUMBER" value="744383130068/0,68uH"/>
</technology>
<technology name="_744383130082">
<attribute name="WE-NUMBER" value="744383130082/0,82uH"/>
</technology>
<technology name="_74438313010">
<attribute name="WE-NUMBER" value="74438313010/1uH"/>
</technology>
<technology name="_74438313012">
<attribute name="WE-NUMBER" value="74438313012/1,2uH"/>
</technology>
<technology name="_74438313015">
<attribute name="WE-NUMBER" value="74438313015/1,5uH"/>
</technology>
<technology name="_74438313022">
<attribute name="WE-NUMBER" value="74438313022/2,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2010" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD Metal Alloy Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;
&lt;br&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt;
&lt;br&gt; Low acoustic noise and low leakage flux noise
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC-converter for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL-converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital camera
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt; Wireless communication devices
&lt;br&gt;
&lt;br&gt; Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAPI?"&gt;http://katalog.we-online.de/en/pbs/WE-MAPI?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAPI_2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383430033">
<attribute name="WE-NUMBER" value="74438343033/0,33uH"/>
</technology>
<technology name="_744383430047">
<attribute name="WE-NUMBER" value="744383430047/0,47uH"/>
</technology>
<technology name="_744383430056">
<attribute name="WE-NUMBER" value="744383430056/0,56uH"/>
</technology>
<technology name="_744383430082">
<attribute name="WE-NUMBER" value="744383430082/0,82uH"/>
</technology>
<technology name="_74438343010">
<attribute name="WE-NUMBER" value="74438343010/1uH"/>
</technology>
<technology name="_74438343012">
<attribute name="WE-NUMBER" value="74438343012/1,2uH"/>
</technology>
<technology name="_74438343015">
<attribute name="WE-NUMBER" value="74438343015/1,5uH"/>
</technology>
<technology name="_74438343022">
<attribute name="WE-NUMBER" value="74438343022/2,2uH"/>
</technology>
<technology name="_744383460068">
<attribute name="WE-NUMBER" value="744383460068/0,68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2506" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD Metal Alloy Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;
&lt;br&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt;
&lt;br&gt; Low acoustic noise and low leakage flux noise
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC-converter for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL-converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital camera
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt; Wireless communication devices
&lt;br&gt;
&lt;br&gt; Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAPI?"&gt;http://katalog.we-online.de/en/pbs/WE-MAPI?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAPI_2506">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383210047">
<attribute name="WE-NUMBER" value="744383210047/0,47uH"/>
</technology>
<technology name="_74438321010">
<attribute name="WE-NUMBER" value="74438321010/1uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2508" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD Metal Alloy Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;
&lt;br&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt;
&lt;br&gt; Low acoustic noise and low leakage flux noise
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC-converter for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL-converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital camera
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt; Wireless communication devices
&lt;br&gt;
&lt;br&gt; Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAPI?"&gt;http://katalog.we-online.de/en/pbs/WE-MAPI?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAPI_2508">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383220047">
<attribute name="WE-NUMBER" value="744383220047/0,47uH"/>
</technology>
<technology name="_74438322010">
<attribute name="WE-NUMBER" value="74438322010/1uH"/>
</technology>
<technology name="_74438322022">
<attribute name="WE-NUMBER" value="74438322022/2,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2510" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD Metal Alloy Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;
&lt;br&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt;
&lt;br&gt; Low acoustic noise and low leakage flux noise
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC-converter for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL-converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital camera
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt; Wireless communication devices
&lt;br&gt;
&lt;br&gt; Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAPI?"&gt;http://katalog.we-online.de/en/pbs/WE-MAPI?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAIA_2510">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383230033">
<attribute name="WE-NUMBER" value="744383230033/0,33uH"/>
</technology>
<technology name="_744383230047">
<attribute name="WE-NUMBER" value="744383230047/0,47uH"/>
</technology>
<technology name="_744383230068">
<attribute name="WE-NUMBER" value="744383230068/0,68uH"/>
</technology>
<technology name="_744383230082">
<attribute name="WE-NUMBER" value="744383230082/0,33uH"/>
</technology>
<technology name="_74438323010">
<attribute name="WE-NUMBER" value="74438323010/1uH"/>
</technology>
<technology name="_74438323012">
<attribute name="WE-NUMBER" value="74438323012/1,2uH"/>
</technology>
<technology name="_74438323015">
<attribute name="WE-NUMBER" value="74438323015/1,5uH"/>
</technology>
<technology name="_74438323022">
<attribute name="WE-NUMBER" value="74438323022/2,2uH"/>
</technology>
<technology name="_74438323033">
<attribute name="WE-NUMBER" value="74438323033/3,3uH"/>
</technology>
<technology name="_74438323047">
<attribute name="WE-NUMBER" value="74438323047/4,7uH"/>
</technology>
<technology name="_74438323068">
<attribute name="WE-NUMBER" value="74438323068/6,8uH"/>
</technology>
<technology name="_74438323082">
<attribute name="WE-NUMBER" value="74438323082/8,2uH"/>
</technology>
<technology name="_74438323100">
<attribute name="WE-NUMBER" value="74438323100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2512" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD Metal Alloy Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;
&lt;br&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt;
&lt;br&gt; Low acoustic noise and low leakage flux noise
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC-converter for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL-converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital camera
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt; Wireless communication devices
&lt;br&gt;
&lt;br&gt; Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAPI?"&gt;http://katalog.we-online.de/en/pbs/WE-MAPI?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAIA_2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383240047">
<attribute name="WE-NUMBER" value="744383240047/0,47uH"/>
</technology>
<technology name="_744383240056">
<attribute name="WE-NUMBER" value="744383240056/0,56uH"/>
</technology>
<technology name="_744383240068">
<attribute name="WE-NUMBER" value="744383240068/0,68uH"/>
</technology>
<technology name="_74438324010">
<attribute name="WE-NUMBER" value="74438324010/1uH"/>
</technology>
<technology name="_74438324012">
<attribute name="WE-NUMBER" value="74438324012/1,2uH"/>
</technology>
<technology name="_74438324015">
<attribute name="WE-NUMBER" value="74438324015/1,5uH"/>
</technology>
<technology name="_74438324022">
<attribute name="WE-NUMBER" value="74438324022/2,2uH"/>
</technology>
<technology name="_74438324033">
<attribute name="WE-NUMBER" value="74438324033/3,3uH"/>
</technology>
<technology name="_74438324047">
<attribute name="WE-NUMBER" value="74438324047/4,7uH"/>
</technology>
<technology name="_74438324056">
<attribute name="WE-NUMBER" value="74438324056/5,6uH"/>
</technology>
<technology name="_74438324068">
<attribute name="WE-NUMBER" value="74438324068/0,68uH"/>
</technology>
<technology name="_74438324082">
<attribute name="WE-NUMBER" value="74438324082/8,2uH"/>
</technology>
<technology name="_74438324100">
<attribute name="WE-NUMBER" value="74438324100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_3010" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD Metal Alloy Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;
&lt;br&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt;
&lt;br&gt; Low acoustic noise and low leakage flux noise
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC-converter for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL-converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital camera
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt; Wireless communication devices
&lt;br&gt;
&lt;br&gt; Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAPI?"&gt;http://katalog.we-online.de/en/pbs/WE-MAPI?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74438333022">
<attribute name="WE-NUMBER" value="74438333022/2,2uH"/>
</technology>
<technology name="_74438333033">
<attribute name="WE-NUMBER" value="74438333033/3,3uH"/>
</technology>
<technology name="_74438333047">
<attribute name="WE-NUMBER" value="74438333047/4,7uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_3012" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD Metal Alloy Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;
&lt;br&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt;
&lt;br&gt; Low acoustic noise and low leakage flux noise
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC-converter for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL-converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital camera
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt; Wireless communication devices
&lt;br&gt;
&lt;br&gt; Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAPI?"&gt;http://katalog.we-online.de/en/pbs/WE-MAPI?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3012_STANDER">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383340033">
<attribute name="WE-NUMBER" value="744383340033/0,33uH"/>
</technology>
<technology name="_744383340047">
<attribute name="WE-NUMBER" value="744383340047/0,47uH"/>
</technology>
<technology name="_744383340056">
<attribute name="WE-NUMBER" value="744383340056/0,56uH"/>
</technology>
<technology name="_744383340068">
<attribute name="WE-NUMBER" value="744383340068/0,68uH"/>
</technology>
<technology name="_74438334010">
<attribute name="WE-NUMBER" value="74438334010/1uH"/>
</technology>
<technology name="_74438334012">
<attribute name="WE-NUMBER" value="74438334012/1,2uH"/>
</technology>
<technology name="_74438334015">
<attribute name="WE-NUMBER" value="74438334015/1,5uH"/>
</technology>
<technology name="_74438334022">
<attribute name="WE-NUMBER" value="74438334022/2,2uH"/>
</technology>
<technology name="_74438334033">
<attribute name="WE-NUMBER" value="74438334033/3,3uH"/>
</technology>
<technology name="_74438334047">
<attribute name="WE-NUMBER" value="74438334047/0,47uH"/>
</technology>
<technology name="_74438334056">
<attribute name="WE-NUMBER" value="74438334056/5,6uH"/>
</technology>
<technology name="_74438334068">
<attribute name="WE-NUMBER" value="74438334068/6,8uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_3015" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD Metal Alloy Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;
&lt;br&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt;
&lt;br&gt; Low acoustic noise and low leakage flux noise
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC-converter for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL-converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital camera
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt; Wireless communication devices
&lt;br&gt;
&lt;br&gt; Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAPI?"&gt;http://katalog.we-online.de/en/pbs/WE-MAPI?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3015/3020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383350047">
<attribute name="WE-NUMBER" value="744383350047/0,47uH"/>
</technology>
<technology name="_744383350068">
<attribute name="WE-NUMBER" value="744383350068/0,68uH"/>
</technology>
<technology name="_744383350082">
<attribute name="WE-NUMBER" value="744383350082/0,82uH"/>
</technology>
<technology name="_74438335010">
<attribute name="WE-NUMBER" value="74438335010/1uH"/>
</technology>
<technology name="_74438335022">
<attribute name="WE-NUMBER" value="74438335022/2,2uH"/>
</technology>
<technology name="_74438335033">
<attribute name="WE-NUMBER" value="74438335033/0,33uH"/>
</technology>
<technology name="_74438335047">
<attribute name="WE-NUMBER" value="74438335047/4,7uH"/>
</technology>
<technology name="_74438335068">
<attribute name="WE-NUMBER" value="74438335068/6,8uH"/>
</technology>
<technology name="_74438335100">
<attribute name="WE-NUMBER" value="74438335100/10uH"/>
</technology>
<technology name="_74438335150">
<attribute name="WE-NUMBER" value="74438335150/15uH"/>
</technology>
<technology name="_74438335220">
<attribute name="WE-NUMBER" value="74438335220/22uH"/>
</technology>
<technology name="_74438335330">
<attribute name="WE-NUMBER" value="74438335330/33uH"/>
</technology>
<technology name="_74438335470">
<attribute name="WE-NUMBER" value="74438335470/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_3020" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD Metal Alloy Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;
&lt;br&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt;
&lt;br&gt; Low acoustic noise and low leakage flux noise
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC-converter for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL-converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital camera
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt; Wireless communication devices
&lt;br&gt;
&lt;br&gt; Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAPI?"&gt;http://katalog.we-online.de/en/pbs/WE-MAPI?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3015/3020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383360033">
<attribute name="WE-NUMBER" value="744383360033/0,33uH"/>
</technology>
<technology name="_744383360047">
<attribute name="WE-NUMBER" value="744383360047/0,47uH"/>
</technology>
<technology name="_744383360068">
<attribute name="WE-NUMBER" value="744383360068/0,68uH"/>
</technology>
<technology name="_74438336010">
<attribute name="WE-NUMBER" value="74438336010/1uH"/>
</technology>
<technology name="_74438336012">
<attribute name="WE-NUMBER" value="74438336012/1,2uH"/>
</technology>
<technology name="_74438336015">
<attribute name="WE-NUMBER" value="74438336015/1,5uH"/>
</technology>
<technology name="_74438336022">
<attribute name="WE-NUMBER" value="74438336022/2,2uH"/>
</technology>
<technology name="_74438336033">
<attribute name="WE-NUMBER" value="74438336033/3,3uH"/>
</technology>
<technology name="_74438336047">
<attribute name="WE-NUMBER" value="74438336047/4,7uH"/>
</technology>
<technology name="_74438336068">
<attribute name="WE-NUMBER" value="74438336068/6,8uH"/>
</technology>
<technology name="_74438336100">
<attribute name="WE-NUMBER" value="74438336100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_20XX_LOWVOID" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD Metal Alloy Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;
&lt;br&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt;
&lt;br&gt; Low acoustic noise and low leakage flux noise
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC-converter for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL-converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital camera
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt; Wireless communication devices
&lt;br&gt;
&lt;br&gt; Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAPI?"&gt;http://katalog.we-online.de/en/pbs/WE-MAPI?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAPI_20XX">
<connects>
<connect gate="G$1" pin="1" pad="1 3 4"/>
<connect gate="G$1" pin="2" pad="2 5 6"/>
</connects>
<technologies>
<technology name="_744383430033">
<attribute name="WE-NUMBER" value="744383430033/0,33uH"/>
</technology>
<technology name="_744383430047">
<attribute name="WE-NUMBER" value="744383430047/0,47uH"/>
</technology>
<technology name="_744383430056">
<attribute name="WE-NUMBER" value="744383430056/0,56uH"/>
</technology>
<technology name="_744383430068">
<attribute name="WE-NUMBER" value="744383430068/0,68uH"/>
</technology>
<technology name="_744383430082">
<attribute name="WE-NUMBER" value="744383430082/0,82uH"/>
</technology>
<technology name="_74438343010">
<attribute name="WE-NUMBER" value="74438343010/1uH"/>
</technology>
<technology name="_74438343012">
<attribute name="WE-NUMBER" value="74438343012/1,2uH"/>
</technology>
<technology name="_74438343015">
<attribute name="WE-NUMBER" value="74438343015/1,5uH"/>
</technology>
<technology name="_74438343022">
<attribute name="WE-NUMBER" value="74438343022/2,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_25XX_LOWVOID" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD Metal Alloy Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;
&lt;br&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt;
&lt;br&gt; Low acoustic noise and low leakage flux noise
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC-converter for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL-converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital camera
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt; Wireless communication devices
&lt;br&gt;
&lt;br&gt; Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAPI?"&gt;http://katalog.we-online.de/en/pbs/WE-MAPI?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAPI_25XX">
<connects>
<connect gate="G$1" pin="1" pad="1 3 4"/>
<connect gate="G$1" pin="2" pad="2 5 6"/>
</connects>
<technologies>
<technology name="_744383210047">
<attribute name="WE-NUMBER" value="744383210047/0,47uH"/>
</technology>
<technology name="_74438321010">
<attribute name="WE-NUMBER" value="74438321010/1uH"/>
</technology>
<technology name="_744383220047">
<attribute name="WE-NUMBER" value="744383220047/0,47uH"/>
</technology>
<technology name="_74438322010">
<attribute name="WE-NUMBER" value="74438322010/1uH"/>
</technology>
<technology name="_74438322022">
<attribute name="WE-NUMBER" value="74438322022/2,2uH"/>
</technology>
<technology name="_744383230033">
<attribute name="WE-NUMBER" value="744383230033/0,33uH"/>
</technology>
<technology name="_744383230047">
<attribute name="WE-NUMBER" value="744383230047/0,47uH"/>
</technology>
<technology name="_744383230068">
<attribute name="WE-NUMBER" value="744383230068/0,68uH"/>
</technology>
<technology name="_744383230082">
<attribute name="WE-NUMBER" value="744383230082/0,82uH"/>
</technology>
<technology name="_74438323010">
<attribute name="WE-NUMBER" value="74438323010/0,1uH"/>
</technology>
<technology name="_74438323012">
<attribute name="WE-NUMBER" value="74438323012/1,2uH"/>
</technology>
<technology name="_74438323015">
<attribute name="WE-NUMBER" value="74438323015/1,5uH"/>
</technology>
<technology name="_74438323022">
<attribute name="WE-NUMBER" value="74438323022/2,2uH"/>
</technology>
<technology name="_74438323033">
<attribute name="WE-NUMBER" value="74438323033/3,3uH"/>
</technology>
<technology name="_74438323047">
<attribute name="WE-NUMBER" value="74438323047/4,7uH"/>
</technology>
<technology name="_74438323068">
<attribute name="WE-NUMBER" value="74438323068/6,8uH"/>
</technology>
<technology name="_74438323082">
<attribute name="WE-NUMBER" value="74438323082/8,2uH"/>
</technology>
<technology name="_74438323100">
<attribute name="WE-NUMBER" value="74438323100/10uH"/>
</technology>
<technology name="_744383240047">
<attribute name="WE-NUMBER" value="744383240047/0,47uH"/>
</technology>
<technology name="_744383240056">
<attribute name="WE-NUMBER" value="744383240056/0,56uH"/>
</technology>
<technology name="_744383240068">
<attribute name="WE-NUMBER" value="744383240068/0,68uH"/>
</technology>
<technology name="_74438324010">
<attribute name="WE-NUMBER" value="74438324010/1uH"/>
</technology>
<technology name="_74438324012">
<attribute name="WE-NUMBER" value="74438324012/1,2uH"/>
</technology>
<technology name="_74438324015">
<attribute name="WE-NUMBER" value="74438324015/1,5uH"/>
</technology>
<technology name="_74438324022">
<attribute name="WE-NUMBER" value="74438324022/2,2uH"/>
</technology>
<technology name="_74438324033">
<attribute name="WE-NUMBER" value="74438324033/3,3uH"/>
</technology>
<technology name="_74438324047">
<attribute name="WE-NUMBER" value="744438324047/4,7uH"/>
</technology>
<technology name="_74438324056">
<attribute name="WE-NUMBER" value="74438324056/5,6uH"/>
</technology>
<technology name="_74438324068">
<attribute name="WE-NUMBER" value="74438324068/6,8uH"/>
</technology>
<technology name="_74438324082">
<attribute name="WE-NUMBER" value="74438324082/8,2uH"/>
</technology>
<technology name="_74438324100">
<attribute name="WE-NUMBER" value="74438324100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_30XX_LOWVOID" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD Metal Alloy Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;
&lt;br&gt; Compact design
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; High current capability and handles high transient current spikes
&lt;br&gt;
&lt;br&gt; Low acoustic noise and low leakage flux noise
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC-converter for high current power supplies
&lt;br&gt;
&lt;br&gt; DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;
&lt;br&gt; POL-converters
&lt;br&gt;
&lt;br&gt; Portable power like PDA, digital camera
&lt;br&gt;
&lt;br&gt; Mainboards/graphic cards
&lt;br&gt;
&lt;br&gt; Battery powered devices
&lt;br&gt;
&lt;br&gt; Wireless communication devices
&lt;br&gt;
&lt;br&gt; Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndMAPI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAPI?"&gt;http://katalog.we-online.de/en/pbs/WE-MAPI?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAPI_30XX">
<connects>
<connect gate="G$1" pin="1" pad="P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10"/>
<connect gate="G$1" pin="2" pad="P$11 P$12 P$13 P$14 P$15 P$16 P$17 P$18 P$19 P$20"/>
</connects>
<technologies>
<technology name="_74438333022">
<attribute name="WE-NUMBER" value="74438333022/2,2uH"/>
</technology>
<technology name="_74438333033">
<attribute name="WE-NUMBER" value="74438333033/3,3uH"/>
</technology>
<technology name="_74438333047">
<attribute name="WE-NUMBER" value="7443833047/4,7uH"/>
</technology>
<technology name="_744383340033">
<attribute name="WE-NUMBER" value="744383340033/0,33uH"/>
</technology>
<technology name="_744383340047">
<attribute name="WE-NUMBER" value="744383340047/0,47uH"/>
</technology>
<technology name="_744383340056">
<attribute name="WE-NUMBER" value="744383340056/0,56uH"/>
</technology>
<technology name="_744383340068">
<attribute name="WE-NUMBER" value="744383340068/0,68uH"/>
</technology>
<technology name="_74438334010">
<attribute name="WE-NUMBER" value="74438334010/1uH"/>
</technology>
<technology name="_74438334012">
<attribute name="WE-NUMBER" value="74438334012/1,2uH"/>
</technology>
<technology name="_74438334015">
<attribute name="WE-NUMBER" value="74438334015/1,5uH"/>
</technology>
<technology name="_74438334022">
<attribute name="WE-NUMBER" value="74438334022/2,2uH"/>
</technology>
<technology name="_74438334033">
<attribute name="WE-NUMBER" value="7438334033/3,3uH"/>
</technology>
<technology name="_74438334047">
<attribute name="WE-NUMBER" value="74438334047/4,7uH"/>
</technology>
<technology name="_74438334056">
<attribute name="WE-NUMBER" value="74438334056/5,6uH"/>
</technology>
<technology name="_74438334068">
<attribute name="WE-NUMBER" value="74438334068/6,8uH"/>
</technology>
<technology name="_744383350047">
<attribute name="WE-NUMBER" value="744383350047/0,47uH"/>
</technology>
<technology name="_744383350068">
<attribute name="WE-NUMBER" value="744383350068/0,68uH"/>
</technology>
<technology name="_744383350082">
<attribute name="WE-NUMBER" value="744383350082/0,82uH"/>
</technology>
<technology name="_74438335010">
<attribute name="WE-NUMBER" value="74438335010/1uH"/>
</technology>
<technology name="_74438335022">
<attribute name="WE-NUMBER" value="74438335022/2,2uH"/>
</technology>
<technology name="_74438335033">
<attribute name="WE-NUMBER" value="74438335033/0,33uH"/>
</technology>
<technology name="_74438335047">
<attribute name="WE-NUMBER" value="74438335047/4.7uH"/>
</technology>
<technology name="_74438335068">
<attribute name="WE-NUMBER" value="74438335068/6,8uH"/>
</technology>
<technology name="_74438335100">
<attribute name="WE-NUMBER" value="74438335100/10uH"/>
</technology>
<technology name="_74438335150">
<attribute name="WE-NUMBER" value="74438335150/15uH"/>
</technology>
<technology name="_74438335220">
<attribute name="WE-NUMBER" value="74438335220/22uH"/>
</technology>
<technology name="_74438335330">
<attribute name="WE-NUMBER" value="74438335330/33uH"/>
</technology>
<technology name="_74438335470">
<attribute name="WE-NUMBER" value="74438335470/47uH"/>
</technology>
<technology name="_744383360033">
<attribute name="WE-NUMBER" value="744383360033/0,33uH"/>
</technology>
<technology name="_744383360047">
<attribute name="WE-NUMBER" value="744383360047/0,47uH"/>
</technology>
<technology name="_744383360068">
<attribute name="WE-NUMBER" value="744383360068/0,68uH"/>
</technology>
<technology name="_74438336010">
<attribute name="WE-NUMBER" value="74438336010/1uH"/>
</technology>
<technology name="_74438336012">
<attribute name="WE-NUMBER" value="74438336012/1,2uH"/>
</technology>
<technology name="_74438336015">
<attribute name="WE-NUMBER" value="74438336015/1,5uH"/>
</technology>
<technology name="_74438336022">
<attribute name="WE-NUMBER" value="74438336022/2,2uH"/>
</technology>
<technology name="_74438336033">
<attribute name="WE-NUMBER" value="74438336033/3,3uH"/>
</technology>
<technology name="_74438336047">
<attribute name="WE-NUMBER" value="74438336047/4,7uH"/>
</technology>
<technology name="_74438336068">
<attribute name="WE-NUMBER" value="74438336068/0,68uH"/>
</technology>
<technology name="_74438336100">
<attribute name="WE-NUMBER" value="74438336100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_7332" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; High Saturation currents up to 25 A
&lt;br&gt;
&lt;br&gt; Very low self-losses at high switching frequency‘s
&lt;br&gt;
&lt;br&gt; Wide inductances spectrum available at all sizes
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt; Integrated DC/DC- converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD?"&gt;http://katalog.we-online.de/en/pbs/WE-PD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD_7332/7345">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744770233">
<attribute name="WE-NUMBER" value="744770233/330uH"/>
</technology>
<technology name="_744778001">
<attribute name="WE-NUMBER" value="744778001/1uH"/>
</technology>
<technology name="_744778002">
<attribute name="WE-NUMBER" value="744778002/2,2uH"/>
</technology>
<technology name="_744778003">
<attribute name="WE-NUMBER" value="744778003/3,3uH"/>
</technology>
<technology name="_744778004">
<attribute name="WE-NUMBER" value="744778004/4,7uH"/>
</technology>
<technology name="_744778005">
<attribute name="WE-NUMBER" value="744778005/0,54uH"/>
</technology>
<technology name="_74477810">
<attribute name="WE-NUMBER" value="74477810/10uH"/>
</technology>
<technology name="_744778112">
<attribute name="WE-NUMBER" value="744778112/12uH"/>
</technology>
<technology name="_744778115">
<attribute name="WE-NUMBER" value="744778115/15uH"/>
</technology>
<technology name="_744778118">
<attribute name="WE-NUMBER" value="744778118/18uH"/>
</technology>
<technology name="_744778122">
<attribute name="WE-NUMBER" value="744778122/22uH"/>
</technology>
<technology name="_744778127">
<attribute name="WE-NUMBER" value="744778127/27uH"/>
</technology>
<technology name="_744778133">
<attribute name="WE-NUMBER" value="744778133/33uH"/>
</technology>
<technology name="_744778139">
<attribute name="WE-NUMBER" value="744778139/39uH"/>
</technology>
<technology name="_744778147">
<attribute name="WE-NUMBER" value="744778147/47uH"/>
</technology>
<technology name="_744778156">
<attribute name="WE-NUMBER" value="744778156/56uH"/>
</technology>
<technology name="_744778168">
<attribute name="WE-NUMBER" value="744778168/68uH"/>
</technology>
<technology name="_744778182">
<attribute name="WE-NUMBER" value="744778182/82uH"/>
</technology>
<technology name="_74477820">
<attribute name="WE-NUMBER" value="74477820/100uH"/>
</technology>
<technology name="_744778212">
<attribute name="WE-NUMBER" value="744778212/120uH"/>
</technology>
<technology name="_744778215">
<attribute name="WE-NUMBER" value="744778215/150uH"/>
</technology>
<technology name="_744778218">
<attribute name="WE-NUMBER" value="744778218/180uH"/>
</technology>
<technology name="_744778222">
<attribute name="WE-NUMBER" value="744778222/220uH"/>
</technology>
<technology name="_744778239">
<attribute name="WE-NUMBER" value="744778239/390uH"/>
</technology>
<technology name="_74477824">
<attribute name="WE-NUMBER" value="74477824/470uH"/>
</technology>
<technology name="_74477825">
<attribute name="WE-NUMBER" value="74477825/560uH"/>
</technology>
<technology name="_74477826">
<attribute name="WE-NUMBER" value="74477826/680uH"/>
</technology>
<technology name="_744778270">
<attribute name="WE-NUMBER" value="744778270/270uH"/>
</technology>
<technology name="_74477828">
<attribute name="WE-NUMBER" value="74477828/820uH"/>
</technology>
<technology name="_74477830">
<attribute name="WE-NUMBER" value="74477830/1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_7345" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; High Saturation currents up to 25 A
&lt;br&gt;
&lt;br&gt; Very low self-losses at high switching frequency‘s
&lt;br&gt;
&lt;br&gt; Wide inductances spectrum available at all sizes
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt; Integrated DC/DC- converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD?"&gt;http://katalog.we-online.de/en/pbs/WE-PD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD_7332/7345">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744777001">
<attribute name="WE-NUMBER" value="744777001/1uH"/>
</technology>
<technology name="_744777002">
<attribute name="WE-NUMBER" value="744777002/2,2uH"/>
</technology>
<technology name="_744777003">
<attribute name="WE-NUMBER" value="744777003/3,3uH"/>
</technology>
<technology name="_744777004">
<attribute name="WE-NUMBER" value="744777004/4,7uH"/>
</technology>
<technology name="_74477710">
<attribute name="WE-NUMBER" value="74477710/10uH"/>
</technology>
<technology name="_744777112">
<attribute name="WE-NUMBER" value="744777112/12uH"/>
</technology>
<technology name="_744777115">
<attribute name="WE-NUMBER" value="744777115/15uH"/>
</technology>
<technology name="_744777118">
<attribute name="WE-NUMBER" value="744777118/18uH"/>
</technology>
<technology name="_744777122">
<attribute name="WE-NUMBER" value="744777122/22uH"/>
</technology>
<technology name="_744777127">
<attribute name="WE-NUMBER" value="744777127/27uH"/>
</technology>
<technology name="_744777133">
<attribute name="WE-NUMBER" value="744777133/33uH"/>
</technology>
<technology name="_744777139">
<attribute name="WE-NUMBER" value="744777139/39uH"/>
</technology>
<technology name="_744777147">
<attribute name="WE-NUMBER" value="744777147/47uH"/>
</technology>
<technology name="_744777156">
<attribute name="WE-NUMBER" value="744777156/56uH"/>
</technology>
<technology name="_744777168">
<attribute name="WE-NUMBER" value="744777168/68uH"/>
</technology>
<technology name="_744777182">
<attribute name="WE-NUMBER" value="744777182/82uH"/>
</technology>
<technology name="_74477720">
<attribute name="WE-NUMBER" value="74477720/100uH"/>
</technology>
<technology name="_744777212">
<attribute name="WE-NUMBER" value="744777212/120uH"/>
</technology>
<technology name="_744777215">
<attribute name="WE-NUMBER" value="744777215/150uH"/>
</technology>
<technology name="_744777218">
<attribute name="WE-NUMBER" value="744777218/180uH"/>
</technology>
<technology name="_744777222">
<attribute name="WE-NUMBER" value="744777222/220uH"/>
</technology>
<technology name="_744777233">
<attribute name="WE-NUMBER" value="744777233/330uH"/>
</technology>
<technology name="_744777239">
<attribute name="WE-NUMBER" value="744777239/390uH"/>
</technology>
<technology name="_74477724">
<attribute name="WE-NUMBER" value="74477724/470uH"/>
</technology>
<technology name="_74477725">
<attribute name="WE-NUMBER" value="74477725/560uH"/>
</technology>
<technology name="_74477726">
<attribute name="WE-NUMBER" value="74477726/680uH"/>
</technology>
<technology name="_744777270">
<attribute name="WE-NUMBER" value="744777270/27uH"/>
</technology>
<technology name="_74477728">
<attribute name="WE-NUMBER" value="74477728/820uH"/>
</technology>
<technology name="_74477730">
<attribute name="WE-NUMBER" value="74477730/1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_1050" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; High Saturation currents up to 25 A
&lt;br&gt;
&lt;br&gt; Very low self-losses at high switching frequency‘s
&lt;br&gt;
&lt;br&gt; Wide inductances spectrum available at all sizes
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt; Integrated DC/DC- converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD?"&gt;http://katalog.we-online.de/en/pbs/WE-PD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD_1030/1050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447714015">
<attribute name="WE-NUMBER" value="7447714015/1,5uH"/>
</technology>
<technology name="_7447714022">
<attribute name="WE-NUMBER" value="7447714022/2,2uH"/>
</technology>
<technology name="_7447714033">
<attribute name="WE-NUMBER" value="7447714033/3,3uH"/>
</technology>
<technology name="_7447714047">
<attribute name="WE-NUMBER" value="7447714047/4,7uH"/>
</technology>
<technology name="_7447714056">
<attribute name="WE-NUMBER" value="7447714056/5,6uH"/>
</technology>
<technology name="_7447714068">
<attribute name="WE-NUMBER" value="7447714068/6,8uH"/>
</technology>
<technology name="_7447714100">
<attribute name="WE-NUMBER" value="7447714100/10uH"/>
</technology>
<technology name="_7447714101">
<attribute name="WE-NUMBER" value="7447714101/100uH"/>
</technology>
<technology name="_7447714102">
<attribute name="WE-NUMBER" value="7447714102/1000uH"/>
</technology>
<technology name="_7447714150">
<attribute name="WE-NUMBER" value="7447714150/15uH"/>
</technology>
<technology name="_7447714151">
<attribute name="WE-NUMBER" value="7447714151/150uH"/>
</technology>
<technology name="_7447714220">
<attribute name="WE-NUMBER" value="7447714220/22uH"/>
</technology>
<technology name="_7447714221">
<attribute name="WE-NUMBER" value="7447714221/220uH"/>
</technology>
<technology name="_7447714330">
<attribute name="WE-NUMBER" value="7447714330/33uH"/>
</technology>
<technology name="_7447714331">
<attribute name="WE-NUMBER" value="7447714331/330uH"/>
</technology>
<technology name="_7447714470">
<attribute name="WE-NUMBER" value="7447714470/47uH"/>
</technology>
<technology name="_7447714471">
<attribute name="WE-NUMBER" value="7447714471/470uH"/>
</technology>
<technology name="_7447714560">
<attribute name="WE-NUMBER" value="7447714560/56uH"/>
</technology>
<technology name="_7447714680">
<attribute name="WE-NUMBER" value="7447714680/68uH"/>
</technology>
<technology name="_7447714681">
<attribute name="WE-NUMBER" value="7447714681/680uH"/>
</technology>
<technology name="_7447714820">
<attribute name="WE-NUMBER" value="7447714820/82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_1245" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; High Saturation currents up to 25 A
&lt;br&gt;
&lt;br&gt; Very low self-losses at high switching frequency‘s
&lt;br&gt;
&lt;br&gt; Wide inductances spectrum available at all sizes
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt; Integrated DC/DC- converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD?"&gt;http://katalog.we-online.de/en/pbs/WE-PD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD_1260/1245/1280/1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447715001">
<attribute name="WE-NUMBER" value="7447715001/1,8uH"/>
</technology>
<technology name="_7447715002">
<attribute name="WE-NUMBER" value="7447715002/2,5uH"/>
</technology>
<technology name="_7447715003">
<attribute name="WE-NUMBER" value="7447715003/3,3uH"/>
</technology>
<technology name="_7447715004">
<attribute name="WE-NUMBER" value="7447715004/4,7uH"/>
</technology>
<technology name="_7447715006">
<attribute name="WE-NUMBER" value="74477150066,8uH"/>
</technology>
<technology name="_7447715100">
<attribute name="WE-NUMBER" value="7447715100/10uH"/>
</technology>
<technology name="_7447715101">
<attribute name="WE-NUMBER" value="7447715101/100uH"/>
</technology>
<technology name="_7447715120">
<attribute name="WE-NUMBER" value="7447715120/12uH"/>
</technology>
<technology name="_7447715180">
<attribute name="WE-NUMBER" value="7447715180/18uH"/>
</technology>
<technology name="_7447715220">
<attribute name="WE-NUMBER" value="7447715220/22uH"/>
</technology>
<technology name="_7447715221">
<attribute name="WE-NUMBER" value="7447715221/220uH"/>
</technology>
<technology name="_7447715330">
<attribute name="WE-NUMBER" value="7447715330/33uH"/>
</technology>
<technology name="_7447715470">
<attribute name="WE-NUMBER" value="7447715470/47uH"/>
</technology>
<technology name="_7447715906">
<attribute name="WE-NUMBER" value="7447715906/6,8uH"/>
</technology>
<technology name="_7447715910">
<attribute name="WE-NUMBER" value="7447715910/1uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_1260" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; High Saturation currents up to 25 A
&lt;br&gt;
&lt;br&gt; Very low self-losses at high switching frequency‘s
&lt;br&gt;
&lt;br&gt; Wide inductances spectrum available at all sizes
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt; Integrated DC/DC- converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD?"&gt;http://katalog.we-online.de/en/pbs/WE-PD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD_1260/1245/1280/1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744771001">
<attribute name="WE-NUMBER" value="744771001/1,5uH"/>
</technology>
<technology name="_744771002">
<attribute name="WE-NUMBER" value="744771002/2,2uH"/>
</technology>
<technology name="_744771003">
<attribute name="WE-NUMBER" value="744771003/3,5uH"/>
</technology>
<technology name="_744771004">
<attribute name="WE-NUMBER" value="744771004/4,7uH"/>
</technology>
<technology name="_744771006">
<attribute name="WE-NUMBER" value="744771006/6,8uH"/>
</technology>
<technology name="_744771008">
<attribute name="WE-NUMBER" value="744771008/8,2uH"/>
</technology>
<technology name="_74477110">
<attribute name="WE-NUMBER" value="74477110/10uH"/>
</technology>
<technology name="_744771112">
<attribute name="WE-NUMBER" value="744771112/12uH"/>
</technology>
<technology name="_744771115">
<attribute name="WE-NUMBER" value="744771115/15uH"/>
</technology>
<technology name="_744771118">
<attribute name="WE-NUMBER" value="744771118/18uH"/>
</technology>
<technology name="_744771122">
<attribute name="WE-NUMBER" value="744771122/22uH"/>
</technology>
<technology name="_744771127">
<attribute name="WE-NUMBER" value="744771127/27uH"/>
</technology>
<technology name="_744771133">
<attribute name="WE-NUMBER" value="744771133/33uH"/>
</technology>
<technology name="_744771139">
<attribute name="WE-NUMBER" value="744771139/39uH"/>
</technology>
<technology name="_744771147">
<attribute name="WE-NUMBER" value="744771147/47uH"/>
</technology>
<technology name="_744771156">
<attribute name="WE-NUMBER" value="744771156/56uH"/>
</technology>
<technology name="_744771168">
<attribute name="WE-NUMBER" value="744771168/68uH"/>
</technology>
<technology name="_744771182">
<attribute name="WE-NUMBER" value="744771182/82uH"/>
</technology>
<technology name="_74477120">
<attribute name="WE-NUMBER" value="74477120/100uH"/>
</technology>
<technology name="_744771212">
<attribute name="WE-NUMBER" value="744771212/120uH"/>
</technology>
<technology name="_744771215">
<attribute name="WE-NUMBER" value="744771215/150uH"/>
</technology>
<technology name="_744771218">
<attribute name="WE-NUMBER" value="744771218/180uH"/>
</technology>
<technology name="_744771220">
<attribute name="WE-NUMBER" value="744771220/220uH"/>
</technology>
<technology name="_744771233">
<attribute name="WE-NUMBER" value="744771233/330uH"/>
</technology>
<technology name="_744771239">
<attribute name="WE-NUMBER" value="744771239/390uH"/>
</technology>
<technology name="_74477124">
<attribute name="WE-NUMBER" value="74477124/470uH"/>
</technology>
<technology name="_74477125">
<attribute name="WE-NUMBER" value="74477125/560uH"/>
</technology>
<technology name="_74477126">
<attribute name="WE-NUMBER" value="74477126/680uH"/>
</technology>
<technology name="_744771270">
<attribute name="WE-NUMBER" value="744771270/270uH"/>
</technology>
<technology name="_74477128">
<attribute name="WE-NUMBER" value="74477128/820uH"/>
</technology>
<technology name="_74477130">
<attribute name="WE-NUMBER" value="74477130/1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_1280" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; High Saturation currents up to 25 A
&lt;br&gt;
&lt;br&gt; Very low self-losses at high switching frequency‘s
&lt;br&gt;
&lt;br&gt; Wide inductances spectrum available at all sizes
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt; Integrated DC/DC- converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD?"&gt;http://katalog.we-online.de/en/pbs/WE-PD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD_1260/1245/1280/1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74477001">
<attribute name="WE-NUMBER" value="74477001/1,2uH"/>
</technology>
<technology name="_744770015">
<attribute name="WE-NUMBER" value="744770015/1,5uH"/>
</technology>
<technology name="_74477002">
<attribute name="WE-NUMBER" value="74477002/2,4uH"/>
</technology>
<technology name="_74477003">
<attribute name="WE-NUMBER" value="74477003/3,5uH"/>
</technology>
<technology name="_74477004">
<attribute name="WE-NUMBER" value="74477004/4,7uH"/>
</technology>
<technology name="_74477005">
<attribute name="WE-NUMBER" value="74477005/5,6uH"/>
</technology>
<technology name="_74477006">
<attribute name="WE-NUMBER" value="74477006/6,1uH"/>
</technology>
<technology name="_74477007">
<attribute name="WE-NUMBER" value="74477007/7,6uH"/>
</technology>
<technology name="_74477008">
<attribute name="WE-NUMBER" value="74477008/0,75uH"/>
</technology>
<technology name="_74477009">
<attribute name="WE-NUMBER" value="74477009/0,47uH"/>
</technology>
<technology name="_74477010">
<attribute name="WE-NUMBER" value="74477010/10uH"/>
</technology>
<technology name="_744770112">
<attribute name="WE-NUMBER" value="744770112/12uH"/>
</technology>
<technology name="_744770115">
<attribute name="WE-NUMBER" value="744770115/15uH"/>
</technology>
<technology name="_744770118">
<attribute name="WE-NUMBER" value="744770118/18uH"/>
</technology>
<technology name="_744770122">
<attribute name="WE-NUMBER" value="744770122/22uH"/>
</technology>
<technology name="_744770127">
<attribute name="WE-NUMBER" value="744770127/27uH"/>
</technology>
<technology name="_744770133">
<attribute name="WE-NUMBER" value="744770133/33uH"/>
</technology>
<technology name="_744770139">
<attribute name="WE-NUMBER" value="744770139/39uH"/>
</technology>
<technology name="_744770147">
<attribute name="WE-NUMBER" value="744770147/47uH"/>
</technology>
<technology name="_744770156">
<attribute name="WE-NUMBER" value="744770150/56uH"/>
</technology>
<technology name="_744770168">
<attribute name="WE-NUMBER" value="744770168/68uH"/>
</technology>
<technology name="_744770182">
<attribute name="WE-NUMBER" value="744770182/82uH"/>
</technology>
<technology name="_74477020">
<attribute name="WE-NUMBER" value="74477020/100uH"/>
</technology>
<technology name="_744770215">
<attribute name="WE-NUMBER" value="744770215/150uH"/>
</technology>
<technology name="_744770218">
<attribute name="WE-NUMBER" value="744770218/180uH"/>
</technology>
<technology name="_744770222">
<attribute name="WE-NUMBER" value="744770222/220uH"/>
</technology>
<technology name="_744770233">
<attribute name="WE-NUMBER" value="744770233/330uH"/>
</technology>
<technology name="_744770247">
<attribute name="WE-NUMBER" value="744770247/470uH"/>
</technology>
<technology name="_744770256">
<attribute name="WE-NUMBER" value="744770256/560uH"/>
</technology>
<technology name="_744770268">
<attribute name="WE-NUMBER" value="744770268/680uH"/>
</technology>
<technology name="_744770282">
<attribute name="WE-NUMBER" value="744770282/820uH"/>
</technology>
<technology name="_74477030">
<attribute name="WE-NUMBER" value="74477030/1000uH"/>
</technology>
<technology name="_744770315">
<attribute name="WE-NUMBER" value="744770315/1500uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_1210" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; High Saturation currents up to 25 A
&lt;br&gt;
&lt;br&gt; Very low self-losses at high switching frequency‘s
&lt;br&gt;
&lt;br&gt; Wide inductances spectrum available at all sizes
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt; Integrated DC/DC- converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD?"&gt;http://katalog.we-online.de/en/pbs/WE-PD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD_1260/1245/1280/1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447709001">
<attribute name="WE-NUMBER" value="7447709001/1uH"/>
</technology>
<technology name="_7447709002">
<attribute name="WE-NUMBER" value="7447709002/2,2uH"/>
</technology>
<technology name="_7447709003">
<attribute name="WE-NUMBER" value="7447709003/3,5uH"/>
</technology>
<technology name="_7447709004">
<attribute name="WE-NUMBER" value="7447709004/4,7uH"/>
</technology>
<technology name="_7447709006">
<attribute name="WE-NUMBER" value="7447709006/6,8uH"/>
</technology>
<technology name="_7447709100">
<attribute name="WE-NUMBER" value="7447709100/10uH"/>
</technology>
<technology name="_7447709101">
<attribute name="WE-NUMBER" value="7447709101/100uH"/>
</technology>
<technology name="_7447709102">
<attribute name="WE-NUMBER" value="7447709102/1000uH"/>
</technology>
<technology name="_7447709150">
<attribute name="WE-NUMBER" value="7447709150/15uH"/>
</technology>
<technology name="_7447709151">
<attribute name="WE-NUMBER" value="7447709151/150uH"/>
</technology>
<technology name="_7447709152">
<attribute name="WE-NUMBER" value="7447709152/1500uH"/>
</technology>
<technology name="_7447709220">
<attribute name="WE-NUMBER" value="7447709220/22uH"/>
</technology>
<technology name="_7447709221">
<attribute name="WE-NUMBER" value="7447709221/220uH"/>
</technology>
<technology name="_7447709270">
<attribute name="WE-NUMBER" value="7447709270/27uH"/>
</technology>
<technology name="_7447709271">
<attribute name="WE-NUMBER" value="7447709271/270uH"/>
</technology>
<technology name="_7447709330">
<attribute name="WE-NUMBER" value="7447709330/33uH"/>
</technology>
<technology name="_7447709331">
<attribute name="WE-NUMBER" value="7447709331/330uH"/>
</technology>
<technology name="_7447709390">
<attribute name="WE-NUMBER" value="7447709390/39uH"/>
</technology>
<technology name="_7447709470">
<attribute name="WE-NUMBER" value="7447709470/47uH"/>
</technology>
<technology name="_7447709471">
<attribute name="WE-NUMBER" value="7447709471/470uH"/>
</technology>
<technology name="_7447709680">
<attribute name="WE-NUMBER" value="7447709680/68uH"/>
</technology>
<technology name="_7447709681">
<attribute name="WE-NUMBER" value="7447709681/680uH"/>
</technology>
<technology name="_7447709820">
<attribute name="WE-NUMBER" value="7447709820/82uH"/>
</technology>
<technology name="_7447709821">
<attribute name="WE-NUMBER" value="7447709821/820uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_6033" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; High Saturation currents up to 25 A
&lt;br&gt;
&lt;br&gt; Very low self-losses at high switching frequency‘s
&lt;br&gt;
&lt;br&gt; Wide inductances spectrum available at all sizes
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt; Integrated DC/DC- converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD?"&gt;http://katalog.we-online.de/en/pbs/WE-PD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD_6033/6050_PLASTIC_BASE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447785001">
<attribute name="WE-NUMBER" value="7447785001/1uH"/>
</technology>
<technology name="_7447785002">
<attribute name="WE-NUMBER" value="7447785002/2,2uH"/>
</technology>
<technology name="_7447785003">
<attribute name="WE-NUMBER" value="7447785003/3,3uH"/>
</technology>
<technology name="_7447785004">
<attribute name="WE-NUMBER" value="7447785004/4,7uH"/>
</technology>
<technology name="_7447785006">
<attribute name="WE-NUMBER" value="7447785006/6,8uH"/>
</technology>
<technology name="_744778510">
<attribute name="WE-NUMBER" value="744778510/10uH"/>
</technology>
<technology name="_7447785115">
<attribute name="WE-NUMBER" value="7447785115/15uH"/>
</technology>
<technology name="_7447785122">
<attribute name="WE-NUMBER" value="7447785122/22uH"/>
</technology>
<technology name="_7447785127">
<attribute name="WE-NUMBER" value="7447785127/27uH"/>
</technology>
<technology name="_7447785133">
<attribute name="WE-NUMBER" value="7447785133/33uH"/>
</technology>
<technology name="_7447785147">
<attribute name="WE-NUMBER" value="7447785147/47uH"/>
</technology>
<technology name="_744778520">
<attribute name="WE-NUMBER" value="744778520/100uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_6050" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; High Saturation currents up to 25 A
&lt;br&gt;
&lt;br&gt; Very low self-losses at high switching frequency‘s
&lt;br&gt;
&lt;br&gt; Wide inductances spectrum available at all sizes
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt; Integrated DC/DC- converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD?"&gt;http://katalog.we-online.de/en/pbs/WE-PD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD_6033/6050_PLASTIC_BASE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447786001">
<attribute name="WE-NUMBER" value="7447786001/1uH"/>
</technology>
<technology name="_7447786002">
<attribute name="WE-NUMBER" value="7447786002/2,2uH"/>
</technology>
<technology name="_7447786004">
<attribute name="WE-NUMBER" value="7447786004/4,7uH"/>
</technology>
<technology name="_7447786006">
<attribute name="WE-NUMBER" value="7447786006/6,8uH"/>
</technology>
<technology name="_7447786008">
<attribute name="WE-NUMBER" value="7447786008/8,2uH"/>
</technology>
<technology name="_744778610">
<attribute name="WE-NUMBER" value="744778610/10uH"/>
</technology>
<technology name="_7447786122">
<attribute name="WE-NUMBER" value="7447786122/22uH"/>
</technology>
<technology name="_7447786147">
<attribute name="WE-NUMBER" value="7447786147/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_7332_PLASTIC" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; High Saturation currents up to 25 A
&lt;br&gt;
&lt;br&gt; Very low self-losses at high switching frequency‘s
&lt;br&gt;
&lt;br&gt; Wide inductances spectrum available at all sizes
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt; Integrated DC/DC- converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD?"&gt;http://katalog.we-online.de/en/pbs/WE-PD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD_7332/7345_PLASTIC_BASE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447789001">
<attribute name="WE-NUMBER" value="7447789001/1uH"/>
</technology>
<technology name="_7447789002">
<attribute name="WE-NUMBER" value="7447789002/2,2uH"/>
</technology>
<technology name="_7447789003">
<attribute name="WE-NUMBER" value="7447789003/3,3uH"/>
</technology>
<technology name="_7447789004">
<attribute name="WE-NUMBER" value="7447789004/4,7uH"/>
</technology>
<technology name="_7447789006">
<attribute name="WE-NUMBER" value="7447789006/6,8uH"/>
</technology>
<technology name="_744778910">
<attribute name="WE-NUMBER" value="744778910/10uH"/>
</technology>
<technology name="_7447789112">
<attribute name="WE-NUMBER" value="7447789112/12uH"/>
</technology>
<technology name="_7447789115">
<attribute name="WE-NUMBER" value="7447789115/15uH"/>
</technology>
<technology name="_7447789118">
<attribute name="WE-NUMBER" value="7447789118/18uH"/>
</technology>
<technology name="_7447789122">
<attribute name="WE-NUMBER" value="7447789122/22uH"/>
</technology>
<technology name="_7447789127">
<attribute name="WE-NUMBER" value="7447789127/27uH"/>
</technology>
<technology name="_7447789133">
<attribute name="WE-NUMBER" value="7447789133/33uH"/>
</technology>
<technology name="_7447789139">
<attribute name="WE-NUMBER" value="7447789139/39uH"/>
</technology>
<technology name="_7447789147">
<attribute name="WE-NUMBER" value="7447789147/47uH"/>
</technology>
<technology name="_7447789156">
<attribute name="WE-NUMBER" value="7447789156/56uH"/>
</technology>
<technology name="_7447789168">
<attribute name="WE-NUMBER" value="7447789168/68uH"/>
</technology>
<technology name="_7447789182">
<attribute name="WE-NUMBER" value="7447789182/82uH"/>
</technology>
<technology name="_744778920">
<attribute name="WE-NUMBER" value="744778920/100uH"/>
</technology>
<technology name="_7447789212">
<attribute name="WE-NUMBER" value="7447789212/120uH"/>
</technology>
<technology name="_7447789215">
<attribute name="WE-NUMBER" value="7447789215/150uH"/>
</technology>
<technology name="_7447789218">
<attribute name="WE-NUMBER" value="7447789218/18uH"/>
</technology>
<technology name="_7447789222">
<attribute name="WE-NUMBER" value="7447789222/220uH"/>
</technology>
<technology name="_7447789233">
<attribute name="WE-NUMBER" value="7447789233/330uH"/>
</technology>
<technology name="_7447789239">
<attribute name="WE-NUMBER" value="7447789239/390uH"/>
</technology>
<technology name="_744778924">
<attribute name="WE-NUMBER" value="744778924/470uH"/>
</technology>
<technology name="_744778925">
<attribute name="WE-NUMBER" value="744778925/560uH"/>
</technology>
<technology name="_744778926">
<attribute name="WE-NUMBER" value="744778926/680uH"/>
</technology>
<technology name="_7447789270">
<attribute name="WE-NUMBER" value="7447789270/270uH"/>
</technology>
<technology name="_744778928">
<attribute name="WE-NUMBER" value="744778928/820uH"/>
</technology>
<technology name="_744778930">
<attribute name="WE-NUMBER" value="744778930/1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_7345_PLASTIC" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; High Saturation currents up to 25 A
&lt;br&gt;
&lt;br&gt; Very low self-losses at high switching frequency‘s
&lt;br&gt;
&lt;br&gt; Wide inductances spectrum available at all sizes
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt; Integrated DC/DC- converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD?"&gt;http://katalog.we-online.de/en/pbs/WE-PD?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD_7332/7345_PLASTIC_BASE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447779001">
<attribute name="WE-NUMBER" value="7447779001/1uH"/>
</technology>
<technology name="_74477790015">
<attribute name="WE-NUMBER" value="74477790015/1,5uH"/>
</technology>
<technology name="_7447779002">
<attribute name="WE-NUMBER" value="7447779002/2,2uH"/>
</technology>
<technology name="_7447779003">
<attribute name="WE-NUMBER" value="7447779003/3,3uH"/>
</technology>
<technology name="_7447779004">
<attribute name="WE-NUMBER" value="7447779004/4,7uH"/>
</technology>
<technology name="_7447779006">
<attribute name="WE-NUMBER" value="7447779006/6,8uH"/>
</technology>
<technology name="_7447779008">
<attribute name="WE-NUMBER" value="744779008/8,2uH"/>
</technology>
<technology name="_744777910">
<attribute name="WE-NUMBER" value="744777910/10uH"/>
</technology>
<technology name="_7447779112">
<attribute name="WE-NUMBER" value="7447779112/12uH"/>
</technology>
<technology name="_7447779115">
<attribute name="WE-NUMBER" value="744779115/15uH"/>
</technology>
<technology name="_7447779118">
<attribute name="WE-NUMBER" value="7447779118/18uH"/>
</technology>
<technology name="_7447779122">
<attribute name="WE-NUMBER" value="7447779122/22uH"/>
</technology>
<technology name="_7447779127">
<attribute name="WE-NUMBER" value="7447779127/27uH"/>
</technology>
<technology name="_7447779133">
<attribute name="WE-NUMBER" value="7447779133/33uH"/>
</technology>
<technology name="_7447779139">
<attribute name="WE-NUMBER" value="7447779139/39uH"/>
</technology>
<technology name="_7447779147">
<attribute name="WE-NUMBER" value="7447779147/47uH"/>
</technology>
<technology name="_7447779156">
<attribute name="WE-NUMBER" value="7447779156/56uH"/>
</technology>
<technology name="_7447779168">
<attribute name="WE-NUMBER" value="7447779168/68uH"/>
</technology>
<technology name="_7447779182">
<attribute name="WE-NUMBER" value="7447779182/82uH"/>
</technology>
<technology name="_744777920">
<attribute name="WE-NUMBER" value="744777920/100uH"/>
</technology>
<technology name="_7447779212">
<attribute name="WE-NUMBER" value="7447779212/12uH"/>
</technology>
<technology name="_7447779215">
<attribute name="WE-NUMBER" value="7447779215/150uH"/>
</technology>
<technology name="_7447779218">
<attribute name="WE-NUMBER" value="7447779218/180uH"/>
</technology>
<technology name="_7447779222">
<attribute name="WE-NUMBER" value="7447779222/220uH"/>
</technology>
<technology name="_7447779233">
<attribute name="WE-NUMBER" value="7447779233/330uH"/>
</technology>
<technology name="_7447779239">
<attribute name="WE-NUMBER" value="7447779239/390uH"/>
</technology>
<technology name="_744777924">
<attribute name="WE-NUMBER" value="744777924/470uH"/>
</technology>
<technology name="_744777925">
<attribute name="WE-NUMBER" value="744777925/560uH"/>
</technology>
<technology name="_744777926">
<attribute name="WE-NUMBER" value="744777926/680uH"/>
</technology>
<technology name="_7447779270">
<attribute name="WE-NUMBER" value="7447779270/270uH"/>
</technology>
<technology name="_744777928">
<attribute name="WE-NUMBER" value="744777928/820uH"/>
</technology>
<technology name="_744777930">
<attribute name="WE-NUMBER" value="744777930/1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UCF_4TURNS" prefix="L" uservalue="yes">
<description>&lt;B&gt;WE-UCF SMD Common Mode Line Filter
&lt;Br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High inductance range
&lt;br&gt;
&lt;br&gt; High current range
&lt;br&gt;
&lt;br&gt; Small package
&lt;br&gt;
&lt;br&gt; Low profile
&lt;br&gt;
&lt;br&gt; Surface mount technology
&lt;br&gt; Wide range of filtering spectrum
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;Br&gt;&lt;/b&gt; Filtering
&lt;br&gt;
&lt;br&gt; DC power lines
&lt;br&gt;
&lt;br&gt; Buck-/Boost Converter filtering
&lt;br&gt;
&lt;br&gt; Data lines with low bitrate
&lt;br&gt;
&lt;br&gt; Heavily influenced lines
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndUCF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndUCF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-UCF?"&gt;http://katalog.we-online.de/en/pbs/WE-UCF?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-UCF">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="2" pad="9 10"/>
<connect gate="G$1" pin="3" pad="6 7"/>
<connect gate="G$1" pin="4" pad="4 5"/>
</connects>
<technologies>
<technology name="_744290121">
<attribute name="WE-NUMBER" value="74429012/2X0,12mH"/>
</technology>
<technology name="_744290130">
<attribute name="WE-NUMBER" value="744290130/2X0,013mH"/>
</technology>
<technology name="_744290560">
<attribute name="WE-NUMBER" value="744290560/2X0,056mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_HV_7345" prefix="L" uservalue="yes">
<description>&lt;b&gt;High Voltage SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Shielded part for ideal wire protection
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Magnetically schielded
&lt;br&gt;
&lt;br&gt; Designed for 400 VDC Applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Non-isolated buck or buck-boost converter like Power Integrations LinkSwitch-TN
&lt;br&gt;
&lt;br&gt; Constant current LED driver
&lt;br&gt;
&lt;br&gt; Utility metering
&lt;br&gt;
&lt;br&gt; Filter for power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD_HV.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD_HV.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD_HV?"&gt;http://katalog.we-online.de/en/pbs/WE-PD_HV?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD_7332/7345_PLASTIC_BASE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7687779102">
<attribute name="WE-NUMBER" value="7687779102/1000uH"/>
</technology>
<technology name="_7687779221">
<attribute name="WE-NUMBER" value="768779221/220uH"/>
</technology>
<technology name="_7687779471">
<attribute name="WE-NUMBER" value="768779471/470uH"/>
</technology>
<technology name="_7687779561">
<attribute name="WE-NUMBER" value="768779561/560uH"/>
</technology>
<technology name="_7687779681">
<attribute name="WE-NUMBER" value="7687779681/680uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_HV_1060" prefix="L" uservalue="yes">
<description>&lt;b&gt;High Voltage SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Shielded part for ideal wire protection
&lt;br&gt;
&lt;br&gt; Operating Temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Magnetically schielded
&lt;br&gt;
&lt;br&gt; Designed for 400 VDC Applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Non-isolated buck or buck-boost converter like Power Integrations LinkSwitch-TN
&lt;br&gt;
&lt;br&gt; Constant current LED driver
&lt;br&gt;
&lt;br&gt; Utility metering
&lt;br&gt;
&lt;br&gt; Filter for power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD_HV.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD_HV.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD_HV?"&gt;http://katalog.we-online.de/en/pbs/WE-PD_HV?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD_HV_1060">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7687714102">
<attribute name="WE-NUMBER" value="7687714102/1000uH"/>
</technology>
<technology name="_7687714152">
<attribute name="WE-NUMBER" value="7687714152/1500uH"/>
</technology>
<technology name="_7687714221">
<attribute name="WE-NUMBER" value="7687714221/220uH"/>
</technology>
<technology name="_7687714222">
<attribute name="WE-NUMBER" value="7687714222/2200uH"/>
</technology>
<technology name="_7687714471">
<attribute name="WE-NUMBER" value="7687714471/470uH"/>
</technology>
<technology name="_7687714681">
<attribute name="WE-NUMBER" value="7687714681/680uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2_5848" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Open size
&lt;br&gt;
&lt;br&gt; Saturation currents up to 14 A
&lt;br&gt;
&lt;br&gt; Low tolerances at high inductance values
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC-converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Optimal attenuation in MHz frequency range
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD2"&gt;http://katalog.we-online.de/en/pbs/WE-PD2&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2_5848/5820">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744774003">
<attribute name="WE-NUMBER" value="744774003/0,33uH"/>
</technology>
<technology name="_744774022">
<attribute name="WE-NUMBER" value="744774022/2,2uH"/>
</technology>
<technology name="_744774027">
<attribute name="WE-NUMBER" value="744774027/2,7uH"/>
</technology>
<technology name="_744774033">
<attribute name="WE-NUMBER" value="744774033/3,3uH"/>
</technology>
<technology name="_744774047">
<attribute name="WE-NUMBER" value="744774047/4,7uH"/>
</technology>
<technology name="_744774068">
<attribute name="WE-NUMBER" value="744774068/6,8uH"/>
</technology>
<technology name="_74477410">
<attribute name="WE-NUMBER" value="74477410/10uH"/>
</technology>
<technology name="_744774112">
<attribute name="WE-NUMBER" value="744774112/12uH"/>
</technology>
<technology name="_744774115">
<attribute name="WE-NUMBER" value="744774115/15uH"/>
</technology>
<technology name="_744774118">
<attribute name="WE-NUMBER" value="744774118/18uH"/>
</technology>
<technology name="_744774122">
<attribute name="WE-NUMBER" value="744774122/22uH"/>
</technology>
<technology name="_744774127">
<attribute name="WE-NUMBER" value="744774127/27uH"/>
</technology>
<technology name="_744774133">
<attribute name="WE-NUMBER" value="744774133/33uH"/>
</technology>
<technology name="_744774139">
<attribute name="WE-NUMBER" value="744774139/39uF"/>
</technology>
<technology name="_744774147">
<attribute name="WE-NUMBER" value="744774147/47uH"/>
</technology>
<technology name="_744774156">
<attribute name="WE-NUMBER" value="744774156/56uH"/>
</technology>
<technology name="_744774168">
<attribute name="WE-NUMBER" value="744774168/68uH"/>
</technology>
<technology name="_744774182">
<attribute name="WE-NUMBER" value="744774182/82uH"/>
</technology>
<technology name="_74477420">
<attribute name="WE-NUMBER" value="74477420/100uH"/>
</technology>
<technology name="_744774212">
<attribute name="WE-NUMBER" value="744774212/12uH"/>
</technology>
<technology name="_744774215">
<attribute name="WE-NUMBER" value="744774215/150uH"/>
</technology>
<technology name="_744774218">
<attribute name="WE-NUMBER" value="744774218/180uH"/>
</technology>
<technology name="_744774222">
<attribute name="WE-NUMBER" value="744774222/220uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2_7850" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Open size
&lt;br&gt;
&lt;br&gt; Saturation currents up to 14 A
&lt;br&gt;
&lt;br&gt; Low tolerances at high inductance values
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC-converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Optimal attenuation in MHz frequency range
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD2"&gt;http://katalog.we-online.de/en/pbs/WE-PD2&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2_7850">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744775022">
<attribute name="WE-NUMBER" value="744775022/2,2uH"/>
</technology>
<technology name="_744775033">
<attribute name="WE-NUMBER" value="744775033/3,3uH"/>
</technology>
<technology name="_744775047">
<attribute name="WE-NUMBER" value="744775047/4,7uH"/>
</technology>
<technology name="_744775056">
<attribute name="WE-NUMBER" value="744775056/5,6uH"/>
</technology>
<technology name="_744775068">
<attribute name="WE-NUMBER" value="744775068/6,8uH"/>
</technology>
<technology name="_744775082">
<attribute name="WE-NUMBER" value="744775082/8,2uH"/>
</technology>
<technology name="_74477510">
<attribute name="WE-NUMBER" value="74477510/10uH"/>
</technology>
<technology name="_744775112">
<attribute name="WE-NUMBER" value="744775112/12uH"/>
</technology>
<technology name="_744775115">
<attribute name="WE-NUMBER" value="744775115/15uH"/>
</technology>
<technology name="_744775118">
<attribute name="WE-NUMBER" value="744775118/18uH"/>
</technology>
<technology name="_744775122">
<attribute name="WE-NUMBER" value="744775122/22uH"/>
</technology>
<technology name="_744775127">
<attribute name="WE-NUMBER" value="744775127/27uH"/>
</technology>
<technology name="_744775133">
<attribute name="WE-NUMBER" value="744775133/33uH"/>
</technology>
<technology name="_744775139">
<attribute name="WE-NUMBER" value="744775139/39uH"/>
</technology>
<technology name="_744775147">
<attribute name="WE-NUMBER" value="744775147/47uH"/>
</technology>
<technology name="_744775156">
<attribute name="WE-NUMBER" value="744775156/56uH"/>
</technology>
<technology name="_744775168">
<attribute name="WE-NUMBER" value="744775168/68uH"/>
</technology>
<technology name="_744775182">
<attribute name="WE-NUMBER" value="744775182/82uH"/>
</technology>
<technology name="_74477520">
<attribute name="WE-NUMBER" value="74477520/100uH"/>
</technology>
<technology name="_744775210">
<attribute name="WE-NUMBER" value="744775210/120uH"/>
</technology>
<technology name="_744775215">
<attribute name="WE-NUMBER" value="744775215/150uH"/>
</technology>
<technology name="_744775218">
<attribute name="WE-NUMBER" value="744775218/180uH"/>
</technology>
<technology name="_744775222">
<attribute name="WE-NUMBER" value="744776222/220uH"/>
</technology>
<technology name="_744775227">
<attribute name="WE-NUMBER" value="744775227/270uH"/>
</technology>
<technology name="_744775233">
<attribute name="WE-NUMBER" value="744775233/330uH"/>
</technology>
<technology name="_744775239">
<attribute name="WE-NUMBER" value="744775239/390uH"/>
</technology>
<technology name="_744775247">
<attribute name="WE-NUMBER" value="744775247/470uH"/>
</technology>
<technology name="_74477530">
<attribute name="WE-NUMBER" value="74477530/1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2_4532" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Open size
&lt;br&gt;
&lt;br&gt; Saturation currents up to 14 A
&lt;br&gt;
&lt;br&gt; Low tolerances at high inductance values
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC-converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Optimal attenuation in MHz frequency range
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD2"&gt;http://katalog.we-online.de/en/pbs/WE-PD2&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2_4532">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447730">
<attribute name="WE-NUMBER" value="7447730/1uH"/>
</technology>
<technology name="_744773014">
<attribute name="WE-NUMBER" value="744773014/1,4uH"/>
</technology>
<technology name="_744773018">
<attribute name="WE-NUMBER" value="744773018/1,8uH"/>
</technology>
<technology name="_744773022">
<attribute name="WE-NUMBER" value="744773022/2,2uH"/>
</technology>
<technology name="_744773027">
<attribute name="WE-NUMBER" value="744773027/2,7uH"/>
</technology>
<technology name="_744773033">
<attribute name="WE-NUMBER" value="744773033/3,3uH"/>
</technology>
<technology name="_744773039">
<attribute name="WE-NUMBER" value="744773039/3,9uH"/>
</technology>
<technology name="_744773047">
<attribute name="WE-NUMBER" value="744773047/4,7uH"/>
</technology>
<technology name="_744773056">
<attribute name="WE-NUMBER" value="744773056/5,6uH"/>
</technology>
<technology name="_744773068">
<attribute name="WE-NUMBER" value="744773068/6.8uH"/>
</technology>
<technology name="_744773082">
<attribute name="WE-NUMBER" value="744773082/8,2uH"/>
</technology>
<technology name="_74477310">
<attribute name="WE-NUMBER" value="74477310/10uH"/>
</technology>
<technology name="_744773112">
<attribute name="WE-NUMBER" value="744773112/12uH"/>
</technology>
<technology name="_744773115">
<attribute name="WE-NUMBER" value="744773115/15uH"/>
</technology>
<technology name="_744773118">
<attribute name="WE-NUMBER" value="744773118/18uH"/>
</technology>
<technology name="_744773122">
<attribute name="WE-NUMBER" value="744773122/22uH"/>
</technology>
<technology name="_744773127">
<attribute name="WE-NUMBER" value="744773127/27uH"/>
</technology>
<technology name="_744773133">
<attribute name="WE-NUMBER" value="744773133/33uH"/>
</technology>
<technology name="_744773139">
<attribute name="WE-NUMBER" value="744773139/39uH"/>
</technology>
<technology name="_744773147">
<attribute name="WE-NUMBER" value="744773147/47uH"/>
</technology>
<technology name="_744773156">
<attribute name="WE-NUMBER" value="744773156/56uH"/>
</technology>
<technology name="_744773168">
<attribute name="WE-NUMBER" value="744773168/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2_HV_7850" prefix="L" uservalue="yes">
<description>&lt;b&gt;High Voltage SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Unshielded construction
&lt;br&gt;
&lt;br&gt; Designed for 400 VDC
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Non-isolated buck or buck-boost converter like Power Integrations LinkSwitch-TN
&lt;br&gt;
&lt;br&gt; Constant current LED driver
&lt;br&gt;
&lt;br&gt; Utility metering
&lt;br&gt;
&lt;br&gt; Filter for power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD2_HV?"&gt;http://katalog.we-online.de/en/pbs/WE-PD2_HV?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2_7850">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_768775256">
<attribute name="WE-NUMBER" value="768775256/560uH"/>
</technology>
<technology name="_768775268">
<attribute name="WE-NUMBER" value="768775268/680uH"/>
</technology>
<technology name="_768775282">
<attribute name="WE-NUMBER" value="768775282/820uH"/>
</technology>
<technology name="_76877530">
<attribute name="WE-NUMBER" value="76877530/1000uH"/>
</technology>
<technology name="_768775312">
<attribute name="WE-NUMBER" value="768775315/1200uH"/>
</technology>
<technology name="_768775322">
<attribute name="WE-NUMBER" value="768775322/2200uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD3_L" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; Working frequency up to 10 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; EMI-filter
&lt;br&gt;
&lt;br&gt; Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Texas Instruments, Maxim, Semtech, ON Semiconductor, Cologne Chip, STMicroelectronics, Maxim, MPS, Diodes, Analogic Tech and Exar
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-pd3_smd_speicherdrossel.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-pd3_smd_speicherdrossel.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD3?"&gt;http://katalog.we-online.de/en/pbs/WE-PD3?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD3_L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74454010">
<attribute name="WE-NUMBER" value="74454010/10uH"/>
</technology>
<technology name="_7445402">
<attribute name="WE-NUMBER" value="7445402/2,2uH"/>
</technology>
<technology name="_7445403">
<attribute name="WE-NUMBER" value="7445403/3uH"/>
</technology>
<technology name="_7445404">
<attribute name="WE-NUMBER" value="7445404/4,7uH"/>
</technology>
<technology name="_74454068">
<attribute name="WE-NUMBER" value="74454068/7uH"/>
</technology>
<technology name="_74454115">
<attribute name="WE-NUMBER" value="74454115/15uH"/>
</technology>
<technology name="_74454122">
<attribute name="WE-NUMBER" value="74454122/22uH"/>
</technology>
<technology name="_74454133">
<attribute name="WE-NUMBER" value="74454133/33uH"/>
</technology>
<technology name="_74454147">
<attribute name="WE-NUMBER" value="74454147/47uH"/>
</technology>
<technology name="_74454168">
<attribute name="WE-NUMBER" value="74454168/68uH"/>
</technology>
<technology name="_7445420">
<attribute name="WE-NUMBER" value="7445420/100uH"/>
</technology>
<technology name="_74454215">
<attribute name="WE-NUMBER" value="74454215/150uH"/>
</technology>
<technology name="_74454220">
<attribute name="WE-NUMBER" value="74454220/220uH"/>
</technology>
<technology name="_74454233">
<attribute name="WE-NUMBER" value="74454233/330uH"/>
</technology>
<technology name="_74454239">
<attribute name="WE-NUMBER" value="74454239/390uH"/>
</technology>
<technology name="_74454247">
<attribute name="WE-NUMBER" value="74454247/470uH"/>
</technology>
<technology name="_74454268">
<attribute name="WE-NUMBER" value="74454268/680uH"/>
</technology>
<technology name="_7445430">
<attribute name="WE-NUMBER" value="7445430/1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD3_M" prefix="M" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; Working frequency up to 10 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; EMI-filter
&lt;br&gt;
&lt;br&gt; Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Texas Instruments, Maxim, Semtech, ON Semiconductor, Cologne Chip, STMicroelectronics, Maxim, MPS, Diodes, Analogic Tech and Exar
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-pd3_smd_speicherdrossel.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-pd3_smd_speicherdrossel.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD3?"&gt;http://katalog.we-online.de/en/pbs/WE-PD3?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD3_M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7445301">
<attribute name="WE-NUMBER" value="7445301/1,5uH"/>
</technology>
<technology name="_74453010">
<attribute name="WE-NUMBER" value="74453010/10uH"/>
</technology>
<technology name="_7445302">
<attribute name="WE-NUMBER" value="7445302/2,2uH"/>
</technology>
<technology name="_7445303">
<attribute name="WE-NUMBER" value="7445303/3,9uH"/>
</technology>
<technology name="_74453031">
<attribute name="WE-NUMBER" value="74453031/3,3uH"/>
</technology>
<technology name="_7445304">
<attribute name="WE-NUMBER" value="7445304/4,7uH"/>
</technology>
<technology name="_7445306">
<attribute name="WE-NUMBER" value="7445306/6,8uH"/>
</technology>
<technology name="_74453112">
<attribute name="WE-NUMBER" value="74453112/12uH"/>
</technology>
<technology name="_74453115">
<attribute name="WE-NUMBER" value="74453115/15uH"/>
</technology>
<technology name="_74453122">
<attribute name="WE-NUMBER" value="74453122/22uH"/>
</technology>
<technology name="_74453133">
<attribute name="WE-NUMBER" value="74453133/33uH"/>
</technology>
<technology name="_74453147">
<attribute name="WE-NUMBER" value="74453147/47uH"/>
</technology>
<technology name="_74453156">
<attribute name="WE-NUMBER" value="74453156/56uH"/>
</technology>
<technology name="_74453168">
<attribute name="WE-NUMBER" value="74453168/68uH"/>
</technology>
<technology name="_74453182">
<attribute name="WE-NUMBER" value="74453182/82uH"/>
</technology>
<technology name="_7445320">
<attribute name="WE-NUMBER" value="7445320/100uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD3_S" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetically shielded version which results in a low leakage field
&lt;br&gt;
&lt;br&gt; Working frequency up to 10 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; EMI-filter
&lt;br&gt;
&lt;br&gt; Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Texas Instruments, Maxim, Semtech, ON Semiconductor, Cologne Chip, STMicroelectronics, Maxim, MPS, Diodes, Analogic Tech and Exar
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-pd3_smd_speicherdrossel.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-pd3_smd_speicherdrossel.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD3?"&gt;http://katalog.we-online.de/en/pbs/WE-PD3?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD3_S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7445101">
<attribute name="WE-NUMBER" value="7445101/1uH"/>
</technology>
<technology name="_74451015">
<attribute name="WE-NUMBER" value="74451015/1,5uH"/>
</technology>
<technology name="_74451022">
<attribute name="WE-NUMBER" value="74451022/2,2uH"/>
</technology>
<technology name="_74451033">
<attribute name="WE-NUMBER" value="74451033/3,3uH"/>
</technology>
<technology name="_74451039">
<attribute name="WE-NUMBER" value="74451039/3,9uH"/>
</technology>
<technology name="_74451047">
<attribute name="WE-NUMBER" value="74451047/4,7uH"/>
</technology>
<technology name="_74451068">
<attribute name="WE-NUMBER" value="74451068/6,8uH"/>
</technology>
<technology name="_7445110">
<attribute name="WE-NUMBER" value="7445110/10uH"/>
</technology>
<technology name="_74451115">
<attribute name="WE-NUMBER" value="74451115/15uH"/>
</technology>
<technology name="_74451122">
<attribute name="WE-NUMBER" value="74451122/22uH"/>
</technology>
<technology name="_74451133">
<attribute name="WE-NUMBER" value="74451133/33uH"/>
</technology>
<technology name="_74451147">
<attribute name="WE-NUMBER" value="74451147/4,7uH"/>
</technology>
<technology name="_74451168">
<attribute name="WE-NUMBER" value="74451168/68uH"/>
</technology>
<technology name="_7445120">
<attribute name="WE-NUMBER" value="7445120/12uH"/>
</technology>
<technology name="_74451215">
<attribute name="WE-NUMBER" value="74451215/150uH"/>
</technology>
<technology name="_74451222">
<attribute name="WE-NUMBER" value="74451222/220uH"/>
</technology>
<technology name="_74451233">
<attribute name="WE-NUMBER" value="74451233/330uH"/>
</technology>
<technology name="_74451247">
<attribute name="WE-NUMBER" value="74451247/470uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD4_S" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Current loading up to 38 A
&lt;br&gt;
&lt;br&gt; Compact size
&lt;br&gt;
&lt;br&gt; Low-loss ferrite core
&lt;br&gt;
&lt;br&gt; Application frequency range up to 10 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Noise suppression
&lt;br&gt;
&lt;br&gt; Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Maxim, Semtech, Texas Instruments, Fairchild Semiconductor, Cologne Chip, ON Semiconductor, STMicroelectronics, MPS, Exar, Analogic Tech and Diodes
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="hhttp://katalog.we-online.de/media/images/v2/Family_WE-PD4.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD4.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD4?"&gt;http://katalog.we-online.de/en/pbs/WE-PD4?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD3_S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7445501">
<attribute name="WE-NUMBER" value="7445501/1uH"/>
</technology>
<technology name="_74455015">
<attribute name="WE-NUMBER" value="74455015/1,5uH"/>
</technology>
<technology name="_74455022">
<attribute name="WE-NUMBER" value="74455022/2,2uH"/>
</technology>
<technology name="_74455033">
<attribute name="WE-NUMBER" value="74455033/3,3uH"/>
</technology>
<technology name="_74455047">
<attribute name="WE-NUMBER" value="74455047/4,7uH"/>
</technology>
<technology name="_74455068">
<attribute name="WE-NUMBER" value="74455068/6,8uH"/>
</technology>
<technology name="_7445510">
<attribute name="WE-NUMBER" value="7445510/10uH"/>
</technology>
<technology name="_74455115">
<attribute name="WE-NUMBER" value="74455115/15uH"/>
</technology>
<technology name="_74455122">
<attribute name="WE-NUMBER" value="74455122/22uH"/>
</technology>
<technology name="_74455133">
<attribute name="WE-NUMBER" value="74455133/33uH"/>
</technology>
<technology name="_74455147">
<attribute name="WE-NUMBER" value="74455147/47uH"/>
</technology>
<technology name="_74455168">
<attribute name="WE-NUMBER" value="74455168/68uH"/>
</technology>
<technology name="_7445520">
<attribute name="WE-NUMBER" value="7445520/100uH"/>
</technology>
<technology name="_74455215">
<attribute name="WE-NUMBER" value="74455215/150uH"/>
</technology>
<technology name="_74455222">
<attribute name="WE-NUMBER" value="74455222/220uH"/>
</technology>
<technology name="_74455233">
<attribute name="WE-NUMBER" value="74455233/330uH"/>
</technology>
<technology name="_74455247">
<attribute name="WE-NUMBER" value="74455247/470uH"/>
</technology>
<technology name="_7445530">
<attribute name="WE-NUMBER" value="7445530/1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD4_X" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Current loading up to 38 A
&lt;br&gt;
&lt;br&gt; Compact size
&lt;br&gt;
&lt;br&gt; Low-loss ferrite core
&lt;br&gt;
&lt;br&gt; Application frequency range up to 10 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Noise suppression
&lt;br&gt;
&lt;br&gt; Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Maxim, Semtech, Texas Instruments, Fairchild Semiconductor, Cologne Chip, ON Semiconductor, STMicroelectronics, MPS, Exar, Analogic Tech and Diodes
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="hhttp://katalog.we-online.de/media/images/v2/Family_WE-PD4.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD4.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD4?"&gt;http://katalog.we-online.de/en/pbs/WE-PD4?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD3_X">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74458001">
<attribute name="WE-NUMBER" value="74458001/1uH"/>
</technology>
<technology name="_74458002">
<attribute name="WE-NUMBER" value="74458002/2,2uH"/>
</technology>
<technology name="_74458003">
<attribute name="WE-NUMBER" value="74458003/3,3uH"/>
</technology>
<technology name="_74458005">
<attribute name="WE-NUMBER" value="74458005/5,6uH"/>
</technology>
<technology name="_74458010">
<attribute name="WE-NUMBER" value="74458010/10uH"/>
</technology>
<technology name="_74458115">
<attribute name="WE-NUMBER" value="74458115/15uH"/>
</technology>
<technology name="_74458122">
<attribute name="WE-NUMBER" value="74458122/22uH"/>
</technology>
<technology name="_74458133">
<attribute name="WE-NUMBER" value="74458133/33uH"/>
</technology>
<technology name="_74458147">
<attribute name="WE-NUMBER" value="74458147/47uH"/>
</technology>
<technology name="_74458168">
<attribute name="WE-NUMBER" value="74458168/68uH"/>
</technology>
<technology name="_7445820">
<attribute name="WE-NUMBER" value="7445820/100uH"/>
</technology>
<technology name="_74458215">
<attribute name="WE-NUMBER" value="74458215/150uH"/>
</technology>
<technology name="_74458220">
<attribute name="WE-NUMBER" value="74458220/220uH"/>
</technology>
<technology name="_74458233">
<attribute name="WE-NUMBER" value="74458233/330uH"/>
</technology>
<technology name="_74458247">
<attribute name="WE-NUMBER" value="74458247/470uH"/>
</technology>
<technology name="_74458268">
<attribute name="WE-NUMBER" value="74458268/680uH"/>
</technology>
<technology name="_7445830">
<attribute name="WE-NUMBER" value="7445830/1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD4_XL" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Current loading up to 38 A
&lt;br&gt;
&lt;br&gt; Compact size
&lt;br&gt;
&lt;br&gt; Low-loss ferrite core
&lt;br&gt;
&lt;br&gt; Application frequency range up to 10 MHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Noise suppression
&lt;br&gt;
&lt;br&gt; Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Maxim, Semtech, Texas Instruments, Fairchild Semiconductor, Cologne Chip, ON Semiconductor, STMicroelectronics, MPS, Exar, Analogic Tech and Diodes
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="hhttp://katalog.we-online.de/media/images/v2/Family_WE-PD4.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD4.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD4?"&gt;http://katalog.we-online.de/en/pbs/WE-PD4?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD4_XL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74457006">
<attribute name="WE-NUMBER" value="74457006/0,47uH"/>
</technology>
<technology name="_74457008">
<attribute name="WE-NUMBER" value="74457008/0,8uH"/>
</technology>
<technology name="_74457010">
<attribute name="WE-NUMBER" value="74457010/1uH"/>
</technology>
<technology name="_74457012">
<attribute name="WE-NUMBER" value="74457012/1,2uH"/>
</technology>
<technology name="_74457018">
<attribute name="WE-NUMBER" value="74457018/1,8uH"/>
</technology>
<technology name="_74457027">
<attribute name="WE-NUMBER" value="74457027/2,7uH"/>
</technology>
<technology name="_74457033">
<attribute name="WE-NUMBER" value="74457033/3,3uH"/>
</technology>
<technology name="_74457047">
<attribute name="WE-NUMBER" value="74457047/4,7uH"/>
</technology>
<technology name="_74457056">
<attribute name="WE-NUMBER" value="74457056/5,6uH"/>
</technology>
<technology name="_74457068">
<attribute name="WE-NUMBER" value="74457068/6,8uH"/>
</technology>
<technology name="_74457082">
<attribute name="WE-NUMBER" value="74457082/8,2uH"/>
</technology>
<technology name="_7445710">
<attribute name="WE-NUMBER" value="7445710/10uH"/>
</technology>
<technology name="_74457112">
<attribute name="WE-NUMBER" value="74457112/12uH"/>
</technology>
<technology name="_74457115">
<attribute name="WE-NUMBER" value="74457115/15uH"/>
</technology>
<technology name="_74457118">
<attribute name="WE-NUMBER" value="74457118/18uH"/>
</technology>
<technology name="_74457122">
<attribute name="WE-NUMBER" value="74457122/22uH"/>
</technology>
<technology name="_74457127">
<attribute name="WE-NUMBER" value="74457127/27uH"/>
</technology>
<technology name="_74457133">
<attribute name="WE-NUMBER" value="74457133/33uH"/>
</technology>
<technology name="_74457139">
<attribute name="WE-NUMBER" value="74457139/39uH"/>
</technology>
<technology name="_74457147">
<attribute name="WE-NUMBER" value="74457147/47uH"/>
</technology>
<technology name="_74457156">
<attribute name="WE-NUMBER" value="74457156/56uH"/>
</technology>
<technology name="_74457168">
<attribute name="WE-NUMBER" value="74457168/68uH"/>
</technology>
<technology name="_74457182">
<attribute name="WE-NUMBER" value="74457182/82uH"/>
</technology>
<technology name="_7445720">
<attribute name="WE-NUMBER" value="7445720/100uH"/>
</technology>
<technology name="_74457212">
<attribute name="WE-NUMBER" value="74457212/120uH"/>
</technology>
<technology name="_74457215">
<attribute name="WE-NUMBER" value="74457215/150uH"/>
</technology>
<technology name="_74457218">
<attribute name="WE-NUMBER" value="74457218/180uH"/>
</technology>
<technology name="_74457222">
<attribute name="WE-NUMBER" value="74457268/680uH"/>
</technology>
<technology name="_74457227">
<attribute name="WE-NUMBER" value="74457227/270uH"/>
</technology>
<technology name="_74457230">
<attribute name="WE-NUMBER" value="74457230/1000uH"/>
</technology>
<technology name="_74457233">
<attribute name="WE-NUMBER" value="74457233/330uH"/>
</technology>
<technology name="_74457239">
<attribute name="WE-NUMBER" value="74457239/390uH"/>
</technology>
<technology name="_74457247">
<attribute name="WE-NUMBER" value="74457247/470uH"/>
</technology>
<technology name="_74457256">
<attribute name="WE-NUMBER" value="74457256/560uH"/>
</technology>
<technology name="_74457268">
<attribute name="WE-NUMBER" value="74457268/680uH"/>
</technology>
<technology name="_74457282">
<attribute name="WE-NUMBER" value="74457282/820uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDF_1064" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Flatwire Power Inductor
&lt;br&gt; 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Core material: NiZn
&lt;br&gt;
&lt;br&gt; Flat wire power inductor
&lt;br&gt;
&lt;br&gt; Advanced operating temperature: –40 °C up to +150 °C
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;br&gt; Low self-losses
&lt;br&gt;
&lt;br&gt; High saturation current
&lt;br&gt;
&lt;br&gt; Flat wire coil for lower losses at high frequency ranges
&lt;br&gt;
&lt;br&gt; High Self Resonance Frequency
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Suitable for high frequency switching regulators
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PDF%20Gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PDF%20Gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PDF?"&gt;http://katalog.we-online.de/en/pbs/WE-PDF?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PDF">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447798022">
<attribute name="WE-NUMBER" value="7447798022/0,22uH"/>
</technology>
<technology name="_7447798050">
<attribute name="WE-NUMBER" value="7447798050/0,5uH"/>
</technology>
<technology name="_7447798110">
<attribute name="WE-NUMBER" value="7447798110/1,1uH"/>
</technology>
<technology name="_7447798111">
<attribute name="WE-NUMBER" value="7447798111/11uH"/>
</technology>
<technology name="_7447798131">
<attribute name="WE-NUMBER" value="7447798131/13uH"/>
</technology>
<technology name="_7447798151">
<attribute name="WE-NUMBER" value="7447798151/15uH"/>
</technology>
<technology name="_7447798180">
<attribute name="WE-NUMBER" value="7447798180/1,8uH"/>
</technology>
<technology name="_7447798181">
<attribute name="WE-NUMBER" value="7447798181/18uH"/>
</technology>
<technology name="_7447798221">
<attribute name="WE-NUMBER" value="7447798221/22uH"/>
</technology>
<technology name="_7447798241">
<attribute name="WE-NUMBER" value="7447798241/24uH"/>
</technology>
<technology name="_7447798250">
<attribute name="WE-NUMBER" value="7447798250/2,5uH"/>
</technology>
<technology name="_7447798271">
<attribute name="WE-NUMBER" value="7447798271/27uH"/>
</technology>
<technology name="_7447798360">
<attribute name="WE-NUMBER" value="7447798360/3,6uH"/>
</technology>
<technology name="_7447798470">
<attribute name="WE-NUMBER" value="7447798470/4,7uH"/>
</technology>
<technology name="_7447798620">
<attribute name="WE-NUMBER" value="7447798620/6,2uH"/>
</technology>
<technology name="_7447798720">
<attribute name="WE-NUMBER" value="7447798720/7,2uH"/>
</technology>
<technology name="_7447798910">
<attribute name="WE-NUMBER" value="7447798910/9,1uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMCI_0603LP" prefix="L" uservalue="yes">
<description>&lt;br&gt;&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PMCI Power Molded Chip
Inductor&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;
&lt;br&gt;Compact inductor chip type
&lt;br&gt;High effciency
&lt;br&gt;Suitable for applications with high currents up to 3.6 A. Very high DC-Bias current
&lt;br&gt;Very small electrical resistance, smallest RDC-Values starting at 19 mΩ
&lt;br&gt;Magnetically shielded construction: No crosstalk
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Available in five sizes and three different types (Low Profile, Standard and High Saturation Current)
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMCI"&gt;http://katalog.we-online.de/en/pbs/WE-PMCI&lt;/a&gt;&lt;p&gt;

&lt;br&gt;&lt;/b&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_0603_74479262XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479262147">
<attribute name="WE-NUMBER" value="74479262147/0,47uH"/>
</technology>
<technology name="_74479262210">
<attribute name="WE-NUMBER" value="74479262210/1uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMCI_0805" prefix="L" uservalue="yes">
<description>&lt;br&gt;&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PMCI Power Molded Chip
Inductor&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;
&lt;br&gt;Compact inductor chip type
&lt;br&gt;High effciency
&lt;br&gt;Suitable for applications with high currents up to 3.6 A. Very high DC-Bias current
&lt;br&gt;Very small electrical resistance, smallest RDC-Values starting at 19 mΩ
&lt;br&gt;Magnetically shielded construction: No crosstalk
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Available in five sizes and three different types (Low Profile, Standard and High Saturation Current)
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMCI"&gt;http://katalog.we-online.de/en/pbs/WE-PMCI&lt;/a&gt;&lt;p&gt;

&lt;br&gt;&lt;/b&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_0805_74479275XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479275147">
<attribute name="WE-NUMBER" value="74479275147/0,47uH"/>
</technology>
<technology name="_74479275210">
<attribute name="WE-NUMBER" value="74479275210/1uH"/>
</technology>
<technology name="_74479275222">
<attribute name="WE-NUMBER" value="74479275222/2,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMCI_0806" prefix="L" uservalue="yes">
<description>&lt;br&gt;&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PMCI Power Molded Chip
Inductor&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;
&lt;br&gt;Compact inductor chip type
&lt;br&gt;High effciency
&lt;br&gt;Suitable for applications with high currents up to 3.6 A. Very high DC-Bias current
&lt;br&gt;Very small electrical resistance, smallest RDC-Values starting at 19 mΩ
&lt;br&gt;Magnetically shielded construction: No crosstalk
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Available in five sizes and three different types (Low Profile, Standard and High Saturation Current)
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMCI"&gt;http://katalog.we-online.de/en/pbs/WE-PMCI&lt;/a&gt;&lt;p&gt;

&lt;br&gt;&lt;/b&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_0806_74479276XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479276124">
<attribute name="WE-NUMBER" value="74479276124/0,24uH"/>
</technology>
<technology name="_74479276147">
<attribute name="WE-NUMBER" value="74479276147/0,47uH"/>
</technology>
<technology name="_74479276168">
<attribute name="WE-NUMBER" value="74479276168/0,68uH"/>
</technology>
<technology name="_74479276210">
<attribute name="WE-NUMBER" value="74479276210/1uH"/>
</technology>
<technology name="_74479276222">
<attribute name="WE-NUMBER" value="74479276222/2,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMCI_0806LR" prefix="L" uservalue="yes">
<description>&lt;br&gt;&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PMCI Power Molded Chip
Inductor&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;
&lt;br&gt;Compact inductor chip type
&lt;br&gt;High effciency
&lt;br&gt;Suitable for applications with high currents up to 3.6 A. Very high DC-Bias current
&lt;br&gt;Very small electrical resistance, smallest RDC-Values starting at 19 mΩ
&lt;br&gt;Magnetically shielded construction: No crosstalk
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Available in five sizes and three different types (Low Profile, Standard and High Saturation Current)
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMCI"&gt;http://katalog.we-online.de/en/pbs/WE-PMCI&lt;/a&gt;&lt;p&gt;

&lt;br&gt;&lt;/b&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_0806_74479276XXXC">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479276147C">
<attribute name="WE-NUMBER" value="74479276147C/0,47uH"/>
</technology>
<technology name="_74479276210C">
<attribute name="WE-NUMBER" value="74479276210C/1uH"/>
</technology>
<technology name="_74479276222C">
<attribute name="WE-NUMBER" value="74479276222C/2,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMCI_1008" prefix="L" uservalue="yes">
<description>&lt;br&gt;&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PMCI Power Molded Chip
Inductor&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;
&lt;br&gt;Compact inductor chip type
&lt;br&gt;High effciency
&lt;br&gt;Suitable for applications with high currents up to 3.6 A. Very high DC-Bias current
&lt;br&gt;Very small electrical resistance, smallest RDC-Values starting at 19 mΩ
&lt;br&gt;Magnetically shielded construction: No crosstalk
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Available in five sizes and three different types (Low Profile, Standard and High Saturation Current)
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMCI"&gt;http://katalog.we-online.de/en/pbs/WE-PMCI&lt;/a&gt;&lt;p&gt;

&lt;br&gt;&lt;/b&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_1008_74479287XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479287147">
<attribute name="WE-NUMBER" value="74479287147/0,47uH"/>
</technology>
<technology name="_74479287210">
<attribute name="WE-NUMBER" value="74479287210/1uH"/>
</technology>
<technology name="_74479287222">
<attribute name="WE-NUMBER" value="74479287222/2,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMCI_1008HS" prefix="L" uservalue="yes">
<description>&lt;br&gt;&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PMCI Power Molded Chip
Inductor&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;
&lt;br&gt;Compact inductor chip type
&lt;br&gt;High effciency
&lt;br&gt;Suitable for applications with high currents up to 3.6 A. Very high DC-Bias current
&lt;br&gt;Very small electrical resistance, smallest RDC-Values starting at 19 mΩ
&lt;br&gt;Magnetically shielded construction: No crosstalk
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Available in five sizes and three different types (Low Profile, Standard and High Saturation Current)
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMCI"&gt;http://katalog.we-online.de/en/pbs/WE-PMCI&lt;/a&gt;&lt;p&gt;

&lt;br&gt;&lt;/b&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_1008_74479288XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479288147">
<attribute name="WE-NUMBER" value="74479288147/0,47uH"/>
</technology>
<technology name="_74479288210">
<attribute name="WE-NUMBER" value="74479288210/1uH"/>
</technology>
<technology name="_74479288215">
<attribute name="WE-NUMBER" value="74479288215/1,5uH"/>
</technology>
<technology name="_74479288222">
<attribute name="WE-NUMBER" value="74479288222/2,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMCI_1210" prefix="L" uservalue="yes">
<description>&lt;br&gt;&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PMCI Power Molded Chip
Inductor&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Characteristics&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;
&lt;br&gt;Compact inductor chip type
&lt;br&gt;High effciency
&lt;br&gt;Suitable for applications with high currents up to 3.6 A. Very high DC-Bias current
&lt;br&gt;Very small electrical resistance, smallest RDC-Values starting at 19 mΩ
&lt;br&gt;Magnetically shielded construction: No crosstalk
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Available in five sizes and three different types (Low Profile, Standard and High Saturation Current)
&lt;br&gt;Recommended soldering profile: Reflow

&lt;P&gt; &lt;font color="#0000FF"&gt;&lt;B&gt;Applications&lt;/B&gt;&lt;/font&gt;&lt;/td&gt;&lt;BR&gt;&lt;BR&gt;
&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;High current power supply, Battery powered devices
&lt;br&gt;Powerable electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMCI"&gt;http://katalog.we-online.de/en/pbs/WE-PMCI&lt;/a&gt;&lt;p&gt;

&lt;br&gt;&lt;/b&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMCI_1210_74479298XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479298147">
<attribute name="WE-NUMBER" value="74479298147/0,47uH"/>
</technology>
<technology name="_74479298210">
<attribute name="WE-NUMBER" value="74479298210/1uH"/>
</technology>
<technology name="_74479298222">
<attribute name="WE-NUMBER" value="74479298222/2,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMI_0603" prefix="L" uservalue="yes">
<description>&lt;b&gt;Power Multilayer Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact multilayer type
&lt;br&gt;
&lt;br&gt; Suitable for applications with high currents up to 2.7 A
&lt;br&gt;
&lt;br&gt; Smallest RDC-Values starting at 40 mΩ
&lt;br&gt;
&lt;br&gt; Magnetically shielded construction: No crosstalk
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Available in four sizes and three different types (Low Profile, Low RDC &amp; High Saturation Current)
&lt;br&gt;
&lt;br&gt; Recommended soldering profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;
&lt;br&gt; Electronic devices with very low profile
&lt;br&gt;
&lt;br&gt; Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMI?"&gt;http://katalog.we-online.de/en/pbs/WE-PMI?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMI_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479762122">
<attribute name="WE-NUMBER" value="74479762122/0,22uH"/>
</technology>
<technology name="_74479762133">
<attribute name="WE-NUMBER" value="74479762133/0,33uH"/>
</technology>
<technology name="_74479762168">
<attribute name="WE-NUMBER" value="74479762168/0,68uH"/>
</technology>
<technology name="_74479763147">
<attribute name="WE-NUMBER" value="74479763147/0,47uH"/>
</technology>
<technology name="_74479763147A">
<attribute name="WE-NUMBER" value="74479763147A/0,47uH"/>
</technology>
<technology name="_74479763168">
<attribute name="WE-NUMBER" value="74479763168/0,68uH"/>
</technology>
<technology name="_74479763210">
<attribute name="WE-NUMBER" value="74479763210/1uH"/>
</technology>
<technology name="_74479763210A">
<attribute name="WE-NUMBER" value="74479763210A/1uH"/>
</technology>
<technology name="_74479763215">
<attribute name="WE-NUMBER" value="74479763215/1,5uH"/>
</technology>
<technology name="_74479763222">
<attribute name="WE-NUMBER" value="74479763222/2,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMI_0805" prefix="L" uservalue="yes">
<description>&lt;b&gt;Power Multilayer Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact multilayer type
&lt;br&gt;
&lt;br&gt; Suitable for applications with high currents up to 2.7 A
&lt;br&gt;
&lt;br&gt; Smallest RDC-Values starting at 40 mΩ
&lt;br&gt;
&lt;br&gt; Magnetically shielded construction: No crosstalk
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Available in four sizes and three different types (Low Profile, Low RDC &amp; High Saturation Current)
&lt;br&gt;
&lt;br&gt; Recommended soldering profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;
&lt;br&gt; Electronic devices with very low profile
&lt;br&gt;
&lt;br&gt; Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMI?"&gt;http://katalog.we-online.de/en/pbs/WE-PMI?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMI_0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479773133">
<attribute name="WE-NUMBER" value="74479773133/0,33uH"/>
</technology>
<technology name="_74479773147">
<attribute name="WE-NUMBER" value="74479773147/0,47uH"/>
</technology>
<technology name="_74479773154">
<attribute name="WE-NUMBER" value="74479773154/0,54uH"/>
</technology>
<technology name="_74479773210">
<attribute name="WE-NUMBER" value="74479773210/1uH"/>
</technology>
<technology name="_74479774147">
<attribute name="WE-NUMBER" value="74479774147/0,47uH"/>
</technology>
<technology name="_74479774210">
<attribute name="WE-NUMBER" value="74479774210/1uH"/>
</technology>
<technology name="_74479774215">
<attribute name="WE-NUMBER" value="74479774215/1,5uH"/>
</technology>
<technology name="_74479774222">
<attribute name="WE-NUMBER" value="74479774222/2,2uH"/>
</technology>
<technology name="_74479775147">
<attribute name="WE-NUMBER" value="74479775147/0,47uH"/>
</technology>
<technology name="_74479775147A">
<attribute name="WE-NUMBER" value="74479775147A/0,47uH"/>
</technology>
<technology name="_74479775210">
<attribute name="WE-NUMBER" value="74479775210/1uH"/>
</technology>
<technology name="_74479775210A">
<attribute name="WE-NUMBER" value="74479775210A/1uH"/>
</technology>
<technology name="_74479775215">
<attribute name="WE-NUMBER" value="74479775215/1,5uH"/>
</technology>
<technology name="_74479775222">
<attribute name="WE-NUMBER" value="74479775222/2,2uH"/>
</technology>
<technology name="_74479775222A">
<attribute name="WE-NUMBER" value="74479775222A/2,2uH"/>
</technology>
<technology name="_74479775233">
<attribute name="WE-NUMBER" value="74479775233/3,3uH"/>
</technology>
<technology name="_74479775247">
<attribute name="WE-NUMBER" value="74479775247/4,7uH"/>
</technology>
<technology name="_74479777268">
<attribute name="WE-NUMBER" value="74479777268/6,8uH"/>
</technology>
<technology name="_74479777310">
<attribute name="WE-NUMBER" value="74479777310/10uH"/>
</technology>
<technology name="_74479777310A">
<attribute name="WE-NUMBER" value="74479777310A/10uH"/>
</technology>
<technology name="_74479875210C">
<attribute name="WE-NUMBER" value="74479875210C/1uH"/>
</technology>
<technology name="_74479875222C">
<attribute name="WE-NUMBER" value="74479875222C/2,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMI_0806" prefix="L" uservalue="yes">
<description>&lt;b&gt;Power Multilayer Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact multilayer type
&lt;br&gt;
&lt;br&gt; Suitable for applications with high currents up to 2.7 A
&lt;br&gt;
&lt;br&gt; Smallest RDC-Values starting at 40 mΩ
&lt;br&gt;
&lt;br&gt; Magnetically shielded construction: No crosstalk
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Available in four sizes and three different types (Low Profile, Low RDC &amp; High Saturation Current)
&lt;br&gt;
&lt;br&gt; Recommended soldering profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;
&lt;br&gt; Electronic devices with very low profile
&lt;br&gt;
&lt;br&gt; Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMI?"&gt;http://katalog.we-online.de/en/pbs/WE-PMI?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMI_0806">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479776147">
<attribute name="WE-NUMBER" value="74479776147/0,47uH"/>
</technology>
<technology name="_74479776210">
<attribute name="WE-NUMBER" value="74479776210/1uH"/>
</technology>
<technology name="_74479776215">
<attribute name="WE-NUMBER" value="74479776215/1,5uH"/>
</technology>
<technology name="_74479776222">
<attribute name="WE-NUMBER" value="74479776222/2,2uH"/>
</technology>
<technology name="_74479776222A">
<attribute name="WE-NUMBER" value="74479776222A/2,2Uh"/>
</technology>
<technology name="_74479776233">
<attribute name="WE-NUMBER" value="74479776233/3,3uH"/>
</technology>
<technology name="_74479776233A">
<attribute name="WE-NUMBER" value="74479776233A/3,3uH"/>
</technology>
<technology name="_74479776247">
<attribute name="WE-NUMBER" value="74479776247/4,7uH"/>
</technology>
<technology name="_74479776247A">
<attribute name="WE-NUMBER" value="74479776247A/4,7uH"/>
</technology>
<technology name="_74479778268">
<attribute name="WE-NUMBER" value="74479778268/6,8uH"/>
</technology>
<technology name="_74479778310">
<attribute name="WE-NUMBER" value="74479778310/10uH"/>
</technology>
<technology name="_74479876124C">
<attribute name="WE-NUMBER" value="74479876124C/0,24uH"/>
</technology>
<technology name="_74479876147">
<attribute name="WE-NUMBER" value="74479876147/0,47uH"/>
</technology>
<technology name="_74479876147C">
<attribute name="WE-NUMBER" value="74479876147C/0,47uH"/>
</technology>
<technology name="_74479876168">
<attribute name="WE-NUMBER" value="74479876168/0,68uH"/>
</technology>
<technology name="_74479876168C">
<attribute name="WE-NUMBER" value="74479876168C/0,68uH"/>
</technology>
<technology name="_74479876210">
<attribute name="WE-NUMBER" value="74479876210/1uH"/>
</technology>
<technology name="_74479876210C">
<attribute name="WE-NUMBER" value="74479876210C/1uH"/>
</technology>
<technology name="_74479876215C">
<attribute name="WE-NUMBER" value="74479876215C/1,5uH"/>
</technology>
<technology name="_74479876222C">
<attribute name="WE-NUMBER" value="74479876222C/2,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMI_1008" prefix="L" uservalue="yes">
<description>&lt;b&gt;Power Multilayer Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact multilayer type
&lt;br&gt;
&lt;br&gt; Suitable for applications with high currents up to 2.7 A
&lt;br&gt;
&lt;br&gt; Smallest RDC-Values starting at 40 mΩ
&lt;br&gt;
&lt;br&gt; Magnetically shielded construction: No crosstalk
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Available in four sizes and three different types (Low Profile, Low RDC &amp; High Saturation Current)
&lt;br&gt;
&lt;br&gt; Recommended soldering profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;
&lt;br&gt; Electronic devices with very low profile
&lt;br&gt;
&lt;br&gt; Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMI?"&gt;http://katalog.we-online.de/en/pbs/WE-PMI?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMI_1008">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479787147A">
<attribute name="WE-NUMBER" value="74479787147A/0,47uH"/>
</technology>
<technology name="_74479787147B">
<attribute name="WE-NUMBER" value="74479787147B/0,47uH"/>
</technology>
<technology name="_74479787210A">
<attribute name="WE-NUMBER" value="74479787210A/1uH"/>
</technology>
<technology name="_74479787210B">
<attribute name="WE-NUMBER" value="74479787210B/1uH"/>
</technology>
<technology name="_74479787215">
<attribute name="WE-NUMBER" value="74479787215/1,5uH"/>
</technology>
<technology name="_74479787215A">
<attribute name="WE-NUMBER" value="74479787215A/1,5uH"/>
</technology>
<technology name="_74479787222">
<attribute name="WE-NUMBER" value="74479787222/2,2uH"/>
</technology>
<technology name="_74479787222A">
<attribute name="WE-NUMBER" value="74479787222A/2,2uH"/>
</technology>
<technology name="_74479787233">
<attribute name="WE-NUMBER" value="74479787233/3,3uH"/>
</technology>
<technology name="_74479787233A">
<attribute name="WE-NUMBER" value="74479787233A/3,3uH"/>
</technology>
<technology name="_74479787247">
<attribute name="WE-NUMBER" value="74479787247/4,7uH"/>
</technology>
<technology name="_74479787247A">
<attribute name="WE-NUMBER" value="74479787247A/4,7uH"/>
</technology>
<technology name="_74479887124C">
<attribute name="WE-NUMBER" value="74479887124C/0,24uH"/>
</technology>
<technology name="_74479887147C">
<attribute name="WE-NUMBER" value="74479887147C/0,47uH"/>
</technology>
<technology name="_74479887210A">
<attribute name="WE-NUMBER" value="74479887210A/1uH"/>
</technology>
<technology name="_74479887210C">
<attribute name="WE-NUMBER" value="74479887210C/1uH"/>
</technology>
<technology name="_74479887222A">
<attribute name="WE-NUMBER" value="74479887222A/2,2uH"/>
</technology>
<technology name="_74479887222C">
<attribute name="WE-NUMBER" value="74479887222C/2,2uH"/>
</technology>
<technology name="_74479887233A">
<attribute name="WE-NUMBER" value="74479887233A/3,3uH"/>
</technology>
<technology name="_74479887247A">
<attribute name="WE-NUMBER" value="74479887247A/2,2uH"/>
</technology>
<technology name="_74479887268A">
<attribute name="WE-NUMBER" value="74479887268A/6,8uH"/>
</technology>
<technology name="_74479887310A">
<attribute name="WE-NUMBER" value="74479887310A/10uH"/>
</technology>
<technology name="_74479888222">
<attribute name="WE-NUMBER" value="74479888222/2,2uH"/>
</technology>
<technology name="_74479888233">
<attribute name="WE-NUMBER" value="74479888233/3,3uH"/>
</technology>
<technology name="_74479888247">
<attribute name="WE-NUMBER" value="74479888247/4,7uH"/>
</technology>
<technology name="_74479888268">
<attribute name="WE-NUMBER" value="74479888268/6,8uH"/>
</technology>
<technology name="_74479888310">
<attribute name="WE-NUMBER" value="74479888310/10uH"/>
</technology>
<technology name="_74479889210">
<attribute name="WE-NUMBER" value="74479889210/1uH"/>
</technology>
<technology name="_74479889222">
<attribute name="WE-NUMBER" value="74479889222/2,2uH"/>
</technology>
<technology name="_74479889233">
<attribute name="WE-NUMBER" value="74479889233/3,3uH"/>
</technology>
<technology name="_74479889247">
<attribute name="WE-NUMBER" value="74479889247/4,7uH"/>
</technology>
<technology name="_74479889268">
<attribute name="WE-NUMBER" value="74479889268/6,8uH"/>
</technology>
<technology name="_74479889310">
<attribute name="WE-NUMBER" value="74479889310/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMMI_0806" prefix="L" uservalue="yes">
<description>&lt;br&gt; &lt;B&gt;WE-PMMI Power Molded
Multilayer Inductor&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics

&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact multilayer type&lt;br&gt;
Suitable for applications with high currents up to 3.5A. Very high DC-bias current up to 4A. &lt;br&gt;
Smallest RDC-Values starting at 15 mΩ&lt;br&gt;
Magnetically shielded construction: No crosstalk&lt;br&gt;
Operating temperature: –40 °C to +125 °C&lt;br&gt;
Available in two sizes and two different types (Low Profile, Standard)&lt;br&gt;
Recommended soldering profile: Reflow&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications

&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Applications

&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;Electronic portable devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks, Digital Cameras, HDD's

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMMI_0805-0806_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMMI_0805-0806_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMMI"&gt;http://katalog.we-online.de/en/pbs/WE-PMMI&lt;/a&gt;&lt;p&gt;


&lt;br&gt;&lt;/b&gt;2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMMI_0806">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479976124">
<attribute name="WE-NUMBER" value="74479976124/0,24uH"/>
</technology>
<technology name="_74479976133">
<attribute name="WE-NUMBER" value="74479976133/0,33uH"/>
</technology>
<technology name="_74479976147">
<attribute name="WE-NUMBER" value="74479976147/0,47uH"/>
</technology>
<technology name="_74479976147A">
<attribute name="WE-NUMBER" value="74479976147A/0,47uH"/>
</technology>
<technology name="_74479976210">
<attribute name="WE-NUMBER" value="74479976210/1uH"/>
</technology>
<technology name="_74479976215">
<attribute name="WE-NUMBER" value="74479976215/1,5uH"/>
</technology>
<technology name="_74479978105">
<attribute name="WE-NUMBER" value="74479978102/0,05uH"/>
</technology>
<technology name="_74479978114">
<attribute name="WE-NUMBER" value="74479978114/0,14uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMMI_0806LP" prefix="L" uservalue="yes">
<description>&lt;br&gt; &lt;B&gt;WE-PMMI Power Molded
Multilayer Inductor&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics

&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact multilayer type&lt;br&gt;
Suitable for applications with high currents up to 3.5A. Very high DC-bias current up to 4A. &lt;br&gt;
Smallest RDC-Values starting at 15 mΩ&lt;br&gt;
Magnetically shielded construction: No crosstalk&lt;br&gt;
Operating temperature: –40 °C to +125 °C&lt;br&gt;
Available in two sizes and two different types (Low Profile, Standard)&lt;br&gt;
Recommended soldering profile: Reflow&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;b&gt; Applications

&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Applications

&lt;br&gt;DC/DC converters especially at high switching frequencies &gt; 1 MHz
&lt;br&gt;Electronic portable devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks, Digital Cameras, HDD's

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PMMI_0805-0806_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PMMI_0805-0806_4C.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PMMI"&gt;http://katalog.we-online.de/en/pbs/WE-PMMI&lt;/a&gt;&lt;p&gt;


&lt;br&gt;&lt;/b&gt;2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMMI_0806">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479977104">
<attribute name="WE-NUMBER" value="74479977104/0,04uH"/>
</technology>
<technology name="_74479977111">
<attribute name="WE-NUMBER" value="74479977111/0,11uH"/>
</technology>
<technology name="_74479977124">
<attribute name="WE-NUMBER" value="74479977124/0,24uH"/>
</technology>
<technology name="_74479977147">
<attribute name="WE-NUMBER" value="74479977147/0,47uH"/>
</technology>
<technology name="_74479977156">
<attribute name="WE-NUMBER" value="74479977156/0,56uH"/>
</technology>
<technology name="_74479977182">
<attribute name="WE-NUMBER" value="74479977182/0,82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPC_4818" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD-Shielded Power Inductor  WE-SPC

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndSPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SPC?"&gt;http://katalog.we-online.de/en/pbs/WE-SPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-SPC_48XX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744089410022">
<attribute name="WE-NUMBER" value="744089410022/0,22uH"/>
</technology>
<technology name="_744089410043">
<attribute name="WE-NUMBER" value="744089410043/0,43uH"/>
</technology>
<technology name="_744089410068">
<attribute name="WE-NUMBER" value="74408910068/0,68uH"/>
</technology>
<technology name="_74408941010">
<attribute name="WE-NUMBER" value="74408941010/1uH"/>
</technology>
<technology name="_74408941022">
<attribute name="WE-NUMBER" value="74408941022/0,22uH"/>
</technology>
<technology name="_74408941029">
<attribute name="WE-NUMBER" value="74408941029/2,9uH"/>
</technology>
<technology name="_74408941035">
<attribute name="WE-NUMBER" value="74408941035/3,5uH"/>
</technology>
<technology name="_74408941050">
<attribute name="WE-NUMBER" value="74408941050/5uH"/>
</technology>
<technology name="_74408941068">
<attribute name="WE-NUMBER" value="74408941068/6,8uH"/>
</technology>
<technology name="_74408941078">
<attribute name="WE-NUMBER" value="74408941078/7,8uH"/>
</technology>
<technology name="_74408941089">
<attribute name="WE-NUMBER" value="74408941089/8,9uH"/>
</technology>
<technology name="_74408941100">
<attribute name="WE-NUMBER" value="74408941100/10uH"/>
</technology>
<technology name="_74408941150">
<attribute name="WE-NUMBER" value="74408941150/15uH"/>
</technology>
<technology name="_74408941220">
<attribute name="WE-NUMBER" value="74408941220/22uH"/>
</technology>
<technology name="_74408941330">
<attribute name="WE-NUMBER" value="74408941330/33uH"/>
</technology>
<technology name="_74408941470">
<attribute name="WE-NUMBER" value="74408941470/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPC_4828" prefix="L" uservalue="yes">
<description>&lt;b&gt; SMD-Shielded Power Inductor  WE-SPC

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndSPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SPC?"&gt;http://katalog.we-online.de/en/pbs/WE-SPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-SPC_48XX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744089420022">
<attribute name="WE-NUMBER" value="744089420022/0,22uH"/>
</technology>
<technology name="_744089420039">
<attribute name="WE-NUMBER" value="744089420039/0,39uH"/>
</technology>
<technology name="_744089420056">
<attribute name="WE-NUMBER" value="744089420056/0,56uH"/>
</technology>
<technology name="_744089420082">
<attribute name="WE-NUMBER" value="744089420082/0,82uH"/>
</technology>
<technology name="_74408942012">
<attribute name="WE-NUMBER" value="74408942012/1,2uH"/>
</technology>
<technology name="_74408942022">
<attribute name="WE-NUMBER" value="74408942022/2,2uH"/>
</technology>
<technology name="_74408942033">
<attribute name="WE-NUMBER" value="74408942033/3,3uH"/>
</technology>
<technology name="_74408942047">
<attribute name="WE-NUMBER" value="74408942047/4,7uH"/>
</technology>
<technology name="_74408942068">
<attribute name="WE-NUMBER" value="74408942068/6,8uH"/>
</technology>
<technology name="_74408942082">
<attribute name="WE-NUMBER" value="74408942082/8,2uH"/>
</technology>
<technology name="_74408942100">
<attribute name="WE-NUMBER" value="74408942100/10uH"/>
</technology>
<technology name="_74408942150">
<attribute name="WE-NUMBER" value="74408942150/15uH"/>
</technology>
<technology name="_74408942220">
<attribute name="WE-NUMBER" value="74408942220/22uH"/>
</technology>
<technology name="_74408942330">
<attribute name="WE-NUMBER" value="74408942330/33uH"/>
</technology>
<technology name="_74408942470">
<attribute name="WE-NUMBER" value="74408942470/47uH"/>
</technology>
<technology name="_74408942560">
<attribute name="WE-NUMBER" value="74408942560/56uH"/>
</technology>
<technology name="_74408942680">
<attribute name="WE-NUMBER" value="74408942680/68uH"/>
</technology>
<technology name="_74408942820">
<attribute name="WE-NUMBER" value="74408942820/82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TDC_8038" prefix="L" uservalue="yes">
<description>&lt;b&gt;SEPIC SMD Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Core material: NiZn
&lt;br&gt;
&lt;br&gt; Low profile
&lt;br&gt;
&lt;br&gt; Magnetical shielded which results in a low leakage field
&lt;br&gt;
&lt;br&gt; 8x8 mm case
&lt;br&gt;
&lt;br&gt; 1:1 transformer
&lt;br&gt;
&lt;br&gt; Low self-losses
&lt;br&gt;
&lt;br&gt; High self resonance frequency
&lt;br&gt;
&lt;br&gt; Coupled inductor with two identical windings
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C up to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Non-isolated flyback converter
&lt;br&gt;
&lt;br&gt; Buck or Boost with AUX winding
&lt;br&gt;
&lt;br&gt; BUCK-BOOST, SEPIC, ZETA &amp; CUK Converter
&lt;br&gt;
&lt;br&gt; Switching regulators with secondary unregulated output voltages
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTDC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTDC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TDC?"&gt;http://katalog.we-online.de/en/pbs/WE-TDC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-TDC_80XX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="3"/>
</connects>
<technologies>
<technology name="_744894400039">
<attribute name="WE-NUMBER" value="744894400039/0,39uH"/>
</technology>
<technology name="_744894400082">
<attribute name="WE-NUMBER" value="744894400082/0,82uH"/>
</technology>
<technology name="_74489440012">
<attribute name="WE-NUMBER" value="74489440012/1,2uH"/>
</technology>
<technology name="_74489440018">
<attribute name="WE-NUMBER" value="74489440018/1,8uH"/>
</technology>
<technology name="_74489440027">
<attribute name="WE-NUMBER" value="74489440027/2,7uH"/>
</technology>
<technology name="_74489440036">
<attribute name="WE-NUMBER" value="74489440036/3,6uH"/>
</technology>
<technology name="_74489440047">
<attribute name="WE-NUMBER" value="74489440047/4,7uH"/>
</technology>
<technology name="_74489440068">
<attribute name="WE-NUMBER" value="74489440068/6,8uH"/>
</technology>
<technology name="_74489440100">
<attribute name="WE-NUMBER" value="74489440100/10uH"/>
</technology>
<technology name="_74489440120">
<attribute name="WE-NUMBER" value="74489440120/12uH"/>
</technology>
<technology name="_74489440150">
<attribute name="WE-NUMBER" value="74489440150/15uH"/>
</technology>
<technology name="_74489440180">
<attribute name="WE-NUMBER" value="74489440180/18uH"/>
</technology>
<technology name="_74489440220">
<attribute name="WE-NUMBER" value="74489440220/22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TI_8095_SHRINKING" prefix="L" uservalue="yes">
<description>&lt;b&gt;Radial Leaded Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Radial through-hole inductor
&lt;br&gt;
&lt;br&gt; High saturation core material
&lt;br&gt;
&lt;br&gt; Small size
&lt;br&gt;
&lt;br&gt; Maximum current up to 8.5 A
&lt;br&gt;
&lt;br&gt; Custom design on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Signal filtering
&lt;br&gt;
&lt;br&gt; Switches, switching power supply for small and medium voltage
&lt;br&gt;
&lt;br&gt; Power supply filter
&lt;br&gt;
&lt;br&gt; EMI filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TI?"&gt;http://katalog.we-online.de/en/pbs/WE-TI?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TI/TIHV_8095_SHRINKING">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744742103">
<attribute name="WE-NUMBER" value="744742103/10000uH"/>
</technology>
<technology name="_744742223">
<attribute name="WE-NUMBER" value="744742223/22000uH"/>
</technology>
<technology name="_7447722473">
<attribute name="WE-NUMBER" value="7447722473/47000uH"/>
</technology>
<technology name="_7447728102">
<attribute name="WE-NUMBER" value="7447728102/1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TI_8075" prefix="L" uservalue="yes">
<description>&lt;b&gt;Radial Leaded Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Radial through-hole inductor
&lt;br&gt;
&lt;br&gt; High saturation core material
&lt;br&gt;
&lt;br&gt; Small size
&lt;br&gt;
&lt;br&gt; Maximum current up to 8.5 A
&lt;br&gt;
&lt;br&gt; Custom design on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Signal filtering
&lt;br&gt;
&lt;br&gt; Switches, switching power supply for small and medium voltage
&lt;br&gt;
&lt;br&gt; Power supply filter
&lt;br&gt;
&lt;br&gt; EMI filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TI?"&gt;http://katalog.we-online.de/en/pbs/WE-TI?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TI_8075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744730392">
<attribute name="WE-NUMBER" value="744730392/3900uH"/>
</technology>
<technology name="_7447721047">
<attribute name="WE-NUMBER" value="7447721047/4700uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TI_8075_SHRINKING" prefix="L" uservalue="yes">
<description>&lt;b&gt;Radial Leaded Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Radial through-hole inductor
&lt;br&gt;
&lt;br&gt; High saturation core material
&lt;br&gt;
&lt;br&gt; Small size
&lt;br&gt;
&lt;br&gt; Maximum current up to 8.5 A
&lt;br&gt;
&lt;br&gt; Custom design on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Signal filtering
&lt;br&gt;
&lt;br&gt; Switches, switching power supply for small and medium voltage
&lt;br&gt;
&lt;br&gt; Power supply filter
&lt;br&gt;
&lt;br&gt; EMI filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TI?"&gt;http://katalog.we-online.de/en/pbs/WE-TI?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TI_8075_SHRINKTUBE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744732015">
<attribute name="WE-NUMBER" value="744732015/1,5uH"/>
</technology>
<technology name="_744732100">
<attribute name="WE-NUMBER" value="744732100/10uH"/>
</technology>
<technology name="_744732102">
<attribute name="WE-NUMBER" value="744732102/1000uH"/>
</technology>
<technology name="_744732121">
<attribute name="WE-NUMBER" value="744732121/120uH"/>
</technology>
<technology name="_744732152">
<attribute name="WE-NUMBER" value="744732152/1500uH"/>
</technology>
<technology name="_744732153">
<attribute name="WE-NUMBER" value="744732153/15000uH"/>
</technology>
<technology name="_744732221">
<attribute name="WE-NUMBER" value="744732221/220uH"/>
</technology>
<technology name="_744732331">
<attribute name="WE-NUMBER" value="744732331/330uH"/>
</technology>
<technology name="_744732470">
<attribute name="WE-NUMBER" value="744732470/47uH"/>
</technology>
<technology name="_744732471">
<attribute name="WE-NUMBER" value="744732471/470uH"/>
</technology>
<technology name="_744732681">
<attribute name="WE-NUMBER" value="744732681/680uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TI_8055" prefix="L" uservalue="yes">
<description>&lt;b&gt;Radial Leaded Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Radial through-hole inductor
&lt;br&gt;
&lt;br&gt; High saturation core material
&lt;br&gt;
&lt;br&gt; Small size
&lt;br&gt;
&lt;br&gt; Maximum current up to 8.5 A
&lt;br&gt;
&lt;br&gt; Custom design on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Signal filtering
&lt;br&gt;
&lt;br&gt; Switches, switching power supply for small and medium voltage
&lt;br&gt;
&lt;br&gt; Power supply filter
&lt;br&gt;
&lt;br&gt; EMI filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TI?"&gt;http://katalog.we-online.de/en/pbs/WE-TI?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TI/TIHV_SHRINK_8055">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744741101">
<attribute name="WE-NUMBER" value="744741101/100uH"/>
</technology>
<technology name="_744741102">
<attribute name="WE-NUMBER" value="744741102/1000uH"/>
</technology>
<technology name="_744741221">
<attribute name="WE-NUMBER" value="744741221/220uH"/>
</technology>
<technology name="_744741222">
<attribute name="WE-NUMBER" value="744741222/2200uH"/>
</technology>
<technology name="_7447412331">
<attribute name="WE-NUMBER" value="7447412331/330uH"/>
</technology>
<technology name="_7447412681">
<attribute name="WE-NUMBER" value="7447412681/680uH"/>
</technology>
<technology name="_744741471">
<attribute name="WE-NUMBER" value="744741471/470uH"/>
</technology>
<technology name="_744741472">
<attribute name="WE-NUMBER" value="744741472/4700uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TI_6065" prefix="L" uservalue="yes">
<description>&lt;b&gt;Radial Leaded Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Radial through-hole inductor
&lt;br&gt;
&lt;br&gt; High saturation core material
&lt;br&gt;
&lt;br&gt; Small size
&lt;br&gt;
&lt;br&gt; Maximum current up to 8.5 A
&lt;br&gt;
&lt;br&gt; Custom design on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Signal filtering
&lt;br&gt;
&lt;br&gt; Switches, switching power supply for small and medium voltage
&lt;br&gt;
&lt;br&gt; Power supply filter
&lt;br&gt;
&lt;br&gt; EMI filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TI?"&gt;http://katalog.we-online.de/en/pbs/WE-TI?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TI_6065">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447790221">
<attribute name="WE-NUMBER" value="7447790221/220uH"/>
</technology>
<technology name="_7447790470">
<attribute name="WE-NUMBER" value="7447790470/47uH"/>
</technology>
<technology name="_744779068">
<attribute name="WE-NUMBER" value="744779068/6,8uH"/>
</technology>
<technology name="_744779100">
<attribute name="WE-NUMBER" value="744779100/10uH"/>
</technology>
<technology name="_744779168">
<attribute name="WE-NUMBER" value="744779168/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TI_5075" prefix="L" uservalue="yes">
<description>&lt;b&gt;Radial Leaded Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Radial through-hole inductor
&lt;br&gt;
&lt;br&gt; High saturation core material
&lt;br&gt;
&lt;br&gt; Small size
&lt;br&gt;
&lt;br&gt; Maximum current up to 8.5 A
&lt;br&gt;
&lt;br&gt; Custom design on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Signal filtering
&lt;br&gt;
&lt;br&gt; Switches, switching power supply for small and medium voltage
&lt;br&gt;
&lt;br&gt; Power supply filter
&lt;br&gt;
&lt;br&gt; EMI filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TI?"&gt;http://katalog.we-online.de/en/pbs/WE-TI?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TI_5075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447462010">
<attribute name="WE-NUMBER" value="7447462010/1uH"/>
</technology>
<technology name="_7447462022">
<attribute name="WE-NUMBER" value="7447462022/2,2uH"/>
</technology>
<technology name="_7447462033">
<attribute name="WE-NUMBER" value="7447462033/3,3uH"/>
</technology>
<technology name="_7447462047">
<attribute name="WE-NUMBER" value="7447462047/4,7uH"/>
</technology>
<technology name="_7447462068">
<attribute name="WE-NUMBER" value="7447462068/6,8uH"/>
</technology>
<technology name="_7447462100">
<attribute name="WE-NUMBER" value="7447462100/10uH"/>
</technology>
<technology name="_7447462101">
<attribute name="WE-NUMBER" value="7447462101/100uH"/>
</technology>
<technology name="_7447462102">
<attribute name="WE-NUMBER" value="7447462102/1000uH"/>
</technology>
<technology name="_7447462152">
<attribute name="WE-NUMBER" value="7447462152/1500uH"/>
</technology>
<technology name="_7447462220">
<attribute name="WE-NUMBER" value="7447462220/22uH"/>
</technology>
<technology name="_7447462221">
<attribute name="WE-NUMBER" value="7447462221/220uH"/>
</technology>
<technology name="_7447462222">
<attribute name="WE-NUMBER" value="7447462222/2200uH"/>
</technology>
<technology name="_7447462330">
<attribute name="WE-NUMBER" value="7447462330/33uH"/>
</technology>
<technology name="_7447462470">
<attribute name="WE-NUMBER" value="7447462470/47uH"/>
</technology>
<technology name="_7447462471">
<attribute name="WE-NUMBER" value="7447462471/470uH"/>
</technology>
<technology name="_7447462680">
<attribute name="WE-NUMBER" value="7447462680/68uH"/>
</technology>
<technology name="_7447462681">
<attribute name="WE-NUMBER" value="7447462681/680uH"/>
</technology>
<technology name="_7447462820">
<attribute name="WE-NUMBER" value="7447462820/82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TI_8012_SHRINKING" uservalue="yes">
<description>&lt;b&gt;Radial Leaded Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Radial through-hole inductor
&lt;br&gt;
&lt;br&gt; High saturation core material
&lt;br&gt;
&lt;br&gt; Small size
&lt;br&gt;
&lt;br&gt; Maximum current up to 8.5 A
&lt;br&gt;
&lt;br&gt; Custom design on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Signal filtering
&lt;br&gt;
&lt;br&gt; Switches, switching power supply for small and medium voltage
&lt;br&gt;
&lt;br&gt; Power supply filter
&lt;br&gt;
&lt;br&gt; EMI filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TI?"&gt;http://katalog.we-online.de/en/pbs/WE-TI?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TI_8012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447452100">
<attribute name="WE-NUMBER" value="7447452100/10uH"/>
</technology>
<technology name="_7447452101">
<attribute name="WE-NUMBER" value="7447452101/100uH"/>
</technology>
<technology name="_7447452102">
<attribute name="WE-NUMBER" value="7447452102/1000uH"/>
</technology>
<technology name="_7447452152">
<attribute name="WE-NUMBER" value="7447452152/1500uH"/>
</technology>
<technology name="_7447452221">
<attribute name="WE-NUMBER" value="7447452221/220uH"/>
</technology>
<technology name="_7447452222">
<attribute name="WE-NUMBER" value="7447452222/2200uH"/>
</technology>
<technology name="_7447452331">
<attribute name="WE-NUMBER" value="7447452331/330uH"/>
</technology>
<technology name="_7447452391">
<attribute name="WE-NUMBER" value="7447452391/390uH"/>
</technology>
<technology name="_7447452392">
<attribute name="WE-NUMBER" value="7447452392/3900uH"/>
</technology>
<technology name="_7447452472">
<attribute name="WE-NUMBER" value="7447452472/4700uH"/>
</technology>
<technology name="_7447452561">
<attribute name="WE-NUMBER" value="7447452561/560uH"/>
</technology>
<technology name="_7447452683">
<attribute name="WE-NUMBER" value="7447452683/68000uH"/>
</technology>
<technology name="_7447452821">
<attribute name="WE-NUMBER" value="7447452821/820uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TI_8012B" prefix="L" uservalue="yes">
<description>&lt;b&gt;Radial Leaded Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Radial through-hole inductor
&lt;br&gt;
&lt;br&gt; High saturation core material
&lt;br&gt;
&lt;br&gt; Small size
&lt;br&gt;
&lt;br&gt; Maximum current up to 8.5 A
&lt;br&gt;
&lt;br&gt; Custom design on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Signal filtering
&lt;br&gt;
&lt;br&gt; Switches, switching power supply for small and medium voltage
&lt;br&gt;
&lt;br&gt; Power supply filter
&lt;br&gt;
&lt;br&gt; EMI filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TI?"&gt;http://katalog.we-online.de/en/pbs/WE-TI?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TI_8012B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744743101">
<attribute name="WE-NUMBER" value="744743101/100uH"/>
</technology>
<technology name="_744743102">
<attribute name="WE-NUMBER" value="744743102/1000uH"/>
</technology>
<technology name="_744743221">
<attribute name="WE-NUMBER" value="744743221/220uH"/>
</technology>
<technology name="_744743331">
<attribute name="WE-NUMBER" value="744743331/330uH"/>
</technology>
<technology name="_744743471">
<attribute name="WE-NUMBER" value="744743471/470uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TI_8012" prefix="L" uservalue="yes">
<description>&lt;b&gt;Radial Leaded Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Radial through-hole inductor
&lt;br&gt;
&lt;br&gt; High saturation core material
&lt;br&gt;
&lt;br&gt; Small size
&lt;br&gt;
&lt;br&gt; Maximum current up to 8.5 A
&lt;br&gt;
&lt;br&gt; Custom design on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Signal filtering
&lt;br&gt;
&lt;br&gt; Switches, switching power supply for small and medium voltage
&lt;br&gt;
&lt;br&gt; Power supply filter
&lt;br&gt;
&lt;br&gt; EMI filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TI?"&gt;http://katalog.we-online.de/en/pbs/WE-TI?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_7447450103" package="WE-TI_8012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="WE-NUMBER" value="7447450103/10000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TI_1014" prefix="L" uservalue="yes">
<description>&lt;b&gt;Radial Leaded Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Radial through-hole inductor
&lt;br&gt;
&lt;br&gt; High saturation core material
&lt;br&gt;
&lt;br&gt; Small size
&lt;br&gt;
&lt;br&gt; Maximum current up to 8.5 A
&lt;br&gt;
&lt;br&gt; Custom design on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Signal filtering
&lt;br&gt;
&lt;br&gt; Switches, switching power supply for small and medium voltage
&lt;br&gt;
&lt;br&gt; Power supply filter
&lt;br&gt;
&lt;br&gt; EMI filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TI?"&gt;http://katalog.we-online.de/en/pbs/WE-TI?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TI_1014">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447480101">
<attribute name="WE-NUMBER" value="7447480101/100uH"/>
</technology>
<technology name="_7447480102">
<attribute name="WE-NUMBER" value="7447480102/1000uH"/>
</technology>
<technology name="_7447480122">
<attribute name="WE-NUMBER" value="7447480122/1200uH"/>
</technology>
<technology name="_7447480151">
<attribute name="WE-NUMBER" value="7447480151/150uH"/>
</technology>
<technology name="_7447480152">
<attribute name="WE-NUMBER" value="7447480152/1500uH"/>
</technology>
<technology name="_7447480221">
<attribute name="WE-NUMBER" value="7447480221/220uH"/>
</technology>
<technology name="_7447480222">
<attribute name="WE-NUMBER" value="7447480222/2200uH"/>
</technology>
<technology name="_7447480331">
<attribute name="WE-NUMBER" value="7447480331/330uH"/>
</technology>
<technology name="_7447480332">
<attribute name="WE-NUMBER" value="7447480332/3300uH"/>
</technology>
<technology name="_7447480471">
<attribute name="WE-NUMBER" value="7447480471/470uH"/>
</technology>
<technology name="_7447480562">
<attribute name="WE-NUMBER" value="7447480562/5600uH"/>
</technology>
<technology name="_7447480681">
<attribute name="WE-NUMBER" value="7447480681/680uH"/>
</technology>
<technology name="_7447480822">
<attribute name="WE-NUMBER" value="7447480822/8200uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TIF_1016" prefix="L" uservalue="yes">
<description>&lt;B&gt;WE-TIF Radial Leaded Wire Wound Inductor with 4 Pins&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Radial through-hole inductor &lt;br&gt;
High saturation core material&lt;br&gt;
 Maximum current up to 3.1 A &lt;br&gt;
2 additional pins for high mechanical stability&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Application&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Signal filtering &lt;br&gt;
EMI and power supply filter&lt;br&gt;
 DC/DC converters &lt;br&gt;
Switching power&lt;br&gt;
 Supplies for small and medium voltage&lt;br&gt; 
Power supply for LED &lt;br&gt;
Nearfield applications &lt;br&gt;



&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTIF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTIF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TIF"&gt;http://katalog.we-online.de/en/pbs/WE-TIF&lt;/a&gt;&lt;p&gt;

Updated on 2015-05-21&lt;br&gt;
2015(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TIF"/>
</gates>
<devices>
<device name="" package="WE-TIF_1016">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447221101">
<attribute name="WE-NUMBER" value="7447221101/100uH"/>
</technology>
<technology name="_7447221102">
<attribute name="WE-NUMBER" value="7447221102/1000uH"/>
</technology>
<technology name="_7447221103">
<attribute name="WE-NUMBER" value="7447221103/10000uH"/>
</technology>
<technology name="_7447221221">
<attribute name="WE-NUMBER" value="7447221221/220uH"/>
</technology>
<technology name="_7447221222">
<attribute name="WE-NUMBER" value="7447221222/2200uH"/>
</technology>
<technology name="_7447221331">
<attribute name="WE-NUMBER" value="7447221331/330uH"/>
</technology>
<technology name="_7447221332">
<attribute name="WE-NUMBER" value="7447221332/3300uH"/>
</technology>
<technology name="_7447221471">
<attribute name="WE-NUMBER" value="7447221471/470uH"/>
</technology>
<technology name="_7447221472">
<attribute name="WE-NUMBER" value="7447221472/4700uH"/>
</technology>
<technology name="_7447221681">
<attribute name="WE-NUMBER" value="7447221681/680uH"/>
</technology>
<technology name="_7447221682">
<attribute name="WE-NUMBER" value="7447221682/6800uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TIF_1018" prefix="L" uservalue="yes">
<description>&lt;B&gt;WE-TIF Radial Leaded Wire Wound Inductor with 4 Pins&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Radial through-hole inductor &lt;br&gt;
High saturation core material&lt;br&gt;
 Maximum current up to 3.1 A &lt;br&gt;
2 additional pins for high mechanical stability&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Application&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Signal filtering &lt;br&gt;
EMI and power supply filter&lt;br&gt;
 DC/DC converters &lt;br&gt;
Switching power&lt;br&gt;
 Supplies for small and medium voltage&lt;br&gt; 
Power supply for LED &lt;br&gt;
Nearfield applications &lt;br&gt;



&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTIF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTIF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TIF"&gt;http://katalog.we-online.de/en/pbs/WE-TIF&lt;/a&gt;&lt;p&gt;

Updated on 2015-05-21&lt;br&gt;
2015(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TIF"/>
</gates>
<devices>
<device name="" package="WE-TIF">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447231101">
<attribute name="WE-NUMBER" value="7447231101/100uH"/>
</technology>
<technology name="_7447231102">
<attribute name="WE-NUMBER" value="7447231102/1000uH"/>
</technology>
<technology name="_7447231103">
<attribute name="WE-NUMBER" value="7447231103/10000uH"/>
</technology>
<technology name="_7447231221">
<attribute name="WE-NUMBER" value="7447231221/220uH"/>
</technology>
<technology name="_7447231222">
<attribute name="WE-NUMBER" value="7447231222/2200uH"/>
</technology>
<technology name="_7447231331">
<attribute name="WE-NUMBER" value="7447231331/330uH"/>
</technology>
<technology name="_7447231332">
<attribute name="WE-NUMBER" value="7447231332/3300uH"/>
</technology>
<technology name="_7447231471">
<attribute name="WE-NUMBER" value="744723147/470uH"/>
</technology>
<technology name="_7447231472">
<attribute name="WE-NUMBER" value="7447231472/4700uH"/>
</technology>
<technology name="_7447231681">
<attribute name="WE-NUMBER" value="7447231681/680uH"/>
</technology>
<technology name="_7447231682">
<attribute name="WE-NUMBER" value="7447231682/6800uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TIS_1111" prefix="L" uservalue="yes">
<description>&lt;b&gt;Shielded Radial Leaded Wire Wound Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Shielded radial through-hole inductor
&lt;br&gt;
&lt;br&gt; High rated and saturation current
&lt;br&gt;
&lt;br&gt; High inductance values
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter choke
&lt;br&gt;
&lt;br&gt; Storage choke
&lt;br&gt;
&lt;br&gt; Class D amplifiers
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTIS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTIS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TIS?"&gt;http://katalog.we-online.de/en/pbs/WE-TIS?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TIS_1111">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447471013">
<attribute name="WE-NUMBER" value="7447471013/1,3uH"/>
</technology>
<technology name="_7447471022">
<attribute name="WE-NUMBER" value="7447471022/2,2uH"/>
</technology>
<technology name="_7447471033">
<attribute name="WE-NUMBER" value="7447471033/3,3uH"/>
</technology>
<technology name="_7447471047">
<attribute name="WE-NUMBER" value="7447471047/4,7uH"/>
</technology>
<technology name="_7447471068">
<attribute name="WE-NUMBER" value="744747168/6,8uH"/>
</technology>
<technology name="_7447471100">
<attribute name="WE-NUMBER" value="7447471100/10uH"/>
</technology>
<technology name="_7447471101">
<attribute name="WE-NUMBER" value="7447471101/100uH"/>
</technology>
<technology name="_7447471102">
<attribute name="WE-NUMBER" value="7447471102/1000uH"/>
</technology>
<technology name="_7447471151">
<attribute name="WE-NUMBER" value="7447471151/150uH"/>
</technology>
<technology name="_7447471220">
<attribute name="WE-NUMBER" value="7447471220/22uH"/>
</technology>
<technology name="_7447471221">
<attribute name="WE-NUMBER" value="7447471221/220uH"/>
</technology>
<technology name="_7447471222">
<attribute name="WE-NUMBER" value="7447471222/220uH"/>
</technology>
<technology name="_7447471330">
<attribute name="WE-NUMBER" value="7447471330/33uH"/>
</technology>
<technology name="_7447471331">
<attribute name="WE-NUMBER" value="7447471331/330uH"/>
</technology>
<technology name="_7447471332">
<attribute name="WE-NUMBER" value="7447471332/3300uH"/>
</technology>
<technology name="_7447471470">
<attribute name="WE-NUMBER" value="7447471470/47uH"/>
</technology>
<technology name="_7447471471">
<attribute name="WE-NUMBER" value="7447471471/470uH"/>
</technology>
<technology name="_7447471472">
<attribute name="WE-NUMBER" value="7447471472/4700uH"/>
</technology>
<technology name="_7447471682">
<attribute name="WE-NUMBER" value="7447471682/6800uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_2811" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_2811/2813_OLD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744028000056">
<attribute name="WE-NUMBER" value="744028000056/0,056uH"/>
</technology>
<technology name="_74402800015">
<attribute name="WE-NUMBER" value="74402800015/0,15uH"/>
</technology>
<technology name="_74402800033">
<attribute name="WE-NUMBER" value="74402800033/0,33uH"/>
</technology>
<technology name="_74402800047">
<attribute name="WE-NUMBER" value="74402800047/0,47uH"/>
</technology>
<technology name="_74402800082">
<attribute name="WE-NUMBER" value="744028000082/0,82uH"/>
</technology>
<technology name="_744028001">
<attribute name="WE-NUMBER" value="744028001/1uH"/>
</technology>
<technology name="_744028002">
<attribute name="WE-NUMBER" value="744028002/2,2uH"/>
</technology>
<technology name="_744028003">
<attribute name="WE-NUMBER" value="744028003/3,3uH"/>
</technology>
<technology name="_744028004">
<attribute name="WE-NUMBER" value="744028004/4,7uH"/>
</technology>
<technology name="_744028006">
<attribute name="WE-NUMBER" value="744028006/6,8uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_2813" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_2811/2813_OLD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744029000068">
<attribute name="WE-NUMBER" value="744029000068/0,068uH"/>
</technology>
<technology name="_74402900016">
<attribute name="WE-NUMBER" value="744029000016/0,16uH"/>
</technology>
<technology name="_74402900033">
<attribute name="WE-NUMBER" value="74402900033/0,33uH"/>
</technology>
<technology name="_74402900047">
<attribute name="WE-NUMBER" value="74402900047/0,47uH"/>
</technology>
<technology name="_74402900082">
<attribute name="WE-NUMBER" value="74402900082/0,82uH"/>
</technology>
<technology name="_744029001">
<attribute name="WE-NUMBER" value="744029001/1uH"/>
</technology>
<technology name="_744029002">
<attribute name="WE-NUMBER" value="744029002/2,2uH"/>
</technology>
<technology name="_744029003">
<attribute name="WE-NUMBER" value="744029003/3,3uH"/>
</technology>
<technology name="_744029004">
<attribute name="WE-NUMBER" value="744029004/4,7uH"/>
</technology>
<technology name="_744029006">
<attribute name="WE-NUMBER" value="744029006/6,8uH"/>
</technology>
<technology name="_744029100">
<attribute name="WE-NUMBER" value="744029100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_2828" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_2828_OLD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74402500030">
<attribute name="WE-NUMBER" value="74402500030/0,3uH"/>
</technology>
<technology name="_74402500047">
<attribute name="WE-NUMBER" value="74402500047/0,47uH"/>
</technology>
<technology name="_74402500072">
<attribute name="WE-NUMBER" value="74402500072/0,72uH"/>
</technology>
<technology name="_744025001">
<attribute name="WE-NUMBER" value="744025001/1,2uH"/>
</technology>
<technology name="_744025002">
<attribute name="WE-NUMBER" value="744025002/2,2uH"/>
</technology>
<technology name="_744025003">
<attribute name="WE-NUMBER" value="744025003/3,3uH"/>
</technology>
<technology name="_744025004">
<attribute name="WE-NUMBER" value="744025004/4,7uH"/>
</technology>
<technology name="_744025006">
<attribute name="WE-NUMBER" value="744025006/6,8uH"/>
</technology>
<technology name="_744025100">
<attribute name="WE-NUMBER" value="744025100/10uH"/>
</technology>
<technology name="_744025150">
<attribute name="WE-NUMBER" value="744025150/15uH"/>
</technology>
<technology name="_744025220">
<attribute name="WE-NUMBER" value="744025220/22uH"/>
</technology>
<technology name="_744025270">
<attribute name="WE-NUMBER" value="744025270/27uH"/>
</technology>
<technology name="_744025330">
<attribute name="WE-NUMBER" value="744025330/33uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_3510" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_3510">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="_744030001">
<attribute name="WE-NUMBER" value="744030001/1,2uH"/>
</technology>
<technology name="_744030002">
<attribute name="WE-NUMBER" value="744030002/2,2uH"/>
</technology>
<technology name="_744030003">
<attribute name="WE-NUMBER" value="744030003/3,3uH"/>
</technology>
<technology name="_744030004">
<attribute name="WE-NUMBER" value="744030004/4,7uH"/>
</technology>
<technology name="_7440300047">
<attribute name="WE-NUMBER" value="7440300047/0,47uH"/>
</technology>
<technology name="_744030006">
<attribute name="WE-NUMBER" value="744030006/6,8uH"/>
</technology>
<technology name="_7440300068">
<attribute name="WE-NUMBER" value="7440300068/6,8uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_3816" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_3816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744031001">
<attribute name="WE-NUMBER" value="744031001/1,5uH"/>
</technology>
<technology name="_744031002">
<attribute name="WE-NUMBER" value="744031002/2,5uH"/>
</technology>
<technology name="_744031003">
<attribute name="WE-NUMBER" value="744031003/3,6uH"/>
</technology>
<technology name="_744031004">
<attribute name="WE-NUMBER" value="744031004/4,7uH"/>
</technology>
<technology name="_7440310047">
<attribute name="WE-NUMBER" value="7440310047/0,47uH"/>
</technology>
<technology name="_744031006">
<attribute name="WE-NUMBER" value="744031006/6,8uH"/>
</technology>
<technology name="_744031010">
<attribute name="WE-NUMBER" value="744031010/1uH"/>
</technology>
<technology name="_744031100">
<attribute name="WE-NUMBER" value="744031100/10uH"/>
</technology>
<technology name="_744031101">
<attribute name="WE-NUMBER" value="744031101/100uH"/>
</technology>
<technology name="_744031150">
<attribute name="WE-NUMBER" value="744031150/15uH"/>
</technology>
<technology name="_744031220">
<attribute name="WE-NUMBER" value="744031220/22uH"/>
</technology>
<technology name="_744031330">
<attribute name="WE-NUMBER" value="744031330/33uH"/>
</technology>
<technology name="_744031470">
<attribute name="WE-NUMBER" value="744031470/47uH"/>
</technology>
<technology name="_744031680">
<attribute name="WE-NUMBER" value="744031680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_4818" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Yingchun,Shan  2017-06-26&lt;br&gt;
&lt;/b&gt;2017(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_4818/4828">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74404200056">
<attribute name="WE-NUMBER" value="74404200056/0,56uH"/>
</technology>
<technology name="_744042001">
<attribute name="WE-NUMBER" value="744042001/1uH"/>
</technology>
<technology name="_7440420018">
<attribute name="WE-NUMBER" value="7440420018/1,8uH"/>
</technology>
<technology name="_7440420027">
<attribute name="WE-NUMBER" value="7440420027/2,7uH"/>
</technology>
<technology name="_744042003">
<attribute name="WE-NUMBER" value="744042003/3,3uH"/>
</technology>
<technology name="_7440420039">
<attribute name="WE-NUMBER" value="7440430039/3,9uH"/>
</technology>
<technology name="_744042004">
<attribute name="WE-NUMBER" value="744042004/4,7uH"/>
</technology>
<technology name="_744042005">
<attribute name="WE-NUMBER" value="744042005/5,6uH"/>
</technology>
<technology name="_744042006">
<attribute name="WE-NUMBER" value="744042006/6,8uH"/>
</technology>
<technology name="_744042008">
<attribute name="WE-NUMBER" value="744042008/8,2uH"/>
</technology>
<technology name="_744042100">
<attribute name="WE-NUMBER" value="744042100/10uH"/>
</technology>
<technology name="_744042101">
<attribute name="WE-NUMBER" value="-"/>
</technology>
<technology name="_744042120">
<attribute name="WE-NUMBER" value="744042120/12uH"/>
</technology>
<technology name="_744042150">
<attribute name="WE-NUMBER" value="-"/>
</technology>
<technology name="_744042180">
<attribute name="WE-NUMBER" value="-"/>
</technology>
<technology name="_744042220">
<attribute name="WE-NUMBER" value="-"/>
</technology>
<technology name="_744042221">
<attribute name="WE-NUMBER" value="744042221/220uH"/>
</technology>
<technology name="_744042330">
<attribute name="WE-NUMBER" value="-"/>
</technology>
<technology name="_744042331">
<attribute name="WE-NUMBER" value="-"/>
</technology>
<technology name="_744042470">
<attribute name="WE-NUMBER" value="-"/>
</technology>
<technology name="_744042680">
<attribute name="WE-NUMBER" value="-"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_4828" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Yingchun,Shan  2017-06-26&lt;br&gt;
&lt;/b&gt;2017(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_4818/4828">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74404300033">
<attribute name="WE-NUMBER" value="74404300033/0,33uH"/>
</technology>
<technology name="_74404300047">
<attribute name="WE-NUMBER" value="74404300047/0,47uH"/>
</technology>
<technology name="_74404300082">
<attribute name="WE-NUMBER" value="74404300082/0,82uH"/>
</technology>
<technology name="_7440430012">
<attribute name="WE-NUMBER" value="7440430012/1,2uH"/>
</technology>
<technology name="_7440430018">
<attribute name="WE-NUMBER" value="7440430018/1,8uH"/>
</technology>
<technology name="_7440430022">
<attribute name="WE-NUMBER" value="7440430022/2,2uH"/>
</technology>
<technology name="_7440430027">
<attribute name="WE-NUMBER" value="7440430027/2,7uH"/>
</technology>
<technology name="_744043003">
<attribute name="WE-NUMBER" value="744043003/3,3uH"/>
</technology>
<technology name="_7440430039">
<attribute name="WE-NUMBER" value="7440430039/3,9uH"/>
</technology>
<technology name="_744043004">
<attribute name="WE-NUMBER" value="744043004/4,7uH"/>
</technology>
<technology name="_744043005">
<attribute name="WE-NUMBER" value="744043005/5,6uH"/>
</technology>
<technology name="_744043006">
<attribute name="WE-NUMBER" value="744043006/6,8uH"/>
</technology>
<technology name="_744043008">
<attribute name="WE-NUMBER" value="744043008/8,2uH"/>
</technology>
<technology name="_744043100">
<attribute name="WE-NUMBER" value="744043100/10uH"/>
</technology>
<technology name="_744043101">
<attribute name="WE-NUMBER" value="744043101/100uH"/>
</technology>
<technology name="_744043102">
<attribute name="WE-NUMBER" value="744043102/1000uH"/>
</technology>
<technology name="_744043120">
<attribute name="WE-NUMBER" value="744043120/12uH"/>
</technology>
<technology name="_744043150">
<attribute name="WE-NUMBER" value="744043150/15uH"/>
</technology>
<technology name="_744043151">
<attribute name="WE-NUMBER" value="744043151/150uH"/>
</technology>
<technology name="_744043152">
<attribute name="WE-NUMBER" value="744043152/1500uH"/>
</technology>
<technology name="_744043180">
<attribute name="WE-NUMBER" value="744043180/18uH"/>
</technology>
<technology name="_744043220">
<attribute name="WE-NUMBER" value="744043220/22uH"/>
</technology>
<technology name="_744043221">
<attribute name="WE-NUMBER" value="744043221/220uH"/>
</technology>
<technology name="_744043270">
<attribute name="WE-NUMBER" value="744043270/27uH"/>
</technology>
<technology name="_744043330">
<attribute name="WE-NUMBER" value="744043330/33uH"/>
</technology>
<technology name="_744043331">
<attribute name="WE-NUMBER" value="744043331/330uH"/>
</technology>
<technology name="_744043390">
<attribute name="WE-NUMBER" value="744043390/39uH"/>
</technology>
<technology name="_744043470">
<attribute name="WE-NUMBER" value="744043470/47uH"/>
</technology>
<technology name="_744043471">
<attribute name="WE-NUMBER" value="744043471/470uH"/>
</technology>
<technology name="_744043561">
<attribute name="WE-NUMBER" value="744043561/560uH"/>
</technology>
<technology name="_744043680">
<attribute name="WE-NUMBER" value="744043680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_5818" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Yingchun,Shan  2017-06-26&lt;br&gt;
&lt;/b&gt;2017(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_5818/5828">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7440520012">
<attribute name="WE-NUMBER" value="7440520012/1,2uH"/>
</technology>
<technology name="_7440520018">
<attribute name="WE-NUMBER" value="7440520018/1,8uH"/>
</technology>
<technology name="_744052002">
<attribute name="WE-NUMBER" value="744052002/2,5uH"/>
</technology>
<technology name="_744052003">
<attribute name="WE-NUMBER" value="744052003/3uH"/>
</technology>
<technology name="_7440520039">
<attribute name="WE-NUMBER" value="7440520039/3,9uH"/>
</technology>
<technology name="_744052005">
<attribute name="WE-NUMBER" value="744052005/5uH"/>
</technology>
<technology name="_744052006">
<attribute name="WE-NUMBER" value="74405006/6,2uH"/>
</technology>
<technology name="_744052007">
<attribute name="WE-NUMBER" value="744052007/7,5uH"/>
</technology>
<technology name="_744052009">
<attribute name="WE-NUMBER" value="744052009/9uH"/>
</technology>
<technology name="_744052100">
<attribute name="WE-NUMBER" value="744052100/10uH"/>
</technology>
<technology name="_744052101">
<attribute name="WE-NUMBER" value="744052101/100uH"/>
</technology>
<technology name="_744052120">
<attribute name="WE-NUMBER" value="744052120/12uH"/>
</technology>
<technology name="_744052150">
<attribute name="WE-NUMBER" value="744052150/15uH"/>
</technology>
<technology name="_744052180">
<attribute name="WE-NUMBER" value="744052180/18uH"/>
</technology>
<technology name="_744052220">
<attribute name="WE-NUMBER" value="744052220/22uH"/>
</technology>
<technology name="_744052221">
<attribute name="WE-NUMBER" value="744052221/220uH"/>
</technology>
<technology name="_744052270">
<attribute name="WE-NUMBER" value="744052270/27uH"/>
</technology>
<technology name="_744052470">
<attribute name="WE-NUMBER" value="744052470/47uH"/>
</technology>
<technology name="_744052471">
<attribute name="WE-NUMBER" value="744052471/470uH"/>
</technology>
<technology name="_744052680">
<attribute name="WE-NUMBER" value="744052680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_5828" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Yingchun,Shan  2017-06-26&lt;br&gt;
&lt;/b&gt;2017(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_5818/5828">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744053002">
<attribute name="WE-NUMBER" value="744053002/2,6uH"/>
</technology>
<technology name="_744053003">
<attribute name="WE-NUMBER" value="744053003/3uH"/>
</technology>
<technology name="_744053004">
<attribute name="WE-NUMBER" value="744053004/4,2uH"/>
</technology>
<technology name="_7440530047">
<attribute name="WE-NUMBER" value="7440530047/4,7uH"/>
</technology>
<technology name="_744053005">
<attribute name="WE-NUMBER" value="744053005/5,3uH"/>
</technology>
<technology name="_744053006">
<attribute name="WE-NUMBER" value="744053006/6,2uH"/>
</technology>
<technology name="_744053008">
<attribute name="WE-NUMBER" value="744053008/8,2uH"/>
</technology>
<technology name="_744053100">
<attribute name="WE-NUMBER" value="744053100/10uH"/>
</technology>
<technology name="_744053101">
<attribute name="WE-NUMBER" value="744053101/100uH"/>
</technology>
<technology name="_744053120">
<attribute name="WE-NUMBER" value="744053120/12uH"/>
</technology>
<technology name="_744053150">
<attribute name="WE-NUMBER" value="744053150/15uH"/>
</technology>
<technology name="_744053180">
<attribute name="WE-NUMBER" value="744053180/18uH"/>
</technology>
<technology name="_744053220">
<attribute name="WE-NUMBER" value="744053220/22uH"/>
</technology>
<technology name="_744053221">
<attribute name="WE-NUMBER" value="744053221/220uH"/>
</technology>
<technology name="_744053270">
<attribute name="WE-NUMBER" value="744053270/27uH"/>
</technology>
<technology name="_744053330">
<attribute name="WE-NUMBER" value="744053330/33uH"/>
</technology>
<technology name="_744053470">
<attribute name="WE-NUMBER" value="744053470/47uH"/>
</technology>
<technology name="_744053680">
<attribute name="WE-NUMBER" value="744053680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_6823" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by Yingchun,Shan  2017-06-26&lt;br&gt;
&lt;/b&gt;2017(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_6823">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744062001">
<attribute name="WE-NUMBER" value="744062001/1uH"/>
</technology>
<technology name="_7440620015">
<attribute name="WE-NUMBER" value="7440620015/0,15uH"/>
</technology>
<technology name="_744062002">
<attribute name="WE-NUMBER" value="744062002/2,2uH"/>
</technology>
<technology name="_744062003">
<attribute name="WE-NUMBER" value="744062003/3,3uH"/>
</technology>
<technology name="_744062005">
<attribute name="WE-NUMBER" value="744062005/5uH"/>
</technology>
<technology name="_744062006">
<attribute name="WE-NUMBER" value="744062006/6,2uH"/>
</technology>
<technology name="_744062007">
<attribute name="WE-NUMBER" value="744062007/7,5uH"/>
</technology>
<technology name="_744062100">
<attribute name="WE-NUMBER" value="744062100/10uH"/>
</technology>
<technology name="_744062101">
<attribute name="WE-NUMBER" value="744062101/100uH"/>
</technology>
<technology name="_744062102">
<attribute name="WE-NUMBER" value="744062102/1000uH"/>
</technology>
<technology name="_744062120">
<attribute name="WE-NUMBER" value="744062120/12uH"/>
</technology>
<technology name="_744062150">
<attribute name="WE-NUMBER" value="744062150/15uH"/>
</technology>
<technology name="_744062151">
<attribute name="WE-NUMBER" value="744062151/150uH"/>
</technology>
<technology name="_744062152">
<attribute name="WE-NUMBER" value="744062152/1500uH"/>
</technology>
<technology name="_744062180">
<attribute name="WE-NUMBER" value="744062180/18uH"/>
</technology>
<technology name="_744062220">
<attribute name="WE-NUMBER" value="744062220/22uH"/>
</technology>
<technology name="_744062221">
<attribute name="WE-NUMBER" value="744062221/220uH"/>
</technology>
<technology name="_744062330">
<attribute name="WE-NUMBER" value="744062330/33uH"/>
</technology>
<technology name="_744062470">
<attribute name="WE-NUMBER" value="744062470/47uH"/>
</technology>
<technology name="_744062680">
<attribute name="WE-NUMBER" value="744062680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_8012" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_8015/8012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="_74406800024">
<attribute name="WE-NUMBER" value="74406800024/0,24uH"/>
</technology>
<technology name="_74406800056">
<attribute name="WE-NUMBER" value="74406800056/0,56uH"/>
</technology>
<technology name="_7440680010">
<attribute name="WE-NUMBER" value="7440680010/1uH"/>
</technology>
<technology name="_7440680017">
<attribute name="WE-NUMBER" value="7440680017/1,7uH"/>
</technology>
<technology name="_7440680027">
<attribute name="WE-NUMBER" value="7440680027/2,7uH"/>
</technology>
<technology name="_7440680033">
<attribute name="WE-NUMBER" value="7440680033/3,3uH"/>
</technology>
<technology name="_7440680047">
<attribute name="WE-NUMBER" value="7440680047/4,7uH"/>
</technology>
<technology name="_7440680056">
<attribute name="WE-NUMBER" value="7440680056/5,6uH"/>
</technology>
<technology name="_7440680068">
<attribute name="WE-NUMBER" value="7440680068/6,8uH"/>
</technology>
<technology name="_7440680082">
<attribute name="WE-NUMBER" value="7440680082/8,2uH"/>
</technology>
<technology name="_7440680100">
<attribute name="WE-NUMBER" value="7440680100/10uH"/>
</technology>
<technology name="_7440680120">
<attribute name="WE-NUMBER" value="7440680120/12uH"/>
</technology>
<technology name="_7440680150">
<attribute name="WE-NUMBER" value="7440680150/15uH"/>
</technology>
<technology name="_7440680180">
<attribute name="WE-NUMBER" value="7440680180/18uH"/>
</technology>
<technology name="_7440680220">
<attribute name="WE-NUMBER" value="7440680220/22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_8015" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_8015/8012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="_74406900022">
<attribute name="WE-NUMBER" value="74406900022/0,22uH"/>
</technology>
<technology name="_74406900052">
<attribute name="WE-NUMBER" value="74406900052/0,52uH"/>
</technology>
<technology name="_7440690010">
<attribute name="WE-NUMBER" value="7440690010/1uH"/>
</technology>
<technology name="_7440690016">
<attribute name="WE-NUMBER" value="7440690016/1,6uH"/>
</technology>
<technology name="_7440690022">
<attribute name="WE-NUMBER" value="7440690022/2,2uH"/>
</technology>
<technology name="_7440690033">
<attribute name="WE-NUMBER" value="7440690033/3,3uH"/>
</technology>
<technology name="_7440690047">
<attribute name="WE-NUMBER" value="7440690047/4,7uH"/>
</technology>
<technology name="_7440690068">
<attribute name="WE-NUMBER" value="7440690068/6,8uH"/>
</technology>
<technology name="_7440690082">
<attribute name="WE-NUMBER" value="7440690082/8,2uH"/>
</technology>
<technology name="_7440690100">
<attribute name="WE-NUMBER" value="7440690100/10uH"/>
</technology>
<technology name="_7440690120">
<attribute name="WE-NUMBER" value="7440690120/12uH"/>
</technology>
<technology name="_7440690150">
<attribute name="WE-NUMBER" value="7440690150/15uH"/>
</technology>
<technology name="_7440690180">
<attribute name="WE-NUMBER" value="7440690180/18uH"/>
</technology>
<technology name="_7440690220">
<attribute name="WE-NUMBER" value="7440690220/22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_8020" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_8020/8043">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="_74407000018">
<attribute name="WE-NUMBER" value="74407000018/0,18uH"/>
</technology>
<technology name="_74407000047">
<attribute name="WE-NUMBER" value="74407000047/0,47uH"/>
</technology>
<technology name="_74407000082">
<attribute name="WE-NUMBER" value="74407000082/0,82uH"/>
</technology>
<technology name="_7440700012">
<attribute name="WE-NUMBER" value="7440700012/1,2uH"/>
</technology>
<technology name="_7440700022">
<attribute name="WE-NUMBER" value="7440700022/2,2uH"/>
</technology>
<technology name="_7440700033">
<attribute name="WE-NUMBER" value="7440700033/3,3uH"/>
</technology>
<technology name="_7440700047">
<attribute name="WE-NUMBER" value="7440700047/4,7uH"/>
</technology>
<technology name="_7440700056">
<attribute name="WE-NUMBER" value="7440700056/5,6uH"/>
</technology>
<technology name="_7440700068">
<attribute name="WE-NUMBER" value="7440700068/6,8uH"/>
</technology>
<technology name="_7440700082">
<attribute name="WE-NUMBER" value="7440700082/8,2uH"/>
</technology>
<technology name="_7440700100">
<attribute name="WE-NUMBER" value="7440700100/10uH"/>
</technology>
<technology name="_7440700150">
<attribute name="WE-NUMBER" value="7440700150/15uH"/>
</technology>
<technology name="_7440700180">
<attribute name="WE-NUMBER" value="7440700180/18uH"/>
</technology>
<technology name="_7440700220">
<attribute name="WE-NUMBER" value="7440700220/22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_8043" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_8020/8043">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="_7440710082">
<attribute name="WE-NUMBER" value="7440710082/0,82uH"/>
</technology>
<technology name="_744071022">
<attribute name="WE-NUMBER" value="744071022/2,2uH"/>
</technology>
<technology name="_744071039">
<attribute name="WE-NUMBER" value="744071039/3,9uH"/>
</technology>
<technology name="_744071047">
<attribute name="WE-NUMBER" value="744071047/4,7uH"/>
</technology>
<technology name="_744071056">
<attribute name="WE-NUMBER" value="744071056/5,6uH"/>
</technology>
<technology name="_744071100">
<attribute name="WE-NUMBER" value="744071100/10uH"/>
</technology>
<technology name="_744071101">
<attribute name="WE-NUMBER" value="744071101/100uH"/>
</technology>
<technology name="_744071102">
<attribute name="WE-NUMBER" value="744071102/1000uH"/>
</technology>
<technology name="_744071150">
<attribute name="WE-NUMBER" value="744071150/15uH"/>
</technology>
<technology name="_744071220">
<attribute name="WE-NUMBER" value="744071220/22uH"/>
</technology>
<technology name="_744071221">
<attribute name="WE-NUMBER" value="744071221/220uH"/>
</technology>
<technology name="_744071330">
<attribute name="WE-NUMBER" value="744071330/33uH"/>
</technology>
<technology name="_744071470">
<attribute name="WE-NUMBER" value="744071470/47uH"/>
</technology>
<technology name="_744071680">
<attribute name="WE-NUMBER" value="744071680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_1028" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_1028/1038">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744065001">
<attribute name="WE-NUMBER" value="744065001/1uH"/>
</technology>
<technology name="_7440650015">
<attribute name="WE-NUMBER" value="7440650015/1,5uH"/>
</technology>
<technology name="_7440650022">
<attribute name="WE-NUMBER" value="7440650022/2,2uH"/>
</technology>
<technology name="_7440650033">
<attribute name="WE-NUMBER" value="7440650033/3,3uH"/>
</technology>
<technology name="_7440650047">
<attribute name="WE-NUMBER" value="7440650047/4,7uH"/>
</technology>
<technology name="_7440650068">
<attribute name="WE-NUMBER" value="7440650068/6,8uH"/>
</technology>
<technology name="_7440650082">
<attribute name="WE-NUMBER" value="7440650082/8,2uH"/>
</technology>
<technology name="_744065100">
<attribute name="WE-NUMBER" value="744065100/10uH"/>
</technology>
<technology name="_744065101">
<attribute name="WE-NUMBER" value="744065101/100uH"/>
</technology>
<technology name="_744065121">
<attribute name="WE-NUMBER" value="744065121/120uH"/>
</technology>
<technology name="_744065150">
<attribute name="WE-NUMBER" value="744065150/15uH"/>
</technology>
<technology name="_744065151">
<attribute name="WE-NUMBER" value="744065151/150uH"/>
</technology>
<technology name="_744065220">
<attribute name="WE-NUMBER" value="744065220/22uH"/>
</technology>
<technology name="_744065221">
<attribute name="WE-NUMBER" value="744065221/220uH"/>
</technology>
<technology name="_744065330">
<attribute name="WE-NUMBER" value="744065330/33uH"/>
</technology>
<technology name="_744065470">
<attribute name="WE-NUMBER" value="744065470/47uH"/>
</technology>
<technology name="_744065560">
<attribute name="WE-NUMBER" value="744065560/56uH"/>
</technology>
<technology name="_744065680">
<attribute name="WE-NUMBER" value="744065680/68uH"/>
</technology>
<technology name="_744065820">
<attribute name="WE-NUMBER" value="744065820/82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_1038" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Shielded Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;
&lt;br&gt; High current capability
&lt;br&gt;
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt;
&lt;brr&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;
&lt;br&gt; DC/DC converter
&lt;br&gt;
&lt;br&gt; Embedded PC
&lt;br&gt;
&lt;br&gt; Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndTPC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TPC?"&gt;http://katalog.we-online.de/en/pbs/WE-TPC?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TPC_1028/1038">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7440660015">
<attribute name="WE-NUMBER" value="7440660015/1,5uH"/>
</technology>
<technology name="_7440660022">
<attribute name="WE-NUMBER" value="7440660022/2,2uH"/>
</technology>
<technology name="_7440660035">
<attribute name="WE-NUMBER" value="7440660035/3,5uH"/>
</technology>
<technology name="_744066005">
<attribute name="WE-NUMBER" value="744066005/5uH"/>
</technology>
<technology name="_7440660062">
<attribute name="WE-NUMBER" value="7440660062/6,2uH"/>
</technology>
<technology name="_744066100">
<attribute name="WE-NUMBER" value="744066100/10uH"/>
</technology>
<technology name="_744066101">
<attribute name="WE-NUMBER" value="744066101/100uH"/>
</technology>
<technology name="_744066150">
<attribute name="WE-NUMBER" value="744066150/15uH"/>
</technology>
<technology name="_744066151">
<attribute name="WE-NUMBER" value="744066151/150uH"/>
</technology>
<technology name="_744066180">
<attribute name="WE-NUMBER" value="744066180/18uH"/>
</technology>
<technology name="_744066220">
<attribute name="WE-NUMBER" value="744066220/22uH"/>
</technology>
<technology name="_744066221">
<attribute name="WE-NUMBER" value="744066221/220uH"/>
</technology>
<technology name="_744066330">
<attribute name="WE-NUMBER" value="744066330/33uH"/>
</technology>
<technology name="_744066331">
<attribute name="WE-NUMBER" value="744066331/330uH"/>
</technology>
<technology name="_744066470">
<attribute name="WE-NUMBER" value="744066470/47uH"/>
</technology>
<technology name="_744066680">
<attribute name="WE-NUMBER" value="744066680/68uH"/>
</technology>
<technology name="_744066681">
<attribute name="WE-NUMBER" value="744066681/680uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CBF_0402" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CBF SMD EMI Suppression Ferrite Bead
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Reliable Ni-Sn electrodes
&lt;br&gt;
&lt;br&gt; High rated current up to 6 A
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfect as data lined filter and for uncoupling of distribution voltage
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeCBF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeCBF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBF"&gt;http://katalog.we-online.de/en/pbs/WE-CBF&lt;/a&gt;&lt;p&gt;

Updated on 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_WB_HS" package="WE-CBF_0402(W=1.5)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279270">
<attribute name="WE-NUMBER" value="74279270/40Ω(Z@100MHz)"/>
</technology>
<technology name="_742792701">
<attribute name="WE-NUMBER" value="742792701/10Ω(Z@100MHz)"/>
</technology>
<technology name="_74279271">
<attribute name="WE-NUMBER" value="74279271/120Ω(Z@100MHz)"/>
</technology>
<technology name="_742792711">
<attribute name="WE-NUMBER" value="742792711/100Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927110">
<attribute name="WE-NUMBER" value="7427924110/10Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927112">
<attribute name="WE-NUMBER" value="7427927112/120Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927115">
<attribute name="WE-NUMBER" value="7427927115/150Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927121">
<attribute name="WE-NUMBER" value="7427927121/220Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927130">
<attribute name="WE-NUMBER" value="7427927130/30Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927140">
<attribute name="WE-NUMBER" value="7427927140/47Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927141">
<attribute name="WE-NUMBER" value="7427927141/470Ω(Z@100MHz)"/>
</technology>
<technology name="_742792716">
<attribute name="WE-NUMBER" value="742792716/60Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927160">
<attribute name="WE-NUMBER" value="7427927160/60Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927161">
<attribute name="WE-NUMBER" value="7427927161/600Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927170">
<attribute name="WE-NUMBER" value="7427927170/75Ω(Z@100MHz)"/>
</technology>
<technology name="_74279272">
<attribute name="WE-NUMBER" value="74279272/300Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927218">
<attribute name="WE-NUMBER" value="7427927218/180Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927241">
<attribute name="WE-NUMBER" value="7427927241/470Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927261">
<attribute name="WE-NUMBER" value="7427927261/600Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927280">
<attribute name="WE-NUMBER" value="7427927280/80Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927281">
<attribute name="WE-NUMBER" value="7427927281/800Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927291">
<attribute name="WE-NUMBER" value="7427927291/600Ω(Z@100MHz)"/>
</technology>
<technology name="_74279273">
<attribute name="WE-NUMBER" value="74279273/20Ω(Z@100MHz)"/>
</technology>
<technology name="_74279274">
<attribute name="WE-NUMBER" value="74279274/30Ω(Z@100MHz)"/>
</technology>
<technology name="_74279276">
<attribute name="WE-NUMBER" value="74279276/60Ω(Z@100MHz)"/>
</technology>
<technology name="_74279277">
<attribute name="WE-NUMBER" value="74279277/70Ω(Z@100MHz)"/>
</technology>
<technology name="_74279278">
<attribute name="WE-NUMBER" value="74279278/240Ω(Z@100MHz)"/>
</technology>
<technology name="_74279279">
<attribute name="WE-NUMBER" value="74279279/600Ω(Z@100MHz)"/>
</technology>
<technology name="_742792796">
<attribute name="WE-NUMBER" value="742792796/1000Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
<device name="_HC" package="WE-CBF_0402(W=2.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742792731">
<attribute name="WE-NUMBER" value="742792731/100Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927310">
<attribute name="WE-NUMBER" value="7427927310/10Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927311">
<attribute name="WE-NUMBER" value="7427927311/200Ω(Z@100MHz)"/>
</technology>
<technology name="_7427927370">
<attribute name="WE-NUMBER" value="7427927370/70Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CBF_0603" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CBF SMD EMI Suppression Ferrite Bead
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Reliable Ni-Sn electrodes
&lt;br&gt;
&lt;br&gt; High rated current up to 6 A
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfect as data lined filter and for uncoupling of distribution voltage
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeCBF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeCBF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBF"&gt;http://katalog.we-online.de/en/pbs/WE-CBF&lt;/a&gt;&lt;p&gt;

Updated on 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_WB_HS" package="WE-CBF_0603(W=2.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279260">
<attribute name="WE-NUMBER" value="74279260/40Ω(Z@100MHz)"/>
</technology>
<technology name="_742792605">
<attribute name="WE-NUMBER" value="742792605/33Ω(Z@100MHz)"/>
</technology>
<technology name="_742792606">
<attribute name="WE-NUMBER" value="742792606/120Ω(Z@100MHz)"/>
</technology>
<technology name="_742792607">
<attribute name="WE-NUMBER" value="742792607/68Ω(Z@100MHz)"/>
</technology>
<technology name="_742792608">
<attribute name="WE-NUMBER" value="742792608/47Ω(Z@100MHz)"/>
</technology>
<technology name="_74279261">
<attribute name="WE-NUMBER" value="74279261/80Ω(Z@100MHz)"/>
</technology>
<technology name="_74279262">
<attribute name="WE-NUMBER" value="74279262/120Ω(Z@100MHz)"/>
</technology>
<technology name="_742792620">
<attribute name="WE-NUMBER" value="742792620/100Ω(Z@100MHz)"/>
</technology>
<technology name="_742792621">
<attribute name="WE-NUMBER" value="742792621/140Ω(Z@100MHz)"/>
</technology>
<technology name="_742792622">
<attribute name="WE-NUMBER" value="742792622/180Ω(Z@100MHz)"/>
</technology>
<technology name="_74279263">
<attribute name="WE-NUMBER" value="74279263/220Ω(Z@100MHz)"/>
</technology>
<technology name="_742792631">
<attribute name="WE-NUMBER" value="742792631/240Ω(Z@100MHz)"/>
</technology>
<technology name="_74279264">
<attribute name="WE-NUMBER" value="74279264/300Ω(Z@100MHz)"/>
</technology>
<technology name="_742792640">
<attribute name="WE-NUMBER" value="742792640/300Ω(Z@100MHz)"/>
</technology>
<technology name="_742792642">
<attribute name="WE-NUMBER" value="742792642/470Ω(Z@100MHz)"/>
</technology>
<technology name="_742792643">
<attribute name="WE-NUMBER" value="742792643/470Ω(Z@100MHz)"/>
</technology>
<technology name="_74279265">
<attribute name="WE-NUMBER" value="74279265/600Ω(Z@100MHz)"/>
</technology>
<technology name="_742792651">
<attribute name="WE-NUMBER" value="742792651/600Ω(Z@100MHz)"/>
</technology>
<technology name="_742792653">
<attribute name="WE-NUMBER" value="742792653/600Ω(Z@100MHz)"/>
</technology>
<technology name="_742792656">
<attribute name="WE-NUMBER" value="742792656/750Ω(Z@100MHz)"/>
</technology>
<technology name="_74279266">
<attribute name="WE-NUMBER" value="74279266/1000Ω(Z@100MHz)"/>
</technology>
<technology name="_742792662">
<attribute name="WE-NUMBER" value="742792662/1000Ω(Z@100MHz)"/>
</technology>
<technology name="_742792663">
<attribute name="WE-NUMBER" value="742792663/1000Ω(Z@100MHz)"/>
</technology>
<technology name="_742792664">
<attribute name="WE-NUMBER" value="742792664/1000Ω(Z@100MHz)"/>
</technology>
<technology name="_74279267">
<attribute name="WE-NUMBER" value="74279267/60Ω(Z@100MHz)"/>
</technology>
<technology name="_74279268">
<attribute name="WE-NUMBER" value="74279268/15Ω(Z@100MHz)"/>
</technology>
<technology name="_74279269">
<attribute name="WE-NUMBER" value="74279269/1200Ω(Z@100MHz)"/>
</technology>
<technology name="_742792691">
<attribute name="WE-NUMBER" value="742792691/1500Ω(Z@100MHz)"/>
</technology>
<technology name="_742792692">
<attribute name="WE-NUMBER" value="742792692/1800Ω(Z@100MHz)"/>
</technology>
<technology name="_742792693">
<attribute name="WE-NUMBER" value="742792693/2200Ω(Z@100MHz)"/>
</technology>
<technology name="_742792695">
<attribute name="WE-NUMBER" value="742792695/2500Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
<device name="_HC" package="WE-CBF_0603(W=2.6)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742792601">
<attribute name="WE-NUMBER" value="742792601/30Ω(Z@100MHz)"/>
</technology>
<technology name="_742792602">
<attribute name="WE-NUMBER" value="742792602/60Ω(Z@100MHz)"/>
</technology>
<technology name="_742792603">
<attribute name="WE-NUMBER" value="742792603/28Ω(Z@100MHz)"/>
</technology>
<technology name="_742792604">
<attribute name="WE-NUMBER" value="742792604/22Ω(Z@100MHz)"/>
</technology>
<technology name="_742792609">
<attribute name="WE-NUMBER" value="742792609/30Ω(Z@100MHz)"/>
</technology>
<technology name="_742792624">
<attribute name="WE-NUMBER" value="742792624/180Ω(Z@100MHz)"/>
</technology>
<technology name="_742792625">
<attribute name="WE-NUMBER" value="742792625/120Ω(Z@100MHz)"/>
</technology>
<technology name="_742792641">
<attribute name="WE-NUMBER" value="742792641/300Ω(Z@100MHz)"/>
</technology>
<technology name="_742792645">
<attribute name="WE-NUMBER" value="742795645/470Ω(Z@100MHz)"/>
</technology>
<technology name="_742792651">
<attribute name="WE-NUMBER" value="742792651/600Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CBF_0805" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CBF SMD EMI Suppression Ferrite Bead
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Reliable Ni-Sn electrodes
&lt;br&gt;
&lt;br&gt; High rated current up to 6 A
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfect as data lined filter and for uncoupling of distribution voltage
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeCBF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeCBF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBF"&gt;http://katalog.we-online.de/en/pbs/WE-CBF&lt;/a&gt;&lt;p&gt;

Updated on 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_WB_HS" package="WE-CBF_0805(W=3.0)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7427920">
<attribute name="WE-NUMBER" value="7427920/11Ω(Z@100MHz)"/>
</technology>
<technology name="_742792005">
<attribute name="WE-NUMBER" value="742792005/5Ω(Z@100MHz)"/>
</technology>
<technology name="_74279201">
<attribute name="WE-NUMBER" value="74279201/32Ω(Z@100MHz)"/>
</technology>
<technology name="_742792015">
<attribute name="WE-NUMBER" value="742792015/56Ω(Z@100MHz)"/>
</technology>
<technology name="_74279202">
<attribute name="WE-NUMBER" value="74279202/120Ω(Z@100MHz)"/>
</technology>
<technology name="_74279203">
<attribute name="WE-NUMBER" value="74279203/150Ω(Z@100MHz)"/>
</technology>
<technology name="_742792032">
<attribute name="WE-NUMBER" value="742792032/400Ω(Z@100MHz)"/>
</technology>
<technology name="_742792034">
<attribute name="WE-NUMBER" value="742792034/220Ω(Z@100MHz)"/>
</technology>
<technology name="_742792035">
<attribute name="WE-NUMBER" value="742792035/300Ω(Z@100MHz)"/>
</technology>
<technology name="_742792036">
<attribute name="WE-NUMBER" value="742792036/470Ω(Z@100MHz)"/>
</technology>
<technology name="_742792038">
<attribute name="WE-NUMBER" value="742792038/240Ω(Z@100MHz)"/>
</technology>
<technology name="_74279204">
<attribute name="WE-NUMBER" value="74279204/600Ω(Z@100MHz)"/>
</technology>
<technology name="_742792041">
<attribute name="WE-NUMBER" value="742792041/600Ω(Z@100MHz)"/>
</technology>
<technology name="_7427920415">
<attribute name="WE-NUMBER" value="7427920415/600Ω(Z@100MHz)"/>
</technology>
<technology name="_742792042">
<attribute name="WE-NUMBER" value="742792042/600Ω(Z@100MHz)"/>
</technology>
<technology name="_742792043">
<attribute name="WE-NUMBER" value="742792043/600Ω(Z@100MHz)"/>
</technology>
<technology name="_742792045">
<attribute name="WE-NUMBER" value="742792045/750Ω(Z@100MHz)"/>
</technology>
<technology name="_74279205">
<attribute name="WE-NUMBER" value="74279205/1000Ω(Z@100MHz)"/>
</technology>
<technology name="_742792062">
<attribute name="WE-NUMBER" value="742792062/80Ω(Z@100MHz)"/>
</technology>
<technology name="_742792064">
<attribute name="WE-NUMBER" value="742792064/75Ω(Z@100MHz)"/>
</technology>
<technology name="_74279208">
<attribute name="WE-NUMBER" value="74279208/40Ω(Z@100MHz)"/>
</technology>
<technology name="_74279209">
<attribute name="WE-NUMBER" value="74279209/1200Ω(Z@100MHz)"/>
</technology>
<technology name="_742792090">
<attribute name="WE-NUMBER" value="742792090/1800Ω(Z@100MHz)"/>
</technology>
<technology name="_742792091">
<attribute name="WE-NUMBER" value="742792091/1500Ω(Z@100MHz)"/>
</technology>
<technology name="_742792092">
<attribute name="WE-NUMBER" value="742792092/2000Ω(Z@100MHz)"/>
</technology>
<technology name="_742792093">
<attribute name="WE-NUMBER" value="742792093/2200Ω(Z@100MHz)"/>
</technology>
<technology name="_742792094">
<attribute name="WE-NUMBER" value="742792094/2200Ω(Z@100MHz)"/>
</technology>
<technology name="_742792095">
<attribute name="WE-NUMBER" value="742792095/2700Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
<device name="_HC" package="WE-CBF_0805(W=4.0)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742792011">
<attribute name="WE-NUMBER" value="742792011/10Ω(Z@100MHz)"/>
</technology>
<technology name="_742792012">
<attribute name="WE-NUMBER" value="742792012/33Ω(Z@100MHz)"/>
</technology>
<technology name="_742792021">
<attribute name="WE-NUMBER" value="742792021/22Ω(Z@100MHz)"/>
</technology>
<technology name="_742792022">
<attribute name="WE-NUMBER" value="742792022/220Ω(Z@100MHz)"/>
</technology>
<technology name="_742792023">
<attribute name="WE-NUMBER" value="742792023/120Ω(Z@100MHz)"/>
</technology>
<technology name="_742792031">
<attribute name="WE-NUMBER" value="742792031/300Ω(Z@100MHz)"/>
</technology>
<technology name="_742792037">
<attribute name="WE-NUMBER" value="742792037/330Ω(Z@100MHz)"/>
</technology>
<technology name="_742792040">
<attribute name="WE-NUMBER" value="742792040/600Ω(Z@100MHz)"/>
</technology>
<technology name="_74279206">
<attribute name="WE-NUMBER" value="74279206/30Ω(Z@100MHz)"/>
</technology>
<technology name="_742792063">
<attribute name="WE-NUMBER" value="742792063/60Ω(Z@100MHz)"/>
</technology>
<technology name="_74279207">
<attribute name="WE-NUMBER" value="74279207/100Ω(Z@100MHz)"/>
</technology>
<technology name="_742792096">
<attribute name="WE-NUMBER" value="742792096/1000Ω(Z@100MHz)"/>
</technology>
<technology name="_742792097">
<attribute name="WE-NUMBER" value="742792097/1500Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CBF_1206" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CBF SMD EMI Suppression Ferrite Bead
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Reliable Ni-Sn electrodes
&lt;br&gt;
&lt;br&gt; High rated current up to 6 A
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfect as data lined filter and for uncoupling of distribution voltage
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeCBF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeCBF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBF"&gt;http://katalog.we-online.de/en/pbs/WE-CBF&lt;/a&gt;&lt;p&gt;

Updated on 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_WB-HS" package="WE-CBF_1206(W=4.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7427921">
<attribute name="WE-NUMBER" value="7427921/32Ω(Z@100MHz)"/>
</technology>
<technology name="_74279211">
<attribute name="WE-NUMBER" value="74279211/90Ω(Z@100MHz)"/>
</technology>
<technology name="_74279212">
<attribute name="WE-NUMBER" value="74279212/150Ω(Z@100MHz)"/>
</technology>
<technology name="_742792122">
<attribute name="WE-NUMBER" value="742792122/220Ω(Z@100MHz)"/>
</technology>
<technology name="_742792124">
<attribute name="WE-NUMBER" value="742792124/470Ω(Z@100MHz)"/>
</technology>
<technology name="_742792131">
<attribute name="WE-NUMBER" value="742792131/600Ω(Z@100MHz)"/>
</technology>
<technology name="_742792133">
<attribute name="WE-NUMBER" value="742792133/600Ω(Z@100MHz)"/>
</technology>
<technology name="_74279214">
<attribute name="WE-NUMBER" value="74279214/1000Ω(Z@100MHz)"/>
</technology>
<technology name="_742792151">
<attribute name="WE-NUMBER" value="742792151/70Ω(Z@100MHz)"/>
</technology>
<technology name="_74279216">
<attribute name="WE-NUMBER" value="74279216/1200Ω(Z@100MHz)"/>
</technology>
<technology name="_74279219">
<attribute name="WE-NUMBER" value="74279219/700Ω(Z@100MHz)"/>
</technology>
<technology name="_7427922">
<attribute name="WE-NUMBER" value="7427922/60Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
<device name="_HC" package="WE-CBF_1206(W=5.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742792110">
<attribute name="WE-NUMBER" value="742792110/19Ω(Z@100MHz)"/>
</technology>
<technology name="_742792111">
<attribute name="WE-NUMBER" value="742792111/26Ω(Z@100MHz)"/>
</technology>
<technology name="_742792112">
<attribute name="WE-NUMBER" value="742792112/31Ω(Z@100MHz)"/>
</technology>
<technology name="_742792113">
<attribute name="WE-NUMBER" value="742792113/120Ω(Z@100MHz)"/>
</technology>
<technology name="_742792114">
<attribute name="WE-NUMBER" value="742792114/50Ω(Z@100MHz)"/>
</technology>
<technology name="_742792116">
<attribute name="WE-NUMBER" value="742792116/500Ω(Z@100MHz)"/>
</technology>
<technology name="_742792118">
<attribute name="WE-NUMBER" value="742792118/600Ω(Z@100MHz)"/>
</technology>
<technology name="_742792121">
<attribute name="WE-NUMBER" value="742792121/300Ω(Z@100MHz)"/>
</technology>
<technology name="_742792141">
<attribute name="WE-NUMBER" value="742792141/1000Ω(Z@100MHz)"/>
</technology>
<technology name="_74279215">
<attribute name="WE-NUMBER" value="74279215/80Ω(Z@100MHz)"/>
</technology>
<technology name="_742792150">
<attribute name="WE-NUMBER" value="742792150/80Ω(Z@100MHz)"/>
</technology>
<technology name="_74279218">
<attribute name="WE-NUMBER" value="74279218/600Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CBF_1210" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CBF SMD EMI Suppression Ferrite Bead
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Reliable Ni-Sn electrodes
&lt;br&gt;
&lt;br&gt; High rated current up to 6 A
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfect as data lined filter and for uncoupling of distribution voltage
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeCBF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeCBF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBF"&gt;http://katalog.we-online.de/en/pbs/WE-CBF&lt;/a&gt;&lt;p&gt;

Updated on 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_WB-HS" package="WE-CBF_1210(W=4.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7427923">
<attribute name="WE-NUMBER" value="7427923/90Ω(Z@100MHz)"/>
</technology>
<technology name="_74279230">
<attribute name="WE-NUMBER" value="74279230/32Ω(Z@100MHz)"/>
</technology>
<technology name="_74279231">
<attribute name="WE-NUMBER" value="74279231/60Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
<device name="_HC" package="WE-CBF_1210(W=5.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742792310">
<attribute name="WE-NUMBER" value="742792310/30Ω(Z@100MHz)"/>
</technology>
<technology name="_742792311">
<attribute name="WE-NUMBER" value="742792311/52Ω(Z@100MHz)"/>
</technology>
<technology name="_742792312">
<attribute name="WE-NUMBER" value="742792312/65Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CBF_1806" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CBF SMD EMI Suppression Ferrite Bead
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Reliable Ni-Sn electrodes
&lt;br&gt;
&lt;br&gt; High rated current up to 6 A
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfect as data lined filter and for uncoupling of distribution voltage
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/FeCBF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_FeCBF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBF"&gt;http://katalog.we-online.de/en/pbs/WE-CBF&lt;/a&gt;&lt;p&gt;

Updated on 2014-06-19&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_WB_HS" package="WE-CBF_1806(W=5.5)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7427924">
<attribute name="WE-NUMBER" value="7427924/60Ω(Z@100MHz)"/>
</technology>
<technology name="_74279241">
<attribute name="WE-NUMBER" value="74279241/80Ω(Z@100MHz)"/>
</technology>
<technology name="_74279242">
<attribute name="WE-NUMBER" value="74279242/150Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
<device name="_HC" package="WE-CBF_1806(W=6.5)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742792410">
<attribute name="WE-NUMBER" value="742792410/60Ω(Z@100MHz)"/>
</technology>
<technology name="_742792411">
<attribute name="WE-NUMBER" value="742792411/80Ω(Z@100MHz)"/>
</technology>
<technology name="_74279243">
<attribute name="WE-NUMBER" value="74279243/75Ω(Z@100MHz)"/>
</technology>
<technology name="_74279244">
<attribute name="WE-NUMBER" value="74279244/850Ω(Z@100MHz)"/>
</technology>
<technology name="_74279245">
<attribute name="WE-NUMBER" value="74279245/110Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CBF_HF_0603" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CBF HF SMD EMI Suppression Ferrite Bead (High Frequency)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Available in 3 types 
&lt;br&gt; Modified internal layout increases the effective suppression range 
&lt;br&gt; The impedance at 1 GHz are at least 3 times higher compared to the WE-CBF product family 
&lt;br&gt; Operating temperature: –55 °C to +125 °C 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;/b&gt; Especially for the suppression of signal lines in the high frequency range 
&lt;br&gt; For fast data lines: CPU, highspeed bus systems, HDD 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/WE-TMSB_74269200x_0201.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/WE-TMSB_74269200x_0201.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CBF_HF?"&gt;http://katalog.we-online.de/en/pbs/WE-CBF_HF?&lt;/a&gt;&lt;p&gt;

Updated on 2015-04-24&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_WB_HS" package="WE-CBF_HF_0603(W=2.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742861118">
<attribute name="WE-NUMBER" value="742861118/180Ω(Z@100MHz)"/>
</technology>
<technology name="_742861160">
<attribute name="WE-NUMBER" value="742861160/600Ω(Z@100MHz)"/>
</technology>
<technology name="_742861210">
<attribute name="WE-NUMBER" value="742861210/1000Ω(Z@100MHz)"/>
</technology>
<technology name="_742862160">
<attribute name="WE-NUMBER" value="742862160/600Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
<device name="_HC" package="WE-CBF_HF_0603(W=2.6)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_742863122">
<attribute name="WE-NUMBER" value="742863122/220Ω(Z@100MHz)"/>
</technology>
<technology name="_742863147">
<attribute name="WE-NUMBER" value="742863147/470Ω(Z@100MHz)"/>
</technology>
<technology name="_742863160">
<attribute name="WE-NUMBER" value="742863160/600Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CMB_NIZN_XS" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CMB NiZn Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Core material: Nickel-Zinc 
&lt;br&gt;
&lt;br&gt; High suppression rates of asymmetric interference at high and medium frequencies 
&lt;br&gt;
&lt;br&gt; Compact size 
&lt;br&gt;
&lt;br&gt; High interference stability against RF interference and burst signals 
&lt;br&gt;
&lt;br&gt; Noise suppression up to 300 MHz
&lt;br&gt;
&lt;br&gt;  Operating temperature: –40 ºC to +125 ºC 
&lt;br&gt;
&lt;br&gt; Custom designs on request 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power electronics 
&lt;br&gt;
&lt;br&gt; Power line in- and output filter 
&lt;br&gt;
&lt;br&gt; Optimized for burst signals
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndCMB_NiZn_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndCMB_NiZn_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CMB_NiZn"&gt;hthttp://katalog.we-online.de/en/pbs/WE-CMB_NiZn&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-30&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-CMB_NIZN_XS">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_744841210">
<attribute name="WE-NUMBER" value="744841210/100uH"/>
</technology>
<technology name="_744841247">
<attribute name="WE-NUMBER" value="744841247/47uH"/>
</technology>
<technology name="_744841330">
<attribute name="WE-NUMBER" value="744841330/30uH"/>
</technology>
<technology name="_744841414">
<attribute name="WE-NUMBER" value="744841414/14uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CNSW_0805" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CNSW SMD Common Mode Line Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High common mode noise suppression at high frequencies
&lt;br&gt;
&lt;br&gt; Small influence on high speed signals through winding symmetry
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC (Size 0805/1206/1812); –40 ºC to +105 ºC (Size 0603)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; USB 2.0 
&lt;br&gt;
&lt;br&gt; IEEE 1394 (Firewire) 
&lt;br&gt;
&lt;br&gt; LVDS 
&lt;br&gt;
&lt;br&gt; High Speed Data Lines 
&lt;br&gt;
&lt;br&gt;LAN 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndCNSW_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndCNSW_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CNSW"&gt;http://katalog.we-online.de/en/pbs/WE-CNSW&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-30&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-CNSW_0805">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_744231061">
<attribute name="WE-NUMBER" value="744231061/67Ω(Z@100MHz)"/>
</technology>
<technology name="_744231091">
<attribute name="WE-NUMBER" value="744231091/90Ω(Z@100MHz)"/>
</technology>
<technology name="_744231121">
<attribute name="WE-NUMBER" value="744231121/120Ω(Z@100MHz)"/>
</technology>
<technology name="_744231181">
<attribute name="WE-NUMBER" value="744231181/180Ω(Z@100MHz)"/>
</technology>
<technology name="_744231261">
<attribute name="WE-NUMBER" value="744231261/260Ω(Z@100MHz)"/>
</technology>
<technology name="_744231371">
<attribute name="WE-NUMBER" value="744231371/370Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CNSW_1206" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CNSW SMD Common Mode Line Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High common mode noise suppression at high frequencies
&lt;br&gt;
&lt;br&gt; Small influence on high speed signals through winding symmetry
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC (Size 0805/1206/1812); –40 ºC to +105 ºC (Size 0603)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; USB 2.0 
&lt;br&gt;
&lt;br&gt; IEEE 1394 (Firewire) 
&lt;br&gt;
&lt;br&gt; LVDS 
&lt;br&gt;
&lt;br&gt; High Speed Data Lines 
&lt;br&gt;
&lt;br&gt;LAN 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndCNSW_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndCNSW_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CNSW"&gt;http://katalog.we-online.de/en/pbs/WE-CNSW&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-30&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-CNSW_1206">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_744232090">
<attribute name="WE-NUMBER" value="744232090/90Ω(Z@100MHz)"/>
</technology>
<technology name="_744232101">
<attribute name="WE-NUMBER" value="744232101/6000Ω(Z@100MHz)"/>
</technology>
<technology name="_744232102">
<attribute name="WE-NUMBER" value="744232102/1000Ω(Z@100MHz)"/>
</technology>
<technology name="_744232161">
<attribute name="WE-NUMBER" value="744232161/160Ω(Z@100MHz)"/>
</technology>
<technology name="_744232222">
<attribute name="WE-NUMBER" value="744232222/2200Ω(Z@100MHz)"/>
</technology>
<technology name="_744232261">
<attribute name="WE-NUMBER" value="744232261/260Ω(Z@100MHz)"/>
</technology>
<technology name="_744232601">
<attribute name="WE-NUMBER" value="744232601/600Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CNSW_1812" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-CNSW SMD Common Mode Line Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High common mode noise suppression at high frequencies
&lt;br&gt;
&lt;br&gt; Small influence on high speed signals through winding symmetry
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC (Size 0805/1206/1812); –40 ºC to +105 ºC (Size 0603)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; USB 2.0 
&lt;br&gt;
&lt;br&gt; IEEE 1394 (Firewire) 
&lt;br&gt;
&lt;br&gt; LVDS 
&lt;br&gt;
&lt;br&gt; High Speed Data Lines 
&lt;br&gt;
&lt;br&gt;LAN 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndCNSW_pf2.jpg"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndCNSW_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CNSW"&gt;http://katalog.we-online.de/en/pbs/WE-CNSW&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-06-30&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-CNSW_1812">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_744235101">
<attribute name="WE-NUMBER" value="744235101/100uH"/>
</technology>
<technology name="_744235110">
<attribute name="WE-NUMBER" value="744235110/11uH"/>
</technology>
<technology name="_744235220">
<attribute name="WE-NUMBER" value="744235220/22uH"/>
</technology>
<technology name="_744235510">
<attribute name="WE-NUMBER" value="744235510/51uH"/>
</technology>
<technology name="_744235601">
<attribute name="WE-NUMBER" value="744235601/1uH"/>
</technology>
<technology name="_744235801">
<attribute name="WE-NUMBER" value="744235801/1,3uH"/>
</technology>
<technology name="_744235900">
<attribute name="WE-NUMBER" value="744235900/0,3uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-CNSW_HF_0504" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-CNSW HF SMD Common Mode Line Filter (High Frequency)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; urrent compensated data line filter
&lt;br&gt;
&lt;br&gt; High common mode noise suppression at high frequencies
&lt;br&gt;
&lt;br&gt; Suitable for high data rates
&lt;br&gt;
&lt;br&gt; Small influence on high speed signals through winding symmetry
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; USB 3.0 
&lt;br&gt;
&lt;br&gt;USB 2.0 
&lt;br&gt; 
&lt;br&gt; HDMI 
&lt;br&gt;
&lt;br&gt; LVDS
&lt;br&gt;
&lt;br&gt; High-Speed data lines 
&lt;br&gt;
&lt;br&gt; IEEE 1394 (Firewire)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndCNSWHF_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndCNSWHF_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-CNSW_HF"&gt;http://katalog.we-online.de/en/pbs/WE-CNSW_HF&lt;/a&gt;&lt;p&gt;
&lt;BR&gt;Created by Dan Xu 2014-6-10&lt;Br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-CNSW_HF_0504">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7442335600">
<attribute name="WE-NUMBER" value="7442335600/60Ω(Z@100MHz)"/>
</technology>
<technology name="_7442335900">
<attribute name="WE-NUMBER" value="7442335900/90Ω(Z@100MHz)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FC_UT20V" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-FC Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Closed rectangular ferrite core
&lt;BR&gt;
&lt;BR&gt; 2-section winding for excellent high frequency performance
&lt;BR&gt;
&lt;BR&gt; 1% stray inductance for symmetrical interference suppression
&lt;BR&gt;
&lt;BR&gt; Operating temperature: –25 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt; 
&lt;br&gt;&lt;/b&gt; Switch mode power supplies
&lt;BR&gt;
&lt;BR&gt; Electronic ballasts for lamps
&lt;BR&gt;
&lt;BR&gt; Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndFC_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/IndFC_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FC?"&gt;http://katalog.we-online.de/en/pbs/WE-FC?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-FC_UT">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7448640406">
<attribute name="WE-NUMBER" value="7448640406/0,82mH"/>
</technology>
<technology name="_7448640407">
<attribute name="WE-NUMBER" value="7448640407/1,2mH"/>
</technology>
<technology name="_7448640408">
<attribute name="WE-NUMBER" value="7448640408/1,8mH"/>
</technology>
<technology name="_7448640409">
<attribute name="WE-NUMBER" value="7448640409/2,2mH"/>
</technology>
<technology name="_7448640410">
<attribute name="WE-NUMBER" value="7448640410/2,7mH"/>
</technology>
<technology name="_7448640411">
<attribute name="WE-NUMBER" value="7448640411/3,3mH"/>
</technology>
<technology name="_7448640412">
<attribute name="WE-NUMBER" value="7448640412/3,9mH"/>
</technology>
<technology name="_7448640413">
<attribute name="WE-NUMBER" value="7448640413/5,6mH"/>
</technology>
<technology name="_7448640414">
<attribute name="WE-NUMBER" value="7448640414/6,8mH"/>
</technology>
<technology name="_7448640415">
<attribute name="WE-NUMBER" value="7448640415/10mH"/>
</technology>
<technology name="_7448640416">
<attribute name="WE-NUMBER" value="7448640416/18mH"/>
</technology>
<technology name="_7448640417">
<attribute name="WE-NUMBER" value="7448640417/22mH"/>
</technology>
<technology name="_7448640418">
<attribute name="WE-NUMBER" value="7448640418/33mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEX_EFD20" prefix="T" uservalue="yes">
<description>&lt;b&gt; WE-FLEX Flexible Transformer for DC/DC Converter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Transformer with 6 identical windings
&lt;BR&gt;
&lt;BR&gt; 4 sizes with 5 different lengths of air gap each
&lt;BR&gt;
&lt;BR&gt; Insulation test voltage 500 VAC
&lt;BR&gt;
&lt;BR&gt; Low leakage inductance
&lt;BR&gt;
&lt;BR&gt; Operating temperature: –40 ºC to +125 ºC
&lt;BR&gt;
&lt;BR&gt; By using different circuits more than 375 transformer solutions and about 125 choke solutions possible. Consequently, quick prototyping possibilities
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; All kind of switching regulators
&lt;br&gt;
&lt;br&gt;-Flyback converters
&lt;br&gt;-Forward converters
&lt;br&gt;-Push-pull converters
&lt;br&gt;-Step-up/step-down converters
&lt;br&gt;-SEPIC converter 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFlex_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtFlex_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FLEX?"&gt;http://katalog.we-online.de/en/pbs/WE-FLEX?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:3W_3"/>
</gates>
<devices>
<device name="" package="WE-FLEX_EFD20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="11"/>
<connect gate="G$1" pin="11" pad="2"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="9"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="10"/>
<connect gate="G$1" pin="9" pad="3"/>
</connects>
<technologies>
<technology name="_749196500"/>
<technology name="_749196501"/>
<technology name="_749196510"/>
<technology name="_749196511"/>
<technology name="_749196520"/>
<technology name="_749196521"/>
<technology name="_749196530"/>
<technology name="_749196531"/>
<technology name="_749196540"/>
<technology name="_749196541"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEX_ER11/5" prefix="T" uservalue="yes">
<description>&lt;b&gt; WE-FLEX Flexible Transformer for DC/DC Converter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Transformer with 6 identical windings
&lt;BR&gt;
&lt;BR&gt; 4 sizes with 5 different lengths of air gap each
&lt;BR&gt;
&lt;BR&gt; Insulation test voltage 500 VAC
&lt;BR&gt;
&lt;BR&gt; Low leakage inductance
&lt;BR&gt;
&lt;BR&gt; Operating temperature: –40 ºC to +125 ºC
&lt;BR&gt;
&lt;BR&gt; By using different circuits more than 375 transformer solutions and about 125 choke solutions possible. Consequently, quick prototyping possibilities
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; All kind of switching regulators
&lt;br&gt;
&lt;br&gt;-Flyback converters
&lt;br&gt;-Forward converters
&lt;br&gt;-Push-pull converters
&lt;br&gt;-Step-up/step-down converters
&lt;br&gt;-SEPIC converter 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFlex_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtFlex_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FLEX?"&gt;http://katalog.we-online.de/en/pbs/WE-FLEX?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:3W_3"/>
</gates>
<devices>
<device name="" package="WE-FLEX_ER11/5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="5"/>
<connect gate="G$1" pin="11" pad="2"/>
<connect gate="G$1" pin="12" pad="4"/>
<connect gate="G$1" pin="2" pad="10"/>
<connect gate="G$1" pin="3" pad="7"/>
<connect gate="G$1" pin="4" pad="11"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="12"/>
<connect gate="G$1" pin="7" pad="9"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="9" pad="3"/>
</connects>
<technologies>
<technology name="_749196101"/>
<technology name="_749196111"/>
<technology name="_749196121"/>
<technology name="_749196131"/>
<technology name="_749196141"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEX_ER14.5/6" prefix="T" uservalue="yes">
<description>&lt;b&gt; WE-FLEX Flexible Transformer for DC/DC Converter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Transformer with 6 identical windings
&lt;BR&gt;
&lt;BR&gt; 4 sizes with 5 different lengths of air gap each
&lt;BR&gt;
&lt;BR&gt; Insulation test voltage 500 VAC
&lt;BR&gt;
&lt;BR&gt; Low leakage inductance
&lt;BR&gt;
&lt;BR&gt; Operating temperature: –40 ºC to +125 ºC
&lt;BR&gt;
&lt;BR&gt; By using different circuits more than 375 transformer solutions and about 125 choke solutions possible. Consequently, quick prototyping possibilities
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; All kind of switching regulators
&lt;br&gt;
&lt;br&gt;-Flyback converters
&lt;br&gt;-Forward converters
&lt;br&gt;-Push-pull converters
&lt;br&gt;-Step-up/step-down converters
&lt;br&gt;-SEPIC converter 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFlex_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtFlex_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FLEX?"&gt;http://katalog.we-online.de/en/pbs/WE-FLEX?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:3W_3"/>
</gates>
<devices>
<device name="" package="WE-FLEX_ER14.5/6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="5"/>
<connect gate="G$1" pin="11" pad="2"/>
<connect gate="G$1" pin="12" pad="4"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="3" pad="9"/>
<connect gate="G$1" pin="4" pad="11"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="10"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="6"/>
<connect gate="G$1" pin="9" pad="3"/>
</connects>
<technologies>
<technology name="_749196201"/>
<technology name="_749196211"/>
<technology name="_749196221"/>
<technology name="_749196231"/>
<technology name="_749196241"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEX+_ETD34" prefix="T" uservalue="yes">
<description>&lt;b&gt; WE-FLEX+ Flexible Transformer for DC/DC Converter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Transformer with 6 identical windings 
&lt;br&gt;
&lt;br&gt; Power up to 300 W possible 
&lt;br&gt;
&lt;br&gt; Isolation voltage 500 VDC 
&lt;br&gt;
&lt;br&gt; Low leakage inductance 
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; All kind of switching regulators
&lt;br&gt; -Flyback converters
&lt;br&gt; -Forward converters
&lt;br&gt; -Push-pull converters
&lt;br&gt; -Step-up/step-down converters
&lt;br&gt; -SEPIC converter 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; 
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFlex_Plus_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtFlex_Plus_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FLEX_Plus?"&gt;http://katalog.we-online.de/en/pbs/WE-FLEX_Plus?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:3W_3"/>
</gates>
<devices>
<device name="" package="WE_FLEX+_ETD34">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="5"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="14"/>
<connect gate="G$1" pin="6" pad="2"/>
<connect gate="G$1" pin="7" pad="13"/>
<connect gate="G$1" pin="8" pad="9"/>
<connect gate="G$1" pin="9" pad="6"/>
</connects>
<technologies>
<technology name="_749197201"/>
<technology name="_749197211"/>
<technology name="_749197221"/>
<technology name="_749197231"/>
<technology name="_749197241"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEX+_ETD39" prefix="T" uservalue="yes">
<description>&lt;b&gt; WE-FLEX+ Flexible Transformer for DC/DC Converter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Transformer with 6 identical windings 
&lt;br&gt;
&lt;br&gt; Power up to 300 W possible 
&lt;br&gt;
&lt;br&gt; Isolation voltage 500 VDC 
&lt;br&gt;
&lt;br&gt; Low leakage inductance 
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; All kind of switching regulators
&lt;br&gt; -Flyback converters
&lt;br&gt; -Forward converters
&lt;br&gt; -Push-pull converters
&lt;br&gt; -Step-up/step-down converters
&lt;br&gt; -SEPIC converter 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; 
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtFlex_Plus_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtFlex_Plus_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FLEX_Plus?"&gt;http://katalog.we-online.de/en/pbs/WE-FLEX_Plus?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:3W_3"/>
</gates>
<devices>
<device name="" package="WE_FLEX+_ETD39">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="10" pad="12"/>
<connect gate="G$1" pin="11" pad="5"/>
<connect gate="G$1" pin="12" pad="13"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="5" pad="15"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="14"/>
<connect gate="G$1" pin="8" pad="11"/>
<connect gate="G$1" pin="9" pad="6"/>
</connects>
<technologies>
<technology name="_749197301"/>
<technology name="_749197311"/>
<technology name="_749197321"/>
<technology name="_749197331"/>
<technology name="_749197341"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-KI_0603A" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Wire Wound Ceramic Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; WE-KI series offers you an excellent Q factor and highest possible self resonant frequencies up to 12.5 GHz
&lt;br&gt;
&lt;br&gt; Inductance tolerances: 5% (2% on request)
&lt;br&gt;
&lt;br&gt; High thermal stability
&lt;br&gt;
&lt;br&gt; Operating temperature: –40°C to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Especially developed for high frequency applications
&lt;br&gt;
&lt;br&gt; RF transceiver/communications
&lt;br&gt;
&lt;br&gt; Bluetooth
&lt;br&gt;
&lt;br&gt; Wireless LAN
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-KI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-KI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-KI"&gt;http://katalog.we-online.de/en/pbs/WE-KI&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-KI_0603A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744761018A">
<attribute name="WE-NUMBER" value="744761018A/1,8nH"/>
</technology>
<technology name="_744761020A">
<attribute name="WE-NUMBER" value="744761020A/2nH"/>
</technology>
<technology name="_744761033A">
<attribute name="WE-NUMBER" value="744761033A/3,3nH"/>
</technology>
<technology name="_744761036A">
<attribute name="WE-NUMBER" value="744761036A/3,6nH"/>
</technology>
<technology name="_744761056A">
<attribute name="WE-NUMBER" value="744761056A/5,6nH"/>
</technology>
<technology name="_744761068A">
<attribute name="WE-NUMBER" value="744761068A/6,8nH"/>
</technology>
<technology name="_744761075A">
<attribute name="WE-NUMBER" value="744761075A/7,5nH"/>
</technology>
<technology name="_744761110A">
<attribute name="WE-NUMBER" value="744761110A/10nH"/>
</technology>
<technology name="_744761112A">
<attribute name="WE-NUMBER" value="744761112A/12nH"/>
</technology>
<technology name="_744761115A">
<attribute name="WE-NUMBER" value="744761115A/15nH"/>
</technology>
<technology name="_744761116A">
<attribute name="WE-NUMBER" value="744761116A/16nH"/>
</technology>
<technology name="_744761122A">
<attribute name="WE-NUMBER" value="744761122A/22nH"/>
</technology>
<technology name="_744761127A">
<attribute name="WE-NUMBER" value="744761127A/27nH"/>
</technology>
<technology name="_744761130A">
<attribute name="WE-NUMBER" value="744761130A/30nH"/>
</technology>
<technology name="_744761168A">
<attribute name="WE-NUMBER" value="744761168A/68nH"/>
</technology>
<technology name="_744761172A">
<attribute name="WE-NUMBER" value="744761172A/72nH"/>
</technology>
<technology name="_744761210A">
<attribute name="WE-NUMBER" value="744761210A/100nH"/>
</technology>
<technology name="_744761215A">
<attribute name="WE-NUMBER" value="744761215A/150nH"/>
</technology>
<technology name="_744761227A">
<attribute name="WE-NUMBER" value="744761227A/270nH"/>
</technology>
<technology name="_744761233A">
<attribute name="WE-NUMBER" value="744761233A/330nH"/>
</technology>
<technology name="_744761239A">
<attribute name="WE-NUMBER" value="744761239A/390nH"/>
</technology>
<technology name="_744761268A">
<attribute name="WE-NUMBER" value="744761268A/680nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-KI_0603C" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Wire Wound Ceramic Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; WE-KI series offers you an excellent Q factor and highest possible self resonant frequencies up to 12.5 GHz
&lt;br&gt;
&lt;br&gt; Inductance tolerances: 5% (2% on request)
&lt;br&gt;
&lt;br&gt; High thermal stability
&lt;br&gt;
&lt;br&gt; Operating temperature: –40°C to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Especially developed for high frequency applications
&lt;br&gt;
&lt;br&gt; RF transceiver/communications
&lt;br&gt;
&lt;br&gt; Bluetooth
&lt;br&gt;
&lt;br&gt; Wireless LAN
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-KI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-KI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-KI"&gt;http://katalog.we-online.de/en/pbs/WE-KI&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-KI_0603C">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744761016C">
<attribute name="WE-NUMBER" value="744761016C/1,6nH"/>
</technology>
<technology name="_744761039C">
<attribute name="WE-NUMBER" value="744761039C/3,9nH"/>
</technology>
<technology name="_744761043C">
<attribute name="WE-NUMBER" value="744761043C/4,3nH"/>
</technology>
<technology name="_744761047C">
<attribute name="WE-NUMBER" value="744761047C/4,7nH"/>
</technology>
<technology name="_744761051C">
<attribute name="WE-NUMBER" value="744761051C/5,1nH"/>
</technology>
<technology name="_744761056C">
<attribute name="WE-NUMBER" value="744761056C/5,6nH"/>
</technology>
<technology name="_744761075C">
<attribute name="WE-NUMBER" value="744761075C/7,5nH"/>
</technology>
<technology name="_744761082C">
<attribute name="WE-NUMBER" value="744761082C/8,2nH"/>
</technology>
<technology name="_744761087C">
<attribute name="WE-NUMBER" value="744761087C/8,7nH"/>
</technology>
<technology name="_744761111C">
<attribute name="WE-NUMBER" value="744761111C/11nH"/>
</technology>
<technology name="_744761112C">
<attribute name="WE-NUMBER" value="744761112C/12nH"/>
</technology>
<technology name="_744761118C">
<attribute name="WE-NUMBER" value="744761118C/18nH"/>
</technology>
<technology name="_744761120C">
<attribute name="WE-NUMBER" value="744761120C/20nH"/>
</technology>
<technology name="_744761124C">
<attribute name="WE-NUMBER" value="744761124C/24nH"/>
</technology>
<technology name="_744761127C">
<attribute name="WE-NUMBER" value="744761127C/27nH"/>
</technology>
<technology name="_744761133C">
<attribute name="WE-NUMBER" value="744761133C/33nH"/>
</technology>
<technology name="_744761136C">
<attribute name="WE-NUMBER" value="744761136C/36nH"/>
</technology>
<technology name="_744761139C">
<attribute name="WE-NUMBER" value="744761139C/39nH"/>
</technology>
<technology name="_744761147C">
<attribute name="WE-NUMBER" value="744761147C/47nH"/>
</technology>
<technology name="_744761151C">
<attribute name="WE-NUMBER" value="744761151C/51nH"/>
</technology>
<technology name="_744761156C">
<attribute name="WE-NUMBER" value="744761156C/56nH"/>
</technology>
<technology name="_744761168C">
<attribute name="WE-NUMBER" value="744761168C/68nH"/>
</technology>
<technology name="_744761182C">
<attribute name="WE-NUMBER" value="744761182C/82nH"/>
</technology>
<technology name="_744761212C">
<attribute name="WE-NUMBER" value="744761212C/120nH"/>
</technology>
<technology name="_744761215C">
<attribute name="WE-NUMBER" value="744761215C/150nH"/>
</technology>
<technology name="_744761218C">
<attribute name="WE-NUMBER" value="744761218C/180nH"/>
</technology>
<technology name="_744761222C">
<attribute name="WE-NUMBER" value="744761222C/220nH"/>
</technology>
<technology name="_744761227C">
<attribute name="WE-NUMBER" value="744761227C/270nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-KI_0805A" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Wire Wound Ceramic Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; WE-KI series offers you an excellent Q factor and highest possible self resonant frequencies up to 12.5 GHz
&lt;br&gt;
&lt;br&gt; Inductance tolerances: 5% (2% on request)
&lt;br&gt;
&lt;br&gt; High thermal stability
&lt;br&gt;
&lt;br&gt; Operating temperature: –40°C to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Especially developed for high frequency applications
&lt;br&gt;
&lt;br&gt; RF transceiver/communications
&lt;br&gt;
&lt;br&gt; Bluetooth
&lt;br&gt;
&lt;br&gt; Wireless LAN
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-KI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-KI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-KI"&gt;http://katalog.we-online.de/en/pbs/WE-KI&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-KI_0805A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744760022A">
<attribute name="WE-NUMBER" value="744760022A/2,2nH"/>
</technology>
<technology name="_744760027A">
<attribute name="WE-NUMBER" value="744760027A/2,7nH"/>
</technology>
<technology name="_744760033A">
<attribute name="WE-NUMBER" value="744760033A/3,3nH"/>
</technology>
<technology name="_744760039A">
<attribute name="WE-NUMBER" value="744760039A/3,9nH"/>
</technology>
<technology name="_744760047A">
<attribute name="WE-NUMBER" value="744760047A/4,7nH"/>
</technology>
<technology name="_744760082A">
<attribute name="WE-NUMBER" value="744760082A/8,2nH"/>
</technology>
<technology name="_744760110A">
<attribute name="WE-NUMBER" value="744760110A/10nH"/>
</technology>
<technology name="_744760122A">
<attribute name="WE-NUMBER" value="744760122A/22nH"/>
</technology>
<technology name="_744760127A">
<attribute name="WE-NUMBER" value="744760127A/27nH"/>
</technology>
<technology name="_744760133A">
<attribute name="WE-NUMBER" value="744760133A/33nH"/>
</technology>
<technology name="_744760136A">
<attribute name="WE-NUMBER" value="744760136A/36nH"/>
</technology>
<technology name="_744760147A">
<attribute name="WE-NUMBER" value="744760147A/47nH"/>
</technology>
<technology name="_744760156A">
<attribute name="WE-NUMBER" value="744760156A/56nH"/>
</technology>
<technology name="_744760182A">
<attribute name="WE-NUMBER" value="744760182A/82nH"/>
</technology>
<technology name="_744760218A">
<attribute name="WE-NUMBER" value="744760218A/180nH"/>
</technology>
<technology name="_744760222A">
<attribute name="WE-NUMBER" value="744760222A/220nH"/>
</technology>
<technology name="_744760233A">
<attribute name="WE-NUMBER" value="744760233A/330nH"/>
</technology>
<technology name="_744760239A">
<attribute name="WE-NUMBER" value="744760239A/390nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-KI_0805C" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Wire Wound Ceramic Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; WE-KI series offers you an excellent Q factor and highest possible self resonant frequencies up to 12.5 GHz
&lt;br&gt;
&lt;br&gt; Inductance tolerances: 5% (2% on request)
&lt;br&gt;
&lt;br&gt; High thermal stability
&lt;br&gt;
&lt;br&gt; Operating temperature: –40°C to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Especially developed for high frequency applications
&lt;br&gt;
&lt;br&gt; RF transceiver/communications
&lt;br&gt;
&lt;br&gt; Bluetooth
&lt;br&gt;
&lt;br&gt; Wireless LAN
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-KI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-KI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-KI"&gt;http://katalog.we-online.de/en/pbs/WE-KI&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-KI_0805C">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744760027C">
<attribute name="WE-NUMBER" value="744760027C/2,7nH"/>
</technology>
<technology name="_744760056C">
<attribute name="WE-NUMBER" value="744760056C/5,6nH"/>
</technology>
<technology name="_744760068C">
<attribute name="WE-NUMBER" value="744760068C/6,8nH"/>
</technology>
<technology name="_74476010C">
<attribute name="WE-NUMBER" value="74476010C/10nH"/>
</technology>
<technology name="_744760112C">
<attribute name="WE-NUMBER" value="744760112C/12nH"/>
</technology>
<technology name="_744760115C">
<attribute name="WE-NUMBER" value="744760115C/15nH"/>
</technology>
<technology name="_744760118C">
<attribute name="WE-NUMBER" value="744760118C/18nH"/>
</technology>
<technology name="_744760127C">
<attribute name="WE-NUMBER" value="744760127C/27nH"/>
</technology>
<technology name="_74476012C">
<attribute name="WE-NUMBER" value="74476012C/22nH"/>
</technology>
<technology name="_744760139C">
<attribute name="WE-NUMBER" value="744760139C/39nH"/>
</technology>
<technology name="_74476013C">
<attribute name="WE-NUMBER" value="74476013C/33nH"/>
</technology>
<technology name="_74476014C">
<attribute name="WE-NUMBER" value="74476014C/47nH"/>
</technology>
<technology name="_74476015C">
<attribute name="WE-NUMBER" value="74476015C/56nH"/>
</technology>
<technology name="_74476016C">
<attribute name="WE-NUMBER" value="74476016C/68nH"/>
</technology>
<technology name="_74476018C">
<attribute name="WE-NUMBER" value="74476018C/82nH"/>
</technology>
<technology name="_744760212C">
<attribute name="WE-NUMBER" value="744760212C/120nH"/>
</technology>
<technology name="_744760215C">
<attribute name="WE-NUMBER" value="744760215C/150nH"/>
</technology>
<technology name="_744760218C">
<attribute name="WE-NUMBER" value="744760218C/180nH"/>
</technology>
<technology name="_744760222C">
<attribute name="WE-NUMBER" value="744760222C/220nH"/>
</technology>
<technology name="_744760227C">
<attribute name="WE-NUMBER" value="744760227C/270nH"/>
</technology>
<technology name="_744760233C">
<attribute name="WE-NUMBER" value="744760233C/330nH"/>
</technology>
<technology name="_744760239C">
<attribute name="WE-NUMBER" value="744760239C/390nH"/>
</technology>
<technology name="_744760256C">
<attribute name="WE-NUMBER" value="744760256C/560nH"/>
</technology>
<technology name="_744760262C">
<attribute name="WE-NUMBER" value="744760262C/620nH"/>
</technology>
<technology name="_744760282C">
<attribute name="WE-NUMBER" value="744760282C/820nH"/>
</technology>
<technology name="_7447602C">
<attribute name="WE-NUMBER" value="7447602C/100nH"/>
</technology>
<technology name="_744760310C">
<attribute name="WE-NUMBER" value="744760310C/1000nH"/>
</technology>
<technology name="_744760312C">
<attribute name="WE-NUMBER" value="744760312C/1200nH"/>
</technology>
<technology name="_744760315C">
<attribute name="WE-NUMBER" value="744760315C/1500nH"/>
</technology>
<technology name="_74476032C">
<attribute name="WE-NUMBER" value="74476032C/470nH"/>
</technology>
<technology name="_7447604C">
<attribute name="WE-NUMBER" value="7447604C/680nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-KI_1008A" uservalue="yes">
<description>&lt;b&gt;SMD Wire Wound Ceramic Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; WE-KI series offers you an excellent Q factor and highest possible self resonant frequencies up to 12.5 GHz
&lt;br&gt;
&lt;br&gt; Inductance tolerances: 5% (2% on request)
&lt;br&gt;
&lt;br&gt; High thermal stability
&lt;br&gt;
&lt;br&gt; Operating temperature: –40°C to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Especially developed for high frequency applications
&lt;br&gt;
&lt;br&gt; RF transceiver/communications
&lt;br&gt;
&lt;br&gt; Bluetooth
&lt;br&gt;
&lt;br&gt; Wireless LAN
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-KI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-KI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-KI"&gt;http://katalog.we-online.de/en/pbs/WE-KI&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-KI_1008A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744762033A">
<attribute name="WE-NUMBER" value="744762033A/3,3nH"/>
</technology>
<technology name="_744762068A">
<attribute name="WE-NUMBER" value="744762068A/6,8nH"/>
</technology>
<technology name="_744762082A">
<attribute name="WE-NUMBER" value="744762082A/8,2nH"/>
</technology>
<technology name="_744762110A">
<attribute name="WE-NUMBER" value="744762110A/10nH"/>
</technology>
<technology name="_744762112A">
<attribute name="WE-NUMBER" value="744762112A/12nH"/>
</technology>
<technology name="_744762115A">
<attribute name="WE-NUMBER" value="744762115A/15nH"/>
</technology>
<technology name="_744762118A">
<attribute name="WE-NUMBER" value="744762118A/18nH"/>
</technology>
<technology name="_744762122A">
<attribute name="WE-NUMBER" value="744762122A/22nH"/>
</technology>
<technology name="_744762127A">
<attribute name="WE-NUMBER" value="744762127A/27nH"/>
</technology>
<technology name="_744762133A">
<attribute name="WE-NUMBER" value="744762133A/33nH"/>
</technology>
<technology name="_744762139A">
<attribute name="WE-NUMBER" value="744762139A/39nH"/>
</technology>
<technology name="_744762147A">
<attribute name="WE-NUMBER" value="744762147A/47nH"/>
</technology>
<technology name="_744762156A">
<attribute name="WE-NUMBER" value="744762156A/56nH"/>
</technology>
<technology name="_744762168A">
<attribute name="WE-NUMBER" value="744762168A/68nH"/>
</technology>
<technology name="_744762182A">
<attribute name="WE-NUMBER" value="744761182A/82nH"/>
</technology>
<technology name="_744762210A">
<attribute name="WE-NUMBER" value="744762210A/100nH"/>
</technology>
<technology name="_744762212A">
<attribute name="WE-NUMBER" value="744762212A/120nH"/>
</technology>
<technology name="_744762215A">
<attribute name="WE-NUMBER" value="744762215A/150nH"/>
</technology>
<technology name="_744762218A">
<attribute name="WE-NUMBER" value="744762218A/180nH"/>
</technology>
<technology name="_744762222A">
<attribute name="WE-NUMBER" value="744762222A/220nH"/>
</technology>
<technology name="_744762227A">
<attribute name="WE-NUMBER" value="744762227A/270nH"/>
</technology>
<technology name="_744762233A">
<attribute name="WE-NUMBER" value="744762233A/330nH"/>
</technology>
<technology name="_744762239A">
<attribute name="WE-NUMBER" value="744762239A/390nH"/>
</technology>
<technology name="_744762247A">
<attribute name="WE-NUMBER" value="744762247A/470nH"/>
</technology>
<technology name="_744762256A">
<attribute name="WE-NUMBER" value="744762256A/560nH"/>
</technology>
<technology name="_744762268A">
<attribute name="WE-NUMBER" value="744762268A/680nH"/>
</technology>
<technology name="_744762282A">
<attribute name="WE-NUMBER" value="744762282A/820nH"/>
</technology>
<technology name="_744762310A">
<attribute name="WE-NUMBER" value="744762310A/1000nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-KIHC_0603" prefix="L" uservalue="yes">
<description>&lt;b&gt;Wire Wound Chip Ceramic Inductor WE-KIHC&lt;/b&gt;&lt;br&gt;

&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt; Inductance values ​​from 1 nH up to 51 nH
&lt;br&gt;High quality factor Q
&lt;br&gt;High self-resonant frequency
&lt;br&gt;High currents up to 2.3 A
&lt;br&gt;2% Inductance tolerance
&lt;br&gt;Operating temperature: -40 ° C to +125 ° C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt; 
&lt;br&gt;Especially for RF application
&lt;br&gt;Ideal for high current applications
&lt;br&gt;Wideband filter
&lt;br&gt;Decoupling
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-ki%20hc_keramik_smd_induktivitaet.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-ki%20hc_keramik_smd_induktivitaet.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-KIHC"&gt;http://katalog.we-online.de/en/pbs/WE-KIHC&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2016 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-KIHC_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744917018">
<attribute name="WE-NUMBER" value="744917018/1,8nH"/>
</technology>
<technology name="_744917022">
<attribute name="WE-NUMBER" value="744917022/2,2nH"/>
</technology>
<technology name="_744917033">
<attribute name="WE-NUMBER" value="744917033/3,3nH"/>
</technology>
<technology name="_744917036">
<attribute name="WE-NUMBER" value="744917036/3,6nH"/>
</technology>
<technology name="_744917039">
<attribute name="WE-NUMBER" value="744917039/3,9nH"/>
</technology>
<technology name="_744917043">
<attribute name="WE-NUMBER" value="744917043/4,3nH"/>
</technology>
<technology name="_744917051">
<attribute name="WE-NUMBER" value="744917051/5,1nH"/>
</technology>
<technology name="_744917056">
<attribute name="WE-NUMBER" value="744917056/5,6nH"/>
</technology>
<technology name="_744917060">
<attribute name="WE-NUMBER" value="744917060/6nH"/>
</technology>
<technology name="_744917068">
<attribute name="WE-NUMBER" value="744917068/6,8nH"/>
</technology>
<technology name="_744917072">
<attribute name="WE-NUMBER" value="744917072/7,2nH"/>
</technology>
<technology name="_744917075">
<attribute name="WE-NUMBER" value="744917075/7,5nH"/>
</technology>
<technology name="_744917082">
<attribute name="WE-NUMBER" value="744917082/8,2nH"/>
</technology>
<technology name="_744917087">
<attribute name="WE-NUMBER" value="744917087/8,7nH"/>
</technology>
<technology name="_744917091">
<attribute name="WE-NUMBER" value="744917091/9,1nH"/>
</technology>
<technology name="_744917095">
<attribute name="WE-NUMBER" value="744917095/9,5nH"/>
</technology>
<technology name="_744917110">
<attribute name="WE-NUMBER" value="744917110/10nH"/>
</technology>
<technology name="_744917111">
<attribute name="WE-NUMBER" value="744917111/11nH"/>
</technology>
<technology name="_744917112">
<attribute name="WE-NUMBER" value="744917112/12nH"/>
</technology>
<technology name="_744917115">
<attribute name="WE-NUMBER" value="744917115/15nH"/>
</technology>
<technology name="_744917116">
<attribute name="WE-NUMBER" value="744917116/16nH"/>
</technology>
<technology name="_744917118">
<attribute name="WE-NUMBER" value="744917118/18nH"/>
</technology>
<technology name="_744917122">
<attribute name="WE-NUMBER" value="744917122/22nH"/>
</technology>
<technology name="_744917123">
<attribute name="WE-NUMBER" value="744917123/23nH"/>
</technology>
<technology name="_744917124">
<attribute name="WE-NUMBER" value="744917124/24nH"/>
</technology>
<technology name="_744917127">
<attribute name="WE-NUMBER" value="744917127/27nH"/>
</technology>
<technology name="_744917130">
<attribute name="WE-NUMBER" value="744917130/30nH"/>
</technology>
<technology name="_744917133">
<attribute name="WE-NUMBER" value="744917133/33nH"/>
</technology>
<technology name="_744917136">
<attribute name="WE-NUMBER" value="744917136/36nH"/>
</technology>
<technology name="_744917139">
<attribute name="WE-NUMBER" value="744917139/39nH"/>
</technology>
<technology name="_744917143">
<attribute name="WE-NUMBER" value="744917143/43nH"/>
</technology>
<technology name="_744917147">
<attribute name="WE-NUMBER" value="744917147/47nH"/>
</technology>
<technology name="_744917151">
<attribute name="WE-NUMBER" value="744917151/51nH"/>
</technology>
<technology name="_744917156">
<attribute name="WE-NUMBER" value="744917156/56nH"/>
</technology>
<technology name="_744917168">
<attribute name="WE-NUMBER" value="744917168/68nH"/>
</technology>
<technology name="_744917172">
<attribute name="WE-NUMBER" value="744917172/72nH"/>
</technology>
<technology name="_744917175">
<attribute name="WE-NUMBER" value="744917175/75nH"/>
</technology>
<technology name="_744917182">
<attribute name="WE-NUMBER" value="744917182/82nH"/>
</technology>
<technology name="_744917191">
<attribute name="WE-NUMBER" value="744917191/91nH"/>
</technology>
<technology name="_744917210">
<attribute name="WE-NUMBER" value="744917210/100nH"/>
</technology>
<technology name="_744917211">
<attribute name="WE-NUMBER" value="744917211/110nH"/>
</technology>
<technology name="_744917212">
<attribute name="WE-NUMBER" value="744917212/120nH"/>
</technology>
<technology name="_744917215">
<attribute name="WE-NUMBER" value="744917215/150nH"/>
</technology>
<technology name="_744917218">
<attribute name="WE-NUMBER" value="744917218/180nH"/>
</technology>
<technology name="_744917220">
<attribute name="WE-NUMBER" value="744917220/200nH"/>
</technology>
<technology name="_744917221">
<attribute name="WE-NUMBER" value="744917221/210nH"/>
</technology>
<technology name="_744917222">
<attribute name="WE-NUMBER" value="744917222/220nH"/>
</technology>
<technology name="_744917225">
<attribute name="WE-NUMBER" value="744917225/250nH"/>
</technology>
<technology name="_744917227">
<attribute name="WE-NUMBER" value="744917227/270nH"/>
</technology>
<technology name="_744917230">
<attribute name="WE-NUMBER" value="744917230/300nH"/>
</technology>
<technology name="_744917233">
<attribute name="WE-NUMBER" value="744917233/330nH"/>
</technology>
<technology name="_744917236">
<attribute name="WE-NUMBER" value="744917236/360nH"/>
</technology>
<technology name="_744917239">
<attribute name="WE-NUMBER" value="744917239/390nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_749020011A" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN LAN Transformer 10/100 Base T&lt;/b&gt;&lt;p&gt;
- Compliant with IEEE 802.3, IEEE 802.3af and IEEE 802.3at standards&lt;br&gt;
- SMT&lt;p&gt;

-- Ethernet&lt;br&gt;
-- Power over Ethernet&lt;br&gt;
-- 1 Gigabit Ethernet&lt;br&gt;
-- Compliant with most IC's for ethernet applications like Intel, AMD, Globespan and Realtek&lt;br&gt;
-- Hub, Router, Switch
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LAN/749020011A"&gt;http://katalog.we-online.de/en/pbs/WE-LAN/749020011A&lt;/a&gt;&lt;p&gt;

2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="749020010A"/>
</gates>
<devices>
<device name="" package="74902001XA">
<connects>
<connect gate="G$1" pin="MCT1" pad="24"/>
<connect gate="G$1" pin="MCT2" pad="21"/>
<connect gate="G$1" pin="MCT3" pad="18"/>
<connect gate="G$1" pin="MCT4" pad="15"/>
<connect gate="G$1" pin="MX1+" pad="23"/>
<connect gate="G$1" pin="MX1-" pad="22"/>
<connect gate="G$1" pin="MX2+" pad="20"/>
<connect gate="G$1" pin="MX2-" pad="19"/>
<connect gate="G$1" pin="MX3+" pad="17"/>
<connect gate="G$1" pin="MX3-" pad="16"/>
<connect gate="G$1" pin="MX4+" pad="14"/>
<connect gate="G$1" pin="MX4-" pad="13"/>
<connect gate="G$1" pin="TCT1" pad="1"/>
<connect gate="G$1" pin="TCT2" pad="4"/>
<connect gate="G$1" pin="TCT3" pad="7"/>
<connect gate="G$1" pin="TCT4" pad="5"/>
<connect gate="G$1" pin="TD1+" pad="2"/>
<connect gate="G$1" pin="TD1-" pad="3"/>
<connect gate="G$1" pin="TD2+" pad="6"/>
<connect gate="G$1" pin="TD2-" pad="8"/>
<connect gate="G$1" pin="TD3+" pad="9"/>
<connect gate="G$1" pin="TD3-" pad="10"/>
<connect gate="G$1" pin="TD4+" pad="11"/>
<connect gate="G$1" pin="TD4-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_MV" prefix="L" uservalue="yes">
<description>&lt;b&gt;Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Easy assembly due to 4 pole housing
&lt;br&gt;
&lt;br&gt; Compact, small size
&lt;br&gt;
&lt;br&gt; 4 soldering pins for perfect mechanical decoupling
&lt;br&gt;
&lt;br&gt; Toroidal core choke with sector winding
&lt;br&gt;
&lt;br&gt; High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Custom designs on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;
&lt;br&gt; Power electronics
&lt;br&gt;
&lt;br&gt; SMPS
&lt;br&gt;
&lt;br&gt; Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LF?"&gt;http://katalog.we-online.de/en/pbs/WE-LF?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-LF_622/MV">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7446220047">
<attribute name="WE-NUMBER" value="7446220047/47mH"/>
</technology>
<technology name="_7446221010">
<attribute name="WE-NUMBER" value="7446221010/10mH"/>
</technology>
<technology name="_7446221012">
<attribute name="WE-NUMBER" value="7446221012/12mH"/>
</technology>
<technology name="_7446221027">
<attribute name="WE-NUMBER" value="7446221027/27mH"/>
</technology>
<technology name="_7446222002">
<attribute name="WE-NUMBER" value="7446222002/2,2mH"/>
</technology>
<technology name="_7446222003">
<attribute name="WE-NUMBER" value="7446222003/3,3mH"/>
</technology>
<technology name="_7446222004">
<attribute name="WE-NUMBER" value="7446222004/4,2mH"/>
</technology>
<technology name="_7446222007">
<attribute name="WE-NUMBER" value="7446222007/6,8mH"/>
</technology>
<technology name="_7446223001">
<attribute name="WE-NUMBER" value="7446223001/1mH"/>
</technology>
<technology name="_74462250007">
<attribute name="WE-NUMBER" value="74462250007/0,7mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_LV" prefix="L" uservalue="yes">
<description>&lt;b&gt;Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Easy assembly due to 4 pole housing
&lt;br&gt;
&lt;br&gt; Compact, small size
&lt;br&gt;
&lt;br&gt; 4 soldering pins for perfect mechanical decoupling
&lt;br&gt;
&lt;br&gt; Toroidal core choke with sector winding
&lt;br&gt;
&lt;br&gt; High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Custom designs on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;
&lt;br&gt; Power electronics
&lt;br&gt;
&lt;br&gt; SMPS
&lt;br&gt;
&lt;br&gt; Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LF?"&gt;http://katalog.we-online.de/en/pbs/WE-LF?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-LF_632/LV">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7446321027">
<attribute name="WE-NUMBER" value="7446321027/27mH"/>
</technology>
<technology name="_7446321033">
<attribute name="WE-NUMBER" value="7446321033/33mH"/>
</technology>
<technology name="_7446321050">
<attribute name="WE-NUMBER" value="7446321050/50mH"/>
</technology>
<technology name="_7446322007">
<attribute name="WE-NUMBER" value="7446322007/6,8mH"/>
</technology>
<technology name="_7446322010">
<attribute name="WE-NUMBER" value="7446322010/10mH"/>
</technology>
<technology name="_7446323003">
<attribute name="WE-NUMBER" value="7446323003/2,7mH"/>
</technology>
<technology name="_7446323004">
<attribute name="WE-NUMBER" value="7446323004/4mH"/>
</technology>
<technology name="_7446326002">
<attribute name="WE-NUMBER" value="7446326002/1,8mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_XV" prefix="L" uservalue="yes">
<description>&lt;b&gt;Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Easy assembly due to 4 pole housing
&lt;br&gt;
&lt;br&gt; Compact, small size
&lt;br&gt;
&lt;br&gt; 4 soldering pins for perfect mechanical decoupling
&lt;br&gt;
&lt;br&gt; Toroidal core choke with sector winding
&lt;br&gt;
&lt;br&gt; High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Custom designs on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;
&lt;br&gt; Power electronics
&lt;br&gt;
&lt;br&gt; SMPS
&lt;br&gt;
&lt;br&gt; Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LF?"&gt;http://katalog.we-online.de/en/pbs/WE-LF?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-LF_642/XV">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7446422007">
<attribute name="WE-NUMBER" value="7446422007/6,8mH"/>
</technology>
<technology name="_7446424002">
<attribute name="WE-NUMBER" value="7446424002/2,2mH"/>
</technology>
<technology name="_7446424003">
<attribute name="WE-NUMBER" value="7446424003/3,3mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_SH" prefix="L" uservalue="yes">
<description>&lt;b&gt;Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Easy assembly due to 4 pole housing
&lt;br&gt;
&lt;br&gt; Compact, small size
&lt;br&gt;
&lt;br&gt; 4 soldering pins for perfect mechanical decoupling
&lt;br&gt;
&lt;br&gt; Toroidal core choke with sector winding
&lt;br&gt;
&lt;br&gt; High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Custom designs on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;
&lt;br&gt; Power electronics
&lt;br&gt;
&lt;br&gt; SMPS
&lt;br&gt;
&lt;br&gt; Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LF?"&gt;http://katalog.we-online.de/en/pbs/WE-LF?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-LF_662/SH">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7446620015">
<attribute name="WE-NUMBER" value="7446620015/15mH"/>
</technology>
<technology name="_7446620027">
<attribute name="WE-NUMBER" value="7446620027/27mH"/>
</technology>
<technology name="_7446620039">
<attribute name="WE-NUMBER" value="7446620039/39mH"/>
</technology>
<technology name="_7446621007">
<attribute name="WE-NUMBER" value="7446621007/6,8mH"/>
</technology>
<technology name="_7446621010">
<attribute name="WE-NUMBER" value="7446621010/10mH"/>
</technology>
<technology name="_7446622001">
<attribute name="WE-NUMBER" value="7446622001/1mH"/>
</technology>
<technology name="_7446622002">
<attribute name="WE-NUMBER" value="7446622002/2,2mH"/>
</technology>
<technology name="_7446622003">
<attribute name="WE-NUMBER" value="7446622003/3,3mH"/>
</technology>
<technology name="_74466240007">
<attribute name="WE-NUMBER" value="74466240007/0,7mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_MH" prefix="L" uservalue="yes">
<description>&lt;b&gt;Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Easy assembly due to 4 pole housing
&lt;br&gt;
&lt;br&gt; Compact, small size
&lt;br&gt;
&lt;br&gt; 4 soldering pins for perfect mechanical decoupling
&lt;br&gt;
&lt;br&gt; Toroidal core choke with sector winding
&lt;br&gt;
&lt;br&gt; High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Custom designs on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;
&lt;br&gt; Power electronics
&lt;br&gt;
&lt;br&gt; SMPS
&lt;br&gt;
&lt;br&gt; Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LF?"&gt;http://katalog.we-online.de/en/pbs/WE-LF?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-LF_672/MH">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7446720047">
<attribute name="WE-NUMBER" value="7446720047/47mH"/>
</technology>
<technology name="_7446721010">
<attribute name="WE-NUMBER" value="7446721010/10mH"/>
</technology>
<technology name="_7446721027">
<attribute name="WE-NUMBER" value="7446721027/27mH"/>
</technology>
<technology name="_7446722002">
<attribute name="WE-NUMBER" value="7446722002/2,2mH"/>
</technology>
<technology name="_7446722004">
<attribute name="WE-NUMBER" value="7446722004/4,2mH"/>
</technology>
<technology name="_7446722007">
<attribute name="WE-NUMBER" value="7446722007/6,8mH"/>
</technology>
<technology name="_7446723001">
<attribute name="WE-NUMBER" value="7446723001/1,2mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_LH" prefix="L" uservalue="yes">
<description>&lt;b&gt;Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Easy assembly due to 4 pole housing
&lt;br&gt;
&lt;br&gt; Compact, small size
&lt;br&gt;
&lt;br&gt; 4 soldering pins for perfect mechanical decoupling
&lt;br&gt;
&lt;br&gt; Toroidal core choke with sector winding
&lt;br&gt;
&lt;br&gt; High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Custom designs on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;
&lt;br&gt; Power electronics
&lt;br&gt;
&lt;br&gt; SMPS
&lt;br&gt;
&lt;br&gt; Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LF?"&gt;http://katalog.we-online.de/en/pbs/WE-LF?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-LF_682/LH">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7446821027">
<attribute name="WE-NUMBER" value="7446821027/27mH"/>
</technology>
<technology name="_7446822006">
<attribute name="WE-NUMBER" value="7446822006/5,6mH"/>
</technology>
<technology name="_7446823003">
<attribute name="WE-NUMBER" value="7446823003/2,7mH"/>
</technology>
<technology name="_7446823006">
<attribute name="WE-NUMBER" value="7446823006/5,6mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_XH" prefix="L" uservalue="yes">
<description>&lt;b&gt;Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Easy assembly due to 4 pole housing
&lt;br&gt;
&lt;br&gt; Compact, small size
&lt;br&gt;
&lt;br&gt; 4 soldering pins for perfect mechanical decoupling
&lt;br&gt;
&lt;br&gt; Toroidal core choke with sector winding
&lt;br&gt;
&lt;br&gt; High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;
&lt;br&gt; Low stray field
&lt;br&gt;
&lt;br&gt; Operating temperature: –25 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Custom designs on request
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;
&lt;br&gt; Power electronics
&lt;br&gt;
&lt;br&gt; SMPS
&lt;br&gt;
&lt;br&gt; Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/we_lf_stroko_netzdrossel.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LF?"&gt;http://katalog.we-online.de/en/pbs/WE-LF?&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H_1"/>
</gates>
<devices>
<device name="" package="WE-LF_692/XH">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7446921027">
<attribute name="WE-NUMBER" value="7446921027/27mH"/>
</technology>
<technology name="_7446923010">
<attribute name="WE-NUMBER" value="7446923010/10mH"/>
</technology>
<technology name="_7446924003">
<attribute name="WE-NUMBER" value="7446924003/3,3mH"/>
</technology>
<technology name="_7446926002">
<attribute name="WE-NUMBER" value="7446926002/1,8mH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LLCR_ETD34" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LLCR Resonant Converter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Transformer for high efficiency power supply
&lt;br&gt;
&lt;br&gt; Input voltage 360–400 VDC
&lt;br&gt;
&lt;br&gt; Switching frequency 70–120 kHz
&lt;br&gt;
&lt;br&gt; Output power 150 W–250 W
&lt;br&gt;
&lt;br&gt; Testing voltage 4 kVAC
&lt;br&gt;
&lt;br&gt; Litz wire for low eddy current losses
&lt;br&gt;
&lt;br&gt; Defined leakage inductance for use without additional resonant inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power supplies for PC, netbook, LED lighting and other power supplies
&lt;br&gt;
&lt;br&gt; High efficient resonant converters
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtLLCR_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtLLCR_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LLCR?"&gt;http://katalog.we-online.de/en/pbs/WE-LLCR?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-LLCR_ETD34">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="8"/>
<connect gate="G$1" pin="3" pad="10"/>
<connect gate="G$1" pin="4" pad="9"/>
<connect gate="G$1" pin="5" pad="11"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="5"/>
<connect gate="G$1" pin="8" pad="2"/>
</connects>
<technologies>
<technology name="_760895431"/>
<technology name="_760895441"/>
<technology name="_760895451"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LLCR_ETD44" prefix="T" uservalue="yes">
<description>&lt;b&gt;&lt;br&gt;WE-LLCR Resonant Converter
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Transformer for high efficiency power supply
&lt;br&gt;
&lt;br&gt; Input voltage 360–400 VDC
&lt;br&gt;
&lt;br&gt; Switching frequency 70–120 kHz
&lt;br&gt;
&lt;br&gt; Output power 150 W–250 W
&lt;br&gt;
&lt;br&gt; Testing voltage 4 kVAC
&lt;br&gt;
&lt;br&gt; Litz wire for low eddy current losses
&lt;br&gt;
&lt;br&gt; Defined leakage inductance for use without additional resonant inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power supplies for PC, netbook, LED lighting and other power supplies
&lt;br&gt;
&lt;br&gt; High efficient resonant converters
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtLLCR_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtLLCR_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LLCR?"&gt;http://katalog.we-online.de/en/pbs/WE-LLCR?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:2W"/>
</gates>
<devices>
<device name="" package="WE-LLCR_ETD44">
<connects>
<connect gate="G$1" pin="1" pad="12"/>
<connect gate="G$1" pin="2" pad="1 2"/>
<connect gate="G$1" pin="3" pad="5 6"/>
<connect gate="G$1" pin="4" pad="3 4"/>
<connect gate="G$1" pin="5" pad="7 8"/>
<connect gate="G$1" pin="6" pad="14"/>
<connect gate="G$1" pin="7" pad="15"/>
<connect gate="G$1" pin="8" pad="10"/>
</connects>
<technologies>
<technology name="_760895731"/>
<technology name="_760895741"/>
<technology name="_760895751"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_2508" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-MAIA SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;

&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;Hight current capability and handles hight transient current spikes
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range:-40°C up to 125°C
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;DC/DC-converter for high current power supplies  
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices 
&lt;br&gt;Wireless communication devices
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAIA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndMAIA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAIA/"&gt;http://katalog.we-online.de/en/pbs/WE-MAIA/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-04
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAIA_2508">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383220047">
<attribute name="WE-NUMBER" value="784383220047/0,47uH"/>
</technology>
<technology name="_78438322010">
<attribute name="WE-NUMBER" value="78438322010/1uH"/>
</technology>
<technology name="_78438322022">
<attribute name="WE-NUMBER" value="78438322022/2,2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_2510" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-MAIA SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;

&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;Hight current capability and handles hight transient current spikes
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range:-40°C up to 125°C
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;DC/DC-converter for high current power supplies  
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices 
&lt;br&gt;Wireless communication devices
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAIA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndMAIA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAIA/"&gt;http://katalog.we-online.de/en/pbs/WE-MAIA/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-04
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAIA_2510">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383230033">
<attribute name="WE-NUMBER" value="784383230033/0,33uH"/>
</technology>
<technology name="_784383230047">
<attribute name="WE-NUMBER" value="784383230047/0,47uH"/>
</technology>
<technology name="_784383230068">
<attribute name="WE-NUMBER" value="784383230068/0,68uH"/>
</technology>
<technology name="_784383230082">
<attribute name="WE-NUMBER" value="784383230082/0,82uH"/>
</technology>
<technology name="_78438323010">
<attribute name="WE-NUMBER" value="78438323010/1uH"/>
</technology>
<technology name="_78438323012">
<attribute name="WE-NUMBER" value="78438323012/1,2uH"/>
</technology>
<technology name="_78438323015">
<attribute name="WE-NUMBER" value="78438323015/1,5uH"/>
</technology>
<technology name="_78438323022">
<attribute name="WE-NUMBER" value="78438323022/2,2uH"/>
</technology>
<technology name="_78438323033">
<attribute name="WE-NUMBER" value="78438323033/3,3uH"/>
</technology>
<technology name="_78438323047">
<attribute name="WE-NUMBER" value="78438323047/4,7uH"/>
</technology>
<technology name="_78438323068">
<attribute name="WE-NUMBER" value="78438323068/6,8uH"/>
</technology>
<technology name="_78438323082">
<attribute name="WE-NUMBER" value="78438323082/8,2uH"/>
</technology>
<technology name="_78438323100">
<attribute name="WE-NUMBER" value="78438323100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_2512" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-MAIA SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;

&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;Hight current capability and handles hight transient current spikes
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range:-40°C up to 125°C
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;DC/DC-converter for high current power supplies  
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices 
&lt;br&gt;Wireless communication devices
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAIA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndMAIA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAIA/"&gt;http://katalog.we-online.de/en/pbs/WE-MAIA/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-04
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAIA_2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383240047">
<attribute name="WE-NUMBER" value="784383240047/0,47uH"/>
</technology>
<technology name="_784383240056">
<attribute name="WE-NUMBER" value="784383240056/0,56uH"/>
</technology>
<technology name="_784383240068">
<attribute name="WE-NUMBER" value="784383240068/6,8uH"/>
</technology>
<technology name="_78438324010">
<attribute name="WE-NUMBER" value="78438324010/1uH"/>
</technology>
<technology name="_78438324012">
<attribute name="WE-NUMBER" value="78438324012/1,2uH"/>
</technology>
<technology name="_78438324015">
<attribute name="WE-NUMBER" value="78438324015/1,5uH"/>
</technology>
<technology name="_78438324022">
<attribute name="WE-NUMBER" value="78438324022/2,2uH"/>
</technology>
<technology name="_78438324033">
<attribute name="WE-NUMBER" value="78438324033/3,3uH"/>
</technology>
<technology name="_78438324047">
<attribute name="WE-NUMBER" value="78438324047/4,7uH"/>
</technology>
<technology name="_78438324056">
<attribute name="WE-NUMBER" value="78438324056/0,56uH"/>
</technology>
<technology name="_78438324068">
<attribute name="WE-NUMBER" value="78438324068/0,68uH"/>
</technology>
<technology name="_78438324082">
<attribute name="WE-NUMBER" value="78438324082/8,2uH"/>
</technology>
<technology name="_78438324100">
<attribute name="WE-NUMBER" value="8438324100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_3010" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-MAIA SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;

&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;Hight current capability and handles hight transient current spikes
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range:-40°C up to 125°C
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;DC/DC-converter for high current power supplies  
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices 
&lt;br&gt;Wireless communication devices
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAIA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndMAIA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAIA/"&gt;http://katalog.we-online.de/en/pbs/WE-MAIA/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-04
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAIA_3010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78438333022">
<attribute name="WE-NUMBER" value="78438333022/2,2uH"/>
</technology>
<technology name="_78438333033">
<attribute name="WE-NUMBER" value="78438333033/3,3uH"/>
</technology>
<technology name="_78438333047">
<attribute name="WE-NUMBER" value="78438333047/4,7uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_3012" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-MAIA SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;

&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;Hight current capability and handles hight transient current spikes
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range:-40°C up to 125°C
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;DC/DC-converter for high current power supplies  
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices 
&lt;br&gt;Wireless communication devices
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAIA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndMAIA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAIA/"&gt;http://katalog.we-online.de/en/pbs/WE-MAIA/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-04
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAIA_3012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383340033">
<attribute name="WE-NUMBER" value="784383340033/0,33uH"/>
</technology>
<technology name="_784383340047">
<attribute name="WE-NUMBER" value="784383340047/0,47uH"/>
</technology>
<technology name="_784383340056">
<attribute name="WE-NUMBER" value="784383340056/0,56uH"/>
</technology>
<technology name="_784383340068">
<attribute name="WE-NUMBER" value="784383340068/0,68uH"/>
</technology>
<technology name="_78438334010">
<attribute name="WE-NUMBER" value="78438334010/1uH"/>
</technology>
<technology name="_78438334012">
<attribute name="WE-NUMBER" value="78438334012/1,2uH"/>
</technology>
<technology name="_78438334015">
<attribute name="WE-NUMBER" value="78438334015/1,5uH"/>
</technology>
<technology name="_78438334022">
<attribute name="WE-NUMBER" value="78438334022/2,2uH"/>
</technology>
<technology name="_78438334033">
<attribute name="WE-NUMBER" value="78438334033/3,3uH"/>
</technology>
<technology name="_78438334047">
<attribute name="WE-NUMBER" value="7843834047/4,7uH"/>
</technology>
<technology name="_78438334056">
<attribute name="WE-NUMBER" value="78438334056/5,6uH"/>
</technology>
<technology name="_78438334068">
<attribute name="WE-NUMBER" value="78438334068/6,8uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_3015" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-MAIA SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;

&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;Hight current capability and handles hight transient current spikes
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range:-40°C up to 125°C
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;DC/DC-converter for high current power supplies  
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices 
&lt;br&gt;Wireless communication devices
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAIA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndMAIA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAIA/"&gt;http://katalog.we-online.de/en/pbs/WE-MAIA/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-04
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAIA_3015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383350047">
<attribute name="WE-NUMBER" value="784383350047/0,47uH"/>
</technology>
<technology name="_784383350068">
<attribute name="WE-NUMBER" value="784383350068/0,68uH"/>
</technology>
<technology name="_784383350082">
<attribute name="WE-NUMBER" value="784383350082/0,82uH"/>
</technology>
<technology name="_78438335010">
<attribute name="WE-NUMBER" value="78438335010/1uH"/>
</technology>
<technology name="_78438335022">
<attribute name="WE-NUMBER" value="78438335022/2,2uH"/>
</technology>
<technology name="_78438335033">
<attribute name="WE-NUMBER" value="78438335033/3,3uH"/>
</technology>
<technology name="_78438335047">
<attribute name="WE-NUMBER" value="78438335047/4,7uH"/>
</technology>
<technology name="_78438335068">
<attribute name="WE-NUMBER" value="78438335068/6,8uH"/>
</technology>
<technology name="_78438335100">
<attribute name="WE-NUMBER" value="78438335100/10uH"/>
</technology>
<technology name="_78438335150">
<attribute name="WE-NUMBER" value="78438335150/15uH"/>
</technology>
<technology name="_78438335220">
<attribute name="WE-NUMBER" value="78438335220/22uH"/>
</technology>
<technology name="_78438335330">
<attribute name="WE-NUMBER" value="78438335330/33uH"/>
</technology>
<technology name="_78438335470">
<attribute name="WE-NUMBER" value="78438335470/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_3020" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-MAIA SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;

&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;Hight current capability and handles hight transient current spikes
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range:-40°C up to 125°C
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;DC/DC-converter for high current power supplies  
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices 
&lt;br&gt;Wireless communication devices
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAIA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndMAIA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAIA/"&gt;http://katalog.we-online.de/en/pbs/WE-MAIA/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-04
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAIA_3020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383360033">
<attribute name="WE-NUMBER" value="784383360033/0,33uH"/>
</technology>
<technology name="_784383360047">
<attribute name="WE-NUMBER" value="794383360047/0,47uH"/>
</technology>
<technology name="_784383360068">
<attribute name="WE-NUMBER" value="784383360068/0,68uH"/>
</technology>
<technology name="_78438336010">
<attribute name="WE-NUMBER" value="78438336010/1uH"/>
</technology>
<technology name="_78438336012">
<attribute name="WE-NUMBER" value="78438336012/1,2uH"/>
</technology>
<technology name="_78438336015">
<attribute name="WE-NUMBER" value="78438336015/1,5uH"/>
</technology>
<technology name="_78438336022">
<attribute name="WE-NUMBER" value="78438336022/2,2uH"/>
</technology>
<technology name="_78438336033">
<attribute name="WE-NUMBER" value="78438336033/3,3uH"/>
</technology>
<technology name="_78438336047">
<attribute name="WE-NUMBER" value="78438336047/4,7uH"/>
</technology>
<technology name="_78438336068">
<attribute name="WE-NUMBER" value="78438336068/6,8uH"/>
</technology>
<technology name="_78438336100">
<attribute name="WE-NUMBER" value="78438336100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_4020" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-MAIA SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;

&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;Hight current capability and handles hight transient current spikes
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range:-40°C up to 125°C
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;DC/DC-converter for high current power supplies  
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices 
&lt;br&gt;Wireless communication devices
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndMAIA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndMAIA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MAIA/"&gt;http://katalog.we-online.de/en/pbs/WE-MAIA/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-04
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MAIA_4020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383560033">
<attribute name="WE-NUMBER" value="784383560033/0,33uH"/>
</technology>
<technology name="_784383560056">
<attribute name="WE-NUMBER" value="784383560056/0,56uH"/>
</technology>
<technology name="_784383560068">
<attribute name="WE-NUMBER" value="784383560068/0,68uH"/>
</technology>
<technology name="_78438356010">
<attribute name="WE-NUMBER" value="78438356010/1uH"/>
</technology>
<technology name="_78438356012">
<attribute name="WE-NUMBER" value="78438356012/1,2uH"/>
</technology>
<technology name="_78438356015">
<attribute name="WE-NUMBER" value="78438356015/1,5uH"/>
</technology>
<technology name="_78438356018">
<attribute name="WE-NUMBER" value="78438356018/1,8uH"/>
</technology>
<technology name="_78438356022">
<attribute name="WE-NUMBER" value="78438356022/2,2uH"/>
</technology>
<technology name="_78438356033">
<attribute name="WE-NUMBER" value="78438356033/3,3uH"/>
</technology>
<technology name="_78438356047">
<attribute name="WE-NUMBER" value="78438356047/4,7uH"/>
</technology>
<technology name="_78438356056">
<attribute name="WE-NUMBER" value="78438356056/5,6uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MI_0805" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Multilayer Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Smallest inductor possible for less space needed on the printed circuit board and therefore perfect suitable for high density mounting
&lt;br&gt;
&lt;br&gt; No cross coupling because of closed magnetic circuits
&lt;br&gt;
&lt;br&gt; No crosstalk
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter circuits
&lt;br&gt;
&lt;br&gt; Oscillators
&lt;br&gt;
&lt;br&gt; Adjustment networks
&lt;br&gt;
&lt;br&gt; Discretely built T- or π-Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MI?"&gt;http://katalog.we-online.de/en/pbs/WE-MI?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MI_0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479014">
<attribute name="WE-NUMBER" value="74479014/0,047uH"/>
</technology>
<technology name="_7447902">
<attribute name="WE-NUMBER" value="7447902/0,1uH"/>
</technology>
<technology name="_74479021">
<attribute name="WE-NUMBER" value="74479021/0,1uH"/>
</technology>
<technology name="_74479022">
<attribute name="WE-NUMBER" value="74479022/0,15uH"/>
</technology>
<technology name="_74479023">
<attribute name="WE-NUMBER" value="74479023/0,22uH"/>
</technology>
<technology name="_74479027">
<attribute name="WE-NUMBER" value="74479027/0,27uH"/>
</technology>
<technology name="_744790282">
<attribute name="WE-NUMBER" value="744790282/8,2uH"/>
</technology>
<technology name="_7447903">
<attribute name="WE-NUMBER" value="7447903/0,33uH"/>
</technology>
<technology name="_74479032">
<attribute name="WE-NUMBER" value="74479032/0,47uH"/>
</technology>
<technology name="_74479035">
<attribute name="WE-NUMBER" value="74479035/0,56uH"/>
</technology>
<technology name="_7447904">
<attribute name="WE-NUMBER" value="7447904/0,68uH"/>
</technology>
<technology name="_74479045">
<attribute name="WE-NUMBER" value="74479045/0,82uH"/>
</technology>
<technology name="_7447905">
<attribute name="WE-NUMBER" value="7447905/1uH"/>
</technology>
<technology name="_74479051">
<attribute name="WE-NUMBER" value="74479051/1,8uH"/>
</technology>
<technology name="_744790515">
<attribute name="WE-NUMBER" value="744790515/1,5uH"/>
</technology>
<technology name="_74479052">
<attribute name="WE-NUMBER" value="74479052/2,2uH"/>
</technology>
<technology name="_74479053">
<attribute name="WE-NUMBER" value="74479053/3,3uH"/>
</technology>
<technology name="_74479056">
<attribute name="WE-NUMBER" value="74479056/5,6uH"/>
</technology>
<technology name="_7447906">
<attribute name="WE-NUMBER" value="7447906/4,7uH"/>
</technology>
<technology name="_74479068">
<attribute name="WE-NUMBER" value="74479068/6,8uH"/>
</technology>
<technology name="_7447908">
<attribute name="WE-NUMBER" value="7447908/10uH"/>
</technology>
<technology name="_74479081">
<attribute name="WE-NUMBER" value="74479081/12uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MI_1206" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Multilayer Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Smallest inductor possible for less space needed on the printed circuit board and therefore perfect suitable for high density mounting
&lt;br&gt;
&lt;br&gt; No cross coupling because of closed magnetic circuits
&lt;br&gt;
&lt;br&gt; No crosstalk
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter circuits
&lt;br&gt;
&lt;br&gt; Oscillators
&lt;br&gt;
&lt;br&gt; Adjustment networks
&lt;br&gt;
&lt;br&gt; Discretely built T- or π-Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MI?"&gt;http://katalog.we-online.de/en/pbs/WE-MI?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MI_1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479114">
<attribute name="WE-NUMBER" value="74479114/0,047uH"/>
</technology>
<technology name="_7447912">
<attribute name="WE-NUMBER" value="7447912/0,1uH"/>
</technology>
<technology name="_74479122">
<attribute name="WE-NUMBER" value="74479122/0,15uH"/>
</technology>
<technology name="_744791220">
<attribute name="WE-NUMBER" value="744791220/0,22uH"/>
</technology>
<technology name="_744791282">
<attribute name="WE-NUMBER" value="744791282/8,2uH"/>
</technology>
<technology name="_7447913">
<attribute name="WE-NUMBER" value="7447913/0,33uH"/>
</technology>
<technology name="_74479132">
<attribute name="WE-NUMBER" value="74479132/0,47uH"/>
</technology>
<technology name="_74479136">
<attribute name="WE-NUMBER" value="74479136/0,68uH"/>
</technology>
<technology name="_74479142">
<attribute name="WE-NUMBER" value="74479142/1,2uH"/>
</technology>
<technology name="_74479145">
<attribute name="WE-NUMBER" value="74479145/1,5uH"/>
</technology>
<technology name="_74479148">
<attribute name="WE-NUMBER" value="74479148/1,8uH"/>
</technology>
<technology name="_7447915">
<attribute name="WE-NUMBER" value="7447915/1uH"/>
</technology>
<technology name="_74479152">
<attribute name="WE-NUMBER" value="74479152/2,2uH"/>
</technology>
<technology name="_74479153">
<attribute name="WE-NUMBER" value="74479153/3,3uH"/>
</technology>
<technology name="_74479157">
<attribute name="WE-NUMBER" value="74479157/2,7uH"/>
</technology>
<technology name="_74479159">
<attribute name="WE-NUMBER" value="74479159/3,9uH"/>
</technology>
<technology name="_7447916">
<attribute name="WE-NUMBER" value="7447916/4,7uH"/>
</technology>
<technology name="_74479168">
<attribute name="WE-NUMBER" value="74479168/6,8uH"/>
</technology>
<technology name="_7447918">
<attribute name="WE-NUMBER" value="7447918/10uH"/>
</technology>
<technology name="_74479183">
<attribute name="WE-NUMBER" value="74479183/22uH"/>
</technology>
<technology name="_74479184">
<attribute name="WE-NUMBER" value="74479184/33uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MK_0402" prefix="L" uservalue="yes">
<description>&lt;b&gt;Multilayer Ceramic SMD Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Windings printed on ceramic substrate
&lt;br&gt;
&lt;br&gt; Extremely high self resonant frequency &gt; 17 GHz
&lt;br&gt;
&lt;br&gt; Inductive tolerances of 5%; ± 0.3 nH
&lt;br&gt;
&lt;br&gt; Operating temperature: –40°C to +120°C
&lt;br&gt;
&lt;br&gt; Inductance is stable over temperature
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; High frequency circuits
&lt;br&gt;
&lt;br&gt; Bluetooth
&lt;br&gt;
&lt;br&gt; Wireless LAN
&lt;br&gt;
&lt;br&gt; Filter circuits
&lt;br&gt;
&lt;br&gt; Oscillators
&lt;br&gt;
&lt;br&gt; Pagers
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; PCMCIA-cards
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-mk_multilayer_keramik_smd_induktivitaet.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-mk_multilayer_keramik_smd_induktivitaet.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MK?"&gt;http://katalog.we-online.de/en/pbs/WE-MK?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MK_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74478401">
<attribute name="WE-NUMBER" value="74478401/1nH"/>
</technology>
<technology name="_744784012">
<attribute name="WE-NUMBER" value="744784012/1,2nH"/>
</technology>
<technology name="_744784018">
<attribute name="WE-NUMBER" value="744784018/1,8nH"/>
</technology>
<technology name="_74478402">
<attribute name="WE-NUMBER" value="74478402/2nH"/>
</technology>
<technology name="_744784022">
<attribute name="WE-NUMBER" value="744784022/2,2nH"/>
</technology>
<technology name="_744784027">
<attribute name="WE-NUMBER" value="744784027/2,7nH"/>
</technology>
<technology name="_744784030">
<attribute name="WE-NUMBER" value="744784030/3nH"/>
</technology>
<technology name="_744784033">
<attribute name="WE-NUMBER" value="744784033/3,3nH"/>
</technology>
<technology name="_744784039">
<attribute name="WE-NUMBER" value="744784039/3,9nH"/>
</technology>
<technology name="_744784047">
<attribute name="WE-NUMBER" value="744784047/4,7uH"/>
</technology>
<technology name="_744784056">
<attribute name="WE-NUMBER" value="744784056/5,6nH"/>
</technology>
<technology name="_744784068">
<attribute name="WE-NUMBER" value="744784068/6,8uH"/>
</technology>
<technology name="_744784075">
<attribute name="WE-NUMBER" value="744784075/7,5nH"/>
</technology>
<technology name="_744784082">
<attribute name="WE-NUMBER" value="744784082/8,2nH"/>
</technology>
<technology name="_74478410">
<attribute name="WE-NUMBER" value="74478410/10nH"/>
</technology>
<technology name="_744784101">
<attribute name="WE-NUMBER" value="744784101/100nH"/>
</technology>
<technology name="_74478412">
<attribute name="WE-NUMBER" value="74478412/12nH"/>
</technology>
<technology name="_74478413">
<attribute name="WE-NUMBER" value="74478413/1,5nH"/>
</technology>
<technology name="_74478415">
<attribute name="WE-NUMBER" value="74478215/15nH"/>
</technology>
<technology name="_74478418">
<attribute name="WE-NUMBER" value="74478418/18nH"/>
</technology>
<technology name="_74478422">
<attribute name="WE-NUMBER" value="74478422/22nH"/>
</technology>
<technology name="_74478427">
<attribute name="WE-NUMBER" value="74478427/27nH"/>
</technology>
<technology name="_74478433">
<attribute name="WE-NUMBER" value="74478433/33nH"/>
</technology>
<technology name="_74478439">
<attribute name="WE-NUMBER" value="74478439/39nH"/>
</technology>
<technology name="_74478447">
<attribute name="WE-NUMBER" value="74478447/47nH"/>
</technology>
<technology name="_74478456">
<attribute name="WE-NUMBER" value="74478456/56nH"/>
</technology>
<technology name="_74478468">
<attribute name="WE-NUMBER" value="74478468/6,8nH"/>
</technology>
<technology name="_74478482">
<attribute name="WE-NUMBER" value="74478482/82nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MK_0402A" prefix="L" uservalue="yes">
<description>&lt;b&gt;Multilayer Ceramic SMD Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Windings printed on ceramic substrate
&lt;br&gt;
&lt;br&gt; Extremely high self resonant frequency &gt; 17 GHz
&lt;br&gt;
&lt;br&gt; Inductive tolerances of 5%; ± 0.3 nH
&lt;br&gt;
&lt;br&gt; Operating temperature: –40°C to +120°C
&lt;br&gt;
&lt;br&gt; Inductance is stable over temperature
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; High frequency circuits
&lt;br&gt;
&lt;br&gt; Bluetooth
&lt;br&gt;
&lt;br&gt; Wireless LAN
&lt;br&gt;
&lt;br&gt; Filter circuits
&lt;br&gt;
&lt;br&gt; Oscillators
&lt;br&gt;
&lt;br&gt; Pagers
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; PCMCIA-cards
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-mk_multilayer_keramik_smd_induktivitaet.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-mk_multilayer_keramik_smd_induktivitaet.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MK?"&gt;http://katalog.we-online.de/en/pbs/WE-MK?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MK_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744784010A">
<attribute name="WE-NUMBER" value="744784010A/1nH"/>
</technology>
<technology name="_744784012A">
<attribute name="WE-NUMBER" value="744784012A/1,2nH"/>
</technology>
<technology name="_744784015A">
<attribute name="WE-NUMBER" value="744784015A/1,5nH"/>
</technology>
<technology name="_744784018A">
<attribute name="WE-NUMBER" value="744784018A/1,8nH"/>
</technology>
<technology name="_744784022A">
<attribute name="WE-NUMBER" value="744784022A/2,2nH"/>
</technology>
<technology name="_744784027A">
<attribute name="WE-NUMBER" value="744784027A/2,7nH"/>
</technology>
<technology name="_744784033A">
<attribute name="WE-NUMBER" value="744784033A/3,3nH"/>
</technology>
<technology name="_744784039A">
<attribute name="WE-NUMBER" value="744784039A/3,9nH"/>
</technology>
<technology name="_744784047A">
<attribute name="WE-NUMBER" value="744784047A/4,7nH"/>
</technology>
<technology name="_744784056A">
<attribute name="WE-NUMBER" value="744784056A/5,6nH"/>
</technology>
<technology name="_744784068A">
<attribute name="WE-NUMBER" value="744784068A/6,8nH"/>
</technology>
<technology name="_744784082A">
<attribute name="WE-NUMBER" value="744784082A/8,2nH"/>
</technology>
<technology name="_744784110A">
<attribute name="WE-NUMBER" value="744784110A/10nH"/>
</technology>
<technology name="_744784112A">
<attribute name="WE-NUMBER" value="744784112A/12nH"/>
</technology>
<technology name="_744784115A">
<attribute name="WE-NUMBER" value="744784115A/15nH"/>
</technology>
<technology name="_744784118A">
<attribute name="WE-NUMBER" value="744784118A/18nH"/>
</technology>
<technology name="_744784122A">
<attribute name="WE-NUMBER" value="744784122A/12nH"/>
</technology>
<technology name="_744784127A">
<attribute name="WE-NUMBER" value="744784127A/27nH"/>
</technology>
<technology name="_744784133A">
<attribute name="WE-NUMBER" value="744784133A/33nH"/>
</technology>
<technology name="_744784139A">
<attribute name="WE-NUMBER" value="744784139A/39nH"/>
</technology>
<technology name="_744784147A">
<attribute name="WE-NUMBER" value="744784147A/47nH"/>
</technology>
<technology name="_744784156A">
<attribute name="WE-NUMBER" value="744784156A/56nH"/>
</technology>
<technology name="_744784168A">
<attribute name="WE-NUMBER" value="744784168A/68nH"/>
</technology>
<technology name="_744784182A">
<attribute name="WE-NUMBER" value="744784182A/82nH"/>
</technology>
<technology name="_744784210A">
<attribute name="WE-NUMBER" value="744784210A/100nH"/>
</technology>
<technology name="_744784212A">
<attribute name="WE-NUMBER" value="744784212A/120nH"/>
</technology>
<technology name="_744784215A">
<attribute name="WE-NUMBER" value="744784215A/150nH"/>
</technology>
<technology name="_744784218A">
<attribute name="WE-NUMBER" value="744784218A/180nH"/>
</technology>
<technology name="_744784222A">
<attribute name="WE-NUMBER" value="744784222A/220nH"/>
</technology>
<technology name="_744784227A">
<attribute name="WE-NUMBER" value="744784227A/270nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MK_0603" prefix="L" uservalue="yes">
<description>&lt;b&gt;Multilayer Ceramic SMD Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Windings printed on ceramic substrate
&lt;br&gt;
&lt;br&gt; Extremely high self resonant frequency &gt; 17 GHz
&lt;br&gt;
&lt;br&gt; Inductive tolerances of 5%; ± 0.3 nH
&lt;br&gt;
&lt;br&gt; Operating temperature: –40°C to +120°C
&lt;br&gt;
&lt;br&gt; Inductance is stable over temperature
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; High frequency circuits
&lt;br&gt;
&lt;br&gt; Bluetooth
&lt;br&gt;
&lt;br&gt; Wireless LAN
&lt;br&gt;
&lt;br&gt; Filter circuits
&lt;br&gt;
&lt;br&gt; Oscillators
&lt;br&gt;
&lt;br&gt; Pagers
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; PCMCIA-cards
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-mk_multilayer_keramik_smd_induktivitaet.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-mk_multilayer_keramik_smd_induktivitaet.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MK?"&gt;http://katalog.we-online.de/en/pbs/WE-MK?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MK_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74478601">
<attribute name="WE-NUMBER" value="74478601/1,5nH"/>
</technology>
<technology name="_744786010">
<attribute name="WE-NUMBER" value="744786010/1nH"/>
</technology>
<technology name="_744786011">
<attribute name="WE-NUMBER" value="744786011/1,8nH"/>
</technology>
<technology name="_744786012">
<attribute name="WE-NUMBER" value="744786012/1,2nH"/>
</technology>
<technology name="_74478602">
<attribute name="WE-NUMBER" value="74478602/2,2nH"/>
</technology>
<technology name="_744786022">
<attribute name="WE-NUMBER" value="744786022/2,7nH"/>
</technology>
<technology name="_74478603">
<attribute name="WE-NUMBER" value="74478603/3,3nH"/>
</technology>
<technology name="_744786033">
<attribute name="WE-NUMBER" value="744786033/3,9nH"/>
</technology>
<technology name="_74478604">
<attribute name="WE-NUMBER" value="74478604/4,7nH"/>
</technology>
<technology name="_74478605">
<attribute name="WE-NUMBER" value="74478605/5,6nH"/>
</technology>
<technology name="_74478606">
<attribute name="WE-NUMBER" value="74478606/6,8nH"/>
</technology>
<technology name="_74478608">
<attribute name="WE-NUMBER" value="74478608/8,2nH"/>
</technology>
<technology name="_74478611">
<attribute name="WE-NUMBER" value="74478611/10nH"/>
</technology>
<technology name="_744786110">
<attribute name="WE-NUMBER" value="744786110/100nH"/>
</technology>
<technology name="_744786112">
<attribute name="WE-NUMBER" value="744786112/12nH"/>
</technology>
<technology name="_744786115">
<attribute name="WE-NUMBER" value="744786115/15nH"/>
</technology>
<technology name="_744786118">
<attribute name="WE-NUMBER" value="744786118/18nH"/>
</technology>
<technology name="_74478612">
<attribute name="WE-NUMBER" value="74478612/22nH"/>
</technology>
<technology name="_744786121">
<attribute name="WE-NUMBER" value="744786121/27nH"/>
</technology>
<technology name="_74478613">
<attribute name="WE-NUMBER" value="74478613/33nH"/>
</technology>
<technology name="_744786131">
<attribute name="WE-NUMBER" value="744786131/39nH"/>
</technology>
<technology name="_74478614">
<attribute name="WE-NUMBER" value="74478614/47nH"/>
</technology>
<technology name="_74478615">
<attribute name="WE-NUMBER" value="74478615/56nH"/>
</technology>
<technology name="_74478616">
<attribute name="WE-NUMBER" value="74478616/68nH"/>
</technology>
<technology name="_74478617">
<attribute name="WE-NUMBER" value="74478617/82nH"/>
</technology>
<technology name="_74478622">
<attribute name="WE-NUMBER" value="74478622/120nH"/>
</technology>
<technology name="_74478625">
<attribute name="WE-NUMBER" value="74478625/150nH"/>
</technology>
<technology name="_74478628">
<attribute name="WE-NUMBER" value="74478628/180nH"/>
</technology>
<technology name="_74478632">
<attribute name="WE-NUMBER" value="74478632/220nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MK_0603A" prefix="L" uservalue="yes">
<description>&lt;b&gt;Multilayer Ceramic SMD Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Windings printed on ceramic substrate
&lt;br&gt;
&lt;br&gt; Extremely high self resonant frequency &gt; 17 GHz
&lt;br&gt;
&lt;br&gt; Inductive tolerances of 5%; ± 0.3 nH
&lt;br&gt;
&lt;br&gt; Operating temperature: –40°C to +120°C
&lt;br&gt;
&lt;br&gt; Inductance is stable over temperature
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; High frequency circuits
&lt;br&gt;
&lt;br&gt; Bluetooth
&lt;br&gt;
&lt;br&gt; Wireless LAN
&lt;br&gt;
&lt;br&gt; Filter circuits
&lt;br&gt;
&lt;br&gt; Oscillators
&lt;br&gt;
&lt;br&gt; Pagers
&lt;br&gt;
&lt;br&gt; Laptops
&lt;br&gt;
&lt;br&gt; PCMCIA-cards
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-mk_multilayer_keramik_smd_induktivitaet.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-mk_multilayer_keramik_smd_induktivitaet.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MK?"&gt;http://katalog.we-online.de/en/pbs/WE-MK?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MK_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744786010A">
<attribute name="WE-NUMBER" value="744786010A/1nH"/>
</technology>
<technology name="_744786012A">
<attribute name="WE-NUMBER" value="744786012A/1,2nH"/>
</technology>
<technology name="_744786015A">
<attribute name="WE-NUMBER" value="744786015A/1,5nH"/>
</technology>
<technology name="_744786018A">
<attribute name="WE-NUMBER" value="744786018A/1,8nH"/>
</technology>
<technology name="_744786022A">
<attribute name="WE-NUMBER" value="744786022A/2,2nH"/>
</technology>
<technology name="_744786027A">
<attribute name="WE-NUMBER" value="744786027A/2,7nH"/>
</technology>
<technology name="_744786033A">
<attribute name="WE-NUMBER" value="744786033A/3,3nH"/>
</technology>
<technology name="_744786039A">
<attribute name="WE-NUMBER" value="744786039A/3,9nH"/>
</technology>
<technology name="_744786047A">
<attribute name="WE-NUMBER" value="744786047A/4,7nH"/>
</technology>
<technology name="_744786056A">
<attribute name="WE-NUMBER" value="744786056A/5,6nH"/>
</technology>
<technology name="_744786068A">
<attribute name="WE-NUMBER" value="744786068A/6,8nH"/>
</technology>
<technology name="_744786082A">
<attribute name="WE-NUMBER" value="744786082A/8,2nH"/>
</technology>
<technology name="_744786110A">
<attribute name="WE-NUMBER" value="744786110A/10nH"/>
</technology>
<technology name="_744786112A">
<attribute name="WE-NUMBER" value="744786112A/12nH"/>
</technology>
<technology name="_744786115A">
<attribute name="WE-NUMBER" value="744786115A/15nH"/>
</technology>
<technology name="_744786118A">
<attribute name="WE-NUMBER" value="744786118A/18nH"/>
</technology>
<technology name="_744786122A">
<attribute name="WE-NUMBER" value="744786122A/22nH"/>
</technology>
<technology name="_744786127A">
<attribute name="WE-NUMBER" value="744786127A/27nH"/>
</technology>
<technology name="_744786133A">
<attribute name="WE-NUMBER" value="744786133A/33nH"/>
</technology>
<technology name="_744786139A">
<attribute name="WE-NUMBER" value="744786139A/39nH"/>
</technology>
<technology name="_744786147A">
<attribute name="WE-NUMBER" value="744786147A/47nH"/>
</technology>
<technology name="_744786156A">
<attribute name="WE-NUMBER" value="744786156A/56nH"/>
</technology>
<technology name="_744786168A">
<attribute name="WE-NUMBER" value="744786168A/68nH"/>
</technology>
<technology name="_744786182A">
<attribute name="WE-NUMBER" value="744786182A/82nH"/>
</technology>
<technology name="_744786210A">
<attribute name="WE-NUMBER" value="744786210A/100nH"/>
</technology>
<technology name="_744786212A">
<attribute name="WE-NUMBER" value="744786212A/120nH"/>
</technology>
<technology name="_744786215A">
<attribute name="WE-NUMBER" value="744786215A/150nH"/>
</technology>
<technology name="_744786218A">
<attribute name="WE-NUMBER" value="744786218A/180nH"/>
</technology>
<technology name="_744786222A">
<attribute name="WE-NUMBER" value="744786222A/220nH"/>
</technology>
<technology name="_744786227A">
<attribute name="WE-NUMBER" value="744786227A/270nH"/>
</technology>
<technology name="_744786233A">
<attribute name="WE-NUMBER" value="744786233A/330nH"/>
</technology>
<technology name="_744786239A">
<attribute name="WE-NUMBER" value="744786239A/390nH"/>
</technology>
<technology name="_744786243A">
<attribute name="WE-NUMBER" value="744786243A/430nH"/>
</technology>
<technology name="_744786247A">
<attribute name="WE-NUMBER" value="744786247A/470nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MPSB_0603_HC" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD EMI Multilayer Power Suppression Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High rated current up to 10 A
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Very low RDC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; 77 EMI suppression of DC/DC converters and DC power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MPSB.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MPSB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MPSB?"&gt;http://katalog.we-online.de/en/pbs/WE-MPSB?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MPSB_0603(W=2.6)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7427922808"/>
<technology name="_74279228111"/>
<technology name="_74279228260"/>
<technology name="_74279228600"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MPSB_0805_HC" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD EMI Multilayer Power Suppression Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High rated current up to 10 A
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Very low RDC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; 77 EMI suppression of DC/DC converters and DC power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MPSB.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MPSB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MPSB?"&gt;http://katalog.we-online.de/en/pbs/WE-MPSB?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MPSB_0805(W=4.0)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279220181"/>
<technology name="_74279220321"/>
<technology name="_74279220601"/>
<technology name="_74279220800"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MPSB_1206_HC" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD EMI Multilayer Power Suppression Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High rated current up to 10 A
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Very low RDC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; 77 EMI suppression of DC/DC converters and DC power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MPSB.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MPSB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MPSB?"&gt;http://katalog.we-online.de/en/pbs/WE-MPSB?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MPSB_1206(W=5.2)">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279221100"/>
<technology name="_74279221111"/>
<technology name="_74279221281"/>
<technology name="_74279221601"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MPSB_1612" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD EMI Multilayer Power Suppression Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High rated current up to 10 A
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Very low RDC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; 77 EMI suppression of DC/DC converters and DC power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MPSB.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MPSB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MPSB?"&gt;http://katalog.we-online.de/en/pbs/WE-MPSB?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MPSB_1612">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279223560"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MPSB_1812" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD EMI Multilayer Power Suppression Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High rated current up to 10 A
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Very low RDC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; 77 EMI suppression of DC/DC converters and DC power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MPSB.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MPSB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MPSB?"&gt;http://katalog.we-online.de/en/pbs/WE-MPSB?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_74279226101" package="WE-MPSB_1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MPSB_2220" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD EMI Multilayer Power Suppression Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High rated current up to 10 A
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Very low RDC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; 77 EMI suppression of DC/DC converters and DC power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MPSB.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MPSB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MPSB?"&gt;http://katalog.we-online.de/en/pbs/WE-MPSB?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MPSB_2220">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279224101"/>
<technology name="_74279224151"/>
<technology name="_74279224171"/>
<technology name="_74279224181"/>
<technology name="_74279224251"/>
<technology name="_74279224271"/>
<technology name="_74279224401"/>
<technology name="_74279224551"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MPSB_3312" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD EMI Multilayer Power Suppression Bead
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High rated current up to 10 A
&lt;br&gt;
&lt;br&gt; Operating temperature: –55 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Very low RDC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; 77 EMI suppression of DC/DC converters and DC power supply
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Variant abbreviation&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
WB means WIDE BAND&lt;br&gt;
HS means HIGH SPEED&lt;br&gt;
HC means HIGH CURRENT&lt;br&gt;

&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-MPSB.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-MPSB.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-MPSB?"&gt;http://katalog.we-online.de/en/pbs/WE-MPSB?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MPSB_3312">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74279225101"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2A_4532" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-PD2A SMD Power Inductor
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;
&lt;/b&gt;&lt;br&gt;Open size
&lt;br&gt;Current capability up to 14A
&lt;br&gt;Operating temperature:-40°C  to 125°C
&lt;br&gt;Recommended soder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;switching regulators with low operating voltage (navigation system, air conditioning, entertainment, park assistance control)
&lt;br&gt;Integrated DC/DC-converter 
&lt;br&gt;Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD2A/"&gt;http://katalog.we-online.de/en/pbs/WE-PD2A/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-04
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2A_4532">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7847730">
<attribute name="WE-NUMBER" value="7847730/1uH"/>
</technology>
<technology name="_784773018">
<attribute name="WE-NUMBER" value="784773018/1,8uH"/>
</technology>
<technology name="_784773022">
<attribute name="WE-NUMBER" value="784773022/2,2uH"/>
</technology>
<technology name="_784773033">
<attribute name="WE-NUMBER" value="784773033/3,3uH"/>
</technology>
<technology name="_784773039">
<attribute name="WE-NUMBER" value="784773039/3,9uH"/>
</technology>
<technology name="_784773047">
<attribute name="WE-NUMBER" value="784773047/4,7uH"/>
</technology>
<technology name="_784773056">
<attribute name="WE-NUMBER" value="784773056/5,6uH"/>
</technology>
<technology name="_784773068">
<attribute name="WE-NUMBER" value="784773068/6,8uH"/>
</technology>
<technology name="_784773082">
<attribute name="WE-NUMBER" value="784773082/8,2uH"/>
</technology>
<technology name="_78477310">
<attribute name="WE-NUMBER" value="78477310/10uH"/>
</technology>
<technology name="_784773112">
<attribute name="WE-NUMBER" value="784773112/12uH"/>
</technology>
<technology name="_784773115">
<attribute name="WE-NUMBER" value="784773115/15uH"/>
</technology>
<technology name="_784773118">
<attribute name="WE-NUMBER" value="784773118/18uH"/>
</technology>
<technology name="_784773122">
<attribute name="WE-NUMBER" value="784773122/22uH"/>
</technology>
<technology name="_784773127">
<attribute name="WE-NUMBER" value="784773127/27uH"/>
</technology>
<technology name="_784773133">
<attribute name="WE-NUMBER" value="784773133/33uH"/>
</technology>
<technology name="_784773139">
<attribute name="WE-NUMBER" value="784773139/39uH"/>
</technology>
<technology name="_784773147">
<attribute name="WE-NUMBER" value="784773147/47uH"/>
</technology>
<technology name="_784773156">
<attribute name="WE-NUMBER" value="784773156/56uH"/>
</technology>
<technology name="_784773168">
<attribute name="WE-NUMBER" value="784773168/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2A_5848" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-PD2A SMD Power Inductor
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;
&lt;/b&gt;&lt;br&gt;Open size
&lt;br&gt;Current capability up to 14A
&lt;br&gt;Operating temperature:-40°C  to 125°C
&lt;br&gt;Recommended soder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;switching regulators with low operating voltage (navigation system, air conditioning, entertainment, park assistance control)
&lt;br&gt;Integrated DC/DC-converter 
&lt;br&gt;Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD2A/"&gt;http://katalog.we-online.de/en/pbs/WE-PD2A/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-04
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2A_5848">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784774003">
<attribute name="WE-NUMBER" value="784774003/0,33uH"/>
</technology>
<technology name="_784774006">
<attribute name="WE-NUMBER" value="784774006/0,6uH"/>
</technology>
<technology name="_784774022">
<attribute name="WE-NUMBER" value="784774022/2,2uH"/>
</technology>
<technology name="_784774027">
<attribute name="WE-NUMBER" value="784774027/2,7uH"/>
</technology>
<technology name="_784774033">
<attribute name="WE-NUMBER" value="784774033/3,3uH"/>
</technology>
<technology name="_784774047">
<attribute name="WE-NUMBER" value="784774047/4,7uH"/>
</technology>
<technology name="_784774068">
<attribute name="WE-NUMBER" value="784774068/6,8uH"/>
</technology>
<technology name="_78477410">
<attribute name="WE-NUMBER" value="78477410/10uH"/>
</technology>
<technology name="_784774112">
<attribute name="WE-NUMBER" value="784774112/12uH"/>
</technology>
<technology name="_784774115">
<attribute name="WE-NUMBER" value="784774115/15uH"/>
</technology>
<technology name="_784774118">
<attribute name="WE-NUMBER" value="784774118/18uH"/>
</technology>
<technology name="_784774122">
<attribute name="WE-NUMBER" value="784774122/22uH"/>
</technology>
<technology name="_784774127">
<attribute name="WE-NUMBER" value="784774127/27uH"/>
</technology>
<technology name="_784774133">
<attribute name="WE-NUMBER" value="784774133/33uH"/>
</technology>
<technology name="_784774139">
<attribute name="WE-NUMBER" value="784774139/39uH"/>
</technology>
<technology name="_784774147">
<attribute name="WE-NUMBER" value="784774147/47uH"/>
</technology>
<technology name="_784774156">
<attribute name="WE-NUMBER" value="784774156/56uH"/>
</technology>
<technology name="_784774168">
<attribute name="WE-NUMBER" value="784774168/68uH"/>
</technology>
<technology name="_784774182">
<attribute name="WE-NUMBER" value="784774182/82uH"/>
</technology>
<technology name="_78477420">
<attribute name="WE-NUMBER" value="78477420/100uH"/>
</technology>
<technology name="_784774212">
<attribute name="WE-NUMBER" value="784774212/120uH"/>
</technology>
<technology name="_784774215">
<attribute name="WE-NUMBER" value="784774215/150uH"/>
</technology>
<technology name="_784774218">
<attribute name="WE-NUMBER" value="784774218/180uH"/>
</technology>
<technology name="_784774222">
<attribute name="WE-NUMBER" value="784774220/220uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2A_7850" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-PD2A SMD Power Inductor
&lt;br&gt;

&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;
&lt;/b&gt;&lt;br&gt;Open size
&lt;br&gt;Current capability up to 14A
&lt;br&gt;Operating temperature:-40°C  to 125°C
&lt;br&gt;Recommended soder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;switching regulators with low operating voltage (navigation system, air conditioning, entertainment, park assistance control)
&lt;br&gt;Integrated DC/DC-converter 
&lt;br&gt;Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD2A/"&gt;http://katalog.we-online.de/en/pbs/WE-PD2A/
&lt;/a&gt;&lt;p&gt;Created: 2015-02-04
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2A_7850">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784775012">
<attribute name="WE-NUMBER" value="784775012/1,2uH"/>
</technology>
<technology name="_784775022">
<attribute name="WE-NUMBER" value="784775022/2,2uH"/>
</technology>
<technology name="_784775033">
<attribute name="WE-NUMBER" value="784775033/3,3uH"/>
</technology>
<technology name="_784775047">
<attribute name="WE-NUMBER" value="784775047/4,7uH"/>
</technology>
<technology name="_784775056">
<attribute name="WE-NUMBER" value="784775056/5,6uH"/>
</technology>
<technology name="_784775068">
<attribute name="WE-NUMBER" value="784775068/6,8uH"/>
</technology>
<technology name="_784775082">
<attribute name="WE-NUMBER" value="784775082/8,2uH"/>
</technology>
<technology name="_78477510">
<attribute name="WE-NUMBER" value="78477510/10uH"/>
</technology>
<technology name="_784775112">
<attribute name="WE-NUMBER" value="784775112/12uH"/>
</technology>
<technology name="_784775115">
<attribute name="WE-NUMBER" value="784775115/15uH"/>
</technology>
<technology name="_784775118">
<attribute name="WE-NUMBER" value="784775118/18uH"/>
</technology>
<technology name="_784775122">
<attribute name="WE-NUMBER" value="784775122/22uH"/>
</technology>
<technology name="_784775127">
<attribute name="WE-NUMBER" value="784775127/27uH"/>
</technology>
<technology name="_784775133">
<attribute name="WE-NUMBER" value="784775133/33uH"/>
</technology>
<technology name="_784775139">
<attribute name="WE-NUMBER" value="784775139/39uH"/>
</technology>
<technology name="_784775147">
<attribute name="WE-NUMBER" value="784775147/47uH"/>
</technology>
<technology name="_784775168">
<attribute name="WE-NUMBER" value="784775168/68uH"/>
</technology>
<technology name="_784775182">
<attribute name="WE-NUMBER" value="784775182/82uH"/>
</technology>
<technology name="_78477520">
<attribute name="WE-NUMBER" value="78477520/100uH"/>
</technology>
<technology name="_784775212">
<attribute name="WE-NUMBER" value="784775212/120uH"/>
</technology>
<technology name="_784775215">
<attribute name="WE-NUMBER" value="784775215/150uH"/>
</technology>
<technology name="_784775218">
<attribute name="WE-NUMBER" value="784775218/180uH"/>
</technology>
<technology name="_784775222">
<attribute name="WE-NUMBER" value="784775222/220uH"/>
</technology>
<technology name="_784775227">
<attribute name="WE-NUMBER" value="784775227/270uH"/>
</technology>
<technology name="_784775233">
<attribute name="WE-NUMBER" value="784775233/330uH"/>
</technology>
<technology name="_784775239">
<attribute name="WE-NUMBER" value="784775239/390uH"/>
</technology>
<technology name="_784775247">
<attribute name="WE-NUMBER" value="784775247/470uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDA_7332" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-PDA SMD Shielded Power Inductor
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;Wire connection:welding technology
&lt;br&gt;Operating temperature:-40°C up to 125°C
&lt;br&gt;Highest possible current loading for SMD Inductors
&lt;br&gt;Magnetically shielded version which results in a low leakage field High storage capacity
&lt;br&gt;Low self-losses
&lt;br&gt;Core Material:NiZn
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;Multimedia applications
&lt;br&gt;Switching regulators with low operating voltages (Computer, Notebook, smart phones)
&lt;br&gt;Integrated DC/DC-converter
&lt;br&gt;Perfect suitable for switching regulators with exrtemely high efficiency (&gt;86%)
&lt;br&gt;

&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-pda.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-pda.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PDA/"&gt;http://katalog.we-online.de/en/pbs/WE-PDA/
&lt;/a&gt;&lt;p&gt;Created: 2015-01-30
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PDA_7332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784778010">
<attribute name="WE-NUMBER" value="784778010/1uH"/>
</technology>
<technology name="_784778022">
<attribute name="WE-NUMBER" value="784778022/2,2uH"/>
</technology>
<technology name="_784778033">
<attribute name="WE-NUMBER" value="784778033/3,3uH"/>
</technology>
<technology name="_784778047">
<attribute name="WE-NUMBER" value="784778047/4,7uH"/>
</technology>
<technology name="_784778068">
<attribute name="WE-NUMBER" value="784778068/6,8uH"/>
</technology>
<technology name="_784778082">
<attribute name="WE-NUMBER" value="784778082/8,2uH"/>
</technology>
<technology name="_784778100">
<attribute name="WE-NUMBER" value="784778100/10uH"/>
</technology>
<technology name="_784778101">
<attribute name="WE-NUMBER" value="784778101/100uH"/>
</technology>
<technology name="_784778102">
<attribute name="WE-NUMBER" value="784778102/1000uH"/>
</technology>
<technology name="_784778220">
<attribute name="WE-NUMBER" value="784778220/22uH"/>
</technology>
<technology name="_784778221">
<attribute name="WE-NUMBER" value="784778221/220uH"/>
</technology>
<technology name="_784778470">
<attribute name="WE-NUMBER" value="784778470/47uH"/>
</technology>
<technology name="_784778471">
<attribute name="WE-NUMBER" value="784778471/470uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDA_7345" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-PDA SMD Shielded Power Inductor
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;Wire connection:welding technology
&lt;br&gt;Operating temperature:-40°C up to 125°C
&lt;br&gt;Highest possible current loading for SMD Inductors
&lt;br&gt;Magnetically shielded version which results in a low leakage field High storage capacity
&lt;br&gt;Low self-losses
&lt;br&gt;Core Material:NiZn
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;Multimedia applications
&lt;br&gt;Switching regulators with low operating voltages (Computer, Notebook, smart phones)
&lt;br&gt;Integrated DC/DC-converter
&lt;br&gt;Perfect suitable for switching regulators with exrtemely high efficiency (&gt;86%)
&lt;br&gt;

&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-pda.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-pda.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PDA/"&gt;http://katalog.we-online.de/en/pbs/WE-PDA/
&lt;/a&gt;&lt;p&gt;Created: 2015-01-30
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PDA_7345">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784777010">
<attribute name="WE-NUMBER" value="784777010/1uH"/>
</technology>
<technology name="_784777022">
<attribute name="WE-NUMBER" value="784777022/2,2uH"/>
</technology>
<technology name="_784777033">
<attribute name="WE-NUMBER" value="784777033/3,3uH"/>
</technology>
<technology name="_784777047">
<attribute name="WE-NUMBER" value="784777047/4,7uH"/>
</technology>
<technology name="_784777068">
<attribute name="WE-NUMBER" value="784777068/6,8uH"/>
</technology>
<technology name="_784777082">
<attribute name="WE-NUMBER" value="784777082/8,2uH"/>
</technology>
<technology name="_784777100">
<attribute name="WE-NUMBER" value="784777100/10uH"/>
</technology>
<technology name="_784777101">
<attribute name="WE-NUMBER" value="784777101/100uH"/>
</technology>
<technology name="_784777102">
<attribute name="WE-NUMBER" value="784777102/1000uH"/>
</technology>
<technology name="_784777220">
<attribute name="WE-NUMBER" value="784777220/22uH"/>
</technology>
<technology name="_784777221">
<attribute name="WE-NUMBER" value="784777221/220uH"/>
</technology>
<technology name="_784777331">
<attribute name="WE-NUMBER" value="784777331/330uH"/>
</technology>
<technology name="_784777470">
<attribute name="WE-NUMBER" value="784777470/47uH"/>
</technology>
<technology name="_784777471">
<attribute name="WE-NUMBER" value="784777471/470uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDA_1260" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-PDA SMD Shielded Power Inductor
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;Wire connection:welding technology
&lt;br&gt;Operating temperature:-40°C up to 125°C
&lt;br&gt;Highest possible current loading for SMD Inductors
&lt;br&gt;Magnetically shielded version which results in a low leakage field High storage capacity
&lt;br&gt;Low self-losses
&lt;br&gt;Core Material:NiZn
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;Multimedia applications
&lt;br&gt;Switching regulators with low operating voltages (Computer, Notebook, smart phones)
&lt;br&gt;Integrated DC/DC-converter
&lt;br&gt;Perfect suitable for switching regulators with exrtemely high efficiency (&gt;86%)
&lt;br&gt;

&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-pda.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-pda.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PDA/"&gt;http://katalog.we-online.de/en/pbs/WE-PDA/
&lt;/a&gt;&lt;p&gt;Created: 2015-01-30
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PDA_1260">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784771010">
<attribute name="WE-NUMBER" value="784771010/1uH"/>
</technology>
<technology name="_784771022">
<attribute name="WE-NUMBER" value="784771022/2,2uH"/>
</technology>
<technology name="_784771033">
<attribute name="WE-NUMBER" value="784771033/3,3uH"/>
</technology>
<technology name="_784771047">
<attribute name="WE-NUMBER" value="784771047/4,7uH"/>
</technology>
<technology name="_784771068">
<attribute name="WE-NUMBER" value="784771068/6,8uH"/>
</technology>
<technology name="_784771082">
<attribute name="WE-NUMBER" value="784771082/8,2uH"/>
</technology>
<technology name="_784771100">
<attribute name="WE-NUMBER" value="784771100/10uH"/>
</technology>
<technology name="_784771101">
<attribute name="WE-NUMBER" value="784771101/100uH"/>
</technology>
<technology name="_784771102">
<attribute name="WE-NUMBER" value="784771102/1000uH"/>
</technology>
<technology name="_784771220">
<attribute name="WE-NUMBER" value="784771220/22uH"/>
</technology>
<technology name="_784771221">
<attribute name="WE-NUMBER" value="784771221/220uH"/>
</technology>
<technology name="_784771330">
<attribute name="WE-NUMBER" value="784771330/33uH"/>
</technology>
<technology name="_784771331">
<attribute name="WE-NUMBER" value="784771331/330uH"/>
</technology>
<technology name="_784771470">
<attribute name="WE-NUMBER" value="784771470/47uH"/>
</technology>
<technology name="_784771471">
<attribute name="WE-NUMBER" value="784771471/470uH"/>
</technology>
<technology name="_784771680">
<attribute name="WE-NUMBER" value="784771680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDA_1280" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-PDA SMD Shielded Power Inductor
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;Wire connection:welding technology
&lt;br&gt;Operating temperature:-40°C up to 125°C
&lt;br&gt;Highest possible current loading for SMD Inductors
&lt;br&gt;Magnetically shielded version which results in a low leakage field High storage capacity
&lt;br&gt;Low self-losses
&lt;br&gt;Core Material:NiZn
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;Multimedia applications
&lt;br&gt;Switching regulators with low operating voltages (Computer, Notebook, smart phones)
&lt;br&gt;Integrated DC/DC-converter
&lt;br&gt;Perfect suitable for switching regulators with exrtemely high efficiency (&gt;86%)
&lt;br&gt;

&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-pda.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-pda.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PDA/"&gt;http://katalog.we-online.de/en/pbs/WE-PDA/
&lt;/a&gt;&lt;p&gt;Created: 2015-01-30
&lt;br&gt;2015 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PDA_1280">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78477010">
<attribute name="WE-NUMBER" value="78477010/1uH"/>
</technology>
<technology name="_784770100">
<attribute name="WE-NUMBER" value="784770100/10uH"/>
</technology>
<technology name="_784770101">
<attribute name="WE-NUMBER" value="784770101/100uH"/>
</technology>
<technology name="_784770102">
<attribute name="WE-NUMBER" value="784770102/1000uH"/>
</technology>
<technology name="_78477022">
<attribute name="WE-NUMBER" value="78477022/2,2uH"/>
</technology>
<technology name="_784770220">
<attribute name="WE-NUMBER" value="784770220/22uH"/>
</technology>
<technology name="_784770221">
<attribute name="WE-NUMBER" value="784770221/220uH"/>
</technology>
<technology name="_78477033">
<attribute name="WE-NUMBER" value="78477033/3,3uH"/>
</technology>
<technology name="_784770330">
<attribute name="WE-NUMBER" value="784770330/33uH"/>
</technology>
<technology name="_784770331">
<attribute name="WE-NUMBER" value="784770331/330uH"/>
</technology>
<technology name="_78477047">
<attribute name="WE-NUMBER" value="78477047/4,7uH"/>
</technology>
<technology name="_784770470">
<attribute name="WE-NUMBER" value="784770470/47uH"/>
</technology>
<technology name="_784770471">
<attribute name="WE-NUMBER" value="784770471/470uH"/>
</technology>
<technology name="_78477068">
<attribute name="WE-NUMBER" value="78477068/6,8uH"/>
</technology>
<technology name="_784770680">
<attribute name="WE-NUMBER" value="784770680/68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-POE_ER11/5" prefix="T" uservalue="yes">
<description>&lt;b&gt;Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Flyback transformer designed for PoE PDs
&lt;br&gt;
&lt;br&gt; Input voltage: 36 V to 57 V
&lt;br&gt;
&lt;br&gt; Switching frequencies: 200–500 kHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Insulation test voltage: 1.5 kVAC/1 min
&lt;br&gt;
&lt;br&gt; Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Suitable for PoE IC’s like LTC4267, TPS 23750, TPS 23770, LM5070, LM 5071, LM 5072
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-poe_uebertrager_power_over_ethernet.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-poe_uebertrager_power_over_ethernet.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PoE?"&gt;http://katalog.we-online.de/en/pbs/WE-PoE?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE"/>
</gates>
<devices>
<device name="" package="WE_ER11/5_SMD_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="9"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="5" pad="12"/>
<connect gate="G$1" pin="6" pad="7"/>
<connect gate="G$1" pin="7" pad="11"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="10"/>
</connects>
<technologies>
<technology name="_749119133"/>
<technology name="_749119150"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-POE_ER14.5/6" prefix="T" uservalue="yes">
<description>&lt;b&gt;Power over Ethernet Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Flyback transformer designed for PoE PDs
&lt;br&gt;
&lt;br&gt; Input voltage: 36 V to 57 V
&lt;br&gt;
&lt;br&gt; Switching frequencies: 200–500 kHz
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt; Insulation test voltage: 1.5 kVAC/1 min
&lt;br&gt;
&lt;br&gt; Different output powers and voltages available
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Suitable for PoE IC’s like LTC4267, TPS 23750, TPS 23770, LM5070, LM 5071, LM 5072
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-poe_uebertrager_power_over_ethernet.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-poe_uebertrager_power_over_ethernet.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PoE?"&gt;http://katalog.we-online.de/en/pbs/WE-PoE?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POE"/>
</gates>
<devices>
<device name="" package="WE_ER14.5/6_SMD_12PIN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="9"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="5" pad="12"/>
<connect gate="G$1" pin="6" pad="7"/>
<connect gate="G$1" pin="7" pad="11"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="10"/>
</connects>
<technologies>
<technology name="_749119218"/>
<technology name="_749119233"/>
<technology name="_749119250"/>
<technology name="_7491192912"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RFI_1008A" prefix="L" uservalue="yes">
<description>&lt;b&gt;Ferrite SMD Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High thermal stability
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +85 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Especially developed for RF applications
&lt;br&gt;
&lt;br&gt; RFID
&lt;br&gt;
&lt;br&gt; Low frequency radio applications (Keyless)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-RFI.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-RFI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-RFI?"&gt;http://katalog.we-online.de/en/pbs/WE-RFI?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-08&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-RFI_1008A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744762312A">
<attribute name="WE-NUMBER" value="744762312A/1,2uH"/>
</technology>
<technology name="_744762315A">
<attribute name="WE-NUMBER" value="744762315A/1,5uH"/>
</technology>
<technology name="_744762318A">
<attribute name="WE-NUMBER" value="744762318A/1,8uH"/>
</technology>
<technology name="_744762322A">
<attribute name="WE-NUMBER" value="744762322A/2,2uH"/>
</technology>
<technology name="_744762327A">
<attribute name="WE-NUMBER" value="744762327A/2,7uH"/>
</technology>
<technology name="_744762333A">
<attribute name="WE-NUMBER" value="744762333A/3,3uH"/>
</technology>
<technology name="_744762339A">
<attribute name="WE-NUMBER" value="744762339A/3,9uH"/>
</technology>
<technology name="_744762347A">
<attribute name="WE-NUMBER" value="744762347A/4,7uH"/>
</technology>
<technology name="_744762356A">
<attribute name="WE-NUMBER" value="744762356A/5,6uH"/>
</technology>
<technology name="_744762368A">
<attribute name="WE-NUMBER" value="744762368A/6,8uH"/>
</technology>
<technology name="_744762382A">
<attribute name="WE-NUMBER" value="744762382A/8,2uH"/>
</technology>
<technology name="_744762410A">
<attribute name="WE-NUMBER" value="744762410A/10uH"/>
</technology>
<technology name="_744762415A">
<attribute name="WE-NUMBER" value="744762415A/15uH"/>
</technology>
<technology name="_744762418A">
<attribute name="WE-NUMBER" value="744762418A/18uH"/>
</technology>
<technology name="_744762422A">
<attribute name="WE-NUMBER" value="744762422A/22uH"/>
</technology>
<technology name="_744762427A">
<attribute name="WE-NUMBER" value="744762427A/27uH"/>
</technology>
<technology name="_744762433A">
<attribute name="WE-NUMBER" value="744762433A/33uH"/>
</technology>
<technology name="_744762439A">
<attribute name="WE-NUMBER" value="744762439A/39uH"/>
</technology>
<technology name="_744762447A">
<attribute name="WE-NUMBER" value="744762447A/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SCC_1210" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Common Mode Line Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Enormous common mode impedance Z
&lt;br&gt;
&lt;br&gt; Small dimensions
&lt;br&gt;
&lt;br&gt; High current ratings
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Attenuation of common mode noise
&lt;br&gt;
&lt;br&gt; Power supplies
&lt;br&gt;
&lt;br&gt; Data lines
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;&lt;a href=&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSCC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndSCC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SCC?"&gt;http://katalog.we-online.de/en/pbs/WE-SCC?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SCC"/>
</gates>
<devices>
<device name="" package="WE-SCC_1260/1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744284100"/>
<technology name="_744284101"/>
<technology name="_744284102"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SCC_7345" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Common Mode Line Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Enormous common mode impedance Z
&lt;br&gt;
&lt;br&gt; Small dimensions
&lt;br&gt;
&lt;br&gt; High current ratings
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Attenuation of common mode noise
&lt;br&gt;
&lt;br&gt; Power supplies
&lt;br&gt;
&lt;br&gt; Data lines
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;&lt;a href=&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/IndSCC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eisos/thb_IndSCC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SCC?"&gt;http://katalog.we-online.de/en/pbs/WE-SCC?&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SCC"/>
</gates>
<devices>
<device name="" package="WE-SCC_7345">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744281100"/>
<technology name="_744281101"/>
<technology name="_744281471"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TCI_0402" prefix="L" uservalue="yes">
<description>&lt;b&gt;Thinfilm Chip Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High self resonant frequency
&lt;br&gt;
&lt;br&gt; Tight tolerances of 2% (1% on request) or ± 0.1 nH and small inductance values
&lt;br&gt;
&lt;br&gt; Outstanding temperature stability
&lt;br&gt;
&lt;br&gt; In high frequency circuit the inductance is very stable
&lt;br&gt;
&lt;br&gt; Small inductance values
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Mobile phone
&lt;br&gt;
&lt;br&gt; Pagers
&lt;br&gt;
&lt;br&gt; GPS products
&lt;br&gt;
&lt;br&gt; Wireless LAN
&lt;br&gt;
&lt;br&gt; Communication appliances
&lt;br&gt;
&lt;br&gt; RF Transceiver Module
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/RfTCI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/RfTCI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TCI?"&gt;http://katalog.we-online.de/en/pbs/WE-TCI?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Dan Xu 2014-07-11&lt;br&gt;
&lt;/b&gt;2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-TCI_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744901010">
<attribute name="WE-NUMBER" value="744901010/1nH"/>
</technology>
<technology name="_744901012">
<attribute name="WE-NUMBER" value="744901012/1,2nH"/>
</technology>
<technology name="_744901015">
<attribute name="WE-NUMBER" value="744901015/1,5nH"/>
</technology>
<technology name="_744901018">
<attribute name="WE-NUMBER" value="744901018/1,8nH"/>
</technology>
<technology name="_744901022">
<attribute name="WE-NUMBER" value="744901022/2,2nH"/>
</technology>
<technology name="_744901027">
<attribute name="WE-NUMBER" value="744901027/2,7nH"/>
</technology>
<technology name="_744901033">
<attribute name="WE-NUMBER" value="744901033/3,3nH"/>
</technology>
<technology name="_744901039">
<attribute name="WE-NUMBER" value="744901039/3,9nH"/>
</technology>
<technology name="_744901047">
<attribute name="WE-NUMBER" value="744901047/4,7nH"/>
</technology>
<technology name="_744901056">
<attribute name="WE-NUMBER" value="744901056/5,6nH"/>
</technology>
<technology name="_744901068">
<attribute name="WE-NUMBER" value="744901068/6,8nH"/>
</technology>
<technology name="_744901082">
<attribute name="WE-NUMBER" value="744901082/8,2nH"/>
</technology>
<technology name="_744901110">
<attribute name="WE-NUMBER" value="744901110/10nH"/>
</technology>
<technology name="_744901112">
<attribute name="WE-NUMBER" value="744901112/12nH"/>
</technology>
<technology name="_744901115">
<attribute name="WE-NUMBER" value="744901115/15nH"/>
</technology>
<technology name="_744901118">
<attribute name="WE-NUMBER" value="744901118/18nH"/>
</technology>
<technology name="_744901122">
<attribute name="WE-NUMBER" value="744901122/22nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVSP_BI_600W" prefix="D" uservalue="yes">
<description>&lt;b&gt; WE-TVSP Power TVS Diode&lt;/b&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVSP/824500101"&gt;http://katalog.we-online.de/en/pbs/WE-TVSP/824500101&lt;/a&gt;&lt;p&gt;

2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="BIDIRECTIONAL"/>
</gates>
<devices>
<device name="" package="VARTVSP_SMB/DO-214AA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_824521101"/>
<technology name="_824521102"/>
<technology name="_824521111"/>
<technology name="_824521121"/>
<technology name="_824521131"/>
<technology name="_824521141"/>
<technology name="_824521151"/>
<technology name="_824521161"/>
<technology name="_824521171"/>
<technology name="_824521181"/>
<technology name="_824521201"/>
<technology name="_824521221"/>
<technology name="_824521241"/>
<technology name="_824521261"/>
<technology name="_824521281"/>
<technology name="_824521301"/>
<technology name="_824521331"/>
<technology name="_824521361"/>
<technology name="_824521401"/>
<technology name="_824521431"/>
<technology name="_824521451"/>
<technology name="_824521481"/>
<technology name="_824521500"/>
<technology name="_824521511"/>
<technology name="_824521541"/>
<technology name="_824521581"/>
<technology name="_824521600"/>
<technology name="_824521601"/>
<technology name="_824521641"/>
<technology name="_824521650"/>
<technology name="_824521700"/>
<technology name="_824521701"/>
<technology name="_824521750"/>
<technology name="_824521751"/>
<technology name="_824521781"/>
<technology name="_824521800"/>
<technology name="_824521850"/>
<technology name="_824521851"/>
<technology name="_824521900"/>
<technology name="_824521901"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVSP_BI_1500W" prefix="D" uservalue="yes">
<description>&lt;b&gt; WE-TVSP Power TVS Diode&lt;/b&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVSP/824500101"&gt;http://katalog.we-online.de/en/pbs/WE-TVSP/824500101&lt;/a&gt;&lt;p&gt;

2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="BIDIRECTIONAL"/>
</gates>
<devices>
<device name="" package="VARTVSP_SMC&amp;SMD/DO-214AB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_824541101"/>
<technology name="_824541102"/>
<technology name="_824541111"/>
<technology name="_824541121"/>
<technology name="_824541131"/>
<technology name="_824541141"/>
<technology name="_824541151"/>
<technology name="_824541161"/>
<technology name="_824541171"/>
<technology name="_824541181"/>
<technology name="_824541201"/>
<technology name="_824541221"/>
<technology name="_824541241"/>
<technology name="_824541261"/>
<technology name="_824541281"/>
<technology name="_824541301"/>
<technology name="_824541331"/>
<technology name="_824541361"/>
<technology name="_824541401"/>
<technology name="_824541431"/>
<technology name="_824541451"/>
<technology name="_824541481"/>
<technology name="_824541500"/>
<technology name="_824541511"/>
<technology name="_824541541"/>
<technology name="_824541581"/>
<technology name="_824541600"/>
<technology name="_824541601"/>
<technology name="_824541641"/>
<technology name="_824541650"/>
<technology name="_824541700"/>
<technology name="_824541701"/>
<technology name="_824541750"/>
<technology name="_824541751"/>
<technology name="_824541781"/>
<technology name="_824541800"/>
<technology name="_824541850"/>
<technology name="_824541851"/>
<technology name="_824541900"/>
<technology name="_824541901"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVSP_BI_3000W" prefix="D" uservalue="yes">
<description>&lt;b&gt; WE-TVSP Power TVS Diode&lt;/b&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVSP/824500101"&gt;http://katalog.we-online.de/en/pbs/WE-TVSP/824500101&lt;/a&gt;&lt;p&gt;

2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="BIDIRECTIONAL"/>
</gates>
<devices>
<device name="" package="VARTVSP_SMC&amp;SMD/DO-214AB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_824551101"/>
<technology name="_824551102"/>
<technology name="_824551111"/>
<technology name="_824551121"/>
<technology name="_824551131"/>
<technology name="_824551141"/>
<technology name="_824551151"/>
<technology name="_824551161"/>
<technology name="_824551171"/>
<technology name="_824551181"/>
<technology name="_824551201"/>
<technology name="_824551221"/>
<technology name="_824551241"/>
<technology name="_824551261"/>
<technology name="_824551281"/>
<technology name="_824551301"/>
<technology name="_824551331"/>
<technology name="_824551361"/>
<technology name="_824551401"/>
<technology name="_824551431"/>
<technology name="_824551451"/>
<technology name="_824551481"/>
<technology name="_824551500"/>
<technology name="_824551511"/>
<technology name="_824551541"/>
<technology name="_824551581"/>
<technology name="_824551600"/>
<technology name="_824551601"/>
<technology name="_824551641"/>
<technology name="_824551650"/>
<technology name="_824551700"/>
<technology name="_824551701"/>
<technology name="_824551750"/>
<technology name="_824551751"/>
<technology name="_824551781"/>
<technology name="_824551800"/>
<technology name="_824551850"/>
<technology name="_824551851"/>
<technology name="_824551900"/>
<technology name="_824551901"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVSP_UNI_600W" prefix="D" uservalue="yes">
<description>&lt;b&gt; WE-TVSP Power TVS Diode&lt;/b&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVSP/824500101"&gt;http://katalog.we-online.de/en/pbs/WE-TVSP/824500101&lt;/a&gt;&lt;p&gt;

2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="UNIDIRECTIONAL"/>
</gates>
<devices>
<device name="" package="VARTVSP_SMB/DO-214AA_UNI">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="_824520101"/>
<technology name="_824520102"/>
<technology name="_824520111"/>
<technology name="_824520121"/>
<technology name="_824520131"/>
<technology name="_824520141"/>
<technology name="_824520151"/>
<technology name="_824520161"/>
<technology name="_824520171"/>
<technology name="_824520181"/>
<technology name="_824520201"/>
<technology name="_824520221"/>
<technology name="_824520241"/>
<technology name="_824520261"/>
<technology name="_824520281"/>
<technology name="_824520301"/>
<technology name="_824520331"/>
<technology name="_824520361"/>
<technology name="_824520401"/>
<technology name="_824520431"/>
<technology name="_824520451"/>
<technology name="_824520481"/>
<technology name="_824520500"/>
<technology name="_824520511"/>
<technology name="_824520541"/>
<technology name="_824520581"/>
<technology name="_824520600"/>
<technology name="_824520601"/>
<technology name="_824520641"/>
<technology name="_824520650"/>
<technology name="_824520700"/>
<technology name="_824520701"/>
<technology name="_824520750"/>
<technology name="_824520751"/>
<technology name="_824520781"/>
<technology name="_824520800"/>
<technology name="_824520850"/>
<technology name="_824520851"/>
<technology name="_824520900"/>
<technology name="_824520901"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVSP_UNI_1500W" prefix="D">
<description>&lt;b&gt; WE-TVSP Power TVS Diode&lt;/b&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVSP/824500101"&gt;http://katalog.we-online.de/en/pbs/WE-TVSP/824500101&lt;/a&gt;&lt;p&gt;

2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="UNIDIRECTIONAL"/>
</gates>
<devices>
<device name="" package="VARTVSP_SMC&amp;SMD/DO-214AB_UNI">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="_824540101"/>
<technology name="_824540102"/>
<technology name="_824540111"/>
<technology name="_824540121"/>
<technology name="_824540131"/>
<technology name="_824540141"/>
<technology name="_824540151"/>
<technology name="_824540161"/>
<technology name="_824540171"/>
<technology name="_824540181"/>
<technology name="_824540201"/>
<technology name="_824540221"/>
<technology name="_824540241"/>
<technology name="_824540261"/>
<technology name="_824540281"/>
<technology name="_824540301"/>
<technology name="_824540331"/>
<technology name="_824540361"/>
<technology name="_824540401"/>
<technology name="_824540431"/>
<technology name="_824540451"/>
<technology name="_824540481"/>
<technology name="_824540500"/>
<technology name="_824540511"/>
<technology name="_824540541"/>
<technology name="_824540581"/>
<technology name="_824540600"/>
<technology name="_824540601"/>
<technology name="_824540641"/>
<technology name="_824540650"/>
<technology name="_824540700"/>
<technology name="_824540701"/>
<technology name="_824540750"/>
<technology name="_824540751"/>
<technology name="_824540781"/>
<technology name="_824540800"/>
<technology name="_824540850"/>
<technology name="_824540851"/>
<technology name="_824540900"/>
<technology name="_824540901"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TVSP_UNI_3000W" prefix="D" uservalue="yes">
<description>&lt;b&gt; WE-TVSP Power TVS Diode&lt;/b&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-TVSP_600W-3000W_D0214AA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-TVSP/824500101"&gt;http://katalog.we-online.de/en/pbs/WE-TVSP/824500101&lt;/a&gt;&lt;p&gt;

2015 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="UNIDIRECTIONAL"/>
</gates>
<devices>
<device name="" package="VARTVSP_SMC&amp;SMD/DO-214AB_UNI">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="_824550101"/>
<technology name="_824550102"/>
<technology name="_824550111"/>
<technology name="_824550121"/>
<technology name="_824550131"/>
<technology name="_824550141"/>
<technology name="_824550151"/>
<technology name="_824550161"/>
<technology name="_824550171"/>
<technology name="_824550181"/>
<technology name="_824550201"/>
<technology name="_824550221"/>
<technology name="_824550241"/>
<technology name="_824550261"/>
<technology name="_824550281"/>
<technology name="_824550301"/>
<technology name="_824550331"/>
<technology name="_824550361"/>
<technology name="_824550401"/>
<technology name="_824550431"/>
<technology name="_824550451"/>
<technology name="_824550481"/>
<technology name="_824550500"/>
<technology name="_824550511"/>
<technology name="_824550541"/>
<technology name="_824550581"/>
<technology name="_824550600"/>
<technology name="_824550601"/>
<technology name="_824550641"/>
<technology name="_824550650"/>
<technology name="_824550700"/>
<technology name="_824550701"/>
<technology name="_824550750"/>
<technology name="_824550751"/>
<technology name="_824550781"/>
<technology name="_824550800"/>
<technology name="_824550850"/>
<technology name="_824550851"/>
<technology name="_824550900"/>
<technology name="_824550901"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_SMT_750871011" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit STM&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_STM?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_STM?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:2W_2"/>
</gates>
<devices>
<device name="" package="WE_E16/8/5_THT_HORIZONTAL_9PIN">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="9"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="2"/>
<connect gate="G$1" pin="7" pad="1"/>
<connect gate="G$1" pin="8" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_SMT_750871030" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit STM&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/UtUNIT_STM_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_STM?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_STM?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_2W:2W_2"/>
</gates>
<devices>
<device name="" package="WE_E16/8/5_THT_HORIZONTAL_9PIN">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="9"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="2"/>
<connect gate="G$1" pin="7" pad="1"/>
<connect gate="G$1" pin="8" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_PI_7508110102" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit PI&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_PI?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_PI?&lt;/a&gt;&lt;p&gt;


Created  by  Yingchun 2016-09-22&lt;br&gt;
2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_4W:1W"/>
</gates>
<devices>
<device name="" package="WE-UNIT_PI_75081101XX">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="1"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="5" pad="3"/>
<connect gate="G$1" pin="6" pad="7"/>
<connect gate="G$1" pin="7" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_PI_750811023" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit PI&lt;/b&gt;&lt;br&gt;&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_PI?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_PI?&lt;/a&gt;&lt;p&gt;


Created  by  Yingchun 2016-09-22&lt;br&gt;
2016 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:1W-2"/>
</gates>
<devices>
<device name="" package="WE-UNIT_EE16/8/5_1">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="5" pad="1"/>
<connect gate="G$1" pin="6" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UNIT_PI_750811016" prefix="T" uservalue="yes">
<description>&lt;b&gt;Off-Line Transformer WE-Unit PI&lt;/b&gt;&lt;br&gt;&lt;br&gt;

- Nominal input voltage: 85-265 VAC&lt;br&gt;
- Output power 4.2 W &lt;br&gt;
- Operating temperature: -40°C to +125 °C&lt;br&gt;
- Clearance and creepage distance 6 mm min.&lt;br&gt;
- Isolation voltage 4 kVAC&lt;br&gt;&lt;br&gt;

-- Especially designed for several ICs from Power Integrations LNK605&lt;br&gt;
-- Universal input&lt;br&gt;
-- Offline-switch mode power supplies

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/ctm/MID-UNIT%20PI_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/ctm/MID-UNIT_PI?"&gt;http://katalog.we-online.de/en/ctm/MID-UNIT_PI?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_3W:1W-1"/>
</gates>
<devices>
<device name="" package="WE-UNIT_PI_750811016">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="9"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-UOST_SCH-2" prefix="T" uservalue="yes">
<description>&lt;b&gt; WE-UOST Universal Offline Standard Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt; Input voltage range 85–265 VAC (125–375 VDC)
&lt;br&gt;
&lt;br&gt; Output power 12–16 W
&lt;br&gt;
&lt;br&gt; Designed to comply with EN61558-2-16: Reinforced insulation
&lt;br&gt;
&lt;br&gt; Creepage and clearance distance &gt;6.5 mm
&lt;br&gt;
&lt;br&gt; Insulation test voltage 4 kVAC
&lt;br&gt;
&lt;br&gt; For SMD assembly
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; SMPS with power up to 16 W
&lt;br&gt;
&lt;br&gt; Auxiliary power supplies
&lt;br&gt;
&lt;br&gt; Usable with all low power AC/DC ICs like LT3798/99, UCC28610, ViPER &amp; Tiny/Link Switch
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/UtUOST_MID_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/UtUOST_MID_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-UOST?"&gt;http://katalog.we-online.de/en/pbs/WE-UOST?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="TRANSFORMER_4L"/>
</gates>
<devices>
<device name="" package="WE-UOST">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3 4"/>
<connect gate="G$1" pin="4" pad="2"/>
<connect gate="G$1" pin="6" pad="5 6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_760871534"/>
<technology name="_760871543"/>
<technology name="_760875532"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VE_0603" prefix="RV" uservalue="yes">
<description>&lt;b&gt;WE-VE ESD Suppressor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast response time
&lt;br&gt;
&lt;br&gt; No leakage current
&lt;br&gt;
&lt;br&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Almost no energy consumption in stand-by mode
&lt;br&gt;
&lt;br&gt; Excellent absorption for ESD-impulses
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;
&lt;br&gt; Nickel barrier
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection of data lines
&lt;br&gt;
&lt;br&gt; Protection of bus systems
&lt;br&gt;
&lt;br&gt; Protection of semiconductors
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2 – 8 kV contact discharge – 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVE_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVE_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VE?"&gt;http://katalog.we-online.de/en/pbs/WE-VE?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-VE"/>
</gates>
<devices>
<device name="" package="WESURGE_0603_REFLOW">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_82356050050"/>
<technology name="_82356050100"/>
<technology name="_82356050101"/>
<technology name="_82356050220"/>
<technology name="_82356050560"/>
<technology name="_82356120050"/>
<technology name="_82356120100"/>
<technology name="_82356120220"/>
<technology name="_82356120330"/>
<technology name="_82356240030"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VE_0805" prefix="RV" uservalue="yes">
<description>&lt;b&gt;WE-VE ESD Suppressor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast response time
&lt;br&gt;
&lt;br&gt; No leakage current
&lt;br&gt;
&lt;br&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Almost no energy consumption in stand-by mode
&lt;br&gt;
&lt;br&gt; Excellent absorption for ESD-impulses
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;
&lt;br&gt; Nickel barrier
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection of data lines
&lt;br&gt;
&lt;br&gt; Protection of bus systems
&lt;br&gt;
&lt;br&gt; Protection of semiconductors
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2 – 8 kV contact discharge – 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVE_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVE_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VE?"&gt;http://katalog.we-online.de/en/pbs/WE-VE?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-VE"/>
</gates>
<devices>
<device name="" package="WESURGE_0805_REFLOW">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_82350120101"/>
<technology name="_82350120560"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VEA_0612" prefix="RV" uservalue="yes">
<description>&lt;b&gt;WE-VEA ESD Suppressor-Array
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; &lt;br&gt;Fast response time (1 ns)
&lt;br&gt;
&lt;br&gt; Low signal insertion loss
&lt;br&gt;
&lt;br&gt; No leakage current
&lt;br&gt;
&lt;br&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Almost no energy consumption in stand-by mode
&lt;br&gt;
&lt;br&gt; Excellent absorption for ESD-impulses
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection of data lines
&lt;br&gt;
&lt;br&gt; Protection of bus systems
&lt;br&gt;
&lt;br&gt; Protection of video transmission lines
&lt;br&gt;
&lt;br&gt; Protection of semiconductors
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVEA_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVEA_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VEA?"&gt;http://katalog.we-online.de/en/pbs/WE-VEA?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-VEA"/>
</gates>
<devices>
<device name="_82380180121" package="WE-VEA_0612">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="5"/>
<connect gate="G$1" pin="4" pad="7"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="4"/>
<connect gate="G$1" pin="8" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VE_ULC_0603" prefix="D" uservalue="yes">
<description>&lt;b&gt; WE-VE ULC ESD Suppressor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast response time
&lt;br&gt;
&lt;br&gt; No leakage current
&lt;br&gt;
&lt;br&gt; Low clamping voltage
&lt;br&gt;
&lt;br&gt; Almost no energy consumption in stand-by mode
&lt;br&gt;
&lt;br&gt; Excellent absorption for ESD-impulses
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;
&lt;br&gt; Nickel barrier
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection of data lines
&lt;br&gt;
&lt;br&gt; Protection of bus systems
&lt;br&gt;
&lt;br&gt; Protection of semiconductors
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2 – 8 kV contact discharge – 15 kV air discharge
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVE_ULC_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVE_ULC_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VE_ULC?"&gt;http://katalog.we-online.de/en/pbs/WE-VE_ULC?&lt;/a&gt;&lt;p&gt;


Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-VE"/>
</gates>
<devices>
<device name="" package="WE-VE_ULC_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_82306050029"/>
<technology name="_82306120029"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VS_0603" prefix="RV" uservalue="yes">
<description>&lt;b&gt;WE-VS SMD Varistor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast response time
&lt;br&gt;
&lt;br&gt; Low leakage current
&lt;br&gt;
&lt;br&gt; Nickel barrier for leadfree soldering
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection of DC distribution
&lt;br&gt;
&lt;br&gt; Protection of power supply
&lt;br&gt;
&lt;br&gt; Protection of bus systems and communication lines
&lt;br&gt;
&lt;br&gt; Limiting of overvoltages
&lt;br&gt;
&lt;br&gt; Protection of semiconductors
&lt;br&gt;
&lt;br&gt; Surge protection in accordance with EN 61000-4-5
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2
&lt;br&gt;
&lt;br&gt; Burst protection in accordance with EN 61000-4-4
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VS?"&gt;http://katalog.we-online.de/en/pbs/WE-VS?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="VARISTOR"/>
</gates>
<devices>
<device name="_REFLOW" package="WESURGE_0603_REFLOW">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_82536040"/>
<technology name="_82536070"/>
<technology name="_82536110"/>
<technology name="_82536140"/>
<technology name="_82556060"/>
<technology name="_82556140"/>
<technology name="_82556170"/>
<technology name="_82556200"/>
<technology name="_82556250"/>
<technology name="_82556300"/>
</technologies>
</device>
<device name="_WAVE" package="WESURGE_0603_WAVE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_82536040"/>
<technology name="_82536070"/>
<technology name="_82536110"/>
<technology name="_82536140"/>
<technology name="_82556060"/>
<technology name="_82556140"/>
<technology name="_82556170"/>
<technology name="_82556200"/>
<technology name="_82556250"/>
<technology name="_82556300"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VS_0805" prefix="RV" uservalue="yes">
<description>&lt;b&gt;WE-VS SMD Varistor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast response time
&lt;br&gt;
&lt;br&gt; Low leakage current
&lt;br&gt;
&lt;br&gt; Nickel barrier for leadfree soldering
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection of DC distribution
&lt;br&gt;
&lt;br&gt; Protection of power supply
&lt;br&gt;
&lt;br&gt; Protection of bus systems and communication lines
&lt;br&gt;
&lt;br&gt; Limiting of overvoltages
&lt;br&gt;
&lt;br&gt; Protection of semiconductors
&lt;br&gt;
&lt;br&gt; Surge protection in accordance with EN 61000-4-5
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2
&lt;br&gt;
&lt;br&gt; Burst protection in accordance with EN 61000-4-4
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VS?"&gt;http://katalog.we-online.de/en/pbs/WE-VS?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="VARISTOR"/>
</gates>
<devices>
<device name="_REFLOW" package="WESURGE_0805_REFLOW">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_82550040"/>
<technology name="_82550060"/>
<technology name="_82550080"/>
<technology name="_82550110"/>
<technology name="_82550140"/>
<technology name="_82550200"/>
<technology name="_82550250"/>
<technology name="_82550300"/>
<technology name="_82550350"/>
</technologies>
</device>
<device name="_WAVE" package="WESURGE_0805_WAVE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_82550040"/>
<technology name="_82550060"/>
<technology name="_82550080"/>
<technology name="_82550110"/>
<technology name="_82550140"/>
<technology name="_82550200"/>
<technology name="_82550250"/>
<technology name="_82550300"/>
<technology name="_82550350"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-VS_1206" prefix="RV" uservalue="yes">
<description>&lt;b&gt;WE-VS SMD Varistor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Fast response time
&lt;br&gt;
&lt;br&gt; Low leakage current
&lt;br&gt;
&lt;br&gt; Nickel barrier for leadfree soldering
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 ºC to +85 ºC
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Protection of DC distribution
&lt;br&gt;
&lt;br&gt; Protection of power supply
&lt;br&gt;
&lt;br&gt; Protection of bus systems and communication lines
&lt;br&gt;
&lt;br&gt; Limiting of overvoltages
&lt;br&gt;
&lt;br&gt; Protection of semiconductors
&lt;br&gt;
&lt;br&gt; Surge protection in accordance with EN 61000-4-5
&lt;br&gt;
&lt;br&gt; ESD protection in accordance with EN 61000-4-2
&lt;br&gt;
&lt;br&gt; Burst protection in accordance with EN 61000-4-4
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eisos/VarVS_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/eisos/VarVS_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-VS?"&gt;http://katalog.we-online.de/en/pbs/WE-VS?&lt;/a&gt;&lt;p&gt;

Updated  by  Dan Xu 2014-07-11&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="VARISTOR"/>
</gates>
<devices>
<device name="_REFLOW" package="WESURGE_1206_REFLOW">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_82531040"/>
<technology name="_82531140"/>
<technology name="_82531400"/>
<technology name="_82541110"/>
<technology name="_82541140"/>
<technology name="_82541250"/>
<technology name="_82541300"/>
<technology name="_82541350"/>
<technology name="_82551140"/>
<technology name="_82551170"/>
<technology name="_82551200"/>
<technology name="_82551250"/>
<technology name="_82551300"/>
<technology name="_82551500"/>
<technology name="_82551600"/>
</technologies>
</device>
<device name="_WAVE" package="WESURGE_1206_WAVE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_82531040"/>
<technology name="_82531140"/>
<technology name="_82531400"/>
<technology name="_82541110"/>
<technology name="_82541140"/>
<technology name="_82541250"/>
<technology name="_82541300"/>
<technology name="_82541350"/>
<technology name="_82551140"/>
<technology name="_82551170"/>
<technology name="_82551200"/>
<technology name="_82551250"/>
<technology name="_82551300"/>
<technology name="_82551500"/>
<technology name="_82551600"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LAN_AQ_749010310" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-LAN AQ 10/100 Base-T SMD Transformer 1 Port&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;100 % machine production
&lt;br&gt;High performance return loss and crosstalk
&lt;br&gt;Improved solderability through half vias
&lt;br&gt;Reduced height (4 mm)
&lt;br&gt;Compatible to standard products

&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;Compatible to industrial ethernet systems like EtherCAT or Profinet
&lt;br&gt;IoT applications
&lt;br&gt;Hubs, routers, switches, IPcameras 
&lt;br&gt;Company networks
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-LAN_AQ_7490x0310_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-LAN_AQ_7490x0310_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-LANAQ/749010310?m"&gt;http://katalog.we-online.de/en/pbs/WE-LANAQ/749010310?m&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2017 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LAN_AQ_749010310"/>
</gates>
<devices>
<device name="" package="WE-LAN_AQ_749010310">
<connects>
<connect gate="G$1" pin="CRD" pad="7"/>
<connect gate="G$1" pin="CRX" pad="10"/>
<connect gate="G$1" pin="CTD" pad="2"/>
<connect gate="G$1" pin="CTX" pad="15"/>
<connect gate="G$1" pin="RD+" pad="6"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="RX+" pad="11"/>
<connect gate="G$1" pin="RX-" pad="9"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
<connect gate="G$1" pin="TX+" pad="16"/>
<connect gate="G$1" pin="TX-" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEXHV_EFD15" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-FLEX HV Flexible Transformer for DC/DC Converter&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;Transformer with 6 identical windings
&lt;br&gt;4 sizes with 5 different lengths of air gap each
&lt;br&gt;Isolation voltage up to 1.5 kVAC
&lt;br&gt;Low leakage inductance
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;By using different circuits more than 375 transformer solutions and about 125 choke solutions possible. Consequently, quick prototyping possibilities
&lt;br&gt;EFD size parts provide Basic insulation for a working voltage of 250VRMS when they are connteced approbiate


&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;Flyback converters
&lt;br&gt;Forward converters
&lt;br&gt;Push-pull converters
&lt;br&gt;&lt;br&gt;Step-up/step-down converters
SEPIC

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FLEXHV/749196308?m"&gt;http://katalog.we-online.de/en/pbs/WE-FLEXHV/749196308?m&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2017 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-FLEXHV_EFD"/>
</gates>
<devices>
<device name="" package="WE-FLEXHV_EFD15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_749196308">
<attribute name="WE-NUMBER" value="749196308/153,8uH"/>
</technology>
<technology name="_749196318">
<attribute name="WE-NUMBER" value="749496318/23,3uH"/>
</technology>
<technology name="_749196328">
<attribute name="WE-NUMBER" value="749196328/14,2uH"/>
</technology>
<technology name="_749196338">
<attribute name="WE-NUMBER" value="749496338/9,3uH"/>
</technology>
<technology name="_749196348">
<attribute name="WE-NUMBER" value="749196348/7,9uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEXHV_EFD20" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-FLEX HV Flexible Transformer for DC/DC Converter&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;Transformer with 6 identical windings
&lt;br&gt;4 sizes with 5 different lengths of air gap each
&lt;br&gt;Isolation voltage up to 1.5 kVAC
&lt;br&gt;Low leakage inductance
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;By using different circuits more than 375 transformer solutions and about 125 choke solutions possible. Consequently, quick prototyping possibilities
&lt;br&gt;EFD size parts provide Basic insulation for a working voltage of 250VRMS when they are connteced approbiate


&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;Flyback converters
&lt;br&gt;Forward converters
&lt;br&gt;Push-pull converters
&lt;br&gt;&lt;br&gt;Step-up/step-down converters
SEPIC

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FLEXHV/749196308?m"&gt;http://katalog.we-online.de/en/pbs/WE-FLEXHV/749196308?m&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2017 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-FLEXHV_EFD"/>
</gates>
<devices>
<device name="" package="WE-FLEXHV_EFD20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_749196507">
<attribute name="WE-NUMBER" value="749196507/0,18uH"/>
</technology>
<technology name="_749196508">
<attribute name="WE-NUMBER" value="749196508/0,24uH"/>
</technology>
<technology name="_749196517">
<attribute name="WE-NUMBER" value="749196517/0,18uH"/>
</technology>
<technology name="_749196518">
<attribute name="WE-NUMBER" value="749196518/0,24uH"/>
</technology>
<technology name="_749196527">
<attribute name="WE-NUMBER" value="749196527/0,18uH"/>
</technology>
<technology name="_749196528">
<attribute name="WE-NUMBER" value="749096528/0,24uH"/>
</technology>
<technology name="_749196537">
<attribute name="WE-NUMBER" value="749196537/0,18uH"/>
</technology>
<technology name="_749196538">
<attribute name="WE-NUMBER" value="749196538/0,24uH"/>
</technology>
<technology name="_749196547">
<attribute name="WE-NUMBER" value="749196547/0,18uH"/>
</technology>
<technology name="_749196548">
<attribute name="WE-NUMBER" value="749196548/0,24uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEXHV_ER11/5" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-FLEX HV Flexible Transformer for DC/DC Converter&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;Transformer with 6 identical windings
&lt;br&gt;4 sizes with 5 different lengths of air gap each
&lt;br&gt;Isolation voltage up to 1.5 kVAC
&lt;br&gt;Low leakage inductance
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;By using different circuits more than 375 transformer solutions and about 125 choke solutions possible. Consequently, quick prototyping possibilities
&lt;br&gt;EFD size parts provide Basic insulation for a working voltage of 250VRMS when they are connteced approbiate


&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;Flyback converters
&lt;br&gt;Forward converters
&lt;br&gt;Push-pull converters
&lt;br&gt;&lt;br&gt;Step-up/step-down converters
SEPIC

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FLEXHV/749196308?m"&gt;http://katalog.we-online.de/en/pbs/WE-FLEXHV/749196308?m&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2017 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-FLEXHV_ER"/>
</gates>
<devices>
<device name="" package="WE-FLEXHV_ER11/5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_749196108">
<attribute name="WE-NUMBER" value="749196108/224,6uH"/>
</technology>
<technology name="_749196118">
<attribute name="WE-NUMBER" value="749196118/27,4uH"/>
</technology>
<technology name="_749196128">
<attribute name="WE-NUMBER" value="749196128/14,7uH"/>
</technology>
<technology name="_749196138">
<attribute name="WE-NUMBER" value="749196138/10,9uH"/>
</technology>
<technology name="_749196148">
<attribute name="WE-NUMBER" value="749196148/8,5uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-FLEXHV_ER14.5/6" prefix="T" uservalue="yes">
<description>&lt;b&gt;WE-FLEX HV Flexible Transformer for DC/DC Converter&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;Transformer with 6 identical windings
&lt;br&gt;4 sizes with 5 different lengths of air gap each
&lt;br&gt;Isolation voltage up to 1.5 kVAC
&lt;br&gt;Low leakage inductance
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;By using different circuits more than 375 transformer solutions and about 125 choke solutions possible. Consequently, quick prototyping possibilities
&lt;br&gt;EFD size parts provide Basic insulation for a working voltage of 250VRMS when they are connteced approbiate


&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;Flyback converters
&lt;br&gt;Forward converters
&lt;br&gt;Push-pull converters
&lt;br&gt;&lt;br&gt;Step-up/step-down converters
SEPIC

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-FLEX_HV_749196xxx_4C_NEU.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-FLEXHV/749196308?m"&gt;http://katalog.we-online.de/en/pbs/WE-FLEXHV/749196308?m&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2017 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-FLEXHV_ER"/>
</gates>
<devices>
<device name="" package="WE-FLEXHV_ER14.5/6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="_749196208">
<attribute name="WE-NUMBER" value="749196208/165uH"/>
</technology>
<technology name="_749196218">
<attribute name="WE-NUMBER" value="749196218/21,6uH"/>
</technology>
<technology name="_749196228">
<attribute name="WE-NUMBER" value="749196228/11,6uH"/>
</technology>
<technology name="_749196238">
<attribute name="WE-NUMBER" value="749196238/8,3uH"/>
</technology>
<technology name="_749196248">
<attribute name="WE-NUMBER" value="749196248/6,6uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-ACHC_1010" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-ACHC High current air coil&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;High quality factor Q
&lt;br&gt;Hight currents
&lt;br&gt;Inductance tolerances +-20 %
&lt;br&gt;Operating temperature: -40 °C to +125 °C
&lt;br&gt;


&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;High power filter
&lt;br&gt;RF-Voltage regulator
&lt;br&gt;High current applications

&lt;br&gt;SEPIC

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-AC_HC_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-AC_HC_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-ACHC/7449150023?m"&gt;http://katalog.we-online.de/en/pbs/WE-ACHC/7449150023?m&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2017 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-ACHC_1010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7449150023">
<attribute name="WE-NUMBER" value="7449150023/23nH"/>
</technology>
<technology name="_7449150046">
<attribute name="WE-NUMBER" value="7449150046/46,5nH"/>
</technology>
<technology name="_7449150079">
<attribute name="WE-NUMBER" value="7449150079/79nH"/>
</technology>
<technology name="_7449150111">
<attribute name="WE-NUMBER" value="7449150111/111nH"/>
</technology>
<technology name="_7449150146">
<attribute name="WE-NUMBER" value="7449150146/146nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-ACHC_1212" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-ACHC High current air coil&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;High quality factor Q
&lt;br&gt;Hight currents
&lt;br&gt;Inductance tolerances +-20 %
&lt;br&gt;Operating temperature: -40 °C to +125 °C
&lt;br&gt;


&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;High power filter
&lt;br&gt;RF-Voltage regulator
&lt;br&gt;High current applications

&lt;br&gt;SEPIC

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-AC_HC_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-AC_HC_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-ACHC/7449150023?m"&gt;http://katalog.we-online.de/en/pbs/WE-ACHC/7449150023?m&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Created by Yingchun Shan &lt;br&gt;
2017 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-ACHC_1212">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7449152022">
<attribute name="WE-NUMBER" value="7449152022/22nH"/>
</technology>
<technology name="_7449152042">
<attribute name="WE-NUMBER" value="7449152042/42nH"/>
</technology>
<technology name="_7449152066">
<attribute name="WE-NUMBER" value="7449152066/66nH"/>
</technology>
<technology name="_7449152090">
<attribute name="WE-NUMBER" value="7449152090/90nH"/>
</technology>
<technology name="_7449152111">
<attribute name="WE-NUMBER" value="7449152111/117nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DPC_HV_5030" prefix="L" uservalue="yes">
<description>&lt;b&gt;WE-DPC HV SMD Dual Powerchokel&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;Our smallest double choke with 1.5kV isolation
&lt;br&gt;Magnetical shielded
&lt;br&gt;1:1 Transformer
&lt;br&gt;Coupled miniature inductor with two identical windings
&lt;br&gt;Operation temperature: -40 °C to +125 °C

&lt;br&gt;


&lt;br&gt;
&lt;br&gt;&lt;B&gt;Applications &lt;/B&gt;
&lt;br&gt;High density Isolated converter application (i.e Flyback converter) 
&lt;br&gt;Buck, Boost, Sepic, Zeta, CUK Converter
&lt;br&gt;Can be used as single inductor with series and parallel connection


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-DPC_HV_5030.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-DPC_HV_5030.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-DPCHV/7448841010?m"&gt;http://katalog.we-online.de/en/pbs/WE-DPCHV/7448841010?m&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;updated by Yingchun Shan 2017-07-18 &lt;br&gt;

2017 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DPC_HV"/>
</gates>
<devices>
<device name="" package="WE-DPC_HV_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_7448841010">
<attribute name="WE-NUMBER" value="7448841010/1uH"/>
</technology>
<technology name="_7448841015">
<attribute name="WE-NUMBER" value="7448841015/1,5uH"/>
</technology>
<technology name="_7448841022">
<attribute name="WE-NUMBER" value="7448841022/2,2uH"/>
</technology>
<technology name="_7448841033">
<attribute name="WE-NUMBER" value="7448841033/3,3uH"/>
</technology>
<technology name="_7448841047">
<attribute name="WE-NUMBER" value="7448841047/4,7uH"/>
</technology>
<technology name="_7448841068">
<attribute name="WE-NUMBER" value="7448841068/6,8uH"/>
</technology>
<technology name="_7448841082">
<attribute name="WE-NUMBER" value="7448841082/8,2uH"/>
</technology>
<technology name="_7448841100">
<attribute name="WE-NUMBER" value="7448841100/10uH"/>
</technology>
<technology name="_7448841150">
<attribute name="WE-NUMBER" value="7448841150/15uH"/>
</technology>
<technology name="_7448841220">
<attribute name="WE-NUMBER" value="7448841220/22uH"/>
</technology>
<technology name="_7448841330">
<attribute name="WE-NUMBER" value="7448841330/33uH"/>
</technology>
<technology name="_7448841470">
<attribute name="WE-NUMBER" value="7448841470/47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCF_2815" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD High Current Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Saturation current up to 75 A
&lt;br&gt;
&lt;br&gt; Very low core losses (MnZn)
&lt;br&gt;
&lt;br&gt; Magnetically shielded
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt; Current capability up to 32 A
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Storage inductor for high efficiency DC/DC converters
&lt;br&gt;
&lt;br&gt; Single and polyphase buck converters
&lt;br&gt;
&lt;br&gt; Filter for audio applications
&lt;br&gt;
&lt;br&gt; Optimized for high current boost applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_we-hcf_smd_hochstrominduktivitaet_11.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_we-hcf_smd_hochstrominduktivitaet_11.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-HCF#vs_ct:1"&gt;http://katalog.we-online.de/en/pbs/WE-HCF#vs_ct:1&lt;/a&gt;&lt;p&gt;


Updated by  Dan Xu 2014-07-07&lt;br&gt;
2014 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCF_2815">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74436410150">
<attribute name="WE-NUMBER" value="74436410150/1,5uH"/>
</technology>
<technology name="_74436410220">
<attribute name="WE-NUMBER" value="74436410220/2,2uH"/>
</technology>
<technology name="_74436410330">
<attribute name="WE-NUMBER" value="74436410330/3,3uH"/>
</technology>
<technology name="_74436410470">
<attribute name="WE-NUMBER" value="74436410470/4,7uH"/>
</technology>
<technology name="_74436410680">
<attribute name="WE-NUMBER" value="74436410680/6,8uH"/>
</technology>
<technology name="_74436411000">
<attribute name="WE-NUMBER" value="74436411000/10uH"/>
</technology>
<technology name="_74436411500">
<attribute name="WE-NUMBER" value="74436411500/15uH"/>
</technology>
<technology name="_74436412200">
<attribute name="WE-NUMBER" value="74436412200/22uH"/>
</technology>
<technology name="_74436413300">
<attribute name="WE-NUMBER" value="74436413300/33uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD2_3521" prefix="L" uservalue="yes">
<description>&lt;b&gt;SMD Power Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Open size
&lt;br&gt;
&lt;br&gt; Saturation currents up to 14 A
&lt;br&gt;
&lt;br&gt; Low tolerances at high inductance values
&lt;br&gt;
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Integrated DC/DC-converter
&lt;br&gt;
&lt;br&gt; Switching regulators with low operating voltages (Graphic cards, embedded PC-Cards, Mainboards)
&lt;br&gt;
&lt;br&gt; Optimal attenuation in MHz frequency range
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-PD2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-PD2"&gt;http://katalog.we-online.de/en/pbs/WE-PD2&lt;/a&gt;&lt;p&gt;


Created  by Yingchun Shan&lt;br&gt;
2017(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2_3521">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447732010">
<attribute name="WE-NUMBER" value="7447732010/1uH"/>
</technology>
<technology name="_7447732015">
<attribute name="WE-NUMBER" value="7447732015/1,5uH"/>
</technology>
<technology name="_7447732022">
<attribute name="WE-NUMBER" value="7447732022/2,2uH"/>
</technology>
<technology name="_7447732033">
<attribute name="WE-NUMBER" value="7447732033/3,3uH"/>
</technology>
<technology name="_7447732047">
<attribute name="WE-NUMBER" value="7447732047/4,7uH"/>
</technology>
<technology name="_7447732068">
<attribute name="WE-NUMBER" value="7447732068/6,8uH"/>
</technology>
<technology name="_7447732110">
<attribute name="WE-NUMBER" value="7447732110/10uH"/>
</technology>
<technology name="_7447732115">
<attribute name="WE-NUMBER" value="7447732115/15uH"/>
</technology>
<technology name="_7447732122">
<attribute name="WE-NUMBER" value="7447732122/22uH"/>
</technology>
<technology name="_7447732133">
<attribute name="WE-NUMBER" value="7447732133/33uH"/>
</technology>
<technology name="_7447732147">
<attribute name="WE-NUMBER" value="7447732147/47uH"/>
</technology>
<technology name="_7447732168">
<attribute name="WE-NUMBER" value="7447732168/68uH"/>
</technology>
<technology name="_7447732210">
<attribute name="WE-NUMBER" value="7447732210/100uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-DPC_5838" prefix="L" uservalue="yes">
<description>&lt;b&gt; WE-DPC SMD Dual Powerchoke
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Characteristics Tiny package: our smalles double choke
&lt;br&gt;Magnetical shielded
&lt;br&gt;1:1 transformer
&lt;br&gt;Coupled miniature inductor with two identical windings
&lt;br&gt;More variants due to parallel and series connection
&lt;br&gt;Operating temperature: -40 °C to +125 °C

&lt;br&gt; 

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Applications Flyback applications
&lt;br&gt;Buck, Boost, Sepic, Zeta, CUK Converter
&lt;br&gt;Switching regulators with secondary unregulated output voltage
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;


&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/v2/Family_WE-DPC_5838_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/images/v2/Family_WE-DPC_5838_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-DPC"&gt;http://katalog.we-online.de/en/pbs/WE-DPC&lt;/a&gt;&lt;p&gt;

&lt;BR&gt;Created by Yingchun,Shan 2017-05-26&lt;br&gt;
2017(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-DPC"/>
</gates>
<devices>
<device name="" package="WE-DPC_5838">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_7448844010">
<attribute name="WE-NUMBER" value="7448844010/1uH"/>
</technology>
<technology name="_7448844100">
<attribute name="WE-NUMBER" value="7448844100/10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
