(module ebay_usb (layer F.Cu) (tedit 5CA802EF)
  (descr "USB Micro-B receptacle, http://www.mouser.com/ds/2/445/629105150521-469306.pdf")
  (tags "usb micro receptacle")
  (attr smd)
  (fp_text reference REF** (at 0 -3.5) (layer F.SilkS))
  (fp_text value superiorbuy2014_usb#3 (at 0 5.6) (layer F.Fab))
  (fp_text user %R (at 0 1.05) (layer F.Fab))
  (fp_text user "PCB Edge" (at 0 3.75) (layer Dwgs.User))
  (pad 7 thru_hole circle (at 2 -0.415) (size 0.6 0.6) (drill 0.55) (layers *.Cu))
  (pad 7 thru_hole circle (at -2 -0.415) (size 0.6 0.6) (drill 0.55) (layers *.Cu))
  (pad 1 smd rect (at -1.3 -1.425) (size 0.4 2.15) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.65 -1.425) (size 0.4 2.15) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0 -1.425) (size 0.4 2.15) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.65 -1.425) (size 0.4 2.15) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.3 -1.425) (size 0.4 2.15) (layers F.Cu F.Paste F.Mask))
  (pad 6 thru_hole oval (at -3.6 -1.735) (size 1.5 2) (drill oval 0.5 1.2) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 3.6 -1.735) (size 1.5 2) (drill oval 0.5 1.2) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at -3.6 1.735) (size 1.5 2) (drill oval 0.5 1.2) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 3.6 1.735) (size 1.5 2) (drill oval 0.5 1.2) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Wuerth_629105150521.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
