(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 36)
    (tracks 1045)
    (zones 0)
    (modules 66)
    (nets 46)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.1)
    (user_trace_width 0.152)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.01)
    (segment_width 1)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.75 2.75)
    (pad_drill 2.75)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFCFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "meta/"))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 /GND_PI)
  (net 3 /VCC3)
  (net 4 GND)
  (net 5 /VDP)
  (net 6 "Net-(CFG1001-Pad1)")
  (net 7 /BUS+)
  (net 8 /VB+)
  (net 9 /TXD_TPUART)
  (net 10 /TXD_PI)
  (net 11 /RXD_PI)
  (net 12 "Net-(IC10-Pad13)")
  (net 13 /STXO)
  (net 14 +5V)
  (net 15 "Net-(K1-Pad27)")
  (net 16 "Net-(K1-Pad28)")
  (net 17 "Net-(LED_PI1-Pad2)")
  (net 18 "Net-(LED_STXO1-Pad2)")
  (net 19 "Net-(LED_TPUART1-Pad2)")
  (net 20 /RXD_TPUART)
  (net 21 "Net-(LED_STXO1-Pad1)")
  (net 22 "Net-(C40-Pad1)")
  (net 23 "Net-(IC40-Pad1)")
  (net 24 "Net-(DIS1-Pad1)")
  (net 25 "Net-(LED_SUP1-Pad2)")
  (net 26 /VCC5_BOOST)
  (net 27 /SOFTSTART)
  (net 28 /BOOST_30V)
  (net 29 /GYRA_C)
  (net 30 /GYRA_E)
  (net 31 /SW)
  (net 32 /DROSSEL_IN)
  (net 33 /FB)
  (net 34 /FREQ)
  (net 35 /GYRA_B)
  (net 36 /COMP)
  (net 37 /COMP1)
  (net 38 /VDDH)
  (net 39 /VSSH)
  (net 40 /BYP)
  (net 41 /RXIN)
  (net 42 /IND)
  (net 43 /X1)
  (net 44 /X2)
  (net 45 "Net-(IC40-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /BOOST_30V)
    (add_net /BUS+)
    (add_net /BYP)
    (add_net /COMP)
    (add_net /COMP1)
    (add_net /DROSSEL_IN)
    (add_net /FB)
    (add_net /FREQ)
    (add_net /GND_PI)
    (add_net /GYRA_B)
    (add_net /GYRA_C)
    (add_net /GYRA_E)
    (add_net /IND)
    (add_net /RXD_PI)
    (add_net /RXD_TPUART)
    (add_net /RXIN)
    (add_net /SOFTSTART)
    (add_net /STXO)
    (add_net /SW)
    (add_net /TXD_PI)
    (add_net /TXD_TPUART)
    (add_net /VB+)
    (add_net /VCC3)
    (add_net /VCC5_BOOST)
    (add_net /VDDH)
    (add_net /VDP)
    (add_net /VSSH)
    (add_net /X1)
    (add_net /X2)
    (add_net GND)
    (add_net "Net-(C40-Pad1)")
    (add_net "Net-(CFG1001-Pad1)")
    (add_net "Net-(DIS1-Pad1)")
    (add_net "Net-(IC10-Pad13)")
    (add_net "Net-(IC40-Pad1)")
    (add_net "Net-(IC40-Pad7)")
    (add_net "Net-(K1-Pad27)")
    (add_net "Net-(K1-Pad28)")
    (add_net "Net-(LED_PI1-Pad2)")
    (add_net "Net-(LED_STXO1-Pad1)")
    (add_net "Net-(LED_STXO1-Pad2)")
    (add_net "Net-(LED_SUP1-Pad2)")
    (add_net "Net-(LED_TPUART1-Pad2)")
  )
  (module Kalassi:Recom_R1SE_5-pin (layer F.Cu) (tedit 5C93F145)
    (at 88.2 53.4 270)
    (fp_text reference IC45 (at 0.8 -6.3 270) (layer F.SilkS))
    (fp_text value R1SE-Kalassi (at -0.1 -0.1 270) (layer F.Fab))
    (pad 8 smd rect (at -3.81 -5.1 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 3.81 -5.1 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 26 /VCC5_BOOST))
    (pad 4 smd rect (at 3.81 5.1 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.27 5.1 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC40-Pad1)"))
    (pad 1 smd rect (at -3.81 5.1 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND_PI))
    (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_RECOM_R1S_SMD.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Kalassi:C0603 (layer F.Cu) (tedit 5C60989B)
    (at 108.6 40.8)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C1 (at -2.3 0) (layer F.SilkS))
    (fp_text value 100nF (at 0.75 1.75) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3) (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND_PI) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_6.3x5.4 (layer F.Cu) (tedit 5BCA39D0)
    (at 125.6 57 90)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic C55, 6.3x5.4mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C19 (at 4.4 2.6 180) (layer F.SilkS))
    (fp_text value CP (at 0 4.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2.8 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 38 /VDDH))
    (pad 2 smd roundrect (at 2.8 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_6.3x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217C7B)
    (at 136.6 36.875)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CCB)
    (at 136.6 85.875)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CB9)
    (at 78.6 85.875)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CA2)
    (at 78.6 36.875)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module Kalassi:KNX (layer F.Cu) (tedit 5CAC53A3)
    (at 133.4 57.6 90)
    (attr virtual)
    (fp_text reference BUS1 (at -0.6 4.9 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 3.81 90) (layer F.Fab))
    (fp_text user VB- (at -2.81 2 90) (layer F.SilkS))
    (fp_text user VB+ (at 2.78 2 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.6 0 90) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Mask)
      (net 7 /BUS+))
    (pad 1 thru_hole circle (at -3.4 0 90) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector.3dshapes/243-211-1.stp
      (offset (xyz -5.8 3.4 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Kalassi:C0603 (layer F.Cu) (tedit 5C60989B)
    (at 93.2 44.2 270)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C4 (at 0.25 -1.75 270) (layer F.SilkS))
    (fp_text value 47nF/50V (at 0.75 1.75 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND_PI) (solder_paste_margin_ratio -0.05))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:C0603 (layer F.Cu) (tedit 5C60989B)
    (at 104.4 43.8 270)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C5 (at -2.5 0.1 270) (layer F.SilkS))
    (fp_text value 47nF/50V (at 0.75 1.75 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC3) (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:C0603 (layer F.Cu) (tedit 5C60989B)
    (at 110 57.4 90)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C10 (at 0.1 1.5 90) (layer F.SilkS))
    (fp_text value 220n (at 0.75 1.75 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /VDP) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:C0603 (layer F.Cu) (tedit 5C60989B)
    (at 110 64.4 270)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C11 (at 0.25 -1.75 270) (layer F.SilkS))
    (fp_text value 220n (at 0.75 1.75 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 38 /VDDH) (solder_paste_margin_ratio -0.05))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 39 /VSSH) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_5x5.9 (layer F.Cu) (tedit 5BCA39CF)
    (at 123.6 65.2)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic B6, 5.0x5.9mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C13 (at 0 -3.7) (layer F.SilkS))
    (fp_text value CP (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.2 0) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 3 /VCC3))
    (pad 2 smd roundrect (at 2.2 0) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_5x5.9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:C0603 (layer F.Cu) (tedit 5C60989B)
    (at 128.2 62 270)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C15 (at 0.1 -1.2 270) (layer F.SilkS))
    (fp_text value 47nF/50V (at 0.75 1.75 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 38 /VDDH) (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:C1206 (layer F.Cu) (tedit 5C609920)
    (at 106 55 90)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C16 (at 0 1.7 270) (layer F.SilkS))
    (fp_text value 47n/50V (at 0.75 1.75 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.4 0 90) (size 1.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 8 /VB+) (solder_paste_margin_ratio -0.05))
    (pad 1 smd rect (at -1.4 0 90) (size 1.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 40 /BYP) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:C1206 (layer F.Cu) (tedit 5C609920)
    (at 103.6 55 90)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C17 (at -3.1 0.1 180) (layer F.SilkS))
    (fp_text value 47n/50V (at 0.75 1.75 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.4 0 90) (size 1.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 41 /RXIN) (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 1.4 0 90) (size 1.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 8 /VB+) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:C0603 (layer F.Cu) (tedit 5C60989B)
    (at 121.2 55.6 270)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C18 (at -0.9 1 270) (layer F.SilkS))
    (fp_text value 10n (at 0.75 1.75 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.05))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC3) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 137 44.2)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference CFG1001 (at 0 -2.33) (layer F.SilkS))
    (fp_text value PIN2_100 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(CFG1001-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND_PI))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:SOT23 (layer F.Cu) (tedit 5C603EDA)
    (at 107.8 44 90)
    (descr SOT-23)
    (tags "SOT23 IPC")
    (fp_text reference D1 (at 2.3 0.8 180) (layer F.SilkS))
    (fp_text value BAS70-06 (at -2.2 -0.4 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0.95 -1.1 90) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /VB+))
    (pad 3 smd rect (at 0 1.1 90) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /BUS+))
    (pad 2 smd rect (at -0.95 -1.1 90) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /VB+))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Diodes_SMD:D_SMA (layer F.Cu) (tedit 586432E5)
    (at 134.2 65.8)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D10 (at 4.3 0.1 90) (layer F.SilkS))
    (fp_text value D_TVS (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 /BUS+))
    (pad 2 smd rect (at 2 0) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:SO8 (layer F.Cu) (tedit 0)
    (at 99.6 44.2 270)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference IC2 (at 3.4 0.1) (layer F.SilkS))
    (fp_text value ADUM1201SOIC8 (at 0 0 270) (layer F.Fab))
    (pad 8 smd oval (at -1.905 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC3))
    (pad 7 smd oval (at -0.635 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 9 /TXD_TPUART))
    (pad 6 smd oval (at 0.635 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 20 /RXD_TPUART))
    (pad 5 smd oval (at 1.905 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 4 smd oval (at 1.905 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND_PI))
    (pad 3 smd oval (at 0.635 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 10 /TXD_PI))
    (pad 2 smd oval (at -0.635 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 11 /RXD_PI))
    (pad 1 smd oval (at -1.905 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
  )
  (module Kalassi:QFN36ePad (layer F.Cu) (tedit 5C603F63)
    (at 116.6 58.6)
    (fp_text reference IC10 (at 0 -1.5) (layer F.SilkS))
    (fp_text value TPUART2QFN (at 0 1.5 90) (layer F.Fab))
    (pad 1 smd oval (at -2 3) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin -0.01))
    (pad 2 smd oval (at -1.5 3) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin -0.01))
    (pad 3 smd oval (at -1 3) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin -0.01))
    (pad 4 smd oval (at -0.5 3) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 38 /VDDH) (solder_paste_margin -0.01))
    (pad 5 smd oval (at 0 3) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 39 /VSSH) (solder_paste_margin -0.01))
    (pad 6 smd oval (at 0.5 3) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 38 /VDDH) (solder_paste_margin -0.01))
    (pad 7 smd oval (at 1 3) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin -0.01))
    (pad 8 smd oval (at 1.5 3) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC3) (solder_paste_margin -0.01))
    (pad 9 smd oval (at 2 3) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 42 /IND) (solder_paste_margin -0.01))
    (pad 10 smd oval (at 3 2 90) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin -0.01))
    (pad 11 smd oval (at 3 1.5 90) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 8 /VB+) (solder_paste_margin -0.01))
    (pad 12 smd oval (at 3 1 90) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 40 /BYP) (solder_paste_margin -0.01))
    (pad 13 smd oval (at 3 0.5 90) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC10-Pad13)") (solder_paste_margin -0.01))
    (pad 14 smd oval (at 3 0 90) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 13 /STXO) (solder_paste_margin -0.01))
    (pad 15 smd oval (at 3 -0.5 90) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 41 /RXIN) (solder_paste_margin -0.01))
    (pad 16 smd oval (at 3 -1 90) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin -0.01))
    (pad 17 smd oval (at 3 -1.5 90) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC3) (solder_paste_margin -0.01))
    (pad 18 smd oval (at 3 -2 90) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin -0.01))
    (pad 22 smd oval (at 0.5 -3 180) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin -0.01))
    (pad 19 smd oval (at 2 -3 180) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin -0.01))
    (pad 21 smd oval (at 1 -3 180) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 9 /TXD_TPUART) (solder_paste_margin -0.01))
    (pad 20 smd oval (at 1.5 -3 180) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 20 /RXD_TPUART) (solder_paste_margin -0.01))
    (pad 23 smd oval (at 0 -3 180) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 43 /X1) (solder_paste_margin -0.01))
    (pad 26 smd oval (at -1.5 -3 180) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin -0.01))
    (pad 24 smd oval (at -0.5 -3 180) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 44 /X2) (solder_paste_margin -0.01))
    (pad 25 smd oval (at -1 -3 180) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 5 /VDP) (solder_paste_margin -0.01))
    (pad 27 smd oval (at -2 -3 180) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin -0.01))
    (pad 31 smd oval (at -3 -0.5 270) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin -0.01))
    (pad 28 smd oval (at -3 -2 270) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 5 /VDP) (solder_paste_margin -0.01))
    (pad 29 smd oval (at -3 -1.5 270) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin -0.01))
    (pad 30 smd oval (at -3 -1 270) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 5 /VDP) (solder_paste_margin -0.01))
    (pad 32 smd oval (at -3 0 270) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin -0.01))
    (pad 35 smd oval (at -3 1.5 270) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 5 /VDP) (solder_paste_margin -0.01))
    (pad 33 smd oval (at -3 0.5 270) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin -0.01))
    (pad 34 smd oval (at -3 1 270) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 5 /VDP) (solder_paste_margin -0.01))
    (pad 36 smd oval (at -3 2 270) (size 0.28 0.94) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin -0.01))
    (pad 37 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 37 thru_hole circle (at 0.7 0.7) (size 1 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 37 thru_hole circle (at -0.7 0.7) (size 1 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 37 thru_hole circle (at -0.7 -0.7) (size 1 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 37 thru_hole circle (at 0.7 -0.7) (size 1 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-36-1EP_6x6mm_P0.5mm_EP3.7x3.7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm locked (layer F.Cu) (tedit 59650533)
    (at 83.425 38.225 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference K1 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value PIN20X2 (at 1.27 50.59 90) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 +5V))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND_PI))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /TXD_PI))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND_PI))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /RXD_PI))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND_PI))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND_PI))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND_PI))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(K1-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(K1-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND_PI))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND_PI))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND_PI))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:L4532M (layer F.Cu) (tedit 5C609A38)
    (at 115.8 65.6)
    (descr INDUCTOR)
    (tags "INDUCTOR IPC")
    (attr smd)
    (fp_text reference L10 (at -2 -2.6) (layer F.SilkS))
    (fp_text value 220uH (at -1.2 2.8) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.9 0) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC3) (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 1.9 0) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 42 /IND) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:R0603 (layer F.Cu) (tedit 5C609595)
    (at 124.8 43.2 90)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R1 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value 3k9 (at 0.75 1.75 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3) (solder_paste_margin_ratio -0.05))
    (pad 1 smd rect (at -0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(K1-Pad28)") (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:R0603 (layer F.Cu) (tedit 5C609595)
    (at 127.2 43.2 90)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R2 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value 3k9 (at 0.75 1.75 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(K1-Pad27)") (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:R0603 (layer F.Cu) (tedit 5C609595)
    (at 129.6 43.2 90)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R3 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value 1k (at 0.75 1.75 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3) (solder_paste_margin_ratio -0.05))
    (pad 1 smd rect (at -0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CFG1001-Pad1)") (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:R0603 (layer F.Cu) (tedit 5C609595)
    (at 122.5 43.2 90)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R4 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value 3k9 (at 0.75 1.75 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC3) (solder_paste_margin_ratio -0.05))
    (pad 1 smd rect (at -0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(LED_STXO1-Pad2)") (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:R0603 (layer F.Cu) (tedit 5C609595)
    (at 105.6 50.6 90)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R5 (at 0.25 -1.75 90) (layer F.SilkS))
    (fp_text value 3k9 (at 0.75 1.75 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(LED_TPUART1-Pad2)") (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC3) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:R0603 (layer F.Cu) (tedit 5C609595)
    (at 132 43.2 90)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R6 (at 2.2 0 90) (layer F.SilkS))
    (fp_text value 3k9 (at 0.75 1.75 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(LED_PI1-Pad2)") (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2010 (layer F.Cu) (tedit 5415D342)
    (at 100.4 54.2 270)
    (descr "Resistor SMD 2010, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2010")
    (attr smd)
    (fp_text reference R11 (at -0.1 2.4 270) (layer F.SilkS))
    (fp_text value 68Ohm/1W (at 0 2.7 270) (layer F.Fab))
    (pad 1 smd rect (at -2.45 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 /VB+))
    (pad 2 smd rect (at 2.45 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC10-Pad13)"))
    (model Resistors_SMD.3dshapes/R_2010.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:SOT23 (layer F.Cu) (tedit 5C603EDA)
    (at 109.8 71)
    (descr SOT-23)
    (tags "SOT23 IPC")
    (fp_text reference T1 (at 2.2 -0.4 90) (layer F.SilkS))
    (fp_text value 2N7002 (at -2.2 -0.4 90) (layer F.Fab) hide)
    (pad 2 smd rect (at -0.95 -1.1) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at 0 1.1) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(LED_STXO1-Pad1)"))
    (pad 1 smd rect (at 0.95 -1.1) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 13 /STXO))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Kalassi:SO8 (layer F.Cu) (tedit 0)
    (at 114.2 42.6 270)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U1 (at 0 0 270) (layer F.SilkS))
    (fp_text value EEPROM24 (at 0 0 270) (layer F.Fab))
    (pad 1 smd oval (at -1.905 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND_PI))
    (pad 2 smd oval (at -0.635 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND_PI))
    (pad 3 smd oval (at 0.635 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND_PI))
    (pad 4 smd oval (at 1.905 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND_PI))
    (pad 5 smd oval (at 1.905 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(K1-Pad27)"))
    (pad 6 smd oval (at 0.635 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(K1-Pad28)"))
    (pad 7 smd oval (at -0.635 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CFG1001-Pad1)"))
    (pad 8 smd oval (at -1.905 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
  )
  (module Kalassi:Crystal_SMD_HC49-SD (layer F.Cu) (tedit 5C93EFC8)
    (at 113.8 51 180)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference XT10 (at 1.8 -3.4 180) (layer F.SilkS))
    (fp_text value CSM-7X-DU (at 0 3.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.25 0 180) (size 4.5 2) (layers F.Cu F.Paste F.Mask)
      (net 43 /X1))
    (pad 2 smd rect (at 4.25 0 180) (size 4.5 2) (layers F.Cu F.Paste F.Mask)
      (net 44 /X2))
    (model ${KISYS3DMOD}/Crystal.3dshapes/HC49-SMD.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:C0603 (layer F.Cu) (tedit 5C60989B)
    (at 88 44.45 270)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C40 (at -2.75 0.1 270) (layer F.SilkS))
    (fp_text value C (at 0.75 1.75 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C40-Pad1)") (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND_PI) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:C0603 (layer F.Cu) (tedit 5C60989B)
    (at 78 79.6 270)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C52 (at 0 1.5 270) (layer F.SilkS))
    (fp_text value 33nF (at 0.75 1.75 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.05))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 27 /SOFTSTART) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:C0603 (layer F.Cu) (tedit 5C60989B)
    (at 79.4 72.6 90)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C55 (at -2.8 0.2 90) (layer F.SilkS))
    (fp_text value 3.3n (at 0.75 1.75 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.05))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 36 /COMP) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:C0603 (layer F.Cu) (tedit 5C60989B)
    (at 77.2 72.6 270)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C56 (at 2.8 0 270) (layer F.SilkS))
    (fp_text value 150nF (at 0.75 1.75 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 37 /COMP1) (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_THT:L_Axial_L23.4mm_D12.7mm_P25.40mm_Horizontal_Vishay_IHA-203 (layer F.Cu) (tedit 587E3FCE)
    (at 111 75)
    (descr "L, Axial series, Axial, Horizontal, pin pitch=25.4mm, , length*diameter=23.37*12.7mm^2, Vishay, IHA-203, http://www.vishay.com/docs/34014/iha.pdf")
    (tags "L Axial series Axial Horizontal pin pitch 25.4mm  length 23.37mm diameter 12.7mm Vishay IHA-203")
    (fp_text reference L60 (at 12.7 5) (layer F.SilkS))
    (fp_text value AIAP-03-272K (at 12.7 7.41) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 32 /DROSSEL_IN))
    (pad 2 thru_hole oval (at 25.4 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 /BUS+))
    (model Inductors_THT.3dshapes/L_Axial_L23.4mm_D12.7mm_P25.40mm_Horizontal_Vishay_IHA-203.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:R0603 (layer F.Cu) (tedit 5C609595)
    (at 85.8 44.4 270)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R40 (at -2.7 -0.5 270) (layer F.SilkS))
    (fp_text value 100k (at 0.75 1.75 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(IC40-Pad7)") (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.8 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC40-Pad1)") (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:R0603 (layer F.Cu) (tedit 5C609595)
    (at 80.2 79.6 270)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R52 (at 2.5 0 270) (layer F.SilkS))
    (fp_text value 100k (at 0.75 1.75 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.8 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.05))
    (pad 1 smd rect (at -0.8 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 34 /FREQ) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:R0603 (layer F.Cu) (tedit 5C609595)
    (at 81.6 72.6 90)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R55 (at -2.8 0 90) (layer F.SilkS))
    (fp_text value 1.65k (at 0.75 1.75 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 37 /COMP1) (solder_paste_margin_ratio -0.05))
    (pad 1 smd rect (at -0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 36 /COMP) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:R0603 (layer F.Cu) (tedit 5C609595)
    (at 83 79 180)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R58 (at 0 1.1 180) (layer F.SilkS))
    (fp_text value 220k (at 0.75 1.75 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8 0 180) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 28 /BOOST_30V) (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.8 0 180) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 33 /FB) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:R0603 (layer F.Cu) (tedit 5C609595)
    (at 83 81.4)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R59 (at -0.1 1.3) (layer F.SilkS))
    (fp_text value 10k (at 0.75 1.75) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.8 0) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.05))
    (pad 1 smd rect (at -0.8 0) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 33 /FB) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:R1210 (layer F.Cu) (tedit 5B87C6CB)
    (at 112.2 84.4 180)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R60 (at 0.9 -2 180) (layer F.SilkS))
    (fp_text value 100R (at 0 2.2 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.4 0 180) (size 1.6 2.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /BUS+) (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 1.4 0 180) (size 1.6 2.7) (layers F.Cu F.Paste F.Mask)
      (net 32 /DROSSEL_IN) (solder_paste_margin_ratio -0.05))
  )
  (module Kalassi:R0603 (layer F.Cu) (tedit 5C609595)
    (at 120.2 84.4 90)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R61 (at 0 1.2 90) (layer F.SilkS))
    (fp_text value 10k (at 0.75 1.75 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 35 /GYRA_B) (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.8 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 7 /BUS+) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:R1210 (layer F.Cu) (tedit 5B87C6CB)
    (at 129.6 84.6 90)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R62 (at -0.5 -2 90) (layer F.SilkS))
    (fp_text value 100R (at 0 2.2 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.4 0 90) (size 1.6 2.7) (layers F.Cu F.Paste F.Mask)
      (net 29 /GYRA_C) (solder_paste_margin_ratio -0.05))
    (pad 1 smd rect (at -1.4 0 90) (size 1.6 2.7) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.05))
  )
  (module Kalassi:C0603 (layer F.Cu) (tedit 5C60989B)
    (at 89.4 79 180)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C58 (at 0.25 -1.75 180) (layer F.SilkS))
    (fp_text value C (at 0.75 1.75 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 28 /BOOST_30V) (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_6.3x5.4 (layer F.Cu) (tedit 5BCA39D0)
    (at 88.6 85 180)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic C55, 6.3x5.4mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C59 (at 0 2.2 180) (layer F.SilkS))
    (fp_text value CP (at 0 4.35 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -2.8 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 28 /BOOST_30V))
    (pad 2 smd roundrect (at 2.8 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_6.3x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:C0603 (layer F.Cu) (tedit 5C60989B)
    (at 124.6 83.2 180)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C61 (at -0.2 1.2 180) (layer F.SilkS))
    (fp_text value 220nF (at 0.75 1.75 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 29 /GYRA_C) (solder_paste_margin_ratio -0.05))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 30 /GYRA_E) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA (layer F.Cu) (tedit 586432E5)
    (at 101.4 79.2 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D50 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value D (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 31 /SW))
    (pad 1 smd rect (at -2 0 90) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 28 /BOOST_30V))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA (layer F.Cu) (tedit 586432E5)
    (at 106.4 83.2 270)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D60 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value D (at 0 2.6 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 32 /DROSSEL_IN))
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 28 /BOOST_30V))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 89.4 73.8 270)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference IC50 (at 0 -2.85 270) (layer F.SilkS))
    (fp_text value TPS55340 (at 0 2.85 270) (layer F.Fab))
    (pad 1 smd oval (at -1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /SW))
    (pad 2 smd oval (at -1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /VCC5_BOOST))
    (pad 3 smd oval (at -1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /VCC5_BOOST))
    (pad 4 smd oval (at -1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 /SOFTSTART))
    (pad 5 smd oval (at -0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd oval (at -0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 7 smd oval (at 0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /COMP))
    (pad 8 smd oval (at 0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /FB))
    (pad 9 smd oval (at 1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 /FREQ))
    (pad 10 smd oval (at 1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 11 smd oval (at 1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 12 smd oval (at 1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 13 smd oval (at 0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 14 smd oval (at 0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 15 smd oval (at -0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /SW))
    (pad 16 smd oval (at -0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /SW))
    (pad 17 smd rect (at 0.45 0.45 270) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 -0.45 270) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45 270) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 -0.45 270) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:Eaton_HC1 (layer F.Cu) (tedit 5CAC92DB)
    (at 101.4 66.2 270)
    (fp_text reference L50 (at 8.4 0.3) (layer F.SilkS))
    (fp_text value "Eaton HC1-100-R" (at 0 8 270) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -5 0 270) (size 4.5 10) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /VCC5_BOOST))
    (pad 2 smd roundrect (at 5 0 270) (size 4.5 10) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /SW))
  )
  (module Kalassi:SOT23 (layer F.Cu) (tedit 5C603EDA)
    (at 124.6 86.6 90)
    (descr SOT-23)
    (tags "SOT23 IPC")
    (fp_text reference Q61 (at -1.6 2.3 180) (layer F.SilkS))
    (fp_text value BC807 (at -2.2 -0.4 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0.95 -1.1 90) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 29 /GYRA_C))
    (pad 3 smd rect (at 0 1.1 90) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 30 /GYRA_E))
    (pad 2 smd rect (at -0.95 -1.1 90) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 35 /GYRA_B))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Kalassi:C0603 (layer F.Cu) (tedit 5C60989B)
    (at 85.6 72.6 270)
    (descr CAPACITOR)
    (tags "CAPACITOR IPC")
    (attr smd)
    (fp_text reference C50 (at -0.1 1.3 270) (layer F.SilkS))
    (fp_text value C (at 0.75 1.75 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 26 /VCC5_BOOST) (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_6.3x5.4 (layer F.Cu) (tedit 5BCA39D0)
    (at 88.4 64.8 180)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic C55, 6.3x5.4mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C51 (at 4.5 2.5 270) (layer F.SilkS))
    (fp_text value CP (at 0 4.35 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -2.8 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 26 /VCC5_BOOST))
    (pad 2 smd roundrect (at 2.8 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_6.3x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 77.8 47.8 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference DIS1 (at 0 -3.1 180) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(DIS1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND_PI))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:DFN-10-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 82.7 44.2 90)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference IC40 (at 0 -2.575 90) (layer F.SilkS))
    (fp_text value STEF05 (at 0 2.575 90) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -1 90) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC40-Pad1)"))
    (pad 2 smd rect (at -1.55 -0.5 90) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC40-Pad1)"))
    (pad 3 smd rect (at -1.55 0 90) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC40-Pad1)"))
    (pad 4 smd rect (at -1.55 0.5 90) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC40-Pad1)"))
    (pad 5 smd rect (at -1.55 1 90) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC40-Pad1)"))
    (pad 6 smd rect (at 1.55 1 90) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 1.55 0.5 90) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(IC40-Pad7)"))
    (pad 8 smd rect (at 1.55 0 90) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(DIS1-Pad1)"))
    (pad 9 smd rect (at 1.55 -0.5 90) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C40-Pad1)"))
    (pad 10 smd rect (at 1.55 -1 90) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND_PI))
    (pad 11 smd rect (at 0.3875 0.62 90) (size 0.775 1.24) (layers F.Cu F.Paste F.Mask)
      (net 14 +5V) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at 0.3875 -0.62 90) (size 0.775 1.24) (layers F.Cu F.Paste F.Mask)
      (net 14 +5V) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at -0.3875 0.62 90) (size 0.775 1.24) (layers F.Cu F.Paste F.Mask)
      (net 14 +5V) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at -0.3875 -0.62 90) (size 0.775 1.24) (layers F.Cu F.Paste F.Mask)
      (net 14 +5V) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/DFN-10-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:R0603 (layer F.Cu) (tedit 5C609595)
    (at 103.5 84 270)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R68 (at -0.1 1.7 270) (layer F.SilkS))
    (fp_text value 3k9 (at 0.75 1.75 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(LED_SUP1-Pad2)") (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.8 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 28 /BOOST_30V) (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:R0603 (layer F.Cu) (tedit 5C609595)
    (at 103.5 80.7 270)
    (descr RESISTOR)
    (tags "RESISTOR IPC")
    (attr smd)
    (fp_text reference R69 (at -2.7 0 270) (layer F.SilkS))
    (fp_text value 100k (at 0.75 1.75 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.8 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.05))
    (pad 2 smd rect (at 0.8 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(LED_SUP1-Pad2)") (solder_paste_margin_ratio -0.05))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kalassi:SOT23 (layer F.Cu) (tedit 5C603EDA)
    (at 117 84.4 270)
    (descr SOT-23)
    (tags "SOT23 IPC")
    (fp_text reference D61 (at -2.2 0.8) (layer F.SilkS))
    (fp_text value BAS70-06 (at -2.2 -0.4) (layer F.Fab) hide)
    (pad 1 smd rect (at 0.95 -1.1 270) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 30 /GYRA_E))
    (pad 3 smd rect (at 0 1.1 270) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /BUS+))
    (pad 2 smd rect (at -0.95 -1.1 270) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 30 /GYRA_E))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5CACDB24)
    (at 118.2 87.6)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED_PI1 (at 0 -1.25) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND_PI))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(LED_PI1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5CACDB2A)
    (at 108.7 87.6)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED_STXO1 (at 0 -1.25) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(LED_STXO1-Pad2)"))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(LED_STXO1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5CACDB1D)
    (at 111.9 87.6 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED_SUP1 (at 0 -1.25 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(LED_SUP1-Pad2)"))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5CACDB35)
    (at 115.2 87.6 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LED_TPUART1 (at 0 -1.25 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(LED_TPUART1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text 3V3 (at 115.2 88.8) (layer F.SilkS))
  (gr_text TX (at 108.4 88.8) (layer F.SilkS))
  (gr_text INT (at 112 88.8) (layer F.SilkS))
  (gr_text PI (at 118.2 88.8) (layer F.SilkS))
  (dimension 56 (width 0.15) (layer Dwgs.User)
    (gr_text "56 mm (Thru-hole socket J2)" (at 75.35 28.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 66 56.5) (xy 76.7 56.5)))
    (feature2 (pts (xy 66 0.5) (xy 76.7 0.5)))
    (crossbar (pts (xy 74 0.5) (xy 74 56.5)))
    (arrow1a (pts (xy 74 56.5) (xy 73.413579 55.373496)))
    (arrow1b (pts (xy 74 56.5) (xy 74.586421 55.373496)))
    (arrow2a (pts (xy 74 0.5) (xy 73.413579 1.626504)))
    (arrow2b (pts (xy 74 0.5) (xy 74.586421 1.626504)))
  )
  (dimension 11.5 (width 0.15) (layer Dwgs.User)
    (gr_text "11.5 mm" (at 39.150001 50.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 43 56.5) (xy 37.800001 56.5)))
    (feature2 (pts (xy 43 45) (xy 37.800001 45)))
    (crossbar (pts (xy 40.500001 45) (xy 40.500001 56.5)))
    (arrow1a (pts (xy 40.500001 56.5) (xy 39.91358 55.373496)))
    (arrow1b (pts (xy 40.500001 56.5) (xy 41.086422 55.373496)))
    (arrow2a (pts (xy 40.500001 45) (xy 39.91358 46.126504)))
    (arrow2b (pts (xy 40.500001 45) (xy 41.086422 46.126504)))
  )
  (dimension 2 (width 0.15) (layer Dwgs.User)
    (gr_text "2 mm" (at 49.75 33) (layer Dwgs.User))
    (feature1 (pts (xy 46 35.5) (xy 46 30.300001)))
    (feature2 (pts (xy 44 35.5) (xy 44 30.300001)))
    (crossbar (pts (xy 44 33.000001) (xy 46 33.000001)))
    (arrow1a (pts (xy 46 33.000001) (xy 44.873496 33.586422)))
    (arrow1b (pts (xy 46 33.000001) (xy 44.873496 32.41358)))
    (arrow2a (pts (xy 44 33.000001) (xy 45.126504 33.586422)))
    (arrow2b (pts (xy 44 33.000001) (xy 45.126504 32.41358)))
  )
  (dimension 17 (width 0.15) (layer Dwgs.User)
    (gr_text "17 mm" (at 51.35 45 270) (layer Dwgs.User))
    (feature1 (pts (xy 47 53.5) (xy 52.7 53.5)))
    (feature2 (pts (xy 47 36.5) (xy 52.7 36.5)))
    (crossbar (pts (xy 50 36.5) (xy 50 53.5)))
    (arrow1a (pts (xy 50 53.5) (xy 49.413579 52.373496)))
    (arrow1b (pts (xy 50 53.5) (xy 50.586421 52.373496)))
    (arrow2a (pts (xy 50 36.5) (xy 49.413579 37.626504)))
    (arrow2b (pts (xy 50 36.5) (xy 50.586421 37.626504)))
  )
  (dimension 3.5 (width 0.15) (layer Dwgs.User)
    (gr_text "3.5 mm" (at 8.5 60) (layer Dwgs.User))
    (feature1 (pts (xy 3.5 57.5) (xy 3.5 62.7)))
    (feature2 (pts (xy 0 57.5) (xy 0 62.7)))
    (crossbar (pts (xy 0 60) (xy 3.5 60)))
    (arrow1a (pts (xy 3.5 60) (xy 2.373496 60.586421)))
    (arrow1b (pts (xy 3.5 60) (xy 2.373496 59.413579)))
    (arrow2a (pts (xy 0 60) (xy 1.126504 60.586421)))
    (arrow2b (pts (xy 0 60) (xy 1.126504 59.413579)))
  )
  (dimension 3.5 (width 0.15) (layer Dwgs.User)
    (gr_text "3.5 mm" (at 10.25 48.25 270) (layer Dwgs.User))
    (feature1 (pts (xy 7 56.5) (xy 12.7 56.5)))
    (feature2 (pts (xy 7 53) (xy 12.7 53)))
    (crossbar (pts (xy 10 53) (xy 10 56.5)))
    (arrow1a (pts (xy 10 56.5) (xy 9.413579 55.373496)))
    (arrow1b (pts (xy 10 56.5) (xy 10.586421 55.373496)))
    (arrow2a (pts (xy 10 53) (xy 9.413579 54.126504)))
    (arrow2b (pts (xy 10 53) (xy 10.586421 54.126504)))
  )
  (dimension 49 (width 0.15) (layer Dwgs.User)
    (gr_text "49 mm" (at 70.349999 28.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 66 53) (xy 71.699999 53)))
    (feature2 (pts (xy 66 4) (xy 71.699999 4)))
    (crossbar (pts (xy 68.999999 4) (xy 68.999999 53)))
    (arrow1a (pts (xy 68.999999 53) (xy 68.413578 51.873496)))
    (arrow1b (pts (xy 68.999999 53) (xy 69.58642 51.873496)))
    (arrow2a (pts (xy 68.999999 4) (xy 68.413578 5.126504)))
    (arrow2b (pts (xy 68.999999 4) (xy 69.58642 5.126504)))
  )
  (dimension 19.5 (width 0.15) (layer Dwgs.User)
    (gr_text "19.5 mm" (at -5.35 46.75 270) (layer Dwgs.User))
    (feature1 (pts (xy -1 56.5) (xy -6.7 56.5)))
    (feature2 (pts (xy -1 37) (xy -6.7 37)))
    (crossbar (pts (xy -4 37) (xy -4 56.5)))
    (arrow1a (pts (xy -4 56.5) (xy -4.586421 55.373496)))
    (arrow1b (pts (xy -4 56.5) (xy -3.413579 55.373496)))
    (arrow2a (pts (xy -4 37) (xy -4.586421 38.126504)))
    (arrow2b (pts (xy -4 37) (xy -3.413579 38.126504)))
  )
  (dimension 17 (width 0.15) (layer Dwgs.User)
    (gr_text "17 mm" (at 9.35 28.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 6 37) (xy 10.7 37)))
    (feature2 (pts (xy 6 20) (xy 10.7 20)))
    (crossbar (pts (xy 8 20) (xy 8 37)))
    (arrow1a (pts (xy 8 37) (xy 7.413579 35.873496)))
    (arrow1b (pts (xy 8 37) (xy 8.586421 35.873496)))
    (arrow2a (pts (xy 8 20) (xy 7.413579 21.126504)))
    (arrow2b (pts (xy 8 20) (xy 8.586421 21.126504)))
  )
  (dimension 5 (width 0.15) (layer Dwgs.User)
    (gr_text "5 mm" (at 8.75 18) (layer Dwgs.User))
    (feature1 (pts (xy 5 20) (xy 5 15.3)))
    (feature2 (pts (xy 0 20) (xy 0 15.3)))
    (crossbar (pts (xy 0 18) (xy 5 18)))
    (arrow1a (pts (xy 5 18) (xy 3.873496 18.586421)))
    (arrow1b (pts (xy 5 18) (xy 3.873496 17.413579)))
    (arrow2a (pts (xy 0 18) (xy 1.126504 18.586421)))
    (arrow2b (pts (xy 0 18) (xy 1.126504 17.413579)))
  )
  (dimension 29 (width 0.15) (layer Dwgs.User)
    (gr_text "29 mm" (at 18 11.849999) (layer Dwgs.User))
    (feature1 (pts (xy 32.5 8) (xy 32.5 13.199999)))
    (feature2 (pts (xy 3.5 8) (xy 3.5 13.199999)))
    (crossbar (pts (xy 3.5 10.499999) (xy 32.5 10.499999)))
    (arrow1a (pts (xy 32.5 10.499999) (xy 31.373496 11.08642)))
    (arrow1b (pts (xy 32.5 10.499999) (xy 31.373496 9.913578)))
    (arrow2a (pts (xy 3.5 10.499999) (xy 4.626504 11.08642)))
    (arrow2b (pts (xy 3.5 10.499999) (xy 4.626504 9.913578)))
  )
  (dimension 58 (width 0.15) (layer Dwgs.User)
    (gr_text "58 mm" (at 32.5 -4.85) (layer Dwgs.User))
    (feature1 (pts (xy 61.5 -1) (xy 61.5 -6.2)))
    (feature2 (pts (xy 3.5 -1) (xy 3.5 -6.2)))
    (crossbar (pts (xy 3.5 -3.5) (xy 61.5 -3.5)))
    (arrow1a (pts (xy 61.5 -3.5) (xy 60.373496 -2.913579)))
    (arrow1b (pts (xy 61.5 -3.5) (xy 60.373496 -4.086421)))
    (arrow2a (pts (xy 3.5 -3.5) (xy 4.626504 -2.913579)))
    (arrow2b (pts (xy 3.5 -3.5) (xy 4.626504 -4.086421)))
  )
  (dimension 65 (width 0.15) (layer Dwgs.User)
    (gr_text "65 mm" (at 32.5 -9.35) (layer Dwgs.User))
    (feature1 (pts (xy 65 -1) (xy 65 -10.7)))
    (feature2 (pts (xy 0 -1) (xy 0 -10.7)))
    (crossbar (pts (xy 0 -8) (xy 65 -8)))
    (arrow1a (pts (xy 65 -8) (xy 63.873496 -7.413579)))
    (arrow1b (pts (xy 65 -8) (xy 63.873496 -8.586421)))
    (arrow2a (pts (xy 0 -8) (xy 1.126504 -7.413579)))
    (arrow2b (pts (xy 0 -8) (xy 1.126504 -8.586421)))
  )
  (dimension 56.5 (width 0.15) (layer Dwgs.User)
    (gr_text "56.5 mm (SMT socket J1)" (at 79.35 28.25 270) (layer Dwgs.User))
    (feature1 (pts (xy 66 56.5) (xy 80.7 56.5)))
    (feature2 (pts (xy 66 0) (xy 80.7 0)))
    (crossbar (pts (xy 78 0) (xy 78 56.5)))
    (arrow1a (pts (xy 78 56.5) (xy 77.413579 55.373496)))
    (arrow1b (pts (xy 78 56.5) (xy 78.586421 55.373496)))
    (arrow2a (pts (xy 78 0) (xy 77.413579 1.126504)))
    (arrow2b (pts (xy 78 0) (xy 78.586421 1.126504)))
  )
  (gr_arc (start 76.1 70.875) (end 75.1 70.875) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 79.1 68.875) (end 80.1 68.875) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 79.1 53.875) (end 79.1 52.875) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 76.1 51.875) (end 76.1 52.875) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 137.1 86.375) (end 140.1 86.375) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 78.1 86.375) (end 78.1 89.375) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 78.1 35.875) (end 75.1 35.875) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 137.1 35.875) (end 137.1 32.875) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.1 70.875) (end 75.1 86.375) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.1 35.875) (end 75.1 51.875) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 76.1 69.875) (end 79.1 69.875) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 76.1 52.875) (end 79.1 52.875) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80.1 53.875) (end 80.1 68.875) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 78.1 89.375) (end 137.1 89.375) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.1 35.875) (end 140.1 86.375) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 78.1 32.875) (end 137.1 32.875) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 31) (net_name /SW) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.6 78.4) (xy 99 78.4) (xy 95 73.7) (xy 90.4 73.7) (xy 90.4 72.8)
        (xy 90 72.8) (xy 90 71.4) (xy 90 69) (xy 106.6 69) (xy 106.6 72.8)
      )
    )
  )
  (zone (net 28) (net_name /BOOST_30V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.4 79.8) (xy 102.4 85.8) (xy 89.6 85.8) (xy 89.6 78.2) (xy 97.4 78.2)
        (xy 99.4 79.8)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.4 73.9) (xy 91.4 77.8) (xy 89 77.8) (xy 89 79.6) (xy 87.6 84.2)
        (xy 87.6 88) (xy 84 88) (xy 84 84) (xy 83 82) (xy 83 80.6)
        (xy 84.4 80.6) (xy 88.8 76) (xy 89 73.9)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.4 64) (xy 87.4 65.8) (xy 87.8 66.8) (xy 87.8 67.6) (xy 83.4 67.6)
        (xy 83.4 64)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.2 72.9) (xy 90.2 77.8) (xy 88.4 77.8) (xy 88.4 72.8)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.2 49.2) (xy 121.2 48.2) (xy 106.6 48.2) (xy 103.8 50.8) (xy 103.8 57.8)
        (xy 108.6 57.8) (xy 108.6 62.2) (xy 121.2 62.2)
      )
    )
  )
  (zone (net 31) (net_name /SW) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.9 73.7) (xy 91.9 77.8) (xy 98.6 77.8) (xy 96 73.4) (xy 92.2 73.4)
      )
    )
  )
)
