(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 1762)
    (zones 0)
    (modules 308)
    (nets 155)
  )
  (page A4)
  (layers
    (0 Kupfer_oben signal)
    (1 GND signal)
    (2 +5VA power)
    (31 Kupfer_unten signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.29337)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.28)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.3 1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010cc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 +5VA)
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 Versorgung_LNB)
  (net 5 "Net-(C7-Pad1)")
  (net 6 "Net-(C9-Pad1)")
  (net 7 "Net-(C10-Pad1)")
  (net 8 "Net-(C12-Pad1)")
  (net 9 "Net-(C13-Pad1)")
  (net 10 "Net-(C15-Pad1)")
  (net 11 3V3_LO_Frontend)
  (net 12 "Net-(C23-Pad1)")
  (net 13 Vcc_TX)
  (net 14 "Net-(C27-Pad1)")
  (net 15 "Net-(C28-Pad1)")
  (net 16 "Net-(C29-Pad1)")
  (net 17 "Net-(C30-Pad1)")
  (net 18 "Net-(C31-Pad2)")
  (net 19 "Net-(C31-Pad1)")
  (net 20 "Net-(C32-Pad1)")
  (net 21 "Net-(C33-Pad1)")
  (net 22 "Net-(C34-Pad1)")
  (net 23 "Net-(C35-Pad1)")
  (net 24 "Net-(C37-Pad2)")
  (net 25 "Net-(C37-Pad1)")
  (net 26 "Net-(C39-Pad1)")
  (net 27 Frontend_Ausgang)
  (net 28 "Net-(C43-Pad1)")
  (net 29 "Net-(C44-Pad2)")
  (net 30 "Net-(C47-Pad2)")
  (net 31 "Net-(C48-Pad2)")
  (net 32 "Net-(C49-Pad1)")
  (net 33 "Net-(C50-Pad1)")
  (net 34 "Net-(C53-Pad1)")
  (net 35 "Net-(C57-Pad1)")
  (net 36 "Net-(C58-Pad1)")
  (net 37 "Net-(C59-Pad1)")
  (net 38 "Net-(C62-Pad2)")
  (net 39 "Net-(C62-Pad1)")
  (net 40 "Net-(C64-Pad1)")
  (net 41 "Net-(C66-Pad1)")
  (net 42 Frontend_Lokaloszillator)
  (net 43 "Net-(C67-Pad1)")
  (net 44 "Net-(C69-Pad1)")
  (net 45 "Net-(C70-Pad2)")
  (net 46 "Net-(C70-Pad1)")
  (net 47 "Net-(C71-Pad2)")
  (net 48 "Net-(C72-Pad2)")
  (net 49 "Net-(C73-Pad2)")
  (net 50 "Net-(C73-Pad1)")
  (net 51 "Net-(C74-Pad1)")
  (net 52 "Net-(C75-Pad2)")
  (net 53 "Net-(C79-Pad2)")
  (net 54 Sendezweig_Mischer_Ausgang)
  (net 55 "Net-(C80-Pad2)")
  (net 56 "Net-(C82-Pad1)")
  (net 57 "Net-(C83-Pad1)")
  (net 58 "Net-(C83-Pad2)")
  (net 59 "Net-(C86-Pad1)")
  (net 60 "Net-(C89-Pad1)")
  (net 61 "Net-(C91-Pad1)")
  (net 62 "Net-(C91-Pad2)")
  (net 63 "Net-(C93-Pad1)")
  (net 64 "Net-(C93-Pad2)")
  (net 65 "Net-(C96-Pad1)")
  (net 66 "Net-(C101-Pad1)")
  (net 67 "Net-(C101-Pad2)")
  (net 68 "Net-(C102-Pad1)")
  (net 69 "Net-(C103-Pad1)")
  (net 70 "Net-(C105-Pad2)")
  (net 71 "Net-(C106-Pad2)")
  (net 72 "Net-(C106-Pad1)")
  (net 73 "Net-(C111-Pad1)")
  (net 74 "Net-(C111-Pad2)")
  (net 75 "Net-(C116-Pad2)")
  (net 76 "Net-(C116-Pad1)")
  (net 77 "Net-(C117-Pad1)")
  (net 78 "Net-(C119-Pad1)")
  (net 79 RX-Frontend-Mischer)
  (net 80 "Net-(C120-Pad1)")
  (net 81 "Net-(C122-Pad2)")
  (net 82 "Net-(C123-Pad1)")
  (net 83 "Net-(C124-Pad1)")
  (net 84 "Net-(C126-Pad1)")
  (net 85 "Net-(C127-Pad2)")
  (net 86 "Net-(C127-Pad1)")
  (net 87 "Net-(C128-Pad1)")
  (net 88 "Net-(C129-Pad2)")
  (net 89 RX_Lokaloszillator)
  (net 90 "Net-(C130-Pad1)")
  (net 91 "Net-(C131-Pad2)")
  (net 92 "Net-(C132-Pad2)")
  (net 93 "Net-(C132-Pad1)")
  (net 94 "Net-(C133-Pad2)")
  (net 95 "Net-(C133-Pad1)")
  (net 96 "Net-(C134-Pad1)")
  (net 97 "Net-(C135-Pad2)")
  (net 98 "Net-(C137-Pad2)")
  (net 99 "Net-(C140-Pad1)")
  (net 100 "Net-(C144-Pad2)")
  (net 101 "Net-(C145-Pad1)")
  (net 102 "Net-(C146-Pad1)")
  (net 103 "Net-(C147-Pad1)")
  (net 104 "Net-(D1-Pad2)")
  (net 105 "Net-(D2-Pad1)")
  (net 106 "Net-(D3-Pad1)")
  (net 107 "Net-(D4-Pad1)")
  (net 108 "Net-(D5-Pad2)")
  (net 109 "Net-(D5-Pad1)")
  (net 110 "Net-(D6-Pad1)")
  (net 111 "Net-(D7-Pad1)")
  (net 112 "Net-(D8-Pad1)")
  (net 113 "Net-(D9-Pad1)")
  (net 114 "Net-(D9-Pad2)")
  (net 115 "Net-(FL1-Pad3)")
  (net 116 "Net-(IC1-Pad3)")
  (net 117 "Net-(IC2-Pad7)")
  (net 118 "Net-(IC4-Pad2)")
  (net 119 "Net-(IC4-Pad11)")
  (net 120 "Net-(IC4-Pad12)")
  (net 121 "Net-(IC6-Pad6)")
  (net 122 "Net-(IC7-Pad1)")
  (net 123 "Net-(J1-Pad2)")
  (net 124 "Net-(J2-Pad2)")
  (net 125 PA_enable)
  (net 126 Eingangs-Umschalter)
  (net 127 RX_CLK)
  (net 128 Sendezweig_CLK)
  (net 129 RX_DATA)
  (net 130 Sendezweig_DATA)
  (net 131 RX_LE)
  (net 132 Sendezweig_LE)
  (net 133 "Net-(K1-Pad6)")
  (net 134 "Net-(K1-Pad14)")
  (net 135 RX_Teil)
  (net 136 "Net-(L18-Pad2)")
  (net 137 "Net-(L14-Pad1)")
  (net 138 "Net-(L20-Pad2)")
  (net 139 "Net-(L44-Pad1)")
  (net 140 "Net-(Q1-Pad1)")
  (net 141 "Net-(Q2-Pad1)")
  (net 142 "Net-(Q3-Pad1)")
  (net 143 "Net-(Q4-Pad1)")
  (net 144 "Net-(Q5-Pad3)")
  (net 145 "Net-(Q5-Pad1)")
  (net 146 "Net-(Q6-Pad1)")
  (net 147 "Net-(R10-Pad1)")
  (net 148 "Net-(R21-Pad1)")
  (net 149 "Net-(R22-Pad2)")
  (net 150 "Net-(R44-Pad1)")
  (net 151 "Net-(R50-Pad2)")
  (net 152 "Net-(T2-Pad1)")
  (net 153 "Net-(T2-Pad3)")
  (net 154 TCXO)
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.29337)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5VA)
    (add_net 3V3_LO_Frontend)
    (add_net Eingangs-Umschalter)
    (add_net Frontend_Ausgang)
    (add_net Frontend_Lokaloszillator)
    (add_net GND)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C101-Pad1)")
    (add_net "Net-(C101-Pad2)")
    (add_net "Net-(C102-Pad1)")
    (add_net "Net-(C103-Pad1)")
    (add_net "Net-(C105-Pad2)")
    (add_net "Net-(C106-Pad1)")
    (add_net "Net-(C106-Pad2)")
    (add_net "Net-(C111-Pad1)")
    (add_net "Net-(C111-Pad2)")
    (add_net "Net-(C116-Pad1)")
    (add_net "Net-(C116-Pad2)")
    (add_net "Net-(C117-Pad1)")
    (add_net "Net-(C119-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C120-Pad1)")
    (add_net "Net-(C122-Pad2)")
    (add_net "Net-(C123-Pad1)")
    (add_net "Net-(C124-Pad1)")
    (add_net "Net-(C126-Pad1)")
    (add_net "Net-(C127-Pad1)")
    (add_net "Net-(C127-Pad2)")
    (add_net "Net-(C128-Pad1)")
    (add_net "Net-(C129-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C130-Pad1)")
    (add_net "Net-(C131-Pad2)")
    (add_net "Net-(C132-Pad1)")
    (add_net "Net-(C132-Pad2)")
    (add_net "Net-(C133-Pad1)")
    (add_net "Net-(C133-Pad2)")
    (add_net "Net-(C134-Pad1)")
    (add_net "Net-(C135-Pad2)")
    (add_net "Net-(C137-Pad2)")
    (add_net "Net-(C140-Pad1)")
    (add_net "Net-(C144-Pad2)")
    (add_net "Net-(C145-Pad1)")
    (add_net "Net-(C146-Pad1)")
    (add_net "Net-(C147-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(C28-Pad1)")
    (add_net "Net-(C29-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C30-Pad1)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C31-Pad2)")
    (add_net "Net-(C32-Pad1)")
    (add_net "Net-(C33-Pad1)")
    (add_net "Net-(C34-Pad1)")
    (add_net "Net-(C35-Pad1)")
    (add_net "Net-(C37-Pad1)")
    (add_net "Net-(C37-Pad2)")
    (add_net "Net-(C39-Pad1)")
    (add_net "Net-(C43-Pad1)")
    (add_net "Net-(C44-Pad2)")
    (add_net "Net-(C47-Pad2)")
    (add_net "Net-(C48-Pad2)")
    (add_net "Net-(C49-Pad1)")
    (add_net "Net-(C50-Pad1)")
    (add_net "Net-(C53-Pad1)")
    (add_net "Net-(C57-Pad1)")
    (add_net "Net-(C58-Pad1)")
    (add_net "Net-(C59-Pad1)")
    (add_net "Net-(C62-Pad1)")
    (add_net "Net-(C62-Pad2)")
    (add_net "Net-(C64-Pad1)")
    (add_net "Net-(C66-Pad1)")
    (add_net "Net-(C67-Pad1)")
    (add_net "Net-(C69-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C70-Pad1)")
    (add_net "Net-(C70-Pad2)")
    (add_net "Net-(C71-Pad2)")
    (add_net "Net-(C72-Pad2)")
    (add_net "Net-(C73-Pad1)")
    (add_net "Net-(C73-Pad2)")
    (add_net "Net-(C74-Pad1)")
    (add_net "Net-(C75-Pad2)")
    (add_net "Net-(C79-Pad2)")
    (add_net "Net-(C80-Pad2)")
    (add_net "Net-(C82-Pad1)")
    (add_net "Net-(C83-Pad1)")
    (add_net "Net-(C83-Pad2)")
    (add_net "Net-(C86-Pad1)")
    (add_net "Net-(C89-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C91-Pad1)")
    (add_net "Net-(C91-Pad2)")
    (add_net "Net-(C93-Pad1)")
    (add_net "Net-(C93-Pad2)")
    (add_net "Net-(C96-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(FL1-Pad3)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC2-Pad7)")
    (add_net "Net-(IC4-Pad11)")
    (add_net "Net-(IC4-Pad12)")
    (add_net "Net-(IC4-Pad2)")
    (add_net "Net-(IC6-Pad6)")
    (add_net "Net-(IC7-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(K1-Pad14)")
    (add_net "Net-(K1-Pad6)")
    (add_net "Net-(L14-Pad1)")
    (add_net "Net-(L18-Pad2)")
    (add_net "Net-(L20-Pad2)")
    (add_net "Net-(L44-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(Q5-Pad3)")
    (add_net "Net-(Q6-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R21-Pad1)")
    (add_net "Net-(R22-Pad2)")
    (add_net "Net-(R44-Pad1)")
    (add_net "Net-(R50-Pad2)")
    (add_net "Net-(T2-Pad1)")
    (add_net "Net-(T2-Pad3)")
    (add_net PA_enable)
    (add_net RX-Frontend-Mischer)
    (add_net RX_CLK)
    (add_net RX_DATA)
    (add_net RX_LE)
    (add_net RX_Lokaloszillator)
    (add_net RX_Teil)
    (add_net Sendezweig_CLK)
    (add_net Sendezweig_DATA)
    (add_net Sendezweig_LE)
    (add_net Sendezweig_Mischer_Ausgang)
    (add_net TCXO)
    (add_net Vcc_TX)
    (add_net Versorgung_LNB)
  )
  (module Capacitors_SMD:CP_Elec_8x10.5 (layer Kupfer_oben) (tedit 58AA8BC3)
    (at 89.9 96.53 180)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5")
    (attr smd)
    (fp_text reference C11 (at 0 5.45 180) (layer F.SilkS))
    (fp_text value 100uF (at 0 -5.45 180) (layer F.Fab))
    (fp_text user %R (at 0 5.45 180) (layer F.Fab))
    (fp_text user + (at -4.78 3.91 180) (layer F.SilkS))
    (fp_text user + (at -2.27 -0.08 180) (layer F.Fab))
    (pad 2 smd rect (at 3.05 0) (size 4 2.5) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.05 0) (size 4 2.5) (layers Kupfer_oben F.Paste F.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x06_Pitch2.54mm_SMD (layer Kupfer_oben) (tedit 58CD5449)
    (at 139.954 82.804 180)
    (descr "surface-mounted straight socket strip, 2x06, 2.54mm pitch, double rows")
    (tags "Surface mounted socket strip SMD 2x06 2.54mm double row")
    (attr smd)
    (fp_text reference J11 (at 0 -8.68 180) (layer F.SilkS))
    (fp_text value Conn_02x06_Odd_Even (at 0 8.68 180) (layer F.Fab))
    (fp_text user %R (at 0 -8.68 180) (layer F.Fab))
    (pad 12 smd rect (at -2.52 6.35 180) (size 3 1) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (pad 11 smd rect (at 2.52 6.35 180) (size 3 1) (layers Kupfer_oben F.Paste F.Mask)
      (net 125 PA_enable))
    (pad 10 smd rect (at -2.52 3.81 180) (size 3 1) (layers Kupfer_oben F.Paste F.Mask)
      (net 126 Eingangs-Umschalter))
    (pad 9 smd rect (at 2.52 3.81 180) (size 3 1) (layers Kupfer_oben F.Paste F.Mask)
      (net 4 Versorgung_LNB))
    (pad 8 smd rect (at -2.52 1.27 180) (size 3 1) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 2.52 1.27 180) (size 3 1) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.52 -1.27 180) (size 3 1) (layers Kupfer_oben F.Paste F.Mask)
      (net 127 RX_CLK))
    (pad 5 smd rect (at 2.52 -1.27 180) (size 3 1) (layers Kupfer_oben F.Paste F.Mask)
      (net 128 Sendezweig_CLK))
    (pad 4 smd rect (at -2.52 -3.81 180) (size 3 1) (layers Kupfer_oben F.Paste F.Mask)
      (net 129 RX_DATA))
    (pad 3 smd rect (at 2.52 -3.81 180) (size 3 1) (layers Kupfer_oben F.Paste F.Mask)
      (net 130 Sendezweig_DATA))
    (pad 2 smd rect (at -2.52 -6.35 180) (size 3 1) (layers Kupfer_oben F.Paste F.Mask)
      (net 131 RX_LE))
    (pad 1 smd rect (at 2.52 -6.35 180) (size 3 1) (layers Kupfer_oben F.Paste F.Mask)
      (net 132 Sendezweig_LE))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x06_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Wuerth_WE-PD-Typ-LS (layer Kupfer_oben) (tedit 5990349D)
    (at 96.62 108.77)
    (descr "Choke, Drossel, WE-PD Typ LS, Wuerth, SMD,")
    (tags "Choke Drossel WE-PDTypLS Wuerth SMD ")
    (attr smd)
    (fp_text reference L4 (at 0 -7.3) (layer F.SilkS))
    (fp_text value 10uH (at 0 7.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.95 0) (size 2.9 5.4) (layers Kupfer_oben F.Paste F.Mask)
      (net 8 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 4.95 0) (size 2.9 5.4) (layers Kupfer_oben F.Paste F.Mask)
      (net 4 Versorgung_LNB))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Wuerth_WE-PD-Typ-LS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:HF353 (layer Kupfer_oben) (tedit 0)
    (at 124.61 61.72 180)
    (descr "HF3 53-2")
    (tags "Relay or Contactor")
    (attr smd)
    (fp_text reference K1 (at -0.05 0 180) (layer F.SilkS))
    (fp_text value HF3-53 (at -0.05 0 180) (layer F.SilkS) hide)
    (fp_text user %R (at -0.05 0 180) (layer F.Fab))
    (pad 1 smd rect (at -6.35 3.75 180) (size 0.7 2.5) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (pad 2 smd rect (at -5.08 4 180) (size 0.9 2) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.27 4 180) (size 0.7 2) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0 4 180) (size 0.9 2) (layers Kupfer_oben F.Paste F.Mask)
      (net 133 "Net-(K1-Pad6)"))
    (pad 7 smd rect (at 1.27 4 180) (size 0.7 2) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 5.08 4 180) (size 0.9 2) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 6.35 3.75 180) (size 0.7 2.5) (layers Kupfer_oben F.Paste F.Mask)
      (net 104 "Net-(D1-Pad2)"))
    (pad 12 smd rect (at 6.35 -3.75 180) (size 0.7 2.5) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 5.08 -4 180) (size 0.7 2) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 3.81 -4 180) (size 0.9 2) (layers Kupfer_oben F.Paste F.Mask)
      (net 134 "Net-(K1-Pad14)"))
    (pad 15 smd rect (at 2.54 -4 180) (size 0.7 2) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 0 -4 180) (size 0.9 2) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at -2.54 -4 180) (size 0.7 2) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at -3.81 -4 180) (size 0.9 2) (layers Kupfer_oben F.Paste F.Mask)
      (net 135 RX_Teil))
    (pad 21 smd rect (at -5.08 -4 180) (size 0.7 2) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at -6.35 -3.75 180) (size 0.7 2.5) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model D:\Kicad\lib\SamacSys_Parts.3dshapes\HF3_53.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer Kupfer_unten) (tedit 58641739)
    (at 161.33 61.47 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D6 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 3,3V (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers Kupfer_unten B.Paste B.Mask)
      (net 110 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer Kupfer_unten) (tedit 58641739)
    (at 164.21 127.72 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 0 1.85 270) (layer B.SilkS))
    (fp_text value 3,3V (at 0.1 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 0 1.85 270) (layer B.Fab))
    (pad 2 smd rect (at 1.05 0 270) (size 0.6 0.45) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.05 0 270) (size 0.6 0.45) (layers Kupfer_unten B.Paste B.Mask)
      (net 105 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer Kupfer_unten) (tedit 58641739)
    (at 159.78 128.63 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at 0 1.85 270) (layer B.SilkS))
    (fp_text value 3,3V (at 0.1 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 0 1.85 270) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 0.6 0.45) (layers Kupfer_unten B.Paste B.Mask)
      (net 106 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.05 0 270) (size 0.6 0.45) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer Kupfer_unten) (tedit 58641739)
    (at 162.14 59.16 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D7 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 3,3V (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers Kupfer_unten B.Paste B.Mask)
      (net 111 "Net-(D7-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer Kupfer_unten) (tedit 58641739)
    (at 152.88 127.76 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D4 (at 0 1.85 270) (layer B.SilkS))
    (fp_text value 3,3V (at 0.1 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 0 1.85 270) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 0.6 0.45) (layers Kupfer_unten B.Paste B.Mask)
      (net 107 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.05 0 270) (size 0.6 0.45) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer Kupfer_unten) (tedit 58641739)
    (at 165.34 56.91)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D8 (at 0 1.85) (layer B.SilkS))
    (fp_text value 3,3V (at 0.1 -1.9) (layer B.Fab))
    (fp_text user %R (at 0 1.85) (layer B.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers Kupfer_unten B.Paste B.Mask)
      (net 112 "Net-(D8-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Shielding_Cabinets:Laird_Technologies_BMI-S-205-F_38.10x25.40mm (layer Kupfer_oben) (tedit 57501709)
    (at 216.13 72.98)
    (descr "Laird Technologies BMI-S-205-F Shielding Cabinet Two Piece SMD 38.10x25.40mm")
    (tags "Shielding Cabinet")
    (attr smd)
    (fp_text reference J9 (at 0 -14.1) (layer F.SilkS))
    (fp_text value SchirmahsuRX-Frontend (at 0 14.1) (layer F.Fab))
    (pad 1 smd rect (at 18.95 11.225) (size 1 1.75) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -18.95 11.225) (size 1 1.75) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 18.95 6) (size 1 3.3) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -18.95 6) (size 1 3.3) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 18.95 0) (size 1 3.3) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -18.95 0) (size 1 3.3) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 18.95 -6) (size 1 3.3) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -18.95 -6) (size 1 3.3) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 18.95 -11.225) (size 1 1.75) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -18.95 -11.225) (size 1 1.75) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 17.4 12.6) (size 2.1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 17.4 -12.6) (size 2.1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 12 12.6) (size 3.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 12 -12.6) (size 3.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 6 12.6) (size 3.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 6 -12.6) (size 3.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 12.6) (size 3.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -12.6) (size 3.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -6 12.6) (size 3.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -6 -12.6) (size 3.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -12 12.6) (size 3.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -12 -12.6) (size 3.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -17.4 12.6) (size 2.1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -17.4 -12.6) (size 2.1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -18.95 12.6) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 18.95 12.6) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 18.95 -12.6) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -18.95 -12.6) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
  )
  (module Shielding_Cabinets:Würth_36103205_20x20mm (layer Kupfer_oben) (tedit 57A3A4A0)
    (at 168.59 98.22)
    (descr "WE-SHC Shielding Cabinet SMD 20x20mm")
    (tags "Shielding Cabinet")
    (attr smd)
    (fp_text reference J13 (at 0 -11.75) (layer F.SilkS))
    (fp_text value Schirmhaus_3.3V (at 0 11.75) (layer F.Fab))
    (pad 1 smd rect (at 10.25 8.6) (size 1 2.3) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -10.25 8.6) (size 1 2.3) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 10.25 3.75) (size 1 2.6) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -10.25 3.75) (size 1 2.6) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 10.25 -3.75) (size 1 2.6) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -10.25 -3.75) (size 1 2.6) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 10.25 -8.6) (size 1 2.3) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -10.25 -8.6) (size 1 2.3) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 8.6 10.25) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 8.6 -10.25) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.75 10.25) (size 2.6 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.75 -10.25) (size 2.6 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.75 10.25) (size 2.6 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.75 -10.25) (size 2.6 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -8.6 10.25) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -8.6 -10.25) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -10.25 10.25) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 10.25 10.25) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 10.25 -10.25) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -10.25 -10.25) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (model Shielding_Cabinets.3dshapes/Würth_36103205_20x20mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 229.2 134.57 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L32 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 3nH (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 63 "Net-(C93-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 229.28 130.02 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L31 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 6,8nH (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 64 "Net-(C93-Pad2)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 232.15 128.92 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L30 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 2,4nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 60 "Net-(C89-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 64 "Net-(C93-Pad2)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 232.14 124.76 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L29 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 6,2nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 60 "Net-(C89-Pad1)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 59 "Net-(C86-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Shielding_Cabinets:Laird_Technologies_BMI-S-101_13.66x12.70mm (layer Kupfer_oben) (tedit 57501709)
    (at 148.24 102.74)
    (descr "Laird Technologies BMI-S-101 Shielding Cabinet One Piece SMD 13.66x12.70mm")
    (tags "Shielding Cabinet")
    (attr smd)
    (fp_text reference J12 (at 0 -8.23) (layer F.SilkS))
    (fp_text value Schirmhaus_TCXO (at 0 8.23) (layer F.Fab))
    (pad 1 smd rect (at 6.25 5.165) (size 1 2.13) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -6.25 5.165) (size 1 2.13) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 6.25 0) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -6.25 0) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 6.25 -5.165) (size 1 2.13) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -6.25 -5.165) (size 1 2.13) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 4.925 6.73) (size 1.65 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 4.925 -6.73) (size 1.65 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 6.73) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -6.73) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -4.925 6.73) (size 1.65 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -4.925 -6.73) (size 1.65 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -6.25 6.73) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 6.25 6.73) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 6.25 -6.73) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -6.25 -6.73) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
  )
  (module Shielding_Cabinets:Laird_Technologies_BMI-S-203-F_26.21x26.21mm (layer Kupfer_oben) (tedit 57501709)
    (at 96.7305 130.494 180)
    (descr "Laird Technologies BMI-S-203-F Shielding Cabinet Two Piece SMD 26.21x26.21mm")
    (tags "Shielding Cabinet")
    (attr smd)
    (fp_text reference J5 (at 0 -14.505 180) (layer F.SilkS))
    (fp_text value SchirmhausTX-Mischer (at 0 14.505 180) (layer F.Fab))
    (pad 1 smd rect (at 13.005 11.22 180) (size 1 2.57) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -13.005 11.22 180) (size 1 2.57) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 13.005 5.835 180) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -13.005 5.835 180) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 13.005 0 180) (size 1 3.47) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -13.005 0 180) (size 1 3.47) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 13.005 -5.835 180) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -13.005 -5.835 180) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 13.005 -11.22 180) (size 1 2.57) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -13.005 -11.22 180) (size 1 2.57) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 11.22 13.005 180) (size 2.57 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 11.22 -13.005 180) (size 2.57 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 5.835 13.005 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 5.835 -13.005 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 13.005 180) (size 3.47 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -13.005 180) (size 3.47 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -5.835 13.005 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -5.835 -13.005 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -11.22 13.005 180) (size 2.57 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -11.22 -13.005 180) (size 2.57 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -13.005 13.005 180) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 13.005 13.005 180) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 13.005 -13.005 180) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -13.005 -13.005 180) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 163.97 100.03)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 164.02 97.89)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 167.21 91.06)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 101.8486 120.1928 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 4 Versorgung_LNB))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 162.41 93.06 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 106.7054 115.3668)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 4 Versorgung_LNB))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 101.9356 122.936 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 104.2362 125.349 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 173.66 96.95 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 6 "Net-(C9-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_10x10.5 (layer Kupfer_oben) (tedit 58AA917F)
    (at 102.62 95.99)
    (descr "SMT capacitor, aluminium electrolytic, 10x10.5")
    (attr smd)
    (fp_text reference C10 (at 0 6.46) (layer F.SilkS))
    (fp_text value 470uF (at 0 -6.46) (layer F.Fab))
    (fp_text user %R (at 0 6.46) (layer F.Fab))
    (fp_text user + (at -5.78 4.97) (layer F.SilkS))
    (fp_text user + (at -2.91 -0.08) (layer F.Fab))
    (pad 2 smd rect (at 4 0 180) (size 4 2.5) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -4 0 180) (size 4 2.5) (layers Kupfer_oben F.Paste F.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (model Capacitors_SMD.3dshapes/CP_Elec_10x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 88.03 107.9 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 8 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 165.95 103.48 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 9 "Net-(C13-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 107.5944 121.4936 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 4 Versorgung_LNB))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 175.67 99.8 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 10 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 98.5724 137.6312 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 161.54 105.58 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 171.96 103.55)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 171.96 105.51)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C19 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_8x10.5 (layer Kupfer_oben) (tedit 58AA8BC3)
    (at 189.103 103.38 270)
    (descr "SMT capacitor, aluminium electrolytic, 8x10.5")
    (attr smd)
    (fp_text reference C20 (at 0 5.45 270) (layer F.SilkS))
    (fp_text value 100uF (at 0 -5.45 270) (layer F.Fab))
    (fp_text user + (at -2.27 -0.08 270) (layer F.Fab))
    (fp_text user + (at -4.78 3.91 270) (layer F.SilkS))
    (fp_text user %R (at 0 5.45 270) (layer F.Fab))
    (pad 1 smd rect (at -3.05 0 90) (size 4 2.5) (layers Kupfer_oben F.Paste F.Mask)
      (net 4 Versorgung_LNB))
    (pad 2 smd rect (at 3.05 0 90) (size 4 2.5) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_8x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 194.818 101.6 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C21 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 4 Versorgung_LNB))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 196.85 101.6 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C22 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 4 Versorgung_LNB))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 214.249 100.564 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C23 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 12 "Net-(C23-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 228.62 108.29 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C24 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 13 Vcc_TX))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 226.46 108.31 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C25 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 13 Vcc_TX))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 224.25 108.28 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C26 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 13 Vcc_TX))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 117.55 130.13 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C27 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 8,2pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 14 "Net-(C27-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 119.36 135.9)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C28 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 15 "Net-(C28-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 124.12 88.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C29 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 150pF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 16 "Net-(C29-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 129.01 135.34 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C30 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 17 "Net-(C30-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 130.2 130.75)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C31 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 18 "Net-(C31-Pad2)"))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 19 "Net-(C31-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 120.86 93.62 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C32 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 1,1pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 20 "Net-(C32-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 16 "Net-(C29-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 115.92 97.06 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C33 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 620pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 21 "Net-(C33-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 128.26 125.03)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C34 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 22 "Net-(C34-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 117.18 100.32 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C35 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 0,8pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 23 "Net-(C35-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 21 "Net-(C33-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 119.11 125.09 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C36 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 22 "Net-(C34-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 132.31 132.69)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C37 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 24 "Net-(C37-Pad2)"))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 25 "Net-(C37-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 120.37 120.88 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C38 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 22 "Net-(C34-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 115.72 103.79 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C39 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 470pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 26 "Net-(C39-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 138.89 133.3)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C40 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 24 "Net-(C37-Pad2)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 27 Frontend_Ausgang))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 122.33 120.9 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C41 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 22 "Net-(C34-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 124.26 120.93 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C42 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 22 "Net-(C34-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 116.98 107.05 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C43 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 2,9pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 28 "Net-(C43-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 26 "Net-(C39-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 115.62 110.52)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C44 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 15pF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 29 "Net-(C44-Pad2)"))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 134.84 120.93 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C45 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 136.82 120.94 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C46 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 115.63 114.65)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C47 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 39pF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 30 "Net-(C47-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 143.51 133.3)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C48 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 330pF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 31 "Net-(C48-Pad2)"))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 27 Frontend_Ausgang))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 174.69 120.89 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C49 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 1,1pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 32 "Net-(C49-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 146.8 134.54 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C50 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 33 "Net-(C50-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 31 "Net-(C48-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 146.8 139.25 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C51 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 33 "Net-(C50-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 148.3 106.14 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C52 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 164.65 127.74 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C53 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 2,6pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 34 "Net-(C53-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 146.26 106.14 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C54 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 154.94 139.7 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C55 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 100pF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 1 +5VA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 144.27 106.12 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C56 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 160.02 139.7 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C57 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 35 "Net-(C57-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 158.97 115.04 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C58 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 36 "Net-(C58-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 166.37 139.7 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C59 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 37 "Net-(C59-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 160.85 115.21 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C60 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 36 "Net-(C58-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 168.275 139.7 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C61 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 37 "Net-(C59-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 158.41 134.46 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C62 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value optional (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 38 "Net-(C62-Pad2)"))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 39 "Net-(C62-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 170.18 139.7 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C63 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 37 "Net-(C59-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 153 114.39 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C64 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 40 "Net-(C64-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 153 116.29 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C65 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 40 "Net-(C64-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 164.65 130.06)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C66 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 41 "Net-(C66-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 42 Frontend_Lokaloszillator))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 147.77 115.37 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C67 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 43 "Net-(C67-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 147.82 117.34 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C68 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 43 "Net-(C67-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 168.87 134.41 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C69 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 44 "Net-(C69-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 149.87 127.16 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C70 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 2nF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 45 "Net-(C70-Pad2)"))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 46 "Net-(C70-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 148.62 123.62 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C71 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 16nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 45 "Net-(C70-Pad2)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 47 "Net-(C71-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 146.61 123.63 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C72 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 48 "Net-(C72-Pad2)"))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 45 "Net-(C70-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 165.91 122.52)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C73 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 0,7pF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 49 "Net-(C73-Pad2)"))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 50 "Net-(C73-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 164.95 116.64 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C74 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 0,7pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 51 "Net-(C74-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 168.42 118.12)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C75 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 49 "Net-(C73-Pad2)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 52 "Net-(C75-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 159.57 114.51 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C76 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 157.62 114.49 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C77 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 11 3V3_LO_Frontend))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 155.7 114.48 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C78 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 100pF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 181.59 133.14 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C79 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 82pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 53 "Net-(C79-Pad2)"))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 54 Sendezweig_Mischer_Ausgang))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 180.58 136.96 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C80 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 82pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 55 "Net-(C80-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 193.16 118.51 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C81 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1,3pF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 54 Sendezweig_Mischer_Ausgang))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 195.37 118.51 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C82 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1,3pF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 56 "Net-(C82-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 212.73 117.28 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C83 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 57 "Net-(C83-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 58 "Net-(C83-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 214.71 125.51 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C84 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 218.55 125.51 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C85 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 229.01 123.66 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C86 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 1pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 59 "Net-(C86-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 220.43 125.51 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C87 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 68pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 216.65 125.51 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C88 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 229.01 125.85 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C89 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 2,4pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 60 "Net-(C89-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 217.33 118.58 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C90 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 100pF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 13 Vcc_TX))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 221.45 117.28 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C91 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 61 "Net-(C91-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 62 "Net-(C91-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 222.27 108.28 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C92 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 3,3nF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 13 Vcc_TX))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 232.15 133.32 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C93 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 1,1pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 63 "Net-(C93-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 64 "Net-(C93-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 230.72 108.3 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C94 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 13 Vcc_TX))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 215.31 118.57 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C95 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 13 Vcc_TX))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 232.16 138.16 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C96 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 2,8pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 63 "Net-(C93-Pad1)"))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 65 "Net-(C96-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 225.39 118.59 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C97 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 13 Vcc_TX))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 223.43 118.62 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C98 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 13 Vcc_TX))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 219.5 118.57 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C99 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 3,3nF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 13 Vcc_TX))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 221.43 118.59 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C100 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 3,3nF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 13 Vcc_TX))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 233.72 81.93)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C101 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 66 "Net-(C101-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 67 "Net-(C101-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 229.03 81.91)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C102 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 2.6pF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 68 "Net-(C102-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 66 "Net-(C101-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 226.44 80.02)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C103 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 4.7pF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 68 "Net-(C102-Pad1)"))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 69 "Net-(C103-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 225.19 75.08 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C104 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 2,4pF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 69 "Net-(C103-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 222.99 81.48 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C105 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 5,9pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 70 "Net-(C105-Pad2)"))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 220.84 73.14 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C106 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 71 "Net-(C106-Pad2)"))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 72 "Net-(C106-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 199.333 80.948 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C107 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 201.293 80.948 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C108 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 203.198 80.948 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C109 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 68pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 205.103 80.948 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C110 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 209.39 67.46)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C111 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 73 "Net-(C111-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 74 "Net-(C111-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 210.691 81.075 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C112 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 212.596 81.075 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C113 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 214.501 81.075 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C114 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 68pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 216.406 81.075 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C115 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 203.9 67.48)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C116 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 75 "Net-(C116-Pad2)"))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 76 "Net-(C116-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 180.69 63.35 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C117 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 77 "Net-(C117-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 182.66 63.38 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C118 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 77 "Net-(C117-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 176.96 62.73 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C119 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 10pF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 78 "Net-(C119-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 191.59 71.53 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C120 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 79 RX-Frontend-Mischer))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 80 "Net-(C120-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 178.84 62.75 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C121 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 0,1uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 78 "Net-(C119-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 185.68 78.25 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C122 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 4,7pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 81 "Net-(C122-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 186 74.83)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C123 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 4,7pF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 82 "Net-(C123-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 80 "Net-(C120-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 175.01 58.62 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C124 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 10pF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 83 "Net-(C124-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 173.05 58.59 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C125 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 0,1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 83 "Net-(C124-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 181.47 80.25 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C126 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 84 "Net-(C126-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 161.92 63.9 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C127 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 85 "Net-(C127-Pad2)"))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 86 "Net-(C127-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 178.68 71.2 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C128 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 4,7pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 87 "Net-(C128-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 160.64 67.46 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C129 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 53nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 88 "Net-(C129-Pad2)"))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 85 "Net-(C127-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 174.98 81.25 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C130 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 89 RX_Lokaloszillator))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 90 "Net-(C130-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 158.04 62.79 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C131 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 91 "Net-(C131-Pad2)"))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 85 "Net-(C127-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 175.62 74.52 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C132 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 4,7pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 92 "Net-(C132-Pad2)"))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 93 "Net-(C132-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 167.09 70.23 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C133 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 0,7pF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 94 "Net-(C133-Pad2)"))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 95 "Net-(C133-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 170.36 69.67)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C134 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 0,7pF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 96 "Net-(C134-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 165.1 72.74 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C135 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 97 "Net-(C135-Pad2)"))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 94 "Net-(C133-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 160.05 65.95 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C136 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 11 3V3_LO_Frontend))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 174.34 69.21 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C137 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 33pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 92 "Net-(C132-Pad2)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 98 "Net-(C137-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 161.88 65.96 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C138 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 11 3V3_LO_Frontend))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 163.72 65.99 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C139 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 100pF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 176.85 80.13)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C140 (at 0 1.75) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 99 "Net-(C140-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 179.57 67.91 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C141 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 150pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 98 "Net-(C137-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 176.85 82)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C142 (at 0 1.75) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 99 "Net-(C140-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 176.85 83.94)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C143 (at 0 1.75) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 99 "Net-(C140-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 174.34 64.49 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C144 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 390pF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 100 "Net-(C144-Pad2)"))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 159.9 78.79 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C145 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 2,3pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 101 "Net-(C145-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 159.88 81.08 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C146 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 7,5pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 102 "Net-(C146-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 176.82 90.08)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C147 (at 0 1.75) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 103 "Net-(C147-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_oben) (tedit 58AA84A8)
    (at 161.64 83.35 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C148 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 2,3pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 89 RX_Lokaloszillator))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Kupfer_unten) (tedit 58AA84A8)
    (at 170.5 86.46 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C149 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 100pF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 1 +5VA))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0805 (layer Kupfer_oben) (tedit 590CE9A4)
    (at 136.1845 57.825 270)
    (descr "Diode SMD in 0805 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D1 (at 0 -1.6 270) (layer F.SilkS))
    (fp_text value 1N4001 (at 0 1.7 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.6 270) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 270) (size 0.8 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 104 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.05 0 270) (size 0.8 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0805 (layer Kupfer_oben) (tedit 590CE9A4)
    (at 179.26 115.34)
    (descr "Diode SMD in 0805 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D5 (at 0 -1.6) (layer F.SilkS))
    (fp_text value LED (at 0 1.7) (layer F.Fab))
    (fp_text user %R (at 0 -1.6) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.8 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 108 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.8 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 109 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0805 (layer Kupfer_oben) (tedit 590CE9A4)
    (at 182.93 58.44)
    (descr "Diode SMD in 0805 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D9 (at 0 -1.6) (layer F.SilkS))
    (fp_text value LED (at 0 1.7) (layer F.Fab))
    (fp_text user %R (at 0 -1.6) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 0.8 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 113 "Net-(D9-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 0.8 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 114 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:DEA162450BT1295A1 (layer Kupfer_oben) (tedit 0)
    (at 198.85 117.26)
    (descr DEA162450BT-1295A1)
    (tags Filter)
    (attr smd)
    (fp_text reference FL1 (at 0.125 0) (layer F.SilkS))
    (fp_text value DEA162450BT-1295A1 (at 0.125 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0.125 0) (layer F.Fab))
    (pad 1 smd rect (at -0.375 0 90) (size 0.3 0.5) (layers Kupfer_oben F.Paste F.Mask)
      (net 56 "Net-(C82-Pad1)"))
    (pad 2 smd rect (at 0.475 0.45 90) (size 0.5 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.325 0 90) (size 0.3 0.5) (layers Kupfer_oben F.Paste F.Mask)
      (net 115 "Net-(FL1-Pad3)"))
    (pad 4 smd rect (at 0.475 -0.45 90) (size 0.5 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
  )
  (module SamacSys_Parts:KTT0003B (layer Kupfer_oben) (tedit 0)
    (at 90.9574 121.2662 270)
    (descr KTT0003B)
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC1 (at 3.448 -0.167 270) (layer F.SilkS))
    (fp_text value LM7805SX_NOPB (at 3.448 -0.167 270) (layer F.SilkS) hide)
    (fp_text user %R (at 3.448 -0.167 270) (layer F.Fab))
    (pad 6 smd rect (at -0.545 4.7825) (size 1.235 1.91) (layers Kupfer_oben F.Paste F.Mask))
    (pad 5 smd rect (at -0.545 -4.7825) (size 1.235 1.91) (layers Kupfer_oben F.Paste F.Mask))
    (pad 4 smd rect (at 2 0 270) (size 7 8.33) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 12.67 -2.54) (size 1.07 2.16) (layers Kupfer_oben F.Paste F.Mask)
      (net 116 "Net-(IC1-Pad3)"))
    (pad 2 smd rect (at 12.67 0) (size 1.07 2.16) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 12.67 2.54) (size 1.07 2.16) (layers Kupfer_oben F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer Kupfer_oben) (tedit 58CD0CDA)
    (at 169.69 98.36 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC2 (at 0 -3.5 90) (layer F.SilkS))
    (fp_text value ADM7154ARDZ-3.3-R7 (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers Kupfer_oben F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers Kupfer_oben F.Paste F.Mask)
      (net 117 "Net-(IC2-Pad7)"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers Kupfer_oben F.Paste F.Mask)
      (net 6 "Net-(C9-Pad1)"))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers Kupfer_oben F.Paste F.Mask)
      (net 6 "Net-(C9-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers Kupfer_oben F.Paste F.Mask)
      (net 10 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers Kupfer_oben F.Paste F.Mask)
      (net 9 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:KTT0003B (layer Kupfer_oben) (tedit 0)
    (at 230.886 101.8105 180)
    (descr KTT0003B)
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC3 (at 3.448 -0.167 180) (layer F.SilkS))
    (fp_text value LM7805SX_NOPB (at 3.448 -0.167 180) (layer F.SilkS) hide)
    (fp_text user %R (at 3.448 -0.167 180) (layer F.Fab))
    (pad 1 smd rect (at 12.67 2.54 270) (size 1.07 2.16) (layers Kupfer_oben F.Paste F.Mask)
      (net 12 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 12.67 0 270) (size 1.07 2.16) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 12.67 -2.54 270) (size 1.07 2.16) (layers Kupfer_oben F.Paste F.Mask)
      (net 13 Vcc_TX))
    (pad 4 smd rect (at 2 0 180) (size 7 8.33) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -0.545 -4.7825 270) (size 1.235 1.91) (layers Kupfer_oben F.Paste F.Mask))
    (pad 6 smd rect (at -0.545 4.7825 270) (size 1.235 1.91) (layers Kupfer_oben F.Paste F.Mask))
  )
  (module SamacSys_Parts:SOP65P640X120-14N (layer Kupfer_oben) (tedit 0)
    (at 123.67 132.04)
    (descr AD8367ARUZ)
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC4 (at 0 0) (layer F.SilkS))
    (fp_text value AD8367ARUZ (at 0 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.938 -1.95 90) (size 0.45 1.475) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.938 -1.3 90) (size 0.45 1.475) (layers Kupfer_oben F.Paste F.Mask)
      (net 118 "Net-(IC4-Pad2)"))
    (pad 3 smd rect (at -2.938 -0.65 90) (size 0.45 1.475) (layers Kupfer_oben F.Paste F.Mask)
      (net 14 "Net-(C27-Pad1)"))
    (pad 4 smd rect (at -2.938 0 90) (size 0.45 1.475) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -2.938 0.65 90) (size 0.45 1.475) (layers Kupfer_oben F.Paste F.Mask)
      (net 15 "Net-(C28-Pad1)"))
    (pad 6 smd rect (at -2.938 1.3 90) (size 0.45 1.475) (layers Kupfer_oben F.Paste F.Mask)
      (net 15 "Net-(C28-Pad1)"))
    (pad 7 smd rect (at -2.938 1.95 90) (size 0.45 1.475) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.938 1.95 90) (size 0.45 1.475) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.938 1.3 90) (size 0.45 1.475) (layers Kupfer_oben F.Paste F.Mask)
      (net 17 "Net-(C30-Pad1)"))
    (pad 10 smd rect (at 2.938 0.65 90) (size 0.45 1.475) (layers Kupfer_oben F.Paste F.Mask)
      (net 25 "Net-(C37-Pad1)"))
    (pad 11 smd rect (at 2.938 0 90) (size 0.45 1.475) (layers Kupfer_oben F.Paste F.Mask)
      (net 119 "Net-(IC4-Pad11)"))
    (pad 12 smd rect (at 2.938 -0.65 90) (size 0.45 1.475) (layers Kupfer_oben F.Paste F.Mask)
      (net 120 "Net-(IC4-Pad12)"))
    (pad 13 smd rect (at 2.938 -1.3 90) (size 0.45 1.475) (layers Kupfer_oben F.Paste F.Mask)
      (net 19 "Net-(C31-Pad1)"))
    (pad 14 smd rect (at 2.938 -1.95 90) (size 0.45 1.475) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model D:\Kicad\lib\SamacSys_Parts.3dshapes\AD8367ARUZ.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:ST-SOT-89 (layer Kupfer_oben) (tedit 0)
    (at 217.09 115.795)
    (descr ST-SOT-89)
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC5 (at -0.313 -1.407) (layer F.SilkS))
    (fp_text value ADL5602 (at -0.313 -1.407) (layer F.SilkS) hide)
    (fp_text user %R (at -0.313 -1.407) (layer F.Fab))
    (pad 1 smd rect (at -1.5 1.475) (size 0.57 1.4) (layers Kupfer_oben F.Paste F.Mask)
      (net 57 "Net-(C83-Pad1)"))
    (pad 2 smd rect (at 0 1.575) (size 0.65 1.2) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.5 1.475) (size 0.57 1.4) (layers Kupfer_oben F.Paste F.Mask)
      (net 62 "Net-(C91-Pad2)"))
    (pad 4 smd rect (at 0 -0.6) (size 2 3.15) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
  )
  (module SamacSys_Parts:SKY6629411 (layer Kupfer_oben) (tedit 0)
    (at 227.99 117.72)
    (descr SKY66294-11-2)
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC6 (at -0.2 0) (layer F.SilkS))
    (fp_text value SKY66292-11 (at -0.2 0) (layer F.SilkS) hide)
    (fp_text user %R (at -0.2 0) (layer F.Fab))
    (pad 1 smd rect (at -2.315 -1.2 90) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.315 -0.4 90) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 61 "Net-(C91-Pad1)"))
    (pad 3 smd rect (at -2.315 0.4 90) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.315 1.2 90) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.2 2.315) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 13 Vcc_TX))
    (pad 6 smd rect (at -0.4 2.315) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 121 "Net-(IC6-Pad6)"))
    (pad 7 smd rect (at 0.4 2.315) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 1.2 2.315) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.315 1.2 90) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 59 "Net-(C86-Pad1)"))
    (pad 10 smd rect (at 2.315 0.4 90) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 2.315 -0.4 90) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 2.315 -1.2 90) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 13 Vcc_TX))
    (pad 13 smd rect (at 1.2 -2.315) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 0.4 -2.315) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 13 Vcc_TX))
    (pad 15 smd rect (at -0.4 -2.315) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at -1.2 -2.315) (size 0.5 0.67) (layers Kupfer_oben F.Paste F.Mask)
      (net 13 Vcc_TX))
    (pad 17 smd rect (at -1 -1) (size 0.875 0.875) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 18 smd rect (at 0 -1) (size 0.875 0.875) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 1 -1) (size 0.875 0.875) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at -1 0) (size 0.875 0.875) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 21 smd rect (at 0 0) (size 0.875 0.875) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 1 0) (size 0.875 0.875) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 23 smd rect (at -1 1) (size 0.875 0.875) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at 0 1) (size 0.875 0.875) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 25 smd rect (at 1 1) (size 0.875 0.875) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model D:\Kicad\lib\SamacSys_Parts.3dshapes\SKY66294-11.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:ST-SOT-89 (layer Kupfer_oben) (tedit 0)
    (at 212.15 71.25 180)
    (descr ST-SOT-89)
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC7 (at -0.313 -1.407 180) (layer F.SilkS))
    (fp_text value ADL5602 (at -0.313 -1.407 180) (layer F.SilkS) hide)
    (fp_text user %R (at -0.313 -1.407 180) (layer F.Fab))
    (pad 4 smd rect (at 0 -0.6 180) (size 2 3.15) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.5 1.475 180) (size 0.57 1.4) (layers Kupfer_oben F.Paste F.Mask)
      (net 74 "Net-(C111-Pad2)"))
    (pad 2 smd rect (at 0 1.575 180) (size 0.65 1.2) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.5 1.475 180) (size 0.57 1.4) (layers Kupfer_oben F.Paste F.Mask)
      (net 122 "Net-(IC7-Pad1)"))
  )
  (module SamacSys_Parts:ST-SOT-89 (layer Kupfer_oben) (tedit 0)
    (at 206.66 71.255 180)
    (descr ST-SOT-89)
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC8 (at -0.313 -1.407 180) (layer F.SilkS))
    (fp_text value ADL5602 (at -0.313 -1.407 180) (layer F.SilkS) hide)
    (fp_text user %R (at -0.313 -1.407 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 1.475 180) (size 0.57 1.4) (layers Kupfer_oben F.Paste F.Mask)
      (net 73 "Net-(C111-Pad1)"))
    (pad 2 smd rect (at 0 1.575 180) (size 0.65 1.2) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.5 1.475 180) (size 0.57 1.4) (layers Kupfer_oben F.Paste F.Mask)
      (net 75 "Net-(C116-Pad2)"))
    (pad 4 smd rect (at 0 -0.6 180) (size 2 3.15) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
  )
  (module TerminalBlocks_WAGO:TerminalBlock_WAGO-236_2Stift_RM5mm_2pol (layer Kupfer_oben) (tedit 0)
    (at 88.54 86.16 90)
    (descr "WAGO-Series 236, 2Stift, 2pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 2pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J1 (at 0 -8.89 90) (layer F.SilkS))
    (fp_text value "Eingang 12V" (at 0 8.89 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.413 -2.54 180) (size 2.99974 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 123 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 2.413 2.54 180) (size 2.99974 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 123 "Net-(J1-Pad2)"))
    (pad 1 thru_hole oval (at -2.54 -2.54 180) (size 2.99974 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole oval (at -2.54 2.54 180) (size 2.99974 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Socket_Strips:Socket_Strip_Straight_2x01_Pitch2.54mm_SMD (layer Kupfer_oben) (tedit 58CD5448)
    (at 97.72 83.717 180)
    (descr "surface-mounted straight socket strip, 2x01, 2.54mm pitch, double rows")
    (tags "Surface mounted socket strip SMD 2x01 2.54mm double row")
    (attr smd)
    (fp_text reference J2 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Pads (at 0 2.33 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 2 smd rect (at -2.52 0 180) (size 3 1) (layers Kupfer_oben F.Paste F.Mask)
      (net 124 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at 2.52 0 180) (size 3 1) (layers Kupfer_oben F.Paste F.Mask)
      (net 123 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x01_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Shielding_Cabinets:Laird_Technologies_BMI-S-203-F_26.21x26.21mm (layer Kupfer_oben) (tedit 57501709)
    (at 125.9 130.46)
    (descr "Laird Technologies BMI-S-203-F Shielding Cabinet Two Piece SMD 26.21x26.21mm")
    (tags "Shielding Cabinet")
    (attr smd)
    (fp_text reference J3 (at 0 -14.505) (layer F.SilkS))
    (fp_text value SchirmhausStromversorgung (at 0 14.505) (layer F.Fab))
    (pad 1 smd rect (at 13.005 11.22) (size 1 2.57) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -13.005 11.22) (size 1 2.57) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 13.005 5.835) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -13.005 5.835) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 13.005 0) (size 1 3.47) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -13.005 0) (size 1 3.47) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 13.005 -5.835) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -13.005 -5.835) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 13.005 -11.22) (size 1 2.57) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -13.005 -11.22) (size 1 2.57) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 11.22 13.005) (size 2.57 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 11.22 -13.005) (size 2.57 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 5.835 13.005) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 5.835 -13.005) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 13.005) (size 3.47 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -13.005) (size 3.47 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -5.835 13.005) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -5.835 -13.005) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -11.22 13.005) (size 2.57 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -11.22 -13.005) (size 2.57 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -13.005 13.005) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 13.005 13.005) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 13.005 -13.005) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -13.005 -13.005) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
  )
  (module w_conn_rf:sma_straight_32k101-400l5 (layer Kupfer_oben) (tedit 0)
    (at 240.43 139.44)
    (descr "SMA straight female connector, Rosenberger 32K101-400L5")
    (fp_text reference J7 (at 0 4.8) (layer F.SilkS))
    (fp_text value TX_Ausgang (at 0 -4.8) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.3 2.3) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(C96-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.5 2.5) (drill 1.45) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.5 2.5) (drill 1.45) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.5 2.5) (drill 1.45) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.5 2.5) (drill 1.45) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model walter/conn_rf/sma_straight_32k101-400l5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_rf:sma_straight_32k101-400l5 (layer Kupfer_oben) (tedit 0)
    (at 240.44 81.9)
    (descr "SMA straight female connector, Rosenberger 32K101-400L5")
    (fp_text reference J8 (at 0 4.8) (layer F.SilkS))
    (fp_text value LNB_Eingang (at 0 -4.8) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.5 2.5) (drill 1.45) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.5 2.5) (drill 1.45) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.5 2.5) (drill 1.45) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.5 2.5) (drill 1.45) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.3 2.3) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(C101-Pad2)"))
    (model walter/conn_rf/sma_straight_32k101-400l5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Shielding_Cabinets:Laird_Technologies_BMI-S-210-F_44.00x30.50mm (layer Kupfer_oben) (tedit 57501709)
    (at 171.77 70.24)
    (descr "Laird Technologies BMI-S-210-F Shielding Cabinet Two Piece SMD 44.00x30.50mm")
    (tags "Shielding Cabinet")
    (attr smd)
    (fp_text reference J10 (at 0 -16.65) (layer F.SilkS))
    (fp_text value SchirmhausFrontend-Mischer (at 0 16.65) (layer F.Fab))
    (pad 1 smd rect (at 21.9 13.875) (size 1 1.55) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 13.875) (size 1 1.55) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 9) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 9) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 3) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 3) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 -3) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 -3) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 -9) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 -9) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 -13.875) (size 1 1.55) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 -13.875) (size 1 1.55) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 20.25 15.15) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 20.25 -15.15) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 15 15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 15 -15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 9 15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 9 -15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3 15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3 -15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3 15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3 -15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -9 15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -9 -15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -15 15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -15 -15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -20.25 15.15) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -20.25 -15.15) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 15.15) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 15.15) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 -15.15) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 -15.15) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_0402_NoSilk (layer Kupfer_oben) (tedit 58E0A804)
    (at 119.56 127.95 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference JP1 (at 0 -1.2 270) (layer F.SilkS))
    (fp_text value Jumper (at 0 1.25 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.2 270) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers Kupfer_oben F.Paste F.Mask)
      (net 118 "Net-(IC4-Pad2)"))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0805_HandSoldering (layer Kupfer_oben) (tedit 58307B90)
    (at 164.17 95.6 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L1 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 326185210 (at 0 2.1 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0805_HandSoldering (layer Kupfer_oben) (tedit 58307B90)
    (at 105.4862 121.586 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L2 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 326385156 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 4 Versorgung_LNB))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0805_HandSoldering (layer Kupfer_oben) (tedit 58307B90)
    (at 85.69 105.3 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L3 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 326385068 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 8 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0805_HandSoldering (layer Kupfer_oben) (tedit 58307B90)
    (at 97.2024 133.9512 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L5 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 326385068 (at 0 2.1 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 116 "Net-(IC1-Pad3)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_Wuerth_WE-PD-Typ-LS (layer Kupfer_oben) (tedit 5990349D)
    (at 205.356 103.505)
    (descr "Choke, Drossel, WE-PD Typ LS, Wuerth, SMD,")
    (tags "Choke Drossel WE-PDTypLS Wuerth SMD ")
    (attr smd)
    (fp_text reference L6 (at 0 -7.3) (layer F.SilkS))
    (fp_text value 10uH (at 0 7.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 4.95 0) (size 2.9 5.4) (layers Kupfer_oben F.Paste F.Mask)
      (net 12 "Net-(C23-Pad1)"))
    (pad 1 smd rect (at -4.95 0) (size 2.9 5.4) (layers Kupfer_oben F.Paste F.Mask)
      (net 4 Versorgung_LNB))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Wuerth_WE-PD-Typ-LS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 116.46 133.31)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L7 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100nH (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 136 "Net-(L18-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 14 "Net-(C27-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 119.76 90.45 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L8 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 7,5nH (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 16 "Net-(C29-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 119.09 95.97 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L9 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 1,1uH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 21 "Net-(C33-Pad1)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 20 "Net-(C32-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 122.02 97.07)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L10 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 2nH (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 21 "Net-(C33-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 118.92 102.68 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L11 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 1,5uH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 23 "Net-(C35-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 26 "Net-(C39-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 133.56 135.87 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L12 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 120nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 24 "Net-(C37-Pad2)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 121.88 103.79)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L13 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 2,7nH (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 26 "Net-(C39-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_1206_HandSoldering (layer Kupfer_oben) (tedit 58307C0D)
    (at 128.56 122.18 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference L14 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value 326396210 (at 0 2.3 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers Kupfer_oben F.Paste F.Mask)
      (net 22 "Net-(C34-Pad1)"))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers Kupfer_oben F.Paste F.Mask)
      (net 137 "Net-(L14-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 118.8 109.41 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L15 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 430nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 28 "Net-(C43-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 29 "Net-(C44-Pad2)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 131.78 119.68)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L16 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10uH (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 137 "Net-(L14-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 118.8 113.55 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L17 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 100nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 30 "Net-(C47-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 29 "Net-(C44-Pad2)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 115.41 129.78 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L18 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 39nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 30 "Net-(C47-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 136 "Net-(L18-Pad2)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 174.57 126.57 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L19 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 6,2nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 32 "Net-(C49-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 34 "Net-(C53-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 147.9 130.48)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L20 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 10nH (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 138 "Net-(L20-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 31 "Net-(C48-Pad2)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 167.88 128.92 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L21 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 2,7nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 42 Frontend_Lokaloszillator))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 34 "Net-(C53-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0805_HandSoldering (layer Kupfer_unten) (tedit 58307B90)
    (at 157.48 139.7 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L22 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 326185210 (at 0 -2.1 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 1 +5VA))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 35 "Net-(C57-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_unten) (tedit 58307AEF)
    (at 163.195 138.43)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L23 (at 0 1.9) (layer B.SilkS))
    (fp_text value 10uH (at 0 -1.9) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers Kupfer_unten B.Paste B.Mask)
      (net 35 "Net-(C57-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers Kupfer_unten B.Paste B.Mask)
      (net 37 "Net-(C59-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 162.73 118.91 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L24 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 10nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 51 "Net-(C74-Pad1)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 162.74 123.61 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L25 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 3,3nH (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 50 "Net-(C73-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 166.06 120.03 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L26 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 3,3nH (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 49 "Net-(C73-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 51 "Net-(C74-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 194.28 115.27)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L27 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 6,2nH (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 54 Sendezweig_Mischer_Ausgang))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 56 "Net-(C82-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 218.57 120.82 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L28 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 470nH (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 62 "Net-(C91-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 240.49 87.86 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L33 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 180nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 4 Versorgung_LNB))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 67 "Net-(C101-Pad2)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 230.32 78.72 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L34 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 8.2nH (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 66 "Net-(C101-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 227.71 76.8 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L35 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 7.5nH (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 68 "Net-(C102-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 225.17 83.05 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L36 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 33nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 69 "Net-(C103-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 224.07 78.28 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L37 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 15nH (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 70 "Net-(C105-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 69 "Net-(C103-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 221.88 76.47 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L38 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 6.2nH (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 71 "Net-(C106-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 70 "Net-(C105-Pad2)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 210.65 75.99 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L39 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 470nH (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 74 "Net-(C111-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 205.15 76.04 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L40 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 470nH (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 75 "Net-(C116-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 191.58 75.98 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L41 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 15nH (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 80 "Net-(C120-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 189.44 75.9 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L42 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 6,8nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 81 "Net-(C122-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 80 "Net-(C120-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 184.75 71.55 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L43 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 6,8nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 82 "Net-(C123-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 178.65 80.2 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L44 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 15nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 90 "Net-(C130-Pad1)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 139 "Net-(L44-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 170.8 67.84 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L45 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 10nH (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 96 "Net-(C134-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 176.9 77.56 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L46 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 270nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 93 "Net-(C132-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 99 "Net-(C140-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 175.53 72.45 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L47 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 270nH (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 87 "Net-(C128-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 92 "Net-(C132-Pad2)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 166.3 67.05)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L48 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 3,3nH (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 95 "Net-(C133-Pad1)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 168.22 73.56)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L49 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 3,3nH (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 94 "Net-(C133-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 96 "Net-(C134-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 174.36 77.65 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L50 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 270nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 92 "Net-(C132-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 99 "Net-(C140-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 176.21 66.83 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L51 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 1uH (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 100 "Net-(C144-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 98 "Net-(C137-Pad2)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_unten) (tedit 58307AEF)
    (at 175.58 87.05 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L52 (at 0 1.9 90) (layer B.SilkS))
    (fp_text value 10uH (at 0 -1.9 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Kupfer_unten B.Paste B.Mask)
      (net 99 "Net-(C140-Pad1)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Kupfer_unten B.Paste B.Mask)
      (net 103 "Net-(C147-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 177.95 64.62 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L53 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 390nH (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 135 RX_Teil))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 100 "Net-(C144-Pad2)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 163.11 80.02 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L54 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 15nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 102 "Net-(C146-Pad1)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 101 "Net-(C145-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603_HandSoldering (layer Kupfer_oben) (tedit 58307AEF)
    (at 164.84 82.22 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L55 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 15nH (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 102 "Net-(C146-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers Kupfer_oben F.Paste F.Mask)
      (net 89 RX_Lokaloszillator))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0805_HandSoldering (layer Kupfer_unten) (tedit 58307B90)
    (at 171.85 90.02 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L56 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 326185210 (at 0 -2.1 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 1 +5VA))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 103 "Net-(C147-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer Kupfer_oben) (tedit 58CE4E7E)
    (at 104.79 84.887 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value IRLML5203 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 140 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 124 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer Kupfer_oben) (tedit 58CE4E7E)
    (at 136.1845 62.765 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value BC817 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 104 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 141 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer Kupfer_oben) (tedit 58CE4E7E)
    (at 117.11 138.75 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value BC858W (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 142 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 15 "Net-(C28-Pad1)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer Kupfer_oben) (tedit 58CE4E7E)
    (at 175.53 115.33)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC817 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 143 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 109 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer Kupfer_oben) (tedit 58CE4E7E)
    (at 222.33 132.53)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC817 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 144 "Net-(Q5-Pad3)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 145 "Net-(Q5-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer Kupfer_oben) (tedit 58CE4E7E)
    (at 179.28 58.48)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC817 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 113 "Net-(D9-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers Kupfer_oben F.Paste F.Mask)
      (net 146 "Net-(Q6-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 167.29 93.03)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 117 "Net-(IC2-Pad7)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 172.2 93.03)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 117 "Net-(IC2-Pad7)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 102.53 87.907 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 140 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 136.5645 66.495)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 126 Eingangs-Umschalter))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 141 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 119.52 141.63 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 142 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 121.47 139.71)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 33k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 142 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2512_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 116.77 71.86 180)
    (descr "Resistor SMD 2512, hand soldering")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R7 (at 0 -2.6 180) (layer F.SilkS))
    (fp_text value 62 (at 0 2.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -3.95 0 180) (size 2.7 3.2) (layers Kupfer_oben F.Paste F.Mask)
      (net 134 "Net-(K1-Pad14)"))
    (pad 2 smd rect (at 3.95 0 180) (size 2.7 3.2) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2816_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 125.67 75.92 90)
    (descr "Resistor SMD 2816, hand soldering, Vishay (see WSL-VISHAY.PDF)")
    (tags "resistor 2816")
    (attr smd)
    (fp_text reference R8 (at 0 -3.36 90) (layer F.SilkS))
    (fp_text value 250 (at 0 3.81 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 4.06 0 90) (size 4.7 4.7) (layers Kupfer_oben F.Paste F.Mask)
      (net 134 "Net-(K1-Pad14)"))
    (pad 1 smd rect (at -4.06 0 90) (size 4.7 4.7) (layers Kupfer_oben F.Paste F.Mask)
      (net 147 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2816.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2512_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 116.77 79.98 180)
    (descr "Resistor SMD 2512, hand soldering")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R9 (at 0 -2.6 180) (layer F.SilkS))
    (fp_text value 62 (at 0 2.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 3.95 0 180) (size 2.7 3.2) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.95 0 180) (size 2.7 3.2) (layers Kupfer_oben F.Paste F.Mask)
      (net 147 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 119.51 83.63 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 62 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 147 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 120.86 87.17 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 250 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 147 "Net-(R10-Pad1)"))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 16 "Net-(C29-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 117.42 88.53 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 62 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 16 "Net-(C29-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 131.78 127.08 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 18 "Net-(C31-Pad2)"))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 124.85 126.39 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 4,7 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 120 "Net-(IC4-Pad12)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 22 "Net-(C34-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 122.44 126.44 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 4,7 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 119 "Net-(IC4-Pad11)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 22 "Net-(C34-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_unten) (tedit 58E0A804)
    (at 162.24 127.93 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 132 Sendezweig_LE))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 105 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 156.34 137.14 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 121 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 38 "Net-(C62-Pad2)"))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 156.34 131.84 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 121 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 39 "Net-(C62-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_unten) (tedit 58E0A804)
    (at 157.58 128.81 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 130 Sendezweig_DATA))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 106 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_unten) (tedit 58E0A804)
    (at 155.07 127.98 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 107 "Net-(D4-Pad1)"))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 128 Sendezweig_CLK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 156.92 115.26 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R21 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 4,7k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 148 "Net-(R21-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 170.99 114.38 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R22 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 149 "Net-(R22-Pad2)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 143 "Net-(Q4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 151.14 123.74 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R23 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 560 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 47 "Net-(C71-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 46 "Net-(C70-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 180.32 118.77 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R24 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 108 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 153.45 123.76 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R25 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 48 "Net-(C72-Pad2)"))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 46 "Net-(C70-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 169.71 123.57 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R26 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value xy (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 52 "Net-(C75-Pad2)"))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 171.08 120.13 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R27 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value xy (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 32 "Net-(C49-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 52 "Net-(C75-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 172.43 123.54 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R28 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value xy (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 32 "Net-(C49-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 202.58 118.62 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R29 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value xy (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 115 "Net-(FL1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 205.95 117.27 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R30 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value xy (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 58 "Net-(C83-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 115 "Net-(FL1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 209.33 118.64 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R31 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value xy (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 58 "Net-(C83-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 220 129.71 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R32 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 125 PA_enable))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 145 "Net-(Q5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 224.17 127.64)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R33 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 121 "Net-(IC6-Pad6)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 225.49 131.17 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R34 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 121 "Net-(IC6-Pad6)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 144 "Net-(Q5-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 218.69 73.14 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R35 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value xy (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 72 "Net-(C106-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 217.35 69.74)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R36 (at 0 -1.7) (layer F.SilkS))
    (fp_text value xy (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 72 "Net-(C106-Pad1)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 122 "Net-(IC7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 216.01 73.15 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R37 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value xy (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 122 "Net-(IC7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 202.66 73.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R38 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value xy (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 76 "Net-(C116-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 201.32 70.11)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R39 (at 0 -1.7) (layer F.SilkS))
    (fp_text value xy (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 76 "Net-(C116-Pad1)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 79 RX-Frontend-Mischer))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 199.97 73.68 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R40 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value xy (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 79 RX-Frontend-Mischer))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_unten) (tedit 58E0A804)
    (at 157.15 61.45)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R41 (at 0 1.7) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 110 "Net-(D6-Pad1)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 131 RX_LE))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_unten) (tedit 58E0A804)
    (at 158.02 59.15)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R42 (at 0 1.7) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 111 "Net-(D7-Pad1)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 129 RX_DATA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_unten) (tedit 58E0A804)
    (at 161.24 56.89)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R43 (at 0 1.7) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 127 RX_CLK))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 112 "Net-(D8-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_unten) (tedit 58E0A804)
    (at 172.85 64.02 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R44 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 4,7k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 150 "Net-(R44-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Kupfer_unten B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 163.16 67.35 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R45 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 150 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 88 "Net-(C129-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 86 "Net-(C127-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 161.51 62 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R46 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 91 "Net-(C131-Pad2)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 86 "Net-(C127-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 159.86 74.07)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R47 (at 0 -1.7) (layer F.SilkS))
    (fp_text value xy (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 97 "Net-(C135-Pad2)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 163.21 75.53 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R48 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value xy (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 101 "Net-(C145-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 97 "Net-(C135-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 159.85 76.85)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R49 (at 0 -1.7) (layer F.SilkS))
    (fp_text value xy (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 101 "Net-(C145-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 174.34 57.44 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R50 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 151 "Net-(R50-Pad2)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 146 "Net-(Q6-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Kupfer_oben) (tedit 58E0A804)
    (at 187.29 58.43)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R51 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 114 "Net-(D9-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:MABA007748CT1160 (layer Kupfer_oben) (tedit 0)
    (at 151.45 134.48 90)
    (descr MABA-007748-CT1160-1)
    (tags Transformer)
    (attr smd)
    (fp_text reference T1 (at 0 0 90) (layer F.SilkS))
    (fp_text value Maba-010125-TC1113 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.27 -1.715 90) (size 0.76 1.4) (layers Kupfer_oben F.Paste F.Mask)
      (net 33 "Net-(C50-Pad1)"))
    (pad 2 smd rect (at 0 -1.715 90) (size 0.76 1.4) (layers Kupfer_oben F.Paste F.Mask))
    (pad 3 smd rect (at 1.27 -1.715 90) (size 0.76 1.4) (layers Kupfer_oben F.Paste F.Mask)
      (net 138 "Net-(L20-Pad2)"))
    (pad 4 smd rect (at 1.27 1.715 90) (size 0.76 1.4) (layers Kupfer_oben F.Paste F.Mask)
      (net 39 "Net-(C62-Pad1)"))
    (pad 5 smd rect (at -1.27 1.715 90) (size 0.76 1.4) (layers Kupfer_oben F.Paste F.Mask)
      (net 38 "Net-(C62-Pad2)"))
    (model D:\Kicad\lib\SamacSys_Parts.3dshapes\MABAES0060.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:ETC16423TR (layer Kupfer_oben) (tedit 0)
    (at 175.64 134.41 90)
    (descr ETC1.6-4-2-3TR-3)
    (tags Transformer)
    (attr smd)
    (fp_text reference T2 (at 0 -0.343 90) (layer F.SilkS))
    (fp_text value ETC1.6-4-2-3TR (at 0 -0.343 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -0.343 90) (layer F.Fab))
    (pad 1 smd rect (at -1.269 -1.716 90) (size 0.762 1.397) (layers Kupfer_oben F.Paste F.Mask)
      (net 152 "Net-(T2-Pad1)"))
    (pad 2 smd rect (at 0 -1.716 90) (size 0.762 1.397) (layers Kupfer_oben F.Paste F.Mask)
      (net 44 "Net-(C69-Pad1)"))
    (pad 3 smd rect (at 1.269 -1.716 90) (size 0.762 1.397) (layers Kupfer_oben F.Paste F.Mask)
      (net 153 "Net-(T2-Pad3)"))
    (pad 4 smd rect (at 1.269 1.716 90) (size 0.762 1.397) (layers Kupfer_oben F.Paste F.Mask)
      (net 53 "Net-(C79-Pad2)"))
    (pad 5 smd rect (at -1.269 1.716 90) (size 0.762 1.397) (layers Kupfer_oben F.Paste F.Mask)
      (net 55 "Net-(C80-Pad2)"))
    (model D:\Kicad\lib\SamacSys_Parts.3dshapes\ETC1.6-4-2-3TR.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer Kupfer_oben) (tedit 5A0F774F)
    (at 166.93 105.57)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP4 (at 0 -1.448) (layer F.SilkS))
    (fp_text value Test (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 11 3V3_LO_Frontend))
  )
  (module w_conn_rf:sma_straight_32k101-400l5 (layer Kupfer_oben) (tedit 0)
    (at 109.74 61.07 270)
    (descr "SMA straight female connector, Rosenberger 32K101-400L5")
    (fp_text reference TP5 (at 0 4.8 270) (layer F.SilkS))
    (fp_text value HF-Eingang (at 0 -4.8 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.3 2.3) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 133 "Net-(K1-Pad6)"))
    (pad 2 thru_hole circle (at 2.54 -2.54 270) (size 2.5 2.5) (drill 1.45) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 270) (size 2.5 2.5) (drill 1.45) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 270) (size 2.5 2.5) (drill 1.45) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 2.54 270) (size 2.5 2.5) (drill 1.45) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model walter/conn_rf/sma_straight_32k101-400l5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer Kupfer_oben) (tedit 5A0F774F)
    (at 152.21 105.69)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP6 (at 0 -1.448) (layer F.SilkS))
    (fp_text value Test (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 154 TCXO))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer Kupfer_oben) (tedit 5A0F774F)
    (at 168.59 57.5)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP14 (at 0 -1.448) (layer F.SilkS))
    (fp_text value Test (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 11 3V3_LO_Frontend))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer Kupfer_oben) (tedit 5A0F774F)
    (at 155.78 61.54)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP15 (at 0 -1.448) (layer F.SilkS))
    (fp_text value Test (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 91 "Net-(C131-Pad2)"))
  )
  (module SamacSys_Parts:QFN50P500X500X80-33N-D (layer Kupfer_oben) (tedit 0)
    (at 158.57 121.19 90)
    (descr "CP-32-7 (LFCSP)")
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference U2 (at 0 0 90) (layer F.SilkS))
    (fp_text value ADF4351 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 33 smd rect (at 0 0 90) (size 3.25 3.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 32 smd rect (at -1.75 -2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 31 smd rect (at -1.25 -2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 30 smd rect (at -0.75 -2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask))
    (pad 29 smd rect (at -0.25 -2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 154 TCXO))
    (pad 28 smd rect (at 0.25 -2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 27 smd rect (at 0.75 -2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 26 smd rect (at 1.25 -2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask))
    (pad 25 smd rect (at 1.75 -2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 149 "Net-(R22-Pad2)"))
    (pad 24 smd rect (at 2.45 -1.75 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 43 "Net-(C67-Pad1)"))
    (pad 23 smd rect (at 2.45 -1.25 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 40 "Net-(C64-Pad1)"))
    (pad 22 smd rect (at 2.45 -0.75 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 148 "Net-(R21-Pad1)"))
    (pad 21 smd rect (at 2.45 -0.25 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 2.45 0.25 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 48 "Net-(C72-Pad2)"))
    (pad 19 smd rect (at 2.45 0.75 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 36 "Net-(C58-Pad1)"))
    (pad 18 smd rect (at 2.45 1.25 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 2.45 1.75 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 16 smd rect (at 1.75 2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 15 smd rect (at 1.25 2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask))
    (pad 14 smd rect (at 0.75 2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask))
    (pad 13 smd rect (at 0.25 2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 51 "Net-(C74-Pad1)"))
    (pad 12 smd rect (at -0.25 2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 50 "Net-(C73-Pad1)"))
    (pad 11 smd rect (at -0.75 2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at -1.25 2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 9 smd rect (at -1.75 2.45 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -2.45 1.75 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -2.45 1.25 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 46 "Net-(C70-Pad1)"))
    (pad 6 smd rect (at -2.45 0.75 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 5 smd rect (at -2.45 0.25 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask))
    (pad 4 smd rect (at -2.45 -0.25 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 3 smd rect (at -2.45 -0.75 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 105 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -2.45 -1.25 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 106 "Net-(D3-Pad1)"))
    (pad 1 smd rect (at -2.45 -1.75 180) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 107 "Net-(D4-Pad1)"))
    (model D:\Kicad\lib\SamacSys_Parts.3dshapes\ADF4351BCPZ-RL7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:QFN50P500X500X80-33N-D (layer Kupfer_oben) (tedit 0)
    (at 168.32 62.73)
    (descr "CP-32-7 (LFCSP)")
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference U4 (at 0 0) (layer F.SilkS))
    (fp_text value ADF4351 (at 0 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.45 -1.75 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 112 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at -2.45 -1.25 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 111 "Net-(D7-Pad1)"))
    (pad 3 smd rect (at -2.45 -0.75 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 110 "Net-(D6-Pad1)"))
    (pad 4 smd rect (at -2.45 -0.25 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 5 smd rect (at -2.45 0.25 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask))
    (pad 6 smd rect (at -2.45 0.75 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 7 smd rect (at -2.45 1.25 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 86 "Net-(C127-Pad1)"))
    (pad 8 smd rect (at -2.45 1.75 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -1.75 2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at -1.25 2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 11 smd rect (at -0.75 2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at -0.25 2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 95 "Net-(C133-Pad1)"))
    (pad 13 smd rect (at 0.25 2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 96 "Net-(C134-Pad1)"))
    (pad 14 smd rect (at 0.75 2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask))
    (pad 15 smd rect (at 1.25 2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask))
    (pad 16 smd rect (at 1.75 2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 17 smd rect (at 2.45 1.75 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 18 smd rect (at 2.45 1.25 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 2.45 0.75 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 77 "Net-(C117-Pad1)"))
    (pad 20 smd rect (at 2.45 0.25 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 91 "Net-(C131-Pad2)"))
    (pad 21 smd rect (at 2.45 -0.25 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 2.45 -0.75 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 150 "Net-(R44-Pad1)"))
    (pad 23 smd rect (at 2.45 -1.25 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 78 "Net-(C119-Pad1)"))
    (pad 24 smd rect (at 2.45 -1.75 90) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 83 "Net-(C124-Pad1)"))
    (pad 25 smd rect (at 1.75 -2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 151 "Net-(R50-Pad2)"))
    (pad 26 smd rect (at 1.25 -2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask))
    (pad 27 smd rect (at 0.75 -2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 28 smd rect (at 0.25 -2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 29 smd rect (at -0.25 -2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 154 TCXO))
    (pad 30 smd rect (at -0.75 -2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask))
    (pad 31 smd rect (at -1.25 -2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 32 smd rect (at -1.75 -2.45) (size 0.3 0.85) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (pad 33 smd rect (at 0 0) (size 3.25 3.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model D:\Kicad\lib\SamacSys_Parts.3dshapes\ADF4351BCPZ-RL7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:XTCLH50M000CHJA3P0 (layer Kupfer_oben) (tedit 0)
    (at 148.25 100.27)
    (descr XTCLH50M000CHJA3P0)
    (tags "Crystal or Oscillator")
    (attr smd)
    (fp_text reference Y1 (at 0 0) (layer F.SilkS))
    (fp_text value XTCLH10M000THJA0P0 (at 0 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 1.25 90) (size 1.3 1.6) (layers Kupfer_oben F.Paste F.Mask))
    (pad 4 smd rect (at 2 1.25 90) (size 1.3 1.6) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2 -1.25 90) (size 1.3 1.6) (layers Kupfer_oben F.Paste F.Mask)
      (net 154 TCXO))
    (pad 8 smd rect (at -2 -1.25 90) (size 1.3 1.6) (layers Kupfer_oben F.Paste F.Mask)
      (net 11 3V3_LO_Frontend))
    (model D:\Kicad\lib\SamacSys_Parts.3dshapes\XTCLH50M000CHJA3P0.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Shielding_Cabinets:Laird_Technologies_BMI-S-210-F_44.00x30.50mm locked (layer Kupfer_oben) (tedit 57501709)
    (at 163.85 127.34 180)
    (descr "Laird Technologies BMI-S-210-F Shielding Cabinet Two Piece SMD 44.00x30.50mm")
    (tags "Shielding Cabinet")
    (attr smd)
    (fp_text reference J4 (at 0 -16.65 180) (layer F.SilkS))
    (fp_text value SchirmhausRx-Teil (at 0 16.65 180) (layer F.Fab))
    (pad 1 smd rect (at 21.9 13.875 180) (size 1 1.55) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 13.875 180) (size 1 1.55) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 9 180) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 9 180) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 3 180) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 3 180) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 -3 180) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 -3 180) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 -9 180) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 -9 180) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 -13.875 180) (size 1 1.55) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 -13.875 180) (size 1 1.55) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 20.25 15.15 180) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 20.25 -15.15 180) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 15 15.15 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 15 -15.15 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 9 15.15 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 9 -15.15 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3 15.15 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3 -15.15 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3 15.15 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3 -15.15 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -9 15.15 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -9 -15.15 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -15 15.15 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -15 -15.15 180) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -20.25 15.15 180) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -20.25 -15.15 180) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 15.15 180) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 15.15 180) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 -15.15 180) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 -15.15 180) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
  )
  (module Housings_DFN_QFN:QFN-16-1EP_4x4mm_Pitch0.65mm (layer Kupfer_oben) (tedit 54130A77)
    (at 163.68 134.39)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -3.4) (layer F.SilkS))
    (fp_text value LT5521EUF-PBF (at 0 3.4) (layer F.Fab))
    (pad 17 smd rect (at -0.625 -0.625) (size 1.25 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.625 0.625) (size 1.25 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.625 -0.625) (size 1.25 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.625 0.625) (size 1.25 1.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 16 smd rect (at -0.975 -2 90) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at -0.325 -2 90) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 41 "Net-(C66-Pad1)"))
    (pad 14 smd rect (at 0.325 -2 90) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 0.975 -2 90) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 2 -0.975) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 153 "Net-(T2-Pad3)"))
    (pad 11 smd rect (at 2 -0.325) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 2 0.325) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2 0.975) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 152 "Net-(T2-Pad1)"))
    (pad 8 smd rect (at 0.975 2 90) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 37 "Net-(C59-Pad1)"))
    (pad 7 smd rect (at 0.325 2 90) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 37 "Net-(C59-Pad1)"))
    (pad 6 smd rect (at -0.325 2 90) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 37 "Net-(C59-Pad1)"))
    (pad 5 smd rect (at -0.975 2 90) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 37 "Net-(C59-Pad1)"))
    (pad 4 smd rect (at -2 0.975) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2 0.325) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 38 "Net-(C62-Pad2)"))
    (pad 2 smd rect (at -2 -0.325) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 39 "Net-(C62-Pad1)"))
    (pad 1 smd rect (at -2 -0.975) (size 0.8 0.35) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-16-1EP_4x4mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:DFN-8-1EP_3x3mm_Pitch0.5mm (layer Kupfer_oben) (tedit 54130A77)
    (at 180.065 75.625 180)
    (descr "DD Package; 8-Lead Plastic DFN (3mm x 3mm) (see Linear Technology DFN_8_05-08-1698.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U3 (at 0 -2.55 180) (layer F.SilkS))
    (fp_text value LT5560EDD-PBF (at 0 2.55 180) (layer F.Fab))
    (pad 9 smd rect (at -0.415 -0.595 180) (size 0.83 1.19) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.415 0.595 180) (size 0.83 1.19) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.415 -0.595 180) (size 0.83 1.19) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.415 0.595 180) (size 0.83 1.19) (layers Kupfer_oben F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 8 smd rect (at 1.4 -0.75 180) (size 0.7 0.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 139 "Net-(L44-Pad1)"))
    (pad 7 smd rect (at 1.4 -0.25 180) (size 0.7 0.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 99 "Net-(C140-Pad1)"))
    (pad 6 smd rect (at 1.4 0.25 180) (size 0.7 0.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 93 "Net-(C132-Pad1)"))
    (pad 5 smd rect (at 1.4 0.75 180) (size 0.7 0.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 87 "Net-(C128-Pad1)"))
    (pad 4 smd rect (at -1.4 0.75 180) (size 0.7 0.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 82 "Net-(C123-Pad1)"))
    (pad 3 smd rect (at -1.4 0.25 180) (size 0.7 0.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 81 "Net-(C122-Pad2)"))
    (pad 2 smd rect (at -1.4 -0.25 180) (size 0.7 0.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 1 +5VA))
    (pad 1 smd rect (at -1.4 -0.75 180) (size 0.7 0.25) (layers Kupfer_oben F.Paste F.Mask)
      (net 84 "Net-(C126-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer Kupfer_oben) (tedit 5A0F774F)
    (at 148.79 120.59)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP11 (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 48 "Net-(C72-Pad2)"))
  )
  (module Shielding_Cabinets:Laird_Technologies_BMI-S-210-F_44.00x30.50mm (layer Kupfer_oben) (tedit 57501709)
    (at 213.05 127.35)
    (descr "Laird Technologies BMI-S-210-F Shielding Cabinet Two Piece SMD 44.00x30.50mm")
    (tags "Shielding Cabinet")
    (attr smd)
    (fp_text reference J14 (at 0 -16.65) (layer F.SilkS))
    (fp_text value SchirmhausRx-Mischer (at 0 16.65) (layer F.Fab))
    (pad 1 smd rect (at 21.9 13.875) (size 1 1.55) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 13.875) (size 1 1.55) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 9) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 9) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 3) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 3) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 -3) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 -3) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 -9) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 -9) (size 1 3.8) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 -13.875) (size 1 1.55) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 -13.875) (size 1 1.55) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 20.25 15.15) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 20.25 -15.15) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 15 15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 15 -15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 9 15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 9 -15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3 15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3 -15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3 15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3 -15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -9 15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -9 -15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -15 15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -15 -15.15) (size 3.8 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -20.25 15.15) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -20.25 -15.15) (size 2.3 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 15.15) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 15.15) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 21.9 -15.15) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -21.9 -15.15) (size 1 1) (layers Kupfer_oben F.Mask)
      (net 2 GND))
  )
  (gr_line (start 79.38 48.42) (end 247.38 48.42) (layer Edge.Cuts) (width 1))
  (gr_line (start 79.38 146.42) (end 79.38 48.42) (layer Edge.Cuts) (width 1))
  (gr_line (start 247.38 48.42) (end 247.38 146.42) (layer Edge.Cuts) (width 1))
  (gr_line (start 247.38 146.42) (end 79.38 146.42) (layer Edge.Cuts) (width 1))
  (gr_text "EsHail-Transverter v.2.0\nDatenschutz alias OExyz\nOrt, Aug. 2019" (at 94.54 65.52 270) (layer Kupfer_oben))
  (gr_text 10Mhz (at 168.14 106.82) (layer F.SilkS))
  (zone (net 0) (net_name "") (layer Kupfer_oben) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.2 52.05) (xy 102.07 51.95) (xy 102.01 78.97) (xy 88.26 79.03)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer Kupfer_unten) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.883 48.9204) (xy 79.883 145.923) (xy 246.888 145.923) (xy 246.888 48.9204)
      )
    )
  )
  (zone (net 1) (net_name +5VA) (layer +5VA) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.8576 48.9204) (xy 79.883 145.923) (xy 246.8626 145.9484) (xy 246.888 48.9204)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer GND) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.883 48.9204) (xy 79.883 145.923) (xy 246.888 145.923) (xy 246.888 48.9204)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer Kupfer_oben) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.8576 48.9204) (xy 79.883 145.923) (xy 246.888 145.923) (xy 246.9134 48.9204)
      )
    )
  )
)
