<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>ESP8266 MCU Modules
&lt;br&gt;&lt;br&gt;
&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
<packages>
<package name="SMT_ESP09">
<description>ESP8266 Module, ESP-09&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="1X05_THT_ESP10">
<description>ESP8266 Module, ESP-10&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X07W_SMT_ESP04">
<description>ESP8266 Module, ESP-04&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X08W_SMT_ESP12">
<description>ESP8266 Module, ESP-12E&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X08W_SMT_ESP07">
</package>
<package name="2X04_THT">
<description>ESP8266 Module, ESP-01&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X08W_THT_ESP12">
<description>ESP8266 Module, ESP-12E, THT version&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="1X08_SMT_ESP11">
<description>ESP8266 Module, ESP-11&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X08W_SMT_ESP12_LONG">
<description>ESP8266 Module, ESP-12E&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X07W_SMT_ESP08">
<description>ESP8266 Module, ESP-08, 14 pin version&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X08W_THT_ESP-SHD">
<description>ESP8266 Adapter, SIP header 0.1", 32mil drill&lt;p&gt;
for ESP-07, ESP-12 and similar.&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X08W_SMT_ESP12Q_LONG">
<description>ESP8266 Module, ESP-12EQ&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X08W_SMT_ESP12Q">
<description>ESP8266 Module, ESP-12EQ&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X06_THT">
<description>ESP8266 Module, ESP-01S with I2C&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X04W_THT">
<description>ESP8266 Module, ESP-02&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X08W_THT_D1-MINI">
<description>Wemos D1 mini, ESP8266 Module, ESP-12&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X07W_SMT_ESP03">
<description>ESP8266 Module, ESP-03&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="SMT_ESP06">
<description>ESP8266 Module, ESP-06&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="1X05_THT_ESP05">
<description>ESP8266 Module, ESP-05, 5 pin version&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X07_THT_ESP-GOOFY">
<description>ESP8266 Module, ESP-01/S, ESP-07, ESP-12&lt;p&gt;
double Breakout aka Goofy Adapter&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X15W_THT_ESP12-DEVKIT">
<description>ESP12E_DEVKIT</description>
</package>
<package name="WEMOS_D1-PACK">
<description>Wemos D1 mini, ESP8266 Module, ESP-12&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X15W_THT_NODEMCU">
</package>
<package name="2X08W_THT_ESP07">
</package>
<package name="2X08W_SMT_ESP07S_ISOLATE">
<description>ESP8266 Module, ESP-07S&lt;br&gt;
with Thermalpad&lt;br&gt;&lt;br&gt;


&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
<package name="2X08W_SMT_ESP07S_GNDPAD">
<description>ESP8266 Module, ESP-07S&lt;br&gt;
with Groundpad&lt;br&gt;&lt;br&gt;


&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
</package>
</packages>
<symbols>
<symbol name="ESP10">
<pin name="TX" direction="out"/>
<pin name="RX" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="ESP09">
<pin name="GND7"/>
<pin name="GND6"/>
<pin name="GND5"/>
<pin name="GND4"/>
<pin name="GND3"/>
<pin name="GND2"/>
<pin name="GND1"/>
<pin name="GND" direction="pwr"/>
<pin name="ANT" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="RST" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="RX" direction="in"/>
<pin name="GPIO0"/>
<pin name="GPIO2"/>
<pin name="GPIO15"/>
<pin name="GPIO13"/>
<pin name="GPIO12"/>
<pin name="GPIO14"/>
<pin name="CH_PD"/>
</symbol>
<symbol name="ESP03/04">
<description>ESP8266 Module ESP-03 / ESP-04</description>
<pin name="GPIO0"/>
<pin name="GPIO2"/>
<pin name="GPIO15"/>
<pin name="GPIO13"/>
<pin name="GPIO12"/>
<pin name="GPIO14"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="UTXD" direction="out"/>
<pin name="URXD" direction="in"/>
<pin name="GPIO18"/>
<pin name="CH_PD"/>
<pin name="ANT" direction="pas"/>
</symbol>
<symbol name="ESP12">
<description>ESP8266-12</description>
<pin name="ADC" direction="in"/>
<pin name="CH_PD"/>
<pin name="GND" direction="pwr"/>
<pin name="GPIO0"/>
<pin name="GPIO2"/>
<pin name="GPIO5"/>
<pin name="GPIO4"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="GPIO14"/>
<pin name="GPIO15"/>
<pin name="GPIO16"/>
<pin name="RST" direction="in"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="ESP01/01S">
<description>ESP8266, ESP-01/S&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
<pin name="GND" direction="pwr"/>
<pin name="GPIO2"/>
<pin name="GPIO0"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="CH_PD"/>
<pin name="RST" direction="in"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="ESP11">
<pin name="GND" direction="pwr"/>
<pin name="ENABLE"/>
<pin name="RST" direction="in"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="GPIO0"/>
<pin name="GPIO2"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="ESP12Q">
<description>ESP8266-12E Module</description>
<pin name="RST" direction="in"/>
<pin name="ADC" direction="in"/>
<pin name="CH_PD"/>
<pin name="GPIO16"/>
<pin name="GPIO14"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GPIO15"/>
<pin name="GPIO2"/>
<pin name="GPIO0"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="CS0"/>
<pin name="MISO"/>
<pin name="*GPIO9"/>
<pin name="*GPIO10"/>
<pin name="MOSI"/>
<pin name="SCLK"/>
</symbol>
<symbol name="ESP08">
<description>ESP8266 Module ESP-07/08 - 14 pins</description>
<pin name="VCC" direction="pwr"/>
<pin name="GPIO14"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="GPIO15"/>
<pin name="GPIO2"/>
<pin name="GPIO0"/>
<pin name="ANT" direction="pas"/>
<pin name="CH_PD"/>
<pin name="GPIO16"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="ESP02">
<pin name="GND" direction="pwr"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GPIO15"/>
<pin name="GPIO0"/>
<pin name="GPIO2"/>
<pin name="RST" direction="in"/>
</symbol>
<symbol name="ESP12-SHIELD">
<description>&lt;b&gt;ESP8266 Adapterboard&lt;/b&gt;&lt;p&gt;
for ESP8266-07, ESP8266-12 and other 8+8 pins.&lt;p&gt;
The adapter has ingegrated 10k pullup on CH_PD/EN and 10k pulldown on GPIO15. Both can be leave unconnected.&lt;p&gt;
On the bottom side is place for a SOT-89 voltage regulator. Default is disabled, bridged with 0R resistor (remove it).&lt;p&gt;&lt;br&gt;
The author cannot warrant that this library is free from error or will meet your specific requirements.&lt;p&gt;
&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;.</description>
<pin name="RST" direction="in"/>
<pin name="ADC" direction="in"/>
<pin name="CH_PD" direction="nc"/>
<pin name="GPIO16"/>
<pin name="GPIO14"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GPIO15" direction="nc"/>
<pin name="GPIO2"/>
<pin name="GPIO0"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
</symbol>
<symbol name="ESP01S-MOD">
<description>ESP8266, ESP-01S_MOD, with GPIO4+5&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
<pin name="GND" direction="pwr"/>
<pin name="GPIO2"/>
<pin name="GPIO0"/>
<pin name="RX" direction="in"/>
<pin name="GPIO4"/>
<pin name="TX" direction="out"/>
<pin name="CH_PD"/>
<pin name="RST" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GPIO5"/>
</symbol>
<symbol name="ESP05">
<pin name="RST" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="ESP06">
<pin name="GND7"/>
<pin name="GND8"/>
<pin name="GND6"/>
<pin name="GND5"/>
<pin name="GND4"/>
<pin name="GND3"/>
<pin name="GND2"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="ANT" direction="pas"/>
<pin name="CH_PD"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="GPIO0"/>
<pin name="GPIO2"/>
<pin name="GPIO15"/>
<pin name="GPIO13"/>
<pin name="GPIO14"/>
<pin name="GPIO12"/>
<pin name="GPIO16"/>
</symbol>
<symbol name="ESP12-GOOFY">
<description>ESP8266 Module, ESP-01/S, ESP-07, ESP-12&lt;p&gt;
on double breakout aka Goofy Adapter&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
<pin name="ADC" direction="in"/>
<pin name="CH_PD"/>
<pin name="GND" direction="pwr"/>
<pin name="GPIO0"/>
<pin name="GPIO2"/>
<pin name="GPIO5"/>
<pin name="GPIO4"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="GPIO14"/>
<pin name="RST" direction="in"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="ESP12-DEVKIT">
<description>ESP12E_DEVKIT</description>
<pin name="AD0"/>
<pin name="RSV@0"/>
<pin name="RSV@1"/>
<pin name="SD3"/>
<pin name="SD2"/>
<pin name="SD1"/>
<pin name="CMD"/>
<pin name="SD0"/>
<pin name="CLK"/>
<pin name="GND@0"/>
<pin name="3V3@0"/>
<pin name="EN"/>
<pin name="RST"/>
<pin name="GND@1"/>
<pin name="VIN"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="3V3@1"/>
<pin name="GND@2"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="GND@3"/>
<pin name="3V3@2"/>
</symbol>
<symbol name="WEMOS_D1-MINI">
<pin name="3V3" direction="pwr"/>
<pin name="D8"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D0"/>
<pin name="A0"/>
<pin name="RST" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="RX" direction="in"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="GND" direction="pwr"/>
<pin name="5V" direction="pwr"/>
</symbol>
<symbol name="NODEMCU">
<pin name="A0"/>
<pin name="GND" direction="pwr"/>
<pin name="VV"/>
<pin name="S3"/>
<pin name="S2"/>
<pin name="S1"/>
<pin name="SC"/>
<pin name="S0"/>
<pin name="SK"/>
<pin name="GND@1" direction="pwr"/>
<pin name="3V" direction="pwr"/>
<pin name="EN"/>
<pin name="RST"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="3V@1" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="TX" direction="out"/>
<pin name="RX" direction="in"/>
<pin name="D8"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="GND@4" direction="pwr"/>
<pin name="3V@2" direction="pwr"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="D0"/>
</symbol>
<symbol name="ESP07">
<description>ESP8266 Module ESP-07 - 16 pins</description>
<pin name="VCC" direction="pwr"/>
<pin name="CH_PD"/>
<pin name="RST" direction="in"/>
<pin name="GPIO0"/>
<pin name="GPIO2"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="GPIO14"/>
<pin name="GPIO15"/>
<pin name="GPIO16"/>
<pin name="TX" direction="out"/>
<pin name="RX" direction="in"/>
<pin name="ADC" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ESP09">
<description>ESP8266 Wifi module ESP-09</description>
<gates>
<gate name="G$1" symbol="ESP09"/>
</gates>
<devices>
<device name="" package="SMT_ESP09">
<connects>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="CH_PD" pad="CH_PD"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4" pad="GND4"/>
<connect gate="G$1" pin="GND5" pad="GND5"/>
<connect gate="G$1" pin="GND6" pad="GND6"/>
<connect gate="G$1" pin="GND7" pad="GND7"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO12" pad="GPIO12"/>
<connect gate="G$1" pin="GPIO13" pad="GPIO13"/>
<connect gate="G$1" pin="GPIO14" pad="GPIO14"/>
<connect gate="G$1" pin="GPIO15" pad="GPIO15"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO02"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP10">
<description>ESP8266 Wifi module ESP-10</description>
<gates>
<gate name="G$1" symbol="ESP10"/>
</gates>
<devices>
<device name="" package="1X05_THT_ESP10">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP04">
<description>ESP8266 Wifi module ESP-04</description>
<gates>
<gate name="G$1" symbol="ESP03/04"/>
</gates>
<devices>
<device name="" package="2X07W_SMT_ESP04">
<connects>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="CH_PD" pad="CH_PD"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO12" pad="GPIO12"/>
<connect gate="G$1" pin="GPIO13" pad="GPIO13"/>
<connect gate="G$1" pin="GPIO14" pad="GPIO14"/>
<connect gate="G$1" pin="GPIO15" pad="GPIO15"/>
<connect gate="G$1" pin="GPIO18" pad="GPIO18"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="URXD" pad="URXD"/>
<connect gate="G$1" pin="UTXD" pad="UTXD"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIMENSIONS" value="14.7 x 12.1 mm"/>
<attribute name="PINS" value="14"/>
<attribute name="PITCH" value="0.078&quot; / 2 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP01" prefix="U" uservalue="yes">
<description>ESP8266 Wifi module ESP-01 512kB/1M&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
<gates>
<gate name="G$1" symbol="ESP01/01S"/>
</gates>
<devices>
<device name="" package="2X04_THT">
<connects>
<connect gate="G$1" pin="CH_PD" pad="CH_PD"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="2X04_THT">
<connects>
<connect gate="G$1" pin="CH_PD" pad="CH_PD"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GOOFY" package="2X07_THT_ESP-GOOFY">
<connects>
<connect gate="G$1" pin="CH_PD" pad="CH_PD"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP11" uservalue="yes">
<description>ESP8266 Wifi module ESP-11</description>
<gates>
<gate name="G$1" symbol="ESP11"/>
</gates>
<devices>
<device name="" package="1X08_SMT_ESP11">
<connects>
<connect gate="G$1" pin="ENABLE" pad="P$2"/>
<connect gate="G$1" pin="GND" pad="P$1"/>
<connect gate="G$1" pin="GPIO0" pad="P$6"/>
<connect gate="G$1" pin="GPIO2" pad="P$7"/>
<connect gate="G$1" pin="RST" pad="P$3"/>
<connect gate="G$1" pin="RX" pad="P$4"/>
<connect gate="G$1" pin="TX" pad="P$5"/>
<connect gate="G$1" pin="VCC" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP12" prefix="U" uservalue="yes">
<description>ESP8266 Wifi module ESP-12 4MB (32Mb)</description>
<gates>
<gate name="G$1" symbol="ESP12"/>
</gates>
<devices>
<device name="THT" package="2X08W_THT_ESP12">
<connects>
<connect gate="G$1" pin="ADC" pad="ADC"/>
<connect gate="G$1" pin="CH_PD" pad="CH_PD"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO12" pad="GPIO12"/>
<connect gate="G$1" pin="GPIO13" pad="GPIO13"/>
<connect gate="G$1" pin="GPIO14" pad="GPIO14"/>
<connect gate="G$1" pin="GPIO15" pad="GPIO15"/>
<connect gate="G$1" pin="GPIO16" pad="GPIO16"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="GPIO4" pad="GPIO5"/>
<connect gate="G$1" pin="GPIO5" pad="GPIO4"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="2X08W_SMT_ESP12_LONG">
<connects>
<connect gate="G$1" pin="ADC" pad="ADC"/>
<connect gate="G$1" pin="CH_PD" pad="CH_PD"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO12" pad="GPIO12"/>
<connect gate="G$1" pin="GPIO13" pad="GPIO13"/>
<connect gate="G$1" pin="GPIO14" pad="GPIO14"/>
<connect gate="G$1" pin="GPIO15" pad="GPIO15"/>
<connect gate="G$1" pin="GPIO16" pad="GPIO16"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="GPIO4" pad="GPIO4"/>
<connect gate="G$1" pin="GPIO5" pad="GPIO5"/>
<connect gate="G$1" pin="RST" pad="RESET"/>
<connect gate="G$1" pin="RX" pad="RXD0"/>
<connect gate="G$1" pin="TX" pad="TXD0"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHORTPADS" package="2X08W_SMT_ESP12">
<connects>
<connect gate="G$1" pin="ADC" pad="2"/>
<connect gate="G$1" pin="CH_PD" pad="3"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GPIO0" pad="12"/>
<connect gate="G$1" pin="GPIO12" pad="6"/>
<connect gate="G$1" pin="GPIO13" pad="7"/>
<connect gate="G$1" pin="GPIO14" pad="5"/>
<connect gate="G$1" pin="GPIO15" pad="10"/>
<connect gate="G$1" pin="GPIO16" pad="4"/>
<connect gate="G$1" pin="GPIO2" pad="11"/>
<connect gate="G$1" pin="GPIO4" pad="13"/>
<connect gate="G$1" pin="GPIO5" pad="14"/>
<connect gate="G$1" pin="RST" pad="1"/>
<connect gate="G$1" pin="RX" pad="15"/>
<connect gate="G$1" pin="TX" pad="16"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ADAPTER" package="2X08W_THT_ESP-SHD">
<connects>
<connect gate="G$1" pin="ADC" pad="2"/>
<connect gate="G$1" pin="CH_PD" pad="3"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GPIO0" pad="12"/>
<connect gate="G$1" pin="GPIO12" pad="6"/>
<connect gate="G$1" pin="GPIO13" pad="7"/>
<connect gate="G$1" pin="GPIO14" pad="5"/>
<connect gate="G$1" pin="GPIO15" pad="10"/>
<connect gate="G$1" pin="GPIO16" pad="4"/>
<connect gate="G$1" pin="GPIO2" pad="11"/>
<connect gate="G$1" pin="GPIO4" pad="13"/>
<connect gate="G$1" pin="GPIO5" pad="14"/>
<connect gate="G$1" pin="RST" pad="1"/>
<connect gate="G$1" pin="RX" pad="15"/>
<connect gate="G$1" pin="TX" pad="16"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP08">
<description>ESP8266 Wifi module ESP-08</description>
<gates>
<gate name="G$1" symbol="ESP08"/>
</gates>
<devices>
<device name="" package="2X07W_SMT_ESP08">
<connects>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="CH_PD" pad="CH_PD"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO12" pad="GPIO12"/>
<connect gate="G$1" pin="GPIO13" pad="GPIO13"/>
<connect gate="G$1" pin="GPIO14" pad="GPIO14"/>
<connect gate="G$1" pin="GPIO15" pad="GPIO15"/>
<connect gate="G$1" pin="GPIO16" pad="GPIO16"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIMENSIONS" value="17.0 x 16.0 mm"/>
<attribute name="PINS" value="14"/>
<attribute name="PITCH" value="0.078&quot; / 2 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP12-SHIELD" prefix="U" uservalue="yes">
<description>&lt;b&gt;ESP8266 Adapterplate&lt;/b&gt;&lt;p&gt;
for ESP-07, ESP-12 and other 2x8 pins.&lt;p&gt;&lt;br&gt;
The adapter have ingegrated 10k pullup on CH_PD/EN and 10k pulldown on GPIO15. Leave both pins non-connected on the pcb.&lt;br&gt;
On the bottom side is place for a SOT-89 voltage regulator. Default is disabled, while bridged with the 0R resistor (remove it!).&lt;br&gt;
&lt;br&gt;&lt;br&gt;
&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
<gates>
<gate name="G$1" symbol="ESP12-SHIELD"/>
</gates>
<devices>
<device name="" package="2X08W_THT_ESP-SHD">
<connects>
<connect gate="G$1" pin="ADC" pad="2"/>
<connect gate="G$1" pin="CH_PD" pad="3"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="GPIO0" pad="13"/>
<connect gate="G$1" pin="GPIO12" pad="6"/>
<connect gate="G$1" pin="GPIO13" pad="7"/>
<connect gate="G$1" pin="GPIO14" pad="5"/>
<connect gate="G$1" pin="GPIO15" pad="15"/>
<connect gate="G$1" pin="GPIO16" pad="4"/>
<connect gate="G$1" pin="GPIO2" pad="14"/>
<connect gate="G$1" pin="GPIO4" pad="12"/>
<connect gate="G$1" pin="GPIO5" pad="11"/>
<connect gate="G$1" pin="RST" pad="1"/>
<connect gate="G$1" pin="RX" pad="10"/>
<connect gate="G$1" pin="TX" pad="9"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP12Q" prefix="U" uservalue="yes">
<description>ESP-12E Module 4MB (32Mb), with long SPI Pads, fixed GPIO4/5&lt;p&gt;

&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
<gates>
<gate name="G$1" symbol="ESP12Q"/>
</gates>
<devices>
<device name="" package="2X08W_SMT_ESP12Q_LONG">
<connects>
<connect gate="G$1" pin="*GPIO10" pad="GPIO10"/>
<connect gate="G$1" pin="*GPIO9" pad="GPIO9"/>
<connect gate="G$1" pin="ADC" pad="ADC"/>
<connect gate="G$1" pin="CH_PD" pad="CH_PD"/>
<connect gate="G$1" pin="CS0" pad="CS0"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO12" pad="GPIO12"/>
<connect gate="G$1" pin="GPIO13" pad="GPIO13"/>
<connect gate="G$1" pin="GPIO14" pad="GPIO14"/>
<connect gate="G$1" pin="GPIO15" pad="GPIO15"/>
<connect gate="G$1" pin="GPIO16" pad="GPIO16"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="GPIO4" pad="GPIO4"/>
<connect gate="G$1" pin="GPIO5" pad="GPIO5"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="SCLK" pad="SCLK"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHORTPADS" package="2X08W_SMT_ESP12Q">
<connects>
<connect gate="G$1" pin="*GPIO10" pad="GPIO10"/>
<connect gate="G$1" pin="*GPIO9" pad="GPIO9"/>
<connect gate="G$1" pin="ADC" pad="ADC"/>
<connect gate="G$1" pin="CH_PD" pad="CH_PD"/>
<connect gate="G$1" pin="CS0" pad="CS0"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO12" pad="GPIO12"/>
<connect gate="G$1" pin="GPIO13" pad="GPIO13"/>
<connect gate="G$1" pin="GPIO14" pad="GPIO14"/>
<connect gate="G$1" pin="GPIO15" pad="GPIO15"/>
<connect gate="G$1" pin="GPIO16" pad="GPIO16"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="GPIO4" pad="GPIO4"/>
<connect gate="G$1" pin="GPIO5" pad="GPIO5"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="SCLK" pad="SCLK"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP01S-MOD" prefix="U" uservalue="yes">
<description>&lt;b&gt;ESP8266-01S *MOD*, with additional I/O&lt;/b&gt;&lt;p&gt;
with deepsleep (RST-GPIO16 connect)&lt;p&gt;
additional I2C pins (GPIO4+GPIO5)&lt;br&gt;&lt;p&gt;
The author cannot warrant that this library is free from error or will meet your specific requirements.&lt;p&gt;
&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
<gates>
<gate name="G$1" symbol="ESP01S-MOD"/>
</gates>
<devices>
<device name="" package="2X06_THT">
<connects>
<connect gate="G$1" pin="CH_PD" pad="CH_PD"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="GPIO4" pad="GPIO4"/>
<connect gate="G$1" pin="GPIO5" pad="GPIO5"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="3V3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GOOFY" package="2X07_THT_ESP-GOOFY">
<connects>
<connect gate="G$1" pin="CH_PD" pad="CH_PD"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="GPIO4" pad="GPIO4"/>
<connect gate="G$1" pin="GPIO5" pad="GPIO5"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP02">
<description>ESP8266 Wifi module ESP-02</description>
<gates>
<gate name="G$1" symbol="ESP02"/>
</gates>
<devices>
<device name="" package="2X04W_THT">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO15" pad="GPIO15/POWERDOWN"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP03">
<description>ESP8266 Wifi module ESP-03</description>
<gates>
<gate name="G$1" symbol="ESP03/04"/>
</gates>
<devices>
<device name="" package="2X07W_SMT_ESP03">
<connects>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="CH_PD" pad="CH_PD"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO12" pad="GPIO12"/>
<connect gate="G$1" pin="GPIO13" pad="GPIO13"/>
<connect gate="G$1" pin="GPIO14" pad="GPIO14"/>
<connect gate="G$1" pin="GPIO15" pad="GPIO15"/>
<connect gate="G$1" pin="GPIO18" pad="GPIO18"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="URXD" pad="URXD"/>
<connect gate="G$1" pin="UTXD" pad="UTXD"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIMENSIONS" value="17.3 x 12.1 mm"/>
<attribute name="PINS" value="14"/>
<attribute name="PITCH" value="0.078&quot; / 2 mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP06">
<description>ESP8266 Wifi module ESP-06</description>
<gates>
<gate name="G$1" symbol="ESP06"/>
</gates>
<devices>
<device name="" package="SMT_ESP06">
<connects>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="CH_PD" pad="CH_PD"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND2" pad="GND1"/>
<connect gate="G$1" pin="GND3" pad="GND2"/>
<connect gate="G$1" pin="GND4" pad="GND3"/>
<connect gate="G$1" pin="GND5" pad="GND4"/>
<connect gate="G$1" pin="GND6" pad="GND5"/>
<connect gate="G$1" pin="GND7" pad="GND6"/>
<connect gate="G$1" pin="GND8" pad="GND7"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO12" pad="GPIO12"/>
<connect gate="G$1" pin="GPIO13" pad="GPIO13"/>
<connect gate="G$1" pin="GPIO14" pad="GPIO14"/>
<connect gate="G$1" pin="GPIO15" pad="GPIO15"/>
<connect gate="G$1" pin="GPIO16" pad="GPIO16"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP05">
<description>ESP8266 Wifi module ESP-05 - 5pin</description>
<gates>
<gate name="G$1" symbol="ESP05"/>
</gates>
<devices>
<device name="" package="1X05_THT_ESP05">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP12-GOOFY" prefix="U" uservalue="yes">
<description>&lt;b&gt;ESP8266 Module&lt;/b&gt;, ESP-01, ESP-07, ESP-12&lt;p&gt;
double breakout aka Goofy Adapter.&lt;br&gt;
Integrated is a pulldown on IO15.&lt;br&gt;
Optional a red SMD LED (on TX/IO1 line) and a blue (on IO2) can be soldered.&lt;br&gt;
IO16 for deep sleep is not out, but can simply direct on the module soldered.&lt;br&gt;
The external connector for the breakout is a HDR-2x07 2.54mm.
&lt;br&gt;&lt;br&gt;
&lt;author&gt;Mr.AtiX, CroNet&lt;/author&gt;</description>
<gates>
<gate name="G$1" symbol="ESP12-GOOFY"/>
</gates>
<devices>
<device name="" package="2X07_THT_ESP-GOOFY">
<connects>
<connect gate="G$1" pin="ADC" pad="ADC"/>
<connect gate="G$1" pin="CH_PD" pad="CH_PD"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO12" pad="GPIO12"/>
<connect gate="G$1" pin="GPIO13" pad="GPIO13"/>
<connect gate="G$1" pin="GPIO14" pad="GPIO14"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="GPIO4" pad="GPIO4"/>
<connect gate="G$1" pin="GPIO5" pad="GPIO5"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP12-DEVKIT">
<description>ESP12E DEVKIT BOARD/ Module</description>
<gates>
<gate name="G$1" symbol="ESP12-DEVKIT"/>
</gates>
<devices>
<device name="" package="2X15W_THT_ESP12-DEVKIT">
<connects>
<connect gate="G$1" pin="3V3@0" pad="3V3@0"/>
<connect gate="G$1" pin="3V3@1" pad="3V3@1"/>
<connect gate="G$1" pin="3V3@2" pad="3V3@2"/>
<connect gate="G$1" pin="AD0" pad="AD0"/>
<connect gate="G$1" pin="CLK" pad="CLK"/>
<connect gate="G$1" pin="CMD" pad="CMD"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="EN" pad="EN"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="GND@3" pad="GND@3"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RSV@0" pad="RSV@0"/>
<connect gate="G$1" pin="RSV@1" pad="RSV@1"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="SD0" pad="SD0"/>
<connect gate="G$1" pin="SD1" pad="SD1"/>
<connect gate="G$1" pin="SD2" pad="SD2"/>
<connect gate="G$1" pin="SD3" pad="SD3"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WEMOS_D1-MINI" prefix="UC">
<description>Wemos D1 mini, ESP8266 Module, ESP-12&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="WEMOS_D1-MINI"/>
</gates>
<devices>
<device name="" package="WEMOS_D1-PACK">
<connects>
<connect gate="G$1" pin="3V3" pad="3V3"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NODEMCU">
<gates>
<gate name="G$1" symbol="NODEMCU"/>
</gates>
<devices>
<device name="" package="2X15W_THT_NODEMCU">
<connects>
<connect gate="G$1" pin="3V" pad="11"/>
<connect gate="G$1" pin="3V@1" pad="16"/>
<connect gate="G$1" pin="3V@2" pad="25"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="D0" pad="30"/>
<connect gate="G$1" pin="D1" pad="29"/>
<connect gate="G$1" pin="D2" pad="28"/>
<connect gate="G$1" pin="D3" pad="27"/>
<connect gate="G$1" pin="D4" pad="26"/>
<connect gate="G$1" pin="D5" pad="23"/>
<connect gate="G$1" pin="D6" pad="22"/>
<connect gate="G$1" pin="D7" pad="21"/>
<connect gate="G$1" pin="D8" pad="20"/>
<connect gate="G$1" pin="EN" pad="12"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="10"/>
<connect gate="G$1" pin="GND@2" pad="14"/>
<connect gate="G$1" pin="GND@3" pad="17"/>
<connect gate="G$1" pin="GND@4" pad="24"/>
<connect gate="G$1" pin="RST" pad="13"/>
<connect gate="G$1" pin="RX" pad="19"/>
<connect gate="G$1" pin="S0" pad="8"/>
<connect gate="G$1" pin="S1" pad="6"/>
<connect gate="G$1" pin="S2" pad="5"/>
<connect gate="G$1" pin="S3" pad="4"/>
<connect gate="G$1" pin="SC" pad="7"/>
<connect gate="G$1" pin="SK" pad="9"/>
<connect gate="G$1" pin="TX" pad="18"/>
<connect gate="G$1" pin="VIN" pad="15"/>
<connect gate="G$1" pin="VV" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP07" prefix="ESP">
<description>ESP8266 Wifi module ESP-07 1MB (8Mb)</description>
<gates>
<gate name="G$1" symbol="ESP07"/>
</gates>
<devices>
<device name="SMT" package="2X08W_SMT_ESP07">
<connects>
<connect gate="G$1" pin="ADC" pad="ADC"/>
<connect gate="G$1" pin="CH_PD" pad="EN"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO12" pad="GPIO12"/>
<connect gate="G$1" pin="GPIO13" pad="GPIO13"/>
<connect gate="G$1" pin="GPIO14" pad="GPIO14"/>
<connect gate="G$1" pin="GPIO15" pad="GPIO15"/>
<connect gate="G$1" pin="GPIO16" pad="GPIO16"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="GPIO4" pad="GPIO4"/>
<connect gate="G$1" pin="GPIO5" pad="GPIO5"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="THT" package="2X08W_THT_ESP07">
<connects>
<connect gate="G$1" pin="ADC" pad="ADC"/>
<connect gate="G$1" pin="CH_PD" pad="EN"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO12" pad="GPIO12"/>
<connect gate="G$1" pin="GPIO13" pad="GPIO13"/>
<connect gate="G$1" pin="GPIO14" pad="GPIO14"/>
<connect gate="G$1" pin="GPIO15" pad="GPIO15"/>
<connect gate="G$1" pin="GPIO16" pad="GPIO16"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="GPIO4" pad="GPIO4"/>
<connect gate="G$1" pin="GPIO5" pad="GPIO5"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S-THERMAL" package="2X08W_SMT_ESP07S_ISOLATE">
<connects>
<connect gate="G$1" pin="ADC" pad="ADC"/>
<connect gate="G$1" pin="CH_PD" pad="EN"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO12" pad="GPIO12"/>
<connect gate="G$1" pin="GPIO13" pad="GPIO13"/>
<connect gate="G$1" pin="GPIO14" pad="GPIO14"/>
<connect gate="G$1" pin="GPIO15" pad="GPIO15"/>
<connect gate="G$1" pin="GPIO16" pad="GPIO16"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="GPIO4" pad="GPIO4"/>
<connect gate="G$1" pin="GPIO5" pad="GPIO5"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S-GND" package="2X08W_SMT_ESP07S_GNDPAD">
<connects>
<connect gate="G$1" pin="ADC" pad="ADC"/>
<connect gate="G$1" pin="CH_PD" pad="EN"/>
<connect gate="G$1" pin="GND" pad="GND GND1"/>
<connect gate="G$1" pin="GPIO0" pad="GPIO0"/>
<connect gate="G$1" pin="GPIO12" pad="GPIO12"/>
<connect gate="G$1" pin="GPIO13" pad="GPIO13"/>
<connect gate="G$1" pin="GPIO14" pad="GPIO14"/>
<connect gate="G$1" pin="GPIO15" pad="GPIO15"/>
<connect gate="G$1" pin="GPIO16" pad="GPIO16"/>
<connect gate="G$1" pin="GPIO2" pad="GPIO2"/>
<connect gate="G$1" pin="GPIO4" pad="GPIO4"/>
<connect gate="G$1" pin="GPIO5" pad="GPIO5"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
