(module SolderJumper-2_Open_Small (layer F.Cu) (tedit 5E47E630)
  (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
  (tags "solder jumper open")
  (attr virtual)
  (fp_text reference JP4 (at 0 -1.8 -180) (layer F.SilkS))
  (fp_text value SolderJumper_2_Open (at 0 1.9 -180) (layer F.Fab))
  (pad 1 connect custom (at -0.508 0) (size 0.508 0.508) (layers F.Cu F.Mask)
    (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_arc (start 0.1047 0) (end 0.1047 -0.4953) (angle -180) (width 0.05))
      (gr_line (start 0.2968 0.4953) (end 0.2968 -0.4953) (width 0.05))
      (gr_line (start 0.2968 -0.4953) (end 0.1047 -0.4953) (width 0.05))
      (gr_line (start 0.2968 0.4953) (end 0.1047 0.4953) (width 0.05))
      (gr_poly (pts
         (xy 0.2714 0.4826) (xy -0.008 0.4572) (xy -0.1477 0.4064) (xy -0.262 0.2921) (xy -0.3509 0.1143)
         (xy -0.3509 -0.1143) (xy -0.262 -0.3048) (xy -0.0207 -0.4572) (xy 0.2714 -0.4699)) (width 0.05))
    ))
  (pad 2 connect custom (at 0.508 0 180) (size 0.508 0.508) (layers F.Cu F.Mask)
    (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_arc (start 0.1047 0) (end 0.1047 -0.4953) (angle -180) (width 0.05))
      (gr_line (start 0.2968 0.4953) (end 0.2968 -0.4953) (width 0.05))
      (gr_line (start 0.2968 -0.4953) (end 0.1047 -0.4953) (width 0.05))
      (gr_line (start 0.2968 0.4953) (end 0.1047 0.4953) (width 0.05))
      (gr_poly (pts
         (xy 0.2714 0.4826) (xy -0.008 0.4572) (xy -0.1477 0.4064) (xy -0.262 0.2921) (xy -0.3509 0.1143)
         (xy -0.3509 -0.1143) (xy -0.262 -0.3048) (xy -0.0207 -0.4572) (xy 0.2714 -0.4699)) (width 0.05))
    ))
)
