(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 1331)
    (zones 0)
    (modules 184)
    (nets 133)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.1)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 2)
    (user_trace_width 3)
    (user_trace_width 4)
    (user_trace_width 5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.09)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.6 0.5)
    (uvia_size 0.6)
    (uvia_drill 0.3)
    (uvias_allowed no)
    (uvia_min_size 0.4)
    (uvia_min_drill 0.3)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 +12V)
  (net 4 +5V)
  (net 5 "Net-(C6-Pad2)")
  (net 6 "Net-(C7-Pad2)")
  (net 7 "Net-(C8-Pad1)")
  (net 8 +8V)
  (net 9 "Net-(C30-Pad2)")
  (net 10 "Net-(C30-Pad1)")
  (net 11 "Net-(C31-Pad1)")
  (net 12 "Net-(C32-Pad2)")
  (net 13 "Net-(C33-Pad2)")
  (net 14 "Net-(C34-Pad2)")
  (net 15 "Net-(C35-Pad2)")
  (net 16 "Net-(C36-Pad1)")
  (net 17 "Net-(C38-Pad1)")
  (net 18 "Net-(C39-Pad2)")
  (net 19 "Net-(C40-Pad1)")
  (net 20 "Net-(C41-Pad1)")
  (net 21 "Net-(C44-Pad1)")
  (net 22 +BATT)
  (net 23 "Net-(D4-Pad2)")
  (net 24 "Net-(D8-Pad2)")
  (net 25 "Net-(D8-Pad1)")
  (net 26 "Net-(D9-Pad1)")
  (net 27 "Net-(D9-Pad2)")
  (net 28 "Net-(D10-Pad1)")
  (net 29 "Net-(D10-Pad2)")
  (net 30 "Net-(D11-Pad1)")
  (net 31 "Net-(D11-Pad2)")
  (net 32 "Net-(D12-Pad2)")
  (net 33 "Net-(D12-Pad1)")
  (net 34 "Net-(D13-Pad1)")
  (net 35 "Net-(D13-Pad2)")
  (net 36 "Net-(D14-Pad2)")
  (net 37 "Net-(D14-Pad1)")
  (net 38 "Net-(D15-Pad2)")
  (net 39 "Net-(D15-Pad1)")
  (net 40 "Net-(K1-PadNC)")
  (net 41 "Net-(K1-PadNO)")
  (net 42 "Net-(K1-PadCOM)")
  (net 43 "Net-(K2-PadCOM)")
  (net 44 "Net-(K2-PadNO)")
  (net 45 "Net-(K2-PadNC)")
  (net 46 "Net-(K3-PadCOM)")
  (net 47 "Net-(K3-PadNO)")
  (net 48 "Net-(K3-PadNC)")
  (net 49 "Net-(K4-PadNC)")
  (net 50 "Net-(K4-PadNO)")
  (net 51 "Net-(K4-PadCOM)")
  (net 52 "Net-(K5-PadCOM)")
  (net 53 "Net-(K5-PadNO)")
  (net 54 "Net-(K5-PadNC)")
  (net 55 "Net-(R1-Pad2)")
  (net 56 "Net-(R1-Pad1)")
  (net 57 "Net-(R2-Pad1)")
  (net 58 "Net-(R2-Pad2)")
  (net 59 "Net-(R3-Pad1)")
  (net 60 "Net-(R6-Pad2)")
  (net 61 "Net-(R6-Pad1)")
  (net 62 "Net-(R10-Pad2)")
  (net 63 "Net-(R11-Pad2)")
  (net 64 "Net-(R12-Pad1)")
  (net 65 "Net-(R13-Pad2)")
  (net 66 "Net-(R13-Pad1)")
  (net 67 "Net-(R15-Pad1)")
  (net 68 "Net-(R15-Pad2)")
  (net 69 "Net-(R25-Pad1)")
  (net 70 "Net-(R26-Pad1)")
  (net 71 "Net-(R26-Pad2)")
  (net 72 "Net-(R30-Pad1)")
  (net 73 "Net-(R33-Pad1)")
  (net 74 "Net-(R33-Pad2)")
  (net 75 "Net-(R38-Pad2)")
  (net 76 "Net-(R40-Pad1)")
  (net 77 "Net-(R42-Pad1)")
  (net 78 "Net-(R42-Pad2)")
  (net 79 "Net-(R44-Pad2)")
  (net 80 "Net-(R44-Pad1)")
  (net 81 "Net-(R47-Pad1)")
  (net 82 "Net-(R50-Pad2)")
  (net 83 P0B)
  (net 84 P2A)
  (net 85 Sound_In)
  (net 86 P3B)
  (net 87 P0A)
  (net 88 M_Vin)
  (net 89 M_Sound)
  (net 90 M_Iges)
  (net 91 NC_K6)
  (net 92 NO_K6)
  (net 93 MISO)
  (net 94 SCK)
  (net 95 MOSI)
  (net 96 Reset)
  (net 97 SDA)
  (net 98 SCL)
  (net 99 RX)
  (net 100 TX)
  (net 101 P1A)
  (net 102 P1W)
  (net 103 P2W)
  (net 104 P0W)
  (net 105 OP_BL1)
  (net 106 OP_BL2)
  (net 107 OP_LEDRT)
  (net 108 OP_LEDGR)
  (net 109 OP_LEDBL)
  (net 110 OI_1)
  (net 111 OI_2)
  (net 112 OI_3)
  (net 113 OI_4)
  (net 114 Analog_OI_1)
  (net 115 P3W)
  (net 116 NC_K7)
  (net 117 NO_K7)
  (net 118 IN_K7)
  (net 119 NC_K8)
  (net 120 NO_K8)
  (net 121 IN_K6)
  (net 122 IN_K8)
  (net 123 "Net-(U15-Pad1)")
  (net 124 "Net-(U15-Pad2)")
  (net 125 "Net-(U15-Pad3)")
  (net 126 "Net-(U15-Pad4)")
  (net 127 "Net-(U15-Pad5)")
  (net 128 "Net-(U15-Pad6)")
  (net 129 "Net-(U15-Pad7)")
  (net 130 "Net-(U15-Pad8)")
  (net 131 "Net-(T1-Pad2)")
  (net 132 "Net-(T2-Pad2)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.6)
    (uvia_drill 0.3)
    (add_net +12V)
    (add_net +5V)
    (add_net +8V)
    (add_net +BATT)
    (add_net Analog_OI_1)
    (add_net GND)
    (add_net IN_K6)
    (add_net IN_K7)
    (add_net IN_K8)
    (add_net MISO)
    (add_net MOSI)
    (add_net M_Iges)
    (add_net M_Sound)
    (add_net M_Vin)
    (add_net NC_K6)
    (add_net NC_K7)
    (add_net NC_K8)
    (add_net NO_K6)
    (add_net NO_K7)
    (add_net NO_K8)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C30-Pad1)")
    (add_net "Net-(C30-Pad2)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C32-Pad2)")
    (add_net "Net-(C33-Pad2)")
    (add_net "Net-(C34-Pad2)")
    (add_net "Net-(C35-Pad2)")
    (add_net "Net-(C36-Pad1)")
    (add_net "Net-(C38-Pad1)")
    (add_net "Net-(C39-Pad2)")
    (add_net "Net-(C40-Pad1)")
    (add_net "Net-(C41-Pad1)")
    (add_net "Net-(C44-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad1)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad1)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(K1-PadCOM)")
    (add_net "Net-(K1-PadNC)")
    (add_net "Net-(K1-PadNO)")
    (add_net "Net-(K2-PadCOM)")
    (add_net "Net-(K2-PadNC)")
    (add_net "Net-(K2-PadNO)")
    (add_net "Net-(K3-PadCOM)")
    (add_net "Net-(K3-PadNC)")
    (add_net "Net-(K3-PadNO)")
    (add_net "Net-(K4-PadCOM)")
    (add_net "Net-(K4-PadNC)")
    (add_net "Net-(K4-PadNO)")
    (add_net "Net-(K5-PadCOM)")
    (add_net "Net-(K5-PadNC)")
    (add_net "Net-(K5-PadNO)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R25-Pad1)")
    (add_net "Net-(R26-Pad1)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R30-Pad1)")
    (add_net "Net-(R33-Pad1)")
    (add_net "Net-(R33-Pad2)")
    (add_net "Net-(R38-Pad2)")
    (add_net "Net-(R40-Pad1)")
    (add_net "Net-(R42-Pad1)")
    (add_net "Net-(R42-Pad2)")
    (add_net "Net-(R44-Pad1)")
    (add_net "Net-(R44-Pad2)")
    (add_net "Net-(R47-Pad1)")
    (add_net "Net-(R50-Pad2)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(T1-Pad2)")
    (add_net "Net-(T2-Pad2)")
    (add_net "Net-(U15-Pad1)")
    (add_net "Net-(U15-Pad2)")
    (add_net "Net-(U15-Pad3)")
    (add_net "Net-(U15-Pad4)")
    (add_net "Net-(U15-Pad5)")
    (add_net "Net-(U15-Pad6)")
    (add_net "Net-(U15-Pad7)")
    (add_net "Net-(U15-Pad8)")
    (add_net OI_1)
    (add_net OI_2)
    (add_net OI_3)
    (add_net OI_4)
    (add_net OP_BL1)
    (add_net OP_BL2)
    (add_net OP_LEDBL)
    (add_net OP_LEDGR)
    (add_net OP_LEDRT)
    (add_net P0A)
    (add_net P0B)
    (add_net P0W)
    (add_net P1A)
    (add_net P1W)
    (add_net P2A)
    (add_net P2W)
    (add_net P3B)
    (add_net P3W)
    (add_net RX)
    (add_net Reset)
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net Sound_In)
    (add_net TX)
  )
  (module RELAY_1-1721150-3 (layer F.Cu) (tedit 0)
    (at 121.0945 124.714 270)
    (fp_text reference K5 (at -7.26069 -8.83584 90) (layer F.SilkS))
    (fp_text value 1-1721150-3 (at -6.62706 8.6677 90) (layer F.SilkS))
    (pad NC thru_hole circle (at 6.1 -6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 54 "Net-(K5-PadNC)"))
    (pad NO thru_hole circle (at 6.1 6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 53 "Net-(K5-PadNO)"))
    (pad A2 thru_hole circle (at -6.1 6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 34 "Net-(D13-Pad1)"))
    (pad COM thru_hole circle (at -8.1 0 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 52 "Net-(K5-PadCOM)"))
    (pad A1 thru_hole rect (at -6.1 -6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +12V))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 128.3335 96.012)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at 0 -1.43 -180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 -180) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +8V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 128.3335 94.234 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1µ (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +8V))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer B.Cu) (tedit 5A02F2D3)
    (at 128.397 95.25)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 5.375) (layer B.SilkS))
    (fp_text value LM324 (at 0 -5.375) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 106 OP_BL2))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 8 +8V))
    (pad 5 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 107 OP_LEDRT))
    (pad 6 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(R6-Pad1)"))
    (pad 8 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(R13-Pad1)"))
    (pad 9 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 108 OP_LEDGR))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 109 OP_LEDBL))
    (pad 13 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(R15-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RELAY_1-1721150-3 (layer F.Cu) (tedit 0)
    (at 157.861 124.714 270)
    (fp_text reference K3 (at -7.26069 -8.83584 90) (layer F.SilkS))
    (fp_text value 1-1721150-3 (at -6.62706 8.6677 90) (layer F.SilkS))
    (pad NC thru_hole circle (at 6.1 -6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 48 "Net-(K3-PadNC)"))
    (pad NO thru_hole circle (at 6.1 6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 47 "Net-(K3-PadNO)"))
    (pad A2 thru_hole circle (at -6.1 6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 30 "Net-(D11-Pad1)"))
    (pad COM thru_hole circle (at -8.1 0 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 46 "Net-(K3-PadCOM)"))
    (pad A1 thru_hole rect (at -6.1 -6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +12V))
  )
  (module RELAY_1-1721150-3 (layer F.Cu) (tedit 0)
    (at 194.691 124.714 270)
    (fp_text reference K1 (at -7.26069 -8.83584 90) (layer F.SilkS))
    (fp_text value 1-1721150-3 (at -6.62706 8.6677 90) (layer F.SilkS))
    (pad NC thru_hole circle (at 6.1 -6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 40 "Net-(K1-PadNC)"))
    (pad NO thru_hole circle (at 6.1 6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 41 "Net-(K1-PadNO)"))
    (pad A2 thru_hole circle (at -6.1 6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 26 "Net-(D9-Pad1)"))
    (pad COM thru_hole circle (at -8.1 0 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 42 "Net-(K1-PadCOM)"))
    (pad A1 thru_hole rect (at -6.1 -6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +12V))
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal (layer F.Cu) (tedit 5B785047)
    (at 80.391 78.486 270)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
    (fp_text reference X1 (at 2.54 -3.2 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 2.54 11.2 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.3 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 131 "Net-(T1-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 22 +BATT))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 147.701 68.834 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C40 (at 0 -1.43 -90) (layer F.SilkS))
    (fp_text value 1µ (at 0 1.43 -90) (layer F.Fab))
    (fp_text user %R (at 0 0 -90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C40-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 133.985 65.659 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R46 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 15k0 (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(R44-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 133.985 68.834 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R44 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 68k0 (at 2.54 0 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(R44-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(R44-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer B.Cu) (tedit 5A02F2D3)
    (at 181.356 61.849 180)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U8 (at 0 5.375) (layer B.SilkS))
    (fp_text value TL064 (at 0 -5.375) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2.7 3.81 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 84 P2A))
    (pad 2 smd rect (at -2.7 2.54 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C36-Pad1)"))
    (pad 3 smd rect (at -2.7 1.27 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 83 P0B))
    (pad 4 smd rect (at -2.7 0 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(C44-Pad1)"))
    (pad 5 smd rect (at -2.7 -1.27 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 115 P3W))
    (pad 6 smd rect (at -2.7 -2.54 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C35-Pad2)"))
    (pad 7 smd rect (at -2.7 -3.81 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C33-Pad2)"))
    (pad 8 smd rect (at 2.7 -3.81 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 87 P0A))
    (pad 9 smd rect (at 2.7 -2.54 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 87 P0A))
    (pad 10 smd rect (at 2.7 -1.27 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C41-Pad1)"))
    (pad 11 smd rect (at 2.7 0 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 2.7 1.27 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C30-Pad1)"))
    (pad 13 smd rect (at 2.7 2.54 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 101 P1A))
    (pad 14 smd rect (at 2.7 3.81 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 101 P1A))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 90.551 59.309 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C2 (at 1 -3.75 180) (layer F.SilkS))
    (fp_text value 10µ (at 1 3.75 180) (layer F.Fab))
    (fp_text user %R (at 1 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_HC49-SD (layer F.Cu) (tedit 5A1AD52C)
    (at 149.6695 91.0844 270)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Q1 (at 0 -3.55 270) (layer F.SilkS))
    (fp_text value 16MHz (at 0 3.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -4.25 0 270) (size 4.5 2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 4.25 0 270) (size 4.5 2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_HC49-SD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprintsSTP:STP16NF06 (layer F.Cu) (tedit 0)
    (at 86.995 84.729 270)
    (fp_text reference T1 (at -2.55 0.762 90) (layer F.SilkS))
    (fp_text value STP16NF06 (at -2.55 0.762 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 3 thru_hole circle (at 0 1.524 270) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.55 1.524 270) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 131 "Net-(T1-Pad2)"))
    (pad 1 thru_hole rect (at -5.1 1.524 270) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 55 "Net-(R1-Pad2)"))
  )
  (module digikey-footprints:TO-220-3 (layer F.Cu) (tedit 5AFA02CB)
    (at 85.471 53.594)
    (descr http://www.st.com/content/ccc/resource/technical/document/datasheet/f9/ed/f5/44/26/b9/43/a4/CD00000911.pdf/files/CD00000911.pdf/jcr:content/translations/en.CD00000911.pdf)
    (fp_text reference U1 (at 2.62 -3.22) (layer F.SilkS))
    (fp_text value LM1085-12 (at 2.27 3.63) (layer F.Fab))
    (fp_text user %R (at 2.52 -0.01) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 186.1335 59.944)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C36 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 180n (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C36-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C34-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 182.626 58.674 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R36 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 P2A))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C36-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RELAY_1-1721150-3 (layer F.Cu) (tedit 0)
    (at 95.631 113.284)
    (fp_text reference K7 (at -7.26069 -8.83584) (layer F.SilkS))
    (fp_text value 1-1721150-3 (at -6.62706 8.6677) (layer F.SilkS))
    (pad A1 thru_hole rect (at -6.1 -6) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad COM thru_hole circle (at -8.1 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 118 IN_K7))
    (pad A2 thru_hole circle (at -6.1 6) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 25 "Net-(D8-Pad1)"))
    (pad NO thru_hole circle (at 6.1 6) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 117 NO_K7))
    (pad NC thru_hole circle (at 6.1 -6) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 116 NC_K7))
  )
  (module RELAY_1-1721150-3 (layer F.Cu) (tedit 0)
    (at 95.631 129.794)
    (fp_text reference K8 (at -7.26069 -8.83584) (layer F.SilkS))
    (fp_text value 1-1721150-3 (at -6.62706 8.6677) (layer F.SilkS))
    (pad NC thru_hole circle (at 6.1 -6) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 119 NC_K8))
    (pad NO thru_hole circle (at 6.1 6) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 120 NO_K8))
    (pad A2 thru_hole circle (at -6.1 6) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 39 "Net-(D15-Pad1)"))
    (pad COM thru_hole circle (at -8.1 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 122 IN_K8))
    (pad A1 thru_hole rect (at -6.1 -6) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +12V))
  )
  (module RELAY_1-1721150-3 (layer F.Cu) (tedit 0)
    (at 98.806 96.774)
    (fp_text reference K6 (at -7.26069 -8.83584) (layer F.SilkS))
    (fp_text value 1-1721150-3 (at -6.62706 8.6677) (layer F.SilkS))
    (pad A1 thru_hole rect (at -6.1 -6) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad COM thru_hole circle (at -8.1 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 121 IN_K6))
    (pad A2 thru_hole circle (at -6.1 6) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 37 "Net-(D14-Pad1)"))
    (pad NO thru_hole circle (at 6.1 6) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 92 NO_K6))
    (pad NC thru_hole circle (at 6.1 -6) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 91 NC_K6))
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal (layer F.Cu) (tedit 5B785047)
    (at 80.391 120.65 270)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
    (fp_text reference X16 (at 2.54 -3.2 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 2.54 11.2 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.3 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 118 IN_K7))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 22 +BATT))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 158.75 94.107 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 0 1.43) (layer B.SilkS))
    (fp_text value 1µ (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 145.288 90.2335)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1µ (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal (layer F.Cu) (tedit 5B785047)
    (at 80.391 64.389 270)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
    (fp_text reference X2 (at 2.54 -3.2 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 2.54 11.2 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.3 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 22 +BATT))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D12.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 93.345 68.8975 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 2.5 -7.5 270) (layer F.SilkS))
    (fp_text value 470µ (at 2.5 7.5 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "footprints AVX_TYP_A_3516:TAJA106K016RNJ" (layer B.Cu) (tedit 0)
    (at 88.0745 56.8325 180)
    (fp_text reference C3 (at 0 0 180) (layer B.SilkS))
    (fp_text value T10µ (at 0 0 180) (layer B.SilkS))
    (fp_text user * (at 0 0 180) (layer B.Fab))
    (fp_text user * (at 0 0 180) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 180) (layer Cmts.User))
    (pad 2 smd rect (at 1.0922 0 90) (size 1.1938 1.3716) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.0922 0 90) (size 1.1938 1.3716) (layers B.Cu B.Paste B.Mask)
      (net 3 +12V))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 97.536 58.674)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 1.43) (layer B.SilkS))
    (fp_text value 330n (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 100.711 58.674 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 145.288 91.8718)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1µ (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C7-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D12.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 206.5655 64.1985 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (fp_text reference C8 (at 2.5 -7.5 270) (layer F.SilkS))
    (fp_text value 470µ (at 2.5 7.5 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 204.0255 66.7385 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 1µ (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C8-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 210.8708 109.7661 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +12V))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 212.7504 109.7915 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 1µ (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +12V))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 197.7644 106.1974 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 199.39 106.1974 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 1µ (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 158.75 95.885)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0 1.43) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 148.082 112.268 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 148.082 110.236)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1µ (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 214.204999 93.829001 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 212.471 93.829001 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 1µ (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 195.961 86.7665 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 197.866 86.7665 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 1µ (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 211.201 129.794 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 209.296 129.794 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 1µ (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 222.474999 129.690001 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 220.726 129.690001 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 1µ (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5E0D19B1)
    (at 89.281 82.804 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 +8V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 89.281 84.582)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at 0 1.43) (layer B.SilkS))
    (fp_text value 1µ (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 +8V))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 178.181 71.374)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at 0 1.43) (layer B.SilkS))
    (fp_text value 4n7 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C30-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C30-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 148.336 61.214 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C31 (at 0 -1.43 -90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.43 -90) (layer F.Fab))
    (fp_text user %R (at 0 0 -90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C31-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 189.4585 74.549 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C32 (at 0 1.43) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 83 P0B))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C32-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 181.991 71.374)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C33 (at 0 1.43) (layer B.SilkS))
    (fp_text value 4n7 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C30-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C33-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 186.1335 57.404)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C34 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 180n (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C34-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 P2A))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 185.801 68.199)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C35 (at 0 1.43) (layer B.SilkS))
    (fp_text value 22p (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C35-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C33-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 215.011 73.914)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C37 (at 0 1.43) (layer B.SilkS))
    (fp_text value 1µ (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 Sound_In))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 P3B))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 152.146 54.839 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C38 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C38-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 178.181 75.184 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C39 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 P0A))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C39-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 174.371 77.724)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C41 (at 0 1.43) (layer B.SilkS))
    (fp_text value 47n (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C41-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 171.704 60.1345 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C42 (at 0 1.43) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 171.704 58.3565 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C43 (at 0 1.43) (layer B.SilkS))
    (fp_text value 1µ (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 181.1655 63.246 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C44 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C44-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 181.1655 61.595 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C45 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1µ (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C44-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 142.1385 62.484)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C46 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +8V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 142.1385 64.389)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C47 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1µ (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +8V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D12.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 103.251 65.659)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (fp_text reference C48 (at 2.5 -7.5) (layer F.SilkS))
    (fp_text value 470µ (at 2.5 7.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 +BATT))
    (pad 2 thru_hole circle (at 5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 117.856 58.674 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C49 (at 0 1.43) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 +8V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D12.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 127.461 59.69)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (fp_text reference C50 (at 2.5 -7.5) (layer F.SilkS))
    (fp_text value 470µ (at 2.5 7.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 +8V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 119.126 78.994)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C51 (at 0 1.43) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 83 P0B))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D12.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 116.586 70.104)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (fp_text reference C52 (at 2.5 -7.5) (layer F.SilkS))
    (fp_text value 470µ (at 2.5 7.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 83 P0B))
    (pad 2 thru_hole circle (at 5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-libraries-master:DO-214AA (layer B.Cu) (tedit 4FF97487)
    (at 87.5665 68.8975 180)
    (descr "DO214AC PACKAGE. MONODIRECTIONAL.")
    (tags "DO214AC PACKAGE. MONODIRECTIONAL.")
    (attr smd)
    (fp_text reference D1 (at 0.0508 2.55016 180) (layer B.SilkS))
    (fp_text value D (at 0.0508 -1.5494 180) (layer B.SilkS))
    (pad 1 smd rect (at -2.11074 0 180) (size 1.62052 2.17932) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2.11074 0 180) (size 1.62052 2.17932) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model smd/do214.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer B.Cu) (tedit 58645DC7)
    (at 180.467 94.615 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 0 2 270) (layer B.SilkS))
    (fp_text value D_Schottky (at 0 -2.1 270) (layer B.Fab))
    (fp_text user %R (at 0 2 270) (layer B.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 88 M_Vin))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer B.Cu) (tedit 58645DC7)
    (at 180.213 101.473 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 0 2 90) (layer B.SilkS))
    (fp_text value D_Schottky (at 0 -2.1 90) (layer B.Fab))
    (fp_text user %R (at 0 2 90) (layer B.Fab))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 88 M_Vin))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 162.179 97.282 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D4 (at 0 2.5 90) (layer B.SilkS))
    (fp_text value LM4040DBZ-4.1 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D4-Pad2)"))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer B.Cu) (tedit 58645DC7)
    (at 206.121 73.279)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D5 (at 0 2) (layer B.SilkS))
    (fp_text value D_Schottky (at 0 -2.1) (layer B.Fab))
    (fp_text user %R (at 0 2) (layer B.Fab))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 85 Sound_In))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer B.Cu) (tedit 58645DC7)
    (at 210.8835 56.8325 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D6 (at 0 2 270) (layer B.SilkS))
    (fp_text value D_Schottky (at 0 -2.1 270) (layer B.Fab))
    (fp_text user %R (at 0 2 270) (layer B.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 89 M_Sound))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer B.Cu) (tedit 58645DC7)
    (at 209.8675 63.1825 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D7 (at 0 2 270) (layer B.SilkS))
    (fp_text value D_Schottky (at 0 -2.1 270) (layer B.Fab))
    (fp_text user %R (at 0 2 270) (layer B.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 89 M_Sound))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 181.991 82.931 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D16 (at 0 -2 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 90 M_Iges))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 177.546 82.931 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D17 (at 0 -2 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 90 M_Iges))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_2920_7451Metric (layer B.Cu) (tedit 5E0D0971)
    (at 89.916 63.754 180)
    (descr "Fuse SMD 2920 (7451 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://www.megastar.com/products/fusetronic/polyswitch/PDF/smd2920.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F1 (at 0 3.68 180) (layer B.SilkS))
    (fp_text value Fuse (at 0 -3.68 180) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -3.3875 0 180) (size 1.925 5.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.12987)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 3.3875 0 180) (size 1.925 5.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.12987)
      (net 22 +BATT))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_2920_7451Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 178.8795 54.356 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Jumper_3_Open (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 +8V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(C44-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 150.622 103.251 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference PG1 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 MISO))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 MOSI))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 Reset))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 89.03 75.692 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 1.82 180) (layer B.SilkS))
    (fp_text value 100R0 (at 0 -1.82 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 55 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 56 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 92.837 93.726 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 1.82 180) (layer B.SilkS))
    (fp_text value 100R0 (at 0 -1.82 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 57 "Net-(R2-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 58 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 186.1566 100.6856 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 10k0 (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 +BATT))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 158.496 98.298 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 1.43) (layer B.SilkS))
    (fp_text value 909R (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D4-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 181.737 98.044)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value 1k0 (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(R3-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 M_Vin))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 116.586 91.059 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 1.82 270) (layer B.SilkS))
    (fp_text value 100R0 (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 60 "Net-(R6-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 61 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 172.593 83.2865 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value 10k0 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 SDA))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 169.545 83.2865 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value 10k0 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.497 83.2865 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 1k0 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 Reset))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 197.485 82.804 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 1.524) (layer B.SilkS))
    (fp_text value 1k0 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 99 RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 197.485 80.264 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 1.43) (layer B.SilkS))
    (fp_text value 1k0 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 100 TX))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 203.5175 62.4205 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 1.82 270) (layer B.SilkS))
    (fp_text value 10k0 (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 7 "Net-(C8-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 64 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 112.141 113.414 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 1.82 270) (layer B.SilkS))
    (fp_text value 100R0 (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 65 "Net-(R13-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 66 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 206.0575 59.1185 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0 1.43) (layer B.SilkS))
    (fp_text value 1k0 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 M_Sound))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 112.141 136.144 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0 1.82 270) (layer B.SilkS))
    (fp_text value 100R0 (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 67 "Net-(R15-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 68 "Net-(R15-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 174.371 71.374 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 0 1.43) (layer B.SilkS))
    (fp_text value 22k0 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C30-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 83 P0B))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 154.686 61.849 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(R25-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C31-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 112.141 125.349 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value 100R0 (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 70 "Net-(R26-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 71 "Net-(R26-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 150.876 61.214 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R27 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value 1M0 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C31-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 181.356 68.834 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R28 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 10k0 (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C30-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 101 P1A))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 185.801 74.549)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R29 (at 0 1.43) (layer B.SilkS))
    (fp_text value 1k0 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C32-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C33-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.956 54.229 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R30 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(R30-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C38-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 185.801 71.374 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R31 (at 0 1.43) (layer B.SilkS))
    (fp_text value 100k0 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C35-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C33-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 181.991 77.724)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R32 (at 0 1.43) (layer B.SilkS))
    (fp_text value 1k0 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C33-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C34-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 122.555 108.966 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R33 (at 0 1.82 180) (layer B.SilkS))
    (fp_text value 100R0 (at 0 -1.82 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 73 "Net-(R33-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 74 "Net-(R33-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 149.606 54.839 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R34 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value 1M0 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C38-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 188.976 58.674 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R35 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 10k0 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C34-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 181.991 74.549)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R37 (at 0 1.43) (layer B.SilkS))
    (fp_text value 12k0 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C33-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C39-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 211.201 72.009 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R38 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value 220R (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 85 Sound_In))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 75 "Net-(R38-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 215.011 69.469 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R39 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value 22k0 (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 85 Sound_In))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 153.416 69.469 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R40 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(R40-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C40-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 174.371 74.549)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R41 (at 0 1.43) (layer B.SilkS))
    (fp_text value 10k0 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C39-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C41-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 112.903 84.582 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R42 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 100R0 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 77 "Net-(R42-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 78 "Net-(R42-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 150.241 68.834 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R43 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value 1M0 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C40-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 136.906 65.659 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R45 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 15k0 (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(R44-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 +8V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 136.906 68.834 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R47 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 100k0 (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(R47-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(R44-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 105.156 78.994)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R48 (at 3.81 -2.37) (layer F.SilkS))
    (fp_text value 4k7 (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +8V))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 P0B))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 115.3795 78.994)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R49 (at 3.81 -2.37) (layer F.SilkS))
    (fp_text value 4k7 (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 P0B))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 186.436 81.026)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R50 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 1k0 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 82 "Net-(R50-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 90 M_Iges))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296Y_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 182.9816 94.9706 90)
    (descr "Potentiometer, vertical, Bourns 3296Y, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296Y")
    (fp_text reference RV1 (at -2.54 -2.39 270) (layer F.SilkS))
    (fp_text value 5k0 (at -2.54 4.94 270) (layer F.Fab))
    (fp_text user %R (at -3.175 1.275 270) (layer F.Fab))
    (pad 3 thru_hole circle (at -5.08 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296Y_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296Y_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 203.2635 58.1025 180)
    (descr "Potentiometer, vertical, Bourns 3296Y, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296Y")
    (fp_text reference RV2 (at -2.54 -2.39) (layer F.SilkS))
    (fp_text value 5k0 (at -2.54 4.94) (layer F.Fab))
    (fp_text user %R (at -3.175 1.275) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(R12-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 2.54 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at -5.08 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296Y_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TO-92-3_Formed_Leads (layer F.Cu) (tedit 5AF4B307)
    (at 159.131 66.929 90)
    (descr http://www.ti.com/lit/ds/symlink/tl431a.pdf)
    (fp_text reference T6 (at 2.6 -3.35 90) (layer F.SilkS))
    (fp_text value BC548CTA (at 2.6 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.6 -1.25 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.6 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 102 P1W))
    (pad 3 thru_hole circle (at 5.2 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 69 "Net-(R25-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 +8V))
  )
  (module digikey-footprints:TO-92-3_Formed_Leads (layer F.Cu) (tedit 5AF4B307)
    (at 160.401 59.309 90)
    (descr http://www.ti.com/lit/ds/symlink/tl431a.pdf)
    (fp_text reference T8 (at 2.6 -3.35 90) (layer F.SilkS))
    (fp_text value BC548CTA (at 2.6 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.6 -1.25 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 +8V))
    (pad 3 thru_hole circle (at 5.2 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 72 "Net-(R30-Pad1)"))
    (pad 2 thru_hole circle (at 2.6 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 103 P2W))
  )
  (module digikey-footprints:TO-92-3_Formed_Leads (layer F.Cu) (tedit 5AF4B307)
    (at 157.861 74.609 90)
    (descr http://www.ti.com/lit/ds/symlink/tl431a.pdf)
    (fp_text reference T10 (at 2.6 -3.35 90) (layer F.SilkS))
    (fp_text value BC548CTA (at 2.6 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.6 -1.25 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.6 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 104 P0W))
    (pad 3 thru_hole circle (at 5.2 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 76 "Net-(R40-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 +8V))
  )
  (module TestPoint:TestPoint_Plated_Hole_D2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 96.901 62.484)
    (descr "Plated Hole as test Point, diameter 2.0mm")
    (tags "test point plated hole")
    (attr virtual)
    (fp_text reference TP1 (at 0 -2.498) (layer F.SilkS))
    (fp_text value 5000 (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module TestPoint:TestPoint_Plated_Hole_D2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 107.696 52.324)
    (descr "Plated Hole as test Point, diameter 2.0mm")
    (tags "test point plated hole")
    (attr virtual)
    (fp_text reference TP2 (at 0 -2.498) (layer F.SilkS))
    (fp_text value 5000 (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 3 +12V))
  )
  (module TestPoint:TestPoint_Plated_Hole_D2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 107.696 56.769)
    (descr "Plated Hole as test Point, diameter 2.0mm")
    (tags "test point plated hole")
    (attr virtual)
    (fp_text reference TP3 (at 0 -2.498) (layer F.SilkS))
    (fp_text value 5000 (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 4 +5V))
  )
  (module TestPoint:TestPoint_Plated_Hole_D2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 171.831 99.06 180)
    (descr "Plated Hole as test Point, diameter 2.0mm")
    (tags "test point plated hole")
    (attr virtual)
    (fp_text reference TP4 (at 0 -2.498) (layer F.SilkS))
    (fp_text value 5000 (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 88 M_Vin))
  )
  (module TestPoint:TestPoint_Plated_Hole_D2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 159.258 103.632)
    (descr "Plated Hole as test Point, diameter 2.0mm")
    (tags "test point plated hole")
    (attr virtual)
    (fp_text reference TP5 (at 0 -2.498) (layer F.SilkS))
    (fp_text value 5000 (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 23 "Net-(D4-Pad2)"))
  )
  (module TestPoint:TestPoint_Plated_Hole_D2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 213.1695 60.6425 90)
    (descr "Plated Hole as test Point, diameter 2.0mm")
    (tags "test point plated hole")
    (attr virtual)
    (fp_text reference TP6 (at 0 -2.498 90) (layer F.SilkS))
    (fp_text value 5000 (at 0 2.45 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 89 M_Sound))
  )
  (module TestPoint:TestPoint_Plated_Hole_D2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 115.316 61.519)
    (descr "Plated Hole as test Point, diameter 2.0mm")
    (tags "test point plated hole")
    (attr virtual)
    (fp_text reference TP7 (at 0 -2.498) (layer F.SilkS))
    (fp_text value 5000 (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 8 +8V))
  )
  (module TestPoint:TestPoint_Plated_Hole_D2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 110.871 74.549)
    (descr "Plated Hole as test Point, diameter 2.0mm")
    (tags "test point plated hole")
    (attr virtual)
    (fp_text reference TP8 (at 0 -2.498) (layer F.SilkS))
    (fp_text value 5000 (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 83 P0B))
  )
  (module TestPoint:TestPoint_Plated_Hole_D2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 167.259 103.632)
    (descr "Plated Hole as test Point, diameter 2.0mm")
    (tags "test point plated hole")
    (attr virtual)
    (fp_text reference TP9 (at 0 -2.498) (layer F.SilkS))
    (fp_text value 5000 (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 90 M_Iges))
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 89.027 78.994)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 0 2.9) (layer B.SilkS))
    (fp_text value LM321 (at 0 -2.9) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 105 OP_BL1))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(R1-Pad1)"))
    (pad 5 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 8 +8V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TO-220-3 (layer F.Cu) (tedit 5AFA02CB)
    (at 96.901 56.134)
    (descr http://www.st.com/content/ccc/resource/technical/document/datasheet/f9/ed/f5/44/26/b9/43/a4/CD00000911.pdf/files/CD00000911.pdf/jcr:content/translations/en.CD00000911.pdf)
    (fp_text reference U3 (at 2.62 -3.22) (layer F.SilkS))
    (fp_text value MC7805CT-BP (at 2.27 3.63) (layer F.Fab))
    (fp_text user %R (at 2.52 -0.01) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
  )
  (module Package_QFP:TQFP-32_7x7mm_P0.8mm (layer F.Cu) (tedit 5A02F146)
    (at 159.6644 95.9612 270)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U5 (at 0 -6.05 270) (layer F.SilkS))
    (fp_text value ATmega328-AU (at 0 6.05 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 109 OP_LEDBL))
    (pad 2 smd rect (at -4.25 -2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 110 OI_1))
    (pad 3 smd rect (at -4.25 -1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -4.25 -0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 5 smd rect (at -4.25 0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.25 1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 7 smd rect (at -4.25 2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad2)"))
    (pad 8 smd rect (at -4.25 2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad2)"))
    (pad 9 smd rect (at -2.8 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 111 OI_2))
    (pad 10 smd rect (at -2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 112 OI_3))
    (pad 11 smd rect (at -1.2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 113 OI_4))
    (pad 12 smd rect (at -0.4 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 105 OP_BL1))
    (pad 13 smd rect (at 0.4 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 106 OP_BL2))
    (pad 14 smd rect (at 1.2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 107 OP_LEDRT))
    (pad 15 smd rect (at 2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 95 MOSI))
    (pad 16 smd rect (at 2.8 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 93 MISO))
    (pad 17 smd rect (at 4.25 2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 94 SCK))
    (pad 18 smd rect (at 4.25 2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 19 smd rect (at 4.25 1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 4.25 0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D4-Pad2)"))
    (pad 21 smd rect (at 4.25 -0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 4.25 -1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 4.25 -2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 114 Analog_OI_1))
    (pad 24 smd rect (at 4.25 -2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 89 M_Sound))
    (pad 25 smd rect (at 2.8 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 90 M_Iges))
    (pad 26 smd rect (at 2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 88 M_Vin))
    (pad 27 smd rect (at 1.2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 97 SDA))
    (pad 28 smd rect (at 0.4 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 98 SCL))
    (pad 29 smd rect (at -0.4 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 96 Reset))
    (pad 30 smd rect (at -1.2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R10-Pad2)"))
    (pad 31 smd rect (at -2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R11-Pad2)"))
    (pad 32 smd rect (at -2.8 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 108 OP_LEDGR))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 202.311 105.664 90)
    (descr "16-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U7 (at 0 -6.25 90) (layer F.SilkS))
    (fp_text value PCF8574A (at 0 6.25 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.65 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -4.65 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -4.65 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -4.65 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(U15-Pad1)"))
    (pad 5 smd rect (at -4.65 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(U15-Pad2)"))
    (pad 6 smd rect (at -4.65 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(U15-Pad3)"))
    (pad 7 smd rect (at -4.65 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(U15-Pad4)"))
    (pad 8 smd rect (at -4.65 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 4.65 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(U15-Pad5)"))
    (pad 10 smd rect (at 4.65 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(U15-Pad6)"))
    (pad 11 smd rect (at 4.65 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(U15-Pad7)"))
    (pad 12 smd rect (at 4.65 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(U15-Pad8)"))
    (pad 13 smd rect (at 4.65 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 4.65 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 98 SCL))
    (pad 15 smd rect (at 4.65 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 97 SDA))
    (pad 16 smd rect (at 4.65 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer B.Cu) (tedit 5A02F2D3)
    (at 141.986 65.659)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U9 (at 0 5.375) (layer B.SilkS))
    (fp_text value LM324 (at 0 -5.375) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 14 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(R26-Pad1)"))
    (pad 13 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(R47-Pad1)"))
    (pad 12 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C31-Pad1)"))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(C38-Pad1)"))
    (pad 9 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(R47-Pad1)"))
    (pad 8 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(R33-Pad1)"))
    (pad 7 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(R42-Pad1)"))
    (pad 6 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(R47-Pad1)"))
    (pad 5 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C40-Pad1)"))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 8 +8V))
    (pad 3 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(R44-Pad1)"))
    (pad 2 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(R47-Pad1)"))
    (pad 1 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(R44-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 114.681 55.499)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference U11 (at 2.54 -4.27) (layer F.SilkS))
    (fp_text value L7808 (at 2.54 2.5) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 +8V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 +BATT))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal (layer F.Cu) (tedit 5B785047)
    (at 80.391 92.71 270)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
    (fp_text reference X3 (at 2.54 -3.2 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 2.54 11.2 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.3 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 22 +BATT))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 132 "Net-(T2-Pad2)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal (layer F.Cu) (tedit 5B785047)
    (at 190.119 138.43)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/3-G-5,08; number of pins: 03; pin pitch: 5.08mm; Angled || order number: 1757255 12A || order number: 1923872 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x03_G_5.08mm")
    (fp_text reference X4 (at 5.08 -3.2) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 5.08 11.2) (layer F.Fab))
    (fp_text user %R (at 5.08 -1.3) (layer F.Fab))
    (pad 3 thru_hole oval (at 10.16 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 40 "Net-(K1-PadNC)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 42 "Net-(K1-PadCOM)"))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 41 "Net-(K1-PadNO)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal (layer F.Cu) (tedit 5B785047)
    (at 171.577 138.43)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/3-G-5,08; number of pins: 03; pin pitch: 5.08mm; Angled || order number: 1757255 12A || order number: 1923872 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x03_G_5.08mm")
    (fp_text reference X5 (at 5.08 -3.2) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 5.08 11.2) (layer F.Fab))
    (fp_text user %R (at 5.08 -1.3) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 44 "Net-(K2-PadNO)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 43 "Net-(K2-PadCOM)"))
    (pad 3 thru_hole oval (at 10.16 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 45 "Net-(K2-PadNC)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal (layer F.Cu) (tedit 5B785047)
    (at 153.035 138.43)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/3-G-5,08; number of pins: 03; pin pitch: 5.08mm; Angled || order number: 1757255 12A || order number: 1923872 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x03_G_5.08mm")
    (fp_text reference X6 (at 5.08 -3.2) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 5.08 11.2) (layer F.Fab))
    (fp_text user %R (at 5.08 -1.3) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 47 "Net-(K3-PadNO)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 46 "Net-(K3-PadCOM)"))
    (pad 3 thru_hole oval (at 10.16 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 48 "Net-(K3-PadNC)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal (layer F.Cu) (tedit 5B785047)
    (at 134.493 138.43)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/3-G-5,08; number of pins: 03; pin pitch: 5.08mm; Angled || order number: 1757255 12A || order number: 1923872 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x03_G_5.08mm")
    (fp_text reference X7 (at 5.08 -3.2) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 5.08 11.2) (layer F.Fab))
    (fp_text user %R (at 5.08 -1.3) (layer F.Fab))
    (pad 3 thru_hole oval (at 10.16 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 49 "Net-(K4-PadNC)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 51 "Net-(K4-PadCOM)"))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 50 "Net-(K4-PadNO)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal (layer F.Cu) (tedit 5B785047)
    (at 115.951 138.43)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/3-G-5,08; number of pins: 03; pin pitch: 5.08mm; Angled || order number: 1757255 12A || order number: 1923872 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x03_G_5.08mm")
    (fp_text reference X8 (at 5.08 -3.2) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 5.08 11.2) (layer F.Fab))
    (fp_text user %R (at 5.08 -1.3) (layer F.Fab))
    (pad 3 thru_hole oval (at 10.16 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 54 "Net-(K5-PadNC)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 52 "Net-(K5-PadCOM)"))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 53 "Net-(K5-PadNO)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal (layer F.Cu) (tedit 5B785047)
    (at 219.202 73.914 90)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/3-G-5,08; number of pins: 03; pin pitch: 5.08mm; Angled || order number: 1757255 12A || order number: 1923872 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x03_G_5.08mm")
    (fp_text reference X9 (at 5.08 -3.2 270) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 5.08 11.2 270) (layer F.Fab))
    (fp_text user %R (at 5.08 -1.3 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 85 Sound_In))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 75 "Net-(R38-Pad2)"))
    (pad 3 thru_hole oval (at 10.16 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 192.151 87.884 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference X10 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(R50-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 207.391 122.809)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference X11 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 SDA))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 SCL))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 213.106 122.809)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference X12 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 SCL))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 SDA))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 224.536 122.809)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference X13 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 SCL))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 SDA))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 218.821 122.809)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference X14 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 SDA))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 SCL))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal (layer F.Cu) (tedit 5B785047)
    (at 80.391 134.62 270)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
    (fp_text reference X15 (at 2.54 -3.2 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 2.54 11.2 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.3 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 22 +BATT))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 122 IN_K8))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal (layer F.Cu) (tedit 5B785047)
    (at 80.391 106.68 270)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/2-G-5,08; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
    (fp_text reference X17 (at 2.54 -3.2 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 2.54 11.2 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.3 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 121 IN_K6))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 22 +BATT))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_2-G-5,08_1x02_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 201.676 90.424 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference X18 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 RX))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 TX))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal (layer F.Cu) (tedit 5B785047)
    (at 219.202 93.345 90)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/3-G-5,08; number of pins: 03; pin pitch: 5.08mm; Angled || order number: 1757255 12A || order number: 1923872 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x03_G_5.08mm")
    (fp_text reference X19 (at 5.08 -3.2 90) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 5.08 11.2 90) (layer F.Fab))
    (fp_text user %R (at 5.08 -1.3 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 4 +5V))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 110 OI_1))
    (pad 3 thru_hole oval (at 10.16 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 111 OI_2))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MSTB:PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal (layer F.Cu) (tedit 5B785047)
    (at 219.202 112.649 90)
    (descr "Generic Phoenix Contact connector footprint for: MSTBA_2,5/3-G-5,08; number of pins: 03; pin pitch: 5.08mm; Angled || order number: 1757255 12A || order number: 1923872 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x03_G_5.08mm")
    (fp_text reference X20 (at 5.08 -3.2 90) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 5.08 11.2 90) (layer F.Fab))
    (fp_text user %R (at 5.08 -1.3 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 10.16 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 114 Analog_OI_1))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 113 OI_4))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 112 OI_3))
    (model ${KISYS3DMOD}/Connector_Phoenix_MSTB.3dshapes/PhoenixContact_MSTBA_2,5_3-G-5,08_1x03_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 84.201 116.459 90)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D8 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 25 "Net-(D8-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 24 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 191.516 113.284)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D9 (at 0 -1.82) (layer F.SilkS))
    (fp_text value LED (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 27 "Net-(D9-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 26 "Net-(D9-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 173.736 113.284)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D10 (at 0 -1.82) (layer F.SilkS))
    (fp_text value LED (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 28 "Net-(D10-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 29 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 154.686 113.284)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D11 (at 0 -1.82) (layer F.SilkS))
    (fp_text value LED (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 30 "Net-(D11-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 31 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 136.271 113.284)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D12 (at 0 -1.82) (layer F.SilkS))
    (fp_text value LED (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 32 "Net-(D12-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 33 "Net-(D12-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 117.856 113.284)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D13 (at 0 -1.82) (layer F.SilkS))
    (fp_text value LED (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 35 "Net-(D13-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 34 "Net-(D13-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 110.236 99.949 90)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D14 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 37 "Net-(D14-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 36 "Net-(D14-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 84.201 132.969 90)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D15 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 38 "Net-(D15-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 39 "Net-(D15-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RELAY_1-1721150-3 (layer F.Cu) (tedit 0)
    (at 176.911 124.714 270)
    (fp_text reference K2 (at -7.26069 -8.83584 90) (layer F.SilkS))
    (fp_text value 1-1721150-3 (at -6.62706 8.6677 90) (layer F.SilkS))
    (pad A1 thru_hole rect (at -6.1 -6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad COM thru_hole circle (at -8.1 0 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 43 "Net-(K2-PadCOM)"))
    (pad A2 thru_hole circle (at -6.1 6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 28 "Net-(D10-Pad1)"))
    (pad NO thru_hole circle (at 6.1 6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 44 "Net-(K2-PadNO)"))
    (pad NC thru_hole circle (at 6.1 -6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 45 "Net-(K2-PadNC)"))
  )
  (module RELAY_1-1721150-3 (layer F.Cu) (tedit 0)
    (at 139.5095 124.714 270)
    (fp_text reference K4 (at -7.26069 -8.83584 90) (layer F.SilkS))
    (fp_text value 1-1721150-3 (at -6.62706 8.6677 90) (layer F.SilkS))
    (pad A1 thru_hole rect (at -6.1 -6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad COM thru_hole circle (at -8.1 0 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 51 "Net-(K4-PadCOM)"))
    (pad A2 thru_hole circle (at -6.1 6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 33 "Net-(D12-Pad1)"))
    (pad NO thru_hole circle (at 6.1 6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 50 "Net-(K4-PadNO)"))
    (pad NC thru_hole circle (at 6.1 -6 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 49 "Net-(K4-PadNC)"))
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 84.201 110.744 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 510R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(D8-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 197.231 113.284 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 510R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(D9-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 179.451 113.284 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 510R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +12V))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 160.401 113.284 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 510R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(D11-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 141.986 113.284 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 510R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +12V))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(D12-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 123.9035 113.284 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 510R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +12V))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(D13-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 110.236 94.234 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 510R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +12V))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(D14-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 84.201 127.254 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 510R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(D15-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprintsSTP:STP16NF06 (layer F.Cu) (tedit 0)
    (at 86.741 96.139 270)
    (fp_text reference T2 (at -2.55 0.762 90) (layer F.SilkS))
    (fp_text value STP16NF06 (at -2.55 0.762 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -5.1 1.524 270) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 58 "Net-(R2-Pad2)"))
    (pad 2 thru_hole circle (at -2.55 1.524 270) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 132 "Net-(T2-Pad2)"))
    (pad 3 thru_hole circle (at 0 1.524 270) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module footprintsSTP:STP16NF06 (layer F.Cu) (tedit 0)
    (at 115.316 97.409 270)
    (fp_text reference T3 (at -2.55 0.762 90) (layer F.SilkS))
    (fp_text value STP16NF06 (at -2.55 0.762 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -5.1 1.524 270) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 60 "Net-(R6-Pad2)"))
    (pad 2 thru_hole circle (at -2.55 1.524 270) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 92 NO_K6))
    (pad 3 thru_hole circle (at 0 1.524 270) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module footprintsSTP:STP16NF06 (layer F.Cu) (tedit 0)
    (at 107.696 109.474 90)
    (fp_text reference T4 (at -2.55 0.762 90) (layer F.SilkS))
    (fp_text value STP16NF06 (at -2.55 0.762 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 3 thru_hole circle (at 0 1.524 90) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.55 1.524 90) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 117 NO_K7))
    (pad 1 thru_hole rect (at -5.1 1.524 90) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 65 "Net-(R13-Pad2)"))
  )
  (module footprintsSTP:STP16NF06 (layer F.Cu) (tedit 0)
    (at 107.696 132.334 90)
    (fp_text reference T5 (at -2.55 0.762 90) (layer F.SilkS))
    (fp_text value STP16NF06 (at -2.55 0.762 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 3 thru_hole circle (at 0 1.524 90) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.55 1.524 90) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 120 NO_K8))
    (pad 1 thru_hole rect (at -5.1 1.524 90) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 68 "Net-(R15-Pad2)"))
  )
  (module Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm (layer B.Cu) (tedit 5C97300E)
    (at 206.756 110.109 270)
    (descr "SOIC, 18 Pin (JEDEC MS-013AB, https://www.analog.com/media/en/package-pcb-resources/package/33254132129439rw_18.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U15 (at 0 6.72 270) (layer B.SilkS))
    (fp_text value ULN2803A (at 0 -6.72 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 18 smd roundrect (at 4.65 5.08 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D9-Pad1)"))
    (pad 17 smd roundrect (at 4.65 3.81 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(D10-Pad1)"))
    (pad 16 smd roundrect (at 4.65 2.54 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(D11-Pad1)"))
    (pad 15 smd roundrect (at 4.65 1.27 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(D12-Pad1)"))
    (pad 14 smd roundrect (at 4.65 0 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(D13-Pad1)"))
    (pad 13 smd roundrect (at 4.65 -1.27 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(D14-Pad1)"))
    (pad 12 smd roundrect (at 4.65 -2.54 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D8-Pad1)"))
    (pad 11 smd roundrect (at 4.65 -3.81 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(D15-Pad1)"))
    (pad 10 smd roundrect (at 4.65 -5.08 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +12V))
    (pad 9 smd roundrect (at -4.65 -5.08 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 8 smd roundrect (at -4.65 -3.81 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 130 "Net-(U15-Pad8)"))
    (pad 7 smd roundrect (at -4.65 -2.54 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 129 "Net-(U15-Pad7)"))
    (pad 6 smd roundrect (at -4.65 -1.27 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 128 "Net-(U15-Pad6)"))
    (pad 5 smd roundrect (at -4.65 0 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 127 "Net-(U15-Pad5)"))
    (pad 4 smd roundrect (at -4.65 1.27 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 126 "Net-(U15-Pad4)"))
    (pad 3 smd roundrect (at -4.65 2.54 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 125 "Net-(U15-Pad3)"))
    (pad 2 smd roundrect (at -4.65 3.81 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 124 "Net-(U15-Pad2)"))
    (pad 1 smd roundrect (at -4.65 5.08 270) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 123 "Net-(U15-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-18W_7.5x11.6mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprintsSTP:STP16NF06 (layer F.Cu) (tedit 0)
    (at 107.696 120.904 90)
    (fp_text reference T7 (at -2.55 0.762 90) (layer F.SilkS))
    (fp_text value STP16NF06 (at -2.55 0.762 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -5.1 1.524 90) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 71 "Net-(R26-Pad2)"))
    (pad 2 thru_hole circle (at -2.55 1.524 90) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 119 NC_K8))
    (pad 3 thru_hole circle (at 0 1.524 90) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module footprintsSTP:STP16NF06 (layer F.Cu) (tedit 0)
    (at 116.586 103.759 90)
    (fp_text reference T9 (at -2.55 0.762 90) (layer F.SilkS))
    (fp_text value STP16NF06 (at -2.55 0.762 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 3 thru_hole circle (at 0 1.524 90) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.55 1.524 90) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 116 NC_K7))
    (pad 1 thru_hole rect (at -5.1 1.524 90) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 74 "Net-(R33-Pad2)"))
  )
  (module footprintsSTP:STP16NF06 (layer F.Cu) (tedit 0)
    (at 101.981 85.979 180)
    (fp_text reference T11 (at -2.55 0.762) (layer F.SilkS))
    (fp_text value STP16NF06 (at -2.55 0.762) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at -5.1 1.524 180) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 78 "Net-(R42-Pad2)"))
    (pad 2 thru_hole circle (at -2.55 1.524 180) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 91 NC_K6))
    (pad 3 thru_hole circle (at 0 1.524 180) (size 2.032 2.032) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module footprintsMCP:MCP4451-103E&slash_ST (layer F.Cu) (tedit 0)
    (at 171.831 61.849)
    (fp_text reference U19 (at 0 0) (layer F.SilkS))
    (fp_text value MCP4451-103E_ST (at 0 0) (layer F.SilkS))
    (fp_text user * (at -1.8669 -3.2258) (layer F.SilkS))
    (fp_text user * (at -1.8669 -3.2258) (layer F.Fab))
    (fp_text user 0.058in/1.473mm (at -2.8194 5.715) (layer Dwgs.User))
    (fp_text user 0.222in/5.639mm (at 0 -5.715) (layer Dwgs.User))
    (fp_text user 0.014in/0.356mm (at 5.8674 -2.925001) (layer Dwgs.User))
    (fp_text user 0.026in/0.65mm (at -5.8674 -2.600001) (layer Dwgs.User))
    (fp_text user * (at -1.8669 -3.2258) (layer F.Fab))
    (fp_text user * (at -1.8669 -3.2258) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 20 smd rect (at 2.8194 -2.924998) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 84 P2A))
    (pad 19 smd rect (at 2.8194 -2.274999) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 103 P2W))
    (pad 18 smd rect (at 2.8194 -1.624998) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 83 P0B))
    (pad 17 smd rect (at 2.8194 -0.974999) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 16 smd rect (at 2.8194 -0.324998) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at 2.8194 0.325001) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 2.8194 0.975002) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 2.8194 1.625001) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 83 P0B))
    (pad 12 smd rect (at 2.8194 2.275002) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 104 P0W))
    (pad 11 smd rect (at 2.8194 2.925) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 87 P0A))
    (pad 10 smd rect (at -2.8194 2.924998) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 101 P1A))
    (pad 9 smd rect (at -2.8194 2.274999) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 102 P1W))
    (pad 8 smd rect (at -2.8194 1.624998) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 83 P0B))
    (pad 7 smd rect (at -2.8194 0.974999) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.8194 0.324998) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 97 SDA))
    (pad 5 smd rect (at -2.8194 -0.325001) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 98 SCL))
    (pad 4 smd rect (at -2.8194 -0.974999) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.8194 -1.625001) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 86 P3B))
    (pad 2 smd rect (at -2.8194 -2.274999) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 115 P3W))
    (pad 1 smd rect (at -2.8194 -2.925) (size 1.4732 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 83 P0B))
  )
  (gr_line (start 70.231 48.514) (end 70.231 148.514) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 230.231 48.514) (end 70.231 48.514) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 230.231 48.514) (end 230.231 148.514) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70.231 148.514) (end 230.231 148.514) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.231 48.184) (xy 230.251 48.184) (xy 230.251 149.149) (xy 70.231 148.514)
      )
    )
  )
  (zone (net 22) (net_name +BATT) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.506 148.514) (xy 70.231 148.514) (xy 70.231 48.184) (xy 129.921 48.184) (xy 129.921 87.554)
        (xy 111.506 87.554)
      )
    )
  )
  (zone (net 3) (net_name +12V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.506 148.514) (xy 230.251 148.514) (xy 230.251 107.874) (xy 111.506 107.874)
      )
    )
  )
  (zone (net 4) (net_name +5V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.506 87.554) (xy 111.506 107.874) (xy 230.251 107.874) (xy 230.251 76.124) (xy 129.921 76.124)
        (xy 129.921 87.554)
      )
    )
  )
  (zone (net 8) (net_name +8V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 230.251 76.124) (xy 230.251 48.184) (xy 129.921 48.184) (xy 129.921 76.124)
      )
    )
  )
)
