(kicad_pcb (version 20171130) (host pcbnew 5.0.2)
  (general
    (thickness 1.6)
    (drawings 10139)
    (tracks 274)
    (zones 0)
    (modules 36)
    (nets 28)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.05)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 1)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad4)")
  (net 2 "Net-(D1-Pad3)")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(D2-Pad4)")
  (net 7 "Net-(D3-Pad3)")
  (net 8 "Net-(D3-Pad1)")
  (net 9 "Net-(D4-Pad2)")
  (net 10 "Net-(D4-Pad4)")
  (net 11 "Net-(D6-Pad4)")
  (net 12 "Net-(D6-Pad2)")
  (net 13 "Net-(D7-Pad4)")
  (net 14 "Net-(D7-Pad3)")
  (net 15 "Net-(D7-Pad2)")
  (net 16 "Net-(D7-Pad1)")
  (net 17 "Net-(D10-Pad1)")
  (net 18 "Net-(D10-Pad3)")
  (net 19 "Net-(D11-Pad2)")
  (net 20 "Net-(D11-Pad4)")
  (net 21 "Net-(D10-Pad4)")
  (net 22 "Net-(D10-Pad2)")
  (net 23 "Net-(D12-Pad2)")
  (net 24 "Net-(D12-Pad4)")
  (net 25 GND)
  (net 26 "Net-(J1-Pad2)")
  (net 27 "Net-(J1-Pad3)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D10-Pad3)")
    (add_net "Net-(D10-Pad4)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D11-Pad4)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D12-Pad4)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D2-Pad4)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad3)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D4-Pad4)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D6-Pad4)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D7-Pad3)")
    (add_net "Net-(D7-Pad4)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 107.696 71.12)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference . (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 46.228 71.12)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference H5 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 107.696 92.456)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference . (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 46.228 92.456)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference H5 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 5EAAD969)
    (at 106.68 59.944)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (attr virtual)
    (fp_text reference - (at 0 2.032) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_DIN965 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 5EAAD957)
    (at 110.236 66.548)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (attr virtual)
    (fp_text reference - (at 0 2.032) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_DIN965 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 5EAAD948)
    (at 114.3 92.964)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (attr virtual)
    (fp_text reference - (at 0 2.032) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_DIN965 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 5EAAD940)
    (at 117.348 100.584)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (attr virtual)
    (fp_text reference - (at 0 2.032) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_DIN965 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 5EAAD920)
    (at 42.672 59.436)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (attr virtual)
    (fp_text reference - (at 0 2.032) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_DIN965 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 5EAAD927)
    (at 46.228 67.056)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (attr virtual)
    (fp_text reference - (at 0 2.032) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_DIN965 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 5EAAD931)
    (at 36.068 92.964)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (attr virtual)
    (fp_text reference - (at 0 2.032) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_DIN965 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 5EAAD938)
    (at 39.624 100.584)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (attr virtual)
    (fp_text reference - (at 0 2.032) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_DIN965 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 29.464 91.44)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 120.904 103.124)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference . (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 119.38 67.056)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference . (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 39.092 73.152 180)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference D1 (at 1.5 -2.65) (layer F.SilkS))
    (fp_text value LED_Dual_CACA (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at 1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at 1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 44.172 63.258 180)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference D2 (at 0.992 -2.65) (layer F.SilkS))
    (fp_text value LED_Dual_CACA (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 2 smd rect (at 1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 3 smd rect (at 1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 4 smd rect (at -1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad4)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 37.06 84.062 180)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference D3 (at 1.5 -2.65) (layer F.SilkS))
    (fp_text value LED_Dual_CACA (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad3)"))
    (pad 3 smd rect (at 1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad3)"))
    (pad 2 smd rect (at 1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 53.34 53.34 180)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference D4 (at 1.016 -2.54) (layer F.SilkS))
    (fp_text value LED_Dual_CACA (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (pad 3 smd rect (at 1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad4)"))
    (pad 4 smd rect (at -1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D4-Pad4)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 38.076 96.762 180)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference D5 (at 1.5 -2.65) (layer F.SilkS))
    (fp_text value LED_Dual_CACA (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 2 smd rect (at 1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad1)"))
    (pad 3 smd rect (at 1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 4 smd rect (at -1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad3)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 66.548 49.784 180)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference D6 (at 1.524 -2.65) (layer F.SilkS))
    (fp_text value LED_Dual_CACA (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D6-Pad4)"))
    (pad 3 smd rect (at 1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D4-Pad4)"))
    (pad 2 smd rect (at 1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 89.94 49.784 180)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference D7 (at 1.04 -2.65) (layer F.SilkS))
    (fp_text value LED_Dual_CACA (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D7-Pad4)"))
    (pad 3 smd rect (at 1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D7-Pad3)"))
    (pad 2 smd rect (at 1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D7-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 115.824 97.028 180)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference D8 (at 1.524 -2.65) (layer F.SilkS))
    (fp_text value LED_Dual_CACA (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 2 smd rect (at 1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D10-Pad1)"))
    (pad 3 smd rect (at 1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 4 smd rect (at -1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D10-Pad3)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 101.068 54.864 180)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference D9 (at 0.484 -2.65) (layer F.SilkS))
    (fp_text value LED_Dual_CACA (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D11-Pad2)"))
    (pad 2 smd rect (at 1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D7-Pad3)"))
    (pad 3 smd rect (at 1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D11-Pad4)"))
    (pad 4 smd rect (at -1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D7-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 117.88 84.57 180)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference D10 (at 2.056 -2.65) (layer F.SilkS))
    (fp_text value LED_Dual_CACA (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D10-Pad4)"))
    (pad 3 smd rect (at 1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D10-Pad3)"))
    (pad 2 smd rect (at 1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at -1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D10-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 108.712 62.992 180)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference D11 (at 1.524 -2.54) (layer F.SilkS))
    (fp_text value LED_Dual_CACA (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D11-Pad4)"))
    (pad 3 smd rect (at 1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 2 smd rect (at 1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 115.316 71.12 180)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference D12 (at 2.032 -2.65) (layer F.SilkS))
    (fp_text value LED_Dual_CACA (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D10-Pad2)"))
    (pad 2 smd rect (at 1.5 -0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D12-Pad2)"))
    (pad 3 smd rect (at 1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D10-Pad4)"))
    (pad 4 smd rect (at -1.5 0.75 180) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D12-Pad4)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_EH_S3B-EH_1x03_P2.50mm_Horizontal (layer B.Cu) (tedit 5C281425)
    (at 80.772 51.308 180)
    (descr "JST EH series connector, S3B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH horizontal")
    (fp_text reference J1 (at 2.5 7.9) (layer B.SilkS))
    (fp_text value Conn_01x03_Male (at 2.5 -2.7) (layer B.Fab))
    (fp_text user %R (at 2.5 2.6) (layer B.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 25 GND))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_S3B-EH_1x03_P2.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 75.184 58.42 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(J1-Pad3)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 75.184 61.468 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.43) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(D1-Pad4)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 69.596 58.42 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.43) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(D6-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 69.596 61.468 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.43) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(J1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D6-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 80.772 58.42 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.43) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(J1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(D7-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 86.36 58.42 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.43) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(J1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(D12-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 80.772 61.468 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.43) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(J1-Pad3)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 86.36 61.468 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.43) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D12-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 21.336 (width 0.12) (layer F.SilkS)
    (gr_text "21,336 mm" (at 143.002 81.788 270) (layer F.SilkS))
    (feature1 (pts (xy 107.696 92.456) (xy 142.318421 92.456)))
    (feature2 (pts (xy 107.696 71.12) (xy 142.318421 71.12)))
    (crossbar (pts (xy 141.732 71.12) (xy 141.732 92.456)))
    (arrow1a (pts (xy 141.732 92.456) (xy 141.145579 91.329496)))
    (arrow1b (pts (xy 141.732 92.456) (xy 142.318421 91.329496)))
    (arrow2a (pts (xy 141.732 71.12) (xy 141.145579 72.246504)))
    (arrow2b (pts (xy 141.732 71.12) (xy 142.318421 72.246504)))
  )
  (dimension 61.468 (width 0.12) (layer F.SilkS)
    (gr_text "61,468 mm" (at 76.962 26.162) (layer F.SilkS))
    (feature1 (pts (xy 107.696 71.12) (xy 107.696 26.845579)))
    (feature2 (pts (xy 46.228 71.12) (xy 46.228 26.845579)))
    (crossbar (pts (xy 46.228 27.432) (xy 107.696 27.432)))
    (arrow1a (pts (xy 107.696 27.432) (xy 106.569496 28.018421)))
    (arrow1b (pts (xy 107.696 27.432) (xy 106.569496 26.845579)))
    (arrow2a (pts (xy 46.228 27.432) (xy 47.354504 28.018421)))
    (arrow2b (pts (xy 46.228 27.432) (xy 47.354504 26.845579)))
  )
  (gr_text . (at 56.388 53.34) (layer F.Cu))
  (gr_text . (at 47.244 63.5) (layer F.Cu))
  (gr_text . (at 42.164 73.152) (layer F.Cu))
  (gr_text . (at 40.132 83.82) (layer F.Cu))
  (gr_text . (at 41.148 97.028) (layer F.Cu))
  (gr_text . (at 118.872 97.028) (layer F.Cu))
  (gr_text . (at 120.904 84.328) (layer F.Cu))
  (gr_text . (at 118.364 71.12) (layer F.Cu))
  (gr_text . (at 111.76 62.992) (layer F.Cu))
  (gr_text . (at 104.14 54.864) (layer F.Cu))
  (gr_text . (at 92.964 49.784) (layer F.Cu))
  (gr_text . (at 69.596 49.784) (layer F.Cu))
  (gr_line (start 34.036 97.028) (end 23.714392 95.895327) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 75.692 90.424) (end 53.340002 43.180002) (angle -70.68931957) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 49.738522 63.258543) (end 50.8 65.024) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 57.912 64.516) (end 59.435999 56.388001) (angle -91.87349301) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 112.775999 86.867999) (end 111.76 87.376) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109.267318 73.655834) (end 108.712 73.66) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 107.188 81.28) (end 112.775999 86.867999) (angle -119.7448813) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 121.48709 64.44091) (end 113.791999 63.500001) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.428 68.072) (end 118.584666 72.904485) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.329745 100.628945) (end 119.379999 99.567999) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.364 106.172) (end 118.364001 106.172001) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.936 105.156) (end 118.364 106.172) (layer Edge.Cuts) (width 0.05))
  (gr_text "Corrado 16VG60" (at 51.816 87.376) (layer F.Cu))
  (gr_text "Design By Ronny Pech" (at 88.9 76.708 16) (layer F.Cu))
  (gr_line (start 111.76 87.376) (end 87.884 94.996) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 108.712 73.66) (end 75.184 83.522419) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 50.8 65.024) (end 67.056 94.996) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 59.436 56.388) (end 74.676001 83.311999) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 44.196 94.996) (end 67.056 94.996) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 44.396054 116.176901) (end 44.196 94.996) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 75.692 86.868) (end 34.036 97.028) (angle -29.41516057) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 60.96 40.21916) (end 53.34 43.18) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 60.96 41.656) (end 61.975999 40.640001) (angle -45) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.040001 44.195999) (end 61.976 40.64) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.548 44.406419) (end 67.529329 44.236247) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 66.548 43.688) (end 66.040001 44.195999) (angle -45) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 76.708 87.376) (end 113.791999 63.500001) (angle -69.23660106) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 118.872 67.056) (end 122.428 68.072) (angle -60.9453959) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 80.772 87.376) (end 119.379999 99.567999) (angle -38.46821892) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 120.904 103.124) (end 122.936 105.156) (angle -105.2551311) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 116.590446 107.625968) (end 116.523376 107.77574) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 119.38 109.22) (end 118.364001 106.172001) (angle -41.82016988) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 98.044 100.076) (end 109.727999 116.331999) (angle -31.67344365) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109.728 94.996) (end 109.728 116.332) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 87.884 94.996) (end 109.728 94.996) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 75.184 82.804) (end 74.676001 83.311999) (angle -45) (layer Edge.Cuts) (width 0.05))
)
