(kicad_pcb (version 20171130) (host pcbnew 5.1.5)
  (general
    (thickness 1.6)
    (drawings 45)
    (tracks 162)
    (zones 0)
    (modules 15)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad4)")
  (net 2 GND)
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D2-Pad2)")
  (net 5 "Net-(D2-Pad4)")
  (net 6 "Net-(D3-Pad4)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 "Net-(D4-Pad2)")
  (net 9 "Net-(D4-Pad4)")
  (net 10 "Net-(D5-Pad2)")
  (net 11 "Net-(D5-Pad4)")
  (net 12 "Net-(D6-Pad4)")
  (net 13 "Net-(D6-Pad2)")
  (net 14 "Net-(J1-Pad3)")
  (net 15 "Net-(J1-Pad2)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D2-Pad4)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D3-Pad4)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D4-Pad4)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D5-Pad4)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D6-Pad4)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
  )
  (module Connector_JST:JST_EH_S3B-EH_1x03_P2.50mm_Horizontal (layer B.Cu) (tedit 5EAC140F)
    (at 131.572 75.732 270)
    (descr "JST EH series connector, S3B-EH (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH horizontal")
    (fp_text reference " " (at 2.5 7.9 90) (layer B.SilkS))
    (fp_text value " " (at 2.5 -2.7 90) (layer B.Fab))
    (fp_text user %R (at 2.5 2.6 90) (layer B.Fab))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_S3B-EH_1x03_P2.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5EAAFEE6)
    (at 96.52 85.852)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference " " (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value " " (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5EAAFEE6)
    (at 146.304 85.852)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference " " (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value " " (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5EAAFEE6)
    (at 146.304 71.12)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference " " (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value " " (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5EAAFEE6)
    (at 96.52 71.12)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference " " (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value " " (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 107.696 83.82)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference " " (at 0 -2.65) (layer F.SilkS))
    (fp_text value " " (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -1.5 0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at 1.5 0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 -0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.5 -0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 107.672 74.41)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference " " (at 0 -2.65) (layer F.SilkS))
    (fp_text value " " (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 -0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 3 smd rect (at 1.5 0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -1.5 0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad4)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5EAD94B7)
    (at 122.428 83.82)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference " " (at 0 -2.65) (layer F.SilkS))
    (fp_text value " " (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -1.5 0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad4)"))
    (pad 3 smd rect (at 1.5 0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad4)"))
    (pad 2 smd rect (at 1.5 -0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.5 -0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5EAD9523)
    (at 122.428 74.168)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference " " (at 0 -2.65) (layer F.SilkS))
    (fp_text value " " (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 1.5 -0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (pad 3 smd rect (at 1.5 0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad4)"))
    (pad 4 smd rect (at -1.5 0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad4)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 136.652 83.82)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference " " (at 0 -2.65) (layer F.SilkS))
    (fp_text value " " (at 0 3.048) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 1.5 -0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D5-Pad2)"))
    (pad 3 smd rect (at 1.5 0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad4)"))
    (pad 4 smd rect (at -1.5 0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D5-Pad4)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW (layer F.Cu) (tedit 5A643BA3)
    (at 136.652 74.168)
    (descr https://docs.broadcom.com/docs/AV02-4186EN)
    (tags "LED Avago PLCC-4 ASMB-MTB0-0A3A2")
    (attr smd)
    (fp_text reference " " (at 0 -2.65) (layer F.SilkS))
    (fp_text value " " (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -1.5 0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D6-Pad4)"))
    (pad 3 smd rect (at 1.5 0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad4)"))
    (pad 2 smd rect (at 1.5 -0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -1.5 -0.75) (size 1.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Avago_PLCC4_3.2x2.8mm_CW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 102.108 73.152)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference " " (at 0 -1.43) (layer F.SilkS))
    (fp_text value " " (at 0 1.524) (layer F.Fab))
    (fp_text user %R (at -0.508 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D5-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 102.108 77.216)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference " " (at 0 -1.43) (layer F.SilkS))
    (fp_text value " " (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(J1-Pad3)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 102.108 81.788)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference " " (at 0 -1.43) (layer F.SilkS))
    (fp_text value " " (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D5-Pad4)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 102.108 86.36)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference " " (at 0 -1.43) (layer F.SilkS))
    (fp_text value " " (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(J1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(D6-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "by Rpnny Pech" (at 146.304 78.232 90) (layer F.SilkS))
  (gr_text "V1.0 Diaplaybeleuchtung" (at 129.54 70.104) (layer F.SilkS))
  (gr_text "Corrado 16VG60" (at 112.268 70.104) (layer F.SilkS))
  (gr_text NIGHT (at 101.092 83.82 90) (layer F.SilkS))
  (gr_text DAY (at 101.6 75.184 90) (layer F.SilkS))
  (gr_text GND (at 138.684 86.36) (layer F.SilkS))
  (gr_text GND (at 138.684 76.708) (layer F.SilkS))
  (gr_text GND (at 124.46 76.708) (layer F.SilkS))
  (gr_text GND (at 124.46 86.36) (layer F.SilkS))
  (gr_text GND (at 135.636 81.28) (layer F.SilkS))
  (gr_text GND (at 135.636 71.628) (layer F.SilkS))
  (gr_text GND (at 121.412 81.28) (layer F.SilkS))
  (gr_text GND (at 121.412 71.628) (layer F.SilkS))
  (gr_text 4 (at 120.904 86.36) (layer F.SilkS))
  (gr_text 4 (at 135.128 86.36) (layer F.SilkS))
  (gr_text 4 (at 135.128 76.708) (layer F.SilkS))
  (gr_text 4 (at 120.904 76.708) (layer F.SilkS))
  (gr_text 4 (at 105.156 86.36) (layer F.SilkS))
  (gr_text 4 (at 106.172 76.708) (layer F.SilkS))
  (gr_text 3 (at 137.668 86.36) (layer F.SilkS))
  (gr_text 3 (at 123.444 86.36) (layer F.SilkS))
  (gr_text 3 (at 137.668 76.708) (layer F.SilkS))
  (gr_text 3 (at 123.444 76.708) (layer F.SilkS))
  (gr_text 3 (at 108.204 86.36) (layer F.SilkS))
  (gr_text 3 (at 108.204 76.708) (layer F.SilkS))
  (gr_text 2 (at 123.952 81.28) (layer F.SilkS))
  (gr_text 2 (at 138.176 81.28) (layer F.SilkS))
  (gr_text 2 (at 138.176 71.628) (layer F.SilkS))
  (gr_text 2 (at 123.952 71.628) (layer F.SilkS))
  (gr_text 2 (at 110.744 81.788) (layer F.SilkS))
  (gr_text 2 (at 109.728 72.136) (layer F.SilkS))
  (gr_text 1 (at 104.648 72.136) (layer F.SilkS))
  (gr_text 1 (at 104.648 81.28) (layer F.SilkS))
  (gr_text 1 (at 134.62 71.628) (layer F.SilkS))
  (gr_text 1 (at 134.62 81.28) (layer F.SilkS))
  (gr_text 1 (at 120.396 81.28) (layer F.SilkS))
  (gr_text 1 (at 120.396 71.628) (layer F.SilkS))
  (gr_text GND (at 105.664 72.136) (layer F.SilkS))
  (gr_text GND (at 105.664 81.28) (layer F.SilkS))
  (gr_text GND (at 109.22 86.36) (layer F.SilkS))
  (gr_text GND (at 109.22 76.708) (layer F.SilkS))
  (gr_line (start 93.98 68.58) (end 93.98 88.392) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148.844 88.392) (end 93.98 88.392) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148.844 68.58) (end 148.844 88.392) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 93.98 68.58) (end 148.844 68.58) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.86 89.408) (xy 92.964 89.408) (xy 92.964 67.564) (xy 149.86 67.564)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.86 89.408) (xy 92.964 89.408) (xy 92.964 67.564) (xy 149.86 67.564)
      )
    )
  )
)
