(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 66)
    (zones 0)
    (modules 44)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (33 F.Adhes user hide)
    (35 F.Paste user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.1)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.1)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.25 1.75)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FF9FF7F)
    (pcbplotparams
      (layerselection 0x010e8_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "c:/"))
  )
  (net 0 "")
  (net 1 "Net-(R1-Pad1)")
  (net 2 "Net-(R2-Pad1)")
  (net 3 "Net-(R3-Pad1)")
  (net 4 "Net-(R4-Pad1)")
  (net 5 "Net-(R5-Pad1)")
  (net 6 "Net-(R6-Pad1)")
  (net 7 "Net-(R7-Pad1)")
  (net 8 "Net-(R8-Pad1)")
  (net 9 "Net-(R10-Pad2)")
  (net 10 "Net-(R10-Pad1)")
  (net 11 "Net-(R11-Pad1)")
  (net 12 "Net-(R12-Pad1)")
  (net 13 "Net-(R13-Pad1)")
  (net 14 "Net-(R14-Pad1)")
  (net 15 "Net-(R15-Pad1)")
  (net 16 "Net-(R16-Pad1)")
  (net 17 "Net-(R17-Pad1)")
  (net 18 "Net-(R18-Pad1)")
  (net 19 /OUT)
  (net 20 /COM1)
  (net 21 /IN)
  (net 22 "Net-(H3-Pad1)")
  (net 23 "Net-(R19-Pad1)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /COM1)
    (add_net /IN)
    (add_net /OUT)
    (add_net "Net-(H3-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5EC113EE)
    (at 62.0125 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175)
      (net 21 /IN))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 63.875 113.65 15)
    (fp_text reference SW3 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(R3-Pad1)"))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(R3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(R3-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EBD8E3A)
    (at 43.875 113.65 15)
    (fp_text reference SW1 (at 0.118293 3.422226 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 7.62 2.37 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(R1-Pad1)"))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(R1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(R1-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 53.875 113.65 15)
    (fp_text reference SW2 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(R2-Pad1)"))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(R2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(R2-Pad1)"))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 69.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 "Net-(R1-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 79.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(R2-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 89.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 "Net-(R3-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 99.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 "Net-(R5-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 109.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 "Net-(R5-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 "Net-(R7-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 129.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 "Net-(R7-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 139.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 9 "Net-(R10-Pad2)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 149.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 10 "Net-(R10-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 9 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 159.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 11 "Net-(R11-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 10 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 169.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 11 "Net-(R11-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 179.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 13 "Net-(R13-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 189.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 13 "Net-(R13-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 "Net-(R14-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 199.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 14 "Net-(R14-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 15 "Net-(R15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 209.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 16 "Net-(R16-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 15 "Net-(R15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 219.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0.25 -1.55) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 16 "Net-(R16-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 17 "Net-(R17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 229.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 18 "Net-(R18-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 17 "Net-(R17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 239.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 23 "Net-(R19-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 18 "Net-(R18-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5EC15F70)
    (at 249.65 106.225 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 23 "Net-(R19-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 19 /OUT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 103.875 113.65 15)
    (fp_text reference SW7 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(R7-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(R7-Pad1)"))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(R7-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 153.875 113.65 15)
    (fp_text reference SW12 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R12-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R12-Pad1)"))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R12-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 163.875 113.65 15)
    (fp_text reference SW13 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(R13-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(R13-Pad1)"))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(R13-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 173.875 113.65 15)
    (fp_text reference SW14 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R14-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R14-Pad1)"))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R14-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 183.875 113.65 15)
    (fp_text reference SW15 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R15-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R15-Pad1)"))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R15-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 193.875 113.65 15)
    (fp_text reference SW16 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R16-Pad1)"))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R16-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R16-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 203.875 113.65 15)
    (fp_text reference SW17 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(R17-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(R17-Pad1)"))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(R17-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 233.875 113.65 15)
    (fp_text reference SW20 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /OUT))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /OUT))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /OUT))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EBD5C79)
    (at 73.875 113.65 15)
    (fp_text reference SW4 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(R4-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(R4-Pad1)"))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(R4-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EBD5D38)
    (at 83.875 113.65 15)
    (fp_text reference SW5 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(R5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(R5-Pad1)"))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(R5-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 93.875 113.65 15)
    (fp_text reference SW6 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(R6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(R6-Pad1)"))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(R6-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 113.875 113.65 15)
    (fp_text reference SW8 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R8-Pad1)"))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R8-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 123.875 113.65 15)
    (fp_text reference SW9 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R10-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R10-Pad2)"))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R10-Pad2)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 133.875 113.65 15)
    (fp_text reference SW10 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R10-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R10-Pad1)"))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R10-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 143.875 113.65 15)
    (fp_text reference SW11 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R11-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R11-Pad1)"))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R11-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EBD8FED)
    (at 213.875 113.65 15)
    (fp_text reference SW18 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R18-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R18-Pad1)"))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R18-Pad1)"))
  )
  (module "_Chris:Hamlin MK6-8" (layer F.Cu) (tedit 5EB06EF6)
    (at 223.875 113.675 15)
    (fp_text reference SW19 (at 1.27 3.81 15) (layer F.SilkS))
    (fp_text value SW_Reed-cw (at 5.08 2.54 15) (layer F.Fab))
    (fp_text user %R (at 7.62 0 15) (layer F.Fab))
    (pad 4 thru_hole oval (at 20.32 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R19-Pad1)"))
    (pad 3 thru_hole oval (at 17.78 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R19-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /COM1))
    (pad 2 thru_hole oval (at 15.24 0 15) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R19-Pad1)"))
  )
  (module _Chris:Testpoint (layer F.Cu) (tedit 5EB151C1)
    (at 56.375 106.225)
    (fp_text reference H1 (at 0 -3.81) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 2.54) (layer F.Fab))
    (fp_text user REF** (at 0 -5.08) (layer F.SilkS))
    (fp_text user %R (at 0 -6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 21 /IN))
  )
  (module _Chris:Testpoint (layer F.Cu) (tedit 5EBECCFE)
    (at 254.45 106.15)
    (fp_text reference H2 (at 0 -3.81) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 2.54) (layer F.Fab))
    (fp_text user REF** (at 0 -5.08) (layer F.SilkS))
    (fp_text user %R (at 0 -6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /OUT))
  )
  (module _Chris:Testpoint (layer F.Cu) (tedit 5EBFAB66)
    (at 245.125 111.175 15)
    (fp_text reference H3 (at 0 -3.81 15) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 2.54 15) (layer F.Fab))
    (fp_text user REF** (at 0 -5.08 15) (layer F.SilkS))
    (fp_text user %R (at 0 -6.35 15) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 15) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(H3-Pad1)"))
  )
  (module _Chris:Testpoint (layer F.Cu) (tedit 5EBEF127)
    (at 52.4 111.325 15)
    (fp_text reference H4 (at 0 -3.81 15) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 2.54 15) (layer F.Fab))
    (fp_text user REF** (at 0 -5.08 15) (layer F.SilkS))
    (fp_text user %R (at 0 -6.35 15) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 15) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(H3-Pad1)"))
  )
  (gr_arc (start 54.4 108.8) (end 54.739684 109.710771) (angle -74.2) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 254.406151 108.814229) (end 254.745835 109.725) (angle -74.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 255.375 105) (end 255.375 108.735364) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 54.739684 109.710771) (end 35 115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 55.375 105) (end 55.368849 108.721135) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 235 115) (end 35 115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 254.75 109.725) (end 235 115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 55.375 105) (end 255.375 105) (layer Edge.Cuts) (width 0.05))
  (zone (net 19) (net_name /OUT) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 255.4 107.25) (xy 252.5 107.25) (xy 252.508375 105.225) (xy 255.408375 105.225)
      )
    )
  )
  (zone (net 22) (net_name "Net-(H3-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53.325 112.225) (xy 46.65 112.225) (xy 46.65 111.875) (xy 53.325 110.1)
      )
    )
  )
  (zone (net 20) (net_name /COM1) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 235.940413 114.75) (xy 232.75 114.75) (xy 232.725 112.5) (xy 244.025 112.525)
      )
    )
  )
  (zone (net 20) (net_name /COM1) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.9 112.35) (xy 44.9 114.75) (xy 35.926563 114.75)
      )
    )
  )
  (zone (net 20) (net_name /COM1) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.9 112.35) (xy 44.9 114.75) (xy 35.926563 114.75)
      )
    )
  )
  (zone (net 22) (net_name "Net-(H3-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 247.725 110.975) (xy 248.75 110.975) (xy 250.05 110.975) (xy 244.525 112.45) (xy 244.5 110.525)
        (xy 247.725 110.525)
      )
    )
  )
  (zone (net 21) (net_name /IN) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.875 107.5) (xy 55.37732 107.5) (xy 55.37732 105.244805) (xy 58.87732 105.244805)
      )
    )
  )
  (zone (net 22) (net_name "Net-(H3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53.325 112.225) (xy 46.65 112.225) (xy 46.65 111.875) (xy 53.325 110.1)
      )
    )
  )
  (zone (net 20) (net_name /COM1) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 235.940413 114.75) (xy 232.75 114.75) (xy 232.725 112.625) (xy 243.625 112.65)
      )
    )
  )
  (zone (net 22) (net_name "Net-(H3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 247.725 110.8) (xy 250.775 110.8) (xy 244.5 112.475) (xy 244.5 110.525) (xy 247.725 110.525)
      )
    )
  )
  (zone (net 19) (net_name /OUT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 255.4 107.25) (xy 252.5 107.25) (xy 252.508375 105.225) (xy 255.408375 105.225)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53.325 112.225) (xy 45.475 112.225) (xy 53.325 110.1)
      )
    )
  )
  (zone (net 21) (net_name /IN) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.875 107.5) (xy 55.37732 107.5) (xy 55.37732 105.244805) (xy 58.87732 105.244805)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.875 107.5) (xy 55.4 107.5) (xy 55.375 105.175) (xy 58.875 105.175)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 235.75 114.75) (xy 232.775 114.75) (xy 232.775 112.525) (xy 244.1 112.525)
      )
    )
  )
  (zone (net 22) (net_name "Net-(H3-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 247.725 110.9) (xy 250 110.9) (xy 244.5 112.4) (xy 244.5 110.525) (xy 247.725 110.525)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 247.725 110.8) (xy 250.7 110.8) (xy 244.5 112.475) (xy 244.525 110.5) (xy 247.725 110.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 255.375 107.25) (xy 252.5 107.25) (xy 252.5 105.225) (xy 255.375 105.225)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 247.725 110.9) (xy 250.375 110.9) (xy 244.45 112.475) (xy 244.45 110.5) (xy 247.725 110.5)
      )
    )
  )
)
