(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 1211)
    (zones 0)
    (modules 301)
    (nets 161)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 1.4)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.5)
    (aux_axis_origin 0 0)
    (visible_elements 7EF9F79F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../../Gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(D10-Pad2)")
  (net 4 "Net-(D10-Pad4)")
  (net 5 "Net-(D100-Pad2)")
  (net 6 "Net-(D100-Pad4)")
  (net 7 +3V3)
  (net 8 "Net-(D1-Pad2)")
  (net 9 "Net-(D2-Pad2)")
  (net 10 "Net-(D3-Pad2)")
  (net 11 "Net-(D4-Pad2)")
  (net 12 "Net-(D5-Pad2)")
  (net 13 "Net-(D6-Pad2)")
  (net 14 "Net-(D7-Pad2)")
  (net 15 "Net-(D8-Pad2)")
  (net 16 "Net-(D11-Pad2)")
  (net 17 "Net-(D12-Pad2)")
  (net 18 "Net-(D13-Pad2)")
  (net 19 "Net-(D14-Pad2)")
  (net 20 "Net-(D15-Pad2)")
  (net 21 "Net-(D16-Pad2)")
  (net 22 "Net-(D17-Pad2)")
  (net 23 "Net-(D18-Pad2)")
  (net 24 "Net-(D19-Pad2)")
  (net 25 "Net-(D20-Pad2)")
  (net 26 "Net-(D21-Pad2)")
  (net 27 "Net-(D22-Pad2)")
  (net 28 "Net-(D23-Pad2)")
  (net 29 "Net-(D24-Pad2)")
  (net 30 "Net-(D25-Pad2)")
  (net 31 "Net-(D26-Pad2)")
  (net 32 "Net-(D27-Pad2)")
  (net 33 "Net-(D28-Pad2)")
  (net 34 "Net-(D29-Pad2)")
  (net 35 "Net-(D30-Pad2)")
  (net 36 "Net-(D31-Pad2)")
  (net 37 "Net-(D32-Pad2)")
  (net 38 "Net-(D33-Pad2)")
  (net 39 "Net-(D34-Pad2)")
  (net 40 "Net-(D35-Pad2)")
  (net 41 "Net-(D36-Pad2)")
  (net 42 "Net-(D37-Pad2)")
  (net 43 "Net-(D38-Pad2)")
  (net 44 "Net-(D39-Pad2)")
  (net 45 "Net-(D40-Pad2)")
  (net 46 "Net-(D41-Pad2)")
  (net 47 "Net-(D42-Pad2)")
  (net 48 "Net-(D43-Pad2)")
  (net 49 "Net-(D44-Pad2)")
  (net 50 "Net-(D45-Pad2)")
  (net 51 "Net-(D46-Pad2)")
  (net 52 "Net-(D47-Pad2)")
  (net 53 "Net-(D48-Pad2)")
  (net 54 "Net-(D49-Pad2)")
  (net 55 "Net-(D50-Pad2)")
  (net 56 "Net-(D51-Pad2)")
  (net 57 "Net-(D52-Pad2)")
  (net 58 "Net-(D53-Pad2)")
  (net 59 "Net-(D54-Pad2)")
  (net 60 "Net-(D55-Pad2)")
  (net 61 "Net-(D56-Pad2)")
  (net 62 "Net-(D57-Pad2)")
  (net 63 "Net-(D58-Pad2)")
  (net 64 "Net-(D59-Pad2)")
  (net 65 "Net-(D60-Pad2)")
  (net 66 "Net-(D61-Pad2)")
  (net 67 "Net-(D62-Pad2)")
  (net 68 "Net-(D63-Pad2)")
  (net 69 "Net-(D64-Pad2)")
  (net 70 "Net-(D65-Pad2)")
  (net 71 "Net-(D66-Pad2)")
  (net 72 "Net-(D67-Pad2)")
  (net 73 "Net-(D68-Pad2)")
  (net 74 "Net-(D69-Pad2)")
  (net 75 "Net-(D70-Pad2)")
  (net 76 "Net-(D71-Pad2)")
  (net 77 "Net-(D72-Pad2)")
  (net 78 "Net-(D73-Pad2)")
  (net 79 "Net-(D74-Pad2)")
  (net 80 "Net-(D75-Pad2)")
  (net 81 "Net-(D76-Pad2)")
  (net 82 "Net-(D77-Pad2)")
  (net 83 "Net-(D78-Pad2)")
  (net 84 "Net-(D79-Pad2)")
  (net 85 "Net-(D80-Pad2)")
  (net 86 "Net-(D81-Pad2)")
  (net 87 "Net-(D82-Pad2)")
  (net 88 "Net-(D83-Pad2)")
  (net 89 "Net-(D84-Pad2)")
  (net 90 "Net-(D85-Pad2)")
  (net 91 "Net-(D86-Pad2)")
  (net 92 "Net-(D87-Pad2)")
  (net 93 "Net-(D88-Pad2)")
  (net 94 "Net-(D89-Pad2)")
  (net 95 "Net-(D90-Pad2)")
  (net 96 "Net-(D91-Pad2)")
  (net 97 "Net-(D92-Pad2)")
  (net 98 "Net-(D93-Pad2)")
  (net 99 "Net-(D94-Pad2)")
  (net 100 "Net-(D95-Pad2)")
  (net 101 "Net-(D96-Pad2)")
  (net 102 "Net-(D97-Pad2)")
  (net 103 "Net-(D98-Pad2)")
  (net 104 "Net-(D101-Pad2)")
  (net 105 "Net-(D102-Pad2)")
  (net 106 "Net-(D103-Pad2)")
  (net 107 "Net-(D104-Pad2)")
  (net 108 "Net-(D105-Pad2)")
  (net 109 "Net-(D106-Pad2)")
  (net 110 "Net-(D107-Pad2)")
  (net 111 "Net-(D108-Pad2)")
  (net 112 "Net-(D109-Pad2)")
  (net 113 "Net-(D110-Pad2)")
  (net 114 "Net-(D111-Pad2)")
  (net 115 "Net-(D112-Pad2)")
  (net 116 "Net-(D113-Pad2)")
  (net 117 /SK6812)
  (net 118 /T3)
  (net 119 /T1)
  (net 120 /T2)
  (net 121 /Guard)
  (net 122 "Net-(ANT1-Pad1)")
  (net 123 "Net-(BT1-Pad1)")
  (net 124 "Net-(C115-Pad2)")
  (net 125 "Net-(C115-Pad1)")
  (net 126 "Net-(C116-Pad1)")
  (net 127 "Net-(C117-Pad1)")
  (net 128 +4V)
  (net 129 "Net-(C122-Pad1)")
  (net 130 "Net-(C123-Pad1)")
  (net 131 "Net-(C133-Pad1)")
  (net 132 "Net-(C134-Pad1)")
  (net 133 "Net-(C136-Pad1)")
  (net 134 "Net-(C138-Pad1)")
  (net 135 "Net-(D117-Pad1)")
  (net 136 "Net-(IC3-Pad4)")
  (net 137 /NRST)
  (net 138 /LDR)
  (net 139 /TCO)
  (net 140 /CS_E)
  (net 141 /CLK)
  (net 142 /MISO)
  (net 143 /MOSI)
  (net 144 "Net-(IC3-Pad24)")
  (net 145 "Net-(IC3-Pad25)")
  (net 146 "Net-(IC3-Pad33)")
  (net 147 /SWDIO)
  (net 148 /SWCLK)
  (net 149 /MTO0)
  (net 150 /MTO1)
  (net 151 /MTO3)
  (net 152 /DQ)
  (net 153 "Net-(IC5-Pad2)")
  (net 154 "Net-(IC5-Pad3)")
  (net 155 "Net-(IC5-Pad6)")
  (net 156 "Net-(IC5-Pad10)")
  (net 157 "Net-(IC5-Pad11)")
  (net 158 "Net-(J8-PadPON)")
  (net 159 "Net-(J8-PadTCO)")
  (net 160 "Net-(R6-Pad2)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +4V)
    (add_net +5V)
    (add_net /CLK)
    (add_net /CS_E)
    (add_net /DQ)
    (add_net /Guard)
    (add_net /LDR)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /MTO0)
    (add_net /MTO1)
    (add_net /MTO3)
    (add_net /NRST)
    (add_net /SK6812)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /T1)
    (add_net /T2)
    (add_net /T3)
    (add_net /TCO)
    (add_net GND)
    (add_net "Net-(ANT1-Pad1)")
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C115-Pad1)")
    (add_net "Net-(C115-Pad2)")
    (add_net "Net-(C116-Pad1)")
    (add_net "Net-(C117-Pad1)")
    (add_net "Net-(C122-Pad1)")
    (add_net "Net-(C123-Pad1)")
    (add_net "Net-(C133-Pad1)")
    (add_net "Net-(C134-Pad1)")
    (add_net "Net-(C136-Pad1)")
    (add_net "Net-(C138-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D10-Pad4)")
    (add_net "Net-(D100-Pad2)")
    (add_net "Net-(D100-Pad4)")
    (add_net "Net-(D101-Pad2)")
    (add_net "Net-(D102-Pad2)")
    (add_net "Net-(D103-Pad2)")
    (add_net "Net-(D104-Pad2)")
    (add_net "Net-(D105-Pad2)")
    (add_net "Net-(D106-Pad2)")
    (add_net "Net-(D107-Pad2)")
    (add_net "Net-(D108-Pad2)")
    (add_net "Net-(D109-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D110-Pad2)")
    (add_net "Net-(D111-Pad2)")
    (add_net "Net-(D112-Pad2)")
    (add_net "Net-(D113-Pad2)")
    (add_net "Net-(D117-Pad1)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D16-Pad2)")
    (add_net "Net-(D17-Pad2)")
    (add_net "Net-(D18-Pad2)")
    (add_net "Net-(D19-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D20-Pad2)")
    (add_net "Net-(D21-Pad2)")
    (add_net "Net-(D22-Pad2)")
    (add_net "Net-(D23-Pad2)")
    (add_net "Net-(D24-Pad2)")
    (add_net "Net-(D25-Pad2)")
    (add_net "Net-(D26-Pad2)")
    (add_net "Net-(D27-Pad2)")
    (add_net "Net-(D28-Pad2)")
    (add_net "Net-(D29-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D30-Pad2)")
    (add_net "Net-(D31-Pad2)")
    (add_net "Net-(D32-Pad2)")
    (add_net "Net-(D33-Pad2)")
    (add_net "Net-(D34-Pad2)")
    (add_net "Net-(D35-Pad2)")
    (add_net "Net-(D36-Pad2)")
    (add_net "Net-(D37-Pad2)")
    (add_net "Net-(D38-Pad2)")
    (add_net "Net-(D39-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D40-Pad2)")
    (add_net "Net-(D41-Pad2)")
    (add_net "Net-(D42-Pad2)")
    (add_net "Net-(D43-Pad2)")
    (add_net "Net-(D44-Pad2)")
    (add_net "Net-(D45-Pad2)")
    (add_net "Net-(D46-Pad2)")
    (add_net "Net-(D47-Pad2)")
    (add_net "Net-(D48-Pad2)")
    (add_net "Net-(D49-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D50-Pad2)")
    (add_net "Net-(D51-Pad2)")
    (add_net "Net-(D52-Pad2)")
    (add_net "Net-(D53-Pad2)")
    (add_net "Net-(D54-Pad2)")
    (add_net "Net-(D55-Pad2)")
    (add_net "Net-(D56-Pad2)")
    (add_net "Net-(D57-Pad2)")
    (add_net "Net-(D58-Pad2)")
    (add_net "Net-(D59-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D60-Pad2)")
    (add_net "Net-(D61-Pad2)")
    (add_net "Net-(D62-Pad2)")
    (add_net "Net-(D63-Pad2)")
    (add_net "Net-(D64-Pad2)")
    (add_net "Net-(D65-Pad2)")
    (add_net "Net-(D66-Pad2)")
    (add_net "Net-(D67-Pad2)")
    (add_net "Net-(D68-Pad2)")
    (add_net "Net-(D69-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D70-Pad2)")
    (add_net "Net-(D71-Pad2)")
    (add_net "Net-(D72-Pad2)")
    (add_net "Net-(D73-Pad2)")
    (add_net "Net-(D74-Pad2)")
    (add_net "Net-(D75-Pad2)")
    (add_net "Net-(D76-Pad2)")
    (add_net "Net-(D77-Pad2)")
    (add_net "Net-(D78-Pad2)")
    (add_net "Net-(D79-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D80-Pad2)")
    (add_net "Net-(D81-Pad2)")
    (add_net "Net-(D82-Pad2)")
    (add_net "Net-(D83-Pad2)")
    (add_net "Net-(D84-Pad2)")
    (add_net "Net-(D85-Pad2)")
    (add_net "Net-(D86-Pad2)")
    (add_net "Net-(D87-Pad2)")
    (add_net "Net-(D88-Pad2)")
    (add_net "Net-(D89-Pad2)")
    (add_net "Net-(D90-Pad2)")
    (add_net "Net-(D91-Pad2)")
    (add_net "Net-(D92-Pad2)")
    (add_net "Net-(D93-Pad2)")
    (add_net "Net-(D94-Pad2)")
    (add_net "Net-(D95-Pad2)")
    (add_net "Net-(D96-Pad2)")
    (add_net "Net-(D97-Pad2)")
    (add_net "Net-(D98-Pad2)")
    (add_net "Net-(IC3-Pad24)")
    (add_net "Net-(IC3-Pad25)")
    (add_net "Net-(IC3-Pad33)")
    (add_net "Net-(IC3-Pad4)")
    (add_net "Net-(IC5-Pad10)")
    (add_net "Net-(IC5-Pad11)")
    (add_net "Net-(IC5-Pad2)")
    (add_net "Net-(IC5-Pad3)")
    (add_net "Net-(IC5-Pad6)")
    (add_net "Net-(J8-PadPON)")
    (add_net "Net-(J8-PadTCO)")
    (add_net "Net-(R6-Pad2)")
  )
  (module Wordclock_V1:SO-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5C509AD1)
    (at 29.75 291.9)
    (descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (attr smd)
    (fp_text reference IC6 (at 0 -3.4) (layer F.SilkS))
    (fp_text value DS18B20Z+ (at 0 3.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 2.575 -1.905) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 2.575 -0.635) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at 2.575 0.635) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at 2.575 1.905) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at -2.575 1.905) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 152 /DQ))
    (pad 3 smd roundrect (at -2.575 0.635) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (pad 2 smd roundrect (at -2.575 -0.635) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -2.575 -1.905) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:CP_Elec_5x5.3 (layer F.Cu) (tedit 5BCA39CF)
    (at 10.1 268.8)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.3mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C125 (at 0 -3.7) (layer F.SilkS))
    (fp_text value "EEE-FK1C101SR (100u)" (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.2 0) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 2 +5V))
    (pad 2 smd roundrect (at 2.2 0) (size 3 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_5x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 9.1 257.8)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J6 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value M22-7140342 (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:SO-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5C509AD1)
    (at 34.5 261.85 90)
    (descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (attr smd)
    (fp_text reference IC4 (at 0 -3.4 90) (layer F.SilkS))
    (fp_text value M95M01-DFMN6TP (at 0 3.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.575 -1.905 90) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (pad 7 smd roundrect (at 2.575 -0.635 90) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (pad 6 smd roundrect (at 2.575 0.635 90) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 141 /CLK))
    (pad 5 smd roundrect (at 2.575 1.905 90) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 143 /MOSI))
    (pad 4 smd roundrect (at -2.575 1.905 90) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at -2.575 0.635 90) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (pad 2 smd roundrect (at -2.575 -0.635 90) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 142 /MISO))
    (pad 1 smd roundrect (at -2.575 -1.905 90) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 /CS_E))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:DCF77_Pollin (layer F.Cu) (tedit 5DE0D4B7)
    (at 22.15 241.75 270)
    (fp_text reference J8 (at -5 13) (layer F.SilkS))
    (fp_text value DCF77_POLLIN (at -3 10) (layer F.Fab))
    (pad VCC thru_hole circle (at 3.46 9.89 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 133 "Net-(C136-Pad1)"))
    (pad GND thru_hole circle (at 3.46 7.35 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad PON thru_hole circle (at 3.46 4.81 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 158 "Net-(J8-PadPON)"))
    (pad TCO thru_hole circle (at 3.46 2.27 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 159 "Net-(J8-PadTCO)"))
  )
  (module Wordclock_V1:R_LDR_4.9x4.2mm_P2.54mm_Vertical (layer F.Cu) (tedit 5B8603A6)
    (at 36.3 292.4 270)
    (descr "Resistor, LDR 4.9x4.2mm")
    (tags "Resistor LDR4.9x4.2")
    (fp_text reference R11 (at 1.27 -2.9 90) (layer F.SilkS))
    (fp_text value R_PHOTO (at 1.17 3.1 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.9 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 138 /LDR))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/R_LDR_4.9x4.2mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 35.6 289.7)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 138 /LDR))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 14.3 251.2 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 133 "Net-(C136-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 134 "Net-(C138-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:L_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 19.1 251.2 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L5 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 47u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 134 "Net-(C138-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 135 "Net-(D117-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm (layer F.Cu) (tedit 5A64794F)
    (at 36.3 299.4 270)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP3 (at 0 -1.8 90) (layer F.SilkS))
    (fp_text value Jumper (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd custom (at 0.725 0 270) (size 0.3 0.3) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.65 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy -0.65 0.75) (xy -0.15 0)
) (width 0))
      ))
    (pad 1 smd custom (at -0.725 0 270) (size 0.3 0.3) (layers F.Cu F.Mask)
      (net 156 "Net-(IC5-Pad10)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.5 -0.75) (xy 0.5 -0.75) (xy 1 0) (xy 0.5 0.75) (xy -0.5 0.75)
) (width 0))
      ))
  )
  (module Wordclock_V1:pad (layer F.Cu) (tedit 5F2A7931)
    (at 35.3 314.9 90)
    (fp_text reference J7 (at 0 -3 90) (layer F.SilkS))
    (fp_text value Guard (at 0 -1.6 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 121 /Guard))
  )
  (module Wordclock_V1:pad (layer F.Cu) (tedit 5F2A7931)
    (at 29.3 315.6 90)
    (fp_text reference J6 (at 0 -3 90) (layer F.SilkS))
    (fp_text value Taster3 (at 0 -1.6 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 118 /T3))
  )
  (module Wordclock_V1:pad (layer F.Cu) (tedit 5F2A7931)
    (at 32.2 315.7 90)
    (fp_text reference J5 (at 0 -3 90) (layer F.SilkS))
    (fp_text value Taster2 (at 0 -1.6 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 120 /T2))
  )
  (module Wordclock_V1:pad (layer F.Cu) (tedit 5F2A7931)
    (at 37.8 314.2 90)
    (fp_text reference J4 (at 0 -3 90) (layer F.SilkS))
    (fp_text value Taster1 (at 0 -1.6 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 119 /T1))
  )
  (module Wordclock_V1:TerminalBlock_Phoenix_PTSM-0,5-2-2.5-V-THR_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5B294EB8)
    (at 9.1 277)
    (descr "Terminal Block Phoenix PTSM-0,5-2-2.5-V-THR, vertical (cable from top), 2 pins, pitch 2.5mm, size 5.5x5mm^2, drill diamater 1.2mm, pad diameter 2mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556444-da-01-de-LEITERPLATTENKL__PTSM_0_5__4_2_5_V_THR.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix PTSM-0,5-2-2.5-V-THR vertical pitch 2.5mm size 5.5x5mm^2 drill 1.2mm pad 2mm")
    (fp_text reference J2 (at 0.4 -5.16) (layer F.SilkS))
    (fp_text value 1770953 (at 0.4 1.96) (layer F.Fab))
    (fp_text user %R (at 0.4 -5.16) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 1 thru_hole rect (at 0 -3.1) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 2.5 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -3.1) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PTSM-0,5-2-2.5-V-THR_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 4.2 256.5 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D117 (at 0 -2) (layer F.SilkS))
    (fp_text value BAS16GWX (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(D117-Pad1)"))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 11.2 251.2 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D116 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value BZX84C3V0LT1G (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(C136-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 17.7 264.5 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D115 (at 0 -2) (layer F.SilkS))
    (fp_text value BAS16GWX (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 128 +4V))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 18.3 254.6)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C121 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 18.3 262)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C120 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 128 +4V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 29.8 284.75 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C132 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 30.2 296.7 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C139 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 31.95 276.1 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C134 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 100n (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 132 "Net-(C134-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 19.4375 279.4 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C133 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 4u7 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 "Net-(C133-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 22.8 272.9 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C128 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 100p (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 20.55 285.55 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C131 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 27 272.6)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C130 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 25.65 269.8 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C116 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0.8p (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 126 "Net-(C116-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 30.45 263.85 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C124 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 25 285.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C127 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 33.6 285.35)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C122 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 6p (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 129 "Net-(C122-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 34.35 281.8 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C123 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 6p (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 "Net-(C123-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 22.8 270.9 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C129 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 6 251.2 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C136 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 133 "Net-(C136-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 27.15 257.05)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C118 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 0.8p (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 125 "Net-(C115-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 16.8 251.2 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C138 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4u7 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 134 "Net-(C138-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:TSSOP-14_4.4x5mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 31.4 302.9 90)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference IC5 (at 0 -3.55 90) (layer F.SilkS))
    (fp_text value MTCH105-I/ST (at 0 3.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -1.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at -2.95 -1.3 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(IC5-Pad2)"))
    (pad 3 smd rect (at -2.95 -0.65 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(IC5-Pad3)"))
    (pad 4 smd rect (at -2.95 0 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 5 smd rect (at -2.95 0.65 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 121 /Guard))
    (pad 6 smd rect (at -2.95 1.3 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(IC5-Pad6)"))
    (pad 7 smd rect (at -2.95 1.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 2.95 1.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.95 1.3 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 151 /MTO3))
    (pad 10 smd rect (at 2.95 0.65 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(IC5-Pad10)"))
    (pad 11 smd rect (at 2.95 0 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(IC5-Pad11)"))
    (pad 12 smd rect (at 2.95 -0.65 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 150 /MTO1))
    (pad 13 smd rect (at 2.95 -1.3 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 149 /MTO0))
    (pad 14 smd rect (at 2.95 -1.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 8.2 251.2 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C137 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4u7 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 133 "Net-(C136-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 27.4 304.9 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C135 (at 1.3 -1.9 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 32.7 309.3 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 153 "Net-(IC5-Pad2)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 /T1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 27.15 251.25)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C119 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 0.3p (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 122 "Net-(ANT1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 27.9 296.7 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 152 /DQ))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 33.6 279)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 136 "Net-(IC3-Pad4)"))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 29.85 269.7875 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C117 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0.3p (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 "Net-(C117-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 20.55 283.55 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C126 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 4u7 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 30.2 309.3 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 1.3 1.1 90) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 154 "Net-(IC5-Pad3)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 120 /T2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 32.5 296.7 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 5k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 138 /LDR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 36.3 303.9 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 157 "Net-(IC5-Pad11)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 160 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 27.4 309.3 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -0.1 1.7 90) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 155 "Net-(IC5-Pad6)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 118 /T3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:BatteryHolder_Keystone_1060_1x2032 (layer F.Cu) (tedit 5B98EF5E)
    (at 15.2 306.2 270)
    (descr http://www.keyelco.com/product-pdf.cfm?p=726)
    (tags "CR2032 BR2032 BatteryHolder Battery")
    (attr smd)
    (fp_text reference BT1 (at -14.125 -5.3 90) (layer F.SilkS))
    (fp_text value 1060TR (at 0 -11.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 14.65 0 90) (size 2.6 3.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -14.65 0 90) (size 2.6 3.6) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_Keystone_1060_1x2032.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:L_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 19.45 281.4 180)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L3 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 146 "Net-(IC3-Pad33)"))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 "Net-(C133-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 14.2 263.7 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 117 /SK6812))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:Antenna_BLE (layer F.Cu) (tedit 5DDFF34E)
    (at 28.5 249.8)
    (fp_text reference ANT1 (at 1.6 -0.9) (layer F.SilkS))
    (fp_text value Antenna_BLE (at 0 -7.7) (layer F.Fab))
    (pad 1 smd rect (at -2.3 -0.65) (size 0.4 1.1) (layers F.Cu)
      (net 122 "Net-(ANT1-Pad1)"))
    (pad ANT smd rect (at -3.45 -1.4) (size 2.7 0.4) (layers F.Cu))
    (pad ANT smd rect (at 1.2 -6.2) (size 6.6 0.4) (layers F.Cu))
    (pad ANT smd rect (at 4.3 -5.6) (size 0.4 0.8) (layers F.Cu))
    (pad ANT smd rect (at -0.15 -5) (size 9.3 0.4) (layers F.Cu))
    (pad ANT smd rect (at -4.6 -4.4) (size 0.4 0.8) (layers F.Cu))
    (pad ANT smd rect (at -0.15 -3.8) (size 9.3 0.4) (layers F.Cu))
    (pad ANT smd rect (at 4.3 -3.2) (size 0.4 0.8) (layers F.Cu))
    (pad ANT smd rect (at -0.15 -2.6) (size 9.3 0.4) (layers F.Cu))
    (pad ANT smd rect (at -4.6 -1.994) (size 0.4 0.8) (layers F.Cu))
  )
  (module Wordclock_V1:Potentiometer_Bourns_TC33X_Vertical (layer F.Cu) (tedit 5C165D15)
    (at 36.3 308.3 90)
    (descr "Potentiometer, Bourns, TC33X, Vertical, https://www.bourns.com/pdfs/TC33.pdf")
    (tags "Potentiometer Bourns TC33X Vertical")
    (attr smd)
    (fp_text reference RV1 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value "TC33X-2-103E (20k)" (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (fp_text user "Wiper may be\nanywhere within\ncircle shown" (at -0.15 -0.8 90) (layer Cmts.User))
    (pad 1 smd rect (at -1.8 -1 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.8 1 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at 1.45 0 90) (size 1.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_TC33X_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:SOT-89-3 (layer F.Cu) (tedit 5A02FF57)
    (at 16.8 258.3)
    (descr SOT-89-3)
    (tags SOT-89-3)
    (attr smd)
    (fp_text reference IC2 (at 0.45 -3.2) (layer F.SilkS))
    (fp_text value AP7365-33YG-13 (at 0.45 3.25) (layer F.Fab))
    (fp_text user %R (at 0.38 0 90) (layer F.Fab))
    (pad 2 smd trapezoid (at -0.0762 0 90) (size 1.5 1) (rect_delta 0 0.7 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.3335 0 270) (size 2.2 1.84) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.48 1.5 270) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 128 +4V))
    (pad 2 smd rect (at -1.3335 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.48 -1.5 270) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd trapezoid (at 2.667 0 270) (size 1.6 0.85) (rect_delta 0 0.6 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:L_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 34.3 276.1 270)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L4 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 47u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 132 "Net-(C134-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 24.2 257.9375 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C115 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 124 "Net-(C115-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 125 "Net-(C115-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:RFBPF1608070A0T (layer F.Cu) (tedit 5DEE665A)
    (at 24.2 262.9 270)
    (fp_text reference IC1 (at 0 -2 90) (layer F.SilkS))
    (fp_text value RFBPF1608070A0T (at 0 -3.8 90) (layer F.Fab))
    (pad 1 smd rect (at 0.9 0 270) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(C117-Pad1)"))
    (pad 3 smd rect (at -0.9 0 270) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(C115-Pad2)"))
    (pad 4 smd rect (at 0 0.5 270) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -0.5 270) (size 1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Wordclock_V1:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm (layer B.Cu) (tedit 5A64794F)
    (at 26.8 237.5 90)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.8 90) (layer B.SilkS))
    (fp_text value Jumper (at 0 -1.9 90) (layer B.Fab))
    (pad 2 smd custom (at 0.725 0 90) (size 0.3 0.3) (layers B.Cu B.Mask)
      (net 139 /TCO) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.65 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy -0.65 -0.75) (xy -0.15 0)
) (width 0))
      ))
    (pad 1 smd custom (at -0.725 0 90) (size 0.3 0.3) (layers B.Cu B.Mask)
      (net 158 "Net-(J8-PadPON)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.5 0.75) (xy 0.5 0.75) (xy 1 0) (xy 0.5 -0.75) (xy -0.5 -0.75)
) (width 0))
      ))
  )
  (module Wordclock_V1:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm (layer B.Cu) (tedit 5A64794F)
    (at 30.75 237.6 90)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 1.8 90) (layer B.SilkS))
    (fp_text value Jumper (at 0 -1.9 90) (layer B.Fab))
    (pad 2 smd custom (at 0.725 0 90) (size 0.3 0.3) (layers B.Cu B.Mask)
      (net 139 /TCO) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.65 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy -0.65 -0.75) (xy -0.15 0)
) (width 0))
      ))
    (pad 1 smd custom (at -0.725 0 90) (size 0.3 0.3) (layers B.Cu B.Mask)
      (net 159 "Net-(J8-PadTCO)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.5 0.75) (xy 0.5 0.75) (xy 1 0) (xy 0.5 -0.75) (xy -0.5 -0.75)
) (width 0))
      ))
  )
  (module Wordclock_V1:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm (layer B.Cu) (tedit 5A64794F)
    (at 19.9 239.9 90)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP5 (at 0 1.8 90) (layer B.SilkS))
    (fp_text value Jumper (at 0 -1.9 90) (layer B.Fab))
    (pad 2 smd custom (at 0.725 0 90) (size 0.3 0.3) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.65 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy -0.65 -0.75) (xy -0.15 0)
) (width 0))
      ))
    (pad 1 smd custom (at -0.725 0 90) (size 0.3 0.3) (layers B.Cu B.Mask)
      (net 159 "Net-(J8-PadTCO)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.5 0.75) (xy 0.5 0.75) (xy 1 0) (xy 0.5 -0.75) (xy -0.5 -0.75)
) (width 0))
      ))
  )
  (module Wordclock_V1:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm (layer B.Cu) (tedit 5A64794F)
    (at 16.5 239.2 90)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP4 (at 0 1.8 90) (layer B.SilkS))
    (fp_text value Jumper (at 0 -1.9 90) (layer B.Fab))
    (pad 2 smd custom (at 0.725 0 90) (size 0.3 0.3) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.65 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy -0.65 -0.75) (xy -0.15 0)
) (width 0))
      ))
    (pad 1 smd custom (at -0.725 0 90) (size 0.3 0.3) (layers B.Cu B.Mask)
      (net 158 "Net-(J8-PadPON)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.5 0.75) (xy 0.5 0.75) (xy 1 0) (xy 0.5 -0.75) (xy -0.5 -0.75)
) (width 0))
      ))
  )
  (module Wordclock_V1:L_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 27.75 269.8 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value ? (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 126 "Net-(C116-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 "Net-(C117-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:Wuerth_36103205_20x20mm (layer F.Cu) (tedit 5A143358)
    (at 26.2 277.4 90)
    (descr "WE-SHC Shielding Cabinet SMD 20x20mm")
    (tags "Shielding Cabinet")
    (attr smd)
    (fp_text reference J1 (at 0 -11.75 90) (layer F.SilkS))
    (fp_text value 36103205 (at 0 11.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -10.25 -10.25 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 10.25 -10.25 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 10.25 10.25 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -10.25 10.25 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -8.6 -10.25 90) (size 2.3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -8.6 10.25 90) (size 2.3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.75 -10.25 90) (size 2.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.75 10.25 90) (size 2.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 3.75 -10.25 90) (size 2.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 3.75 10.25 90) (size 2.6 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 8.6 -10.25 90) (size 2.3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 8.6 10.25 90) (size 2.3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -10.25 -8.6 90) (size 1 2.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 10.25 -8.6 90) (size 1 2.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -10.25 -3.75 90) (size 1 2.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 10.25 -3.75 90) (size 1 2.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -10.25 3.75 90) (size 1 2.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 10.25 3.75 90) (size 1 2.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -10.25 8.6 90) (size 1 2.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 10.25 8.6 90) (size 1 2.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/RF_Shielding.3dshapes/Wuerth_36103205_20x20mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:Crystal_Epson_FC135 (layer F.Cu) (tedit 5DE3EF60)
    (at 32.1 282.05 90)
    (fp_text reference Y1 (at 0 -4 90) (layer F.SilkS))
    (fp_text value "FC-135 32.7680KA-A" (at 0 -6 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(C123-Pad1)"))
    (pad 1 smd rect (at -1.25 0 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(C122-Pad1)"))
  )
  (module Wordclock_V1:Crystal_SMD_Abracon_ABM8G-4Pin_3.2x2.5mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 20.55 276.25 270)
    (descr "Abracon Miniature Ceramic Smd Crystal ABM8G http://www.abracon.com/Resonators/ABM8G.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y2 (at 0 -2.45 90) (layer F.SilkS))
    (fp_text value ABM8AIG-32.000MHz-8-2Z-T (at 0 2.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(IC3-Pad24)"))
    (pad 2 smd rect (at 1.1 0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 -0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(IC3-Pad25)"))
    (pad 4 smd rect (at -1.1 -0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_Abracon_ABM8G-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:L_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 26.2 254.15 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L2 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value ? (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 125 "Net-(C115-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 122 "Net-(ANT1-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:PinHeader_2x03_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 11.64 286.44 180)
    (descr "Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x03 2.54mm double row")
    (fp_text reference J3 (at 5.655 -2.27) (layer F.SilkS))
    (fp_text value M20-9740346 (at 5.655 7.35) (layer F.Fab))
    (fp_text user %R (at 5.31 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 148 /SWCLK))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 147 /SWDIO))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 137 /NRST))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm_ThermalVias (layer F.Cu) (tedit 5DE41079)
    (at 26.6 278.75 180)
    (descr "VQFN, 48 Pin (http://www.ti.com/lit/ds/symlink/cc1312r.pdf#page=48), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (attr smd)
    (fp_text reference IC3 (at 0 -4.82) (layer F.SilkS))
    (fp_text value STM32WB55CEU6 (at 0 4.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 49 smd roundrect (at 0 0 180) (size 5.15 5.15) (layers F.Cu F.Mask) (roundrect_rratio 0.048544)
      (net 1 GND))
    (pad 49 thru_hole circle (at -2.325 -2.325 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at -1.1625 -2.325 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at 0 -2.325 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at 1.1625 -2.325 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at 2.325 -2.325 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at -2.325 -1.1625 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at -1.1625 -1.1625 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at 0 -1.1625 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at 1.1625 -1.1625 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at 2.325 -1.1625 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at -2.325 0 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at -1.1625 0 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at 0 0 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at 1.1625 0 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at 2.325 0 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at -2.325 1.1625 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at -1.1625 1.1625 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at 0 1.1625 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at 1.1625 1.1625 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at 2.325 1.1625 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at -2.325 2.325 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at -1.1625 2.325 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at 0 2.325 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at 1.1625 2.325 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 49 thru_hole circle (at 2.325 2.325 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad "" smd roundrect (at -1.29 -1.29 180) (size 2.08 2.08) (layers F.Paste) (roundrect_rratio 0.120192))
    (pad "" smd roundrect (at -1.29 1.29 180) (size 2.08 2.08) (layers F.Paste) (roundrect_rratio 0.120192))
    (pad "" smd roundrect (at 1.29 -1.29 180) (size 2.08 2.08) (layers F.Paste) (roundrect_rratio 0.120192))
    (pad "" smd roundrect (at 1.29 1.29 180) (size 2.08 2.08) (layers F.Paste) (roundrect_rratio 0.120192))
    (pad 1 smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 123 "Net-(BT1-Pad1)"))
    (pad 2 smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 129 "Net-(C122-Pad1)"))
    (pad 3 smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 "Net-(C123-Pad1)"))
    (pad 4 smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 136 "Net-(IC3-Pad4)"))
    (pad 5 smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 137 /NRST))
    (pad 8 smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 132 "Net-(C134-Pad1)"))
    (pad 9 smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 138 /LDR))
    (pad 10 smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 11 smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 12 smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 139 /TCO))
    (pad 13 smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 /CS_E))
    (pad 14 smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 141 /CLK))
    (pad 15 smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 142 /MISO))
    (pad 16 smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 143 /MOSI))
    (pad 17 smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 18 smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 19 smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 20 smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (pad 21 smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 126 "Net-(C116-Pad1)"))
    (pad 22 smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 23 smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (pad 24 smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 144 "Net-(IC3-Pad24)"))
    (pad 25 smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 145 "Net-(IC3-Pad25)"))
    (pad 26 smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 27 smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 28 smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 29 smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 30 smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 31 smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 "Net-(C133-Pad1)"))
    (pad 32 smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 33 smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 146 "Net-(IC3-Pad33)"))
    (pad 34 smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (pad 35 smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (pad 36 smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 37 smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 117 /SK6812))
    (pad 38 smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 39 smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 147 /SWDIO))
    (pad 40 smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (pad 41 smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 148 /SWCLK))
    (pad 42 smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 43 smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 149 /MTO0))
    (pad 44 smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 150 /MTO1))
    (pad 45 smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 151 /MTO3))
    (pad 46 smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 152 /DQ))
    (pad 47 smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 152 /DQ))
    (pad 48 smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/VQFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:MountingHole_6mm (layer F.Cu) (tedit 56D1B4CB)
    (at 15 15)
    (descr "Mounting Hole 6mm, no annular")
    (tags "mounting hole 6mm no annular")
    (attr virtual)
    (fp_text reference H4 (at 0 -7) (layer F.SilkS))
    (fp_text value MountingHole (at 0 7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 6 6) (drill 6) (layers *.Cu *.Mask))
  )
  (module Wordclock_V1:MountingHole_6mm (layer F.Cu) (tedit 56D1B4CB)
    (at 355 355)
    (descr "Mounting Hole 6mm, no annular")
    (tags "mounting hole 6mm no annular")
    (attr virtual)
    (fp_text reference H3 (at 0 -7) (layer F.SilkS))
    (fp_text value MountingHole (at 0 7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 6 6) (drill 6) (layers *.Cu *.Mask))
  )
  (module Wordclock_V1:MountingHole_6mm (layer F.Cu) (tedit 56D1B4CB)
    (at 355 15)
    (descr "Mounting Hole 6mm, no annular")
    (tags "mounting hole 6mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -7) (layer F.SilkS))
    (fp_text value MountingHole (at 0 7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 6 6) (drill 6) (layers *.Cu *.Mask))
  )
  (module Wordclock_V1:MountingHole_6mm (layer F.Cu) (tedit 56D1B4CB)
    (at 15 355)
    (descr "Mounting Hole 6mm, no annular")
    (tags "mounting hole 6mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -7) (layer F.SilkS))
    (fp_text value MountingHole (at 0 7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 6 6) (drill 6) (layers *.Cu *.Mask))
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 144.5 350 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D114 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 117 /SK6812))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 116 "Net-(D113-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 171.5 350 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D113 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 116 "Net-(D113-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 115 "Net-(D112-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 198.5 350 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D112 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 115 "Net-(D112-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 114 "Net-(D111-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 225.5 350 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D111 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 114 "Net-(D111-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 113 "Net-(D110-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 320 320)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D110 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 113 "Net-(D110-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 112 "Net-(D109-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 293 320)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D109 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 112 "Net-(D109-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 111 "Net-(D108-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 266 320)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D108 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 111 "Net-(D108-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 110 "Net-(D107-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 239 320)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D107 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 110 "Net-(D107-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 109 "Net-(D106-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 212 320)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D106 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 109 "Net-(D106-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 108 "Net-(D105-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 185 320)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D105 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 108 "Net-(D105-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 107 "Net-(D104-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 158 320)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D104 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 107 "Net-(D104-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 106 "Net-(D103-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 131 320)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D103 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 106 "Net-(D103-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 105 "Net-(D102-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 104 320)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D102 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 105 "Net-(D102-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 104 "Net-(D101-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 77 320)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D101 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 104 "Net-(D101-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D100-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 50 320)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D100 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D100-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D100-Pad4)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 50 290 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D99 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D100-Pad4)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 103 "Net-(D98-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 77 290 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D98 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 103 "Net-(D98-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 102 "Net-(D97-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 104 290 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D97 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 102 "Net-(D97-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 101 "Net-(D96-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 131 290 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D96 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 101 "Net-(D96-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 100 "Net-(D95-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 158 290 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D95 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 100 "Net-(D95-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 99 "Net-(D94-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 185 290 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D94 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 99 "Net-(D94-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(D93-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 212 290 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D93 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(D93-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 97 "Net-(D92-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 239 290 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D92 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 97 "Net-(D92-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 96 "Net-(D91-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 266 290 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D91 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 96 "Net-(D91-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 95 "Net-(D90-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 293 290 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D90 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 95 "Net-(D90-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 94 "Net-(D89-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 320 290 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D89 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 94 "Net-(D89-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(D88-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 320 260)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D88 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(D88-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(D87-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 293 260)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D87 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(D87-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 91 "Net-(D86-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 266 260)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D86 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 91 "Net-(D86-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 90 "Net-(D85-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 239 260)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D85 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 90 "Net-(D85-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 89 "Net-(D84-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 212 260)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D84 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 89 "Net-(D84-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 88 "Net-(D83-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 185 260)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D83 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 88 "Net-(D83-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 87 "Net-(D82-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 158 260)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D82 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 87 "Net-(D82-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 86 "Net-(D81-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 131 260)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D81 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 86 "Net-(D81-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 85 "Net-(D80-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 104 260)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D80 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 85 "Net-(D80-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 84 "Net-(D79-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 77 260)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D79 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 84 "Net-(D79-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(D78-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 50 260)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D78 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(D78-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(D77-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 50 230 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D77 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(D77-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(D76-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 77 230 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D76 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(D76-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(D75-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 104 230 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D75 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(D75-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(D74-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 131 230 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D74 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(D74-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(D73-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 158 230 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D73 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(D73-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(D72-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 185 230 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D72 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(D72-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(D71-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 212 230 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D71 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(D71-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(D70-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 239 230 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D70 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(D70-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(D69-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 266 230 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D69 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(D69-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(D68-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 293 230 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D68 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(D68-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(D67-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 320 230 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D67 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(D67-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(D66-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 320 200)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D66 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(D66-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(D65-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 293 200)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D65 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(D65-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(D64-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 266 200)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D64 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(D64-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(D63-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 239 200)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D63 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(D63-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(D62-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 212 200)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D62 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(D62-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(D61-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 185 200)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D61 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(D61-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(D60-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 158 200)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D60 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(D60-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(D59-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 131 200)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D59 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(D59-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(D58-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 104 200)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D58 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(D58-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(D57-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 77 200)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D57 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(D57-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(D56-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 50 200)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D56 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(D56-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(D55-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 50 170 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D55 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(D55-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(D54-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 77 170 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D54 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(D54-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(D53-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 104 170 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D53 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(D53-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(D52-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 131 170 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D52 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(D52-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(D51-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 158 170 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D51 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(D51-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(D50-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 185 170 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D50 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(D50-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(D49-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 212 170 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D49 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(D49-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(D48-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 239 170 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D48 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(D48-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(D47-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 266 170 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D47 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(D47-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(D46-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 293 170 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D46 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(D46-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(D45-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 320 170 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D45 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(D45-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(D44-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 320 140)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D44 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(D44-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(D43-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 293 140)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D43 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(D43-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(D42-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 266 140)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D42 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(D42-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(D41-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 239 140)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D41 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(D41-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(D40-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 212 140)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D40 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(D40-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(D39-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 185 140)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D39 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(D39-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(D38-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 158 140)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D38 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(D38-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(D37-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 131 140)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D37 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(D37-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(D36-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 104 140)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D36 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(D36-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(D35-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 77 140)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D35 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(D35-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(D34-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 50 140)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D34 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(D34-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(D33-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 50 110 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D33 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(D33-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(D32-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 77 110 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D32 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(D32-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(D31-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 104 110 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D31 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(D31-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(D30-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 131 110 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D30 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(D30-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(D29-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 158 110 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D29 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(D29-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(D28-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 185 110 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D28 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(D28-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(D27-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 212 110 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D27 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(D27-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(D26-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 239 110 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D26 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(D26-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(D25-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 266 110 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D25 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(D25-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(D24-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 293 110 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D24 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(D24-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(D23-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 320 110 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D23 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(D23-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(D22-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 320 80)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D22 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(D22-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(D21-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 293 80)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D21 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(D21-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(D20-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 266 80)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D20 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(D20-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D19-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 239 80)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D19 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D19-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D18-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 212 80)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D18 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D18-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D17-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 185 80)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D17 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D17-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D16-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 158 80)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D16 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D16-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D15-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 131 80)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D15 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D15-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D14-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 104 80)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D14 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D14-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D13-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 77 80)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D13 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D13-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D12-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 50 80)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D12 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D12-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D11-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 50 50 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D11 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D11-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D10-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 77 50 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D10 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D10-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D10-Pad4)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 104 50 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D9 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D10-Pad4)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D8-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 131 50 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D8 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D8-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D7-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 158 50 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D7 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D7-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D6-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 185 50 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D6 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D6-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D5-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 212 50 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D5 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D5-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D4-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 239 50 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D4 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D4-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D3-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 266 50 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D3 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D3-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 293 50 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D2 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer B.Cu) (tedit 5EF0970F)
    (at 320 50 180)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D1 (at 0 3.5) (layer B.SilkS))
    (fp_text value SK6812 (at 0 -4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at 2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (pad 4 smd rect (at -2.65 -1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -2.65 1.6 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 146 345.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C114 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 173 345.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C113 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 200 345.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C112 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 227 345.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C111 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 318.5 324.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C110 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 291.5 324.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C109 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 264.5 324.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C108 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 237.5 324.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C107 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 210.5 324.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C106 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 183.5 324.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C105 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 156.5 324.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C104 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 129.5 324.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C103 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 102.5 324.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C102 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 75.5 324.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C101 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 48.5 324.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C100 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 51.5 285.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C99 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 78.5 285.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C98 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 105.5 285.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C97 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 132.5 285.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C96 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 159.5 285.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C95 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 186.5 285.45)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C94 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 213.5 285.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C93 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 240.5 285.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C92 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 267.5 285.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C91 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 294.5 285.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C90 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 321.5 285.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C89 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 318.5 264.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C88 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 291.5 264.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C87 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 264.5 264.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C86 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 237.5 264.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C85 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 210.5 264.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C84 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 183.5 264.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C83 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 156.5 264.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C82 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 129.5 264.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C81 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 102.5 264.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C80 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 75.5 264.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C79 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 48.5 264.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C78 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 51.5 225.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C77 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 78.5 225.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C76 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 105.5 225.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C75 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 132.5 225.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C74 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 159.5 225.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C73 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 186.5 225.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C72 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 213.5 225.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C71 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 240.5 225.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C70 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 267.5 225.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C69 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 294.5 225.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C68 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 321.5 225.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C67 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 318.5 204.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C66 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 291.5 204.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C65 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 264.5 204.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C64 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 237.5 204.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C63 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 210.5 204.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C62 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 183.5 204.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C61 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 156.5 204.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C60 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 129.5 204.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C59 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 102.5 204.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C58 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 75.5 204.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C57 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 48.5 204.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C56 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 51.5 165.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C55 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 78.5 165.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C54 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 105.5 165.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C53 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 132.5 165.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C52 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 159.5 165.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C51 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 186.5 165.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C50 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 213.5 165.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C49 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 240.5 165.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C48 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 267.5 165.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C47 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 294.5 165.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C46 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 321.5 165.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C45 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 318.5 144.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C44 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 291.5 144.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C43 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 264.5 144.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C42 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 237.5 144.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C41 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 210.5 144.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C40 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 183.5625 144.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C39 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 156.5 144.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C38 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 129.5 144.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C37 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 102.5 144.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C36 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 75.5 144.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C35 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 48.5 144.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C34 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 51.5 105.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C33 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 78.5 105.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C32 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 105.5 105.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C31 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 132.5 105.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 159.5 105.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 186.5 105.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 213.5 105.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 240.5 105.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 267.5 105.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 294.5 105.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 321.5 105.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 318.5 84.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 291.5 84.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 264.5 84.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 237.5 84.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 210.5 84.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 183.5 84.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 156.5 84.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 129.5 84.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 102.5 84.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 75.5 84.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 48.5 84.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 51.5 45.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 78.5 45.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 105.5 45.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 132.5625 45.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 159.5 45.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 186.5 45.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 213.5 45.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 240.5 45.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 267.5 45.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 294.5 45.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wordclock_V1:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 321.5 45.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 1.65) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Wordclock\n11.12.2019" (at 459.7 318.6 90) (layer F.Mask))
  (gr_text "Wordclock\n11.12.2019" (at 358.6 252.8 180) (layer F.Mask))
  (gr_line (start 0 0) (end 0 370) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 370 370) (end 0 370) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 370 0) (end 370 370) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 0) (end 370 0) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 370 327.5) (xy 0 327.5) (xy 0 0) (xy 370 0)
      )
    )
  )
  (zone (net 119) (net_name /T1) (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 120 370) (xy 0 370) (xy 0 330) (xy 120 330)
      )
    )
  )
  (zone (net 120) (net_name /T2) (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 245 370) (xy 125 370) (xy 125 330) (xy 245 330)
      )
    )
  )
  (zone (net 118) (net_name /T3) (layer In2.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 370 370) (xy 250 370) (xy 250 330) (xy 370 330)
      )
    )
  )
  (zone (net 121) (net_name /Guard) (layer In1.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 370 370) (xy 0 370) (xy 0 330) (xy 370 330)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 370 327.5) (xy 0 327.5) (xy 0 0) (xy 370 0)
      )
    )
  )
  (zone (net 7) (net_name +3V3) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 370 327.5) (xy 0 327.5) (xy 0 0) (xy 370 0)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 370 370) (xy 0 370) (xy 0 0) (xy 370 0)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.925 259.4) (xy 12.8 264.9) (xy 10.3 264.9) (xy 10.3 278.3) (xy 4.45 278.3)
        (xy 4.475 259.4)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.925 259.4) (xy 12.8 264.9) (xy 10.15 264.9) (xy 10.1 267.1) (xy 10.15 278.3)
        (xy 4.45 278.3) (xy 4.475 259.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16 254) (xy 16 255.4) (xy 13.6 255.4) (xy 13.6 254)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.925 259.4) (xy 12.8 264.9) (xy 10.15 264.9) (xy 10.1 267.1) (xy 10.15 278.3)
        (xy 4.45 278.3) (xy 4.475 259.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23.4 275.1) (xy 30.1 275.1) (xy 30.1 282.1) (xy 23.3 282.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.1 274.9) (xy 30.1 282.4) (xy 23.1 282.4) (xy 23.1 274.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19.2 317.1) (xy 19.2 323.1) (xy 11.2 323.1) (xy 11.2 317.1)
      )
    )
  )
)
