(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 32)
    (tracks 0)
    (zones 0)
    (modules 2)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 5)
    (pad_drill 2.5)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module MountingHole:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 122.75 89)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS))
    (fp_text value MountingHole_2.5mm_Pad (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 103.25 58.5)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS))
    (fp_text value MountingHole_2.5mm_Pad (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (gr_line (start 126 53.5) (end 126 69.25) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 126 78.25) (end 122.5 78.25) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 122.5 69.25) (end 122.5 78.25) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 122.5 69.25) (end 126 69.25) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 100 69.25) (end 100 53.5) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 103.5 78.25) (end 100 78.25) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 103.5 69.25) (end 103.5 78.25) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 100 69.25) (end 103.5 69.25) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 100 94) (end 100 78.25) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 106 94) (end 100 94) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 106 100) (end 106 94) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 106 100) (end 120 100) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 120 94) (end 120 100) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 126 94) (end 120 94) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 126 78.25) (end 126 94) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 100 53.5) (end 126 53.5) (layer Edge.Cuts) (width 0.2))
)
