(module Connector_FFC-FPC:Hirose_FH12-6S-0.5SH_1x06-1MP_P0.50mm_Horizontal (layer F.Cu) (tedit 5D24667B)
  (descr "Hirose FH12, FFC/FPC connector, FH12-6S-0.5SH, 6 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
  (tags "connector Hirose FH12 horizontal")
  (attr smd)
  (fp_text reference REF** (at 0 -3.7) (layer F.SilkS))
  (fp_text value Hirose_FH12-6S-0.5SH_1x06-1MP_P0.50mm_Horizontal (at 0 5.6) (layer F.Fab))
  (fp_text user %R (at 0 3.7) (layer F.Fab))
  (pad 6 smd rect (at 1.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.75 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -1.25 -1.85) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask))
  (pad MP smd rect (at -3.15 1.4) (size 1.8 2.2) (layers F.Cu F.Paste F.Mask))
  (pad MP smd rect (at 3.15 1.4) (size 1.8 2.2) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/Hirose_FH12-6S-0.5SH_1x06-1MP_P0.50mm_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
