(footprint "B02B-PASK-1LFSN" (version 20210126) (generator pcbnew) (layer "F.Cu")
  (tedit 602FBC1C)
  (attr through_hole)
  (fp_text reference "REF**" (at -1 0) (layer "F.SilkS"))
  (fp_text value "CONN_B02B-PASK-1_JST" (at -1 0) (layer "F.SilkS"))
  (fp_text user "*" (at 0 0) (layer "F.SilkS"))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
  (fp_text user "*" (at 0 0) (layer "F.Fab"))
  (pad "" np_thru_hole circle (at 1.5 -1.7) (locked) (size 1.1938 1.1938) (drill 1.1938) (layers F&B.Cu *.Mask))
  (pad "1" thru_hole circle (at 0.000001 0) (locked) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at -2.000001 0) (locked) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
)
