(kicad_symbol_lib (version 20201005) (generator kicad_symbol_editor)
  (symbol "em20b:EM20B" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "SW" (id 0) (at 0 10.16 0))
    (property "Value" "EM20B" (id 1) (at 0 -10.16 0))
    (property "Footprint" "dp:EM20B" (id 2) (at 0 -12.7 0))
    (property "Datasheet" "https://www.mouser.de/datasheet/2/15/EM20B-587875.pdf" (id 3) (at 1.27 -16.51 0))
    (property "ki_keywords" "Magnetic Rotray encoder" (id 4) (at 0 0 0))
    (property "ki_description" "Magnetic Rotray encoder" (id 5) (at 0 0 0))
    (symbol "EM20B_0_1")
    (symbol "EM20B_1_1"
      (pin passive line (at -7.62 1.27 0) (length 2.54)
        (name "A")
        (number "A")
      )
      (pin passive line (at -7.62 -1.27 0) (length 2.54)
        (name "B")
        (number "B")
      )
      (pin passive line (at -7.62 -5.08 0) (length 2.54)
        (name "GA")
        (number "GA")
      )
      (pin passive line (at -7.62 -7.62 0) (length 2.54)
        (name "GB")
        (number "GB")
      )
      (pin passive line (at 7.62 -7.62 180) (length 2.54)
        (name "M")
        (number "M1")
      )
      (pin passive line (at 7.62 2.54 180) (length 2.54)
        (name "S1")
        (number "S1")
      )
      (pin passive line (at 7.62 -2.54 180) (length 2.54)
        (name "S2")
        (number "S2")
      )
      (pin passive line (at -7.62 7.62 0) (length 2.54)
        (name "VA")
        (number "VA")
      )
      (pin passive line (at -7.62 5.08 0) (length 2.54)
        (name "VB")
        (number "VB")
      )
    )
  )
  (symbol "em20b:EM20B_LedRing" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 13.97 0))
    (property "Value" "EM20B_LedRing" (id 1) (at 0 11.43 0))
    (property "Footprint" "dp:EM20B_LedRing" (id 2) (at 0 -15.24 0))
    (property "Datasheet" "http://www.farnell.com/datasheets/1837003.pdf" (id 3) (at -1.27 -12.7 0))
    (property "ki_keywords" "EM20B LedRing" (id 4) (at 0 0 0))
    (property "ki_description" "EM20B LedRing" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "HDSM?541B?HDSM?543B*" (id 6) (at 0 0 0))
    (symbol "EM20B_LedRing_0_1")
    (symbol "EM20B_LedRing_1_1"
      (pin passive line (at -8.89 -6.35 0) (length 2.54) hide
        (name "GND")
        (number "1")
      )
      (pin bidirectional line (at 8.89 6.35 180) (length 2.54)
        (name "SDA3")
        (number "10")
      )
      (pin input line (at 8.89 3.81 180) (length 2.54)
        (name "SCL3")
        (number "11")
      )
      (pin passive line (at -8.89 -6.35 0) (length 2.54) hide
        (name "GND")
        (number "12")
      )
      (pin bidirectional line (at 8.89 -3.81 180) (length 2.54)
        (name "SDA1")
        (number "2")
      )
      (pin input line (at 8.89 -6.35 180) (length 2.54)
        (name "SCL1")
        (number "3")
      )
      (pin bidirectional line (at 8.89 1.27 180) (length 2.54)
        (name "SDA2")
        (number "4")
      )
      (pin input line (at 8.89 -1.27 180) (length 2.54)
        (name "SCL2")
        (number "5")
      )
      (pin power_in line (at -8.89 6.35 0) (length 2.54)
        (name "VCC")
        (number "8")
      )
      (pin power_in line (at -8.89 -6.35 0) (length 2.54)
        (name "GND")
        (number "9")
      )
    )
  )
)
