(footprint "EM20B" (version 20210108) (generator pcbnew) (layer "F.Cu")
  (tedit 600E059F)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 1.2) (layer "F.SilkS"))
  (fp_text value "EM20B" (at 0 -1) (layer "F.Fab"))
  (pad "A" thru_hole circle (at 1.3456 10.1904) (locked) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  (pad "B" thru_hole circle (at -3.8043 9.5488) (locked) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  (pad "GA" thru_hole circle (at 2.5754 9.8695) (locked) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  (pad "GB" thru_hole circle (at -2.5754 9.8695) (locked) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  (pad "M1" thru_hole oval (at -5 0) (size 2.4 3.2) (drill oval 1.8 2.6) (layers *.Cu *.Mask))
  (pad "M1" thru_hole oval (at 5 0) (size 2.4 3.2) (drill oval 1.8 2.6) (layers *.Cu *.Mask))
  (pad "S1" thru_hole circle (at -2.5 -7) (locked) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
  (pad "S2" thru_hole circle (at 2.5 -7) (locked) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
  (pad "VA" thru_hole circle (at 3.8043 9.5488) (locked) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  (pad "VB" thru_hole circle (at -1.3456 10.1904) (locked) (size 1 1) (drill 0.6) (layers *.Cu *.Mask))
  (model ":dp:em20b4014000.step"
    (offset (xyz 0 0 12.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
