(footprint "EM20B_LedRing" (version 20210108) (generator pcbnew) (layer "F.Cu")
  (tedit 600F5747)
  (descr "EM20B_LedRing")
  (attr smd)
  (fp_text reference "REF**" (at 0 1) (layer "F.SilkS"))
  (fp_text value "EM20B_LedRing" (at 0 -1) (layer "F.SilkS"))
  (fp_text user "${REFERENCE}" (at 0 1) (layer "F.Fab"))
  (pad "1" thru_hole circle (at -8.3147 -5.5557) (locked) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at -8.3147 5.5557) (locked) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask))
  (pad "3" thru_hole circle (at -6.9151 7.2236) (locked) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask))
  (pad "4" thru_hole circle (at -5.1877 8.5491) (locked) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask))
  (pad "5" thru_hole circle (at -3.2144 9.4693) (locked) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask))
  (pad "8" thru_hole circle (at 3.2144 9.4693) (locked) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask))
  (pad "9" thru_hole circle (at 5.1877 8.5491) (locked) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask))
  (pad "10" thru_hole circle (at 6.9151 7.2237) (locked) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask))
  (pad "11" thru_hole circle (at 8.3147 5.5557) (locked) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask))
  (pad "12" thru_hole circle (at 8.3147 -5.5557) (locked) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask))
  (model ":dp:em20b_ledrring.step"
    (offset (xyz 0 0 16))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
